{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Price List January 2025","Sheet1"],"not_rendered":{"charts":0,"images":5,"macros":1,"external_links":0,"defined_names":3,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Price List January 2025","index":0,"n_rows":110147,"n_cols":9,"rows_kept":4500,"cut":true,"hidden":false,"merged":[[0,1,0,2],[1,0,1,6],[2,2,2,6],[2,0,2,1],[0,3,0,8]],"bounds":{"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0}}
[null,"Siemens Digital Industries\nΤιμοκατάλογος Προϊόντων Βιομηχανίας 2025",null,"Ισχύει από την 01.01.2025 και καταργεί κάθε προηγούμενο. Οι τιμές και τα τεχνικά χαρακτηριστικά των υλικών υπόκεινται σε οποιαδήποτε αλλαγή χωρίς προηγούμενη ειδοποίηση και δεν περιλαμβάνουν ΦΠΑ. "]
["Περιλαμβάνει τις παρακάτω κατηγορίες υλικών:"]
["Βιομηχανικός αυτοματισμός SIMATIC (SIMATIC)\nLOGO!, τροφοδοτικά LOGO! Power (LOGO!)\nΌργανα Μέτρησης Πεδίου (PI1…PI7)\n",null,"Βιομηχανικό / Ηλεκτρολογικό Υλικό Χαμηλής Τάσης (EP) \nΡυθμιστές στροφών και συστήματα Motion control (GMC) \n"]
["Αναζήτηση υλικού","Αναζήτηση με:"]
["Κωδικός","Περιγραφή","Τιμή καταλόγου \n(€)","Μον. \nΜέτρησης","Ποσ. μονάδας μέτρησης","Κατηγορία \nυλικού","Ελάχιστη ποσότητα παραγγελίας",null,"Γρήγορη επιλογή κατηγορίας"]
["1FK2102-0AG00-0MA0","SIMOTICS S-1FK2 HD servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D8x25mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1354,"ST",1,"GMC",1,"1FK21020AG000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-0AG00-0SA0","SIMOTICS S-1FK2 HD servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D8x25mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",955,"ST",1,"GMC",1,"1FK21020AG000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-0AG00-1MA0","SIMOTICS S-1FK2 HD servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D8x25mm with fitted key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1354,"ST",1,"GMC",1,"1FK21020AG001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-0AG00-1SA0","SIMOTICS S-1FK2 HD servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D8x25mm with fitted key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",955,"ST",1,"GMC",1,"1FK21020AG001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-0AG01-0MA0","SIMOTICS S-1FK2 HD servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D8x25mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1465,"ST",1,"GMC",1,"1FK21020AG010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-0AG01-0SA0","SIMOTICS S-1FK2 HD servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D8x25mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1066,"ST",1,"GMC",1,"1FK21020AG010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-0AG01-1MA0","SIMOTICS S-1FK2 HD servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D8x25mm with fitted key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1465,"ST",1,"GMC",1,"1FK21020AG011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-0AG01-1SA0","SIMOTICS S-1FK2 HD servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D8x25mm with fitted key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1066,"ST",1,"GMC",1,"1FK21020AG011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-0AG10-0MA0","SIMOTICS S-1FK2 HD servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D8x25mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1620,"ST",1,"GMC",1,"1FK21020AG100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-0AG10-0SA0","SIMOTICS S-1FK2 HD servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D8x25mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1221,"ST",1,"GMC",1,"1FK21020AG100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-0AG10-1MA0","SIMOTICS S-1FK2 HD servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D8x25mm with fitted key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1620,"ST",1,"GMC",1,"1FK21020AG101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-0AG10-1SA0","SIMOTICS S-1FK2 HD servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D8x25mm with fitted key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1221,"ST",1,"GMC",1,"1FK21020AG101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-0AG11-0MA0","SIMOTICS S-1FK2 HD servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D8x25mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1732,"ST",1,"GMC",1,"1FK21020AG110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-0AG11-0SA0","SIMOTICS S-1FK2 HD servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D8x25mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1333,"ST",1,"GMC",1,"1FK21020AG110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-0AG11-1MA0","SIMOTICS S-1FK2 HD servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D8x25mm with fitted key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1732,"ST",1,"GMC",1,"1FK21020AG111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-0AG11-1SA0","SIMOTICS S-1FK2 HD servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D8x25mm with fitted key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1333,"ST",1,"GMC",1,"1FK21020AG111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-1AG00-0MA0","SIMOTICS S-1FK2 HD servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D8x25mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1380,"ST",1,"GMC",1,"1FK21021AG000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-1AG00-0SA0","SIMOTICS S-1FK2 HD servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D8x25mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",982,"ST",1,"GMC",1,"1FK21021AG000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-1AG00-1MA0","SIMOTICS S-1FK2 HD servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D8x25mm with fitted key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1380,"ST",1,"GMC",1,"1FK21021AG001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-1AG00-1SA0","SIMOTICS S-1FK2 HD servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D8x25mm with fitted key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",982,"ST",1,"GMC",1,"1FK21021AG001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-1AG01-0MA0","SIMOTICS S-1FK2 HD servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D8x25mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1492,"ST",1,"GMC",1,"1FK21021AG010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-1AG01-0SA0","SIMOTICS S-1FK2 HD servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D8x25mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1093,"ST",1,"GMC",1,"1FK21021AG010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-1AG01-1MA0","SIMOTICS S-1FK2 HD servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D8x25mm with fitted key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1492,"ST",1,"GMC",1,"1FK21021AG011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-1AG01-1SA0","SIMOTICS S-1FK2 HD servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D8x25mm with fitted key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1093,"ST",1,"GMC",1,"1FK21021AG011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-1AG10-0MA0","SIMOTICS S-1FK2 HD servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D8x25mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1647,"ST",1,"GMC",1,"1FK21021AG100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-1AG10-0SA0","SIMOTICS S-1FK2 HD servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D8x25mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1248,"ST",1,"GMC",1,"1FK21021AG100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-1AG10-1MA0","SIMOTICS S-1FK2 HD servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D8x25mm with fitted key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1647,"ST",1,"GMC",1,"1FK21021AG101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-1AG10-1SA0","SIMOTICS S-1FK2 HD servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D8x25mm with fitted key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1248,"ST",1,"GMC",1,"1FK21021AG101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-1AG11-0MA0","SIMOTICS S-1FK2 HD servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D8x25mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1758,"ST",1,"GMC",1,"1FK21021AG110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-1AG11-0SA0","SIMOTICS S-1FK2 HD servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D8x25mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1359,"ST",1,"GMC",1,"1FK21021AG110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-1AG11-1MA0","SIMOTICS S-1FK2 HD servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D8x25mm with fitted key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1758,"ST",1,"GMC",1,"1FK21021AG111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-1AG11-1SA0","SIMOTICS S-1FK2 HD servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D8x25mm with fitted key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1359,"ST",1,"GMC",1,"1FK21021AG111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AG00-0MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1460,"ST",1,"GMC",1,"1FK21032AG000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AG00-0SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1061,"ST",1,"GMC",1,"1FK21032AG000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AG00-1MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1460,"ST",1,"GMC",1,"1FK21032AG001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AG00-1SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1061,"ST",1,"GMC",1,"1FK21032AG001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AG00-2MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1460,"ST",1,"GMC",1,"1FK21032AG002MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AG00-2SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1061,"ST",1,"GMC",1,"1FK21032AG002SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AG01-0MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1571,"ST",1,"GMC",1,"1FK21032AG010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AG01-0SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1172,"ST",1,"GMC",1,"1FK21032AG010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AG01-1MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1571,"ST",1,"GMC",1,"1FK21032AG011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AG01-1SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1172,"ST",1,"GMC",1,"1FK21032AG011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AG01-2MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M12, rotatable; .",1571,"ST",1,"GMC",1,"1FK21032AG012MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AG01-2SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M12, rotatable; .",1172,"ST",1,"GMC",1,"1FK21032AG012SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AG10-0MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1780,"ST",1,"GMC",1,"1FK21032AG100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AG10-0SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1381,"ST",1,"GMC",1,"1FK21032AG100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AG10-1MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1780,"ST",1,"GMC",1,"1FK21032AG101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AG10-1SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1381,"ST",1,"GMC",1,"1FK21032AG101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AG10-2MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1780,"ST",1,"GMC",1,"1FK21032AG102MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AG10-2SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1381,"ST",1,"GMC",1,"1FK21032AG102SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AG11-0MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1891,"ST",1,"GMC",1,"1FK21032AG110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AG11-0SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1492,"ST",1,"GMC",1,"1FK21032AG110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AG11-1MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1891,"ST",1,"GMC",1,"1FK21032AG111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AG11-1SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1492,"ST",1,"GMC",1,"1FK21032AG111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AG11-2MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M12, rotatable; .",1891,"ST",1,"GMC",1,"1FK21032AG112MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AG11-2SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M12, rotatable; .",1492,"ST",1,"GMC",1,"1FK21032AG112SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH00-0MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1460,"ST",1,"GMC",1,"1FK21032AH000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH00-0MB0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1460,"ST",1,"GMC",1,"1FK21032AH000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH00-0SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1061,"ST",1,"GMC",1,"1FK21032AH000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH00-0SB0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1061,"ST",1,"GMC",1,"1FK21032AH000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH00-1MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1460,"ST",1,"GMC",1,"1FK21032AH001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH00-1MB0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1460,"ST",1,"GMC",1,"1FK21032AH001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH00-1SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1061,"ST",1,"GMC",1,"1FK21032AH001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH00-1SB0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1061,"ST",1,"GMC",1,"1FK21032AH001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH00-2MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1460,"ST",1,"GMC",1,"1FK21032AH002MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH00-2MB0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1460,"ST",1,"GMC",1,"1FK21032AH002MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH00-2SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1061,"ST",1,"GMC",1,"1FK21032AH002SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH00-2SB0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1061,"ST",1,"GMC",1,"1FK21032AH002SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH01-0MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1571,"ST",1,"GMC",1,"1FK21032AH010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH01-0MB0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1571,"ST",1,"GMC",1,"1FK21032AH010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH01-0SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1172,"ST",1,"GMC",1,"1FK21032AH010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH01-0SB0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1172,"ST",1,"GMC",1,"1FK21032AH010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH01-1MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1571,"ST",1,"GMC",1,"1FK21032AH011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH01-1MB0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1571,"ST",1,"GMC",1,"1FK21032AH011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH01-1SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1172,"ST",1,"GMC",1,"1FK21032AH011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH01-1SB0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1172,"ST",1,"GMC",1,"1FK21032AH011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH01-2MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable; .",1571,"ST",1,"GMC",1,"1FK21032AH012MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH01-2MB0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17; .",1571,"ST",1,"GMC",1,"1FK21032AH012MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH01-2SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable; .",1172,"ST",1,"GMC",1,"1FK21032AH012SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH01-2SB0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17; .",1172,"ST",1,"GMC",1,"1FK21032AH012SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH10-0MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1780,"ST",1,"GMC",1,"1FK21032AH100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH10-0MB0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1780,"ST",1,"GMC",1,"1FK21032AH100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH10-0SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1381,"ST",1,"GMC",1,"1FK21032AH100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH10-0SB0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1381,"ST",1,"GMC",1,"1FK21032AH100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH10-1MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1780,"ST",1,"GMC",1,"1FK21032AH101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH10-1MB0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1780,"ST",1,"GMC",1,"1FK21032AH101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH10-1SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1381,"ST",1,"GMC",1,"1FK21032AH101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH10-1SB0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1381,"ST",1,"GMC",1,"1FK21032AH101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH10-2MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1780,"ST",1,"GMC",1,"1FK21032AH102MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH10-2MB0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1780,"ST",1,"GMC",1,"1FK21032AH102MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH10-2SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1381,"ST",1,"GMC",1,"1FK21032AH102SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH10-2SB0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1381,"ST",1,"GMC",1,"1FK21032AH102SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH11-0MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1891,"ST",1,"GMC",1,"1FK21032AH110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH11-0MB0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1891,"ST",1,"GMC",1,"1FK21032AH110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH11-0SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1492,"ST",1,"GMC",1,"1FK21032AH110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH11-0SB0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1492,"ST",1,"GMC",1,"1FK21032AH110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH11-1MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1891,"ST",1,"GMC",1,"1FK21032AH111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH11-1MB0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1891,"ST",1,"GMC",1,"1FK21032AH111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH11-1SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1492,"ST",1,"GMC",1,"1FK21032AH111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH11-1SB0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1492,"ST",1,"GMC",1,"1FK21032AH111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH11-2MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable; .",1891,"ST",1,"GMC",1,"1FK21032AH112MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH11-2MB0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1891,"ST",1,"GMC",1,"1FK21032AH112MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH11-2SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable; .",1492,"ST",1,"GMC",1,"1FK21032AH112SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH11-2SB0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1492,"ST",1,"GMC",1,"1FK21032AH112SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AG00-0MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1619,"ST",1,"GMC",1,"1FK21034AG000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AG00-0SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1220,"ST",1,"GMC",1,"1FK21034AG000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AG00-1MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1619,"ST",1,"GMC",1,"1FK21034AG001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AG00-1SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1220,"ST",1,"GMC",1,"1FK21034AG001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AG00-2MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1619,"ST",1,"GMC",1,"1FK21034AG002MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AG00-2SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1220,"ST",1,"GMC",1,"1FK21034AG002SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AG01-0MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1730,"ST",1,"GMC",1,"1FK21034AG010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AG01-0SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1332,"ST",1,"GMC",1,"1FK21034AG010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AG01-1MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1730,"ST",1,"GMC",1,"1FK21034AG011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AG01-1SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1332,"ST",1,"GMC",1,"1FK21034AG011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AG01-2MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M12, rotatable; .",1730,"ST",1,"GMC",1,"1FK21034AG012MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AG01-2SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M12, rotatable; .",1332,"ST",1,"GMC",1,"1FK21034AG012SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AG10-0MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1939,"ST",1,"GMC",1,"1FK21034AG100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AG10-0SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1540,"ST",1,"GMC",1,"1FK21034AG100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AG10-1MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1939,"ST",1,"GMC",1,"1FK21034AG101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AG10-1SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1540,"ST",1,"GMC",1,"1FK21034AG101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AG10-2MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1939,"ST",1,"GMC",1,"1FK21034AG102MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AG10-2SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1540,"ST",1,"GMC",1,"1FK21034AG102SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AG11-0MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",2050,"ST",1,"GMC",1,"1FK21034AG110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AG11-0SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1651,"ST",1,"GMC",1,"1FK21034AG110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AG11-1MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",2050,"ST",1,"GMC",1,"1FK21034AG111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AG11-1SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1651,"ST",1,"GMC",1,"1FK21034AG111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AG11-2MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M12, rotatable; .",2050,"ST",1,"GMC",1,"1FK21034AG112MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AG11-2SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M12, rotatable; .",1651,"ST",1,"GMC",1,"1FK21034AG112SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH00-0MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1619,"ST",1,"GMC",1,"1FK21034AH000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH00-0MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1619,"ST",1,"GMC",1,"1FK21034AH000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH00-0SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1220,"ST",1,"GMC",1,"1FK21034AH000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH00-0SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1220,"ST",1,"GMC",1,"1FK21034AH000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH00-1MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1619,"ST",1,"GMC",1,"1FK21034AH001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH00-1MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1619,"ST",1,"GMC",1,"1FK21034AH001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH00-1SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1220,"ST",1,"GMC",1,"1FK21034AH001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH00-1SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1220,"ST",1,"GMC",1,"1FK21034AH001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH00-2MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1619,"ST",1,"GMC",1,"1FK21034AH002MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH00-2MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1619,"ST",1,"GMC",1,"1FK21034AH002MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH00-2SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1220,"ST",1,"GMC",1,"1FK21034AH002SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH00-2SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1220,"ST",1,"GMC",1,"1FK21034AH002SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH01-0MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1730,"ST",1,"GMC",1,"1FK21034AH010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH01-0MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1730,"ST",1,"GMC",1,"1FK21034AH010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH01-0SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1332,"ST",1,"GMC",1,"1FK21034AH010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH01-0SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1332,"ST",1,"GMC",1,"1FK21034AH010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH01-1MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1730,"ST",1,"GMC",1,"1FK21034AH011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH01-1MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1730,"ST",1,"GMC",1,"1FK21034AH011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH01-1SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1332,"ST",1,"GMC",1,"1FK21034AH011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH01-1SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1332,"ST",1,"GMC",1,"1FK21034AH011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH01-2MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable; .",1730,"ST",1,"GMC",1,"1FK21034AH012MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH01-2MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17; .",1730,"ST",1,"GMC",1,"1FK21034AH012MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH01-2SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable; .",1332,"ST",1,"GMC",1,"1FK21034AH012SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH01-2SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17; .",1332,"ST",1,"GMC",1,"1FK21034AH012SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH10-0MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1939,"ST",1,"GMC",1,"1FK21034AH100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH10-0MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1939,"ST",1,"GMC",1,"1FK21034AH100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH10-0SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1540,"ST",1,"GMC",1,"1FK21034AH100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH10-0SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1540,"ST",1,"GMC",1,"1FK21034AH100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH10-1MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1939,"ST",1,"GMC",1,"1FK21034AH101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH10-1MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1939,"ST",1,"GMC",1,"1FK21034AH101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH10-1SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1540,"ST",1,"GMC",1,"1FK21034AH101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH10-1SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1540,"ST",1,"GMC",1,"1FK21034AH101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH10-2MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1939,"ST",1,"GMC",1,"1FK21034AH102MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH10-2MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1939,"ST",1,"GMC",1,"1FK21034AH102MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH10-2SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1540,"ST",1,"GMC",1,"1FK21034AH102SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH10-2SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1540,"ST",1,"GMC",1,"1FK21034AH102SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH11-0MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2050,"ST",1,"GMC",1,"1FK21034AH110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH11-0MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2050,"ST",1,"GMC",1,"1FK21034AH110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH11-0SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1651,"ST",1,"GMC",1,"1FK21034AH110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH11-0SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1651,"ST",1,"GMC",1,"1FK21034AH110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH11-1MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2050,"ST",1,"GMC",1,"1FK21034AH111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH11-1MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2050,"ST",1,"GMC",1,"1FK21034AH111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH11-1SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1651,"ST",1,"GMC",1,"1FK21034AH111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH11-1SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1651,"ST",1,"GMC",1,"1FK21034AH111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH11-2MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable; .",2050,"ST",1,"GMC",1,"1FK21034AH112MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH11-2MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",2050,"ST",1,"GMC",1,"1FK21034AH112MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH11-2SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable; .",1651,"ST",1,"GMC",1,"1FK21034AH112SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH11-2SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1651,"ST",1,"GMC",1,"1FK21034AH112SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF00-0MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1619,"ST",1,"GMC",1,"1FK21044AF000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF00-0MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1619,"ST",1,"GMC",1,"1FK21044AF000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF00-0SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1220,"ST",1,"GMC",1,"1FK21044AF000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF00-0SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1220,"ST",1,"GMC",1,"1FK21044AF000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF00-1MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1619,"ST",1,"GMC",1,"1FK21044AF001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF00-1MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1619,"ST",1,"GMC",1,"1FK21044AF001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF00-1SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1220,"ST",1,"GMC",1,"1FK21044AF001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF00-1SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1220,"ST",1,"GMC",1,"1FK21044AF001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF00-2MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1619,"ST",1,"GMC",1,"1FK21044AF002MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF00-2MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1619,"ST",1,"GMC",1,"1FK21044AF002MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF00-2SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1220,"ST",1,"GMC",1,"1FK21044AF002SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF00-2SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1220,"ST",1,"GMC",1,"1FK21044AF002SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF01-0MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1730,"ST",1,"GMC",1,"1FK21044AF010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF01-0MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1730,"ST",1,"GMC",1,"1FK21044AF010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF01-0SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1332,"ST",1,"GMC",1,"1FK21044AF010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF01-0SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1332,"ST",1,"GMC",1,"1FK21044AF010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF01-1MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1730,"ST",1,"GMC",1,"1FK21044AF011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF01-1MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1730,"ST",1,"GMC",1,"1FK21044AF011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF01-1SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1332,"ST",1,"GMC",1,"1FK21044AF011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF01-1SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1332,"ST",1,"GMC",1,"1FK21044AF011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF01-2MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480V); PN = 0.2 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M17, rotatable; .",1730,"ST",1,"GMC",1,"1FK21044AF012MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF01-2MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480V); PN = 0.2 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1730,"ST",1,"GMC",1,"1FK21044AF012MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF01-2SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480V); PN = 0.2 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M17, rotatable; .",1332,"ST",1,"GMC",1,"1FK21044AF012SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF01-2SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480V); PN = 0.2 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1332,"ST",1,"GMC",1,"1FK21044AF012SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF10-0MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1939,"ST",1,"GMC",1,"1FK21044AF100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF10-0MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1939,"ST",1,"GMC",1,"1FK21044AF100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF10-0SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1540,"ST",1,"GMC",1,"1FK21044AF100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF10-0SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1540,"ST",1,"GMC",1,"1FK21044AF100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF10-1MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1939,"ST",1,"GMC",1,"1FK21044AF101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF10-1MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1939,"ST",1,"GMC",1,"1FK21044AF101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF10-1SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1540,"ST",1,"GMC",1,"1FK21044AF101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF10-1SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1540,"ST",1,"GMC",1,"1FK21044AF101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF10-2MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1939,"ST",1,"GMC",1,"1FK21044AF102MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF10-2MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1939,"ST",1,"GMC",1,"1FK21044AF102MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF10-2SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1540,"ST",1,"GMC",1,"1FK21044AF102SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF10-2SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1540,"ST",1,"GMC",1,"1FK21044AF102SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF11-0MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2050,"ST",1,"GMC",1,"1FK21044AF110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF11-0MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2050,"ST",1,"GMC",1,"1FK21044AF110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF11-0SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1651,"ST",1,"GMC",1,"1FK21044AF110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF11-0SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1651,"ST",1,"GMC",1,"1FK21044AF110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF11-1MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2050,"ST",1,"GMC",1,"1FK21044AF111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF11-1MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2050,"ST",1,"GMC",1,"1FK21044AF111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF11-1SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1651,"ST",1,"GMC",1,"1FK21044AF111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF11-1SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1651,"ST",1,"GMC",1,"1FK21044AF111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF11-2MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480V); PN = 0.2 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M17, rotatable; .",2050,"ST",1,"GMC",1,"1FK21044AF112MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF11-2MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480V); PN = 0.2 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",2050,"ST",1,"GMC",1,"1FK21044AF112MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF11-2SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480V); PN = 0.2 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M17, rotatable; .",1651,"ST",1,"GMC",1,"1FK21044AF112SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF11-2SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480V); PN = 0.2 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1651,"ST",1,"GMC",1,"1FK21044AF112SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK00-0MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1619,"ST",1,"GMC",1,"1FK21044AK000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK00-0MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1619,"ST",1,"GMC",1,"1FK21044AK000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK00-0SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1220,"ST",1,"GMC",1,"1FK21044AK000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK00-0SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1220,"ST",1,"GMC",1,"1FK21044AK000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK00-1MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1619,"ST",1,"GMC",1,"1FK21044AK001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK00-1MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1619,"ST",1,"GMC",1,"1FK21044AK001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK00-1SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1220,"ST",1,"GMC",1,"1FK21044AK001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK00-1SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1220,"ST",1,"GMC",1,"1FK21044AK001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK00-2MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1619,"ST",1,"GMC",1,"1FK21044AK002MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK00-2MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1619,"ST",1,"GMC",1,"1FK21044AK002MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK00-2SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1220,"ST",1,"GMC",1,"1FK21044AK002SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK00-2SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1220,"ST",1,"GMC",1,"1FK21044AK002SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK01-0MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1730,"ST",1,"GMC",1,"1FK21044AK010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK01-0MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1730,"ST",1,"GMC",1,"1FK21044AK010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK01-0SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1332,"ST",1,"GMC",1,"1FK21044AK010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK01-0SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1332,"ST",1,"GMC",1,"1FK21044AK010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK01-1MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1730,"ST",1,"GMC",1,"1FK21044AK011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK01-1MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1730,"ST",1,"GMC",1,"1FK21044AK011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK01-1SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1332,"ST",1,"GMC",1,"1FK21044AK011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK01-1SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1332,"ST",1,"GMC",1,"1FK21044AK011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK01-2MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480V); PN = 0.4 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M17, rotatable; .",1730,"ST",1,"GMC",1,"1FK21044AK012MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK01-2MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1730,"ST",1,"GMC",1,"1FK21044AK012MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK01-2SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480V); PN = 0.4 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M17, rotatable; .",1332,"ST",1,"GMC",1,"1FK21044AK012SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK01-2SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1332,"ST",1,"GMC",1,"1FK21044AK012SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK10-0MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1939,"ST",1,"GMC",1,"1FK21044AK100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK10-0MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1939,"ST",1,"GMC",1,"1FK21044AK100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK10-0SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1540,"ST",1,"GMC",1,"1FK21044AK100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK10-0SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1540,"ST",1,"GMC",1,"1FK21044AK100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK10-1MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1939,"ST",1,"GMC",1,"1FK21044AK101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK10-1MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1939,"ST",1,"GMC",1,"1FK21044AK101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK10-1SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1540,"ST",1,"GMC",1,"1FK21044AK101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK10-1SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1540,"ST",1,"GMC",1,"1FK21044AK101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK10-2MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1939,"ST",1,"GMC",1,"1FK21044AK102MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK10-2MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1939,"ST",1,"GMC",1,"1FK21044AK102MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK10-2SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1540,"ST",1,"GMC",1,"1FK21044AK102SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK10-2SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1540,"ST",1,"GMC",1,"1FK21044AK102SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK11-0MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2050,"ST",1,"GMC",1,"1FK21044AK110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK11-0MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2050,"ST",1,"GMC",1,"1FK21044AK110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK11-0SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1651,"ST",1,"GMC",1,"1FK21044AK110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK11-0SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1651,"ST",1,"GMC",1,"1FK21044AK110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK11-1MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2050,"ST",1,"GMC",1,"1FK21044AK111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK11-1MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2050,"ST",1,"GMC",1,"1FK21044AK111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK11-1SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1651,"ST",1,"GMC",1,"1FK21044AK111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK11-1SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1651,"ST",1,"GMC",1,"1FK21044AK111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK11-2MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480V); PN = 0.4 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M17, rotatable; .",2050,"ST",1,"GMC",1,"1FK21044AK112MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK11-2MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",2050,"ST",1,"GMC",1,"1FK21044AK112MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK11-2SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480V); PN = 0.4 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M17, rotatable; .",1651,"ST",1,"GMC",1,"1FK21044AK112SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK11-2SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1651,"ST",1,"GMC",1,"1FK21044AK112SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF00-0MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1752,"ST",1,"GMC",1,"1FK21045AF000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF00-0MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1752,"ST",1,"GMC",1,"1FK21045AF000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF00-0SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1353,"ST",1,"GMC",1,"1FK21045AF000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF00-0SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1353,"ST",1,"GMC",1,"1FK21045AF000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF00-1MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1752,"ST",1,"GMC",1,"1FK21045AF001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF00-1MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1752,"ST",1,"GMC",1,"1FK21045AF001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF00-1SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1353,"ST",1,"GMC",1,"1FK21045AF001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF00-1SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1353,"ST",1,"GMC",1,"1FK21045AF001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF00-2MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1752,"ST",1,"GMC",1,"1FK21045AF002MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF00-2MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1752,"ST",1,"GMC",1,"1FK21045AF002MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF00-2SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1353,"ST",1,"GMC",1,"1FK21045AF002SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF00-2SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1353,"ST",1,"GMC",1,"1FK21045AF002SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF01-0MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1863,"ST",1,"GMC",1,"1FK21045AF010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF01-0MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1863,"ST",1,"GMC",1,"1FK21045AF010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF01-0SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1464,"ST",1,"GMC",1,"1FK21045AF010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF01-0SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1464,"ST",1,"GMC",1,"1FK21045AF010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF01-1MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1863,"ST",1,"GMC",1,"1FK21045AF011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF01-1MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1863,"ST",1,"GMC",1,"1FK21045AF011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF01-1SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1464,"ST",1,"GMC",1,"1FK21045AF011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF01-1SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1464,"ST",1,"GMC",1,"1FK21045AF011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF01-2MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480V); PN = 0.375 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M17, rotatable; .",1863,"ST",1,"GMC",1,"1FK21045AF012MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF01-2MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480V); PN = 0.375 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1863,"ST",1,"GMC",1,"1FK21045AF012MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF01-2SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480V); PN = 0.375 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M17, rotatable; .",1464,"ST",1,"GMC",1,"1FK21045AF012SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF01-2SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480V); PN = 0.375 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1464,"ST",1,"GMC",1,"1FK21045AF012SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF10-0MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2071,"ST",1,"GMC",1,"1FK21045AF100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF10-0MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2071,"ST",1,"GMC",1,"1FK21045AF100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF10-0SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1672,"ST",1,"GMC",1,"1FK21045AF100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF10-0SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1672,"ST",1,"GMC",1,"1FK21045AF100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF10-1MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2071,"ST",1,"GMC",1,"1FK21045AF101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF10-1MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2071,"ST",1,"GMC",1,"1FK21045AF101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF10-1SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1672,"ST",1,"GMC",1,"1FK21045AF101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF10-1SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1672,"ST",1,"GMC",1,"1FK21045AF101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF10-2MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2071,"ST",1,"GMC",1,"1FK21045AF102MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF10-2MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2071,"ST",1,"GMC",1,"1FK21045AF102MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF10-2SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1672,"ST",1,"GMC",1,"1FK21045AF102SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF10-2SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1672,"ST",1,"GMC",1,"1FK21045AF102SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF11-0MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2183,"ST",1,"GMC",1,"1FK21045AF110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF11-0MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2183,"ST",1,"GMC",1,"1FK21045AF110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF11-0SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1784,"ST",1,"GMC",1,"1FK21045AF110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF11-0SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1784,"ST",1,"GMC",1,"1FK21045AF110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF11-1MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2183,"ST",1,"GMC",1,"1FK21045AF111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF11-1MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2183,"ST",1,"GMC",1,"1FK21045AF111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF11-1SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1784,"ST",1,"GMC",1,"1FK21045AF111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF11-1SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1784,"ST",1,"GMC",1,"1FK21045AF111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF11-2MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480V); PN = 0.375 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M17, rotatable; .",2183,"ST",1,"GMC",1,"1FK21045AF112MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF11-2MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480V); PN = 0.375 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",2183,"ST",1,"GMC",1,"1FK21045AF112MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF11-2SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480V); PN = 0.375 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M17, rotatable; .",1784,"ST",1,"GMC",1,"1FK21045AF112SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF11-2SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480V); PN = 0.375 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1784,"ST",1,"GMC",1,"1FK21045AF112SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK00-0MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1752,"ST",1,"GMC",1,"1FK21045AK000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK00-0MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1752,"ST",1,"GMC",1,"1FK21045AK000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK00-0SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1353,"ST",1,"GMC",1,"1FK21045AK000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK00-0SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1353,"ST",1,"GMC",1,"1FK21045AK000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK00-1MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1752,"ST",1,"GMC",1,"1FK21045AK001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK00-1MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1752,"ST",1,"GMC",1,"1FK21045AK001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK00-1SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1353,"ST",1,"GMC",1,"1FK21045AK001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK00-1SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1353,"ST",1,"GMC",1,"1FK21045AK001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK00-2MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1752,"ST",1,"GMC",1,"1FK21045AK002MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK00-2MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1752,"ST",1,"GMC",1,"1FK21045AK002MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK00-2SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1353,"ST",1,"GMC",1,"1FK21045AK002SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK00-2SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1353,"ST",1,"GMC",1,"1FK21045AK002SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK01-0MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1863,"ST",1,"GMC",1,"1FK21045AK010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK01-0MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1863,"ST",1,"GMC",1,"1FK21045AK010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK01-0SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1464,"ST",1,"GMC",1,"1FK21045AK010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK01-0SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1464,"ST",1,"GMC",1,"1FK21045AK010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK01-1MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1863,"ST",1,"GMC",1,"1FK21045AK011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK01-1MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1863,"ST",1,"GMC",1,"1FK21045AK011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK01-1SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1464,"ST",1,"GMC",1,"1FK21045AK011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK01-1SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1464,"ST",1,"GMC",1,"1FK21045AK011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK01-2MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480V); PN = 0.75 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M17, rotatable; .",1863,"ST",1,"GMC",1,"1FK21045AK012MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK01-2MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1863,"ST",1,"GMC",1,"1FK21045AK012MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK01-2SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480V); PN = 0.75 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M17, rotatable; .",1464,"ST",1,"GMC",1,"1FK21045AK012SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK01-2SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1464,"ST",1,"GMC",1,"1FK21045AK012SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK10-0MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2071,"ST",1,"GMC",1,"1FK21045AK100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK10-0MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2071,"ST",1,"GMC",1,"1FK21045AK100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK10-0SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1672,"ST",1,"GMC",1,"1FK21045AK100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK10-0SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1672,"ST",1,"GMC",1,"1FK21045AK100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK10-1MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2071,"ST",1,"GMC",1,"1FK21045AK101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK10-1MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2071,"ST",1,"GMC",1,"1FK21045AK101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK10-1SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1672,"ST",1,"GMC",1,"1FK21045AK101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK10-1SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1672,"ST",1,"GMC",1,"1FK21045AK101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK10-2MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2071,"ST",1,"GMC",1,"1FK21045AK102MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK10-2MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2071,"ST",1,"GMC",1,"1FK21045AK102MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK10-2SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1672,"ST",1,"GMC",1,"1FK21045AK102SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK10-2SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1672,"ST",1,"GMC",1,"1FK21045AK102SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK11-0MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2183,"ST",1,"GMC",1,"1FK21045AK110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK11-0MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2183,"ST",1,"GMC",1,"1FK21045AK110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK11-0SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1784,"ST",1,"GMC",1,"1FK21045AK110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK11-0SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1784,"ST",1,"GMC",1,"1FK21045AK110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK11-1MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2183,"ST",1,"GMC",1,"1FK21045AK111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK11-1MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2183,"ST",1,"GMC",1,"1FK21045AK111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK11-1SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1784,"ST",1,"GMC",1,"1FK21045AK111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK11-1SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1784,"ST",1,"GMC",1,"1FK21045AK111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK11-2MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480V); PN = 0.75 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M17, rotatable; .",2183,"ST",1,"GMC",1,"1FK21045AK112MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK11-2MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",2183,"ST",1,"GMC",1,"1FK21045AK112MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK11-2SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480V); PN = 0.75 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M17, rotatable; .",1784,"ST",1,"GMC",1,"1FK21045AK112SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK11-2SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1784,"ST",1,"GMC",1,"1FK21045AK112SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF00-0MA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1831,"ST",1,"GMC",1,"1FK21046AF000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF00-0MB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1831,"ST",1,"GMC",1,"1FK21046AF000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF00-0SA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1432,"ST",1,"GMC",1,"1FK21046AF000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF00-0SB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1432,"ST",1,"GMC",1,"1FK21046AF000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF00-1MA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1831,"ST",1,"GMC",1,"1FK21046AF001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF00-1MB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1831,"ST",1,"GMC",1,"1FK21046AF001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF00-1SA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1432,"ST",1,"GMC",1,"1FK21046AF001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF00-1SB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1432,"ST",1,"GMC",1,"1FK21046AF001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF00-2MA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1831,"ST",1,"GMC",1,"1FK21046AF002MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF00-2MB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1831,"ST",1,"GMC",1,"1FK21046AF002MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF00-2SA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1432,"ST",1,"GMC",1,"1FK21046AF002SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF00-2SB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1432,"ST",1,"GMC",1,"1FK21046AF002SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF01-0MA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1943,"ST",1,"GMC",1,"1FK21046AF010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF01-0MB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1943,"ST",1,"GMC",1,"1FK21046AF010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF01-0SA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1544,"ST",1,"GMC",1,"1FK21046AF010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF01-0SB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1544,"ST",1,"GMC",1,"1FK21046AF010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF01-1MA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1943,"ST",1,"GMC",1,"1FK21046AF011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF01-1MB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1943,"ST",1,"GMC",1,"1FK21046AF011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF01-1SA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1544,"ST",1,"GMC",1,"1FK21046AF011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF01-1SB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1544,"ST",1,"GMC",1,"1FK21046AF011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF01-2MA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480V); PN = 0.5 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M17, rotatable; .",1943,"ST",1,"GMC",1,"1FK21046AF012MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF01-2MB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480V); PN = 0.5 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1943,"ST",1,"GMC",1,"1FK21046AF012MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF01-2SA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480V); PN = 0.5 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M17, rotatable; .",1544,"ST",1,"GMC",1,"1FK21046AF012SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF01-2SB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480V); PN = 0.5 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1544,"ST",1,"GMC",1,"1FK21046AF012SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF10-0MA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2151,"ST",1,"GMC",1,"1FK21046AF100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF10-0MB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2151,"ST",1,"GMC",1,"1FK21046AF100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF10-0SA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1752,"ST",1,"GMC",1,"1FK21046AF100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF10-0SB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1752,"ST",1,"GMC",1,"1FK21046AF100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF10-1MA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2151,"ST",1,"GMC",1,"1FK21046AF101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF10-1MB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2151,"ST",1,"GMC",1,"1FK21046AF101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF10-1SA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1752,"ST",1,"GMC",1,"1FK21046AF101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF10-1SB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1752,"ST",1,"GMC",1,"1FK21046AF101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF10-2MA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2151,"ST",1,"GMC",1,"1FK21046AF102MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF10-2MB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2151,"ST",1,"GMC",1,"1FK21046AF102MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF10-2SA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1752,"ST",1,"GMC",1,"1FK21046AF102SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF10-2SB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1752,"ST",1,"GMC",1,"1FK21046AF102SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF11-0MA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2262,"ST",1,"GMC",1,"1FK21046AF110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF11-0MB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2262,"ST",1,"GMC",1,"1FK21046AF110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF11-0SA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1863,"ST",1,"GMC",1,"1FK21046AF110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF11-0SB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1863,"ST",1,"GMC",1,"1FK21046AF110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF11-1MA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2262,"ST",1,"GMC",1,"1FK21046AF111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF11-1MB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2262,"ST",1,"GMC",1,"1FK21046AF111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF11-1SA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1863,"ST",1,"GMC",1,"1FK21046AF111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF11-1SB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1863,"ST",1,"GMC",1,"1FK21046AF111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF11-2MA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480V); PN = 0.5 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M17, rotatable; .",2262,"ST",1,"GMC",1,"1FK21046AF112MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF11-2MB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480V); PN = 0.5 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",2262,"ST",1,"GMC",1,"1FK21046AF112MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF11-2SA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480V); PN = 0.5 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M17, rotatable; .",1863,"ST",1,"GMC",1,"1FK21046AF112SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF11-2SB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480V); PN = 0.5 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1863,"ST",1,"GMC",1,"1FK21046AF112SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF00-0MA0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2038,"ST",1,"GMC",1,"1FK21054AF000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF00-0MB0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2038,"ST",1,"GMC",1,"1FK21054AF000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF00-0SA0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1639,"ST",1,"GMC",1,"1FK21054AF000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF00-0SB0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1639,"ST",1,"GMC",1,"1FK21054AF000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF00-1MA0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2038,"ST",1,"GMC",1,"1FK21054AF001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF00-1MB0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2038,"ST",1,"GMC",1,"1FK21054AF001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF00-1SA0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1639,"ST",1,"GMC",1,"1FK21054AF001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF00-1SB0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1639,"ST",1,"GMC",1,"1FK21054AF001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF01-0MA0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2150,"ST",1,"GMC",1,"1FK21054AF010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF01-0MB0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2150,"ST",1,"GMC",1,"1FK21054AF010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF01-0SA0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1751,"ST",1,"GMC",1,"1FK21054AF010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF01-0SB0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1751,"ST",1,"GMC",1,"1FK21054AF010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF01-1MA0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2150,"ST",1,"GMC",1,"1FK21054AF011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF01-1MB0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2150,"ST",1,"GMC",1,"1FK21054AF011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF01-1SA0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1751,"ST",1,"GMC",1,"1FK21054AF011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF01-1SB0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1751,"ST",1,"GMC",1,"1FK21054AF011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF10-0MA0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2411,"ST",1,"GMC",1,"1FK21054AF100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF10-0MB0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2411,"ST",1,"GMC",1,"1FK21054AF100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF10-0SA0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",2012,"ST",1,"GMC",1,"1FK21054AF100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF10-0SB0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2012,"ST",1,"GMC",1,"1FK21054AF100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF10-1MA0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2411,"ST",1,"GMC",1,"1FK21054AF101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF10-1MB0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2411,"ST",1,"GMC",1,"1FK21054AF101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF10-1SA0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",2012,"ST",1,"GMC",1,"1FK21054AF101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF10-1SB0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2012,"ST",1,"GMC",1,"1FK21054AF101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF11-0MA0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2523,"ST",1,"GMC",1,"1FK21054AF110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF11-0MB0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2523,"ST",1,"GMC",1,"1FK21054AF110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF11-0SA0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",2124,"ST",1,"GMC",1,"1FK21054AF110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF11-0SB0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2124,"ST",1,"GMC",1,"1FK21054AF110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF11-1MA0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2523,"ST",1,"GMC",1,"1FK21054AF111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF11-1MB0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2523,"ST",1,"GMC",1,"1FK21054AF111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF11-1SA0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",2124,"ST",1,"GMC",1,"1FK21054AF111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF11-1SB0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2124,"ST",1,"GMC",1,"1FK21054AF111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF00-0MA0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2361,"ST",1,"GMC",1,"1FK21056AF000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF00-0MB0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2361,"ST",1,"GMC",1,"1FK21056AF000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF00-0SA0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1963,"ST",1,"GMC",1,"1FK21056AF000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF00-0SB0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1963,"ST",1,"GMC",1,"1FK21056AF000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF00-1MA0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2361,"ST",1,"GMC",1,"1FK21056AF001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF00-1MB0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2361,"ST",1,"GMC",1,"1FK21056AF001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF00-1SA0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1963,"ST",1,"GMC",1,"1FK21056AF001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF00-1SB0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1963,"ST",1,"GMC",1,"1FK21056AF001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF01-0MA0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2473,"ST",1,"GMC",1,"1FK21056AF010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF01-0MB0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2473,"ST",1,"GMC",1,"1FK21056AF010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF01-0SA0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",2074,"ST",1,"GMC",1,"1FK21056AF010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF01-0SB0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2074,"ST",1,"GMC",1,"1FK21056AF010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF01-1MA0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2473,"ST",1,"GMC",1,"1FK21056AF011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF01-1MB0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2473,"ST",1,"GMC",1,"1FK21056AF011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF01-1SA0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",2074,"ST",1,"GMC",1,"1FK21056AF011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF01-1SB0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2074,"ST",1,"GMC",1,"1FK21056AF011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF10-0MA0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2735,"ST",1,"GMC",1,"1FK21056AF100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF10-0MB0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2735,"ST",1,"GMC",1,"1FK21056AF100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF10-0SA0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",2336,"ST",1,"GMC",1,"1FK21056AF100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF10-0SB0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2336,"ST",1,"GMC",1,"1FK21056AF100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF10-1MA0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2735,"ST",1,"GMC",1,"1FK21056AF101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF10-1MB0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2735,"ST",1,"GMC",1,"1FK21056AF101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF10-1SA0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",2336,"ST",1,"GMC",1,"1FK21056AF101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF10-1SB0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2336,"ST",1,"GMC",1,"1FK21056AF101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF11-0MA0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2846,"ST",1,"GMC",1,"1FK21056AF110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF11-0MB0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2846,"ST",1,"GMC",1,"1FK21056AF110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF11-0SA0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",2447,"ST",1,"GMC",1,"1FK21056AF110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF11-0SB0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2447,"ST",1,"GMC",1,"1FK21056AF110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF11-1MA0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2846,"ST",1,"GMC",1,"1FK21056AF111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF11-1MB0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2846,"ST",1,"GMC",1,"1FK21056AF111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF11-1SA0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",2447,"ST",1,"GMC",1,"1FK21056AF111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF11-1SB0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2447,"ST",1,"GMC",1,"1FK21056AF111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF00-0MA0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2436,"ST",1,"GMC",1,"1FK21063AF000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF00-0MB0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2436,"ST",1,"GMC",1,"1FK21063AF000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF00-0SA0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2037,"ST",1,"GMC",1,"1FK21063AF000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF00-0SB0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2037,"ST",1,"GMC",1,"1FK21063AF000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF00-1MA0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2436,"ST",1,"GMC",1,"1FK21063AF001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF00-1MB0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2436,"ST",1,"GMC",1,"1FK21063AF001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF00-1SA0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2037,"ST",1,"GMC",1,"1FK21063AF001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF00-1SB0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2037,"ST",1,"GMC",1,"1FK21063AF001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF01-0MA0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2547,"ST",1,"GMC",1,"1FK21063AF010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF01-0MB0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2547,"ST",1,"GMC",1,"1FK21063AF010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF01-0SA0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2148,"ST",1,"GMC",1,"1FK21063AF010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF01-0SB0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2148,"ST",1,"GMC",1,"1FK21063AF010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF01-1MA0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2547,"ST",1,"GMC",1,"1FK21063AF011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF01-1MB0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2547,"ST",1,"GMC",1,"1FK21063AF011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF01-1SA0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2148,"ST",1,"GMC",1,"1FK21063AF011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF01-1SB0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2148,"ST",1,"GMC",1,"1FK21063AF011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF10-0MA0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2862,"ST",1,"GMC",1,"1FK21063AF100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF10-0MB0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2862,"ST",1,"GMC",1,"1FK21063AF100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF10-0SA0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2463,"ST",1,"GMC",1,"1FK21063AF100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF10-0SB0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2463,"ST",1,"GMC",1,"1FK21063AF100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF10-1MA0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2862,"ST",1,"GMC",1,"1FK21063AF101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF10-1MB0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2862,"ST",1,"GMC",1,"1FK21063AF101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF10-1SA0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2463,"ST",1,"GMC",1,"1FK21063AF101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF10-1SB0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2463,"ST",1,"GMC",1,"1FK21063AF101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF11-0MA0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2974,"ST",1,"GMC",1,"1FK21063AF110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF11-0MB0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2974,"ST",1,"GMC",1,"1FK21063AF110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF11-0SA0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2575,"ST",1,"GMC",1,"1FK21063AF110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF11-0SB0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2575,"ST",1,"GMC",1,"1FK21063AF110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF11-1MA0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2974,"ST",1,"GMC",1,"1FK21063AF111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF11-1MB0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2974,"ST",1,"GMC",1,"1FK21063AF111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF11-1SA0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2575,"ST",1,"GMC",1,"1FK21063AF111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF11-1SB0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2575,"ST",1,"GMC",1,"1FK21063AF111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF00-0MA0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2619,"ST",1,"GMC",1,"1FK21064AF000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF00-0MB0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2619,"ST",1,"GMC",1,"1FK21064AF000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF00-0SA0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2220,"ST",1,"GMC",1,"1FK21064AF000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF00-0SB0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2220,"ST",1,"GMC",1,"1FK21064AF000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF00-1MA0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2619,"ST",1,"GMC",1,"1FK21064AF001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF00-1MB0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2619,"ST",1,"GMC",1,"1FK21064AF001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF00-1SA0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2220,"ST",1,"GMC",1,"1FK21064AF001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF00-1SB0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2220,"ST",1,"GMC",1,"1FK21064AF001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF01-0MA0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2731,"ST",1,"GMC",1,"1FK21064AF010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF01-0MB0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2731,"ST",1,"GMC",1,"1FK21064AF010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF01-0SA0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2332,"ST",1,"GMC",1,"1FK21064AF010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF01-0SB0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2332,"ST",1,"GMC",1,"1FK21064AF010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF01-1MA0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2731,"ST",1,"GMC",1,"1FK21064AF011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF01-1MB0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2731,"ST",1,"GMC",1,"1FK21064AF011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF01-1SA0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2332,"ST",1,"GMC",1,"1FK21064AF011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF01-1SB0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2332,"ST",1,"GMC",1,"1FK21064AF011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF10-0MA0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3046,"ST",1,"GMC",1,"1FK21064AF100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF10-0MB0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3046,"ST",1,"GMC",1,"1FK21064AF100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF10-0SA0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2647,"ST",1,"GMC",1,"1FK21064AF100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF10-0SB0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2647,"ST",1,"GMC",1,"1FK21064AF100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF10-1MA0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3046,"ST",1,"GMC",1,"1FK21064AF101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF10-1MB0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3046,"ST",1,"GMC",1,"1FK21064AF101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF10-1SA0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2647,"ST",1,"GMC",1,"1FK21064AF101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF10-1SB0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2647,"ST",1,"GMC",1,"1FK21064AF101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF11-0MA0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3157,"ST",1,"GMC",1,"1FK21064AF110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF11-0MB0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3157,"ST",1,"GMC",1,"1FK21064AF110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF11-0SA0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2758,"ST",1,"GMC",1,"1FK21064AF110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF11-0SB0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2758,"ST",1,"GMC",1,"1FK21064AF110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF11-1MA0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3157,"ST",1,"GMC",1,"1FK21064AF111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF11-1MB0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3157,"ST",1,"GMC",1,"1FK21064AF111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF11-1SA0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2758,"ST",1,"GMC",1,"1FK21064AF111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF11-1SB0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2758,"ST",1,"GMC",1,"1FK21064AF111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF00-0MA0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3012,"ST",1,"GMC",1,"1FK21066AF000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF00-0MB0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3012,"ST",1,"GMC",1,"1FK21066AF000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF00-0SA0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2613,"ST",1,"GMC",1,"1FK21066AF000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF00-0SB0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2613,"ST",1,"GMC",1,"1FK21066AF000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF00-1MA0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3012,"ST",1,"GMC",1,"1FK21066AF001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF00-1MB0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3012,"ST",1,"GMC",1,"1FK21066AF001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF00-1SA0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2613,"ST",1,"GMC",1,"1FK21066AF001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF00-1SB0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2613,"ST",1,"GMC",1,"1FK21066AF001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF01-0MA0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3123,"ST",1,"GMC",1,"1FK21066AF010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF01-0MB0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3123,"ST",1,"GMC",1,"1FK21066AF010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF01-0SA0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2724,"ST",1,"GMC",1,"1FK21066AF010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF01-0SB0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2724,"ST",1,"GMC",1,"1FK21066AF010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF01-1MA0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3123,"ST",1,"GMC",1,"1FK21066AF011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF01-1MB0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3123,"ST",1,"GMC",1,"1FK21066AF011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF01-1SA0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2724,"ST",1,"GMC",1,"1FK21066AF011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF01-1SB0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2724,"ST",1,"GMC",1,"1FK21066AF011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF10-0MA0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3438,"ST",1,"GMC",1,"1FK21066AF100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF10-0MB0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3438,"ST",1,"GMC",1,"1FK21066AF100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF10-0SA0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3039,"ST",1,"GMC",1,"1FK21066AF100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF10-0SB0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3039,"ST",1,"GMC",1,"1FK21066AF100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF10-1MA0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3438,"ST",1,"GMC",1,"1FK21066AF101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF10-1MB0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3438,"ST",1,"GMC",1,"1FK21066AF101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF10-1SA0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3039,"ST",1,"GMC",1,"1FK21066AF101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF10-1SB0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3039,"ST",1,"GMC",1,"1FK21066AF101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF11-0MA0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3550,"ST",1,"GMC",1,"1FK21066AF110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF11-0MB0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3550,"ST",1,"GMC",1,"1FK21066AF110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF11-0SA0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3151,"ST",1,"GMC",1,"1FK21066AF110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF11-0SB0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3151,"ST",1,"GMC",1,"1FK21066AF110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF11-1MA0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3550,"ST",1,"GMC",1,"1FK21066AF111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF11-1MB0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3550,"ST",1,"GMC",1,"1FK21066AF111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF11-1SA0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3151,"ST",1,"GMC",1,"1FK21066AF111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF11-1SB0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3151,"ST",1,"GMC",1,"1FK21066AF111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AG00-0MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1460,"ST",1,"GMC",1,"1FK22032AG000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AG00-0SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1061,"ST",1,"GMC",1,"1FK22032AG000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AG00-1MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1460,"ST",1,"GMC",1,"1FK22032AG001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AG00-1SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1061,"ST",1,"GMC",1,"1FK22032AG001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AG00-2MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1460,"ST",1,"GMC",1,"1FK22032AG002MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AG00-2SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1061,"ST",1,"GMC",1,"1FK22032AG002SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AG01-0MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1571,"ST",1,"GMC",1,"1FK22032AG010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AG01-0SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1172,"ST",1,"GMC",1,"1FK22032AG010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AG01-1MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1571,"ST",1,"GMC",1,"1FK22032AG011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AG01-1SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1172,"ST",1,"GMC",1,"1FK22032AG011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AG01-2MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M12, rotatable; .",1571,"ST",1,"GMC",1,"1FK22032AG012MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AG01-2SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M12, rotatable; .",1172,"ST",1,"GMC",1,"1FK22032AG012SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AG10-0MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1780,"ST",1,"GMC",1,"1FK22032AG100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AG10-0SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1381,"ST",1,"GMC",1,"1FK22032AG100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AG10-1MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1780,"ST",1,"GMC",1,"1FK22032AG101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AG10-1SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1381,"ST",1,"GMC",1,"1FK22032AG101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AG10-2MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1780,"ST",1,"GMC",1,"1FK22032AG102MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AG10-2SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1381,"ST",1,"GMC",1,"1FK22032AG102SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AG11-0MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1891,"ST",1,"GMC",1,"1FK22032AG110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AG11-0SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1492,"ST",1,"GMC",1,"1FK22032AG110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AG11-1MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1891,"ST",1,"GMC",1,"1FK22032AG111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AG11-1SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1492,"ST",1,"GMC",1,"1FK22032AG111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AG11-2MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M12, rotatable; .",1891,"ST",1,"GMC",1,"1FK22032AG112MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AG11-2SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M12, rotatable; .",1492,"ST",1,"GMC",1,"1FK22032AG112SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK00-0MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1460,"ST",1,"GMC",1,"1FK22032AK000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK00-0MB0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1460,"ST",1,"GMC",1,"1FK22032AK000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK00-0SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1061,"ST",1,"GMC",1,"1FK22032AK000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK00-0SB0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1061,"ST",1,"GMC",1,"1FK22032AK000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK00-1MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1460,"ST",1,"GMC",1,"1FK22032AK001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK00-1MB0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1460,"ST",1,"GMC",1,"1FK22032AK001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK00-1SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1061,"ST",1,"GMC",1,"1FK22032AK001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK00-1SB0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1061,"ST",1,"GMC",1,"1FK22032AK001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK00-2MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1460,"ST",1,"GMC",1,"1FK22032AK002MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK00-2MB0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1460,"ST",1,"GMC",1,"1FK22032AK002MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK00-2SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1061,"ST",1,"GMC",1,"1FK22032AK002SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK00-2SB0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1061,"ST",1,"GMC",1,"1FK22032AK002SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK01-0MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1571,"ST",1,"GMC",1,"1FK22032AK010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK01-0MB0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1571,"ST",1,"GMC",1,"1FK22032AK010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK01-0SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1172,"ST",1,"GMC",1,"1FK22032AK010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK01-0SB0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1172,"ST",1,"GMC",1,"1FK22032AK010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK01-1MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1571,"ST",1,"GMC",1,"1FK22032AK011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK01-1MB0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1571,"ST",1,"GMC",1,"1FK22032AK011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK01-1SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1172,"ST",1,"GMC",1,"1FK22032AK011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK01-1SB0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1172,"ST",1,"GMC",1,"1FK22032AK011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK01-2MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable; .",1571,"ST",1,"GMC",1,"1FK22032AK012MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK01-2MB0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17; .",1571,"ST",1,"GMC",1,"1FK22032AK012MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK01-2SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable; .",1172,"ST",1,"GMC",1,"1FK22032AK012SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK01-2SB0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17; .",1172,"ST",1,"GMC",1,"1FK22032AK012SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK10-0MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1780,"ST",1,"GMC",1,"1FK22032AK100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK10-0MB0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1780,"ST",1,"GMC",1,"1FK22032AK100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK10-0SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1381,"ST",1,"GMC",1,"1FK22032AK100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK10-0SB0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1381,"ST",1,"GMC",1,"1FK22032AK100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK10-1MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1780,"ST",1,"GMC",1,"1FK22032AK101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK10-1MB0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1780,"ST",1,"GMC",1,"1FK22032AK101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK10-1SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1381,"ST",1,"GMC",1,"1FK22032AK101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK10-1SB0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1381,"ST",1,"GMC",1,"1FK22032AK101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK10-2MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1780,"ST",1,"GMC",1,"1FK22032AK102MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK10-2MB0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1780,"ST",1,"GMC",1,"1FK22032AK102MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK10-2SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1381,"ST",1,"GMC",1,"1FK22032AK102SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK10-2SB0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1381,"ST",1,"GMC",1,"1FK22032AK102SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK11-0MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1891,"ST",1,"GMC",1,"1FK22032AK110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK11-0MB0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1891,"ST",1,"GMC",1,"1FK22032AK110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK11-0SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1492,"ST",1,"GMC",1,"1FK22032AK110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK11-0SB0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1492,"ST",1,"GMC",1,"1FK22032AK110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK11-1MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1891,"ST",1,"GMC",1,"1FK22032AK111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK11-1MB0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1891,"ST",1,"GMC",1,"1FK22032AK111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK11-1SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1492,"ST",1,"GMC",1,"1FK22032AK111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK11-1SB0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1492,"ST",1,"GMC",1,"1FK22032AK111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK11-2MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable; .",1891,"ST",1,"GMC",1,"1FK22032AK112MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK11-2MB0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1891,"ST",1,"GMC",1,"1FK22032AK112MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK11-2SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable; .",1492,"ST",1,"GMC",1,"1FK22032AK112SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK11-2SB0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1492,"ST",1,"GMC",1,"1FK22032AK112SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AG00-0MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1619,"ST",1,"GMC",1,"1FK22034AG000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AG00-0SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1220,"ST",1,"GMC",1,"1FK22034AG000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AG00-1MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1619,"ST",1,"GMC",1,"1FK22034AG001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AG00-1SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1220,"ST",1,"GMC",1,"1FK22034AG001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AG00-2MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1619,"ST",1,"GMC",1,"1FK22034AG002MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AG00-2SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1220,"ST",1,"GMC",1,"1FK22034AG002SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AG01-0MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1730,"ST",1,"GMC",1,"1FK22034AG010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AG01-0SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1332,"ST",1,"GMC",1,"1FK22034AG010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AG01-1MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1730,"ST",1,"GMC",1,"1FK22034AG011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AG01-1SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1332,"ST",1,"GMC",1,"1FK22034AG011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AG01-2MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M12, rotatable; .",1730,"ST",1,"GMC",1,"1FK22034AG012MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AG01-2SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M12, rotatable; .",1332,"ST",1,"GMC",1,"1FK22034AG012SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AG10-0MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1939,"ST",1,"GMC",1,"1FK22034AG100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AG10-0SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1540,"ST",1,"GMC",1,"1FK22034AG100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AG10-1MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1939,"ST",1,"GMC",1,"1FK22034AG101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AG10-1SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1540,"ST",1,"GMC",1,"1FK22034AG101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AG10-2MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1939,"ST",1,"GMC",1,"1FK22034AG102MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AG10-2SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1540,"ST",1,"GMC",1,"1FK22034AG102SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AG11-0MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",2050,"ST",1,"GMC",1,"1FK22034AG110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AG11-0SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1651,"ST",1,"GMC",1,"1FK22034AG110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AG11-1MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",2050,"ST",1,"GMC",1,"1FK22034AG111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AG11-1SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1651,"ST",1,"GMC",1,"1FK22034AG111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AG11-2MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M12, rotatable; .",2050,"ST",1,"GMC",1,"1FK22034AG112MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AG11-2SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M12, rotatable; .",1651,"ST",1,"GMC",1,"1FK22034AG112SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK00-0MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1619,"ST",1,"GMC",1,"1FK22034AK000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK00-0MB0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1619,"ST",1,"GMC",1,"1FK22034AK000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK00-0SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1220,"ST",1,"GMC",1,"1FK22034AK000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK00-0SB0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1220,"ST",1,"GMC",1,"1FK22034AK000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK00-1MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1619,"ST",1,"GMC",1,"1FK22034AK001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK00-1MB0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1619,"ST",1,"GMC",1,"1FK22034AK001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK00-1SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1220,"ST",1,"GMC",1,"1FK22034AK001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK00-1SB0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1220,"ST",1,"GMC",1,"1FK22034AK001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK00-2MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1619,"ST",1,"GMC",1,"1FK22034AK002MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK00-2MB0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1619,"ST",1,"GMC",1,"1FK22034AK002MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK00-2SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1220,"ST",1,"GMC",1,"1FK22034AK002SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK00-2SB0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1220,"ST",1,"GMC",1,"1FK22034AK002SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK01-0MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1730,"ST",1,"GMC",1,"1FK22034AK010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK01-0MB0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1730,"ST",1,"GMC",1,"1FK22034AK010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK01-0SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1332,"ST",1,"GMC",1,"1FK22034AK010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK01-0SB0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1332,"ST",1,"GMC",1,"1FK22034AK010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK01-1MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1730,"ST",1,"GMC",1,"1FK22034AK011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK01-1MB0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1730,"ST",1,"GMC",1,"1FK22034AK011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK01-1SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1332,"ST",1,"GMC",1,"1FK22034AK011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK01-1SB0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1332,"ST",1,"GMC",1,"1FK22034AK011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK01-2MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable; .",1730,"ST",1,"GMC",1,"1FK22034AK012MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK01-2MB0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17; .",1730,"ST",1,"GMC",1,"1FK22034AK012MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK01-2SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable; .",1332,"ST",1,"GMC",1,"1FK22034AK012SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK01-2SB0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17; .",1332,"ST",1,"GMC",1,"1FK22034AK012SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK10-0MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1939,"ST",1,"GMC",1,"1FK22034AK100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK10-0MB0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1939,"ST",1,"GMC",1,"1FK22034AK100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK10-0SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1540,"ST",1,"GMC",1,"1FK22034AK100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK10-0SB0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1540,"ST",1,"GMC",1,"1FK22034AK100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK10-1MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1939,"ST",1,"GMC",1,"1FK22034AK101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK10-1MB0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1939,"ST",1,"GMC",1,"1FK22034AK101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK10-1SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1540,"ST",1,"GMC",1,"1FK22034AK101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK10-1SB0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1540,"ST",1,"GMC",1,"1FK22034AK101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK10-2MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1939,"ST",1,"GMC",1,"1FK22034AK102MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK10-2MB0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1939,"ST",1,"GMC",1,"1FK22034AK102MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK10-2SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1540,"ST",1,"GMC",1,"1FK22034AK102SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK10-2SB0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1540,"ST",1,"GMC",1,"1FK22034AK102SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK11-0MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2050,"ST",1,"GMC",1,"1FK22034AK110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK11-0MB0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2050,"ST",1,"GMC",1,"1FK22034AK110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK11-0SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1651,"ST",1,"GMC",1,"1FK22034AK110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK11-0SB0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1651,"ST",1,"GMC",1,"1FK22034AK110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK11-1MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2050,"ST",1,"GMC",1,"1FK22034AK111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK11-1MB0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2050,"ST",1,"GMC",1,"1FK22034AK111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK11-1SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1651,"ST",1,"GMC",1,"1FK22034AK111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK11-1SB0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1651,"ST",1,"GMC",1,"1FK22034AK111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK11-2MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable; .",2050,"ST",1,"GMC",1,"1FK22034AK112MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK11-2MB0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",2050,"ST",1,"GMC",1,"1FK22034AK112MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK11-2SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable; .",1651,"ST",1,"GMC",1,"1FK22034AK112SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK11-2SB0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1651,"ST",1,"GMC",1,"1FK22034AK112SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF00-0MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1752,"ST",1,"GMC",1,"1FK22045AF000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF00-0MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1752,"ST",1,"GMC",1,"1FK22045AF000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF00-0SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1353,"ST",1,"GMC",1,"1FK22045AF000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF00-0SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1353,"ST",1,"GMC",1,"1FK22045AF000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF00-1MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1752,"ST",1,"GMC",1,"1FK22045AF001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF00-1MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1752,"ST",1,"GMC",1,"1FK22045AF001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF00-1SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1353,"ST",1,"GMC",1,"1FK22045AF001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF00-1SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1353,"ST",1,"GMC",1,"1FK22045AF001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF00-2MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1752,"ST",1,"GMC",1,"1FK22045AF002MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF00-2MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1752,"ST",1,"GMC",1,"1FK22045AF002MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF00-2SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1353,"ST",1,"GMC",1,"1FK22045AF002SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF00-2SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1353,"ST",1,"GMC",1,"1FK22045AF002SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF01-0MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1863,"ST",1,"GMC",1,"1FK22045AF010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF01-0MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1863,"ST",1,"GMC",1,"1FK22045AF010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF01-0SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1464,"ST",1,"GMC",1,"1FK22045AF010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF01-0SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1464,"ST",1,"GMC",1,"1FK22045AF010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF01-1MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1863,"ST",1,"GMC",1,"1FK22045AF011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF01-1MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1863,"ST",1,"GMC",1,"1FK22045AF011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF01-1SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1464,"ST",1,"GMC",1,"1FK22045AF011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF01-1SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1464,"ST",1,"GMC",1,"1FK22045AF011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF01-2MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480V); PN = 0.375 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M17, rotatable; .",1863,"ST",1,"GMC",1,"1FK22045AF012MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF01-2MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480V); PN = 0.375 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1863,"ST",1,"GMC",1,"1FK22045AF012MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF01-2SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480V); PN = 0.375 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M17, rotatable; .",1464,"ST",1,"GMC",1,"1FK22045AF012SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF01-2SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480V); PN = 0.375 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1464,"ST",1,"GMC",1,"1FK22045AF012SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF10-0MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2071,"ST",1,"GMC",1,"1FK22045AF100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF10-0MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2071,"ST",1,"GMC",1,"1FK22045AF100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF10-0SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1672,"ST",1,"GMC",1,"1FK22045AF100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF10-0SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1672,"ST",1,"GMC",1,"1FK22045AF100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF10-1MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2071,"ST",1,"GMC",1,"1FK22045AF101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF10-1MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2071,"ST",1,"GMC",1,"1FK22045AF101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF10-1SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1672,"ST",1,"GMC",1,"1FK22045AF101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF10-1SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1672,"ST",1,"GMC",1,"1FK22045AF101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF10-2MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2071,"ST",1,"GMC",1,"1FK22045AF102MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF10-2MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2071,"ST",1,"GMC",1,"1FK22045AF102MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF10-2SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1672,"ST",1,"GMC",1,"1FK22045AF102SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF10-2SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1672,"ST",1,"GMC",1,"1FK22045AF102SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF11-0MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2183,"ST",1,"GMC",1,"1FK22045AF110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF11-0MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2183,"ST",1,"GMC",1,"1FK22045AF110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF11-0SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1784,"ST",1,"GMC",1,"1FK22045AF110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF11-0SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1784,"ST",1,"GMC",1,"1FK22045AF110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF11-1MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2183,"ST",1,"GMC",1,"1FK22045AF111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF11-1MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2183,"ST",1,"GMC",1,"1FK22045AF111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF11-1SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1784,"ST",1,"GMC",1,"1FK22045AF111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF11-1SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1784,"ST",1,"GMC",1,"1FK22045AF111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF11-2MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480V); PN = 0.375 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M17, rotatable; .",2183,"ST",1,"GMC",1,"1FK22045AF112MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF11-2MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480V); PN = 0.375 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",2183,"ST",1,"GMC",1,"1FK22045AF112MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF11-2SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480V); PN = 0.375 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M17, rotatable; .",1784,"ST",1,"GMC",1,"1FK22045AF112SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF11-2SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480V); PN = 0.375 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1784,"ST",1,"GMC",1,"1FK22045AF112SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK00-0MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1752,"ST",1,"GMC",1,"1FK22045AK000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK00-0MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Âµs;",1752,"ST",1,"GMC",1,"1FK22045AK000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK00-0SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1353,"ST",1,"GMC",1,"1FK22045AK000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK00-0SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Âµs;",1353,"ST",1,"GMC",1,"1FK22045AK000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK00-1MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1752,"ST",1,"GMC",1,"1FK22045AK001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK00-1MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Âµs;",1752,"ST",1,"GMC",1,"1FK22045AK001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK00-1SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1353,"ST",1,"GMC",1,"1FK22045AK001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK00-1SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Âµs;",1353,"ST",1,"GMC",1,"1FK22045AK001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK00-2MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1752,"ST",1,"GMC",1,"1FK22045AK002MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK00-2MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Âµs;",1752,"ST",1,"GMC",1,"1FK22045AK002MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK00-2SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1353,"ST",1,"GMC",1,"1FK22045AK002SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK00-2SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Âµs;",1353,"ST",1,"GMC",1,"1FK22045AK002SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK01-0MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1863,"ST",1,"GMC",1,"1FK22045AK010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK01-0MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Âµs;",1863,"ST",1,"GMC",1,"1FK22045AK010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK01-0SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1464,"ST",1,"GMC",1,"1FK22045AK010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK01-0SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Âµs;",1464,"ST",1,"GMC",1,"1FK22045AK010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK01-1MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1863,"ST",1,"GMC",1,"1FK22045AK011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK01-1MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Âµs;",1863,"ST",1,"GMC",1,"1FK22045AK011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK01-1SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1464,"ST",1,"GMC",1,"1FK22045AK011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK01-1SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Âµs;",1464,"ST",1,"GMC",1,"1FK22045AK011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK01-2MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480V); PN = 0.75 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M17, rotatable; .",1863,"ST",1,"GMC",1,"1FK22045AK012MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK01-2MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480V); PN = 0.75 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Âµs; .",1863,"ST",1,"GMC",1,"1FK22045AK012MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK01-2SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480V); PN = 0.75 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M17, rotatable; .",1464,"ST",1,"GMC",1,"1FK22045AK012SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK01-2SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480V); PN = 0.75 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Âµs; .",1464,"ST",1,"GMC",1,"1FK22045AK012SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK10-0MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2071,"ST",1,"GMC",1,"1FK22045AK100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK10-0MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Âµs;",2071,"ST",1,"GMC",1,"1FK22045AK100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK10-0SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1672,"ST",1,"GMC",1,"1FK22045AK100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK10-0SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Âµs;",1672,"ST",1,"GMC",1,"1FK22045AK100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK10-1MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2071,"ST",1,"GMC",1,"1FK22045AK101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK10-1MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Âµs;",2071,"ST",1,"GMC",1,"1FK22045AK101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK10-1SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1672,"ST",1,"GMC",1,"1FK22045AK101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK10-1SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Âµs;",1672,"ST",1,"GMC",1,"1FK22045AK101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK10-2MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2071,"ST",1,"GMC",1,"1FK22045AK102MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK10-2MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Âµs;",2071,"ST",1,"GMC",1,"1FK22045AK102MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK10-2SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1672,"ST",1,"GMC",1,"1FK22045AK102SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK10-2SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Âµs;",1672,"ST",1,"GMC",1,"1FK22045AK102SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK11-0MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2183,"ST",1,"GMC",1,"1FK22045AK110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK11-0MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Âµs;",2183,"ST",1,"GMC",1,"1FK22045AK110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK11-0SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1784,"ST",1,"GMC",1,"1FK22045AK110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK11-0SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Âµs;",1784,"ST",1,"GMC",1,"1FK22045AK110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK11-1MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2183,"ST",1,"GMC",1,"1FK22045AK111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK11-1MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Âµs;",2183,"ST",1,"GMC",1,"1FK22045AK111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK11-1SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1784,"ST",1,"GMC",1,"1FK22045AK111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK11-1SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Âµs;",1784,"ST",1,"GMC",1,"1FK22045AK111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK11-2MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480V); PN = 0.75 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M17, rotatable; .",2183,"ST",1,"GMC",1,"1FK22045AK112MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK11-2MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480V); PN = 0.75 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Âµs; .",2183,"ST",1,"GMC",1,"1FK22045AK112MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK11-2SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480V); PN = 0.75 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M17, rotatable; .",1784,"ST",1,"GMC",1,"1FK22045AK112SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK11-2SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480V); PN = 0.75 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Âµs; .",1784,"ST",1,"GMC",1,"1FK22045AK112SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF00-0MA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1831,"ST",1,"GMC",1,"1FK22046AF000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF00-0MB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1831,"ST",1,"GMC",1,"1FK22046AF000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF00-0SA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1432,"ST",1,"GMC",1,"1FK22046AF000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF00-0SB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1432,"ST",1,"GMC",1,"1FK22046AF000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF00-1MA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1831,"ST",1,"GMC",1,"1FK22046AF001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF00-1MB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1831,"ST",1,"GMC",1,"1FK22046AF001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF00-1SA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1432,"ST",1,"GMC",1,"1FK22046AF001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF00-1SB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1432,"ST",1,"GMC",1,"1FK22046AF001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF00-2MA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1831,"ST",1,"GMC",1,"1FK22046AF002MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF00-2MB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1831,"ST",1,"GMC",1,"1FK22046AF002MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF00-2SA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1432,"ST",1,"GMC",1,"1FK22046AF002SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF00-2SB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1432,"ST",1,"GMC",1,"1FK22046AF002SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF01-0MA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1943,"ST",1,"GMC",1,"1FK22046AF010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF01-0MB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1943,"ST",1,"GMC",1,"1FK22046AF010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF01-0SA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1544,"ST",1,"GMC",1,"1FK22046AF010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF01-0SB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1544,"ST",1,"GMC",1,"1FK22046AF010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF01-1MA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1943,"ST",1,"GMC",1,"1FK22046AF011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF01-1MB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1943,"ST",1,"GMC",1,"1FK22046AF011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF01-1SA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1544,"ST",1,"GMC",1,"1FK22046AF011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF01-1SB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1544,"ST",1,"GMC",1,"1FK22046AF011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF01-2MA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480V); PN = 0.5 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M17, rotatable; .",1943,"ST",1,"GMC",1,"1FK22046AF012MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF01-2MB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480V); PN = 0.5 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1943,"ST",1,"GMC",1,"1FK22046AF012MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF01-2SA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480V); PN = 0.5 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M17, rotatable; .",1544,"ST",1,"GMC",1,"1FK22046AF012SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF01-2SB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480V); PN = 0.5 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1544,"ST",1,"GMC",1,"1FK22046AF012SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF10-0MA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2151,"ST",1,"GMC",1,"1FK22046AF100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF10-0MB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2151,"ST",1,"GMC",1,"1FK22046AF100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF10-0SA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1752,"ST",1,"GMC",1,"1FK22046AF100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF10-0SB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1752,"ST",1,"GMC",1,"1FK22046AF100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF10-1MA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2151,"ST",1,"GMC",1,"1FK22046AF101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF10-1MB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2151,"ST",1,"GMC",1,"1FK22046AF101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF10-1SA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1752,"ST",1,"GMC",1,"1FK22046AF101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF10-1SB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1752,"ST",1,"GMC",1,"1FK22046AF101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF10-2MA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2151,"ST",1,"GMC",1,"1FK22046AF102MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF10-2MB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2151,"ST",1,"GMC",1,"1FK22046AF102MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF10-2SA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1752,"ST",1,"GMC",1,"1FK22046AF102SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF10-2SB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1752,"ST",1,"GMC",1,"1FK22046AF102SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF11-0MA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2262,"ST",1,"GMC",1,"1FK22046AF110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF11-0MB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2262,"ST",1,"GMC",1,"1FK22046AF110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF11-0SA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1863,"ST",1,"GMC",1,"1FK22046AF110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF11-0SB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1863,"ST",1,"GMC",1,"1FK22046AF110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF11-1MA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2262,"ST",1,"GMC",1,"1FK22046AF111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF11-1MB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2262,"ST",1,"GMC",1,"1FK22046AF111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF11-1SA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1863,"ST",1,"GMC",1,"1FK22046AF111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF11-1SB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1863,"ST",1,"GMC",1,"1FK22046AF111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF11-2MA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480V); PN = 0.5 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M17, rotatable; .",2262,"ST",1,"GMC",1,"1FK22046AF112MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF11-2MB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480V); PN = 0.5 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",2262,"ST",1,"GMC",1,"1FK22046AF112MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF11-2SA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480V); PN = 0.5 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M17, rotatable; .",1863,"ST",1,"GMC",1,"1FK22046AF112SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF11-2SB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480V); PN = 0.5 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1863,"ST",1,"GMC",1,"1FK22046AF112SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF00-0MA0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1860,"ST",1,"GMC",1,"1FK22052AF000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF00-0MB0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1860,"ST",1,"GMC",1,"1FK22052AF000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF00-0SA0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1461,"ST",1,"GMC",1,"1FK22052AF000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF00-0SB0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1461,"ST",1,"GMC",1,"1FK22052AF000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF00-1MA0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1860,"ST",1,"GMC",1,"1FK22052AF001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF00-1MB0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1860,"ST",1,"GMC",1,"1FK22052AF001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF00-1SA0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1461,"ST",1,"GMC",1,"1FK22052AF001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF00-1SB0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1461,"ST",1,"GMC",1,"1FK22052AF001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF01-0MA0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1971,"ST",1,"GMC",1,"1FK22052AF010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF01-0MB0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1971,"ST",1,"GMC",1,"1FK22052AF010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF01-0SA0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1572,"ST",1,"GMC",1,"1FK22052AF010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF01-0SB0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1572,"ST",1,"GMC",1,"1FK22052AF010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF01-1MA0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1971,"ST",1,"GMC",1,"1FK22052AF011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF01-1MB0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1971,"ST",1,"GMC",1,"1FK22052AF011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF01-1SA0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1572,"ST",1,"GMC",1,"1FK22052AF011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF01-1SB0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1572,"ST",1,"GMC",1,"1FK22052AF011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF10-0MA0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2233,"ST",1,"GMC",1,"1FK22052AF100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF10-0MB0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2233,"ST",1,"GMC",1,"1FK22052AF100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF10-0SA0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1834,"ST",1,"GMC",1,"1FK22052AF100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF10-0SB0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1834,"ST",1,"GMC",1,"1FK22052AF100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF10-1MA0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2233,"ST",1,"GMC",1,"1FK22052AF101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF10-1MB0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2233,"ST",1,"GMC",1,"1FK22052AF101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF10-1SA0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1834,"ST",1,"GMC",1,"1FK22052AF101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF10-1SB0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1834,"ST",1,"GMC",1,"1FK22052AF101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF11-0MA0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2344,"ST",1,"GMC",1,"1FK22052AF110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF11-0MB0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2344,"ST",1,"GMC",1,"1FK22052AF110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF11-0SA0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1945,"ST",1,"GMC",1,"1FK22052AF110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF11-0SB0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1945,"ST",1,"GMC",1,"1FK22052AF110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF11-1MA0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2344,"ST",1,"GMC",1,"1FK22052AF111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF11-1MB0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2344,"ST",1,"GMC",1,"1FK22052AF111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF11-1SA0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1945,"ST",1,"GMC",1,"1FK22052AF111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF11-1SB0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1945,"ST",1,"GMC",1,"1FK22052AF111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF00-0MA0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2123,"ST",1,"GMC",1,"1FK22054AF000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF00-0MB0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2123,"ST",1,"GMC",1,"1FK22054AF000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF00-0SA0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1724,"ST",1,"GMC",1,"1FK22054AF000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF00-0SB0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1724,"ST",1,"GMC",1,"1FK22054AF000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF00-1MA0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2123,"ST",1,"GMC",1,"1FK22054AF001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF00-1MB0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2123,"ST",1,"GMC",1,"1FK22054AF001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF00-1SA0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1724,"ST",1,"GMC",1,"1FK22054AF001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF00-1SB0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1724,"ST",1,"GMC",1,"1FK22054AF001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF01-0MA0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2234,"ST",1,"GMC",1,"1FK22054AF010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF01-0MB0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2234,"ST",1,"GMC",1,"1FK22054AF010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF01-0SA0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1835,"ST",1,"GMC",1,"1FK22054AF010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF01-0SB0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1835,"ST",1,"GMC",1,"1FK22054AF010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF01-1MA0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2234,"ST",1,"GMC",1,"1FK22054AF011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF01-1MB0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2234,"ST",1,"GMC",1,"1FK22054AF011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF01-1SA0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1835,"ST",1,"GMC",1,"1FK22054AF011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF01-1SB0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1835,"ST",1,"GMC",1,"1FK22054AF011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF10-0MA0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2496,"ST",1,"GMC",1,"1FK22054AF100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF10-0MB0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2496,"ST",1,"GMC",1,"1FK22054AF100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF10-0SA0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",2097,"ST",1,"GMC",1,"1FK22054AF100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF10-0SB0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2097,"ST",1,"GMC",1,"1FK22054AF100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF10-1MA0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2496,"ST",1,"GMC",1,"1FK22054AF101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF10-1MB0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2496,"ST",1,"GMC",1,"1FK22054AF101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF10-1SA0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",2097,"ST",1,"GMC",1,"1FK22054AF101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF10-1SB0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2097,"ST",1,"GMC",1,"1FK22054AF101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF11-0MA0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2607,"ST",1,"GMC",1,"1FK22054AF110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF11-0MB0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2607,"ST",1,"GMC",1,"1FK22054AF110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF11-0SA0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",2208,"ST",1,"GMC",1,"1FK22054AF110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF11-0SB0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2208,"ST",1,"GMC",1,"1FK22054AF110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF11-1MA0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2607,"ST",1,"GMC",1,"1FK22054AF111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF11-1MB0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2607,"ST",1,"GMC",1,"1FK22054AF111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF11-1SA0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",2208,"ST",1,"GMC",1,"1FK22054AF111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF11-1SB0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2208,"ST",1,"GMC",1,"1FK22054AF111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF00-0MA0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2171,"ST",1,"GMC",1,"1FK22062AF000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF00-0MB0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2171,"ST",1,"GMC",1,"1FK22062AF000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF00-0SA0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",1772,"ST",1,"GMC",1,"1FK22062AF000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF00-0SB0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",1772,"ST",1,"GMC",1,"1FK22062AF000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF00-1MA0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2171,"ST",1,"GMC",1,"1FK22062AF001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF00-1MB0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2171,"ST",1,"GMC",1,"1FK22062AF001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF00-1SA0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",1772,"ST",1,"GMC",1,"1FK22062AF001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF00-1SB0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",1772,"ST",1,"GMC",1,"1FK22062AF001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF01-0MA0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2283,"ST",1,"GMC",1,"1FK22062AF010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF01-0MB0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2283,"ST",1,"GMC",1,"1FK22062AF010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF01-0SA0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",1884,"ST",1,"GMC",1,"1FK22062AF010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF01-0SB0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",1884,"ST",1,"GMC",1,"1FK22062AF010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF01-1MA0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2283,"ST",1,"GMC",1,"1FK22062AF011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF01-1MB0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2283,"ST",1,"GMC",1,"1FK22062AF011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF01-1SA0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",1884,"ST",1,"GMC",1,"1FK22062AF011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF01-1SB0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",1884,"ST",1,"GMC",1,"1FK22062AF011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF10-0MA0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2598,"ST",1,"GMC",1,"1FK22062AF100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF10-0MB0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2598,"ST",1,"GMC",1,"1FK22062AF100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF10-0SA0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2199,"ST",1,"GMC",1,"1FK22062AF100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF10-0SB0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2199,"ST",1,"GMC",1,"1FK22062AF100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF10-1MA0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2598,"ST",1,"GMC",1,"1FK22062AF101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF10-1MB0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2598,"ST",1,"GMC",1,"1FK22062AF101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF10-1SA0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2199,"ST",1,"GMC",1,"1FK22062AF101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF10-1SB0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2199,"ST",1,"GMC",1,"1FK22062AF101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF11-0MA0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2709,"ST",1,"GMC",1,"1FK22062AF110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF11-0MB0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2709,"ST",1,"GMC",1,"1FK22062AF110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF11-0SA0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2310,"ST",1,"GMC",1,"1FK22062AF110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF11-0SB0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2310,"ST",1,"GMC",1,"1FK22062AF110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF11-1MA0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2709,"ST",1,"GMC",1,"1FK22062AF111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF11-1MB0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2709,"ST",1,"GMC",1,"1FK22062AF111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF11-1SA0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2310,"ST",1,"GMC",1,"1FK22062AF111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF11-1SB0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2310,"ST",1,"GMC",1,"1FK22062AF111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF00-0MA0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2706,"ST",1,"GMC",1,"1FK22064AF000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF00-0MB0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2706,"ST",1,"GMC",1,"1FK22064AF000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF00-0SA0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2307,"ST",1,"GMC",1,"1FK22064AF000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF00-0SB0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2307,"ST",1,"GMC",1,"1FK22064AF000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF00-1MA0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2706,"ST",1,"GMC",1,"1FK22064AF001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF00-1MB0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2706,"ST",1,"GMC",1,"1FK22064AF001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF00-1SA0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2307,"ST",1,"GMC",1,"1FK22064AF001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF00-1SB0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2307,"ST",1,"GMC",1,"1FK22064AF001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF01-0MA0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2818,"ST",1,"GMC",1,"1FK22064AF010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF01-0MB0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2818,"ST",1,"GMC",1,"1FK22064AF010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF01-0SA0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2419,"ST",1,"GMC",1,"1FK22064AF010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF01-0SB0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2419,"ST",1,"GMC",1,"1FK22064AF010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF01-1MA0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2818,"ST",1,"GMC",1,"1FK22064AF011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF01-1MB0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2818,"ST",1,"GMC",1,"1FK22064AF011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF01-1SA0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2419,"ST",1,"GMC",1,"1FK22064AF011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF01-1SB0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2419,"ST",1,"GMC",1,"1FK22064AF011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF10-0MA0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3133,"ST",1,"GMC",1,"1FK22064AF100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF10-0MB0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3133,"ST",1,"GMC",1,"1FK22064AF100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF10-0SA0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2734,"ST",1,"GMC",1,"1FK22064AF100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF10-0SB0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2734,"ST",1,"GMC",1,"1FK22064AF100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF10-1MA0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3133,"ST",1,"GMC",1,"1FK22064AF101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF10-1MB0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3133,"ST",1,"GMC",1,"1FK22064AF101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF10-1SA0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2734,"ST",1,"GMC",1,"1FK22064AF101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF10-1SB0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2734,"ST",1,"GMC",1,"1FK22064AF101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF11-0MA0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3244,"ST",1,"GMC",1,"1FK22064AF110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF11-0MB0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3244,"ST",1,"GMC",1,"1FK22064AF110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF11-0SA0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2845,"ST",1,"GMC",1,"1FK22064AF110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF11-0SB0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2845,"ST",1,"GMC",1,"1FK22064AF110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF11-1MA0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3244,"ST",1,"GMC",1,"1FK22064AF111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF11-1MB0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3244,"ST",1,"GMC",1,"1FK22064AF111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF11-1SA0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2845,"ST",1,"GMC",1,"1FK22064AF111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF11-1SB0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2845,"ST",1,"GMC",1,"1FK22064AF111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC00-0MA0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3172,"ST",1,"GMC",1,"1FK22083AC000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC00-0MB0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3172,"ST",1,"GMC",1,"1FK22083AC000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC00-0SA0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2773,"ST",1,"GMC",1,"1FK22083AC000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC00-0SB0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2773,"ST",1,"GMC",1,"1FK22083AC000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC00-1MA0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3172,"ST",1,"GMC",1,"1FK22083AC001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC00-1MB0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3172,"ST",1,"GMC",1,"1FK22083AC001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC00-1SA0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2773,"ST",1,"GMC",1,"1FK22083AC001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC00-1SB0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2773,"ST",1,"GMC",1,"1FK22083AC001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC01-0MA0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3283,"ST",1,"GMC",1,"1FK22083AC010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC01-0MB0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3283,"ST",1,"GMC",1,"1FK22083AC010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC01-0SA0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2884,"ST",1,"GMC",1,"1FK22083AC010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC01-0SB0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2884,"ST",1,"GMC",1,"1FK22083AC010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC01-1MA0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3283,"ST",1,"GMC",1,"1FK22083AC011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC01-1MB0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3283,"ST",1,"GMC",1,"1FK22083AC011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC01-1SA0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2884,"ST",1,"GMC",1,"1FK22083AC011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC01-1SB0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2884,"ST",1,"GMC",1,"1FK22083AC011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC10-0MA0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3705,"ST",1,"GMC",1,"1FK22083AC100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC10-0MB0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3705,"ST",1,"GMC",1,"1FK22083AC100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC10-0SA0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3306,"ST",1,"GMC",1,"1FK22083AC100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC10-0SB0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3306,"ST",1,"GMC",1,"1FK22083AC100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC10-1MA0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3705,"ST",1,"GMC",1,"1FK22083AC101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC10-1MB0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3705,"ST",1,"GMC",1,"1FK22083AC101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC10-1SA0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3306,"ST",1,"GMC",1,"1FK22083AC101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC10-1SB0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3306,"ST",1,"GMC",1,"1FK22083AC101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC11-0MA0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3816,"ST",1,"GMC",1,"1FK22083AC110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC11-0MB0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3816,"ST",1,"GMC",1,"1FK22083AC110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC11-0SA0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3417,"ST",1,"GMC",1,"1FK22083AC110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC11-0SB0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3417,"ST",1,"GMC",1,"1FK22083AC110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC11-1MA0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3816,"ST",1,"GMC",1,"1FK22083AC111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC11-1MB0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3816,"ST",1,"GMC",1,"1FK22083AC111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC11-1SA0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3417,"ST",1,"GMC",1,"1FK22083AC111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC11-1SB0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3417,"ST",1,"GMC",1,"1FK22083AC111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC00-0MA0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3489,"ST",1,"GMC",1,"1FK22084AC000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC00-0MB0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3489,"ST",1,"GMC",1,"1FK22084AC000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC00-0SA0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3090,"ST",1,"GMC",1,"1FK22084AC000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC00-0SB0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3090,"ST",1,"GMC",1,"1FK22084AC000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC00-1MA0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3489,"ST",1,"GMC",1,"1FK22084AC001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC00-1MB0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3489,"ST",1,"GMC",1,"1FK22084AC001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC00-1SA0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3090,"ST",1,"GMC",1,"1FK22084AC001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC00-1SB0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3090,"ST",1,"GMC",1,"1FK22084AC001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC01-0MA0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3600,"ST",1,"GMC",1,"1FK22084AC010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC01-0MB0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3600,"ST",1,"GMC",1,"1FK22084AC010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC01-0SA0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3202,"ST",1,"GMC",1,"1FK22084AC010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC01-0SB0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3202,"ST",1,"GMC",1,"1FK22084AC010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC01-1MA0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3600,"ST",1,"GMC",1,"1FK22084AC011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC01-1MB0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3600,"ST",1,"GMC",1,"1FK22084AC011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC01-1SA0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3202,"ST",1,"GMC",1,"1FK22084AC011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC01-1SB0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3202,"ST",1,"GMC",1,"1FK22084AC011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC10-0MA0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4022,"ST",1,"GMC",1,"1FK22084AC100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC10-0MB0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4022,"ST",1,"GMC",1,"1FK22084AC100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC10-0SA0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3623,"ST",1,"GMC",1,"1FK22084AC100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC10-0SB0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3623,"ST",1,"GMC",1,"1FK22084AC100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC10-1MA0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4022,"ST",1,"GMC",1,"1FK22084AC101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC10-1MB0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4022,"ST",1,"GMC",1,"1FK22084AC101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC10-1SA0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3623,"ST",1,"GMC",1,"1FK22084AC101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC10-1SB0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3623,"ST",1,"GMC",1,"1FK22084AC101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC11-0MA0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4133,"ST",1,"GMC",1,"1FK22084AC110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC11-0MB0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4133,"ST",1,"GMC",1,"1FK22084AC110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC11-0SA0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3734,"ST",1,"GMC",1,"1FK22084AC110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC11-0SB0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3734,"ST",1,"GMC",1,"1FK22084AC110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC11-1MA0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4133,"ST",1,"GMC",1,"1FK22084AC111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC11-1MB0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4133,"ST",1,"GMC",1,"1FK22084AC111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC11-1SA0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3734,"ST",1,"GMC",1,"1FK22084AC111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC11-1SB0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3734,"ST",1,"GMC",1,"1FK22084AC111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC00-0MA0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3888,"ST",1,"GMC",1,"1FK22085AC000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC00-0MB0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3888,"ST",1,"GMC",1,"1FK22085AC000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC00-0SA0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3489,"ST",1,"GMC",1,"1FK22085AC000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC00-0SB0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3489,"ST",1,"GMC",1,"1FK22085AC000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC00-1MA0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3888,"ST",1,"GMC",1,"1FK22085AC001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC00-1MB0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3888,"ST",1,"GMC",1,"1FK22085AC001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC00-1SA0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3489,"ST",1,"GMC",1,"1FK22085AC001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC00-1SB0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3489,"ST",1,"GMC",1,"1FK22085AC001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC01-0MA0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3999,"ST",1,"GMC",1,"1FK22085AC010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC01-0MB0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3999,"ST",1,"GMC",1,"1FK22085AC010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC01-0SA0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3600,"ST",1,"GMC",1,"1FK22085AC010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC01-0SB0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3600,"ST",1,"GMC",1,"1FK22085AC010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC01-1MA0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3999,"ST",1,"GMC",1,"1FK22085AC011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC01-1MB0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3999,"ST",1,"GMC",1,"1FK22085AC011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC01-1SA0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3600,"ST",1,"GMC",1,"1FK22085AC011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC01-1SB0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3600,"ST",1,"GMC",1,"1FK22085AC011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC10-0MA0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4421,"ST",1,"GMC",1,"1FK22085AC100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC10-0MB0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4421,"ST",1,"GMC",1,"1FK22085AC100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC10-0SA0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",4022,"ST",1,"GMC",1,"1FK22085AC100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC10-0SB0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4022,"ST",1,"GMC",1,"1FK22085AC100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC10-1MA0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4421,"ST",1,"GMC",1,"1FK22085AC101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC10-1MB0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4421,"ST",1,"GMC",1,"1FK22085AC101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC10-1SA0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",4022,"ST",1,"GMC",1,"1FK22085AC101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC10-1SB0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4022,"ST",1,"GMC",1,"1FK22085AC101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC11-0MA0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4532,"ST",1,"GMC",1,"1FK22085AC110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC11-0MB0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4532,"ST",1,"GMC",1,"1FK22085AC110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC11-0SA0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",4133,"ST",1,"GMC",1,"1FK22085AC110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC11-0SB0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4133,"ST",1,"GMC",1,"1FK22085AC110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC11-1MA0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4532,"ST",1,"GMC",1,"1FK22085AC111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC11-1MB0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4532,"ST",1,"GMC",1,"1FK22085AC111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC11-1SA0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",4133,"ST",1,"GMC",1,"1FK22085AC111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC11-1SB0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4133,"ST",1,"GMC",1,"1FK22085AC111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB00-0MA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4101,"ST",1,"GMC",1,"1FK22103AB000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB00-0MB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4101,"ST",1,"GMC",1,"1FK22103AB000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB00-0SA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3702,"ST",1,"GMC",1,"1FK22103AB000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB00-0SB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3702,"ST",1,"GMC",1,"1FK22103AB000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB00-1MA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4101,"ST",1,"GMC",1,"1FK22103AB001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB00-1MB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4101,"ST",1,"GMC",1,"1FK22103AB001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB00-1SA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3702,"ST",1,"GMC",1,"1FK22103AB001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB00-1SB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3702,"ST",1,"GMC",1,"1FK22103AB001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB01-0MA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4212,"ST",1,"GMC",1,"1FK22103AB010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB01-0MB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4212,"ST",1,"GMC",1,"1FK22103AB010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB01-0SA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3813,"ST",1,"GMC",1,"1FK22103AB010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB01-0SB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3813,"ST",1,"GMC",1,"1FK22103AB010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB01-1MA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4212,"ST",1,"GMC",1,"1FK22103AB011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB01-1MB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4212,"ST",1,"GMC",1,"1FK22103AB011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB01-1SA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3813,"ST",1,"GMC",1,"1FK22103AB011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB01-1SB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3813,"ST",1,"GMC",1,"1FK22103AB011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB10-0MA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4687,"ST",1,"GMC",1,"1FK22103AB100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB10-0MB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4687,"ST",1,"GMC",1,"1FK22103AB100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB10-0SA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",4288,"ST",1,"GMC",1,"1FK22103AB100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB10-0SB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4288,"ST",1,"GMC",1,"1FK22103AB100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB10-1MA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4687,"ST",1,"GMC",1,"1FK22103AB101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB10-1MB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4687,"ST",1,"GMC",1,"1FK22103AB101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB10-1SA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",4288,"ST",1,"GMC",1,"1FK22103AB101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB10-1SB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4288,"ST",1,"GMC",1,"1FK22103AB101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB11-0MA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4799,"ST",1,"GMC",1,"1FK22103AB110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB11-0MB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4799,"ST",1,"GMC",1,"1FK22103AB110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB11-0SA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",4400,"ST",1,"GMC",1,"1FK22103AB110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB11-0SB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4400,"ST",1,"GMC",1,"1FK22103AB110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB11-1MA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4799,"ST",1,"GMC",1,"1FK22103AB111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB11-1MB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4799,"ST",1,"GMC",1,"1FK22103AB111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB11-1SA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",4400,"ST",1,"GMC",1,"1FK22103AB111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB11-1SB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4400,"ST",1,"GMC",1,"1FK22103AB111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC00-0MA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4101,"ST",1,"GMC",1,"1FK22103AC000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC00-0MB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4101,"ST",1,"GMC",1,"1FK22103AC000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC00-0SA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3702,"ST",1,"GMC",1,"1FK22103AC000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC00-0SB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3702,"ST",1,"GMC",1,"1FK22103AC000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC00-1MA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4101,"ST",1,"GMC",1,"1FK22103AC001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC00-1MB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4101,"ST",1,"GMC",1,"1FK22103AC001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC00-1SA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3702,"ST",1,"GMC",1,"1FK22103AC001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC00-1SB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3702,"ST",1,"GMC",1,"1FK22103AC001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC01-0MA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4212,"ST",1,"GMC",1,"1FK22103AC010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC01-0MB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4212,"ST",1,"GMC",1,"1FK22103AC010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC01-0SA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3813,"ST",1,"GMC",1,"1FK22103AC010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC01-0SB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3813,"ST",1,"GMC",1,"1FK22103AC010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC01-1MA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4212,"ST",1,"GMC",1,"1FK22103AC011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC01-1MB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4212,"ST",1,"GMC",1,"1FK22103AC011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC01-1SA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3813,"ST",1,"GMC",1,"1FK22103AC011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC01-1SB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3813,"ST",1,"GMC",1,"1FK22103AC011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC10-0MA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4687,"ST",1,"GMC",1,"1FK22103AC100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC10-0MB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4687,"ST",1,"GMC",1,"1FK22103AC100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC10-0SA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",4288,"ST",1,"GMC",1,"1FK22103AC100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC10-0SB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4288,"ST",1,"GMC",1,"1FK22103AC100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC10-1MA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4687,"ST",1,"GMC",1,"1FK22103AC101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC10-1MB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4687,"ST",1,"GMC",1,"1FK22103AC101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC10-1SA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",4288,"ST",1,"GMC",1,"1FK22103AC101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC10-1SB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4288,"ST",1,"GMC",1,"1FK22103AC101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC11-0MA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4799,"ST",1,"GMC",1,"1FK22103AC110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC11-0MB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4799,"ST",1,"GMC",1,"1FK22103AC110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC11-0SA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",4400,"ST",1,"GMC",1,"1FK22103AC110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC11-0SB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4400,"ST",1,"GMC",1,"1FK22103AC110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC11-1MA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4799,"ST",1,"GMC",1,"1FK22103AC111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC11-1MB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4799,"ST",1,"GMC",1,"1FK22103AC111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC11-1SA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",4400,"ST",1,"GMC",1,"1FK22103AC111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC11-1SB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4400,"ST",1,"GMC",1,"1FK22103AC111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB00-0MA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4931,"ST",1,"GMC",1,"1FK22104AB000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB00-0MB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4931,"ST",1,"GMC",1,"1FK22104AB000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB00-0SA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",4532,"ST",1,"GMC",1,"1FK22104AB000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB00-0SB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4532,"ST",1,"GMC",1,"1FK22104AB000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB00-1MA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4931,"ST",1,"GMC",1,"1FK22104AB001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB00-1MB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4931,"ST",1,"GMC",1,"1FK22104AB001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB00-1SA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",4532,"ST",1,"GMC",1,"1FK22104AB001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB00-1SB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4532,"ST",1,"GMC",1,"1FK22104AB001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB01-0MA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",5042,"ST",1,"GMC",1,"1FK22104AB010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB01-0MB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",5042,"ST",1,"GMC",1,"1FK22104AB010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB01-0SA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",4643,"ST",1,"GMC",1,"1FK22104AB010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB01-0SB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4643,"ST",1,"GMC",1,"1FK22104AB010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB01-1MA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",5042,"ST",1,"GMC",1,"1FK22104AB011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB01-1MB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",5042,"ST",1,"GMC",1,"1FK22104AB011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB01-1SA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",4643,"ST",1,"GMC",1,"1FK22104AB011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB01-1SB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4643,"ST",1,"GMC",1,"1FK22104AB011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB10-0MA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",5517,"ST",1,"GMC",1,"1FK22104AB100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB10-0MB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",5517,"ST",1,"GMC",1,"1FK22104AB100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB10-0SA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",5118,"ST",1,"GMC",1,"1FK22104AB100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB10-0SB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",5118,"ST",1,"GMC",1,"1FK22104AB100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB10-1MA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",5517,"ST",1,"GMC",1,"1FK22104AB101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB10-1MB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",5517,"ST",1,"GMC",1,"1FK22104AB101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB10-1SA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",5118,"ST",1,"GMC",1,"1FK22104AB101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB10-1SB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",5118,"ST",1,"GMC",1,"1FK22104AB101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB11-0MA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",5628,"ST",1,"GMC",1,"1FK22104AB110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB11-0MB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",5628,"ST",1,"GMC",1,"1FK22104AB110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB11-0SA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",5229,"ST",1,"GMC",1,"1FK22104AB110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB11-0SB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",5229,"ST",1,"GMC",1,"1FK22104AB110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB11-1MA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",5628,"ST",1,"GMC",1,"1FK22104AB111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB11-1MB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",5628,"ST",1,"GMC",1,"1FK22104AB111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB11-1SA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",5229,"ST",1,"GMC",1,"1FK22104AB111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB11-1SB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",5229,"ST",1,"GMC",1,"1FK22104AB111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC00-0MA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4931,"ST",1,"GMC",1,"1FK22104AC000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC00-0MB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4931,"ST",1,"GMC",1,"1FK22104AC000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC00-0SA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",4532,"ST",1,"GMC",1,"1FK22104AC000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC00-0SB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4532,"ST",1,"GMC",1,"1FK22104AC000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC00-1MA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4931,"ST",1,"GMC",1,"1FK22104AC001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC00-1MB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4931,"ST",1,"GMC",1,"1FK22104AC001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC00-1SA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",4532,"ST",1,"GMC",1,"1FK22104AC001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC00-1SB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4532,"ST",1,"GMC",1,"1FK22104AC001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC01-0MA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",5042,"ST",1,"GMC",1,"1FK22104AC010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC01-0MB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",5042,"ST",1,"GMC",1,"1FK22104AC010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC01-0SA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",4643,"ST",1,"GMC",1,"1FK22104AC010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC01-0SB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4643,"ST",1,"GMC",1,"1FK22104AC010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC01-1MA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",5042,"ST",1,"GMC",1,"1FK22104AC011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC01-1MB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",5042,"ST",1,"GMC",1,"1FK22104AC011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC01-1SA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",4643,"ST",1,"GMC",1,"1FK22104AC011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC01-1SB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4643,"ST",1,"GMC",1,"1FK22104AC011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC10-0MA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",5517,"ST",1,"GMC",1,"1FK22104AC100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC10-0MB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",5517,"ST",1,"GMC",1,"1FK22104AC100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC10-0SA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",5118,"ST",1,"GMC",1,"1FK22104AC100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC10-0SB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",5118,"ST",1,"GMC",1,"1FK22104AC100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC10-1MA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",5517,"ST",1,"GMC",1,"1FK22104AC101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC10-1MB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",5517,"ST",1,"GMC",1,"1FK22104AC101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC10-1SA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",5118,"ST",1,"GMC",1,"1FK22104AC101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC10-1SB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",5118,"ST",1,"GMC",1,"1FK22104AC101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC11-0MA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",5628,"ST",1,"GMC",1,"1FK22104AC110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC11-0MB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",5628,"ST",1,"GMC",1,"1FK22104AC110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC11-0SA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",5229,"ST",1,"GMC",1,"1FK22104AC110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC11-0SB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",5229,"ST",1,"GMC",1,"1FK22104AC110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC11-1MA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",5628,"ST",1,"GMC",1,"1FK22104AC111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC11-1MB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",5628,"ST",1,"GMC",1,"1FK22104AC111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC11-1SA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",5229,"ST",1,"GMC",1,"1FK22104AC111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC11-1SB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",5229,"ST",1,"GMC",1,"1FK22104AC111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-5AC00-0MB0","SIMOTICS S-1FK2 CT servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M40;",5741,"ST",1,"GMC",1,"1FK22105AC000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-5AC00-0SB0","SIMOTICS S-1FK2 CT servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M40;",5342,"ST",1,"GMC",1,"1FK22105AC000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-5AC00-1MB0","SIMOTICS S-1FK2 CT servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M40;",5741,"ST",1,"GMC",1,"1FK22105AC001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-5AC00-1SB0","SIMOTICS S-1FK2 CT servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M40;",5342,"ST",1,"GMC",1,"1FK22105AC001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-5AC01-0MB0","SIMOTICS S-1FK2 CT servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M40;",5852,"ST",1,"GMC",1,"1FK22105AC010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-5AC01-0SB0","SIMOTICS S-1FK2 CT servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M40;",5453,"ST",1,"GMC",1,"1FK22105AC010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-5AC01-1MB0","SIMOTICS S-1FK2 CT servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M40;",5852,"ST",1,"GMC",1,"1FK22105AC011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-5AC01-1SB0","SIMOTICS S-1FK2 CT servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M40;",5453,"ST",1,"GMC",1,"1FK22105AC011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-5AC10-0MB0","SIMOTICS S-1FK2 CT servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M40;",6327,"ST",1,"GMC",1,"1FK22105AC100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-5AC10-0SB0","SIMOTICS S-1FK2 CT servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M40;",5928,"ST",1,"GMC",1,"1FK22105AC100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-5AC10-1MB0","SIMOTICS S-1FK2 CT servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M40;",6327,"ST",1,"GMC",1,"1FK22105AC101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-5AC10-1SB0","SIMOTICS S-1FK2 CT servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M40;",5928,"ST",1,"GMC",1,"1FK22105AC101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-5AC11-0MB0","SIMOTICS S-1FK2 CT servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M40;",6439,"ST",1,"GMC",1,"1FK22105AC110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-5AC11-0SB0","SIMOTICS S-1FK2 CT servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M40;",6040,"ST",1,"GMC",1,"1FK22105AC110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-5AC11-1MB0","SIMOTICS S-1FK2 CT servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M40;",6439,"ST",1,"GMC",1,"1FK22105AC111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-5AC11-1SB0","SIMOTICS S-1FK2 CT servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M40;",6040,"ST",1,"GMC",1,"1FK22105AC111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-2AC00-0MB0","SIMOTICS S-1FK2 HI servo motor M0=6 Nm; PN = 1.15 kW at NN=2000 rpm, (380-480 V); degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2123,"ST",1,"GMC",1,"1FK23062AC000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-2AC00-0SB0","SIMOTICS S-1FK2 HI servo motor M0=6 Nm; PN = 1.15 kW at NN=2000 rpm, (380-480 V); degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",1724,"ST",1,"GMC",1,"1FK23062AC000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-2AC00-1MB0","SIMOTICS S-1FK2 HI servo motor M0=6 Nm; PN = 1.15 kW at NN=2000 rpm, (380-480 V); degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2123,"ST",1,"GMC",1,"1FK23062AC001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-2AC00-1SB0","SIMOTICS S-1FK2 HI servo motor M0=6 Nm; PN = 1.15 kW at NN=2000 rpm, (380-480 V); degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",1724,"ST",1,"GMC",1,"1FK23062AC001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-2AC01-0MB0","SIMOTICS S-1FK2 HI servo motor M0=6 Nm; PN = 1.15 kW at NN=2000 rpm, (380-480 V); degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2234,"ST",1,"GMC",1,"1FK23062AC010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-2AC01-0SB0","SIMOTICS S-1FK2 HI servo motor M0=6 Nm; PN = 1.15 kW at NN=2000 rpm, (380-480 V); degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",1835,"ST",1,"GMC",1,"1FK23062AC010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-2AC01-1MB0","SIMOTICS S-1FK2 HI servo motor M0=6 Nm; PN = 1.15 kW at NN=2000 rpm, (380-480 V); degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2234,"ST",1,"GMC",1,"1FK23062AC011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-2AC01-1SB0","SIMOTICS S-1FK2 HI servo motor M0=6 Nm; PN = 1.15 kW at NN=2000 rpm, (380-480 V); degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",1835,"ST",1,"GMC",1,"1FK23062AC011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-2AC10-0MB0","SIMOTICS S-1FK2 HI servo motor M0=6 Nm; PN = 1.15 kW at NN=2000 rpm, (380-480 V); with holding brake; degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2549,"ST",1,"GMC",1,"1FK23062AC100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-2AC10-0SB0","SIMOTICS S-1FK2 HI servo motor M0=6 Nm; PN = 1.15 kW at NN=2000 rpm, (380-480 V); with holding brake; degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2150,"ST",1,"GMC",1,"1FK23062AC100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-2AC10-1MB0","SIMOTICS S-1FK2 HI servo motor M0=6 Nm; PN = 1.15 kW at NN=2000 rpm, (380-480 V); with holding brake; degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2549,"ST",1,"GMC",1,"1FK23062AC101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-2AC10-1SB0","SIMOTICS S-1FK2 HI servo motor M0=6 Nm; PN = 1.15 kW at NN=2000 rpm, (380-480 V); with holding brake; degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2150,"ST",1,"GMC",1,"1FK23062AC101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-2AC11-0MB0","SIMOTICS S-1FK2 HI servo motor M0=6 Nm; PN = 1.15 kW at NN=2000 rpm, (380-480 V); with holding brake; degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2661,"ST",1,"GMC",1,"1FK23062AC110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-2AC11-0SB0","SIMOTICS S-1FK2 HI servo motor M0=6 Nm; PN = 1.15 kW at NN=2000 rpm, (380-480 V); with holding brake; degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2262,"ST",1,"GMC",1,"1FK23062AC110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-2AC11-1MB0","SIMOTICS S-1FK2 HI servo motor M0=6 Nm; PN = 1.15 kW at NN=2000 rpm, (380-480 V); with holding brake; degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2661,"ST",1,"GMC",1,"1FK23062AC111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-2AC11-1SB0","SIMOTICS S-1FK2 HI servo motor M0=6 Nm; PN = 1.15 kW at NN=2000 rpm, (380-480 V); with holding brake; degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2262,"ST",1,"GMC",1,"1FK23062AC111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-4AC00-0MB0","SIMOTICS S-1FK2 HI servo motor M0=12 Nm; PN = 2.2 kW at NN=2000 rpm, (380-480 V); degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2706,"ST",1,"GMC",1,"1FK23064AC000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-4AC00-0SB0","SIMOTICS S-1FK2 HI servo motor M0=12 Nm; PN = 2.2 kW at NN=2000 rpm, (380-480 V); degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2307,"ST",1,"GMC",1,"1FK23064AC000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-4AC00-1MB0","SIMOTICS S-1FK2 HI servo motor M0=12 Nm; PN = 2.2 kW at NN=2000 rpm, (380-480 V); degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2706,"ST",1,"GMC",1,"1FK23064AC001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-4AC00-1SB0","SIMOTICS S-1FK2 HI servo motor M0=12 Nm; PN = 2.2 kW at NN=2000 rpm, (380-480 V); degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2307,"ST",1,"GMC",1,"1FK23064AC001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-4AC01-0MB0","SIMOTICS S-1FK2 HI servo motor M0=12 Nm; PN = 2.2 kW at NN=2000 rpm, (380-480 V); degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2818,"ST",1,"GMC",1,"1FK23064AC010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-4AC01-0SB0","SIMOTICS S-1FK2 HI servo motor M0=12 Nm; PN = 2.2 kW at NN=2000 rpm, (380-480 V); degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2419,"ST",1,"GMC",1,"1FK23064AC010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-4AC01-1MB0","SIMOTICS S-1FK2 HI servo motor M0=12 Nm; PN = 2.2 kW at NN=2000 rpm, (380-480 V); degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2818,"ST",1,"GMC",1,"1FK23064AC011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-4AC01-1SB0","SIMOTICS S-1FK2 HI servo motor M0=12 Nm; PN = 2.2 kW at NN=2000 rpm, (380-480 V); degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2419,"ST",1,"GMC",1,"1FK23064AC011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-4AC10-0MB0","SIMOTICS S-1FK2 HI servo motor M0=12 Nm; PN = 2.2 kW at NN=2000 rpm, (380-480 V); with holding brake; degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3133,"ST",1,"GMC",1,"1FK23064AC100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-4AC10-0SB0","SIMOTICS S-1FK2 HI servo motor M0=12 Nm; PN = 2.2 kW at NN=2000 rpm, (380-480 V); with holding brake; degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2734,"ST",1,"GMC",1,"1FK23064AC100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-4AC10-1MB0","SIMOTICS S-1FK2 HI servo motor M0=12 Nm; PN = 2.2 kW at NN=2000 rpm, (380-480 V); with holding brake; degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3133,"ST",1,"GMC",1,"1FK23064AC101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-4AC10-1SB0","SIMOTICS S-1FK2 HI servo motor M0=12 Nm; PN = 2.2 kW at NN=2000 rpm, (380-480 V); with holding brake; degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2734,"ST",1,"GMC",1,"1FK23064AC101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-4AC11-0MB0","SIMOTICS S-1FK2 HI servo motor M0=12 Nm; PN = 2.2 kW at NN=2000 rpm, (380-480 V); with holding brake; degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3244,"ST",1,"GMC",1,"1FK23064AC110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-4AC11-0SB0","SIMOTICS S-1FK2 HI servo motor M0=12 Nm; PN = 2.2 kW at NN=2000 rpm, (380-480 V); with holding brake; degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2845,"ST",1,"GMC",1,"1FK23064AC110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-4AC11-1MB0","SIMOTICS S-1FK2 HI servo motor M0=12 Nm; PN = 2.2 kW at NN=2000 rpm, (380-480 V); with holding brake; degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3244,"ST",1,"GMC",1,"1FK23064AC111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-4AC11-1SB0","SIMOTICS S-1FK2 HI servo motor M0=12 Nm; PN = 2.2 kW at NN=2000 rpm, (380-480 V); with holding brake; degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2845,"ST",1,"GMC",1,"1FK23064AC111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-3AB00-0MB0","SIMOTICS S-1FK2 HI servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3172,"ST",1,"GMC",1,"1FK23083AB000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-3AB00-0SB0","SIMOTICS S-1FK2 HI servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2773,"ST",1,"GMC",1,"1FK23083AB000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-3AB00-1MB0","SIMOTICS S-1FK2 HI servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3172,"ST",1,"GMC",1,"1FK23083AB001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-3AB00-1SB0","SIMOTICS S-1FK2 HI servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2773,"ST",1,"GMC",1,"1FK23083AB001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-3AB01-0MB0","SIMOTICS S-1FK2 HI servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3283,"ST",1,"GMC",1,"1FK23083AB010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-3AB01-0SB0","SIMOTICS S-1FK2 HI servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2884,"ST",1,"GMC",1,"1FK23083AB010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-3AB01-1MB0","SIMOTICS S-1FK2 HI servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3283,"ST",1,"GMC",1,"1FK23083AB011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-3AB01-1SB0","SIMOTICS S-1FK2 HI servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2884,"ST",1,"GMC",1,"1FK23083AB011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-3AB10-0MB0","SIMOTICS S-1FK2 HI servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); with holding brake; degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3705,"ST",1,"GMC",1,"1FK23083AB100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-3AB10-0SB0","SIMOTICS S-1FK2 HI servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); with holding brake; degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3306,"ST",1,"GMC",1,"1FK23083AB100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-3AB10-1MB0","SIMOTICS S-1FK2 HI servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); with holding brake; degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3705,"ST",1,"GMC",1,"1FK23083AB101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-3AB10-1SB0","SIMOTICS S-1FK2 HI servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); with holding brake; degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3306,"ST",1,"GMC",1,"1FK23083AB101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-3AB11-0MB0","SIMOTICS S-1FK2 HI servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); with holding brake; degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3816,"ST",1,"GMC",1,"1FK23083AB110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-3AB11-0SB0","SIMOTICS S-1FK2 HI servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); with holding brake; degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3417,"ST",1,"GMC",1,"1FK23083AB110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-3AB11-1MB0","SIMOTICS S-1FK2 HI servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); with holding brake; degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3816,"ST",1,"GMC",1,"1FK23083AB111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-3AB11-1SB0","SIMOTICS S-1FK2 HI servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); with holding brake; degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3417,"ST",1,"GMC",1,"1FK23083AB111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-4AB00-0MB0","SIMOTICS S-1FK2 HI servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3489,"ST",1,"GMC",1,"1FK23084AB000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-4AB00-0SB0","SIMOTICS S-1FK2 HI servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3090,"ST",1,"GMC",1,"1FK23084AB000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-4AB00-1MB0","SIMOTICS S-1FK2 HI servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3489,"ST",1,"GMC",1,"1FK23084AB001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-4AB00-1SB0","SIMOTICS S-1FK2 HI servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3090,"ST",1,"GMC",1,"1FK23084AB001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-4AB01-0MB0","SIMOTICS S-1FK2 HI servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3600,"ST",1,"GMC",1,"1FK23084AB010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-4AB01-0SB0","SIMOTICS S-1FK2 HI servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3202,"ST",1,"GMC",1,"1FK23084AB010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-4AB01-1MB0","SIMOTICS S-1FK2 HI servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3600,"ST",1,"GMC",1,"1FK23084AB011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-4AB01-1SB0","SIMOTICS S-1FK2 HI servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3202,"ST",1,"GMC",1,"1FK23084AB011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-4AB10-0MB0","SIMOTICS S-1FK2 HI servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); with holding brake; degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4022,"ST",1,"GMC",1,"1FK23084AB100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-4AB10-0SB0","SIMOTICS S-1FK2 HI servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); with holding brake; degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3623,"ST",1,"GMC",1,"1FK23084AB100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-4AB10-1MB0","SIMOTICS S-1FK2 HI servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); with holding brake; degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4022,"ST",1,"GMC",1,"1FK23084AB101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-4AB10-1SB0","SIMOTICS S-1FK2 HI servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); with holding brake; degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3623,"ST",1,"GMC",1,"1FK23084AB101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-4AB11-0MB0","SIMOTICS S-1FK2 HI servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); with holding brake; degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4133,"ST",1,"GMC",1,"1FK23084AB110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-4AB11-0SB0","SIMOTICS S-1FK2 HI servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); with holding brake; degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3734,"ST",1,"GMC",1,"1FK23084AB110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-4AB11-1MB0","SIMOTICS S-1FK2 HI servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); with holding brake; degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4133,"ST",1,"GMC",1,"1FK23084AB111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-4AB11-1SB0","SIMOTICS S-1FK2 HI servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); with holding brake; degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3734,"ST",1,"GMC",1,"1FK23084AB111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK24-1AA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1918,"ST",1,"GMC",1,"1FK70115AK241AA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK24-1AB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",2253,"ST",1,"GMC",1,"1FK70115AK241AB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK24-1AG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1853,"ST",1,"GMC",1,"1FK70115AK241AG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK24-1AH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",2117,"ST",1,"GMC",1,"1FK70115AK241AH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK24-1JA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor absolute encoder 16 S/R (encoder A-16); derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1717,"ST",1,"GMC",1,"1FK70115AK241JA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK24-1JB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor absolute encoder 16 S/R (encoder A-16); derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",2053,"ST",1,"GMC",1,"1FK70115AK241JB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK24-1JG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor absolute encoder 16 S/R (encoder A-16); derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1653,"ST",1,"GMC",1,"1FK70115AK241JG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK24-1JH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor absolute encoder 16 S/R (encoder A-16); derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1917,"ST",1,"GMC",1,"1FK70115AK241JH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK24-1SA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1043,"ST",1,"GMC",1,"1FK70115AK241SA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK24-1SB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1379,"ST",1,"GMC",1,"1FK70115AK241SB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK24-1SG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",979,"ST",1,"GMC",1,"1FK70115AK241SG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK24-1SH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1243,"ST",1,"GMC",1,"1FK70115AK241SH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK24-1TA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1043,"ST",1,"GMC",1,"1FK70115AK241TA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK24-1TB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1379,"ST",1,"GMC",1,"1FK70115AK241TB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK24-1TG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",979,"ST",1,"GMC",1,"1FK70115AK241TG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK24-1TH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1243,"ST",1,"GMC",1,"1FK70115AK241TH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK74-1AA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1918,"ST",1,"GMC",1,"1FK70115AK741AA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK74-1AB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",2253,"ST",1,"GMC",1,"1FK70115AK741AB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK74-1AG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1853,"ST",1,"GMC",1,"1FK70115AK741AG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK74-1AH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",2117,"ST",1,"GMC",1,"1FK70115AK741AH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK74-1JA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor absolute encoder 16 S/R (encoder A-16); derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1717,"ST",1,"GMC",1,"1FK70115AK741JA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK74-1JB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor absolute encoder 16 S/R (encoder A-16); derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",2053,"ST",1,"GMC",1,"1FK70115AK741JB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK74-1JG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor absolute encoder 16 S/R (encoder A-16); derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1653,"ST",1,"GMC",1,"1FK70115AK741JG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK74-1JH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor absolute encoder 16 S/R (encoder A-16); derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1917,"ST",1,"GMC",1,"1FK70115AK741JH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK74-1SA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1043,"ST",1,"GMC",1,"1FK70115AK741SA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK74-1SB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1379,"ST",1,"GMC",1,"1FK70115AK741SB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK74-1SG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",979,"ST",1,"GMC",1,"1FK70115AK741SG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK74-1SH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1243,"ST",1,"GMC",1,"1FK70115AK741SH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK74-1TA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1043,"ST",1,"GMC",1,"1FK70115AK741TA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK74-1TB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1379,"ST",1,"GMC",1,"1FK70115AK741TB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK74-1TG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",979,"ST",1,"GMC",1,"1FK70115AK741TG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK74-1TH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1243,"ST",1,"GMC",1,"1FK70115AK741TH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK24-1AA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",2041,"ST",1,"GMC",1,"1FK70155AK241AA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK24-1AB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",2376,"ST",1,"GMC",1,"1FK70155AK241AB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK24-1AG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1976,"ST",1,"GMC",1,"1FK70155AK241AG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK24-1AH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",2240,"ST",1,"GMC",1,"1FK70155AK241AH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK24-1JA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor absolute encoder 16 S/R (encoder A-16); derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1840,"ST",1,"GMC",1,"1FK70155AK241JA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK24-1JB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor absolute encoder 16 S/R (encoder A-16); derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",2176,"ST",1,"GMC",1,"1FK70155AK241JB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK24-1JG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor absolute encoder 16 S/R (encoder A-16); derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1776,"ST",1,"GMC",1,"1FK70155AK241JG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK24-1JH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor absolute encoder 16 S/R (encoder A-16); derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",2040,"ST",1,"GMC",1,"1FK70155AK241JH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK24-1SA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1166,"ST",1,"GMC",1,"1FK70155AK241SA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK24-1SB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1502,"ST",1,"GMC",1,"1FK70155AK241SB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK24-1SG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1102,"ST",1,"GMC",1,"1FK70155AK241SG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK24-1SH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1366,"ST",1,"GMC",1,"1FK70155AK241SH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK24-1TA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1166,"ST",1,"GMC",1,"1FK70155AK241TA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK24-1TB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1502,"ST",1,"GMC",1,"1FK70155AK241TB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK24-1TG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1102,"ST",1,"GMC",1,"1FK70155AK241TG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK24-1TH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1366,"ST",1,"GMC",1,"1FK70155AK241TH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK74-1AA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",2041,"ST",1,"GMC",1,"1FK70155AK741AA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK74-1AB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",2376,"ST",1,"GMC",1,"1FK70155AK741AB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK74-1AG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1976,"ST",1,"GMC",1,"1FK70155AK741AG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK74-1AH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",2240,"ST",1,"GMC",1,"1FK70155AK741AH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK74-1JA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor absolute encoder 16 S/R (encoder A-16); derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1840,"ST",1,"GMC",1,"1FK70155AK741JA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK74-1JB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor absolute encoder 16 S/R (encoder A-16); derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",2176,"ST",1,"GMC",1,"1FK70155AK741JB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK74-1JG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor absolute encoder 16 S/R (encoder A-16); derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1776,"ST",1,"GMC",1,"1FK70155AK741JG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK74-1JH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor absolute encoder 16 S/R (encoder A-16); derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",2040,"ST",1,"GMC",1,"1FK70155AK741JH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK74-1SA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1166,"ST",1,"GMC",1,"1FK70155AK741SA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK74-1SB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1502,"ST",1,"GMC",1,"1FK70155AK741SB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK74-1SG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1102,"ST",1,"GMC",1,"1FK70155AK741SG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK74-1SH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1366,"ST",1,"GMC",1,"1FK70155AK741SH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK74-1TA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1166,"ST",1,"GMC",1,"1FK70155AK741TA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK74-1TB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1502,"ST",1,"GMC",1,"1FK70155AK741TB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK74-1TG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1102,"ST",1,"GMC",1,"1FK70155AK741TG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK74-1TH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1366,"ST",1,"GMC",1,"1FK70155AK741TH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AF04-1AB0","SIMOTICS S-1FK7 Synchronous servo motor 1FK7 Compact; naturally cooled; NN=3000rpm; UDC=24V; IMB 5 design; Power connector rotatable; Incremental encoder sin/cos 1VSS 2048 S/R (encoder I-2048); Shaft with feather key Tolerance N with holding brake; Degree of protection IP64; Customer-specific version customer-specific motor",2682,"ST",1,"GMC",1,"1FK70225AF041AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1DA0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2749,"ST",1,"GMC",1,"1FK70225AK211DA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1DA2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2893,"ST",1,"GMC",1,"1FK70225AK211DA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1DA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2819,"ST",1,"GMC",1,"1FK70225AK211DA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1DA5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2962,"ST",1,"GMC",1,"1FK70225AK211DA5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1DA8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3116,"ST",1,"GMC",1,"1FK70225AK211DA8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1DB0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",3085,"ST",1,"GMC",1,"1FK70225AK211DB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1DB2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",3229,"ST",1,"GMC",1,"1FK70225AK211DB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1DB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",3155,"ST",1,"GMC",1,"1FK70225AK211DB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1DB5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",3298,"ST",1,"GMC",1,"1FK70225AK211DB5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1DB8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3451,"ST",1,"GMC",1,"1FK70225AK211DB8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1DG0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2617,"ST",1,"GMC",1,"1FK70225AK211DG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1DG2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2760,"ST",1,"GMC",1,"1FK70225AK211DG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1DG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2687,"ST",1,"GMC",1,"1FK70225AK211DG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1DG5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2830,"ST",1,"GMC",1,"1FK70225AK211DG5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1DG8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2983,"ST",1,"GMC",1,"1FK70225AK211DG8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1DH0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2949,"ST",1,"GMC",1,"1FK70225AK211DH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1DH2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",3093,"ST",1,"GMC",1,"1FK70225AK211DH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1DH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",3019,"ST",1,"GMC",1,"1FK70225AK211DH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1DH5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",3162,"ST",1,"GMC",1,"1FK70225AK211DH5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1DH8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3315,"ST",1,"GMC",1,"1FK70225AK211DH8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1LA0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",3316,"ST",1,"GMC",1,"1FK70225AK211LA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1LA2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",3459,"ST",1,"GMC",1,"1FK70225AK211LA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1LA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",3385,"ST",1,"GMC",1,"1FK70225AK211LA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1LA5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",3529,"ST",1,"GMC",1,"1FK70225AK211LA5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1LA8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3682,"ST",1,"GMC",1,"1FK70225AK211LA8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1LB0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",3652,"ST",1,"GMC",1,"1FK70225AK211LB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1LB2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",3795,"ST",1,"GMC",1,"1FK70225AK211LB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1LB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",3721,"ST",1,"GMC",1,"1FK70225AK211LB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1LB5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",3865,"ST",1,"GMC",1,"1FK70225AK211LB5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1LB8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",4018,"ST",1,"GMC",1,"1FK70225AK211LB8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1LG0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",3183,"ST",1,"GMC",1,"1FK70225AK211LG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1LG2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",3327,"ST",1,"GMC",1,"1FK70225AK211LG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1LG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",3253,"ST",1,"GMC",1,"1FK70225AK211LG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1LG5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",3396,"ST",1,"GMC",1,"1FK70225AK211LG5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1LG8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3550,"ST",1,"GMC",1,"1FK70225AK211LG8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1LH0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",3516,"ST",1,"GMC",1,"1FK70225AK211LH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1LH2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",3659,"ST",1,"GMC",1,"1FK70225AK211LH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1LH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",3585,"ST",1,"GMC",1,"1FK70225AK211LH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1LH5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",3729,"ST",1,"GMC",1,"1FK70225AK211LH5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1LH8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3882,"ST",1,"GMC",1,"1FK70225AK211LH8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1PA0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1850,"ST",1,"GMC",1,"1FK70225AK211PA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1PA2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1994,"ST",1,"GMC",1,"1FK70225AK211PA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1PA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1920,"ST",1,"GMC",1,"1FK70225AK211PA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1PA5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2063,"ST",1,"GMC",1,"1FK70225AK211PA5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1PA8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2217,"ST",1,"GMC",1,"1FK70225AK211PA8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1PB0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2186,"ST",1,"GMC",1,"1FK70225AK211PB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1PB2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2330,"ST",1,"GMC",1,"1FK70225AK211PB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1PB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2256,"ST",1,"GMC",1,"1FK70225AK211PB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1PB5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2399,"ST",1,"GMC",1,"1FK70225AK211PB5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1PB8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2553,"ST",1,"GMC",1,"1FK70225AK211PB8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1PG0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1718,"ST",1,"GMC",1,"1FK70225AK211PG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1PG2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1862,"ST",1,"GMC",1,"1FK70225AK211PG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1PG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1788,"ST",1,"GMC",1,"1FK70225AK211PG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1PG5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1931,"ST",1,"GMC",1,"1FK70225AK211PG5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1PG8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2084,"ST",1,"GMC",1,"1FK70225AK211PG8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1PH0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2050,"ST",1,"GMC",1,"1FK70225AK211PH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1PH2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2194,"ST",1,"GMC",1,"1FK70225AK211PH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1PH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2120,"ST",1,"GMC",1,"1FK70225AK211PH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1PH5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2263,"ST",1,"GMC",1,"1FK70225AK211PH5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1PH8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2417,"ST",1,"GMC",1,"1FK70225AK211PH8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1UA0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1806,"ST",1,"GMC",1,"1FK70225AK211UA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1UA2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1950,"ST",1,"GMC",1,"1FK70225AK211UA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1UA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1876,"ST",1,"GMC",1,"1FK70225AK211UA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1UA5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2019,"ST",1,"GMC",1,"1FK70225AK211UA5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1UA8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2173,"ST",1,"GMC",1,"1FK70225AK211UA8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1UB0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2142,"ST",1,"GMC",1,"1FK70225AK211UB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1UB2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2286,"ST",1,"GMC",1,"1FK70225AK211UB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1UB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2212,"ST",1,"GMC",1,"1FK70225AK211UB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1UB5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2355,"ST",1,"GMC",1,"1FK70225AK211UB5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1UB8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2509,"ST",1,"GMC",1,"1FK70225AK211UB8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1UG0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1674,"ST",1,"GMC",1,"1FK70225AK211UG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1UG2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1818,"ST",1,"GMC",1,"1FK70225AK211UG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1UG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1744,"ST",1,"GMC",1,"1FK70225AK211UG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1UG5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1887,"ST",1,"GMC",1,"1FK70225AK211UG5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1UG8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2040,"ST",1,"GMC",1,"1FK70225AK211UG8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1UH0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2006,"ST",1,"GMC",1,"1FK70225AK211UH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1UH2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2150,"ST",1,"GMC",1,"1FK70225AK211UH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1UH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2076,"ST",1,"GMC",1,"1FK70225AK211UH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1UH5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2219,"ST",1,"GMC",1,"1FK70225AK211UH5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1UH8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2373,"ST",1,"GMC",1,"1FK70225AK211UH8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK24-1AA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2425,"ST",1,"GMC",1,"1FK70225AK241AA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK24-1AA5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2568,"ST",1,"GMC",1,"1FK70225AK241AA5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK24-1AB0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2691,"ST",1,"GMC",1,"1FK70225AK241AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1DA0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2749,"ST",1,"GMC",1,"1FK70225AK711DA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1DA2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2893,"ST",1,"GMC",1,"1FK70225AK711DA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1DA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2819,"ST",1,"GMC",1,"1FK70225AK711DA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1DA5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2962,"ST",1,"GMC",1,"1FK70225AK711DA5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1DA8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3116,"ST",1,"GMC",1,"1FK70225AK711DA8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1DB0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",3085,"ST",1,"GMC",1,"1FK70225AK711DB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1DB2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",3229,"ST",1,"GMC",1,"1FK70225AK711DB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1DB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",3155,"ST",1,"GMC",1,"1FK70225AK711DB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1DB5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",3298,"ST",1,"GMC",1,"1FK70225AK711DB5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1DB8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3451,"ST",1,"GMC",1,"1FK70225AK711DB8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1DG0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2617,"ST",1,"GMC",1,"1FK70225AK711DG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1DG2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2760,"ST",1,"GMC",1,"1FK70225AK711DG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1DG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2687,"ST",1,"GMC",1,"1FK70225AK711DG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1DG5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2830,"ST",1,"GMC",1,"1FK70225AK711DG5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1DG8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2983,"ST",1,"GMC",1,"1FK70225AK711DG8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1DH0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2949,"ST",1,"GMC",1,"1FK70225AK711DH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1DH2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",3093,"ST",1,"GMC",1,"1FK70225AK711DH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1DH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",3019,"ST",1,"GMC",1,"1FK70225AK711DH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1DH5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",3162,"ST",1,"GMC",1,"1FK70225AK711DH5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1DH8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3315,"ST",1,"GMC",1,"1FK70225AK711DH8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1LA0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",3316,"ST",1,"GMC",1,"1FK70225AK711LA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1LA2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",3459,"ST",1,"GMC",1,"1FK70225AK711LA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1LA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",3385,"ST",1,"GMC",1,"1FK70225AK711LA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1LA5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",3529,"ST",1,"GMC",1,"1FK70225AK711LA5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1LA8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3682,"ST",1,"GMC",1,"1FK70225AK711LA8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1LB0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",3652,"ST",1,"GMC",1,"1FK70225AK711LB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1LB2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",3795,"ST",1,"GMC",1,"1FK70225AK711LB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1LB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",3721,"ST",1,"GMC",1,"1FK70225AK711LB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1LB5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",3865,"ST",1,"GMC",1,"1FK70225AK711LB5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1LB8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",4018,"ST",1,"GMC",1,"1FK70225AK711LB8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1LG0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",3183,"ST",1,"GMC",1,"1FK70225AK711LG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1LG2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",3327,"ST",1,"GMC",1,"1FK70225AK711LG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1LG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",3253,"ST",1,"GMC",1,"1FK70225AK711LG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1LG5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",3396,"ST",1,"GMC",1,"1FK70225AK711LG5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1LG8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3550,"ST",1,"GMC",1,"1FK70225AK711LG8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1LH0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",3516,"ST",1,"GMC",1,"1FK70225AK711LH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1LH2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",3659,"ST",1,"GMC",1,"1FK70225AK711LH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1LH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",3585,"ST",1,"GMC",1,"1FK70225AK711LH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1LH5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",3729,"ST",1,"GMC",1,"1FK70225AK711LH5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1LH8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3882,"ST",1,"GMC",1,"1FK70225AK711LH8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1PA0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1850,"ST",1,"GMC",1,"1FK70225AK711PA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1PA2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1994,"ST",1,"GMC",1,"1FK70225AK711PA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1PA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1920,"ST",1,"GMC",1,"1FK70225AK711PA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1PA5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2063,"ST",1,"GMC",1,"1FK70225AK711PA5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1PA8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2217,"ST",1,"GMC",1,"1FK70225AK711PA8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1PB0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2186,"ST",1,"GMC",1,"1FK70225AK711PB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1PB2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2330,"ST",1,"GMC",1,"1FK70225AK711PB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1PB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2256,"ST",1,"GMC",1,"1FK70225AK711PB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1PB5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2399,"ST",1,"GMC",1,"1FK70225AK711PB5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1PB8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2553,"ST",1,"GMC",1,"1FK70225AK711PB8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1PG0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1718,"ST",1,"GMC",1,"1FK70225AK711PG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1PG2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1862,"ST",1,"GMC",1,"1FK70225AK711PG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1PG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1788,"ST",1,"GMC",1,"1FK70225AK711PG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1PG5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1931,"ST",1,"GMC",1,"1FK70225AK711PG5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1PG8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2084,"ST",1,"GMC",1,"1FK70225AK711PG8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1PH0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2050,"ST",1,"GMC",1,"1FK70225AK711PH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1PH2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2194,"ST",1,"GMC",1,"1FK70225AK711PH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1PH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2120,"ST",1,"GMC",1,"1FK70225AK711PH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1PH5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2263,"ST",1,"GMC",1,"1FK70225AK711PH5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1PH8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2417,"ST",1,"GMC",1,"1FK70225AK711PH8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1UA0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1850,"ST",1,"GMC",1,"1FK70225AK711UA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1UA2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1994,"ST",1,"GMC",1,"1FK70225AK711UA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1UA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1920,"ST",1,"GMC",1,"1FK70225AK711UA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1UA5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2063,"ST",1,"GMC",1,"1FK70225AK711UA5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1UA8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2217,"ST",1,"GMC",1,"1FK70225AK711UA8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1UB0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2186,"ST",1,"GMC",1,"1FK70225AK711UB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1UB2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2330,"ST",1,"GMC",1,"1FK70225AK711UB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1UB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2256,"ST",1,"GMC",1,"1FK70225AK711UB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1UB5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2399,"ST",1,"GMC",1,"1FK70225AK711UB5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1UB8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2553,"ST",1,"GMC",1,"1FK70225AK711UB8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1UG0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1718,"ST",1,"GMC",1,"1FK70225AK711UG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1UG2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1862,"ST",1,"GMC",1,"1FK70225AK711UG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1UG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1788,"ST",1,"GMC",1,"1FK70225AK711UG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1UG5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1931,"ST",1,"GMC",1,"1FK70225AK711UG5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1UG8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2084,"ST",1,"GMC",1,"1FK70225AK711UG8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1UH0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2050,"ST",1,"GMC",1,"1FK70225AK711UH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1UH2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2194,"ST",1,"GMC",1,"1FK70225AK711UH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1UH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2120,"ST",1,"GMC",1,"1FK70225AK711UH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1UH5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2263,"ST",1,"GMC",1,"1FK70225AK711UH5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1UH8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2417,"ST",1,"GMC",1,"1FK70225AK711UH8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1AA0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2355,"ST",1,"GMC",1,"1FK70225AK741AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1AA2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2498,"ST",1,"GMC",1,"1FK70225AK741AA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1AA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2425,"ST",1,"GMC",1,"1FK70225AK741AA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1AA5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2568,"ST",1,"GMC",1,"1FK70225AK741AA5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1AB0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2691,"ST",1,"GMC",1,"1FK70225AK741AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1AB2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2834,"ST",1,"GMC",1,"1FK70225AK741AB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1AB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2760,"ST",1,"GMC",1,"1FK70225AK741AB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1AB5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2904,"ST",1,"GMC",1,"1FK70225AK741AB5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1AG0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2223,"ST",1,"GMC",1,"1FK70225AK741AG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1AG2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2366,"ST",1,"GMC",1,"1FK70225AK741AG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1AG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2292,"ST",1,"GMC",1,"1FK70225AK741AG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1AG5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2436,"ST",1,"GMC",1,"1FK70225AK741AG5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1AH0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2555,"ST",1,"GMC",1,"1FK70225AK741AH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1AH2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2698,"ST",1,"GMC",1,"1FK70225AK741AH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1AH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2624,"ST",1,"GMC",1,"1FK70225AK741AH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1AH5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2768,"ST",1,"GMC",1,"1FK70225AK741AH5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1HA0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2949,"ST",1,"GMC",1,"1FK70225AK741HA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1HA2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",3093,"ST",1,"GMC",1,"1FK70225AK741HA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1HA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",3019,"ST",1,"GMC",1,"1FK70225AK741HA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1HA5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",3162,"ST",1,"GMC",1,"1FK70225AK741HA5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1HB0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",3285,"ST",1,"GMC",1,"1FK70225AK741HB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1HB2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",3429,"ST",1,"GMC",1,"1FK70225AK741HB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1HB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",3355,"ST",1,"GMC",1,"1FK70225AK741HB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1HB5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",3498,"ST",1,"GMC",1,"1FK70225AK741HB5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1HG0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2817,"ST",1,"GMC",1,"1FK70225AK741HG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1HG2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2961,"ST",1,"GMC",1,"1FK70225AK741HG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1HG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2887,"ST",1,"GMC",1,"1FK70225AK741HG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1HG5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",3030,"ST",1,"GMC",1,"1FK70225AK741HG5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1HH0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",3149,"ST",1,"GMC",1,"1FK70225AK741HH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1HH2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",3293,"ST",1,"GMC",1,"1FK70225AK741HH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1HH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",3219,"ST",1,"GMC",1,"1FK70225AK741HH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1HH5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",3362,"ST",1,"GMC",1,"1FK70225AK741HH5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1SA0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1481,"ST",1,"GMC",1,"1FK70225AK741SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1SA2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1624,"ST",1,"GMC",1,"1FK70225AK741SA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1SA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1550,"ST",1,"GMC",1,"1FK70225AK741SA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1SA5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1694,"ST",1,"GMC",1,"1FK70225AK741SA5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1SB0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1817,"ST",1,"GMC",1,"1FK70225AK741SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1SB2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1960,"ST",1,"GMC",1,"1FK70225AK741SB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1SB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1886,"ST",1,"GMC",1,"1FK70225AK741SB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1SB5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2030,"ST",1,"GMC",1,"1FK70225AK741SB5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1SG0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1348,"ST",1,"GMC",1,"1FK70225AK741SG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1SG2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1492,"ST",1,"GMC",1,"1FK70225AK741SG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1SG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1418,"ST",1,"GMC",1,"1FK70225AK741SG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1SG5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1561,"ST",1,"GMC",1,"1FK70225AK741SG5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1SH0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1681,"ST",1,"GMC",1,"1FK70225AK741SH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1SH2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1824,"ST",1,"GMC",1,"1FK70225AK741SH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1SH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1750,"ST",1,"GMC",1,"1FK70225AK741SH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1SH5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1894,"ST",1,"GMC",1,"1FK70225AK741SH5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1TA0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1481,"ST",1,"GMC",1,"1FK70225AK741TA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1TA2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1624,"ST",1,"GMC",1,"1FK70225AK741TA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1TA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1550,"ST",1,"GMC",1,"1FK70225AK741TA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1TA5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1694,"ST",1,"GMC",1,"1FK70225AK741TA5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1TB0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1817,"ST",1,"GMC",1,"1FK70225AK741TB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1TB2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1960,"ST",1,"GMC",1,"1FK70225AK741TB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1TB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1886,"ST",1,"GMC",1,"1FK70225AK741TB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1TB5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2030,"ST",1,"GMC",1,"1FK70225AK741TB5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1TG0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1348,"ST",1,"GMC",1,"1FK70225AK741TG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1TG2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1492,"ST",1,"GMC",1,"1FK70225AK741TG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1TG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1418,"ST",1,"GMC",1,"1FK70225AK741TG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1TG5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1561,"ST",1,"GMC",1,"1FK70225AK741TG5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1TH0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1681,"ST",1,"GMC",1,"1FK70225AK741TH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1TH2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1824,"ST",1,"GMC",1,"1FK70225AK741TH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1TH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1750,"ST",1,"GMC",1,"1FK70225AK741TH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1TH5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1894,"ST",1,"GMC",1,"1FK70225AK741TH5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-7TG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, 0.85Nm , 100K, 6000rpm, 0.38kW Naturally cooled Bare cable end 0.5m Outlet directions NDE with connector size 1 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1736,"ST",1,"GMC",1,"1FK70225AK747TG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-8HG0","SIMOTICS S Synchronous servo motor 1FK7 Compact, 0.85Nm 100K, 6000rpm, 0.38kW Naturally cooled Bare cable end 0.5m Outlet directions DE with connector size 1 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",3135,"ST",1,"GMC",1,"1FK70225AK748HG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-8HH2","SIMOTICS S Synchronous servo motor 1FK7 Compact, 0.85Nm 100K, 6000rpm, 0.38kW Naturally cooled Bare cable end 0.5m Outlet directions DE with connector size 1 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",3611,"ST",1,"GMC",1,"1FK70225AK748HH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7024-5AK71-1LB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, 1.1Nm 100K, 6000rpm, 0.50kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Â° absolute encoder 512 S/R (encoder A-512) with DRIVE-CLiQ interface Derating 10% due to absolute encoder Shaft with feather key tolerance N with holding brake Degree of protection IP64 paint finish RAL7016",3950,"ST",1,"GMC",1,"1FK70245AK711LB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7024-5AK71-1LG0","SIMOTICS S Synchronous servo motor 1FK7 Compact, 1.1Nm 100K, 6000rpm, 0.50kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Â° absolute encoder 512 S/R (encoder A-512) with DRIVE-CLiQ interface Derating 10% due to absolute encoder Smooth shaft Tolerance N without holding brake Degree of protection IP65",3412,"ST",1,"GMC",1,"1FK70245AK711LG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7024-5AK71-1LG2","SIMOTICS S Synchronous servo motor 1FK7 Compact, 1.1Nm 100K, 6000rpm, 0.50kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Â° absolute encoder 512 S/R (encoder A-512) with DRIVE-CLiQ interface Derating 10% due to absolute encoder Smooth shaft Tolerance N without holding brake Degree of protection IP65 DE flange IP67",3556,"ST",1,"GMC",1,"1FK70245AK711LG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1BA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) shaft with feather key, tolerance N without holding brake degree of protection IP64",2679,"ST",1,"GMC",1,"1FK70322AF211BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1BA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65",2815,"ST",1,"GMC",1,"1FK70322AF211BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1BA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65, DE flange IP67",2815,"ST",1,"GMC",1,"1FK70322AF211BA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1BB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) shaft with feather key, tolerance N with holding brake degree of protection IP64",2999,"ST",1,"GMC",1,"1FK70322AF211BB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1BB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65",3135,"ST",1,"GMC",1,"1FK70322AF211BB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1BB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65, DE flange IP67",3135,"ST",1,"GMC",1,"1FK70322AF211BB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1BG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N without holding brake degree of protection IP64",2553,"ST",1,"GMC",1,"1FK70322AF211BG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1BG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N without holding brake degree of protection IP65",2689,"ST",1,"GMC",1,"1FK70322AF211BG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1BG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N without holding brake degree of protection IP65, DE flange IP67",2689,"ST",1,"GMC",1,"1FK70322AF211BG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1BH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N with holding brake degree of protection IP64",2869,"ST",1,"GMC",1,"1FK70322AF211BH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1BH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N with holding brake degree of protection IP65",3006,"ST",1,"GMC",1,"1FK70322AF211BH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1BH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N with holding brake degree of protection IP65, DE flange IP67",3006,"ST",1,"GMC",1,"1FK70322AF211BH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1CA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N without holding brake degree of protection IP64",3218,"ST",1,"GMC",1,"1FK70322AF211CA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1CA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65",3355,"ST",1,"GMC",1,"1FK70322AF211CA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1CA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65, DE flange IP67",3355,"ST",1,"GMC",1,"1FK70322AF211CA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1CB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N with holding brake degree of protection IP64",3538,"ST",1,"GMC",1,"1FK70322AF211CB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1CB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65",3675,"ST",1,"GMC",1,"1FK70322AF211CB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1CB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65, DE flange IP67",3675,"ST",1,"GMC",1,"1FK70322AF211CB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1CG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N without holding brake degree of protection IP64",3092,"ST",1,"GMC",1,"1FK70322AF211CG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1CG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N without holding brake degree of protection IP65",3229,"ST",1,"GMC",1,"1FK70322AF211CG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1CG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N without holding brake degree of protection IP65, DE flange IP67",3229,"ST",1,"GMC",1,"1FK70322AF211CG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1CH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N with holding brake degree of protection IP64",3408,"ST",1,"GMC",1,"1FK70322AF211CH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1CH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N with holding brake degree of protection IP65",3545,"ST",1,"GMC",1,"1FK70322AF211CH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1CH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N with holding brake degree of protection IP65, DE flange IP67",3545,"ST",1,"GMC",1,"1FK70322AF211CH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1DA0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.31kW; UDC=300V; M0=1.2Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2796,"ST",1,"GMC",1,"1FK70322AF211DA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1DA1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.31kW; UDC=300V; M0=1.2Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2930,"ST",1,"GMC",1,"1FK70322AF211DA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1DB0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.31kW; UDC=300V; M0=1.2Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",3116,"ST",1,"GMC",1,"1FK70322AF211DB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1DG0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.31kW; UDC=300V; M0=1.2Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2670,"ST",1,"GMC",1,"1FK70322AF211DG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1DH0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.31kW; UDC=300V; M0=1.2Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2986,"ST",1,"GMC",1,"1FK70322AF211DH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1FA0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.31kW; UDC=300V; M0=1.2Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",3335,"ST",1,"GMC",1,"1FK70322AF211FA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1FB0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.31kW; UDC=300V; M0=1.2Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",3655,"ST",1,"GMC",1,"1FK70322AF211FB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1FB1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.31kW; UDC=300V; M0=1.2Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",3789,"ST",1,"GMC",1,"1FK70322AF211FB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1FG0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.31kW; UDC=300V; M0=1.2Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",3209,"ST",1,"GMC",1,"1FK70322AF211FG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1FH0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.31kW; UDC=300V; M0=1.2Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",3526,"ST",1,"GMC",1,"1FK70322AF211FH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1FH2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.31kW; UDC=300V; M0=1.2Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",3660,"ST",1,"GMC",1,"1FK70322AF211FH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1PA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, type of protection IP64",1823,"ST",1,"GMC",1,"1FK70322AF211PA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1PA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, type of protection IP65",1959,"ST",1,"GMC",1,"1FK70322AF211PA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1PA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, degree of protection IP65 DE flange IP67",1959,"ST",1,"GMC",1,"1FK70322AF211PA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1PB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, type of protection IP64",2142,"ST",1,"GMC",1,"1FK70322AF211PB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1PB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, type of protection IP65",2279,"ST",1,"GMC",1,"1FK70322AF211PB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1PB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, degree of protection IP65 DE flange IP67",2279,"ST",1,"GMC",1,"1FK70322AF211PB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1PG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, type of protection IP64",1697,"ST",1,"GMC",1,"1FK70322AF211PG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1PG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, type of protection IP65",1833,"ST",1,"GMC",1,"1FK70322AF211PG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1PG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, degree of protection IP65 DE flange IP67",1833,"ST",1,"GMC",1,"1FK70322AF211PG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1PH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, type of protection IP64",2013,"ST",1,"GMC",1,"1FK70322AF211PH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1PH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, type of protection IP65",2150,"ST",1,"GMC",1,"1FK70322AF211PH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1PH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, degree of protection IP65 DE flange IP67",2150,"ST",1,"GMC",1,"1FK70322AF211PH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1QA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N without holding brake degree of protection IP64",1973,"ST",1,"GMC",1,"1FK70322AF211QA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1QA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65",2110,"ST",1,"GMC",1,"1FK70322AF211QA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1QA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65, DE flange IP67",2110,"ST",1,"GMC",1,"1FK70322AF211QA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1QB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N with holding brake degree of protection IP64",2293,"ST",1,"GMC",1,"1FK70322AF211QB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1QB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65",2430,"ST",1,"GMC",1,"1FK70322AF211QB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1QB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65, DE flange IP67",2430,"ST",1,"GMC",1,"1FK70322AF211QB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1QG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UZK=300V M0=1.2Nm (100K); NN=3000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 power connector rotatable absolute encoder single-turn 20-bit with Drive-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N without holding brake degree of protection IP64",1847,"ST",1,"GMC",1,"1FK70322AF211QG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1QG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N without holding brake degree of protection IP65",1984,"ST",1,"GMC",1,"1FK70322AF211QG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1QG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N without holding brake degree of protection IP65, DE flange IP67",1984,"ST",1,"GMC",1,"1FK70322AF211QG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1QH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N with holding brake degree of protection IP64",2164,"ST",1,"GMC",1,"1FK70322AF211QH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1QH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N with holding brake degree of protection IP65",2300,"ST",1,"GMC",1,"1FK70322AF211QH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1QH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N with holding brake degree of protection IP65, DE flange IP67",2300,"ST",1,"GMC",1,"1FK70322AF211QH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1RA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N without holding brake degree of protection IP64",2520,"ST",1,"GMC",1,"1FK70322AF211RA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1RA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65",2656,"ST",1,"GMC",1,"1FK70322AF211RA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1RA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65, DE flange IP67",2656,"ST",1,"GMC",1,"1FK70322AF211RA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1RB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N with holding brake degree of protection IP64",2840,"ST",1,"GMC",1,"1FK70322AF211RB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1RB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65",2976,"ST",1,"GMC",1,"1FK70322AF211RB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1RB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65, DE flange IP67",2976,"ST",1,"GMC",1,"1FK70322AF211RB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1RG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N without holding brake degree of protection IP64",2394,"ST",1,"GMC",1,"1FK70322AF211RG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1RG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N without holding brake degree of protection IP65",2530,"ST",1,"GMC",1,"1FK70322AF211RG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1RG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N without holding brake degree of protection IP65, DE flange IP67",2530,"ST",1,"GMC",1,"1FK70322AF211RG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1RH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N with holding brake degree of protection IP64",2710,"ST",1,"GMC",1,"1FK70322AF211RH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1RH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N with holding brake degree of protection IP65",2847,"ST",1,"GMC",1,"1FK70322AF211RH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1RH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N with holding brake degree of protection IP65, DE flange IP67",2847,"ST",1,"GMC",1,"1FK70322AF211RH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1UA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, type of protection IP64",1823,"ST",1,"GMC",1,"1FK70322AF211UA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1UA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, type of protection IP65",1959,"ST",1,"GMC",1,"1FK70322AF211UA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1UA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, degree of protection IP65 DE flange IP67",1959,"ST",1,"GMC",1,"1FK70322AF211UA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1UB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, type of protection IP64",2142,"ST",1,"GMC",1,"1FK70322AF211UB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1UB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, type of protection IP65",2279,"ST",1,"GMC",1,"1FK70322AF211UB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1UB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, degree of protection IP65 DE flange IP67",2279,"ST",1,"GMC",1,"1FK70322AF211UB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1UG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, type of protection IP64",1697,"ST",1,"GMC",1,"1FK70322AF211UG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1UG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, type of protection IP65",1833,"ST",1,"GMC",1,"1FK70322AF211UG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1UG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, degree of protection IP65 DE flange IP67",1833,"ST",1,"GMC",1,"1FK70322AF211UG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1UH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, type of protection IP64",2013,"ST",1,"GMC",1,"1FK70322AF211UH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1UH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, type of protection IP65",2150,"ST",1,"GMC",1,"1FK70322AF211UH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1UH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, degree of protection IP65 DE flange IP67",2150,"ST",1,"GMC",1,"1FK70322AF211UH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1EH2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.31kW; UDC=300V; M0=1.2Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",3194,"ST",1,"GMC",1,"1FK70322AF241EH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1SA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N without holding brake degree of protection IP64",1470,"ST",1,"GMC",1,"1FK70322AF241SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1SA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N without holding brake degree of protection IP65",1607,"ST",1,"GMC",1,"1FK70322AF241SA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1SA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N without holding brake degree of protection IP65, DE flange IP67",1607,"ST",1,"GMC",1,"1FK70322AF241SA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1SB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N with holding brake degree of protection IP64",1790,"ST",1,"GMC",1,"1FK70322AF241SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1SB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N with holding brake degree of protection IP65",1927,"ST",1,"GMC",1,"1FK70322AF241SB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1SB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N with holding brake degree of protection IP65, DE flange IP67",1927,"ST",1,"GMC",1,"1FK70322AF241SB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1SG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N without holding brake, type of protection IP64",1344,"ST",1,"GMC",1,"1FK70322AF241SG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1SG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N without holding brake, type of protection IP65",1481,"ST",1,"GMC",1,"1FK70322AF241SG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1SG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N without holding brake, type of protection IP65 DE flange IP67",1481,"ST",1,"GMC",1,"1FK70322AF241SG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1SH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N with holding brake, type of protection IP64",1661,"ST",1,"GMC",1,"1FK70322AF241SH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1SH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N with holding brake, type of protection IP65",1797,"ST",1,"GMC",1,"1FK70322AF241SH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1SH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N with holding brake, degree of protection IP65 DE Flange IP67",1797,"ST",1,"GMC",1,"1FK70322AF241SH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1TA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N without holding brake degree of protection IP64",1470,"ST",1,"GMC",1,"1FK70322AF241TA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1TA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N without holding brake degree of protection IP65",1607,"ST",1,"GMC",1,"1FK70322AF241TA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1TA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N without holding brake degree of protection IP65, DE flange IP67",1607,"ST",1,"GMC",1,"1FK70322AF241TA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1TB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N with holding brake degree of protection IP64",1790,"ST",1,"GMC",1,"1FK70322AF241TB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1TB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N with holding brake degree of protection IP65",1927,"ST",1,"GMC",1,"1FK70322AF241TB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1TB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N with holding brake degree of protection IP65, DE flange IP67",1927,"ST",1,"GMC",1,"1FK70322AF241TB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1TG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N without holding brake, type of protection IP64",1344,"ST",1,"GMC",1,"1FK70322AF241TG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1TG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N without holding brake, type of protection IP65",1481,"ST",1,"GMC",1,"1FK70322AF241TG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1TG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N without holding brake, type of protection IP65 DE flange IP67",1481,"ST",1,"GMC",1,"1FK70322AF241TG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1TH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N with holding brake, type of protection IP64",1661,"ST",1,"GMC",1,"1FK70322AF241TH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1TH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N with holding brake, type of protection IP65",1797,"ST",1,"GMC",1,"1FK70322AF241TH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1TH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N with holding brake, degree of protection IP65 DE Flange IP67",1797,"ST",1,"GMC",1,"1FK70322AF241TH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1BA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) Shaft with feather key, tolerance N without Holding brake, degree of protection IP64",2679,"ST",1,"GMC",1,"1FK70322AK711BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1BA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) Shaft with feather key, tolerance N without Holding brake, degree of protection IP65",2815,"ST",1,"GMC",1,"1FK70322AK711BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1BA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) Shaft with feather key, tolerance N without Holding brake, degree of protection IP65 DE flange IP67",2815,"ST",1,"GMC",1,"1FK70322AK711BA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1BB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) Shaft with feather key, tolerance N with Holding brake, degree of protection IP64",2999,"ST",1,"GMC",1,"1FK70322AK711BB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1BB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) Shaft with feather key, tolerance N with Holding brake, degree of protection IP65",3135,"ST",1,"GMC",1,"1FK70322AK711BB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1BB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) Shaft with feather key, tolerance N with Holding brake, degree of protection IP65 DE flange IP67",3135,"ST",1,"GMC",1,"1FK70322AK711BB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1BG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N without Holding brake, degree of protection IP64",2553,"ST",1,"GMC",1,"1FK70322AK711BG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1BG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N without Holding brake, degree of protection IP65",2689,"ST",1,"GMC",1,"1FK70322AK711BG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1BG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N without Holding brake, degree of protection IP65 DE flange IP67",2689,"ST",1,"GMC",1,"1FK70322AK711BG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1BH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N with Holding brake, degree of protection IP64",2869,"ST",1,"GMC",1,"1FK70322AK711BH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1BH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N with Holding brake, degree of protection IP65",3006,"ST",1,"GMC",1,"1FK70322AK711BH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1BH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N with Holding brake, degree of protection IP65 DE flange IP67",3006,"ST",1,"GMC",1,"1FK70322AK711BH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1CA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 24 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) Shaft with feather key, tolerance N without Holding brake, degree of protection IP64",3218,"ST",1,"GMC",1,"1FK70322AK711CA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1CA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 24 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) Shaft with feather key, tolerance N without Holding brake, degree of protection IP65",3355,"ST",1,"GMC",1,"1FK70322AK711CA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1CA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 24 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) Shaft with feather key, tolerance N without Holding brake, degree of protection IP65 DE flange IP67",3355,"ST",1,"GMC",1,"1FK70322AK711CA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1CB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 24 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) Shaft with feather key, tolerance N with Holding brake, degree of protection IP64",3538,"ST",1,"GMC",1,"1FK70322AK711CB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1CB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 24 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) Shaft with feather key, tolerance N with Holding brake, degree of protection IP65",3675,"ST",1,"GMC",1,"1FK70322AK711CB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1CB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 24 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) Shaft with feather key, tolerance N with Holding brake, degree of protection IP65 DE flange IP67",3675,"ST",1,"GMC",1,"1FK70322AK711CB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1CG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 24 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N without Holding brake, degree of protection IP64",3092,"ST",1,"GMC",1,"1FK70322AK711CG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1CG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 24 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N without Holding brake, degree of protection IP65",3229,"ST",1,"GMC",1,"1FK70322AK711CG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1CG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 24 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N without Holding brake, degree of protection IP65 DE flange IP67",3229,"ST",1,"GMC",1,"1FK70322AK711CG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1CH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 24 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N with Holding brake, degree of protection IP64",3408,"ST",1,"GMC",1,"1FK70322AK711CH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1CH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 24 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N with Holding brake, degree of protection IP65",3545,"ST",1,"GMC",1,"1FK70322AK711CH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1CH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 24 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N with Holding brake, degree of protection IP65 DE flange IP67",3545,"ST",1,"GMC",1,"1FK70322AK711CH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1DA0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2796,"ST",1,"GMC",1,"1FK70322AK711DA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1DA1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2930,"ST",1,"GMC",1,"1FK70322AK711DA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1DB0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",3116,"ST",1,"GMC",1,"1FK70322AK711DB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1DG0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2670,"ST",1,"GMC",1,"1FK70322AK711DG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1DG1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2804,"ST",1,"GMC",1,"1FK70322AK711DG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1DG2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2804,"ST",1,"GMC",1,"1FK70322AK711DG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1DH0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2986,"ST",1,"GMC",1,"1FK70322AK711DH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1DH1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",3120,"ST",1,"GMC",1,"1FK70322AK711DH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1FA0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",3335,"ST",1,"GMC",1,"1FK70322AK711FA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1FA2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",3469,"ST",1,"GMC",1,"1FK70322AK711FA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1FB0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",3655,"ST",1,"GMC",1,"1FK70322AK711FB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1FB1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",3789,"ST",1,"GMC",1,"1FK70322AK711FB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1FG0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",3209,"ST",1,"GMC",1,"1FK70322AK711FG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1FG1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",3343,"ST",1,"GMC",1,"1FK70322AK711FG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1FH0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",3526,"ST",1,"GMC",1,"1FK70322AK711FH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1FH1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",3660,"ST",1,"GMC",1,"1FK70322AK711FH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1PA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, type of protection IP64",1823,"ST",1,"GMC",1,"1FK70322AK711PA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1PA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, type of protection IP65",1959,"ST",1,"GMC",1,"1FK70322AK711PA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1PA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, degree of protection IP65 DE flange IP67",1959,"ST",1,"GMC",1,"1FK70322AK711PA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1PB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, type of protection IP64",2142,"ST",1,"GMC",1,"1FK70322AK711PB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1PB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, type of protection IP65",2279,"ST",1,"GMC",1,"1FK70322AK711PB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1PB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, degree of protection IP65 DE flange IP67",2279,"ST",1,"GMC",1,"1FK70322AK711PB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1PG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, type of protection IP64",1697,"ST",1,"GMC",1,"1FK70322AK711PG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1PG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, type of protection IP65",1833,"ST",1,"GMC",1,"1FK70322AK711PG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1PG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, degree of protection IP65 DE flange IP67",1833,"ST",1,"GMC",1,"1FK70322AK711PG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1PH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, type of protection IP64",2013,"ST",1,"GMC",1,"1FK70322AK711PH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1PH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, type of protection IP65",2150,"ST",1,"GMC",1,"1FK70322AK711PH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1PH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, degree of protection IP65 DE flange IP67",2150,"ST",1,"GMC",1,"1FK70322AK711PH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1QA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) Shaft with feather key, tolerance N without Holding brake, degree of protection IP64",1973,"ST",1,"GMC",1,"1FK70322AK711QA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1QA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) Shaft with feather key, tolerance N without Holding brake, degree of protection IP65",2110,"ST",1,"GMC",1,"1FK70322AK711QA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1QA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) Shaft with feather key, tolerance N without Holding brake, degree of protection IP65 DE flange IP67",2110,"ST",1,"GMC",1,"1FK70322AK711QA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1QB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) Shaft with feather key, tolerance N with Holding brake, degree of protection IP64",2293,"ST",1,"GMC",1,"1FK70322AK711QB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1QB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) Shaft with feather key, tolerance N with Holding brake, degree of protection IP65",2430,"ST",1,"GMC",1,"1FK70322AK711QB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1QB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) Shaft with feather key, tolerance N with Holding brake, degree of protection IP65 DE flange IP67",2430,"ST",1,"GMC",1,"1FK70322AK711QB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1QG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N without Holding brake, degree of protection IP64",1847,"ST",1,"GMC",1,"1FK70322AK711QG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1QG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N without Holding brake, degree of protection IP65",1984,"ST",1,"GMC",1,"1FK70322AK711QG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1QG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N without Holding brake, degree of protection IP65 DE flange IP67",1984,"ST",1,"GMC",1,"1FK70322AK711QG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1QH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N with Holding brake, degree of protection IP64",2164,"ST",1,"GMC",1,"1FK70322AK711QH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1QH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N with Holding brake, degree of protection IP65",2300,"ST",1,"GMC",1,"1FK70322AK711QH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1QH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N with Holding brake, degree of protection IP65 DE flange IP67",2300,"ST",1,"GMC",1,"1FK70322AK711QH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1RA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 20 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) Shaft with feather key, tolerance N without Holding brake, degree of protection IP64",2520,"ST",1,"GMC",1,"1FK70322AK711RA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1RA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 20 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) Shaft with feather key, tolerance N without Holding brake, degree of protection IP65",2656,"ST",1,"GMC",1,"1FK70322AK711RA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1RA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 20 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) Shaft with feather key, tolerance N without Holding brake, degree of protection IP65 DE flange IP67",2656,"ST",1,"GMC",1,"1FK70322AK711RA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1RB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 20 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) Shaft with feather key, tolerance N with Holding brake, degree of protection IP64",2840,"ST",1,"GMC",1,"1FK70322AK711RB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1RB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 20 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) Shaft with feather key, tolerance N with Holding brake, degree of protection IP65",2976,"ST",1,"GMC",1,"1FK70322AK711RB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1RB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 20 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) Shaft with feather key, tolerance N with Holding brake, degree of protection IP65 DE flange IP67",2976,"ST",1,"GMC",1,"1FK70322AK711RB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1RG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 20 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N without Holding brake, degree of protection IP64",2394,"ST",1,"GMC",1,"1FK70322AK711RG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1RG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 20 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N without Holding brake, degree of protection IP65",2530,"ST",1,"GMC",1,"1FK70322AK711RG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1RG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 20 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N without Holding brake, degree of protection IP65 DE flange IP67",2530,"ST",1,"GMC",1,"1FK70322AK711RG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1RH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 20 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N with Holding brake, degree of protection IP64",2710,"ST",1,"GMC",1,"1FK70322AK711RH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1RH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 20 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N with Holding brake, degree of protection IP65",2847,"ST",1,"GMC",1,"1FK70322AK711RH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1RH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 20 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N with Holding brake, degree of protection IP65 DE flange IP67",2847,"ST",1,"GMC",1,"1FK70322AK711RH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1UA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, type of protection IP64",1823,"ST",1,"GMC",1,"1FK70322AK711UA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1UA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, type of protection IP65",1959,"ST",1,"GMC",1,"1FK70322AK711UA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1UA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, degree of protection IP65 DE flange IP67",1959,"ST",1,"GMC",1,"1FK70322AK711UA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1UB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, type of protection IP64",2142,"ST",1,"GMC",1,"1FK70322AK711UB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1UB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, type of protection IP65",2279,"ST",1,"GMC",1,"1FK70322AK711UB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1UB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, degree of protection IP65 DE flange IP67",2279,"ST",1,"GMC",1,"1FK70322AK711UB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1UG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, type of protection IP64",1697,"ST",1,"GMC",1,"1FK70322AK711UG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1UG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, type of protection IP65",1833,"ST",1,"GMC",1,"1FK70322AK711UG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1UG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, degree of protection IP65 DE flange IP67",1833,"ST",1,"GMC",1,"1FK70322AK711UG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1UH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, type of protection IP64",2013,"ST",1,"GMC",1,"1FK70322AK711UH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1UH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, type of protection IP65",2150,"ST",1,"GMC",1,"1FK70322AK711UH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1UH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, degree of protection IP65 DE flange IP67",2150,"ST",1,"GMC",1,"1FK70322AK711UH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1AA0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2327,"ST",1,"GMC",1,"1FK70322AK741AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1AA1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2460,"ST",1,"GMC",1,"1FK70322AK741AA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1AA2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2460,"ST",1,"GMC",1,"1FK70322AK741AA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1AB0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2646,"ST",1,"GMC",1,"1FK70322AK741AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1AB1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2780,"ST",1,"GMC",1,"1FK70322AK741AB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1AB2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2780,"ST",1,"GMC",1,"1FK70322AK741AB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1AG0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2201,"ST",1,"GMC",1,"1FK70322AK741AG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1AG1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2334,"ST",1,"GMC",1,"1FK70322AK741AG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1AG2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2334,"ST",1,"GMC",1,"1FK70322AK741AG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1AH0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2517,"ST",1,"GMC",1,"1FK70322AK741AH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1AH1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2651,"ST",1,"GMC",1,"1FK70322AK741AH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1AH2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2651,"ST",1,"GMC",1,"1FK70322AK741AH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1EA0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2869,"ST",1,"GMC",1,"1FK70322AK741EA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1EA1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",3003,"ST",1,"GMC",1,"1FK70322AK741EA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1EA2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",3003,"ST",1,"GMC",1,"1FK70322AK741EA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1EB0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",3189,"ST",1,"GMC",1,"1FK70322AK741EB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1EB1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",3323,"ST",1,"GMC",1,"1FK70322AK741EB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1EB2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",3323,"ST",1,"GMC",1,"1FK70322AK741EB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1EG0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2743,"ST",1,"GMC",1,"1FK70322AK741EG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1EG1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2877,"ST",1,"GMC",1,"1FK70322AK741EG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1EG2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2877,"ST",1,"GMC",1,"1FK70322AK741EG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1EH0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",3060,"ST",1,"GMC",1,"1FK70322AK741EH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1EH1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",3194,"ST",1,"GMC",1,"1FK70322AK741EH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1EH2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",3194,"ST",1,"GMC",1,"1FK70322AK741EH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1SA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N without holding brake degree of protection IP64",1470,"ST",1,"GMC",1,"1FK70322AK741SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1SA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N without holding brake degree of protection IP65",1607,"ST",1,"GMC",1,"1FK70322AK741SA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1SA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N without holding brake degree of protection IP65, DE flange IP67",1607,"ST",1,"GMC",1,"1FK70322AK741SA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1SB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N with holding brake degree of protection IP64",1790,"ST",1,"GMC",1,"1FK70322AK741SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1SB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N with holding brake degree of protection IP65",1927,"ST",1,"GMC",1,"1FK70322AK741SB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1SB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N with holding brake degree of protection IP65, DE flange IP67",1927,"ST",1,"GMC",1,"1FK70322AK741SB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1SG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N without holding brake, type of protection IP64",1344,"ST",1,"GMC",1,"1FK70322AK741SG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1SG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N without holding brake, type of protection IP65",1481,"ST",1,"GMC",1,"1FK70322AK741SG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1SG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N without holding brake, type of protection IP65 DE flange IP67",1481,"ST",1,"GMC",1,"1FK70322AK741SG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1SH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N with holding brake, type of protection IP64",1661,"ST",1,"GMC",1,"1FK70322AK741SH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1SH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N with holding brake, type of protection IP65",1797,"ST",1,"GMC",1,"1FK70322AK741SH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1SH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N with holding brake, degree of protection IP65 DE flange IP67",1797,"ST",1,"GMC",1,"1FK70322AK741SH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1TA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N without holding brake degree of protection IP64",1470,"ST",1,"GMC",1,"1FK70322AK741TA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1TA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N without holding brake degree of protection IP65",1607,"ST",1,"GMC",1,"1FK70322AK741TA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1TA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N without holding brake degree of protection IP65, DE flange IP67",1607,"ST",1,"GMC",1,"1FK70322AK741TA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1TB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N with holding brake degree of protection IP64",1790,"ST",1,"GMC",1,"1FK70322AK741TB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1TB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N with holding brake degree of protection IP65",1927,"ST",1,"GMC",1,"1FK70322AK741TB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1TB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N with holding brake degree of protection IP65, DE flange IP67",1927,"ST",1,"GMC",1,"1FK70322AK741TB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1TG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N without holding brake, type of protection IP64",1344,"ST",1,"GMC",1,"1FK70322AK741TG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1TG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N without holding brake, type of protection IP65",1481,"ST",1,"GMC",1,"1FK70322AK741TG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1TG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N without holding brake, type of protection IP65 DE flange IP67",1481,"ST",1,"GMC",1,"1FK70322AK741TG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1TH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N with holding brake, type of protection IP64",1661,"ST",1,"GMC",1,"1FK70322AK741TH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1TH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N with holding brake, type of protection IP65",1797,"ST",1,"GMC",1,"1FK70322AK741TH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1TH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N with holding brake, degree of protection IP65 DE flange IP67",1797,"ST",1,"GMC",1,"1FK70322AK741TH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1BA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2743,"ST",1,"GMC",1,"1FK70334CF211BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1BA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2877,"ST",1,"GMC",1,"1FK70334CF211BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1BA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2877,"ST",1,"GMC",1,"1FK70334CF211BA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1BB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",3063,"ST",1,"GMC",1,"1FK70334CF211BB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1BB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",3197,"ST",1,"GMC",1,"1FK70334CF211BB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1BB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",3197,"ST",1,"GMC",1,"1FK70334CF211BB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1BG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2617,"ST",1,"GMC",1,"1FK70334CF211BG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1BG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2751,"ST",1,"GMC",1,"1FK70334CF211BG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1BG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2751,"ST",1,"GMC",1,"1FK70334CF211BG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1BH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2934,"ST",1,"GMC",1,"1FK70334CF211BH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1BH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",3068,"ST",1,"GMC",1,"1FK70334CF211BH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1BH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",3068,"ST",1,"GMC",1,"1FK70334CF211BH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1CA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",3283,"ST",1,"GMC",1,"1FK70334CF211CA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1CA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",3417,"ST",1,"GMC",1,"1FK70334CF211CA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1CA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",3417,"ST",1,"GMC",1,"1FK70334CF211CA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1CB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",3603,"ST",1,"GMC",1,"1FK70334CF211CB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1CB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",3737,"ST",1,"GMC",1,"1FK70334CF211CB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1CB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",3737,"ST",1,"GMC",1,"1FK70334CF211CB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1CG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",3157,"ST",1,"GMC",1,"1FK70334CF211CG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1CG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",3291,"ST",1,"GMC",1,"1FK70334CF211CG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1CG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",3291,"ST",1,"GMC",1,"1FK70334CF211CG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1CH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",3473,"ST",1,"GMC",1,"1FK70334CF211CH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1CH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",3607,"ST",1,"GMC",1,"1FK70334CF211CH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1CH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",3607,"ST",1,"GMC",1,"1FK70334CF211CH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1DA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2860,"ST",1,"GMC",1,"1FK70334CF211DA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1DA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2994,"ST",1,"GMC",1,"1FK70334CF211DA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1DH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",3185,"ST",1,"GMC",1,"1FK70334CF211DH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1PA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1887,"ST",1,"GMC",1,"1FK70334CF211PA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1PA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2021,"ST",1,"GMC",1,"1FK70334CF211PA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1PA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2021,"ST",1,"GMC",1,"1FK70334CF211PA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1PB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2207,"ST",1,"GMC",1,"1FK70334CF211PB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1PB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2341,"ST",1,"GMC",1,"1FK70334CF211PB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1PB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2341,"ST",1,"GMC",1,"1FK70334CF211PB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1PG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1761,"ST",1,"GMC",1,"1FK70334CF211PG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1PG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1895,"ST",1,"GMC",1,"1FK70334CF211PG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1PG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1895,"ST",1,"GMC",1,"1FK70334CF211PG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1PH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2078,"ST",1,"GMC",1,"1FK70334CF211PH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1PH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2211,"ST",1,"GMC",1,"1FK70334CF211PH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1PH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2211,"ST",1,"GMC",1,"1FK70334CF211PH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1QA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2038,"ST",1,"GMC",1,"1FK70334CF211QA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1QA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2172,"ST",1,"GMC",1,"1FK70334CF211QA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1QA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2172,"ST",1,"GMC",1,"1FK70334CF211QA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1QB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2358,"ST",1,"GMC",1,"1FK70334CF211QB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1QB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2492,"ST",1,"GMC",1,"1FK70334CF211QB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1QB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2492,"ST",1,"GMC",1,"1FK70334CF211QB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1QG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1912,"ST",1,"GMC",1,"1FK70334CF211QG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1QG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2046,"ST",1,"GMC",1,"1FK70334CF211QG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1QG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2046,"ST",1,"GMC",1,"1FK70334CF211QG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1QH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2228,"ST",1,"GMC",1,"1FK70334CF211QH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1QH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2362,"ST",1,"GMC",1,"1FK70334CF211QH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1QH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2362,"ST",1,"GMC",1,"1FK70334CF211QH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1RA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2584,"ST",1,"GMC",1,"1FK70334CF211RA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1RA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2718,"ST",1,"GMC",1,"1FK70334CF211RA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1RA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2718,"ST",1,"GMC",1,"1FK70334CF211RA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1RB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2904,"ST",1,"GMC",1,"1FK70334CF211RB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1RB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",3038,"ST",1,"GMC",1,"1FK70334CF211RB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1RB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",3038,"ST",1,"GMC",1,"1FK70334CF211RB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1RG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2458,"ST",1,"GMC",1,"1FK70334CF211RG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1RG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2592,"ST",1,"GMC",1,"1FK70334CF211RG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1RG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2592,"ST",1,"GMC",1,"1FK70334CF211RG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1RH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2775,"ST",1,"GMC",1,"1FK70334CF211RH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1RH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2909,"ST",1,"GMC",1,"1FK70334CF211RH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1RH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2909,"ST",1,"GMC",1,"1FK70334CF211RH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1UA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1887,"ST",1,"GMC",1,"1FK70334CF211UA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1UA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2021,"ST",1,"GMC",1,"1FK70334CF211UA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1UA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2021,"ST",1,"GMC",1,"1FK70334CF211UA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1UB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2207,"ST",1,"GMC",1,"1FK70334CF211UB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1UB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2341,"ST",1,"GMC",1,"1FK70334CF211UB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1UB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2341,"ST",1,"GMC",1,"1FK70334CF211UB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1UG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1761,"ST",1,"GMC",1,"1FK70334CF211UG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1UG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1895,"ST",1,"GMC",1,"1FK70334CF211UG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1UG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1895,"ST",1,"GMC",1,"1FK70334CF211UG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1UH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2078,"ST",1,"GMC",1,"1FK70334CF211UH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1UH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2211,"ST",1,"GMC",1,"1FK70334CF211UH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1UH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2211,"ST",1,"GMC",1,"1FK70334CF211UH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF24-1AA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2525,"ST",1,"GMC",1,"1FK70334CF241AA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF24-1AH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2582,"ST",1,"GMC",1,"1FK70334CF241AH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF24-1EG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2808,"ST",1,"GMC",1,"1FK70334CF241EG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1BA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2743,"ST",1,"GMC",1,"1FK70334CK711BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1BA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2877,"ST",1,"GMC",1,"1FK70334CK711BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1BA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2877,"ST",1,"GMC",1,"1FK70334CK711BA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1BB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",3063,"ST",1,"GMC",1,"1FK70334CK711BB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1BB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",3197,"ST",1,"GMC",1,"1FK70334CK711BB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1BB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",3197,"ST",1,"GMC",1,"1FK70334CK711BB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1BG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2617,"ST",1,"GMC",1,"1FK70334CK711BG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1BG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2751,"ST",1,"GMC",1,"1FK70334CK711BG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1BG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2751,"ST",1,"GMC",1,"1FK70334CK711BG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1BH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2934,"ST",1,"GMC",1,"1FK70334CK711BH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1BH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",3068,"ST",1,"GMC",1,"1FK70334CK711BH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1BH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",3068,"ST",1,"GMC",1,"1FK70334CK711BH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1CA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",3283,"ST",1,"GMC",1,"1FK70334CK711CA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1CA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",3417,"ST",1,"GMC",1,"1FK70334CK711CA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1CA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",3417,"ST",1,"GMC",1,"1FK70334CK711CA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1CB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",3603,"ST",1,"GMC",1,"1FK70334CK711CB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1CB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",3737,"ST",1,"GMC",1,"1FK70334CK711CB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1CB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",3737,"ST",1,"GMC",1,"1FK70334CK711CB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1CG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",3157,"ST",1,"GMC",1,"1FK70334CK711CG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1CG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",3291,"ST",1,"GMC",1,"1FK70334CK711CG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1CG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",3291,"ST",1,"GMC",1,"1FK70334CK711CG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1CH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",3473,"ST",1,"GMC",1,"1FK70334CK711CH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1CH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",3607,"ST",1,"GMC",1,"1FK70334CK711CH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1CH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",3607,"ST",1,"GMC",1,"1FK70334CK711CH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1DA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2860,"ST",1,"GMC",1,"1FK70334CK711DA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1DA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2994,"ST",1,"GMC",1,"1FK70334CK711DA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1DG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2734,"ST",1,"GMC",1,"1FK70334CK711DG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1PA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1887,"ST",1,"GMC",1,"1FK70334CK711PA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1PA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2021,"ST",1,"GMC",1,"1FK70334CK711PA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1PA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2021,"ST",1,"GMC",1,"1FK70334CK711PA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1PB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2207,"ST",1,"GMC",1,"1FK70334CK711PB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1PB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2341,"ST",1,"GMC",1,"1FK70334CK711PB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1PB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2341,"ST",1,"GMC",1,"1FK70334CK711PB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1PG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1761,"ST",1,"GMC",1,"1FK70334CK711PG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1PG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1895,"ST",1,"GMC",1,"1FK70334CK711PG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1PG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1895,"ST",1,"GMC",1,"1FK70334CK711PG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1PH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2078,"ST",1,"GMC",1,"1FK70334CK711PH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1PH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2211,"ST",1,"GMC",1,"1FK70334CK711PH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1PH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2211,"ST",1,"GMC",1,"1FK70334CK711PH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1QA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2038,"ST",1,"GMC",1,"1FK70334CK711QA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1QA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2172,"ST",1,"GMC",1,"1FK70334CK711QA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1QA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2172,"ST",1,"GMC",1,"1FK70334CK711QA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1QB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2358,"ST",1,"GMC",1,"1FK70334CK711QB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1QB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2492,"ST",1,"GMC",1,"1FK70334CK711QB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1QB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2492,"ST",1,"GMC",1,"1FK70334CK711QB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1QG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1912,"ST",1,"GMC",1,"1FK70334CK711QG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1QG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2046,"ST",1,"GMC",1,"1FK70334CK711QG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1QG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2046,"ST",1,"GMC",1,"1FK70334CK711QG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1QH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2228,"ST",1,"GMC",1,"1FK70334CK711QH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1QH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2362,"ST",1,"GMC",1,"1FK70334CK711QH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1QH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2362,"ST",1,"GMC",1,"1FK70334CK711QH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1RA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2584,"ST",1,"GMC",1,"1FK70334CK711RA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1RA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2718,"ST",1,"GMC",1,"1FK70334CK711RA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1RA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2718,"ST",1,"GMC",1,"1FK70334CK711RA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1RB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2904,"ST",1,"GMC",1,"1FK70334CK711RB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1RB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",3038,"ST",1,"GMC",1,"1FK70334CK711RB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1RB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",3038,"ST",1,"GMC",1,"1FK70334CK711RB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1RG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2458,"ST",1,"GMC",1,"1FK70334CK711RG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1RG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2592,"ST",1,"GMC",1,"1FK70334CK711RG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1RG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2592,"ST",1,"GMC",1,"1FK70334CK711RG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1RH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2775,"ST",1,"GMC",1,"1FK70334CK711RH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1RH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2909,"ST",1,"GMC",1,"1FK70334CK711RH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1RH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2909,"ST",1,"GMC",1,"1FK70334CK711RH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1UA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1887,"ST",1,"GMC",1,"1FK70334CK711UA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1UA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2021,"ST",1,"GMC",1,"1FK70334CK711UA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1UA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2021,"ST",1,"GMC",1,"1FK70334CK711UA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1UB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2207,"ST",1,"GMC",1,"1FK70334CK711UB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1UB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2341,"ST",1,"GMC",1,"1FK70334CK711UB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1UB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2341,"ST",1,"GMC",1,"1FK70334CK711UB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1UG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1761,"ST",1,"GMC",1,"1FK70334CK711UG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1UG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1895,"ST",1,"GMC",1,"1FK70334CK711UG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1UG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1895,"ST",1,"GMC",1,"1FK70334CK711UG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1UH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2078,"ST",1,"GMC",1,"1FK70334CK711UH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1UH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2211,"ST",1,"GMC",1,"1FK70334CK711UH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1UH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2211,"ST",1,"GMC",1,"1FK70334CK711UH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK74-1AA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2391,"ST",1,"GMC",1,"1FK70334CK741AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK74-1AA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2525,"ST",1,"GMC",1,"1FK70334CK741AA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK74-1AA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2525,"ST",1,"GMC",1,"1FK70334CK741AA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK74-1AB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2711,"ST",1,"GMC",1,"1FK70334CK741AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7034-2AF21-1BB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65, DE flange IP67",3274,"ST",1,"GMC",1,"1FK70342AF211BB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7034-2AF21-1FB2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.47kW; UDC=300V; M0=1.6Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",3931,"ST",1,"GMC",1,"1FK70342AF211FB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7034-2AF24-1TH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N with holding brake, type of protection IP64",1800,"ST",1,"GMC",1,"1FK70342AF241TH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7034-2AK71-1FH2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",3798,"ST",1,"GMC",1,"1FK70342AK711FH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7034-2AK74-1SA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.63 kW; UDC=600V M0=1.6 Nm (100K); NN=6000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N without holding brake degree of protection IP65, DE flange IP67",1746,"ST",1,"GMC",1,"1FK70342AK741SA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7040-2AK71-1BH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.69 kW; UDC=600V M0=1.6 Nm (100K); NN=6000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N with holding brake degree of protection IP64",3024,"ST",1,"GMC",1,"1FK70402AK711BH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7040-2AK71-1PB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.69 kW; UDC=600V M0=1.6 Nm (100K); NN=6000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, degree of protection IP65 DE flange IP67",2434,"ST",1,"GMC",1,"1FK70402AK711PB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7040-2AK74-1SG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.69 kW; UDC=600V M0=1.6 Nm (100K); NN=6000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=4) smooth shaft, tolerance N without holding brake, type of protection IP65 DE flange IP67",1575,"ST",1,"GMC",1,"1FK70402AK741SG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7042-2AC71-1DB0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.59kW; UDC=600V M0=3Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",3364,"ST",1,"GMC",1,"1FK70422AC711DB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7042-2AC74-1AH1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.59kW; UDC=600V M0=3Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2900,"ST",1,"GMC",1,"1FK70422AC741AH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7042-2AC74-1SG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.59 kW; UDC=600V M0=3Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=4) smooth shaft, tolerance N without holding brake, type of protection IP65",1668,"ST",1,"GMC",1,"1FK70422AC741SG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7042-2AF21-1UG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.82 kW; UDC=300 V M0=3 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake degree of protection IP65 DE flange IP67",2021,"ST",1,"GMC",1,"1FK70422AF211UG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7042-2AF24-1TH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.82 kW; UDC=300 V M0=3Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N with holding brake, type of protection IP65",2046,"ST",1,"GMC",1,"1FK70422AF241TH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7042-2AF71-1RB0","SIMOTICS S SIMOTICS S-1FK7 1FK7-CT synchronous motor PN=0.82 kW UDC=600 V M0=3 Nm (100K); NN=3000 r/min; naturally cooled design MB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 20 bit +12 bit multiturn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N with holding brake degree of protection IP64",3088,"ST",1,"GMC",1,"1FK70422AF711RB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7042-2AF74-1EG0","SIMOTICS S SIMOTICS S-1FK7 Synchronous motor 1FK7-CT PN=0.82kW; UDC=600V M0=3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2931,"ST",1,"GMC",1,"1FK70422AF741EG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7042-2AK71-1PG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.94 kW; UDC=600 V M0=3 Nm (100K); NN=6000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake degree of protection IP65",2021,"ST",1,"GMC",1,"1FK70422AK711PG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7042-2AK71-1UA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.94 kW; UDC=600 V M0=3 Nm (100K); NN=6000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake degree of protection IP65",2147,"ST",1,"GMC",1,"1FK70422AK711UA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7042-2AK74-1EH0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.94kW; UDC=600V M0=3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",3309,"ST",1,"GMC",1,"1FK70422AK741EH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7042-3BK71-1QH2","SIMOTICS S synchronous motor 1FK7-HI PN=0.94 kW; UDC=600 V M0=3 Nm (100K); NN=6000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N with holding brake degree of protection IP65 DE flange IP67",2549,"ST",1,"GMC",1,"1FK70423BK711QH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7043-4CF21-1BG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.94kW; UDC=300V; M0=3. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2805,"ST",1,"GMC",1,"1FK70434CF211BG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7043-4CH71-1BB2","SIMOTICS S Synchronous motor 1FK7-HD PN=1.2kW; UDC=600V M0=3.5Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",3446,"ST",1,"GMC",1,"1FK70434CH711BB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7043-4CH71-1QH1","SIMOTICS S Synchronous motor 1FK7-HD PN=1.2kW; UDC=600V M0=3.5Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2611,"ST",1,"GMC",1,"1FK70434CH711QH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7043-4CK71-1BB1","SIMOTICS S Synchronous motor 1FK7-HD PN=1.3kW; UDC=600V M0=3.5Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",3446,"ST",1,"GMC",1,"1FK70434CK711BB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7043-4CK71-1CH0","SIMOTICS S Synchronous motor 1FK7-HD PN=1.3kW; UDC=600V M0=3.5Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",3722,"ST",1,"GMC",1,"1FK70434CK711CH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7043-4CK71-1UA2","SIMOTICS S Synchronous motor 1FK7-HD PN=1.3kW; UDC=600V M0=3.5Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2209,"ST",1,"GMC",1,"1FK70434CK711UA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7044-4CF71-1CB2","SIMOTICS S Synchronous motor 1FK7-HD PN=1.2kW; UDC=600V M0=4.5Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",4089,"ST",1,"GMC",1,"1FK70444CF711CB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7044-4CF74-1AB2","SIMOTICS S Synchronous motor 1FK7-HD PN=1.2kW; UDC=600V M0=4.5Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",3197,"ST",1,"GMC",1,"1FK70444CF741AB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7044-4CH71-1BA0","SIMOTICS S Synchronous motor 1FK7-HD PN=1.4kW; UDC=600V M0=4.5Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",3034,"ST",1,"GMC",1,"1FK70444CH711BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7044-4CH71-1QA0","SIMOTICS S Synchronous motor 1FK7-HD PN=1.4kW; UDC=600V M0=4.5Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2329,"ST",1,"GMC",1,"1FK70444CH711QA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7044-4CH74-1TB1","SIMOTICS S Synchronous motor 1FK7-HD PN=1.4kW; UDC=600V M0=4.5Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2341,"ST",1,"GMC",1,"1FK70444CH741TB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7060-2AC71-1CA1","SIMOTICS S Synchronous motor 1FK7-CT PN=1.1kW; UDC=600V M0=6Nm (100K); NN=2000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 24-bit +12-bit multi-turn with Drive-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N without holding brake IP65 degree of protection",3856,"ST",1,"GMC",1,"1FK70602AC711CA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7060-2AC71-1UH0","SIMOTICS S synchronous motor 1FK7-CT PN=1.1 kW; UDC=600 V M0=6 Nm (100K); NN=2000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake degree of protection IP64",2643,"ST",1,"GMC",1,"1FK70602AC711UH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7060-2AC74-1TB1","SIMOTICS S synchronous motor 1FK7-CT PN=1.1 kW; UDC=600V M0=6Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N with holding brake degree of protection IP65",2550,"ST",1,"GMC",1,"1FK70602AC741TB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7060-2AF71-1DB1","SIMOTICS S Synchronous motor 1FK7-CT PN=1.5kW; UDC=600V M0=6Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",3873,"ST",1,"GMC",1,"1FK70602AF711DB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7060-2AF71-1UG1","SIMOTICS S synchronous motor 1FK7-CT PN=1.5 kW; UDC=600 V M0=6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake degree of protection IP65",2334,"ST",1,"GMC",1,"1FK70602AF711UG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7060-2AH71-1PG0","SIMOTICS S synchronous motor 1FK7-CT PN=1.7 kW; UDC=600 V M0=6 Nm (100K); NN=4500 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake degree of protection IP64",2197,"ST",1,"GMC",1,"1FK70602AH711PG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7060-2AH71-1RB0","SIMOTICS S synchronous motor 1FK7-CT PN=1.7 kW; UDC=600 V M0=6 Nm (100K); NN=4500 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 20-bit +12- bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N with holding brake degree of protection IP64",3463,"ST",1,"GMC",1,"1FK70602AH711RB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7060-2AH74-1EH1","SIMOTICS S Synchronous motor 1FK7-CT PN=1.7kW; UDC=600V M0=6Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",3827,"ST",1,"GMC",1,"1FK70602AH741EH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7060-3BF71-1QH1","SIMOTICS S synchronous motor 1FK7-HI PN=1.5 kW; UDC=600 V M0=6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N with holding brake degree of protection IP65",2930,"ST",1,"GMC",1,"1FK70603BF711QH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7061-4CF71-1CA1","SIMOTICS S Synchronous motor 1FK7-HD PN=1.7kW; UDC=600V M0=6.4Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",4014,"ST",1,"GMC",1,"1FK70614CF711CA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7061-4CF71-1UH1","SIMOTICS S Synchronous motor 1FK7-HD PN=1.7kW; UDC=600V M0=6.4Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2939,"ST",1,"GMC",1,"1FK70614CF711UH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7061-4CF74-1EG1","SIMOTICS S Synchronous motor 1FK7-HD PN=1.7kW; UDC=600V M0=6.4Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",3540,"ST",1,"GMC",1,"1FK70614CF741EG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7061-4CH71-1UG2","SIMOTICS S Synchronous motor 1FK7-HD PN=2kW; UDC=600V M0=6.4Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2493,"ST",1,"GMC",1,"1FK70614CH711UG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7061-4CH74-1EB2","SIMOTICS S Synchronous motor 1FK7-HD PN=2kW; UDC=600V M0=6.4Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",4108,"ST",1,"GMC",1,"1FK70614CH741EB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7062-2AC71-1PG0","SIMOTICS S synchronous motor 1FK7-CT PN=1.5 kW; UDC=600 V M0=8.5 Nm (100K); NN=2000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake degree of protection IP64",2387,"ST",1,"GMC",1,"1FK70622AC711PG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7062-2AC74-1EA2","SIMOTICS S Synchronous motor 1FK7-CT PN=1.5kW; UDC=600V M0=8.5Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",3694,"ST",1,"GMC",1,"1FK70622AC741EA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7062-2AF71-1DG1","SIMOTICS S Synchronous motor 1FK7-CT PN=1.9kW; UDC=600V M0=8.5Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",3497,"ST",1,"GMC",1,"1FK70622AF711DG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7062-2AF71-1QA1","SIMOTICS S synchronous motor 1FK7-CT PN=1.9 kW; UDC=600 V M0=8.5 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65",2800,"ST",1,"GMC",1,"1FK70622AF711QA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7062-2AF74-1AG2","SIMOTICS S Synchronous motor 1FK7-CT PN=1.9kW; UDC=600V M0=8.5Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",3027,"ST",1,"GMC",1,"1FK70622AF741AG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7062-2AH71-1PB1","SIMOTICS S synchronous motor 1FK7-CT PN=1.4 kW; UDC=600V M0=8.5Nm (100K); NN=4500rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, type of protection IP65",3092,"ST",1,"GMC",1,"1FK70622AH711PB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7062-2AH74-1AG0","SIMOTICS S Synchronous motor 1FK7-CT PN=1.4kW; UDC=600V M0=8.5Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2891,"ST",1,"GMC",1,"1FK70622AH741AG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7062-3BF71-1DA1","SIMOTICS S Synchronous motor 1FK7-HI PN=1.9kW; UDC=600V M0=8.5Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",3620,"ST",1,"GMC",1,"1FK70623BF711DA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7063-2AC71-1CA0","SIMOTICS S synchronous motor 1FK7-CT PN=1.9kW; UDC=600V M0=11Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 24-bit + 12-bit multiturn with DRIVE-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N without holding brake, degree of protection IP64",4045,"ST",1,"GMC",1,"1FK70632AC711CA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7063-2AC71-1QG0","SIMOTICS S synchronous motor 1FK7-CT PN=1.9kW; UDC=600V M0=11Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 20-bit with Drive-CLiQ interface (encoder AS20DQI) Smooth shaft, tolerance N without holding brake, degree of protection IP64",2674,"ST",1,"GMC",1,"1FK70632AC711QG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7063-2AC71-1UB0","SIMOTICS S synchronous motor 1FK7-CT PN=1.9 kW; UDC=600 V M0=11 Nm (100K); NN=2000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake degree of protection IP64",3092,"ST",1,"GMC",1,"1FK70632AC711UB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7063-2AF71-1FG1","SIMOTICS S Synchronous motor 1FK7-CT PN=2.3kW; UDC=600V M0=11Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",4170,"ST",1,"GMC",1,"1FK70632AF711FG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7063-2AF71-1UB0","SIMOTICS S synchronous motor 1FK7-CT PN=2.3 kW; UDC=600 V M0=11 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake degree of protection IP64",3092,"ST",1,"GMC",1,"1FK70632AF711UB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7063-2AF74-1TB2","SIMOTICS S synchronous motor 1FK7-CT PN=2.3 kW; UDC=600V M0=11 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N with holding brake degree of protection IP65, DE flange IP67",2877,"ST",1,"GMC",1,"1FK70632AF741TB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7063-2AH71-1PB0","SIMOTICS S synchronous motor 1FK7-CT PN=1.4 kW; UDC=600 V M0=11 Nm (100K); NN=4500 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake degree of protection IP64",3092,"ST",1,"GMC",1,"1FK70632AH711PB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7063-2AH74-1SG0","SIMOTICS S synchronous motor 1FK7-CT PN=1.4 kW; UDC=600V M0=11 Nm (100K); NN=4500rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=4) smooth shaft, tolerance N without holding brake, type of protection IP64",2172,"ST",1,"GMC",1,"1FK70632AH741SG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7064-4CC71-1BB0","SIMOTICS S Synchronous motor 1FK7-HD PN=2.1kW; UDC=600V M0=12Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",4181,"ST",1,"GMC",1,"1FK70644CC711BB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7064-4CC71-1QG2","SIMOTICS S Synchronous motor 1FK7-HD PN=2.1kW; UDC=600V M0=12Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",3041,"ST",1,"GMC",1,"1FK70644CC711QG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7064-4CC74-1SH0","SIMOTICS S Synchronous motor 1FK7-HD PN=2.1kW; UDC=600V M0=12Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2850,"ST",1,"GMC",1,"1FK70644CC741SH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7064-4CF71-1PH0","SIMOTICS S Synchronous motor 1FK7-HD PN=2.5kW; UDC=600V M0=12Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",3202,"ST",1,"GMC",1,"1FK70644CF711PH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7064-4CF74-1TA0","SIMOTICS S Synchronous motor 1FK7-HD PN=2.5kW; UDC=600V M0=12Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2530,"ST",1,"GMC",1,"1FK70644CF741TA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7064-4CH71-1BH0","SIMOTICS S Synchronous motor 1FK7-HD PN=2.4kW; UDC=600V M0=12Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",4058,"ST",1,"GMC",1,"1FK70644CH711BH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7064-4CH74-1SB1","SIMOTICS S Synchronous motor 1FK7-HD PN=2.4kW; UDC=600V M0=12Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",3107,"ST",1,"GMC",1,"1FK70644CH741SB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7080-2AF71-1FG2","SIMOTICS S Synchronous motor 1FK7-CT PN=2.1kW; UDC=600V M0=8Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",4093,"ST",1,"GMC",1,"1FK70802AF711FG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7080-2AF71-1UB0","SIMOTICS S synchronous motor 1FK7-CT PN=2.1 kW; UDC=600 V M0=8 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake degree of protection IP64",3173,"ST",1,"GMC",1,"1FK70802AF711UB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7080-2AF74-1SH1","SIMOTICS S synchronous motor 1FK7-CT PN=2.1 kW; UDC=600V M0=8Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=4) smooth shaft, tolerance N with holding brake, type of protection IP65",2831,"ST",1,"GMC",1,"1FK70802AF741SH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7080-2AH71-1RH0","SIMOTICS S synchronous motor 1FK7-CT PN=2.1 kW; UDC=600 V M0=8 Nm (100K); NN=4500 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 20-bit +12- bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N with holding brake degree of protection IP64",3744,"ST",1,"GMC",1,"1FK70802AH711RH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7080-2AH74-1SB1","SIMOTICS S synchronous motor 1FK7-CT PN=2.1 kW; UDC=600V M0=8Nm (100K); NN=4500rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=4) shaft with feather key, tolerance N with holding brake degree of protection IP65",2958,"ST",1,"GMC",1,"1FK70802AH741SB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7081-2AC71-1BA1","SIMOTICS S synchronous motor 1FK7-CT PN=2.1 kW; UDC=600V M0=12Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65",3882,"ST",1,"GMC",1,"1FK70812AC711BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7081-2AC71-1UB0","SIMOTICS S synchronous motor 1FK7-CT PN=2.1 kW; UDC=600V M0=12Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, type of protection IP64",3491,"ST",1,"GMC",1,"1FK70812AC711UB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7081-2AC74-1TA1","SIMOTICS S synchronous motor 1FK7-CT PN=2.1 kW; UDC=600V M0=12Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N without holding brake degree of protection IP65",2674,"ST",1,"GMC",1,"1FK70812AC741TA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7081-2AF71-1RG1","SIMOTICS S synchronous motor 1FK7-CT PN=2.7 kW; UDC=600 V M0=12 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 20-bit +12- bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N without holding brake degree of protection IP65",3598,"ST",1,"GMC",1,"1FK70812AF711RG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7081-2AF74-1SA2","SIMOTICS S synchronous motor 1FK7-CT PN=2.7 kW; UDC=600V M0=12Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=4) shaft with feather key, tolerance N without holding brake degree of protection IP65, DE flange IP67",2674,"ST",1,"GMC",1,"1FK70812AF741SA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7081-2AH71-1RA2","SIMOTICS S synchronous motor 1FK7-CT PN=1.8 kW; UDC=600V M0=12Nm (100K); NN=4500rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65, DE flange IP67",3723,"ST",1,"GMC",1,"1FK70812AH711RA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7081-2AH71-1UH2","SIMOTICS S synchronous motor 1FK7-CT PN=1.8 kW; UDC=600V M0=12Nm (100K); NN=4500rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, degree of protection IP65 DE flange IP67",3501,"ST",1,"GMC",1,"1FK70812AH711UH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7081-3BF71-1DB0","SIMOTICS S Synchronous motor 1FK7-HI PN=2.7kW; UDC=600V M0=12Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",4464,"ST",1,"GMC",1,"1FK70813BF711DB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7081-3BF74-1AB1","SIMOTICS S Synchronous motor 1FK7-HI PN=2.7kW; UDC=600V M0=12Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VP 2048 S/R WITH C- AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",4129,"ST",1,"GMC",1,"1FK70813BF741AB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7083-2AC71-1QH0","SIMOTICS S synchronous motor 1FK7-CT PN=2.6kW; UDC=600V M0=16Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 20-bit with Drive-CLiQ interface (encoder AS20DQI) Smooth shaft, tolerance N with holding brake, degree of protection IP64",3672,"ST",1,"GMC",1,"1FK70832AC711QH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7083-2AC74-1EB1","SIMOTICS S Synchronous motor 1FK7-CT PN=2.6kW; UDC=600V M0=16Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",4829,"ST",1,"GMC",1,"1FK70832AC741EB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7083-2AF71-1FH1","SIMOTICS S Synchronous motor 1FK7-CT PN=3.3kW; UDC=600V M0=16Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",5169,"ST",1,"GMC",1,"1FK70832AF711FH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7083-2AF71-1QB0","SIMOTICS S synchronous motor 1FK7-CT PN=3.3kW; UDC=600V M0=16Nm (100K); NN=3000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 20-bit with Drive-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N with holding brake, degree of protection IP64",3798,"ST",1,"GMC",1,"1FK70832AF711QB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7083-2AF74-1EA1","SIMOTICS S Synchronous motor 1FK7-CT PN=3.3kW; UDC=600V M0=16Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",4228,"ST",1,"GMC",1,"1FK70832AF741EA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7083-2AH71-1PB0","SIMOTICS S synchronous motor 1FK7-CT PN=1.4 kW; UDC=600 V M0=16 Nm (100K); NN=4500 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake degree of protection IP64",3648,"ST",1,"GMC",1,"1FK70832AH711PB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7083-2AH71-1UH1","SIMOTICS S synchronous motor 1FK7-CT PN=1.4 kW; UDC=600 V M0=16 Nm (100K); NN=4500 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake degree of protection IP65",3659,"ST",1,"GMC",1,"1FK70832AH711UH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7084-2AC71-1DA2","SIMOTICS S Synchronous motor 1FK7-CT PN=3.1kW; UDC=600V M0=20Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",4592,"ST",1,"GMC",1,"1FK70842AC711DA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7084-2AC71-1PG0","SIMOTICS S synchronous motor 1FK7-CT PN=3.1 kW; UDC=600 V M0=20 Nm (100K); NN=2000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake degree of protection IP64",3356,"ST",1,"GMC",1,"1FK70842AC711PG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7084-2AC74-1TG2","SIMOTICS S synchronous motor 1FK7-CT PN=3.1 kW; UDC=600V M0=20Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N without holding brake, type of protection IP65 DE flange IP67",3141,"ST",1,"GMC",1,"1FK70842AC741TG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7084-2AF71-1DB1","SIMOTICS S Synchronous motor 1FK7-CT PN=3.1kW; UDC=600V M0=20Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",5190,"ST",1,"GMC",1,"1FK70842AF711DB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7084-2AF71-1RH2","SIMOTICS S synchronous motor 1FK7-CT PN=3.1kW; UDC=600V M0=20Nm (100K); NN=3000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 20-bit + 12-bit multiturn with DRIVE-CLiQ interface (encoder AM20DQI) Smooth shaft, tolerance N with holding brake, degree of protection IP65 DE Flange, IP67",4791,"ST",1,"GMC",1,"1FK70842AF711RH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7084-3BC71-1CA2","SIMOTICS S synchronous motor 1FK7-HI PN=3.1kW; UDC=600V M0=20Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 24-bit + 12-bit multiturn with DRIVE-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N without holding brake, degree of protection IP65 DE Flange, IP67",5014,"ST",1,"GMC",1,"1FK70843BC711CA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7084-3BC74-1EH1","SIMOTICS S Synchronous motor 1FK7-HI PN=3.1kW; UDC=600V M0=20Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) Smooth shaft, tolerance N With holding brake Degree of protection IP65",5138,"ST",1,"GMC",1,"1FK70843BC741EH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7084-3BF71-1FH0","SIMOTICS S Synchronous motor 1FK7-HI PN=3.1kW; UDC=600V M0=20Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) Smooth shaft, tolerance N With holding brake PROTECTION CLASS IP64;",5470,"ST",1,"GMC",1,"1FK70843BF711FH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7084-3BF74-1AA0","SIMOTICS S Synchronous motor 1FK7-HI PN=3.1kW; UDC=600V M0=20Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VP 2048 S/R WITH C- AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",3986,"ST",1,"GMC",1,"1FK70843BF741AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7085-4CC71-1UG0","SIMOTICS S Synchronous motor 1FK7-HD PN=3.1kW; UDC=600V M0=22Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",3561,"ST",1,"GMC",1,"1FK70854CC711UG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7085-4CC74-1EB0","SIMOTICS S Synchronous motor 1FK7-HD PN=3.1kW; UDC=600V M0=22Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",5334,"ST",1,"GMC",1,"1FK70854CC741EB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7085-4CF71-1PH2","SIMOTICS S Synchronous motor 1FK7-HD PN=2kW; UDC=600V M0=22Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",4296,"ST",1,"GMC",1,"1FK70854CF711PH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7085-4CF74-1AG0","SIMOTICS S Synchronous motor 1FK7-HD PN=2kW; UDC=600V M0=22Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",4065,"ST",1,"GMC",1,"1FK70854CF741AG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7086-4CC71-1PB2","SIMOTICS S Synchronous motor 1FK7-HD PN=3.8kW; UDC=600V M0=28Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",5003,"ST",1,"GMC",1,"1FK70864CC711PB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7086-4CC71-1RA2","SIMOTICS S Synchronous motor 1FK7-HD PN=3.8kW; UDC=600V M0=28Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",5099,"ST",1,"GMC",1,"1FK70864CC711RA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7086-4CF71-1FA0","SIMOTICS S Synchronous motor 1FK7-HD PN=2kW; UDC=600V M0=28Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",5781,"ST",1,"GMC",1,"1FK70864CF711FA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7086-4CF71-1QB2","SIMOTICS S Synchronous motor 1FK7-HD PN=2kW; UDC=600V M0=28Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",5154,"ST",1,"GMC",1,"1FK70864CF711QB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7086-4CF74-1EA0","SIMOTICS S Synchronous motor 1FK7-HD PN=2kW; UDC=600V M0=28Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",5315,"ST",1,"GMC",1,"1FK70864CF741EA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7100-2AC71-1BH1","SIMOTICS S synchronous motor 1FK7-CT PN=3 kW; UDC=600V M0=18Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N with holding brake degree of protection IP65",4877,"ST",1,"GMC",1,"1FK71002AC711BH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7100-2AC71-1QG0","SIMOTICS S synchronous motor 1FK7-CT PN=3 kW; UDC=600V M0=18Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N without holding brake degree of protection IP64",3433,"ST",1,"GMC",1,"1FK71002AC711QG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7100-2AF71-1BA2","SIMOTICS S Synchronous motor 1FK7-CT PN=3.8kW; UDC=600V M0=18Nm (100K); NN=3000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 24-bit with Drive-CLiQ interface (encoder AS24DQI) shaft with feather key, tolerance N without holding brake IP65 degree of protection DE flange IP67",4402,"ST",1,"GMC",1,"1FK71002AF711BA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7100-2AF71-1CH2","SIMOTICS S Synchronous motor 1FK7-CT PN=3.8kW; UDC=600V M0=18Nm (100K); NN=3000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 24-bit +12-bit multi-turn with Drive-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N with holding brake IP65 degree of protection DE flange IP67",5416,"ST",1,"GMC",1,"1FK71002AF711CH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7100-2AF74-1SH1","SIMOTICS S synchronous motor 1FK7-CT PN=3.8 kW; UDC=600V M0=18Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=4) smooth shaft, tolerance N with holding brake, type of protection IP65",3668,"ST",1,"GMC",1,"1FK71002AF741SH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7100-3BC71-1BG1","SIMOTICS S synchronous motor 1FK7-HI PN=3 kW; UDC=600V M0=18Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N without holding brake degree of protection IP65",4263,"ST",1,"GMC",1,"1FK71003BC711BG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7101-2AC71-1BG1","SIMOTICS S Synchronous motor 1FK7-CT PN=4.3kW; UDC=600V M0=27Nm (100K); NN=2000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 24-bit with Drive-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N without holding brake IP65 degree of protection",4744,"ST",1,"GMC",1,"1FK71012AC711BG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7101-2AC71-1PH1","SIMOTICS S synchronous motor 1FK7-CT PN=4.3 kW; UDC=600 V M0=27 Nm (100K); NN=2000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake degree of protection IP65",4489,"ST",1,"GMC",1,"1FK71012AC711PH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7101-2AC74-1TA0","SIMOTICS S synchronous motor 1FK7-CT PN=4.3 kW; UDC=600V M0=27 Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N without holding brake degree of protection IP64",3525,"ST",1,"GMC",1,"1FK71012AC741TA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7101-2AF71-1BH0","SIMOTICS S synchronous motor 1FK7-CT PN=4.9kW; UDC=600V M0=27Nm (100K); NN=3000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 24-bit with Drive-CLiQ interface (encoder AS24DQI) Smooth shaft, tolerance N with holding brake, degree of protection IP64",5208,"ST",1,"GMC",1,"1FK71012AF711BH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7101-2AF71-1QA1","SIMOTICS S synchronous motor 1FK7-CT PN=4.9kW; UDC=600V M0=27Nm (100K); NN=3000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 20-bit with Drive-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N without holding brake, degree of protection IP65",4164,"ST",1,"GMC",1,"1FK71012AF711QA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7101-2AF74-1TB0","SIMOTICS S synchronous motor 1FK7-CT PN=4.9 kW; UDC=600V M0=27 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N with holding brake degree of protection IP64",4126,"ST",1,"GMC",1,"1FK71012AF741TB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7101-3BC71-1QA0","SIMOTICS S synchronous motor 1FK7-HI PN=4.3kW; UDC=600V M0=27Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 20-bit with Drive-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N without holding brake, degree of protection IP64",4009,"ST",1,"GMC",1,"1FK71013BC711QA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7101-3BF71-1QH0","SIMOTICS S synchronous motor 1FK7-HI PN=4.9 kW; UDC=600V M0=27 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N with holding brake degree of protection IP64",4484,"ST",1,"GMC",1,"1FK71013BF711QH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7101-3BF74-1AG0","SIMOTICS S Synchronous motor 1FK7-HI PN=4.9kW; UDC=600V M0=27Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VP 2048 S/R WITH C- AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",4237,"ST",1,"GMC",1,"1FK71013BF741AG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7103-2AC71-1UG2","SIMOTICS S synchronous motor 1FK7-CT PN=5.2 kW; UDC=600 V M0=36 Nm (100K); NN=2000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake degree of protection IP65 DE flange IP67",4505,"ST",1,"GMC",1,"1FK71032AC711UG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7103-2AC74-1EB2","SIMOTICS S Synchronous motor 1FK7-CT PN=5.2kW; UDC=600V M0=36Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",6276,"ST",1,"GMC",1,"1FK71032AC741EB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7103-2AF71-1PB1","SIMOTICS S synchronous motor 1FK7-CT PN=4.4 kW; UDC=600 V M0=36 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake degree of protection IP65",5232,"ST",1,"GMC",1,"1FK71032AF711PB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7103-2AF74-1AG2","SIMOTICS S Synchronous motor 1FK7-CT PN=4.4kW; UDC=600V M0=36Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",5006,"ST",1,"GMC",1,"1FK71032AF741AG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7103-3BC71-1QA0","SIMOTICS S synchronous motor 1FK7-HI PN=5.2kW; UDC=600V M0=36Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 20-bit with Drive-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N without holding brake, degree of protection IP64",4620,"ST",1,"GMC",1,"1FK71033BC711QA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7103-3BC74-1EG1","SIMOTICS S Synchronous motor 1FK7-HI PN=5.2kW; UDC=600V M0=36Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",5524,"ST",1,"GMC",1,"1FK71033BC741EG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7103-3BF74-1EH0","SIMOTICS S Synchronous motor 1FK7-HI PN=4.4kW; UDC=600V M0=36Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",5991,"ST",1,"GMC",1,"1FK71033BF741EH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7105-2AC71-1CG0","SIMOTICS S Synchronous motor 1FK7-CT PN=7.7kW; UDC=600V M0=48Nm (100K); NN=2000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 24-bit +12-bit multi-turn with Drive-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N without holding brake IP64 degree of protection",7315,"ST",1,"GMC",1,"1FK71052AC711CG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7105-2AC71-1QG1","SIMOTICS S Synchronous motor 1FK7-CT PN=7.7kW; UDC=600V M0=48Nm (100K); NN=2000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 20-bit with Drive-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N without holding brake IP65 degree of protection",6206,"ST",1,"GMC",1,"1FK71052AC711QG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7105-2AC74-1EG0","SIMOTICS S Synchronous motor 1FK7-CT PN=7.7kW; UDC=600V M0=48Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",6966,"ST",1,"GMC",1,"1FK71052AC741EG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7105-2AF71-1FH0","SIMOTICS S Synchronous motor 1FK7-CT PN=8.2kW; UDC=600V M0=48Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",8033,"ST",1,"GMC",1,"1FK71052AF711FH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7105-2AF74-1SA1","SIMOTICS S synchronous motor 1FK7-CT PN=8.2 kW; UDC=600V M0=48Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=4) shaft with feather key, tolerance N without holding brake degree of protection IP65",5829,"ST",1,"GMC",1,"1FK71052AF741SA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7105-2AF74-1TH1","SIMOTICS S synchronous motor 1FK7-CT PN=8.2 kW; UDC=600V M0=48Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N with holding brake, type of protection IP65",6304,"ST",1,"GMC",1,"1FK71052AF741TH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FL2102-2AF11-1MC0","SIMOTICS S-1FL2 Supply voltage 400V 3AC Pn=50W;Nn=3000rpm M0=0.16Nm;Mn=0.16Nm Shaft height 20mm With hybrid connector AM21bit With shaft key, Tolerance N With holding brake Protection class IP65 with oil seal Matching drive SINAMICS S200",1394,"ST",1,"GMC",1,"1FL21022AF111MC0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FL2102-4AF10-0SC0","SIMOTICS S-1FL2 Supply voltage 400V 3AC Pn=100W;Nn=3000rpm M0=0.32Nm;Mn=0.32Nm Shaft height 20mm With hybrid connector AS21bit Plain shaft, Tolerance N With holding brake Protection class IP54 without oil seal Matching drive SINAMICS S200",1093,"ST",1,"GMC",1,"1FL21024AF100SC0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FL2103-2AF11-1HC0","SIMOTICS S-1FL2 Supply voltage 400V 3AC Pn=0.2kW;Nn=3000rpm M0=0.64Nm;Mn=0.64Nm Shaft height 30mm With hybrid connector AS17bit With shaft key, Tolerance N With holding brake Protection class IP65 with oil seal Matching drive SINAMICS S200",949,"ST",1,"GMC",1,"1FL21032AF111HC0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FL2103-4AF10-1MC0","SIMOTICS S-1FL2 Supply voltage 400V 3AC Pn=0.4kW;Nn=3000rpm M0=1.27Nm;Mn=1.27Nm Shaft height 30mm With hybrid connector AM21bit With shaft key, Tolerance N With holding brake Protection class IP54 without oil seal Matching drive SINAMICS S200",1519,"ST",1,"GMC",1,"1FL21034AF101MC0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FL2104-2AG11-0MC0","SIMOTICS S-1FL2 Supply voltage 200V 3AC Pn=0.75kW;Nn=3000rpm M0=2.4Nm;Mn=2.4Nm Shaft height 40mm With hybrid connector AM21bit Plain shaft, Tolerance N With holding brake Protection class IP65 with oil seal Matching drive SINAMICS S200",1787,"ST",1,"GMC",1,"1FL21042AG110MC0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FL2104-4AG10-0SC0","SIMOTICS S-1FL2 Supply voltage 200V 3AC Pn=1kW;Nn=3000rpm M0=3.2Nm;Mn=3.2Nm Shaft height 40mm With hybrid connector AS21bit Plain shaft, Tolerance N With holding brake Protection class IP54 without oil seal Matching drive SINAMICS S200",1513,"ST",1,"GMC",1,"1FL21044AG100SC0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FL2105-2AF11-1SB0","SIMOTICS S-1FL2 Supply voltage 400V 3AC Pn=1.5kW;Nn=3000rpm M0=5Nm;Mn=4.6Nm Shaft height 52mm With angular connector AS21bit With shaft key, Tolerance N With holding brake Protection class IP65 with oil seal Matching drive SINAMICS S200",1786,"ST",1,"GMC",1,"1FL21052AF111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FL2203-2AG11-0SC0","SIMOTICS S-1FL2 Supply voltage 200V 3AC Pn=0.2kW;Nn=3000rpm M0=0.64Nm;Mn=0.64Nm Shaft height 30mm With hybrid connector AS21bit Plain shaft, Tolerance N With holding brake Protection class IP65 with oil seal Matching drive SINAMICS S200",1226,"ST",1,"GMC",1,"1FL22032AG110SC0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FL2204-2AF01-0SC0","SIMOTICS S-1FL2 Supply voltage 400V 3AC Pn=0.75kW;Nn=3000rpm M0=2.4Nm;Mn=2.4Nm Shaft height 40mm With hybrid connector AS21bit Plain shaft, Tolerance N Without holding brake Protection class IP65 with oil seal Matching drive SINAMICS S200",1140,"ST",1,"GMC",1,"1FL22042AF010SC0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FL2204-4AG01-1SC0","SIMOTICS S-1FL2 Supply voltage 200V 3AC Pn=1kW;Nn=3000rpm M0=3.2Nm;Mn=3.2Nm Shaft height 40mm With hybrid connector AS21bit With shaft key, Tolerance N Without holding brake Protection class IP65 with oil seal Matching drive SINAMICS S200",1217,"ST",1,"GMC",1,"1FL22044AG011SC0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FL2304-2AF11-0HB0","SIMOTICS S-1FL2 Supply voltage 400V 3AC Pn=0.4kW;Nn=3000rpm M0=1.45Nm;Mn=1.27Nm Shaft height 45mm With angular connector AS17bit Plain shaft, Tolerance N With holding brake Protection class IP65 with oil seal Matching drive SINAMICS S200",1056,"ST",1,"GMC",1,"1FL23042AF110HB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FL2306-7AC11-1HB0","SIMOTICS S-1FL2 Supply voltage 400V 3AC Pn=2kW;Nn=2000rpm M0=13.3Nm;Mn=9.55Nm Shaft height 65mm With angular connector AS17bit With shaft key, Tolerance N With holding brake Protection class IP65 with oil seal Matching drive SINAMICS S200",2102,"ST",1,"GMC",1,"1FL23067AC111HB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FL2310-2AC11-0HB0","SIMOTICS S-1FL2 Supply voltage 400V 3AC Pn=3.5kW;Nn=2000rpm M0=18.1Nm;Mn=16.7Nm Shaft height 90mm With angular connector AS17bit Plain shaft, Tolerance N With holding brake Protection class IP65 with oil seal Matching drive SINAMICS S200",2733,"ST",1,"GMC",1,"1FL23102AC110HB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FL6032-2AF21-1MA1","SIMOTICS S-1FL6 voltage supply 230 V 3AC Pn=0.2 kW; Nn=3000 rpm M0=0.64 Nm; MN=0.64 Nm. Shaft height 30 mm absolute encoder Single-turn 21-bit with feather key Tolerance N without holding brake Degree of protection IP65 with fitting oil seal for drive SINAMICS V90",825,"ST",1,"GMC",1,"1FL60322AF211MA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FL6044-2AF21-1MH1","SIMOTICS S-1FL6 voltage supply 230 V 3AC Pn=1 kW; Nn=3000 rpm M0=3.18 Nm; MN=3.18 Nm. Shaft height 40 mm absolute encoder Single-turn 21-bit with smooth shaft Tolerance N with holding brake Degree of protection IP65 with fitting oil seal for drive V90",1411,"ST",1,"GMC",1,"1FL60442AF211MH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FL6092-1AC61-2AG1","SIMOTICS S-1FL6-1FL6 Operating voltage 3AC 400 V Pn=3.5 kW; Nn=2000 rpm M0=22 Nm; MN=16.7 Nm Shaft height 90 mm, with angle plug; incremental encoder 2500 incr./rev. plain shaft, Tolerance N without holding brake Degree of protection IP65 with sealing ring compatible with the converters SINAMICS V70 & V90",2256,"ST",1,"GMC",1,"1FL60921AC612AG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT2105-6AF02-1SB0","SIMOTICS S-1FT2 HD synchronous motor M0=8 Nm; PN=2.1 kW at 3000 rpm (380-480 V); with DRIVE-CLiQ plug M17; power connector size M17; without brake; degree of protection IP67; shaft extension with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC);",2456,"ST",1,"GMC",1,"1FT21056AF021SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7034-5AK70-1BB2","SIMOTICS S Synchronous motor 1FT7, M0=2Nm (100K) NN=6000rpm, PN=0.88kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",5572,"ST",1,"GMC",1,"1FT70345AK701BB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7034-5AK70-1BD3","SIMOTICS S Synchronous motor 1FT7, M0=2Nm (100K) NN=6000rpm, PN=0.88kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",4864,"ST",1,"GMC",1,"1FT70345AK701BD3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7034-5AK71-1CA0","SIMOTICS S Synchronous motor 1FT7, M0=2Nm (100K) NN=6000rpm, PN=0.88kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",5507,"ST",1,"GMC",1,"1FT70345AK711CA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7034-5AK71-1LG0","SIMOTICS S Synchronous motor 1FT7, M0=2Nm (100K) NN=6000rpm, PN=0.88kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) AND M17-CONNECTOR PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",5935,"ST",1,"GMC",1,"1FT70345AK711LG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7036-5AK70-1DB0","SIMOTICS S Synchronous motor 1FT7, M0=3Nm (100K) NN=6000rpm, PN=1.07kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",5634,"ST",1,"GMC",1,"1FT70365AK701DB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7036-5AK71-1FG3","SIMOTICS S Synchronous motor 1FT7, M0=3Nm (100K) NN=6000rpm, PN=1.07kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",6041,"ST",1,"GMC",1,"1FT70365AK711FG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7042-5AF70-1BH1","SIMOTICS S Synchronous motor 1FT7, M0=3Nm (100K) NN=3000rpm, PN=0.85kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",5789,"ST",1,"GMC",1,"1FT70425AF701BH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7042-5AF71-1BH2","SIMOTICS S Synchronous motor 1FT7, M0=3Nm (100K) NN=3000rpm, PN=0.85kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",5903,"ST",1,"GMC",1,"1FT70425AF711BH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7042-5AF71-1DH0","SIMOTICS S Synchronous motor 1FT7, M0=3Nm (100K) NN=3000rpm, PN=0.85kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",5766,"ST",1,"GMC",1,"1FT70425AF711DH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7042-5AF74-1MG2","SIMOTICS S Synchronous motor 1FT7, M0=3Nm (100K) NN=3000rpm, PN=0.85kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible), with Pt1000 temperature sensor POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER A-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",5515,"ST",1,"GMC",1,"1FT70425AF741MG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7042-5AK71-1CE0","SIMOTICS S Synchronous motor 1FT7, M0=3Nm (100K) NN=6000rpm, PN=1.26kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",6967,"ST",1,"GMC",1,"1FT70425AK711CE0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7044-1AF74-1MG1","SIMOTICS S Synchronous motor 1FT7, M0=5Nm (100K) NN=3000rpm, PN=1.35kW naturally cooled; Power connector rotatable; Vibration severity A Degree of protection IP65 Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible), with Pt1000 temperature sensor ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER A-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACCURACY TOLERANCE N",4655,"ST",1,"GMC",1,"1FT70441AF741MG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7044-5AF70-1DD4","SIMOTICS S Synchronous motor 1FT7, M0=5Nm (100K) NN=3000rpm, PN=1.35kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",5893,"ST",1,"GMC",1,"1FT70445AF701DD4","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7044-5AF71-1CL1","SIMOTICS S Synchronous motor 1FT7, M0=5Nm (100K) NN=3000rpm, PN=1.35kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE R VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",7621,"ST",1,"GMC",1,"1FT70445AF711CL1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7044-5AF75-1NG2","SIMOTICS S Synchronous motor 1FT7, M0=5Nm (100K) NN=3000rpm, PN=1.35kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact), with Pt1000  temperature sensor POWER CONNECTOR ROTATABLE INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",4957,"ST",1,"GMC",1,"1FT70445AF751NG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7044-5AK70-1CG1","SIMOTICS S Synchronous motor 1FT7, M0=5Nm (100K) NN=6000rpm, PN=1.41kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",6420,"ST",1,"GMC",1,"1FT70445AK701CG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7044-5AK71-1DG3","SIMOTICS S Synchronous motor 1FT7, M0=5Nm (100K) NN=6000rpm, PN=1.41kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",5527,"ST",1,"GMC",1,"1FT70445AK711DG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7046-5AF70-1BH2","SIMOTICS S Synchronous motor 1FT7, M0=7Nm (100K) NN=3000rpm, PN=1.76kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",6855,"ST",1,"GMC",1,"1FT70465AF701BH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7046-5AF71-1BE5","SIMOTICS S Synchronous motor 1FT7, M0=7Nm (100K) NN=3000rpm, PN=1.76kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 67",7301,"ST",1,"GMC",1,"1FT70465AF711BE5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7046-5AF71-1DB2","SIMOTICS S Synchronous motor 1FT7, M0=7Nm (100K) NN=3000rpm, PN=1.76kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",6969,"ST",1,"GMC",1,"1FT70465AF711DB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7046-5AH70-1CH0","SIMOTICS S Synchronous motor 1FT7, M0=7Nm (100K) NN=4500rpm, PN=1.32kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",7696,"ST",1,"GMC",1,"1FT70465AH701CH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7062-1AF70-1CG1","SIMOTICS S Synchronous motor 1FT7, M0=6Nm (100K) NN=3000rpm, PN=1.70kW naturally cooled; Power connector rotatable; Vibration severity A Degree of protection IP65 Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACCURACY TOLERANCE N",5094,"ST",1,"GMC",1,"1FT70621AF701CG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7062-5AF70-1BH2","SIMOTICS S Synchronous motor 1FT7, M0=6Nm (100K) NN=3000rpm, PN=1.70kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",6499,"ST",1,"GMC",1,"1FT70625AF701BH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7062-5AF71-1CH2","SIMOTICS S Synchronous motor 1FT7, M0=6Nm (100K) NN=3000rpm, PN=1.70kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",7590,"ST",1,"GMC",1,"1FT70625AF711CH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7062-5AF71-1FA1","SIMOTICS S Synchronous motor 1FT7, M0=6Nm (100K) NN=3000rpm, PN=1.70kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE Absolute encoder 22-bit Multiturn with DRIVE-CLiQ interface (encoder AM22DQ) Rotatable connector SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",6459,"ST",1,"GMC",1,"1FT70625AF711FA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7062-5AK71-1FH0","SIMOTICS S Synchronous motor 1FT7, M0=6Nm (100K) NN=6000rpm, PN=2.13kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE Absolute encoder 22-bit Multiturn with DRIVE-CLiQ interface (encoder AM22DQ) Rotatable connector PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",7454,"ST",1,"GMC",1,"1FT70625AK711FH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7062-5WF71-1BG3","SIMOTICS S Synchronous motor 1FT7, M0=10Nm (100K) NN=3000rpm, PN=3.10kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",6251,"ST",1,"GMC",1,"1FT70625WF711BG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7064-1AF71-1LG1","SIMOTICS S Synchronous motor 1FT7, M0=9Nm (100K) NN=3000rpm, PN=2.39kW naturally cooled; Power connector rotatable; Vibration severity A Degree of protection IP65 Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) AND M17-CONNECTOR PLAIN SHAFT, W/O HOLDING BRAKE; ACCURACY TOLERANCE N",5951,"ST",1,"GMC",1,"1FT70641AF711LG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7064-5AF70-1CB2","SIMOTICS S Synchronous motor 1FT7, M0=9Nm (100K) NN=3000rpm, PN=2.39kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",8195,"ST",1,"GMC",1,"1FT70645AF701CB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7064-5AF71-1CB4","SIMOTICS S Synchronous motor 1FT7, M0=9Nm (100K) NN=3000rpm, PN=2.39kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",8304,"ST",1,"GMC",1,"1FT70645AF711CB4","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7064-5AF71-1DH1","SIMOTICS S Synchronous motor 1FT7, M0=9Nm (100K) NN=3000rpm, PN=2.39kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",7105,"ST",1,"GMC",1,"1FT70645AF711DH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7064-5AK71-1CB1","SIMOTICS S Synchronous motor 1FT7, M0=9Nm (100K) NN=6000rpm, PN=2.59kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",8082,"ST",1,"GMC",1,"1FT70645AK711CB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7064-5AK71-1DK5","SIMOTICS S Synchronous motor 1FT7, M0=9Nm (100K) NN=6000rpm, PN=2.59kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 67",6536,"ST",1,"GMC",1,"1FT70645AK711DK5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7064-5WF71-1CL4","SIMOTICS S Synchronous motor 1FT7, M0=16Nm (100K) NN=3000rpm, PN=5.00kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",9443,"ST",1,"GMC",1,"1FT70645WF711CL4","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7065-7WF70-1DA3","SIMOTICS S Synchronous motor 1FT7, M0=19Nm (100K) NN=3000rpm, PN=5.70kW water-cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",7485,"ST",1,"GMC",1,"1FT70657WF701DA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7066-5AF70-1FH0","SIMOTICS S Synchronous motor 1FT7, M0=12Nm (100K) NN=3000rpm, PN=2.92kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE Absolute encoder 22-bit Multiturn with DRIVE-CLiQ interface (encoder AM22DQ) Rotatable connector PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",8501,"ST",1,"GMC",1,"1FT70665AF701FH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7066-5AF71-1DA2","SIMOTICS S Synchronous motor 1FT7, M0=12Nm (100K) NN=3000rpm, PN=2.92kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",6528,"ST",1,"GMC",1,"1FT70665AF711DA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7066-5AF71-1FB0","SIMOTICS S Synchronous motor 1FT7, M0=12Nm (100K) NN=3000rpm, PN=2.92kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE Absolute encoder 22-bit Multiturn with DRIVE-CLiQ interface (encoder AM22DQ) Rotatable connector SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",8501,"ST",1,"GMC",1,"1FT70665AF711FB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7066-5AH71-1DD5","SIMOTICS S Synchronous motor 1FT7, M0=12Nm (100K) NN=4500rpm, PN=2.55kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 67",6978,"ST",1,"GMC",1,"1FT70665AH711DD5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7066-5AH74-1MB0","SIMOTICS S Synchronous motor 1FT7, M0=12Nm (100K) NN=4500rpm, PN=2.55kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible), with Pt1000 temperature sensor POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER A-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",7885,"ST",1,"GMC",1,"1FT70665AH741MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7067-7SH71-1BB0","SIMOTICS S Synchronous motor 1FT7, M0=17Nm (100K) NN=4500rpm, PN=6.10kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",8719,"ST",1,"GMC",1,"1FT70677SH711BB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7068-5AF70-1BD5","SIMOTICS S Synchronous motor 1FT7, M0=15Nm (100K) NN=3000rpm, PN=3.42kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 67",7305,"ST",1,"GMC",1,"1FT70685AF701BD5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7068-5AF71-1CH0","SIMOTICS S Synchronous motor 1FT7, M0=15Nm (100K) NN=3000rpm, PN=3.42kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",8828,"ST",1,"GMC",1,"1FT70685AF711CH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7068-5AF71-1FH0","SIMOTICS S Synchronous motor 1FT7, M0=15Nm (100K) NN=3000rpm, PN=3.42kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE Absolute encoder 22-bit Multiturn with DRIVE-CLiQ interface (encoder AM22DQ) Rotatable connector PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",8942,"ST",1,"GMC",1,"1FT70685AF711FH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7068-5WF70-1FH1","SIMOTICS S Synchronous motor 1FT7, M0=30Nm (100K) NN=3000rpm, PN=9.30kW water-cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE Absolute encoder 22-bit Multiturn with DRIVE-CLiQ interface (encoder AM22DQ) Rotatable connector PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",9994,"ST",1,"GMC",1,"1FT70685WF701FH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7082-5AC70-1DA3","SIMOTICS S Synchronous motor 1FT7, M0=13Nm (100K) NN=2000rpm, PN=2.39kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",6056,"ST",1,"GMC",1,"1FT70825AC701DA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7082-5AC71-1CA1","SIMOTICS S Synchronous motor 1FT7, M0=13Nm (100K) NN=2000rpm, PN=2.39kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",6950,"ST",1,"GMC",1,"1FT70825AC711CA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7082-5AF70-1FB0","SIMOTICS S Synchronous motor 1FT7, M0=13Nm (100K) NN=3000rpm, PN=3.24kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",8207,"ST",1,"GMC",1,"1FT70825AF701FB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7082-5AF71-1CG0","SIMOTICS S Synchronous motor 1FT7, M0=13Nm (100K) NN=3000rpm, PN=3.24kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",6813,"ST",1,"GMC",1,"1FT70825AF711CG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7082-5AH70-1CB0","SIMOTICS S Synchronous motor 1FT7, M0=13Nm (100K) NN=4500rpm, PN=3.77kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",8093,"ST",1,"GMC",1,"1FT70825AH701CB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7082-5AH70-1FB3","SIMOTICS S Synchronous motor 1FT7, M0=13Nm (100K) NN=4500rpm, PN=3.77kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",8428,"ST",1,"GMC",1,"1FT70825AH701FB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7084-1AF70-1DG1","SIMOTICS S Synchronous motor 1FT7, M0=20Nm (100K) NN=3000rpm, PN=4.56kW naturally cooled; Power connector rotatable; Vibration severity A Degree of protection IP65 Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACCURACY TOLERANCE N",5322,"ST",1,"GMC",1,"1FT70841AF701DG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7084-1AH71-1BG1","SIMOTICS S Synchronous motor 1FT7, M0=20Nm (100K) NN=4500rpm, PN=4.82kW naturally cooled; Power connector rotatable; Vibration severity A Degree of protection IP65 Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACCURACY TOLERANCE N",5207,"ST",1,"GMC",1,"1FT70841AH711BG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7084-5AC71-1BA0","SIMOTICS S Synchronous motor 1FT7, M0=20Nm (100K) NN=2000rpm, PN=3.54kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",6794,"ST",1,"GMC",1,"1FT70845AC711BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7084-5AC71-1DB1","SIMOTICS S Synchronous motor 1FT7, M0=20Nm (100K) NN=2000rpm, PN=3.54kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",8326,"ST",1,"GMC",1,"1FT70845AC711DB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7084-5AF70-1DB1","SIMOTICS S Synchronous motor 1FT7, M0=20Nm (100K) NN=3000rpm, PN=4.55kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",8326,"ST",1,"GMC",1,"1FT70845AF701DB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7084-5AF71-1CA2","SIMOTICS S Synchronous motor 1FT7, M0=20Nm (100K) NN=3000rpm, PN=4.55kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",8136,"ST",1,"GMC",1,"1FT70845AF711CA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7084-5AF71-1DA1","SIMOTICS S Synchronous motor 1FT7, M0=20Nm (100K) NN=3000rpm, PN=4.55kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",7045,"ST",1,"GMC",1,"1FT70845AF711DA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7084-5AH70-1FH2","SIMOTICS S Synchronous motor 1FT7, M0=20Nm (100K) NN=4500rpm, PN=4.82kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",9530,"ST",1,"GMC",1,"1FT70845AH701FH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7084-5AH71-1CB2","SIMOTICS S Synchronous motor 1FT7, M0=20Nm (100K) NN=4500rpm, PN=4.82kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",9416,"ST",1,"GMC",1,"1FT70845AH711CB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7084-5SF70-1CH1","SIMOTICS S Synchronous motor 1FT7, M0=27Nm (100K) NN=3000rpm, PN=7.20kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",10217,"ST",1,"GMC",1,"1FT70845SF701CH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7084-5SF71-1CK0","SIMOTICS S Synchronous motor 1FT7, M0=27Nm (100K) NN=3000rpm, PN=7.20kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",9027,"ST",1,"GMC",1,"1FT70845SF711CK0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7084-5WF75-1MH1","SIMOTICS S Synchronous motor 1FT7, M0=35Nm (100K) NN=3000rpm, PN=11.00kW water-cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact), with Pt1000  temperature sensor POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER A-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",9716,"ST",1,"GMC",1,"1FT70845WF751MH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7084-5WH71-1BK1","SIMOTICS S Synchronous motor 1FT7, M0=35Nm (100K) NN=4500rpm, PN=14.60kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",8073,"ST",1,"GMC",1,"1FT70845WH711BK1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7085-7SH70-1CA0","SIMOTICS S Synchronous motor 1FT7, M0=34Nm (100K) NN=4500rpm, PN=8.20kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",10182,"ST",1,"GMC",1,"1FT70857SH701CA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7086-1AH74-1MH1","SIMOTICS S Synchronous motor 1FT7, M0=28Nm (100K) NN=4500rpm, PN=4.71kW naturally cooled; Power connector rotatable; Vibration severity A Degree of protection IP65 Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible), with Pt1000 temperature sensor ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER A-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE, ACCURACY TOLERANCE N",7834,"ST",1,"GMC",1,"1FT70861AH741MH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7086-5AC71-1BG5","SIMOTICS S Synchronous motor 1FT7, M0=28Nm (100K) NN=2000rpm, PN=4.71kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 67",8654,"ST",1,"GMC",1,"1FT70865AC711BG5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7086-5AC71-1DG1","SIMOTICS S Synchronous motor 1FT7, M0=28Nm (100K) NN=2000rpm, PN=4.71kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",8433,"ST",1,"GMC",1,"1FT70865AC711DG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7086-5AC71-1FG2","SIMOTICS S Synchronous motor 1FT7, M0=28Nm (100K) NN=2000rpm, PN=4.71kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",9638,"ST",1,"GMC",1,"1FT70865AC711FG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7086-5AF71-1BH5","SIMOTICS S Synchronous motor 1FT7, M0=28Nm (100K) NN=3000rpm, PN=5.65kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 67",9935,"ST",1,"GMC",1,"1FT70865AF711BH5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7086-5AF71-1CH2","SIMOTICS S Synchronous motor 1FT7, M0=28Nm (100K) NN=3000rpm, PN=5.65kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",10804,"ST",1,"GMC",1,"1FT70865AF711CH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7086-5AF74-1NK2","SIMOTICS S Synchronous motor 1FT7, M0=28Nm (100K) NN=3000rpm, PN=5.65kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible), with Pt1000 temperature sensor POWER CONNECTOR ROTATABLE INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",8174,"ST",1,"GMC",1,"1FT70865AF741NK2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7086-5AH70-1FH2","SIMOTICS S Synchronous motor 1FT7, M0=28Nm (100K) NN=4500rpm, PN=4.71kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",10918,"ST",1,"GMC",1,"1FT70865AH701FH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7086-5SC71-1CH1","SIMOTICS S Synchronous motor 1FT7, M0=36Nm (100K) NN=2000rpm, PN=6.70kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",11605,"ST",1,"GMC",1,"1FT70865SC711CH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7086-5SF71-1BD1","SIMOTICS S Synchronous motor 1FT7, M0=36Nm (100K) NN=3000rpm, PN=9.10kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",9460,"ST",1,"GMC",1,"1FT70865SF711BD1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7086-5WC70-1BH1","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=2000rpm, PN=10.50kW water-cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",10513,"ST",1,"GMC",1,"1FT70865WC701BH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7086-5WF71-1CL3","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=3000rpm, PN=15.40kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",11912,"ST",1,"GMC",1,"1FT70865WF711CL3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7086-5WH71-1CH1","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=4500rpm, PN=20.30kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",11605,"ST",1,"GMC",1,"1FT70865WH711CH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7087-7SH71-1CB3","SIMOTICS S Synchronous motor 1FT7, M0=48Nm (100K) NN=4500rpm, PN=10.80kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONTRAVERSE RIGHT ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",12824,"ST",1,"GMC",1,"1FT70877SH711CB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7102-1AC71-1CH1","SIMOTICS S Synchronous motor 1FT7, M0=30Nm (100K) NN=2000rpm, PN=5.03kW naturally cooled; Power connector rotatable; Vibration severity A Degree of protection IP65 Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N",8153,"ST",1,"GMC",1,"1FT71021AC711CH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7102-5AB70-1DG0","SIMOTICS S Synchronous motor 1FT7, M0=30Nm (100K) NN=1500rpm, PN=4.08kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",7854,"ST",1,"GMC",1,"1FT71025AB701DG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7102-5AB71-1CK2","SIMOTICS S Synchronous motor 1FT7, M0=30Nm (100K) NN=1500rpm, PN=4.08kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",9309,"ST",1,"GMC",1,"1FT71025AB711CK2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7102-5AC70-1CL1","SIMOTICS S Synchronous motor 1FT7, M0=30Nm (100K) NN=2000rpm, PN=5.03kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE R VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",10640,"ST",1,"GMC",1,"1FT71025AC701CL1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7102-5AC71-1CB0","SIMOTICS S Synchronous motor 1FT7, M0=30Nm (100K) NN=2000rpm, PN=5.03kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",10275,"ST",1,"GMC",1,"1FT71025AC711CB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7102-5AF70-1CG1","SIMOTICS S Synchronous motor 1FT7, M0=30Nm (100K) NN=3000rpm, PN=6.28kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",8968,"ST",1,"GMC",1,"1FT71025AF701CG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7102-5AF71-1BG1","SIMOTICS S Synchronous motor 1FT7, M0=30Nm (100K) NN=3000rpm, PN=6.28kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",7877,"ST",1,"GMC",1,"1FT71025AF711BG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7102-5AF71-1DK3","SIMOTICS S Synchronous motor 1FT7, M0=30Nm (100K) NN=3000rpm, PN=6.28kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",8302,"ST",1,"GMC",1,"1FT71025AF711DK3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7102-5WC74-1NH1","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=2000rpm, PN=10.40kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible), with Pt1000 temperature sensor POWER CONNECTOR ROTATABLE INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",9750,"ST",1,"GMC",1,"1FT71025WC741NH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7105-1AC71-1CG1","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=2000rpm, PN=7.96kW naturally cooled; Power connector rotatable; Vibration severity A Degree of protection IP65 Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACCURACY TOLERANCE N",8673,"ST",1,"GMC",1,"1FT71051AC711CG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7105-5AB71-1BA0","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=1500rpm, PN=6.60kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",9916,"ST",1,"GMC",1,"1FT71055AB711BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7105-5AB71-1DA2","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=1500rpm, PN=6.60kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",10281,"ST",1,"GMC",1,"1FT71055AB711DA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7105-5AC70-1DA3","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=2000rpm, PN=7.96kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",10251,"ST",1,"GMC",1,"1FT71055AC701DA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7105-5AC71-1CG2","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=2000rpm, PN=7.96kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",11258,"ST",1,"GMC",1,"1FT71055AC711CG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7105-5AC74-1NG1","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=2000rpm, PN=7.96kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible), with Pt1000 temperature sensor POWER CONNECTOR ROTATABLE INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",9567,"ST",1,"GMC",1,"1FT71055AC741NG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7105-5AF70-1CB3","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=3000rpm, PN=8.80kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",12672,"ST",1,"GMC",1,"1FT71055AF701CB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7105-5AF71-1CA5","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=3000rpm, PN=8.80kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 67",11480,"ST",1,"GMC",1,"1FT71055AF711CA5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7105-5AF71-1DG3","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=3000rpm, PN=8.80kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",10251,"ST",1,"GMC",1,"1FT71055AF711DG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7105-5SC70-1CG1","SIMOTICS S Synchronous motor 1FT7, M0=65Nm (100K) NN=2000rpm, PN=11.70kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",12059,"ST",1,"GMC",1,"1FT71055SC701CG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7105-5SC71-1BH1","SIMOTICS S Synchronous motor 1FT7, M0=65Nm (100K) NN=2000rpm, PN=11.70kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",12412,"ST",1,"GMC",1,"1FT71055SC711BH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7105-5SF71-3BA0","SIMOTICS S Synchronous motor 1FT7, M0=65Nm (100K) NN=3000rpm, PN=15.10kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONAXIAL NON-DRIVE END ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",10830,"ST",1,"GMC",1,"1FT71055SF713BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7105-5SF71-4BG0","SIMOTICS S Synchronous motor 1FT7, M0=65Nm (100K) NN=3000rpm, PN=15.10kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONAXIAL DRIVE END ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",10830,"ST",1,"GMC",1,"1FT71055SF714BG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7105-5WB70-1BG1","SIMOTICS S Synchronous motor 1FT7, M0=90Nm (100K) NN=1500rpm, PN=14.10kW water-cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",10968,"ST",1,"GMC",1,"1FT71055WB701BG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7105-5WF70-4BH4","SIMOTICS S Synchronous motor 1FT7, M0=90Nm (100K) NN=3000rpm, PN=24.80kW water-cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONAXIAL DRIVE END ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",12634,"ST",1,"GMC",1,"1FT71055WF704BH4","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7105-5WF71-6BH1","SIMOTICS S Synchronous motor 1FT7, M0=90Nm (100K) NN=3000rpm, PN=24.80kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) FOR CONNECT. OF TERMINAL BOXAND SIGNAL CONNECTOR, TERMINALBOX TRAVERSE LEFT ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",12412,"ST",1,"GMC",1,"1FT71055WF716BH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7108-5AB70-1FB2","SIMOTICS S Synchronous motor 1FT7, M0=70Nm (100K) NN=1500rpm, PN=9.58kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",15686,"ST",1,"GMC",1,"1FT71085AB701FB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7108-5AB71-1BG0","SIMOTICS S Synchronous motor 1FT7, M0=70Nm (100K) NN=1500rpm, PN=9.58kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",12786,"ST",1,"GMC",1,"1FT71085AB711BG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7108-5AC70-1BH3","SIMOTICS S Synchronous motor 1FT7, M0=70Nm (100K) NN=2000rpm, PN=10.50kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",14451,"ST",1,"GMC",1,"1FT71085AC701BH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7108-5AC70-1DA3","SIMOTICS S Synchronous motor 1FT7, M0=70Nm (100K) NN=2000rpm, PN=10.50kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",13121,"ST",1,"GMC",1,"1FT71085AC701DA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7108-5AC71-1DA1","SIMOTICS S Synchronous motor 1FT7, M0=70Nm (100K) NN=2000rpm, PN=10.50kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",13037,"ST",1,"GMC",1,"1FT71085AC711DA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7108-5AC71-1DL4","SIMOTICS S Synchronous motor 1FT7, M0=70Nm (100K) NN=2000rpm, PN=10.50kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",14931,"ST",1,"GMC",1,"1FT71085AC711DL4","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7108-5AF70-1FH5","SIMOTICS S Synchronous motor 1FT7, M0=70Nm (100K) NN=3000rpm, PN=6.28kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 67",15909,"ST",1,"GMC",1,"1FT71085AF701FH5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7108-5AF71-1DG0","SIMOTICS S Synchronous motor 1FT7, M0=70Nm (100K) NN=3000rpm, PN=6.28kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",12900,"ST",1,"GMC",1,"1FT71085AF711DG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7108-5AF71-1FH1","SIMOTICS S Synchronous motor 1FT7, M0=70Nm (100K) NN=3000rpm, PN=6.28kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",15573,"ST",1,"GMC",1,"1FT71085AF711FH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7108-5SC74-1NB1","SIMOTICS S Synchronous motor 1FT7, M0=91Nm (100K) NN=2000rpm, PN=15.30kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible), with Pt1000 temperature sensor POWER CONNECTOR ROTATABLE INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",14796,"ST",1,"GMC",1,"1FT71085SC741NB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7108-5SF70-4CB0","SIMOTICS S Synchronous motor 1FT7, M0=91Nm (100K) NN=3000rpm, PN=18.80kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONAXIAL DRIVE END ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",16236,"ST",1,"GMC",1,"1FT71085SF704CB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7108-5SF71-8BG0","SIMOTICS S Synchronous motor 1FT7, M0=91Nm (100K) NN=3000rpm, PN=18.80kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) FOR CONNECT. OF TERMINAL BOXAND SIGNAL CONNECTOR, TERMINALBOX AXIAL DRIVE END ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",13700,"ST",1,"GMC",1,"1FT71085SF718BG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7108-5WB70-1FH3","SIMOTICS S Synchronous motor 1FT7, M0=125Nm (100K) NN=1500rpm, PN=19.60kW water-cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",16571,"ST",1,"GMC",1,"1FT71085WB701FH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7108-5WF70-3DA1","SIMOTICS S Synchronous motor 1FT7, M0=125Nm (100K) NN=3000rpm, PN=34.20kW water-cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONAXIAL NON-DRIVE END INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",13952,"ST",1,"GMC",1,"1FT71085WF703DA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7108-5WF71-1BH0","SIMOTICS S Synchronous motor 1FT7, M0=125Nm (100K) NN=3000rpm, PN=34.20kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONTRAVERSE RIGHT ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",15145,"ST",1,"GMC",1,"1FT71085WF711BH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7132-5AC71-1BB1","SIMOTICS S Synchronous motor 1FT7, M0=90Nm (100K) NN=2000rpm, PN=11.50kW naturally cooled; Power connector rotatable Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",16879,"ST",1,"GMC",1,"1FT71325AC711BB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7132-5AC71-1CG1","SIMOTICS S Synchronous motor 1FT7, M0=90Nm (100K) NN=2000rpm, PN=11.50kW naturally cooled; Power connector rotatable Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",15488,"ST",1,"GMC",1,"1FT71325AC711CG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7132-5SC71-7BH1","SIMOTICS S Synchronous motor 1FT7, M0=140Nm (100K) NN=2000rpm, PN=26.5 kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) FOR CONNECT. OF TERMINAL BOXAND SIGNAL CONNECTOR, TERMINALBOX AXIAL NON-DRIVE END NOT IN COMBINATION WITH DEGREE OF PROTECTION IP67 ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",17927,"ST",1,"GMC",1,"1FT71325SC717BH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7134-5AB71-1BG0","SIMOTICS S Synchronous motor 1FT7, M0=118Nm (100K) NN=1500rpm, PN=12.9kW naturally cooled; Power connector rotatable Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",16096,"ST",1,"GMC",1,"1FT71345AB711BG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7134-5SF71-7CA0","SIMOTICS S Synchronous motor 1FT7, M0=190 Nm (100K) NN=3000rpm, PN=45.5 kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) FOR CONNECT. OF TERMINAL BOXAND SIGNAL CONNECTOR, TERMINALBOX AXIAL NON-DRIVE END NOT IN COMBINATION WITH DEGREE OF PROTECTION IP67 ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",18101,"ST",1,"GMC",1,"1FT71345SF717CA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7136-5AC71-1CG1","SIMOTICS S Synchronous motor 1FT7, M0=140Nm (100K) NN=2000rpm, PN=14.9kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONTRAVERSE RIGHT ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",18773,"ST",1,"GMC",1,"1FT71365AC711CG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7136-5AC71-4CH2","SIMOTICS S Synchronous motor 1FT7, M0=140Nm (100K) NN=2000rpm, PN=14.9kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR OUTGOING CONNECTOR DIRECTION AXIAL DE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",21368,"ST",1,"GMC",1,"1FT71365AC714CH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH3103-1DF02-2LA0","main motor for SINAMICS S120;3 operating voltage 380 V 3AC Pn=5.5 kW; Nn=1500 rpm MN=35 Nm shaft height 100 mm IC22DQ shaft with feather key, half-key balancing forced ventilation, direction of air flow D IP55 compatible with SI converters vibration severity S shaft extension and flange precision power and signal port",7511,"ST",1,"GMC",1,"1PH31031DF022LA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH3107-1DF00-0LA0","Main motor 1PH3 Supply voltage 380V 3AC Pn=9kW;Nn=1500U/min Mn=57Nm Pn=9kW;Nn=1500U/min Mn=57Nm Plain shaft fan cooled, air direction DE to NDE, IP55 Matching drive SINAMICS S120 vibration level grade S shaft end and flange accuracy R power and signal cable outlet: Left/right side",7739,"ST",1,"GMC",1,"1PH31071DF000LA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH3136-1DD02-2GA0","main motor for SINAMICS S120;3 operating voltage 380 V 3AC Pn=15 kW; Nn=1000 rpm Mn=143 Nm shaft height 132 mm IC22DQ shaft with feather key, half-key balancing forced ventilation, direction of air flow D IP55 compatible with SI converters vibration severity S shaft extension and flange precision power and signal port",8112,"ST",1,"GMC",1,"1PH31361DD022GA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8083-1AF00-0BA2","SIMOTICS M compact asynchronous motor 1500 r/min 2.8 kW 17.8 Nm 7.5 A 346 V 1750 r/min 3.3 kW 18 Nm 7.5 A 398 V 2000 r/min 3.7 kW 17.7 Nm 7.6 A 447 V 2200 r/min 4.1 kW 17.8 Nm 7.6 A 480 V forced ventilation; direction of air flow DE --> NDE; IP55 degree of protection Without encoder With temperature sensor Pt1000 DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4847,"ST",1,"GMC",1,"1PH80831AF000BA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8083-1DG00-1BA1","SIMOTICS M compact asynchronous motor 2000 r/min 3.7 kW 17.7 Nm 11.6 A 293 V 2300 r/min 4.1 kW 17 Nm 11.3 A 332 V 2650 r/min 4.6 kW 16.6 Nm 11.2 A 376 V 2800 r/min 4.8 kW 16.4 Nm 11.3 A 400 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7014,"ST",1,"GMC",1,"1PH80831DG001BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8083-1DG02-2BA1","SIMOTICS M compact asynchronous motor 2000 r/min 3.7 kW 17.7 Nm 11.6 A 293 V 2300 r/min 4.1 kW 17 Nm 11.3 A 332 V 2650 r/min 4.6 kW 16.6 Nm 11.2 A 376 V 2800 r/min 4.8 kW 16.4 Nm 11.3 A 400 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7248,"ST",1,"GMC",1,"1PH80831DG022BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8083-1FF00-0GE1","SIMOTICS M compact asynchronous motor 1500 r/min 2.8 kW 17.8 Nm 7.5 A 346 V 1750 r/min 3.3 kW 18 Nm 7.5 A 398 V 2000 r/min 3.7 kW 17.7 Nm 7.6 A 447 V 2200 r/min 4.1 kW 17.8 Nm 7.6 A 480 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7978,"ST",1,"GMC",1,"1PH80831FF000GE1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8083-1HF02-1BA2","SIMOTICS M compact asynchronous motor 1500 r/min 2.8 kW 17.8 Nm 7.5 A 346 V 1750 r/min 3.3 kW 18 Nm 7.5 A 398 V 2000 r/min 3.7 kW 17.7 Nm 7.6 A 447 V 2200 r/min 4.1 kW 17.8 Nm 7.6 A 480 V forced ventilation; direction of air flow DE --> NDE; IP55 degree of protection Incremental encoder HTL 1024 S/R (encoder HTL1024S/R) With temperature sensor Pt1000 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5679,"ST",1,"GMC",1,"1PH80831HF021BA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8083-1UM02-0LH1","SIMOTICS M compact asynchronous motor 3000 r/min 4.1 kW 13.1 Nm 13.6 A 298 V 3300 r/min 4.5 kW 13 Nm 13.5 A 327 V 3600 r/min 4.9 kW 13 Nm 14 A 355 V 3900 r/min 5.3 kW 13 Nm 14 A 372 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 20-bit Without commutation position (encoder IN20DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL POWER CONNECTOR (ABOVE) CABLE ENTRY D-END SIGNAL CONNECTION LEFT",8409,"ST",1,"GMC",1,"1PH80831UM020LH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8087-1DF02-1HF1","SIMOTICS M compact asynchronous motor 1500 r/min 3.7 kW 23.6 Nm 10 A 336 V 1750 r/min 4.3 kW 23.5 Nm 10 A 396 V 2000 r/min 4.9 kW 23.4 Nm 10 A 435 V 2200 r/min 5.3 kW 23 Nm 10 A 480 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE S/A, SHAFT AND FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",7366,"ST",1,"GMC",1,"1PH80871DF021HF1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8087-1DF12-1BE1","SIMOTICS M compact asynchronous motor 1500 r/min 3.7 kW 23.6 Nm 10 A 336 V 1750 r/min 4.3 kW 23.5 Nm 10 A 396 V 2000 r/min 4.9 kW 23.4 Nm 10 A 435 V 2200 r/min 5.3 kW 23 Nm 10 A 480 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7505,"ST",1,"GMC",1,"1PH80871DF121BE1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8087-1DM12-2GH1","SIMOTICS M compact asynchronous motor 3000 r/min 4.8 kW 15.3 Nm 17.3 A 284 V 3300 r/min 5.2 kW 15 Nm 17.1 A 303 V 3600 r/min 5.7 kW 15.1 Nm 17.1 A 329 V 3900 r/min 6 kW 14.7 Nm 17.1 A 357 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY D-END SIGNAL CONNECTION LEFT",7066,"ST",1,"GMC",1,"1PH80871DM122GH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8087-1FG02-0GA1","SIMOTICS M compact asynchronous motor 2000 r/min 4.9 kW 23.4 Nm 14.1 A 320 V 2300 r/min 5.4 kW 22.4 Nm 13.7 A 353 V 2650 r/min 6 kW 21.6 Nm 13.6 A 390 V 2800 r/min 6.3 kW 21.5 Nm 13.5 A 425 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8468,"ST",1,"GMC",1,"1PH80871FG020GA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8087-1UM00-0LA1","SIMOTICS M compact asynchronous motor 3000 r/min 4.8 kW 15.3 Nm 17.3 A 284 V 3300 r/min 5.2 kW 15 Nm 17.1 A 303 V 3600 r/min 5.7 kW 15.1 Nm 17.1 A 329 V 3900 r/min 6 kW 14.7 Nm 17.1 A 357 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 20-bit Without commutation position (encoder IN20DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8432,"ST",1,"GMC",1,"1PH80871UM000LA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8101-1DF02-1GA1","SIMOTICS M compact asynchronous motor 1500 r/min 3.7 kW 24 Nm 12.5 A 265 V 1750 r/min 4.3 kW 23 Nm 12.5 A 304 V 2000 r/min 4.7 kW 22 Nm 12.5 A 343 V 2200 r/min 5.1 kW 22 Nm 12.5 A 363 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7243,"ST",1,"GMC",1,"1PH81011DF021GA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8101-1FS00-1QC1","SIMOTICS M compact asynchronous motor Y2000RPM, 4.9 kW 23 Nm, 13.2 A, 328 V D5000RPM, 4.9 kW 9 Nm, 13.5 A, 360 V Y1500RPM, 3.7 kW 24 Nm, 13.2 A, 253 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: ADVANCED LIFETIME VIBRATION SEVERITY S/A SHAFT A. FLANGE ACCURACY GR. R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",9326,"ST",1,"GMC",1,"1PH81011FS001QC1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8101-1US03-1LA1","SIMOTICS M compact asynchronous motor Y2000RPM, 4.9 kW 23 Nm, 13.2 A, 328 V D5000RPM, 4.9 kW 9 Nm, 13.5 A, 360 V Y1500RPM, 3.7 kW 24 Nm, 13.2 A, 253 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 20-bit Without commutation position (encoder IN20DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",9156,"ST",1,"GMC",1,"1PH81011US031LA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8103-1DD10-1GA1","SIMOTICS M compact asynchronous motor 1000 r/min 3.7 kW 35 Nm 10 A 333 V 1150 r/min 4.3 kW 36 Nm 10 A 380 V 1350 r/min 4.7 kW 33 Nm 9.7 A 423 V 1500 r/min 5.2 kW 33 Nm 9.7 A 470 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7107,"ST",1,"GMC",1,"1PH81031DD101GA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8103-1DF02-1GA1","SIMOTICS M compact asynchronous motor 1500 r/min 5.5 kW 35 Nm 13.5 A 368 V 1750 r/min 6.3 kW 34 Nm 13.1 A 412 V 2000 r/min 7 kW 33 Nm 12.7 A 460 V 2200 r/min 7.7 kW 33 Nm 12.7 A 480 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7408,"ST",1,"GMC",1,"1PH81031DF021GA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8103-1DF10-2DG1","SIMOTICS M compact asynchronous motor 1500 r/min 5.5 kW 35 Nm 13.5 A 368 V 1750 r/min 6.3 kW 34 Nm 13.1 A 412 V 2000 r/min 7 kW 33 Nm 12.7 A 460 V 2200 r/min 7.7 kW 33 Nm 12.7 A 480 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: SR/A, SHAFT AND FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",7954,"ST",1,"GMC",1,"1PH81031DF102DG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8103-1DG02-1CA1","SIMOTICS M compact asynchronous motor 2000 r/min 7 kW 33 Nm 17.5 A 345 V 2300 r/min 7.5 kW 31 Nm 17 A 382 V 2650 r/min 8 kW 29 Nm 16 A 434 V 2800 r/min 8.5 kW 29 Nm 16 A 455 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8147,"ST",1,"GMC",1,"1PH81031DG021CA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8103-1DM00-1LA1","SIMOTICS M compact asynchronous motor 3000 r/min 8.4 kW 27 Nm 25.7 A 297 V 3300 r/min 9.3 kW 27 Nm 25.7 A 326 V 3600 r/min 10 kW 27 Nm 25.4 A 355 V 3900 r/min 10.8 kW 26 Nm 25 A 383 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8335,"ST",1,"GMC",1,"1PH81031DM001LA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8103-1DM22-1LA1","SIMOTICS M compact asynchronous motor 3000 r/min 10.6 kW 34 Nm 30 A 309 V 3300 r/min 11.7 kW 34 Nm 30 A 340 V 3600 r/min 12.7 kW 34 Nm 29.7 A 368 V 3900 r/min 13 kW 32 Nm 29 A 397 V water cooling degree of protection IP65 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",9273,"ST",1,"GMC",1,"1PH81031DM221LA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8103-1FF10-2BA1","SIMOTICS M compact asynchronous motor 1500 r/min 5.5 kW 35 Nm 13.5 A 368 V 1750 r/min 6.3 kW 34 Nm 13.1 A 412 V 2000 r/min 7 kW 33 Nm 12.7 A 460 V 2200 r/min 7.7 kW 33 Nm 12.7 A 480 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8948,"ST",1,"GMC",1,"1PH81031FF102BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8103-1HM00-2FA2","SIMOTICS M compact asynchronous motor 3000 r/min 8.4 kW 27 Nm 25.7 A 297 V 3300 r/min 9.3 kW 27 Nm 25.7 A 326 V 3600 r/min 10 kW 27 Nm 25.4 A 355 V 3900 r/min 10.8 kW 26 Nm 25 A 383 V forced ventilation; direction of air flow DE --> NDE; IP55 degree of protection Incremental encoder HTL 1024 S/R (encoder HTL1024S/R) With temperature sensor Pt1000 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: INCREASED RADIAL FORCES, VIBRATION SEVERITY GRADE: R/A, SHAFT+FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6105,"ST",1,"GMC",1,"1PH81031HM002FA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8103-1SM00-1LA1","SIMOTICS M compact asynchronous motor 3000 r/min 8.4 kW 27 Nm 25.7 A 297 V 3300 r/min 9.3 kW 27 Nm 25.7 A 326 V 3600 r/min 10 kW 27 Nm 25.4 A 355 V 3900 r/min 10.8 kW 26 Nm 25 A 383 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 19-bit Without commutation position (encoder IN19DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",10405,"ST",1,"GMC",1,"1PH81031SM001LA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8105-1DF02-0CB1","SIMOTICS M compact asynchronous motor 1500 r/min 7 kW 45 Nm 17.5 A 348 V 1750 r/min 8 kW 44 Nm 17.5 A 400 V 2000 r/min 9 kW 43 Nm 17 A 453 V 2200 r/min 9.9 kW 43 Nm 17 A 485 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",8440,"ST",1,"GMC",1,"1PH81051DF020CB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8105-1DF03-1CA1","SIMOTICS M compact asynchronous motor 1500 r/min 7 kW 45 Nm 17.5 A 348 V 1750 r/min 8 kW 44 Nm 17.5 A 400 V 2000 r/min 9 kW 43 Nm 17 A 453 V 2200 r/min 9.9 kW 43 Nm 17 A 485 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8807,"ST",1,"GMC",1,"1PH81051DF031CA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8105-1DF12-2GC1","SIMOTICS M compact asynchronous motor 1500 r/min 7 kW 45 Nm 17.5 A 348 V 1750 r/min 8 kW 44 Nm 17.5 A 400 V 2000 r/min 9 kW 43 Nm 17 A 453 V 2200 r/min 9.9 kW 43 Nm 17 A 485 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",7701,"ST",1,"GMC",1,"1PH81051DF122GC1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8105-1FF00-1BC1","SIMOTICS M compact asynchronous motor 1500 r/min 7 kW 45 Nm 17.5 A 348 V 1750 r/min 8 kW 44 Nm 17.5 A 400 V 2000 r/min 9 kW 43 Nm 17 A 453 V 2200 r/min 9.9 kW 43 Nm 17 A 485 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",9241,"ST",1,"GMC",1,"1PH81051FF001BC1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8105-1HF02-2BA2","SIMOTICS M compact asynchronous motor 1500 r/min 7 kW 45 Nm 17.5 A 348 V 1750 r/min 8 kW 44 Nm 17.5 A 400 V 2000 r/min 9 kW 43 Nm 17 A 453 V 2200 r/min 9.9 kW 43 Nm 17 A 485 V forced ventilation; direction of air flow DE --> NDE; IP55 degree of protection Incremental encoder HTL 1024 S/R (encoder HTL1024S/R) With temperature sensor Pt1000 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6571,"ST",1,"GMC",1,"1PH81051HF022BA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8107-1DB02-2CD1","SIMOTICS M compact asynchronous motor 400 r/min 2.5 kW 60 Nm 9 A 290 V 500 r/min 3.2 kW 61 Nm 9 A 347 V 600 r/min 3.8 kW 60 Nm 9 A 406 V 700 r/min 4.4 kW 60 Nm 9 A 452 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE D-END SIGNAL CONNECTION LEFT",8867,"ST",1,"GMC",1,"1PH81071DB022CD1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8107-1DD02-1QA1","SIMOTICS M compact asynchronous motor 1000 r/min 6.3 kW 60 Nm 17.5 A 307 V 1150 r/min 7.2 kW 60 Nm 17.5 A 348 V 1350 r/min 8 kW 57 Nm 17 A 400 V 1500 r/min 8.8 kW 56 Nm 17 A 440 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: ADVANCED LIFETIME VIBRATION SEVERITY S/A SHAFT A. FLANGE ACCURACY GR. R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8900,"ST",1,"GMC",1,"1PH81071DD021QA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8107-1DF00-1BG1","SIMOTICS M compact asynchronous motor 1500 r/min 9 kW 57 Nm 23.5 A 330 V 1750 r/min 10 kW 55 Nm 22 A 380 V 2000 r/min 11 kW 53 Nm 21.5 A 428 V 2200 r/min 12.1 kW 53 Nm 21.5 A 470 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",8057,"ST",1,"GMC",1,"1PH81071DF001BG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8107-1DF02-2FB1","SIMOTICS M compact asynchronous motor 1500 r/min 9 kW 57 Nm 23.5 A 330 V 1750 r/min 10 kW 55 Nm 22 A 380 V 2000 r/min 11 kW 53 Nm 21.5 A 428 V 2200 r/min 12.1 kW 53 Nm 21.5 A 470 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: INCREASED RADIAL FORCES, VIBRATION SEVERITY GRADE: R/A, SHAFT+FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",8485,"ST",1,"GMC",1,"1PH81071DF022FB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8107-1DF13-1BB1","SIMOTICS M compact asynchronous motor 1500 r/min 9 kW 57 Nm 23.5 A 330 V 1750 r/min 10 kW 55 Nm 22 A 380 V 2000 r/min 11 kW 53 Nm 21.5 A 428 V 2200 r/min 12.1 kW 53 Nm 21.5 A 470 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",8725,"ST",1,"GMC",1,"1PH81071DF131BB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8107-1DF22-1BA1","SIMOTICS M compact asynchronous motor 1500 r/min 14 kW 89 Nm 43.7 A 277 V 1750 r/min 15.5 kW 85 Nm 42 A 314 V 2000 r/min 18 kW 86 Nm 42.6 A 363 V 2200 r/min 19.8 kW 86 Nm 42.6 A 381 V water cooling degree of protection IP65 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",9485,"ST",1,"GMC",1,"1PH81071DF221BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8107-1DG03-1BE1","SIMOTICS M compact asynchronous motor 2000 r/min 10.5 kW 50 Nm 26 A 355 V 2300 r/min 12 kW 50 Nm 26 A 406 V 2650 r/min 13 kW 47 Nm 24 A 460 V 2800 r/min 13.7 kW 47 Nm 24 A 480 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8725,"ST",1,"GMC",1,"1PH81071DG031BE1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8107-1DG13-2BC1","SIMOTICS M compact asynchronous motor 2000 r/min 10.5 kW 50 Nm 26 A 355 V 2300 r/min 12 kW 50 Nm 26 A 406 V 2650 r/min 13 kW 47 Nm 24 A 460 V 2800 r/min 13.7 kW 47 Nm 24 A 480 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",8725,"ST",1,"GMC",1,"1PH81071DG132BC1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8107-1FD00-1BA1","SIMOTICS M compact asynchronous motor 1000 r/min 6.3 kW 60 Nm 17.5 A 307 V 1150 r/min 7.2 kW 60 Nm 17.5 A 348 V 1350 r/min 8 kW 57 Nm 17 A 400 V 1500 r/min 8.8 kW 56 Nm 17 A 440 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",9459,"ST",1,"GMC",1,"1PH81071FD001BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8107-1FF12-2BA1","SIMOTICS M compact asynchronous motor 1500 r/min 9 kW 57 Nm 23.5 A 330 V 1750 r/min 10 kW 55 Nm 22 A 380 V 2000 r/min 11 kW 53 Nm 21.5 A 428 V 2200 r/min 12.1 kW 53 Nm 21.5 A 470 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",9760,"ST",1,"GMC",1,"1PH81071FF122BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8107-1HD00-2FB2","SIMOTICS M compact asynchronous motor 1000 r/min 6.3 kW 60 Nm 17.5 A 307 V 1150 r/min 7.2 kW 60 Nm 17.5 A 348 V 1350 r/min 8 kW 57 Nm 17 A 400 V 1500 r/min 8.8 kW 56 Nm 17 A 440 V forced ventilation; direction of air flow DE --> NDE; IP55 degree of protection Incremental encoder HTL 1024 S/R (encoder HTL1024S/R) With temperature sensor Pt1000 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: INCREASED RADIAL FORCES, VIBRATION SEVERITY GRADE: R/A, SHAFT+FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",6616,"ST",1,"GMC",1,"1PH81071HD002FB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8107-1HM03-0GA2","SIMOTICS M compact asynchronous motor 3000 r/min 12 kW 38 Nm 38 A 294 V 3300 r/min 13 kW 38 Nm 38 A 314 V 3600 r/min 14 kW 37 Nm 37.5 A 350 V 3900 r/min 14 kW 34 Nm 35 A 380 V forced ventilation; direction of air flow DE --> NDE; IP55 degree of protection Incremental encoder HTL 1024 S/R (encoder HTL1024S/R) With temperature sensor Pt1000 Design IM B35 (IM V15, (IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6717,"ST",1,"GMC",1,"1PH81071HM030GA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8107-1SM00-0LC1","SIMOTICS M compact asynchronous motor 3000 r/min 12 kW 38 Nm 38 A 294 V 3300 r/min 13 kW 38 Nm 38 A 314 V 3600 r/min 14 kW 37 Nm 37.5 A 350 V 3900 r/min 14 kW 34 Nm 35 A 380 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 19-bit Without commutation position (encoder IN19DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",10916,"ST",1,"GMC",1,"1PH81071SM000LC1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8131-1DF00-0FE1","SIMOTICS M compact asynchronous motor 1500 r/min 11 kW 70 Nm 24 A 360 V 1750 r/min 13 kW 71 Nm 24 A 416 V 2000 r/min 15 kW 72 Nm 24 A 460 V 2200 r/min 16.5 kW 72 Nm 24 A 500 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: INCREASED RADIAL FORCES, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8504,"ST",1,"GMC",1,"1PH81311DF000FE1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8131-1DF02-2BH1","SIMOTICS M compact asynchronous motor 1500 r/min 11 kW 70 Nm 24 A 360 V 1750 r/min 13 kW 71 Nm 24 A 416 V 2000 r/min 15 kW 72 Nm 24 A 460 V 2200 r/min 16.5 kW 72 Nm 24 A 500 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE D-END SIGNAL CONNECTION LEFT",8669,"ST",1,"GMC",1,"1PH81311DF022BH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8131-1DF13-2BA1","SIMOTICS M compact asynchronous motor 1500 r/min 11 kW 70 Nm 24 A 360 V 1750 r/min 13 kW 71 Nm 24 A 416 V 2000 r/min 15 kW 72 Nm 24 A 460 V 2200 r/min 16.5 kW 72 Nm 24 A 500 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",9136,"ST",1,"GMC",1,"1PH81311DF132BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8131-1DG23-0BA1","SIMOTICS M compact asynchronous motor 2000 r/min 18 kW 86 Nm 40 A 352 V 2300 r/min 20 kW 83 Nm 39 A 400 V 2650 r/min 23 kW 83 Nm 39 A 458 V 2800 r/min 24 kW 82 Nm 39 A 472 V water cooling degree of protection IP65 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",10320,"ST",1,"GMC",1,"1PH81311DG230BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8131-1UF12-2LA1","SIMOTICS M compact asynchronous motor 1500 r/min 11 kW 70 Nm 24 A 360 V 1750 r/min 13 kW 71 Nm 24 A 416 V 2000 r/min 15 kW 72 Nm 24 A 460 V 2200 r/min 16.5 kW 72 Nm 24 A 500 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Incremental encoder 20-bit Without commutation position (encoder IN20DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE: SPECIAL/B, SHAFT AND FLANGE ACCURACY: SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",9829,"ST",1,"GMC",1,"1PH81311UF122LA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8131-2DF02-0BE1","SIMOTICS M compact synchronous motor 1500 r/min, 15.7 kW 100 Nm, 29 A, 388 V 1750 r/min, 18 kW 98 Nm, 29 A, 415 V 2000 r/min, 19.9 kW 95 Nm, 29 A, 449 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",16898,"ST",1,"GMC",1,"1PH81312DF020BE1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8131-2FF22-1BA1","SIMOTICS M compact synchronous motor 1500 r/min, 17.6 kW 112 Nm, 40 A, 326 V 1750 r/min, 20.4 kW 112 Nm, 40 A, 377 V 2000 r/min, 23.2 kW 111 Nm, 39 A, 427 V water cooling degree of protection IP65 Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",17597,"ST",1,"GMC",1,"1PH81312FF221BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8133-1DD00-1BC1","SIMOTICS M compact asynchronous motor 1000 r/min 12 kW 115 Nm 30 A 319 V 1150 r/min 13.5 kW 112 Nm 29 A 361 V 1350 r/min 15 kW 106 Nm 28 A 417 V 1500 r/min 16.6 kW 106 Nm 28 A 459 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",8494,"ST",1,"GMC",1,"1PH81331DD001BC1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8133-1DD03-0CA1","SIMOTICS M compact asynchronous motor 1000 r/min 12 kW 115 Nm 30 A 319 V 1150 r/min 13.5 kW 112 Nm 29 A 361 V 1350 r/min 15 kW 106 Nm 28 A 417 V 1500 r/min 16.6 kW 106 Nm 28 A 459 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",9629,"ST",1,"GMC",1,"1PH81331DD030CA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8133-1DD10-2LE1","SIMOTICS M compact asynchronous motor 1000 r/min 12 kW 115 Nm 30 A 319 V 1150 r/min 13.5 kW 112 Nm 29 A 361 V 1350 r/min 15 kW 106 Nm 28 A 417 V 1500 r/min 16.6 kW 106 Nm 28 A 459 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE: SPECIAL/B, SHAFT AND FLANGE ACCURACY: SPECIAL POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",9336,"ST",1,"GMC",1,"1PH81331DD102LE1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8133-1DD13-2BA1","SIMOTICS M compact asynchronous motor 1000 r/min 12 kW 115 Nm 30 A 319 V 1150 r/min 13.5 kW 112 Nm 29 A 361 V 1350 r/min 15 kW 106 Nm 28 A 417 V 1500 r/min 16.6 kW 106 Nm 28 A 459 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",9329,"ST",1,"GMC",1,"1PH81331DD132BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8133-1DF03-0BA1","SIMOTICS M compact asynchronous motor 1500 r/min 15 kW 96 Nm 34 A 342 V 1750 r/min 17.5 kW 96 Nm 34 A 392 V 2000 r/min 20 kW 96 Nm 34 A 445 V 2200 r/min 22 kW 96 Nm 34 A 480 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",9329,"ST",1,"GMC",1,"1PH81331DF030BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8133-1DF10-2BF1","SIMOTICS M compact asynchronous motor 1500 r/min 15 kW 96 Nm 34 A 342 V 1750 r/min 17.5 kW 96 Nm 34 A 392 V 2000 r/min 20 kW 96 Nm 34 A 445 V 2200 r/min 22 kW 96 Nm 34 A 480 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R POWER CONNECTOR(ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",8494,"ST",1,"GMC",1,"1PH81331DF102BF1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8133-1DF23-1BA1","SIMOTICS M compact asynchronous motor 1500 r/min 17 kW 108 Nm 38 A 345 V 1750 r/min 19.5 kW 106 Nm 38 A 403 V 2000 r/min 22.5 kW 107 Nm 38 A 452 V 2200 r/min 24 kW 104 Nm 37 A 495 V water cooling degree of protection IP65 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",10570,"ST",1,"GMC",1,"1PH81331DF231BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8133-1DG02-0HE1","SIMOTICS M compact asynchronous motor 2000 r/min 20 kW 96 Nm 45 A 350 V 2300 r/min 22.5 kW 93 Nm 44 A 400 V 2650 r/min 24 kW 86 Nm 41 A 456 V 2800 r/min 25 kW 85 Nm 41 A 480 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8723,"ST",1,"GMC",1,"1PH81331DG020HE1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8133-1FD00-2BA1","SIMOTICS M compact asynchronous motor 1000 r/min 12 kW 115 Nm 30 A 319 V 1150 r/min 13.5 kW 112 Nm 29 A 361 V 1350 r/min 15 kW 106 Nm 28 A 417 V 1500 r/min 16.6 kW 106 Nm 28 A 459 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",9896,"ST",1,"GMC",1,"1PH81331FD002BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8133-1FD10-1BA1","SIMOTICS M compact asynchronous motor 1000 r/min 12 kW 115 Nm 30 A 319 V 1150 r/min 13.5 kW 112 Nm 29 A 361 V 1350 r/min 15 kW 106 Nm 28 A 417 V 1500 r/min 16.6 kW 106 Nm 28 A 459 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",9896,"ST",1,"GMC",1,"1PH81331FD101BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8133-1FF13-0BB1","SIMOTICS M compact asynchronous motor 1500 r/min 15 kW 96 Nm 34 A 342 V 1750 r/min 17.5 kW 96 Nm 34 A 392 V 2000 r/min 20 kW 96 Nm 34 A 445 V 2200 r/min 22 kW 96 Nm 34 A 480 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",10731,"ST",1,"GMC",1,"1PH81331FF130BB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8133-1SF02-2LB1","SIMOTICS M compact asynchronous motor 1500 r/min 15 kW 96 Nm 34 A 342 V 1750 r/min 17.5 kW 96 Nm 34 A 392 V 2000 r/min 20 kW 96 Nm 34 A 445 V 2200 r/min 22 kW 96 Nm 34 A 480 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 19-bit Without commutation position (encoder IN19DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE: SPECIAL/B, SHAFT AND FLANGE ACCURACY: SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",11773,"ST",1,"GMC",1,"1PH81331SF022LB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8133-1UF02-0LA1","SIMOTICS M compact asynchronous motor 1500 r/min 15 kW 96 Nm 34 A 342 V 1750 r/min 17.5 kW 96 Nm 34 A 392 V 2000 r/min 20 kW 96 Nm 34 A 445 V 2200 r/min 22 kW 96 Nm 34 A 480 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 20-bit Without commutation position (encoder IN20DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE: SPECIAL/B, SHAFT AND FLANGE ACCURACY: SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",10021,"ST",1,"GMC",1,"1PH81331UF020LA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8133-2DF00-0CA1","SIMOTICS M compact synchronous motor 1500 r/min, 19.9 kW 127 Nm, 44 A, 316 V 1750 r/min, 23.1 kW 126 Nm, 43 A, 366 V 2000 r/min, 26.2 kW 125 Nm, 43 A, 415 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",17582,"ST",1,"GMC",1,"1PH81332DF000CA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8133-2FL00-0GA1","SIMOTICS M compact synchronous motor 2500 r/min, 31.7 kW 121 Nm, 55 A, 371 V 2800 r/min, 35.2 kW 120 Nm, 54 A, 415 V 3000 r/min, 37.4 kW 119 Nm, 54 A, 449 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",18245,"ST",1,"GMC",1,"1PH81332FL000GA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8135-1DF00-1CA1","SIMOTICS M compact asynchronous motor 1500 r/min 18.5 kW 118 Nm 43 A 330 V 1750 r/min 21.5 kW 117 Nm 43 A 383 V 2000 r/min 24 kW 115 Nm 43 A 434 V 2200 r/min 26.4 kW 115 Nm 43 A 468 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",9438,"ST",1,"GMC",1,"1PH81351DF001CA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8135-1DF00-2QA1","SIMOTICS M compact asynchronous motor 1500 r/min 18.5 kW 118 Nm 43 A 330 V 1750 r/min 21.5 kW 117 Nm 43 A 383 V 2000 r/min 24 kW 115 Nm 43 A 434 V 2200 r/min 26.4 kW 115 Nm 43 A 468 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: ADVANCED LIFETIME VIBRATION SEVERITY S/A SHAFT A. FLANGE ACCURACY GR. R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",9801,"ST",1,"GMC",1,"1PH81351DF002QA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8135-1DF10-2BC1","SIMOTICS M compact asynchronous motor 1500 r/min 18.5 kW 118 Nm 43 A 330 V 1750 r/min 21.5 kW 117 Nm 43 A 383 V 2000 r/min 24 kW 115 Nm 43 A 434 V 2200 r/min 26.4 kW 115 Nm 43 A 468 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",9138,"ST",1,"GMC",1,"1PH81351DF102BC1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8135-1DF23-0LB1","SIMOTICS M compact asynchronous motor 1500 r/min 22 kW 140 Nm 51 A 342 V 1750 r/min 25.5 kW 139 Nm 51 A 395 V 2000 r/min 29 kW 138 Nm 52 A 448 V 2200 r/min 31 kW 135 Nm 50 A 480 V water cooling degree of protection IP65 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE: SPECIAL/B, SHAFT AND FLANGE ACCURACY: SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",12280,"ST",1,"GMC",1,"1PH81351DF230LB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8135-1FF12-1BB1","SIMOTICS M compact asynchronous motor 1500 r/min 18.5 kW 118 Nm 43 A 330 V 1750 r/min 21.5 kW 117 Nm 43 A 383 V 2000 r/min 24 kW 115 Nm 43 A 434 V 2200 r/min 26.4 kW 115 Nm 43 A 468 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",10907,"ST",1,"GMC",1,"1PH81351FF121BB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8135-1HF13-1GA2","SIMOTICS M compact asynchronous motor 1500 r/min 18.5 kW 118 Nm 43 A 330 V 1750 r/min 21.5 kW 117 Nm 43 A 383 V 2000 r/min 24 kW 115 Nm 43 A 434 V 2200 r/min 26.4 kW 115 Nm 43 A 468 V forced ventilation; direction of air flow NDE --> DE; IP55 degree of protection Incremental encoder HTL 1024 S/R (encoder HTL1024S/R) With temperature sensor Pt1000 Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7965,"ST",1,"GMC",1,"1PH81351HF131GA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8135-2DG02-0CA1","SIMOTICS M compact synchronous motor 2000 r/min, 31.4 kW 150 Nm, 59 A, 356 V 2300 r/min, 35.6 kW 148 Nm, 59 A, 407 V 2650 r/min, 40.2 kW 145 Nm, 58 A, 449 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",18700,"ST",1,"GMC",1,"1PH81352DG020CA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8135-2DG20-2QC1","SIMOTICS M compact synchronous motor 2000 r/min, 39 kW 186 Nm, 81 A, 346 V 2300 r/min, 44.3 kW 184 Nm, 80 A, 395 V 2300 r/min, 44.3 kW 184 Nm, 80 A, 395 V water cooling degree of protection IP65 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: ADVANCED LIFETIME VIBRATION SEVERITY S/A SHAFT A. FLANGE ACCURACY GR. R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",18541,"ST",1,"GMC",1,"1PH81352DG202QC1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8137-1DB00-1FA1","SIMOTICS M compact asynchronous motor 400 r/min 6.9 kW 165 Nm 18 A 323 V 500 r/min 8.6 kW 164 Nm 18 A 391 V 600 r/min 10.3 kW 164 Nm 18 A 458 V 700 r/min 11.5 kW 157 Nm 17.5 A 500 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: INCREASED RADIAL FORCES, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",9765,"ST",1,"GMC",1,"1PH81371DB001FA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8137-1DD00-2FA1","SIMOTICS M compact asynchronous motor 1000 r/min 17 kW 162 Nm 43 A 307 V 1150 r/min 19.5 kW 162 Nm 43 A 350 V 1350 r/min 22 kW 156 Nm 42 A 404 V 1500 r/min 24 kW 153 Nm 41 A 447 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: INCREASED RADIAL FORCES, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",9765,"ST",1,"GMC",1,"1PH81371DD002FA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8137-1DD03-2LA1","SIMOTICS M compact asynchronous motor 1000 r/min 17 kW 162 Nm 43 A 307 V 1150 r/min 19.5 kW 162 Nm 43 A 350 V 1350 r/min 22 kW 156 Nm 42 A 404 V 1500 r/min 24 kW 153 Nm 41 A 447 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE: SPECIAL/B, SHAFT AND FLANGE ACCURACY: SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",11239,"ST",1,"GMC",1,"1PH81371DD032LA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8137-1DD13-2GC1","SIMOTICS M compact asynchronous motor 1000 r/min 17 kW 162 Nm 43 A 307 V 1150 r/min 19.5 kW 162 Nm 43 A 350 V 1350 r/min 22 kW 156 Nm 42 A 404 V 1500 r/min 24 kW 153 Nm 41 A 447 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",9958,"ST",1,"GMC",1,"1PH81371DD132GC1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8137-1DF00-1GC1","SIMOTICS M compact asynchronous motor 1500 r/min 22 kW 140 Nm 56 A 308 V 1750 r/min 25 kW 136 Nm 56 A 352 V 2000 r/min 28 kW 134 Nm 55 A 401 V 2200 r/min 30 kW 130 Nm 53 A 440 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",9124,"ST",1,"GMC",1,"1PH81371DF001GC1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8137-1DF03-2QB1","SIMOTICS M compact asynchronous motor 1500 r/min 22 kW 140 Nm 56 A 308 V 1750 r/min 25 kW 136 Nm 56 A 352 V 2000 r/min 28 kW 134 Nm 55 A 401 V 2200 r/min 30 kW 130 Nm 53 A 440 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: ADVANCED LIFETIME VIBRATION SEVERITY S/A SHAFT A. FLANGE ACCURACY GR. R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",11060,"ST",1,"GMC",1,"1PH81371DF032QB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8137-1DF13-2LA1","SIMOTICS M compact asynchronous motor 1500 r/min 22 kW 140 Nm 56 A 308 V 1750 r/min 25 kW 136 Nm 56 A 352 V 2000 r/min 28 kW 134 Nm 55 A 401 V 2200 r/min 30 kW 130 Nm 53 A 440 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE: SPECIAL/B, SHAFT AND FLANGE ACCURACY: SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",11239,"ST",1,"GMC",1,"1PH81371DF132LA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8137-1DG02-2CB1","SIMOTICS M compact asynchronous motor 2000 r/min 28 kW 134 Nm 60 A 350 V 2300 r/min 29 kW 120 Nm 56 A 398 V 2650 r/min 30 kW 108 Nm 52 A 460 V 2800 r/min 31 kW 106 Nm 52 A 494 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",10230,"ST",1,"GMC",1,"1PH81371DG022CB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8137-1DG12-0CH1","SIMOTICS M compact asynchronous motor 2000 r/min 28 kW 134 Nm 60 A 350 V 2300 r/min 29 kW 120 Nm 56 A 398 V 2650 r/min 30 kW 108 Nm 52 A 460 V 2800 r/min 31 kW 106 Nm 52 A 494 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE D-END SIGNAL CONNECTION LEFT",10230,"ST",1,"GMC",1,"1PH81371DG120CH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8137-1FD12-1BA1","SIMOTICS M compact asynchronous motor 1000 r/min 17 kW 162 Nm 43 A 307 V 1150 r/min 19.5 kW 162 Nm 43 A 350 V 1350 r/min 22 kW 156 Nm 42 A 404 V 1500 r/min 24 kW 153 Nm 41 A 447 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",11332,"ST",1,"GMC",1,"1PH81371FD121BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8137-1FF02-2GA1","SIMOTICS M compact asynchronous motor 1500 r/min 22 kW 140 Nm 56 A 308 V 1750 r/min 25 kW 136 Nm 56 A 352 V 2000 r/min 28 kW 134 Nm 55 A 401 V 2200 r/min 30 kW 130 Nm 53 A 440 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",10893,"ST",1,"GMC",1,"1PH81371FF022GA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8137-1MB10-2GA2","SIMOTICS M compact asynchronous motor 400 r/min 6.9 kW 165 Nm 18 A 323 V 500 r/min 8.6 kW 164 Nm 18 A 391 V 600 r/min 10.3 kW 164 Nm 18 A 458 V 700 r/min 11.5 kW 157 Nm 17.5 A 500 V forced ventilation; direction of air flow NDE --> DE; IP55 degree of protection Incremental encoder SIN/COS 1 VPP 2048 S/R with C and D track (encoder IC2048S/R) with temperature sensor Pt1000 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8056,"ST",1,"GMC",1,"1PH81371MB102GA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8137-1SF12-2LA1","SIMOTICS M compact asynchronous motor 1500 r/min 22 kW 140 Nm 56 A 308 V 1750 r/min 25 kW 136 Nm 56 A 352 V 2000 r/min 28 kW 134 Nm 55 A 401 V 2200 r/min 30 kW 130 Nm 53 A 440 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Incremental encoder 19-bit Without commutation position (encoder IN19DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE: SPECIAL/B, SHAFT AND FLANGE ACCURACY: SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",12841,"ST",1,"GMC",1,"1PH81371SF122LA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8137-1UF02-0LH1","SIMOTICS M compact asynchronous motor 1500 r/min 22 kW 140 Nm 56 A 308 V 1750 r/min 25 kW 136 Nm 56 A 352 V 2000 r/min 28 kW 134 Nm 55 A 401 V 2200 r/min 30 kW 130 Nm 53 A 440 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 20-bit Without commutation position (encoder IN20DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE: SPECIAL/B, SHAFT AND FLANGE ACCURACY: SPECIAL POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE D-END SIGNAL CONNECTION LEFT",11090,"ST",1,"GMC",1,"1PH81371UF020LH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8137-2DF12-0BA1","SIMOTICS M compact synchronous motor 1500 r/min, 30.6 kW 195 Nm, 60 A, 356 V 1750 r/min, 35.6 kW 194 Nm, 59 A, 412 V 2000 r/min, 40 kW 191 Nm, 59 A, 449 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",20000,"ST",1,"GMC",1,"1PH81372DF120BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8137-2FF00-1BA1","SIMOTICS M compact synchronous motor 1500 r/min, 30.6 kW 195 Nm, 60 A, 356 V 1750 r/min, 35.6 kW 194 Nm, 59 A, 412 V 2000 r/min, 40 kW 191 Nm, 59 A, 449 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",21035,"ST",1,"GMC",1,"1PH81372FF001BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8137-2FM02-0CA1","SIMOTICS M compact synchronous motor 3000 r/min, 57.5 kW 183 Nm, 104 A, 370 V 3300 r/min, 62.2 kW 180 Nm, 102 A, 405 V 3600 r/min, 66.7 kW 177 Nm, 100 A, 440 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",21702,"ST",1,"GMC",1,"1PH81372FM020CA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8138-1DF22-0CD1","SIMOTICS M compact asynchronous motor 1500 r/min 30 kW 191 Nm 80 A 289 V 1750 r/min 33 kW 180 Nm 77 A 332 V 2000 r/min 37 kW 177 Nm 76 A 380 V 2200 r/min 39 kW 169 Nm 72 A 410 V water cooling degree of protection IP65 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE D-END SIGNAL CONNECTION LEFT",12888,"ST",1,"GMC",1,"1PH81381DF220CD1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8138-2FG22-0BA1","SIMOTICS M compact synchronous motor 2000 r/min, 59.3 kW 283 Nm, 131 A, 374 V 2300 r/min, 67.7 kW 281 Nm, 130 A, 415 V 2650 r/min, 76.3 kW 275 Nm, 30 A, 449 V water cooling degree of protection IP65 Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",22039,"ST",1,"GMC",1,"1PH81382FG220BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8163-1DB03-0CB1","SIMOTICS M compact asynchronous motor 400 r/min 9.5 kW 227 Nm 30 A 260 V 500 r/min 12 kW 229 Nm 30 A 325 V 600 r/min 14.5 kW 231 Nm 30 A 370 V 700 r/min 16.9 kW 231 Nm 30 A 427 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",12311,"ST",1,"GMC",1,"1PH81631DB030CB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8163-1DD03-0CA1","SIMOTICS M compact asynchronous motor 1000 r/min 22 kW 210 Nm 55 A 300 V 1150 r/min 25 kW 208 Nm 55 A 343 V 1350 r/min 28 kW 198 Nm 52 A 400 V 1500 r/min 31 kW 197 Nm 52 A 442 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",12311,"ST",1,"GMC",1,"1PH81631DD030CA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8163-1DD10-2FB1","SIMOTICS M compact asynchronous motor 1000 r/min 22 kW 210 Nm 55 A 300 V 1150 r/min 25 kW 208 Nm 55 A 343 V 1350 r/min 28 kW 198 Nm 52 A 400 V 1500 r/min 31 kW 197 Nm 52 A 442 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: INCREASED RADIAL FORCES, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",11587,"ST",1,"GMC",1,"1PH81631DD102FB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8163-1DF03-0HD1","SIMOTICS M compact asynchronous motor 1500 r/min 30 kW 191 Nm 71 A 319 V 1750 r/min 34 kW 186 Nm 70 A 366 V 2000 r/min 37 kW 177 Nm 68 A 416 V 2200 r/min 40.7 kW 177 Nm 68 A 456 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE D-END SIGNAL CONNECTION LEFT",12171,"ST",1,"GMC",1,"1PH81631DF030HD1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8163-1DF03-2HA1","SIMOTICS M compact asynchronous motor 1500 r/min 30 kW 191 Nm 71 A 319 V 1750 r/min 34 kW 186 Nm 70 A 366 V 2000 r/min 37 kW 177 Nm 68 A 416 V 2200 r/min 40.7 kW 177 Nm 68 A 456 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",12173,"ST",1,"GMC",1,"1PH81631DF032HA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8163-1DF20-2BA1","SIMOTICS M compact asynchronous motor 1500 r/min 37 kW 236 Nm 84 A 328 V 1750 r/min 43 kW 235 Nm 84 A 380 V 2000 r/min 49 kW 234 Nm 84 A 430 V 2200 r/min 53 kW 230 Nm 83 A 460 V water cooling degree of protection IP65 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",13491,"ST",1,"GMC",1,"1PH81631DF202BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8163-1DG13-2GA1","SIMOTICS M compact asynchronous motor 2000 r/min 36 kW 172 Nm 83 A 324 V 2300 r/min 38 kW 158 Nm 78 A 370 V 2650 r/min 40 kW 144 Nm 76 A 390 V 2800 r/min 42 kW 143 Nm 75 A 447 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",11873,"ST",1,"GMC",1,"1PH81631DG132GA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8163-1FD03-0CA1","SIMOTICS M compact asynchronous motor 1000 r/min 22 kW 210 Nm 55 A 300 V 1150 r/min 25 kW 208 Nm 55 A 343 V 1350 r/min 28 kW 198 Nm 52 A 400 V 1500 r/min 31 kW 197 Nm 52 A 442 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",13713,"ST",1,"GMC",1,"1PH81631FD030CA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8163-1HF10-1QA2","SIMOTICS M compact asynchronous motor 1500 r/min 30 kW 191 Nm 71 A 319 V 1750 r/min 34 kW 186 Nm 70 A 366 V 2000 r/min 37 kW 177 Nm 68 A 416 V 2200 r/min 40.7 kW 177 Nm 68 A 456 V forced ventilation; direction of air flow NDE --> DE; IP55 degree of protection INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) TEMPERATURE SENSOR Pt1000 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: ADVANCED LIFETIME VIBRATION SEVERITY S/A SHAFT A. FLANGE ACCURACY GR. R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",10550,"ST",1,"GMC",1,"1PH81631HF101QA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8163-1UD00-0LA1","SIMOTICS M compact asynchronous motor 1000 r/min 22 kW 210 Nm 55 A 300 V 1150 r/min 25 kW 208 Nm 55 A 343 V 1350 r/min 28 kW 198 Nm 52 A 400 V 1500 r/min 31 kW 197 Nm 52 A 442 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 20-bit Without commutation position (encoder IN20DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",12341,"ST",1,"GMC",1,"1PH81631UD000LA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8165-1DB10-2QA1","SIMOTICS M compact asynchronous motor 400 r/min 13 kW 310 Nm 36 A 300 V 500 r/min 16 kW 306 Nm 36 A 365 V 600 r/min 19 kW 302 Nm 35 A 420 V 700 r/min 22 kW 300 Nm 35 A 475 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: ADVANCED LIFETIME VIBRATION SEVERITY S/A SHAFT A. FLANGE ACCURACY GR. R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",12970,"ST",1,"GMC",1,"1PH81651DB102QA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8165-1DD00-0GA1","SIMOTICS M compact asynchronous motor 1000 r/min 28 kW 267 Nm 71 A 292 V 1150 r/min 31 kW 257 Nm 69 A 333 V 1350 r/min 34 kW 241 Nm 66 A 387 V 1500 r/min 37.7 kW 240 Nm 65 A 430 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",11422,"ST",1,"GMC",1,"1PH81651DD000GA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8165-1DD03-2CC1","SIMOTICS M compact asynchronous motor 1000 r/min 28 kW 267 Nm 71 A 292 V 1150 r/min 31 kW 257 Nm 69 A 333 V 1350 r/min 34 kW 241 Nm 66 A 387 V 1500 r/min 37.7 kW 240 Nm 65 A 430 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",13463,"ST",1,"GMC",1,"1PH81651DD032CC1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8165-1DF00-0CB1","SIMOTICS M compact asynchronous motor 1500 r/min 37 kW 236 Nm 78 A 350 V 1750 r/min 41 kW 224 Nm 76 A 400 V 2000 r/min 45 kW 215 Nm 75 A 440 V 2200 r/min 49.5 kW 215 Nm 75 A 493 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",12161,"ST",1,"GMC",1,"1PH81651DF000CB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8165-1DF03-1CC1","SIMOTICS M compact asynchronous motor 1500 r/min 37 kW 236 Nm 78 A 350 V 1750 r/min 41 kW 224 Nm 76 A 400 V 2000 r/min 45 kW 215 Nm 75 A 440 V 2200 r/min 49.5 kW 215 Nm 75 A 493 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",13463,"ST",1,"GMC",1,"1PH81651DF031CC1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8165-1DF10-2BC1","SIMOTICS M compact asynchronous motor 1500 r/min 37 kW 236 Nm 78 A 350 V 1750 r/min 41 kW 224 Nm 76 A 400 V 2000 r/min 45 kW 215 Nm 75 A 440 V 2200 r/min 49.5 kW 215 Nm 75 A 493 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",12161,"ST",1,"GMC",1,"1PH81651DF102BC1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8165-1DF13-1BB1","SIMOTICS M compact asynchronous motor 1500 r/min 37 kW 236 Nm 78 A 350 V 1750 r/min 41 kW 224 Nm 76 A 400 V 2000 r/min 45 kW 215 Nm 75 A 440 V 2200 r/min 49.5 kW 215 Nm 75 A 493 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",13162,"ST",1,"GMC",1,"1PH81651DF131BB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8165-1DG02-2CA1","SIMOTICS M compact asynchronous motor 2000 r/min 41 kW 196 Nm 88 A 350 V 2300 r/min 44 kW 183 Nm 85 A 394 V 2650 r/min 50 kW 180 Nm 85 A 440 V 2800 r/min 50 kW 171 Nm 81 A 483 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",13463,"ST",1,"GMC",1,"1PH81651DG022CA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8165-1DG13-0LC1","SIMOTICS M compact asynchronous motor 2000 r/min 41 kW 196 Nm 88 A 350 V 2300 r/min 44 kW 183 Nm 85 A 394 V 2650 r/min 50 kW 180 Nm 85 A 440 V 2800 r/min 50 kW 171 Nm 81 A 483 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",13875,"ST",1,"GMC",1,"1PH81651DG130LC1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8165-1FF03-0BA1","SIMOTICS M compact asynchronous motor 1500 r/min 37 kW 236 Nm 78 A 350 V 1750 r/min 41 kW 224 Nm 76 A 400 V 2000 r/min 45 kW 215 Nm 75 A 440 V 2200 r/min 49.5 kW 215 Nm 75 A 493 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",14264,"ST",1,"GMC",1,"1PH81651FF030BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8165-1HB13-1FB2","SIMOTICS M compact asynchronous motor 400 r/min 13 kW 310 Nm 36 A 300 V 500 r/min 16 kW 306 Nm 36 A 365 V 600 r/min 19 kW 302 Nm 35 A 420 V 700 r/min 22 kW 300 Nm 35 A 475 V forced ventilation; direction of air flow NDE --> DE; IP55 degree of protection INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) TEMPERATURE SENSOR Pt1000 Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: INCREASED RADIAL FORCES, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",11870,"ST",1,"GMC",1,"1PH81651HB131FB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8165-1UF00-0MA1","SIMOTICS M compact asynchronous motor 1500 r/min 37 kW 236 Nm 78 A 350 V 1750 r/min 41 kW 224 Nm 76 A 400 V 2000 r/min 45 kW 215 Nm 75 A 440 V 2200 r/min 49.5 kW 215 Nm 75 A 493 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 20-bit Without commutation position (encoder IN20DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: HIGH PERFORMANCE VIBRATION SEVERITY GRADE SPECIAL/B SHAFT AND FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",14410,"ST",1,"GMC",1,"1PH81651UF000MA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8165-2DF03-0CA1","SIMOTICS M compact synchronous motor 1500 r/min, 61 kW 390 Nm, 119 A, 340 V 1750 r/min, 69 kW 375 Nm, 115 A, 395 V 2000 r/min, 74 kW 355 Nm, 110 A, 445 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",24215,"ST",1,"GMC",1,"1PH81652DF030CA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8166-1DG23-0DC1","SIMOTICS M compact asynchronous motor 2000 r/min 64 kW 306 Nm 125 A 376 V 2300 r/min 72 kW 299 Nm 124 A 420 V 2650 r/min 83 kW 299 Nm 125 A 460 V 2800 r/min 87 kW 297 Nm 124 A 500 V water cooling degree of protection IP65 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE SR/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",18306,"ST",1,"GMC",1,"1PH81661DG230DC1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8166-1TF23-2LA2","SIMOTICS M compact asynchronous motor 1500 r/min 52 kW 331 Nm 116 A 332 V 1750 r/min 61 kW 333 Nm 116 A 381 V 2000 r/min 68 kW 325 Nm 116 A 426 V 2200 r/min 75 kW 326 Nm 116 A 470 V water cooling degree of protection IP65 INCREMENTAL ENCODER SIN/COS 1VPP 512 S/R WITHOUT ND-END AT TERMINAL BOX (ENCODER IC512S/R) with TEMPERATURE SENSOR PT1000 Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",18442,"ST",1,"GMC",1,"1PH81661TF232LA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8184-1AF30-2AA2","SIMOTICS M compact asynchronous motor 1500 r/min, 76 kW, 484 Nm, 162 A, 335 V 1750 r/min, 89 kW, 486 Nm, 162 A, 390 V 2000 r/min, 98 kW, 468 Nm, 156 A, 450 V open-circuit ventilation direction of air flow DE-->NDE degree of protection IP23 Without encoder With temperature sensor Pt1000 DESIGN IM B3 (IMB6, IMB7, IMB8, IMV6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD VIBRATION SEVERITY GRADE A; SHAFT A.FLANGE ACCURACY GR.N TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",14782,"ST",1,"GMC",1,"1PH81841AF302AA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8184-1DD10-0BA1","SIMOTICS M compact asynchronous motor 1000 r/min, 39 kW, 372 Nm, 87 A, 340 V 1150 r/min, 44 kW, 365 Nm, 86 A, 390 V 1350 r/min, 50 kW, 354 Nm, 84 A, 450 V forced ventilation direction of air flow NDE-->DE IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IMB6, IMB7, IMB8, IMV6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD VIBRATION SEVERITY GRADE R/A; SHAFT A.FLANGE ACCURACY GR. R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",15289,"ST",1,"GMC",1,"1PH81841DD100BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8184-1FL00-0BA1","SIMOTICS M compact asynchronous motor 2500 r/min, 78 kW 298 Nm, 166 A, 340 V 2900 r/min, 81 kW 267 Nm, 152 A, 395 V 3400 r/min, 65 kW 183 Nm, 120 A, 460 V forced ventilation direction of air flow DE-->NDE IP55 degree of protection Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IMB6, IMB7, IMB8, IMV6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD VIBRATION SEVERITY GRADE R/A; SHAFT A.FLANGE ACCURACY GR. R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",16947,"ST",1,"GMC",1,"1PH81841FL000BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8186-1AF40-1BA2","SIMOTICS M compact asynchronous motor 1500 r/min, 108 kW, 688 Nm, 225 A, 330 V 1750 r/min, 125 kW, 682 Nm, 225 A, 385 V 2000 r/min, 135 kW, 645 Nm, 210 A, 445 V open-circuit ventilation direction of air flow NDE-->DE degree of protection IP23 Without encoder With temperature sensor Pt1000 DESIGN IM B3 (IMB6, IMB7, IMB8, IMV6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD VIBRATION SEVERITY GRADE R/A; SHAFT A.FLANGE ACCURACY GR. R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",23168,"ST",1,"GMC",1,"1PH81861AF401BA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8186-1DC00-1EA1","SIMOTICS M compact asynchronous motor 700 r/min, 35 kW, 478 Nm, 83 A, 330 V 800 r/min, 40 kW, 478 Nm, 83 A, 450 V 1000 r/min, 50 kW, 478 Nm, 83 A, 450 V forced ventilation direction of air flow DE-->NDE IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IMB6, IMB7, IMB8, IMV6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: GREATER CANTILEVER FORCES; VIBRATION SEVERITY GRADE A; SHAFT AND FLANGE ACCURACY GR. N TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",21342,"ST",1,"GMC",1,"1PH81861DC001EA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8186-1DF30-2BC1","SIMOTICS M compact asynchronous motor 1500 r/min, 108 kW 688 Nm, 225 A, 330 V 1750 r/min, 125 kW 682 Nm, 225 A, 385 V 2000 r/min, 135 kW 645 Nm, 210 A, 445 V open-circuit ventilation direction of air flow DE-->NDE degree of protection IP23 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IMB6, IMB7, IMB8, IMV6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD VIBRATION SEVERITY GRADE R/A; SHAFT A.FLANGE ACCURACY GR. R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION RIGHT",25548,"ST",1,"GMC",1,"1PH81861DF302BC1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8186-2DD03-0CC1","SIMOTICS M compact synchronous motor 1000 r/min, 62 kW, 592 Nm, 148 A, 275 V 1150 r/min, 71 kW 590 Nm, 148 A, 315 V 1350 r/min, 83 kW, 587 Nm, 146 A, 368 V forced ventilation direction of air flow DE-->NDE IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 with flange A450 (IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD VIBRATION SEVERITY GRADE S/A SHAFT A.FLANGE ACCURACY GR.R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION RIGHT",33701,"ST",1,"GMC",1,"1PH81862DD030CC1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8224-1DF00-0BA1","SIMOTICS M compact asynchronous motor 1500 r/min, 95 kW, 605 Nm, 200 A, 340 V 1750 r/min, 110 kW, 600 Nm, 198 A, 395 V 2000 r/min, 124 kW, 592 Nm, 196 A, 460 V forced ventilation direction of air flow DE-->NDE IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IMB6, IMB7, IMB8, IMV6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD VIBRATION SEVERITY GRADE R/A; SHAFT A.FLANGE ACCURACY GR. R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",26299,"ST",1,"GMC",1,"1PH82241DF000BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8226-1DD00-0BA1","SIMOTICS M compact asynchronous motor 1000 r/min, 92 kW, 879 Nm, 194 A, 340 V 1150 r/min, 105 kW, 872 Nm, 192 A, 390 V 1350 r/min, 120 kW, 849 Nm, 188 A, 460 V forced ventilation direction of air flow DE-->NDE IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IMB6, IMB7, IMB8, IMV6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD VIBRATION SEVERITY GRADE R/A; SHAFT A.FLANGE ACCURACY GR. R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",32663,"ST",1,"GMC",1,"1PH82261DD000BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["3KC8456-0JA22-0GA3","SENTRON, ATE, transfer switching equipment 3KC, automatically, ATSE, 4- pole, Iu: 2000 A, Ue AC: 415 V, Ie at AC-33 B at 415 V: 1250 A, screw mounting, motorized operating mechanism, at the right end, long handle, busbar connection",19041.3,"ΤΕΜ",1,"EP",1,"3KC84560JA220GA3","3KC Μεταγωγικοί διακόπτες"]
["3KC9118-2","Accessories for 3KC0 SZ 1 Connecting jumper for load-side connection 4-pole for 3KC0 SZ1 contains 1 unit",122.96,"ΤΕΜ",1,"EP",1,"3KC91182","3KC Μεταγωγικοί διακόπτες"]
["3KC9818-3","Accessory for 3KC4, 3KC8 Connecting jumper for load-side connection 1-pole for 400 A contains 1 unit incl. 3 screws and 3 washers",67.63,"ΤΕΜ",1,"EP",1,"3KC98183","3KC Μεταγωγικοί διακόπτες"]
["3KD0342-2LG20-3","Switch disconnector 63A, size 02, 4-pole Front operating mechanism center Complete unit with direct operating mechanism gray Box terminal",115.06,"ΤΕΜ",1,"EP",1,"3KD03422LG203","3KD  Διακόπτες φορτίου μεχρι 2000Α"]
["3KD2830-2NE20-0","Switch disconnector 80 A, Size 2, 3-pole Front operating mechanism center Basic unit without handle Box terminal",104.69,"ΤΕΜ",1,"EP",1,"3KD28302NE200","3KD  Διακόπτες φορτίου μεχρι 2000Α"]
["3KD3040-0NE20-0","Switch disconnector 100 A, Size 2, 4-pole Front operating mechanism center Basic unit without handle flat terminal incl. phase barriers",160.99,"ΤΕΜ",1,"EP",1,"3KD30400NE200","3KD  Διακόπτες φορτίου μεχρι 2000Α"]
["3KD3232-2NE10-0","Switch disconnector 125 A, Size 2, 3-pole Front operating mechanism left Complete unit with direct operating mechanism gray Box terminal",217.3,"ΤΕΜ",1,"EP",1,"3KD32322NE100","3KD  Διακόπτες φορτίου μεχρι 2000Α"]
["3KD3842-0PE10-0","Switch disconnector 250 A, Size 3, 4-pole Front operating mechanism left Complete unit with direct operating mechanism gray flat terminal",455.71,"ΤΕΜ",1,"EP",1,"3KD38420PE100","3KD  Διακόπτες φορτίου μεχρι 2000Α"]
["3KD4442-0QE10-0","Switch disconnector 500 A, Size 4, 4-pole Front operating mechanism left Complete unit with direct operating mechanism gray flat terminal",872.71,"ΤΕΜ",1,"EP",1,"3KD44420QE100","3KD  Διακόπτες φορτίου μεχρι 2000Α"]
["3KD5240-0RE10-0","Switch disconnector 1250 A, Size 5, 4-pole Front operating mechanism left Basic unit without handle flat terminal",3334.25,"ΤΕΜ",1,"EP",1,"3KD52400RE100","3KD  Διακόπτες φορτίου μεχρι 2000Α"]
["3KD9201-0","Accessory for 3KD size 2 Direct operating mechanism, gray Flat version Can be locked in OFF position with one padlock",37.479999999999997,"ΤΕΜ",1,"EP",1,"3KD92010","3KD  Διακόπτες φορτίου μεχρι 2000Α"]
["3KF1308-0LB51","Switch disconnector with fuse 3KF SITOR, 80 A, Size 1, 3-pole, for LV HRC fuse Sz. 000 for semiconductor protection Front operating mechanism left, basic unit without handle, box terminal without fuses",294.08999999999997,"ΤΕΜ",1,"EP",1,"3KF13080LB51","3KF  Διακόπτες φορτίου με ασφάλειες"]
["3KF2312-0MF11","Switch disconnector with fuse 125 A, Size 2, 3-pole for LV HRC fuse Sz. 000 and 00 Front operating mechanism center Basic unit without handle flat terminal",262.33999999999997,"ΤΕΜ",1,"EP",1,"3KF23120MF11","3KF  Διακόπτες φορτίου με ασφάλειες"]
["3KF9206-0AA00","Accessory for 3KF size 2 neutral conductor terminal with removable jumper flat terminal",48.54,"ΤΕΜ",1,"EP",1,"3KF92060AA00","3KF  Διακόπτες φορτίου με ασφάλειες"]
["3KF9401-1AA00","Accessory for 3KF size 4 Direct operating mechanism, gray Can be locked in OFF position with three padlocks",69.45,"ΤΕΜ",1,"EP",1,"3KF94011AA00","3KF  Διακόπτες φορτίου με ασφάλειες"]
["3LD2050-1TL11","SENTRON, Switch disconnector 3LD, main switch, 4-pole, Iu: 16 A, Operating power / at AC-23 A at 400 V: 7.5 kW, front-mounted, knob-operated mechanism, black, central mounting 22.5 mm of the handle",44.2,"ΤΕΜ",1,"EP",1,"3LD20501TL11","3LD Διακόπτες φορτίου μεχρι 250Α"]
["3LD2130-0TK11-0AF5","SENTRON, Switch disconnector 3LD, main switch, 3-pole, Iu: 25 A, Operating power / at AC-23 A at 400 V: 9.5 kW, installation in distribution boards, knob-operated mechanism, black, handle direct at the switch",35.11,"ΤΕΜ",1,"EP",100,"3LD21300TK110AF5","3LD Διακόπτες φορτίου μεχρι 250Α"]
["3LD2244-1TL51","SENTRON, Switch disconnector 3LD, main switch, 4-pole, Iu: 32 A, Operating power / at AC-23 A at 400 V: 11.5 kW, floor mounting with door coupling, rotary operating mechanism, black, central mounting 22.5 mm of the handle",90.1,"ΤΕΜ",1,"EP",1,"3LD22441TL51","3LD Διακόπτες φορτίου μεχρι 250Α"]
["3LD2284-2GP21","SENTRON switch disconnector 3LD in molded-plastic enclosure , repair and maintenance switch with EMC plate, 3-pole Iu: 32A, AC23A 400V at 50/60Hz: 11,5kW, used with frequency converter: AC20 400V at 0-550Hz: 7,5kW, 1NO + 1NC 20-150ms leading,β€‹ molded-plastic encapsulation for metric cable gland, knob-operated mechanism, black, lockable in 0- and I-position, incl. cable shield clamps",124.95,"ΤΕΜ",1,"EP",1,"3LD22842GP21","3LD Διακόπτες φορτίου μεχρι 250Α"]
["3LD2405-0TK13","SENTRON, Switch disconnector 3LD, emergency switching-off switch, 3- pole, Iu=250 A, operating power / at AC-23 A 400 V: 132 kW, front-mounted, knob-operated mechanism, red/yellow, 4-hole mounting of the handle",469.2,"ΤΕΜ",1,"EP",1,"3LD24050TK13","3LD Διακόπτες φορτίου μεχρι 250Α"]
["3LD2565-2TC53-0AC4","SENTRON, Switch disconnector 3LD, emergency switching-off switch, 4- pole, 63 A, operating power at AC-23 A at 400 V: 22 kW, molded-plastic encapsulation for metric cable gland, rotary operating mechanism, red/yellow",168.3,"ΤΕΜ",1,"EP",1,"3LD25652TC530AC4","3LD Διακόπτες φορτίου μεχρι 250Α"]
["3LD2866-0TB53-0US2","SENTRON, Switch disconnector 3LD, emergency switching-off switch, 3- pole, Iu: 125 A, operating power / at AC-23 A 400 V: 45 kW, Molded plastic encapsulation for inch cable gland, rotary operating mechanism, red/yellow",587.35,"ΤΕΜ",1,"EP",1,"3LD28660TB530US2","3LD Διακόπτες φορτίου μεχρι 250Α"]
["3LD3148-1TK53","Load disconnector 3LD3, Iu 25 A Main switch 3-pole Rated operating capacity at AC-23 A at 400V 9.0kW floor mounting Basic switch with door coupling Central hole mounting 22.5mm Rotary actuator red / yellow 66 x 66 mm with auxiliary switch 1OE + 1S",66.91,"ΤΕΜ",1,"EP",1,"3LD31481TK53","3LD Διακόπτες φορτίου μεχρι 250Α"]
["3LD3248-1TK51","Load disconnector 3LD3, Iu 32 A Main switch 3-pole Rated operating capacity for AC-23 A at 400V 11.5kW floor mounting Basic switch with door coupling Central hole mounting 22.5mm Rotating drive black 66 x 66 mm with auxiliary switch 1OE + 1S",61.43,"ΤΕΜ",1,"EP",1,"3LD32481TK51","3LD Διακόπτες φορτίου μεχρι 250Α"]
["3LD3430-1TL13","Load disconnector 3LD3, Iu 63 A Main switch 3-pole + N Rated operating capacity at AC-23 A at 400V 22.0 kW Installation in distribution boards, Basic switch with selector knob red / yellow with auxiliary switch 1OE + 1S",67.430000000000007,"ΤΕΜ",1,"EP",1,"3LD34301TL13","3LD Διακόπτες φορτίου μεχρι 250Α"]
["3LD3450-1TK11","Load disconnector 3LD3, Iu 63 A Main switch 3-pole Rated operating capacity at AC-23 A at 400V 22.0 kW Front plate mounting Basic switch with Central hole mounting 22.5mm Toggle drive black 48x48 mm with auxiliary switch 1OE + 1S",77.63,"ΤΕΜ",1,"EP",1,"3LD34501TK11","3LD Διακόπτες φορτίου μεχρι 250Α"]
["3LD5820-0TK13","SENTRON, Molded case switch 3LD5 UL, Emergency switching-off, 3-pole, certified according to UL489 UL60947-4-1 and IEC60947-3, UL: 150A, SCCR 50kA at 480VAC, Operating power at 480VAC 3-phase: 100hp, IEC: 160A, Operating power at AC-23A at 400V: 75kW, front-mounted, rotary operating mechanism, red/yellow, 4-hole mounting of the handle, incl. terminal covers for the infeed side",377.25,"ΤΕΜ",1,"EP",1,"3LD58200TK13","3LD Διακόπτες φορτίου μεχρι 250Α"]
["3LD9250-2CA","Neutral conductor/PE terminal, continuous, for floor mounting, installation in distribution boards, Molded-plastic encapsulation, accessory for main and emergency switching-off switch 3LD25 for 63A and for molded case switch 3LD5 UL for 30A",16.239999999999998,"ΤΕΜ",1,"EP",1,"3LD92502CA","3LD Διακόπτες φορτίου μεχρι 250Α"]
["3LD9344-5C","rotary operating mechanism, red / yellow 66x66 mm Front plate mounting Central hole mounting 22.5mm mm, accessory for Load disconnector 3LD3",7.5,"ΤΕΜ",1,"EP",1,"3LD93445C","3LD Διακόπτες φορτίου μεχρι 250Α"]
["3NA3242-6","LV HRC fuse element, NH2, In: 224 A, gG, Un AC: 690 V, Un DC: 440 V, Front indicator, live grip lugs",74.06,"ΤΕΜ",1,"EP",3,"3NA32426","3ΝΑ Μαχαιρωτές ασφάλειες"]
["3NA3352-6","LV HRC fuse element, NH3, In: 315 A, gG, Un AC: 690 V, Un DC: 440 V, Front indicator, live grip lugs",146.91999999999999,"ΤΕΜ",1,"EP",3,"3NA33526","3ΝΑ Μαχαιρωτές ασφάλειες"]
["3NA6224-6","LV HRC fuse element, NH2, In: 80 A, gG, Un AC: 690 V, Un DC: 440 V, Combined indicator, Insulated grip lugs",91.59,"ΤΕΜ",1,"EP",3,"3NA62246","3ΝΑ Μαχαιρωτές ασφάλειες"]
["3NA6240","LV HRC fuse element, NH2, In: 200 A, gG, Un AC: 500 V, Un DC: 440 V, Combined indicator, Insulated grip lugs",29.28,"ΤΕΜ",1,"EP",3,"3NA6240","3ΝΑ Μαχαιρωτές ασφάλειες"]
["3NA7140","LV HRC fuse element, NH1, In: 200 A, gG, Un AC: 500 V, Un DC: 440 V, Combined indicator, live grip lugs",18.510000000000002,"ΤΕΜ",1,"EP",3,"3NA7140","3ΝΑ Μαχαιρωτές ασφάλειες"]
["3NA7817","LV HRC fuse element, NH000, In: 40 A, gG, Un AC: 500 V, Un DC: 250 V, Combined indicator, live grip lugs",6.51,"ΤΕΜ",1,"EP",3,"3NA7817","3ΝΑ Μαχαιρωτές ασφάλειες"]
["3NC1416-0MK","SITOR cylindrical fuse link, 14x51 mm, 16 A, gR, Un AC: 690 V, Un DC: 600 V",12.96,"ΤΕΜ",1,"EP",10,"3NC14160MK","3NC Κυλινδρικές ασφάλειες"]
["3NC2240-0MK","SITOR cylindrical fuse link, 22x58 mm, 40 A, gR, Un AC: 690 V, Un DC: 440 V",16.89,"ΤΕΜ",1,"EP",10,"3NC22400MK","3NC Κυλινδρικές ασφάλειες"]
["3NC3241-1U","SITOR fuse link, with slotted blade contacts, NH3, In: 1000 A, aR, Un AC: 690 V, Un DC: 440 V, front indicator",248.07,"ΤΕΜ",1,"EP",3,"3NC32411U","3NC Ασφάλειες υπερταχείας aR"]
["3NC5841","SITOR fuse link, with internal thread and bolt terminal, In: 630 A, aR, Un AC: 800 V, Un DC: 440 V, front indicator",497.45,"ΤΕΜ",1,"EP",3,"3NC5841","3NC Ασφάλειες υπερταχείας aR"]
["3ND2254","LV HRC fuse element, NH2, In: 355 A, aM, Un AC: 690 V, Un DC: 250 V, Front indicator, live grip lugs",72.48,"ΤΕΜ",1,"EP",3,"3ND2254","3ND Μαχαιρωτές ασφάλειες aM"]
["3NE1814-0","SITOR fuse link, with blade contacts, NH000, In: 20 A, gS, Un AC: 690 V, Un DC: 250 V, front indicator",49.09,"ΤΕΜ",1,"EP",3,"3NE18140","3NE Ασφάλειες υπερταχείας gS"]
["3NE5320-0MK06","SITOR fuse link, with slotted blade contacts, NH2, In: 80 A, aR, Un AC: 1500 V, Un DC: 1000 V, without Indicator",208.48,"ΤΕΜ",1,"EP",1,"3NE53200MK06","3NE Ασφάλειες υπερταχείας aR"]
["3NE8024-1","SITOR fuse link, with blade contacts, NH00, In: 160 A, aR, Un AC: 690 V, Un DC: 440 V, front indicator",71.650000000000006,"ΤΕΜ",1,"EP",3,"3NE80241","3NE Ασφάλειες υπερταχείας aR"]
["3NE8236-3MK","SITOR fuse link, with slotted blade contacts, NH1, In: 630 A, aR, Un AC: 690 V, Un DC: 440 V, front indicator",159.66,"ΤΕΜ",1,"EP",3,"3NE82363MK","3NE Ασφάλειες υπερταχείας aR"]
["3NJ4143-3BF11","In-line fuse switch disconnector 3-pole selectable, Sz. 3 I=630 A, U=690 V Screw terminal M12, new design Current transformer installation possible",970,"ΤΕΜ",1,"EP",1,"3NJ41433BF11","3NJ Ασφαλειοαποζεύκτες"]
["3NJ4912-1AA01","accessory for in-line fuse switch disconnectors 3NJ41 Cover in new design",34.54,"ΤΕΜ",1,"EP",1,"3NJ49121AA01","3NJ Ασφαλειοαποζεύκτες"]
["3NJ6312-3AA00-0AA0","Switch connector with fuses In-line design, pluggable NH1 250 A, 2-pole DC23B 230V , 100 (DC230V) kA manual operating without auxiliary switch without current transformer without ammeter",2699.24,"ΤΕΜ",1,"EP",1,"3NJ63123AA000AA0","3NJ Ασφαλειοαποζεύκτες"]
["3NJ6900-4HH21","accessory for Switch disconnector with fuses In-line design, pluggable Ammeter, Moving iron 300/5 A, Cl. 1, 0.6 VA 2-fold overload",126.75,"ΤΕΜ",1,"EP",1,"3NJ69004HH21","3NJ Ασφαλειοαποζεύκτες"]
["3NJ6930-3BG21","accessory for Switch disconnector with fuses In-line design, pluggable current transformer 250/5 A, Cl. 1, 2.5 VA",106.35,"ΤΕΜ",1,"EP",1,"3NJ69303BG21","3NJ Ασφαλειοαποζεύκτες"]
["3NJ6940-3BH22","accessory for Switch disconnector with fuses In-line design, pluggable current transformer 300/5 A, Cl. 0.5, 5 VA",309.42,"ΤΕΜ",1,"EP",1,"3NJ69403BH22","3NJ Ασφαλειοαποζεύκτες"]
["3NP1113-2BC26","SENTRON, Fuse switch disconnector 3NP1, 3-pole, NH000 narrow, 125 A, for busbar systems 60 mm, box terminal, cable outlet upwards with auxiliary switch 1 CO Cover level 32/60/70 mm",181.87,"ΤΕΜ",1,"EP",1,"3NP11132BC26","3NP Ασφαλειοαποζεύκτες"]
["3NP1141-1DA14","SENTRON, fuse switch disconnector 3NP1, 1-pole, NH1, 250 A, for assembly and installation on mounting plate, Flat terminal, Fuse monitoring electronic EFM15, cover level 70mm",304.89,"ΤΕΜ",1,"EP",1,"3NP11411DA14","3NP Ασφαλειοαποζεύκτες"]
["3NP1153-1BC14","SENTRON, fuse switch disconnector 3NP1, 3-pole, NH2, 400 A, for 60mm 8US busbar system, flat terminal, Fuse monitoring electronic EFM15, cover level 32/70 mm",848.58,"ΤΕΜ",1,"EP",1,"3NP11531BC14","3NP Ασφαλειοαποζεύκτες"]
["3NP1921-1CB00","Cable connection cover, for Size NH000 1-pole, accessories for fuse switch disconnector 3NP1",13.95,"ΤΕΜ",1,"EP",1,"3NP19211CB00","3NP Ασφαλειοαποζεύκτες"]
["3NP1924-1ED10","Mounting kit, for creation 4-pole 3NP1 for mounting on 60 mm busbar system 8US for Size NH000 with box terminal, accessory for fuse switch disconnector 3NP1",46.05,"ΤΕΜ",1,"EP",1,"3NP19241ED10","3NP Ασφαλειοαποζεύκτες"]
["3NP1953-1BB10","Prism terminal single 120 - 240 mm2, for size NH2 with screw terminal, accessory for fuse switch disconnector 3NP1 Contains 3 terminals",70.14,"ΤΕΜ",1,"EP",1,"3NP19531BB10","3NP Ασφαλειοαποζεύκτες"]
["3NP1961-1CB00","Cable connection cover, for size NH3 1-pole, accessories for 3NP1 fuse switch disconnectors",27.72,"ΤΕΜ",1,"EP",1,"3NP19611CB00","3NP Ασφαλειοαποζεύκτες"]
["3NP5260-0EA86","SENTRON, Fuse switch disconnector 3NP5, 3-pole, NH1, 250 A, for assembly and installation on mounting plate, with High-speed closing, screw terminal, Fuse monitoring: through 3RV, Auxiliary switch at Switch disconnector: 1 NO+1 NC, Auxiliary switch at the Fuse monitoring: 1 NO+1 NC",1555.18,"ΤΕΜ",1,"EP",1,"3NP52600EA86","3NP Ασφαλειοαποζεύκτες"]
["3NW6103-1","SENTRON, cylindrical fuse link, 14x51 mm, 10 A, gG, Un AC: 690 V",4.5199999999999996,"ΤΕΜ",1,"EP",10,"3NW61031","3NW Κυλινδρικές ασφάλειες "]
["3NW7354","SENTRON, cylindrical fuse holder, 8x32 mm, 1P+N, In: 20 A, Un AC: 400 V, LED signal detector",24.79,"ΤΕΜ",1,"EP",1,"3NW7354","3NW Κυλινδρικές ασφάλειες "]
["3NW8008-1","SENTRON, cylindrical fuse link, 10 x 38 mm, 8 A, aM, Un AC: 500 V",6.18,"ΤΕΜ",1,"EP",10,"3NW80081","3NW Κυλινδρικές ασφάλειες "]
["3RA1931-1BA00","Link module Electrical and mechanical For 3RV1.31 and 3RT1.3. DC operation (individual unit packaging) !!! Phased-out product !!! Successor is SIRIUS 3RA2 Preferred successor type is >>3RA2931-1AA00<<",23.69,"ΤΕΜ",1,"EP",1,"3RA19311BA00","3RA1 εξαρτήματα για 3RV/3RT/3RW"]
["3RA1954-2G","connector for YD combination, Module. S6-S6-S3 (2x 3RT1.5, 1x 3RT2.4)",62.04,"ΤΕΜ",1,"EP",1,"3RA19542G","3RA1 εξαρτήματα για 3RV/3RT/3RW"]
["3RA2110-0DD15-1FB4","Load feeder fuseless, Direct-on-line starting 400 V AC, Size S00 0.22...0.32 A 24 V DC screw terminal for 60 mm busbar systems (also fulfills type of coordination 1) Type of coordination 2, Iq = 150 kA 1 NO (contactor) with diode (integrated)",222.01,"ΤΕΜ",1,"EP",1,"3RA21100DD151FB4","3RA Εκκινητές"]
["3RA2110-1AD15-1AP0","Load feeder fuseless, Direct-on-line starting 400 V AC, Size S00 1.10...1.60 A 230 V AC screw terminal for 60 mm busbar systems (also fulfills type of coordination 1) Type of coordination 2, Iq = 150 kA 1 NO (contactor)",217.86,"ΤΕΜ",1,"EP",1,"3RA21101AD151AP0","3RA Εκκινητές"]
["3RA2110-1EA15-1FB4","Load feeder fuseless, Direct-on-line starting 400 V AC, Size S00 2.80...4.00 A 24 V DC screw terminal for installation on standard mounting rail (also fulfills type of coordination 1) Type of coordination 2, Iq = 150 kA 1 NO (contactor) with diode (integrated)",186.74,"ΤΕΜ",1,"EP",1,"3RA21101EA151FB4","3RA Εκκινητές"]
["3RA2115-0KA16-2BB4","Load feeder fuseless, Direct-on-line starting 400 V AC, Size S00 0.90...1.25 A 24 V DC screw terminal for installation on standard mounting rail (also fulfills type of coordination 1) Type of coordination 2, Iq = 150 kA 1 NC (contactor) 1 NO+1 NC (circuit breaker, transverse)",200.22,"ΤΕΜ",1,"EP",1,"3RA21150KA162BB4","3RA Εκκινητές"]
["3RA2115-1DA16-2BB4","Load feeder fuseless, Direct-on-line starting 400 V AC, Size S00 2.20...3.20 A 24 V DC screw terminal for installation on standard mounting rail (also fulfills type of coordination 1) Type of coordination 2, Iq = 150 kA 1 NC (contactor) 1 NO+1 NC (circuit breaker, transverse)",204.37,"ΤΕΜ",1,"EP",1,"3RA21151DA162BB4","3RA Εκκινητές"]
["3RA2120-4CH27-0AP0","Load feeder fuseless, Direct-on-line starting 400 V AC, Size S0 16...22 A 230 V AC Spring-type terminal for 60 mm busbar systems (also fulfills type of coordination 1) Type of coordination 2, Iq = 150 kA 1 NO+1 NC (contactor)",392.15,"ΤΕΜ",1,"EP",1,"3RA21204CH270AP0","3RA Εκκινητές"]
["3RA2120-4EH27-0AP0","Load feeder fuseless, Direct-on-line starting 400 V AC, Size S0 27.0...32.0 A 230 V AC Spring-type terminal for 60 mm busbar systems (also fulfills type of coordination 1) Type of coordination 2, Iq = 150 kA 1 NO+1 NC (contactor)",451.28,"ΤΕΜ",1,"EP",1,"3RA21204EH270AP0","3RA Εκκινητές"]
["3RA2130-4UA35-0NB3","Load feeder fuseless, Direct-on-line starting 400 V AC, Size S2 32...40 A 20 ... 33 V AC/DC screw terminal for installation on standard mounting rail (also fulfills type of coordination 1) Type of coordination 2, Iq = 100 kA 1 NO+1 NC (contactor) with circuit (integrated)",648.39,"ΤΕΜ",1,"EP",1,"3RA21304UA350NB3","3RA Εκκινητές"]
["3RA2210-0HA03-0SB4","Load feeder fuseless, Reversing duty 400 V AC, Size S00 0.55...0.80 A 24 V DC screw terminal for installation on standard mounting rail Type of coordination 1, Iq = 50 kA",433.64,"ΤΕΜ",1,"EP",1,"3RA22100HA030SB4","3RA Εκκινητές"]
["3RA2210-1EH15-2AP0","Load feeder fuseless, Reversing duty 400 V AC, Size S00 2.80...4.00 A 230 V AC Spring-type terminal for 60 mm busbar systems (also fulfills type of coordination 1) Type of coordination 2, Iq = 150 kA 1 NC (contactor)",330.94,"ΤΕΜ",1,"EP",1,"3RA22101EH152AP0","3RA Εκκινητές"]
["3RA2210-1KE17-2AP0","Load feeder fuseless, Reversing duty 400 V AC, Size S00 9.00...12.5 A 230 V AC Spring-type terminal for installation on standard mounting rail Type of coordination 1, Iq = 150 kA 1 NC (contactor)",285.3,"ΤΕΜ",1,"EP",1,"3RA22101KE172AP0","3RA Εκκινητές"]
["3RA2220-1FD24-0BB4","Load feeder fuseless, Reversing duty 400 V AC, Size S0 3.50...5.00 A 24 V DC screw terminal for 60 mm busbar systems (also fulfills type of coordination 1) Type of coordination 2, Iq = 150 kA 1 NO+1 NC (contactor)",525.97,"ΤΕΜ",1,"EP",1,"3RA22201FD240BB4","3RA Εκκινητές"]
["3RA2220-4DH27-0AP0","Load feeder fuseless, Reversing duty 400 V AC, Size S0 18...25 A 230 V AC Spring-type terminal for 60 mm busbar systems (also fulfills type of coordination 1) Type of coordination 2, Iq = 150 kA 1 NO+1 NC (contactor)",653.57000000000005,"ΤΕΜ",1,"EP",1,"3RA22204DH270AP0","3RA Εκκινητές"]
["3RA2316-8XB30-1BB4","Reversing contactor assembly AC-3, 4 kW/400 V, 24 V DC 3-pole, Size S00 screw terminal electrical and mechanical interlock",147.29,"ΤΕΜ",1,"EP",1,"3RA23168XB301BB4","3RA Εκκινητές"]
["3RA2324-8XB30-2AC2","Reversing contactor assembly AC-3,5,5 kW/400 V,AC24V,50/60Hz 3-pole, Size S0 Spring-type terminal electrical and mechanical interlock",177.3,"ΤΕΜ",1,"EP",1,"3RA23248XB302AC2","3RA Εκκινητές"]
["3RA2325-8XD30-1DM4","Reversing contactor assembly AC-3, 7.5 kW/400 V, 220 V DC 3-pole, Size S0, screw terminal, with varistor, with auxiliary switch 2x 2 NO+2 NC",410.9,"ΤΕΜ",1,"EP",1,"3RA23258XD301DM4","3RA Εκκινητές"]
["3RA2338-8XB30-1NB3","Reversing contactor assembly AC-3, 37 kW/400 V, AC/DC 20-33V 3-pole, Size S2 screw terminal electrical and mechanical Interlock 2 NO integrated",1013.17,"ΤΕΜ",1,"EP",1,"3RA23388XB301NB3","3RA Εκκινητές"]
["3RA2415-8XF31-2AB0","Contactor assembly for star-delta (wye-delta) start AC-3, 5.5 kW/400 V, 24 V AC 50/60 Hz, 3-pole, Size S00 Spring-type terminals electrical and mechanical interlock 3 NO integrated",395.89,"ΤΕΜ",1,"EP",1,"3RA24158XF312AB0","3RA Εκκινητές"]
["3RA2423-8XH32-2BB4","Contactor assembly for star-delta (wye-delta) start, AS-i AC-3, 11 kW/400 V, 24 V DC 3-pole, size S0 Spring-type terminals electrical and mechanical interlock 3 NO + 3 NC integrated",777.7,"ΤΕΜ",1,"EP",1,"3RA24238XH322BB4","3RA Εκκινητές"]
["3RA2711-0EE06","Module connector, 9 cm, for Function modules 3RA27 14-pole",17.829999999999998,"ΤΕΜ",1,"EP",1,"3RA27110EE06","3RA Εκκινητές"]
["3RA2815-2AW10","Solid-state time-delayed auxiliary switch OFF delay without control signal Relay 1 changeover contact 24...240 V AC/DC Time range 0.05...100 s Can be snapped on at the front For 3RT2 S00-S3 contactors and 3RH2 S00 contactor relays Spring-type terminal Varistor for attenuation of the contactor coil integrated",100.83,"ΤΕΜ",1,"EP",1,"3RA28152AW10","3RA Εκκινητές"]
["3RA2933-1BB1","Wiring kit Electrical and mechanical complete for load feeders for reversing fuseless, Size S2 including mechanical connectors for standard mounting rail mounting",129.34,"ΤΕΜ",1,"EP",1,"3RA29331BB1","3RA Εκκινητές"]
["3RA6120-2DP33","SIRIUS Compact load feeder DOL starter 690 V 110...240 V AC/DC 50...60 Hz 3...12 A IP20 Connection main circuit: plug-in, without terminals Connection auxiliary circuit: Spring-type terminal",745.29,"ΤΕΜ",1,"EP",1,"3RA61202DP33","3RA6 Compact εκκινητές"]
["3RA6250-2AB34","SIRIUS Compact load feeder Reversing starter 690 V 24 V AC/DC 50...60 Hz 0.1...0.4 A IP20 Connection main circuit: Spring-type terminal Connection control circuit: plug-in, without terminals",1125.03,"ΤΕΜ",1,"EP",1,"3RA62502AB34","3RA6 Compact εκκινητές"]
["3RA6250-2EP32","SIRIUS Compact load feeder Reversing starter 400 V 110...240 V AC/DC 50...60 Hz 8...32 A IP20 Connection main circuit: Spring-type terminal Connection control circuit: Spring-type terminal",1774.5,"ΤΕΜ",1,"EP",1,"3RA62502EP32","3RA6 Compact εκκινητές"]
["3RA6830-5AC","Infeed left or right Connection main circuit: Spring-type terminal Connection terminal maximum 25 mm2,",82.52,"ΤΕΜ",1,"EP",1,"3RA68305AC","3RA6 Compact εκκινητές"]
["3RB2066-2GC2","Overload relay 55...250 A for motor protection Size S10/S12, Class 20E Contactor mounting/stand-alone installation Main circuit: busbar connection Auxiliary circuit: Screw terminal Manual-Automatic-Reset",371.52,"ΤΕΜ",1,"EP",1,"3RB20662GC2","3RB Ηλεκτρονικά θερμικά"]
["3RB3026-2VE0","Overload relay 10...40 A Electronic For motor protection Size S0, Class 20 Contactor mounting Main circuit: Spring-type terminal Auxiliary circuit: Spring-type terminal Manual-Automatic-Reset",179.16,"ΤΕΜ",1,"EP",1,"3RB30262VE0","3RB Ηλεκτρονικά θερμικά"]
["3RB3123-4NB0","Overload relay 0.32...1.25 A Electronic For motor protection Size S0, Class 5...30 Contactor mounting Main circuit: Screw Auxiliary circuit: Screw Manual-Automatic-Reset Internal ground fault detection",183.18,"ΤΕΜ",1,"EP",1,"3RB31234NB0","3RB Ηλεκτρονικά θερμικά"]
["3RF2050-1AA06","Semiconductor relay, 1-phase 3RF2 Overall width 45 mm, 50 A 48-600 V / 24 V DC screw terminal",93.95,"ΤΕΜ",1,"EP",1,"3RF20501AA06","3RF Ρελέ ημιαγωγών"]
["3RF2090-1AA26","Semiconductor relay, 1-phase 3RF2 Overall width 45 mm, 90 A 48-600 V / 110-230 V AC screw terminal",117.43,"ΤΕΜ",1,"EP",1,"3RF20901AA26","3RF Ρελέ ημιαγωγών"]
["3RF2150-3AA24","Semiconductor relay, 1-phase 3RF2 Overall width 22.5 mm, 50 A 48-460 V / 110-230 V AC Ring cable connection",74.28,"ΤΕΜ",1,"EP",1,"3RF21503AA24","3RF Ρελέ ημιαγωγών"]
["3RF2310-1BA02","Solid-state contactor 1-phase 3RF2 AC 15 / 6 A / 40 Β°C 24-230 V / 24 V DC Instantaneous switching",78.77,"ΤΕΜ",1,"EP",1,"3RF23101BA02","3RF Ρελέ ημιαγωγών"]
["3RF2330-1AA22","Solid-state contactor 1-phase 3RF2 AC 51 / 30 A / 40 Β°C 24-230 V / 110-230 V AC screw terminal",98.34,"ΤΕΜ",1,"EP",1,"3RF23301AA22","3RF Ρελέ ημιαγωγών"]
["3RF2340-3AA06","Solid-state contactor 1-phase 3RF2 AC 51 / 40 A / 40 Β°C 48-600 V / 24 V DC Ring cable connection",137.49,"ΤΕΜ",1,"EP",1,"3RF23403AA06","3RF Ρελέ ημιαγωγών"]
["3RF2350-3AA04","Solid-state contactor 1-phase 3RF2 AC 51 / 50 A / 40 Β°C 48-460 V / 24 V DC Ring cable connection",130.81,"ΤΕΜ",1,"EP",1,"3RF23503AA04","3RF Ρελέ ημιαγωγών"]
["3RF2950-0KA13","power controller current range 50 A / 40 Β°C 110 β€¦ 230 V 24 V AC/DC with partial load monitoring for semiconductor relay / contactor",401.01,"ΤΕΜ",1,"EP",1,"3RF29500KA13","3RF Ρελέ ημιαγωγών"]
["3RG9002-0DA00","AS-Interface module F90, digital 4 DI/4 DQ, IP20 4 x inputs for 3-wire sensor 4 x output, 2 A, 24 V DC maximal 6 A for all outputs Connection via screw terminals Width 90 mm",392.51,"ΤΕΜ",1,"EP",1,"3RG90020DA00","3RG AS-Interface module"]
["3RH2122-1AH00","Contactor relay, 2 NO + 2 NC, 48 V AC, 50 / 60 Hz, Size S00, screw terminal",40.24,"ΤΕΜ",1,"EP",1,"3RH21221AH00","3RH21 βοηθητικά ρελέ"]
["3RH2122-1MB40-0KT0","Coupling contactor relay, 2 NO + 2 NC 24 V DC, 0.85 ... 1.85* US, Size S00, screw terminal",46.59,"ΤΕΜ",1,"EP",1,"3RH21221MB400KT0","3RH21 βοηθητικά ρελέ"]
["3RH2122-4AR60","Contactor relay, 2 NO + 2 NC, 400 V AC, 50 Hz, 400 .. 440 V, 60 Hz, Size S00, ring cable lug connection",44.21,"ΤΕΜ",1,"EP",1,"3RH21224AR60","3RH21 βοηθητικά ρελέ"]
["3RH2131-1JB40","Coupling contactor relay, 3 NO + 1 NC, 24 V DC, 0.7 ... 1.25* US, with integrated diode, Size S00, screw terminal suitable for PLC outputs",53.79,"ΤΕΜ",1,"EP",1,"3RH21311JB40","3RH21 βοηθητικά ρελέ"]
["3RH2131-2LF40-0LA0","Contactor relay for railway, 3 NO, 110 V DC, 0.7 ... 1.25* US, with integrated varistor, 3-pole, integrated, Size S00, Spring-type terminal",80.22,"ΤΕΜ",1,"EP",1,"3RH21312LF400LA0","3RH21 βοηθητικά ρελέ"]
["3RH2140-1SB40","Coupling contactor relay, 4 NO 24 V DC, 0.85-1.85*US with integrated suppressor diode Size S00 screw terminal",52.4,"ΤΕΜ",1,"EP",1,"3RH21401SB40","3RH21 βοηθητικά ρελέ"]
["3RH2140-4AN60","Contactor relay, 4 NO, 200 V AC, 50 Hz, 200 .. 220 V, 60 Hz, Size S00, ring cable lug connection",44.21,"ΤΕΜ",1,"EP",1,"3RH21404AN60","3RH21 βοηθητικά ρελέ"]
["3RH2344-1DM40","Contactor relay with auxiliary switch 220 V DC Size S00, screw terminal, 4 NC basic unit / EN Varistor plugged on",86.38,"ΤΕΜ",1,"EP",1,"3RH23441DM40","3RH21 βοηθητικά ρελέ"]
["3RH2911-1AA10","Auxiliary switch on the front, 1 NO Current path 1 NO Connection from top for 3RH and 3RT screw terminal 73/74",9.3699999999999992,"ΤΕΜ",1,"EP",1,"3RH29111AA10","3RH βοηθητικές επαφές για 3RT"]
["3RH2911-1XA31-0MA0","Auxiliary switch on the front, 3 NO + 1 NC Current path 1 NO, 1 NC, 1 NO, 1 NO for 3RH and 3RT screw terminal 53/54, 61/62, 71374, 83/84",20.059999999999999,"ΤΕΜ",1,"EP",1,"3RH29111XA310MA0","3RH βοηθητικές επαφές για 3RT"]
["3RH2911-4GA40","Auxiliary switch on the front, 4 NO Current path 1 NO, 1 NO, 1 NO, 1 NO for contactor relays Size S00 Ring cable lug connection 53/54, 63/64, 73/74, 83/84 Physically coded; only with contactor relays 3RH2140* and 3RH2440* can be combined (according to EN 50011)",20.059999999999999,"ΤΕΜ",1,"EP",1,"3RH29114GA40","3RH βοηθητικές επαφές για 3RT"]
["3RK1200-0CQ00-0AA3","AS-i compact module K60 digital 4 DI, IP67 4 x input, maximum 200 mA 4 x M12 socket Y-II assignment Mounting plate 3RK1901-0CA00 must be ordered separately",264.16000000000003,"ΤΕΜ",1,"EP",1,"3RK12000CQ000AA3","3RK AS-I module"]
["3RK1304-0HS00-6AA0","ET 200 RSM Maintenance switch module Up to 25 A Up to 25 A Disconnector function for Main circuit Han Q4/2",708.13,"ΤΕΜ",1,"EP",1,"3RK13040HS006AA0","3RK ET200 εκκινητές"]
["3RK1315-6LS41-1AA0","SIRIUS motor starter M200D AS-i Communication: AS-Interface Reversing starter Basic Mechanical switching AC-3, 5.5 kW / 400 V 1.5 A...12.00 A Electronic overload protection Thermistor: THERMOCLICK / PTC without brake contact 2DI AS-i + 2DI / 1DO on device Han Q4/2 - Han Q8/0",1253.27,"ΤΕΜ",1,"EP",1,"3RK13156LS411AA0","3RK ET200 εκκινητές"]
["3RK1325-6KS71-3AA3","SIRIUS motor starter M200D AS-i Communication: AS-Interface Reversing starter standard Electronic switching AC-3, 0.75KW / 400 V 0.15 A...2.00 A Electronic overload protection Thermistor: THERMOCLICK / PTC with brake contact 400 V AC 4 DI / 1 DO AS-i Han Q4/2 - Han Q8/0 with manual on-site operation and key-operated switch",1787.25,"ΤΕΜ",1,"EP",1,"3RK13256KS713AA3","3RK ET200 εκκινητές"]
["3RK1400-0CE00-0AA3","AS-i flat module, digital 4 DI/4 DQ, IP20 4 x inputs for 3-wire sensor 4 x output, 24 V DC Output supply via U_ASI Screw terminals",266.99,"ΤΕΜ",1,"EP",1,"3RK14000CE000AA3","3RK AS-I module"]
["3RK1400-1DQ02-0AA3","AS-i compact module K60 digital 2 x (2 DI/2 DQ), IP67 2 x 2 inputs, maximum 200 mA 2 x 2 outputs, 1 A, 24 V DC 4 x M12 standard socket Y assignment Mounting plate 3RK1901-0CA00 must be ordered separately",410.45,"ΤΕΜ",1,"EP",1,"3RK14001DQ020AA3","3RK AS-I module"]
["3RK1901-3MB00","3-pole screw terminal for AS-i data decoupling DCM 1271 for connection of the power supply unit",12.24,"ΤΕΜ",1,"EP",1,"3RK19013MB00","3RK AS-I module"]
["3RK1911-0DB13","Energy connection cable single-sided, open on one side Han Q4/2 angled 4 x 4 mm2 Length 1.5 m",239.4,"ΤΕΜ",1,"EP",1,"3RK19110DB13","3RK AS-I module"]
["3RK2100-1CE00-2AA2","AS-i SlimLine Compact module SC22.5 digital, A/B slave 4 DQ, IP20 4 x output, 2 A, 24 V DC maximal 4 A for all outputs Screw terminals Width 22.5 mm",272.97000000000003,"ΤΕΜ",1,"EP",1,"3RK21001CE002AA2","3RK AS-I module"]
["3RK4324-3CR51-1BC0","SIRIUS MCU motor starter Enclosure degree of protection IP54 plastic Communication AS-Interface electromechanically switching Short-circuit protection with circuit breaker Reversing starter Brake without Performance class 1 A Motor circuit breaker with bi-metal thermal without manual operation Connection power M screw connection Special variant new design A/B slave AS-i SPEC V2.1 Sensor-actuator 1x AS-i 3xDI/DO Supply sensor U-AUX",1686.65,"ΤΕΜ",1,"EP",1,"3RK43243CR511BC0","3RK AS-I module"]
["3RK4340-3MR51-0BA0","SIRIUS MCU motor starter Enclosure degree of protection IP55 plastic Communication without electromechanically switching Short-circuit protection with circuit breaker DOL starter Brake without Performance class 8.00 A Motor circuit breaker with bi-metal thermal Manual operation without Connection power M screw connection Standard product",810.59,"ΤΕΜ",1,"EP",1,"3RK43403MR510BA0","3RK AS-I module"]
["3RM1101-1AA04","Fail-safe direct starter, 3RM1, 500 V, 0 - 0.12 kW, 0.1 - 0.5 A, 24 V DC, screw terminals",287.33999999999997,"ΤΕΜ",1,"EP",1,"3RM11011AA04","3RM Εκκινητές μέχρι 7Α"]
["3RM1201-2AA14","Reversing starter, 3RM1, 500 V, 0 - 0.12 kW, 0.1 - 0.5 A, 110-230 V AC, spring-type terminals",270.98,"ΤΕΜ",1,"EP",1,"3RM12012AA14","3RM Εκκινητές μέχρι 7Α"]
["3RN2000-2AW30","Thermistor motor protection relay Compact evaluation unit, 17.5 mm enclosure, spring-type terminals, 1 changeover contact, US = 24 V-240 V AC/DC, Auto RESET, suitable for bimetallic switch, supply =output voltage, 1 LED (tripped)",73.180000000000007,"ΤΕΜ",1,"EP",1,"3RN20002AW30","3RN Ρελέ επιτήρησης θερμίστορ"]
["3RP2535-2AW30","Timing relay, OFF delay with control signal 1 change-over contact, 15 time ranges 0.05 s...100 h 12-240 V DC, Wide voltage range at 50/60 Hz AC with LED, Spring-type terminal (push-in)",120.03,"ΤΕΜ",1,"EP",1,"3RP25352AW30","3RP Χρονικά "]
["3RQ3038-2AF01","Input coupler Relay coupler, 1 change-over contact hard gold-plated 230 V AC/DC Spring-type terminal (push-in) Overall width 6.2 mm Thermal current 6A",59.84,"ΤΕΜ",1,"EP",5,"3RQ30382AF01","3RQ Coupling ρελέ"]
["3RQ3118-1AE00","Output coupler with plug-in Relay, 1 change-over contact screw terminal 115 V AC/DC Enclosure width 6.2 mm Thermal current 6A",34.700000000000003,"ΤΕΜ",1,"EP",5,"3RQ31181AE00","3RQ Coupling ρελέ"]
["3RR2243-1FW30","Monitoring relay, can be mounted to Contactor 3RT2, Size S2 standard, digitally adjustable Apparant/active current monitoring 8...80 A, 20...400 Hz, 3-phase Supply 24-240 V AC/DC 1 change-over contact, 1 semiconductor output for alarm and warning Monitoring for Current overshoot and undershoot Phase failure, Cable break Phase sequence Residual current Blocking current Warning and alarm thresholds with or without fault buffer ON delay 0-99 s Noise pulse suppression 0-30 s Pause after fault 0-300 min Screw connection system",399.94,"ΤΕΜ",1,"EP",1,"3RR22431FW30","3RR Επιτηρητές εντασης"]
["3RT1054-1AU36","Power contactor, AC-3 115 A, 55 kW / 400 V AC (50-60 Hz) / DC operation 240-277 V UC Auxiliary contacts 2 NO + 2 NC 3-pole, Size S6 with box terminals Drive: conventional screw terminal",484.41,"ΤΕΜ",1,"EP",1,"3RT10541AU36","3RT Ρελέ ισχύος"]
["3RT1054-3AV36","Power contactor, AC-3 115 A, 55 kW / 400 V AC (50-60 Hz) / DC operation 380-420 V UC Auxiliary contacts 2 NO + 2 NC 3-pole, Size S6 with box terminals Drive: conventional Spring-type terminal",484.41,"ΤΕΜ",1,"EP",1,"3RT10543AV36","3RT Ρελέ ισχύος"]
["3RT1055-6SP36-3PA0","Power contactor, AC-3 150 A, 75 kW / 400 V Coil AC 50/60 Hz and DC 200-277 V x (0.8-1.1) F-SPS input 24 V DC 3-pole size S6 Auxiliary contacts 2 NO + 2 NC permanently mounted Main circuit: Busbar Control and auxiliary circuit: Screw terminal",693.59,"ΤΕΜ",1,"EP",1,"3RT10556SP363PA0","3RT Ρελέ ισχύος"]
["3RT1056-6AV36","Power contactor, AC-3 185 A, 90 kW / 400 V AC (50-60 Hz) / DC operation 380-420 V UC Auxiliary contacts 2 NO + 2 NC 3-pole, Size S6 Busbar connections Drive: conventional screw terminal",692.86,"ΤΕΜ",1,"EP",1,"3RT10566AV36","3RT Ρελέ ισχύος"]
["3RT1065-2AT36","Power contactor, AC-3 265 A, 132 kW / 400 V AC (50-60 Hz) / DC operation 575-600 V UC Auxiliary contacts 2 NO + 2 NC 3-pole, Size S10 Busbar connections Drive: conventional Spring-type terminal",1207.8399999999999,"ΤΕΜ",1,"EP",1,"3RT10652AT36","3RT Ρελέ ισχύος"]
["3RT1065-6NP36-3PA0","Power contactor, AC-3 265 A, 132 kW / 400 V AC (50-60 Hz) / DC operation 200-277 V UC Auxiliary contacts 2 NO + 2 NC 3-pole, Size S10 Busbar connections Drive: electronic with PLC interface 24 V DC screw terminal Captive auxiliary switch DIN 50012",1315.54,"ΤΕΜ",1,"EP",1,"3RT10656NP363PA0","3RT Ρελέ ισχύος"]
["3RT1076-2AM36","Power contactor, AC-3 500 A, 250 kW / 400 V AC (50-60 Hz) / DC 200-220 V UC Auxiliary contacts 2 NO + 2 NC 3-pole, size S12 Busbar connections Operating mechanism: conventional Spring-type terminals",2181.14,"ΤΕΜ",1,"EP",1,"3RT10762AM36","3RT Ρελέ ισχύος"]
["3RT1076-6AR36","Power contactor, AC-3 500 A, 250 kW / 400 V AC (50-60 Hz) / DC 440-480 V UC Auxiliary contacts 2 NO + 2 NC 3-pole, size S12 Busbar connections Operating mechanism: conventional screw terminals",2082.9699999999998,"ΤΕΜ",1,"EP",1,"3RT10766AR36","3RT Ρελέ ισχύος"]
["3RT1265-6NB36","Vacuum contactor, AC-3 265 A, 132 kW / 400 V AC (50-60 Hz) / DC operation 21-27.3 V UC Auxiliary contacts 2 NO + 2 NC 3-pole, Size S10 Busbar connections Drive: electronic with PLC interface 24 V DC",2109.46,"ΤΕΜ",1,"EP",1,"3RT12656NB36","3RT Ρελέ ισχύος"]
["3RT1374-6AP36","Contactor, AC-1, 500 A/400 V/40 Β°C, S12, 4-pole, 100-250 V AC/DC, 2 NO+2 NC, Connection rail/ screw terminal",3039.52,"ΤΕΜ",1,"EP",1,"3RT13746AP36","3RT Ρελέ ισχύος"]
["3RT1476-6AR36","Contactor, AC-1, 690 A/690 V/40 Β°C, S12, 3-pole, 440-480 V AC/DC, with varistor, 2 NO+2 NC, Connection rail/ screw terminal",2134.77,"ΤΕΜ",1,"EP",1,"3RT14766AR36","3RT Ρελέ ισχύος"]
["3RT1926-2ED11","solid-state time-delayed front-side auxiliary switch Time range 0.05...1 s, 200 ... 240 V AC, 1 NO contact, 1 NC contact ON delay, for 3RT1",98.27,"ΤΕΜ",1,"EP",1,"3RT19262ED11","3RT Ρελέ ισχύος"]
["3RT1926-4RD01","Adapter for motor outgoing connector 3RT1900-4RE01 for 3RT2.2",28.78,"ΤΕΜ",1,"EP",1,"3RT19264RD01","3RT Ρελέ ισχύος"]
["3RT1956-4G","Box terminal for contactor 3RT1, 3RB2 Size S6 max. connection approx. 120 mm2",64.48,"ΤΕΜ",1,"EP",1,"3RT19564G","3RT Ρελέ ισχύος"]
["3RT1965-6A","Replacement contact pieces for 3RT1065 consists of 3 movable and 6 fixed contacts with mounting parts",732.64,"ΤΕΜ",1,"EP",1,"3RT19656A","3RT Ρελέ ισχύος"]
["3RT1983-5AP31","Changeover operating mechanism for 3RT1483, AC (50...60 Hz) / DC operation 100...240 V AC / 100...220 V DC",644.45000000000005,"ΤΕΜ",1,"EP",1,"3RT19835AP31","3RT Ρελέ ισχύος"]
["3RT2015-1AR62","Power contactor, AC-3 7 A, 3 kW / 400 V 1 NC, 400 V AC, 50 Hz 400-440 V, 60 Hz, 3-pole, Size S00, screw terminal",39.32,"ΤΕΜ",1,"EP",1,"3RT20151AR62","3RT Ρελέ ισχύος"]
["3RT2015-2AP02-1AA0","Power contactor, AC-3 7 A, 3 kW / 400 V 1 NC, 220 V AC, 50 / 60 Hz 3-pole, Size S00 Spring-type terminal upright mounting position",39.06,"ΤΕΜ",1,"EP",1,"3RT20152AP021AA0","3RT Ρελέ ισχύος"]
["3RT2015-2BM42","Power contactor, AC-3 7 A, 3 kW / 400 V 1 NC, 220 V DC 3-pole, Size S00 Spring-type terminal",41.7,"ΤΕΜ",1,"EP",1,"3RT20152BM42","3RT Ρελέ ισχύος"]
["3RT2015-4BB42","Power contactor, AC-3 7 A, 3 kW / 400 V 1 NC, 24 V DC 3-pole, Size S00 ring cable lug connection",41.7,"ΤΕΜ",1,"EP",1,"3RT20154BB42","3RT Ρελέ ισχύος"]
["3RT2016-1CK64-3MA0","Power contactor, AC-3 9 A, 4 kW / 400 V 2 NO + 2 NC, 110 V AC, 50 Hz 120 V, 60 Hz, with plugged on varistor, 3-pole, Size S00 Screw terminal Captive auxiliary switch",69.099999999999994,"ΤΕΜ",1,"EP",1,"3RT20161CK643MA0","3RT Ρελέ ισχύος"]
["3RT2016-2AD01","Power contactor, AC-3 9 A, 4 kW / 400 V 1 NO, 42 V AC, 50 / 60 Hz, 3-pole, Size S00 Spring-type terminal",40.99,"ΤΕΜ",1,"EP",1,"3RT20162AD01","3RT Ρελέ ισχύος"]
["3RT2016-2XF41-0LA2","Traction contactor, AC-3 9 A, 4 kW / 400 V 1 NO, 72 - 125 V DC, 0.7-1.25* US with integrated varistor Size S00, Spring-type terminal suitable for PLC outputs",78.75,"ΤΕΜ",1,"EP",1,"3RT20162XF410LA2","3RT Ρελέ ισχύος"]
["3RT2017-1AD02-1AA0","power contactor, AC-3 12 A, 5.5 kW / 400 V 1 NC, 42 V AC, 50 / 60 Hz 3-pole, frame size S00 screw terminal upright mounting position",54.32,"ΤΕΜ",1,"EP",1,"3RT20171AD021AA0","3RT Ρελέ ισχύος"]
["3RT2017-2AK64-3MA0","Power contactor, AC-3 12 A, 5.5 kW / 400 V 2 NO + 2 NC, 110 V AC, 50 Hz 120 V, 60 Hz 3-pole, Size S00 Spring type terminal Captive auxiliary switch",64.53,"ΤΕΜ",1,"EP",1,"3RT20172AK643MA0","3RT Ρελέ ισχύος"]
["3RT2017-2BF41","power contactor, AC-3 12 A, 5.5 kW / 400 V 1 NO, 110 V DC 3-pole, Size S00 Spring-type terminal",50.09,"ΤΕΜ",1,"EP",1,"3RT20172BF41","3RT Ρελέ ισχύος"]
["3RT2018-1AF01","Contactor, AC-3, 7.5 KW / 400 V, 1 NO, 110 V AC, 50 / 60 Hz, 3-pole, Size S00 screw terminal",56.26,"ΤΕΜ",1,"EP",1,"3RT20181AF01","3RT Ρελέ ισχύος"]
["3RT2018-1AS01","Power contactor, AC-3 16 A, 7.5 kW / 400 V 1 NO, 500 V AC, 50/60 Hz 3-pole, Size S00 screw terminals",59.88,"ΤΕΜ",1,"EP",1,"3RT20181AS01","3RT Ρελέ ισχύος"]
["3RT2018-2BW42","Power contactor, AC-3 16 A, 7.5 kW / 400 V 1 NC, 48 V DC 3-pole, Size S00 Spring-type terminals",90.15,"ΤΕΜ",1,"EP",1,"3RT20182BW42","3RT Ρελέ ισχύος"]
["3RT2023-1AF00","power contactor, AC-3 9 A, 4 kW / 400 V 1 NO + 1 NC, 110 V AC, 50 Hz 3-pole, Size S0 screw terminal",39.97,"ΤΕΜ",1,"EP",1,"3RT20231AF00","3RT Ρελέ ισχύος"]
["3RT2023-2NB30","power contactor, AC-3 9 A, 4 kW / 400 V 1 NO + 1 NC, AC (50-60 Hz) DC operation 21-28 V AC/DC, 3-pole, Size S0, Spring-type terminal",105.11,"ΤΕΜ",1,"EP",1,"3RT20232NB30","3RT Ρελέ ισχύος"]
["3RT2024-1AG20","power contactor, AC-3 12 A, 5.5 kW / 400 V 1 NO + 1 NC, 110 V AC 50 / 60 Hz, 3-pole Size S0, screw terminal",47.07,"ΤΕΜ",1,"EP",1,"3RT20241AG20","3RT Ρελέ ισχύος"]
["3RT2024-1CK64-3MA0","Power contactor, AC-3 12 A, 5.5 kW / 400 V 2 NO + 2 NC, 110 V AC, 50 Hz 120 V, 60 Hz, with plugged-in varistor, 3-pole, Size S0 Screw terminal Captive auxiliary switch",76.760000000000005,"ΤΕΜ",1,"EP",1,"3RT20241CK643MA0","3RT Ρελέ ισχύος"]
["3RT2025-1AD20-1AA0","power contactor, AC-3 17 A, 7.5 kW / 400 V 1 NO + 1 NC, 42 V AC, 50 / 60 Hz, 3-pole, Size S0, screw terminal upright mounting position",73.510000000000005,"ΤΕΜ",1,"EP",1,"3RT20251AD201AA0","3RT Ρελέ ισχύος"]
["3RT2025-2AL24-3MA0","Power contactor, AC-3 17 A, 7.5 kW / 400 V 2 NO + 2 NC, 230 V AC, 50/60 Hz 3-pole, Size S0 Spring type terminal Captive auxiliary switch",81.37,"ΤΕΜ",1,"EP",1,"3RT20252AL243MA0","3RT Ρελέ ισχύος"]
["3RT2025-4AR60","power contactor, AC-3 17 A, 7.5 kW / 400 V 1 NO + 1 NC, 400 V AC, 50 Hz, 400-440 V, 60 Hz, 3-pole, Size S0, ring cable lug connection",66.86,"ΤΕΜ",1,"EP",1,"3RT20254AR60","3RT Ρελέ ισχύος"]
["3RT2026-1AK60","power contactor, AC-3 25 A, 11 kW / 400 V 1 NO + 1 NC, 110 V AC, 50 Hz, 120 V, 60 Hz, 3-pole, Size S0, screw terminal",84.41,"ΤΕΜ",1,"EP",1,"3RT20261AK60","3RT Ρελέ ισχύος"]
["3RT2026-2CK64-3MA0","Power contactor, AC-3 25 A, 11 kW / 400 V 2 NO + 2 NC, 110 V AC, 50 Hz 120 V, 60 Hz, with inserted varistor, 3-pole, Size S0 Spring type terminal Captive auxiliary switch",116.14,"ΤΕΜ",1,"EP",1,"3RT20262CK643MA0","3RT Ρελέ ισχύος"]
["3RT2027-1AC20","Power contactor, AC-3 32 A, 15 kW / 400 V 1 NO + 1 NC, 24 V AC 50/60 Hz, 3-pole Size S0, screw terminals",120.49,"ΤΕΜ",1,"EP",1,"3RT20271AC20","3RT Ρελέ ισχύος"]
["3RT2027-1NB30","Power contactor, AC-3 32 A, 15 kW / 400 V 1 NO + 1 NC, AC 50-60 Hz / DC 21-28 V AC / DC 3-pole, size S0 screw terminals",211.68,"ΤΕΜ",1,"EP",1,"3RT20271NB30","3RT Ρελέ ισχύος"]
["3RT2027-2EL20","Power contactor, AC-3 32 A, 15 kW / 400 V 1 NO + 1 NC, 230 V AC 50/60 Hz, 3-pole Size S0, Spring-type terminals with RC element plugged-in",140.84,"ΤΕΜ",1,"EP",1,"3RT20272EL20","3RT Ρελέ ισχύος"]
["3RT2028-1BM40","Power contactor, AC-3 38 A, 18.5 kW / 400 V 1 NO + 1 NC, 220 V DC 3-pole, size S0 screw terminals",193.42,"ΤΕΜ",1,"EP",1,"3RT20281BM40","3RT Ρελέ ισχύος"]
["3RT2028-2BG40","Power contactor, AC-3 38 A, 18.5 kW / 400 V 1 NO + 1 NC, 125 V DC 3-pole, size S0 Spring-type terminals",199.77,"ΤΕΜ",1,"EP",1,"3RT20282BG40","3RT Ρελέ ισχύος"]
["3RT2035-1AB04","power contactor, AC-3 40 A, 18.5 kW / 400 V 2 NO + 2 NC, 24 V AC 50 Hz, 3-pole, Size S2, screw terminal",162.1,"ΤΕΜ",1,"EP",1,"3RT20351AB04","3RT Ρελέ ισχύος"]
["3RT2035-3AF04","power contactor, AC-3 40 A, 18.5 kW / 400 V 2 NO + 2 NC, 110 V AC 50 Hz, 3-pole, Size S2, Spring-type terminal",162.1,"ΤΕΜ",1,"EP",1,"3RT20353AF04","3RT Ρελέ ισχύος"]
["3RT2036-1AF00-1AA0","power contactor, AC-3 50 A, 22 kW / 400 V 1 NO + 1 NC, 110 V AC, 50 Hz, 3-pole, Size S2, screw terminal upright mounting position",199.4,"ΤΕΜ",1,"EP",1,"3RT20361AF001AA0","3RT Ρελέ ισχύος"]
["3RT2036-3AK60","power contactor, AC-3 50 A, 22 kW / 400 V 1 NO + 1 NC, 110 V AC 50 Hz / 120 V, 60 Hz, 3-pole, Size S2, Spring-type terminal",184.6,"ΤΕΜ",1,"EP",1,"3RT20363AK60","3RT Ρελέ ισχύος"]
["3RT2036-3SP30","contactor, AC-3, 50 A/400 V/60 Β°C S2, 3-pole, 175-280 V AC/DC, F-PLC-IN, with varistor, 1 NC, spring-type terminal",351.32,"ΤΕΜ",1,"EP",1,"3RT20363SP30","3RT Ρελέ ισχύος"]
["3RT2037-3SB30","contactor, AC-3, 65 A/400 V/60 Β°C S2, 3-pole, 21-33 V AC/DC, F-PLC-IN, with varistor, 1 NC, spring-loaded terminal",453.93,"ΤΕΜ",1,"EP",1,"3RT20373SB30","3RT Ρελέ ισχύος"]
["3RT2038-1AV60","Power contactor, AC-3 80 A, 37 kW / 400 V 1 NO + 1 NC, 480 V AC, 60 Hz 3-pole, size S2 screw terminals",327.10000000000002,"ΤΕΜ",1,"EP",1,"3RT20381AV60","3RT Ρελέ ισχύος"]
["3RT2045-1AK60","power contactor, AC-3 80 A, 37 kW / 400 V 1 NO + 1 NC, 110 V AC/50 Hz 120 V/60 Hz 3-pole, 3 NO, Size S3 screw terminal",308.64,"ΤΕΜ",1,"EP",1,"3RT20451AK60","3RT Ρελέ ισχύος"]
["3RT2045-1AT60","power contactor, AC-3 80 A, 37 kW / 400 V 1 NO + 1 NC, 600 V AC/60 Hz 3-pole, 3 NO, Size S3 screw terminal",318.5,"ΤΕΜ",1,"EP",1,"3RT20451AT60","3RT Ρελέ ισχύος"]
["3RT2046-1AK64-3MA0","power contactor, AC-3 95 A, 45 kW / 400 V 2 NO + 2 NC, 110 V AC, 50 Hz Hz 120 V/60 Hz 3-pole, 3 NO, Size S3 screw terminal",409.61,"ΤΕΜ",1,"EP",1,"3RT20461AK643MA0","3RT Ρελέ ισχύος"]
["3RT2046-1NP30","power contactor, AC-3 95 A, 45 kW / 400 V 1 NO + 1 NC, 175-280 V AC/DC 3-pole, 3 NO, Size S3 screw terminal integrated varistor",502.36,"ΤΕΜ",1,"EP",1,"3RT20461NP30","3RT Ρελέ ισχύος"]
["3RT2047-3NB30","Power contactor, AC-3 115 A, 55 kW /  400 V 1 NO + 1 NC, 20-33 V AC/DC 3-pole, 3 NO, Size S3 Spring-type terminals integrated varistor",521.24,"ΤΕΜ",1,"EP",1,"3RT20473NB30","3RT Ρελέ ισχύος"]
["3RT2047-3XB40-0LA2","Traction contactor, AC-3 115 A, 55 kW /  400 V 1 NO + 1 NC, 24 V DC 0.7-1.25*Us 3-pole, 3 NO, Size S3 integrated varistor Spring-type terminals",786.38,"ΤΕΜ",1,"EP",1,"3RT20473XB400LA2","3RT Ρελέ ισχύος"]
["3RT2325-1AG20","Contactor, AC-1, 35 A/400 V/40 Β°C, S0, 4-pole, 110 V AC, 50/60 Hz, 1 NO+1 NC, screw terminal",80.39,"ΤΕΜ",1,"EP",1,"3RT23251AG20","3RT Ρελέ ισχύος"]
["3RT2327-1AP60","Contactor, AC-1, 50 A/400 V/40 Β°C, S0, 4-pole, 220 V AC/50 Hz, 240 V/60 Hz, 1 NO+1 NC, screw terminal",146.55000000000001,"ΤΕΜ",1,"EP",1,"3RT23271AP60","3RT Ρελέ ισχύος"]
["3RT2337-1AF00","Contactor, AC-1, 110 A/400 V/40 Β°C, S2, 4-pole, 110 V AC/50 Hz, 1 NO+1 NC, screw terminal",354.95,"ΤΕΜ",1,"EP",1,"3RT23371AF00","3RT Ρελέ ισχύος"]
["3RT2448-1NB30","Contactor, AC-1, 160 A/690 V/40 Β°C, S3, 3-pole, 20-33 V AC/DC, with varistor, 1 NO+1 NC, box terminal/screw terminal",496.36,"ΤΕΜ",1,"EP",1,"3RT24481NB30","3RT Ρελέ ισχύος"]
["3RT2517-2BW40","Power contactor, AC-3 12 A, 5.5 kW / 400 V 2 NO + 2 NC 48 V DC 4-pole Size S00 Spring-type terminals",57.57,"ΤΕΜ",1,"EP",1,"3RT25172BW40","3RT Ρελέ ισχύος"]
["3RT2535-1AC20","Power contactor, AC-3 40 A, 18.5 kW / 400 V 2 NO + 2 NC 24 V AC, /50/60 Hz 4-pole size S2 screw terminals 1 NO+1 NC integrated",181.47,"ΤΕΜ",1,"EP",1,"3RT25351AC20","3RT Ρελέ ισχύος"]
["3RT2536-1NF30","Power contactor, AC-3 50 A, 22 kW / 400 V 2 NO + 2 NC 83-155 V AC/DC varistor, 4-pole size S2 screw terminals 1 NO + 1 NC integrated",378.05,"ΤΕΜ",1,"EP",1,"3RT25361NF30","3RT Ρελέ ισχύος"]
["3RT2625-1NB35","Capacitor contactor, AC-6b 16.7 kVAr, / 400 V 1 NO + 2 NC, 50-60 Hz AC 21-28 V DC 3-pole, Size S0 screw terminal",222.81,"ΤΕΜ",1,"EP",1,"3RT26251NB35","3RT Ρελέ ισχύος"]
["3RT2645-1AF03","Capacitor contactor, AC-6b 75 kVAr, / 400 V 1 NO + 1 NC, 110 V AC, 50 Hz 3-pole, Size S3 screw terminal",480.21,"ΤΕΜ",1,"EP",1,"3RT26451AF03","3RT Ρελέ ισχύος"]
["3RT2924-5AN21","Magnet coil for contactors 7.5 kW 220 V AC, 50 / 60 Hz, for motor contactors, Size S0, Screw terminal",21.33,"ΤΕΜ",1,"EP",1,"3RT29245AN21","3RT Ρελέ ισχύος"]
["3RT2926-5AM21","Magnet coil for contactors 18.5 kW 208 V AC, 50 / 60 Hz, for motor contactors, Size S0, Screw terminal",25.4,"ΤΕΜ",1,"EP",1,"3RT29265AM21","3RT Ρελέ ισχύος"]
["3RT2926-5AP01","Magnet coil for contactors 18.5 kW 230 V AC, 50 Hz, for motor contactors, Size S0, Screw terminal",21.33,"ΤΕΜ",1,"EP",1,"3RT29265AP01","3RT Ρελέ ισχύος"]
["3RT2944-5AH21","Magnet coil for contactor S3, 48 V AC, 50 / 60 Hz,",46.17,"ΤΕΜ",1,"EP",1,"3RT29445AH21","3RT Ρελέ ισχύος"]
["3RU2116-0BC0","Overload relay 0.14...0.20 A Thermal For motor protection Size S00, Class 10 Contactor mounting Main circuit: Spring-type terminal Auxiliary circuit: spring-type terminal Manual-Automatic-Reset",60.81,"ΤΕΜ",1,"EP",1,"3RU21160BC0","3RU Θερμικό υπερφόρτωσης"]
["3RU2116-1GC0","Overload relay 4.5...6.3 A Thermal For motor protection Size S00, Class 10 Contactor mounting Main circuit: Spring-type terminal Auxiliary circuit: spring-type terminal Manual-Automatic-Reset",60.81,"ΤΕΜ",1,"EP",1,"3RU21161GC0","3RU Θερμικό υπερφόρτωσης"]
["3RU2126-1JJ0","Overload relay 7.0...10 A Thermal For motor protection Size S0, Class 10 Contactor mounting Main circuit: Ring cable lug Auxiliary circuit: ring cable lug Manual-Automatic-Reset",59.48,"ΤΕΜ",1,"EP",1,"3RU21261JJ0","3RU Θερμικό υπερφόρτωσης"]
["3RU2136-4EB1","Overload relay 22...32 A Thermal For motor protection Size S2, Class 10 Stand-alone installation Main circuit: Screw Auxiliary circuit: Screw Manual-Automatic-Reset",127.8,"ΤΕΜ",1,"EP",1,"3RU21364EB1","3RU Θερμικό υπερφόρτωσης"]
["3RU2146-4KB1","Overload relay 57...75 A Thermal For motor protection Size S3, Class 10 Stand-alone installation Main circuit: Screw Auxiliary circuit: Screw Manual-Automatic-Reset",177.48,"ΤΕΜ",1,"EP",1,"3RU21464KB1","3RU Θερμικό υπερφόρτωσης"]
["3RV1915-1BB","3-phase busbars Modular spacing 45 mm for 3 switches Fork shape connections",15.03,"ΤΕΜ",1,"EP",1,"3RV19151BB","3RV Θερμομαγνητικοί διακόπτες ισχύος"]
["3RV1923-1GA01","Cast aluminum surface mounting enclosure Degree of protection IP65 72 mm installation width, PE terminal with rotary operating mechanism yellow/red for circuit breaker Size S0",77.89,"ΤΕΜ",1,"EP",1,"3RV19231GA01","3RV Θερμομαγνητικοί διακόπτες ισχύος"]
["3RV2011-1AA15","Circuit breaker size S00 for motor protection, CLASS 10 A-release 1.1...1.6 A N-release 21 A screw terminal Standard switching capacity with transverse auxiliary switches 1 NO+1 NC",81.739999999999995,"ΤΕΜ",1,"EP",1,"3RV20111AA15","3RV Θερμομαγνητικοί διακόπτες ισχύος"]
["3RV2011-1CA40","Circuit breaker size S00 for motor protection, CLASS 10 A-release 1.8...2.5 A N-release 33 A ring cable lug connection Standard switching capacity",68.13,"ΤΕΜ",1,"EP",1,"3RV20111CA40","3RV Θερμομαγνητικοί διακόπτες ισχύος"]
["3RV2021-1EA10-0DA0","Circuit breaker size S0 for system protection without phase failure protection A-release 2.8...4 A Short-circuit release 52 A Screw terminal Standard switching capacity",94.15,"ΤΕΜ",1,"EP",1,"3RV20211EA100DA0","3RV Θερμομαγνητικοί διακόπτες ισχύος"]
["3RV2021-4BA10-0DA0","Circuit breaker size S0 for system protection without phase failure protection A-release 13...20 A N-release 260 A screw terminal Standard switching capacity",105.18,"ΤΕΜ",1,"EP",1,"3RV20214BA100DA0","3RV Θερμομαγνητικοί διακόπτες ισχύος"]
["3RV2021-4EA10-0BA0","Special type Circuit breaker size S0 for motor protection, CLASS 10 A-release 27...32 A N-release 400 A screw terminal Standard switching capacity Ambient temperature -50 Β°C 500 switching cycles",155.94,"ΤΕΜ",1,"EP",1,"3RV20214EA100BA0","3RV Θερμομαγνητικοί διακόπτες ισχύος"]
["3RV2031-4VA15","Circuit breaker size S2 for motor protection, CLASS 10 A-release 35...45 A N-release 650 A screw terminal Standard switching capacity with transverse auxiliary switches 1 NO+1 NC",272.82,"ΤΕΜ",1,"EP",1,"3RV20314VA15","3RV Θερμομαγνητικοί διακόπτες ισχύος"]
["3RV2041-4HA15","Circuit breaker size S3 for motor protection, CLASS 10 A-release 36...50 A N-release 650 A screw terminal Standard switching capacity with transverse auxiliary switches 1 NO+1 NC",293.87,"ΤΕΜ",1,"EP",1,"3RV20414HA15","3RV Θερμομαγνητικοί διακόπτες ισχύος"]
["3RV2131-4VA10","Circuit breaker size S2 for motor protection, CLASS 10 with overload relay function A-release 35...45 A N-release 650 A Standard switching capacity",311.10000000000002,"ΤΕΜ",1,"EP",1,"3RV21314VA10","3RV Θερμομαγνητικοί διακόπτες ισχύος"]
["3RV2311-4AC20-0BA0","Special type Circuit breaker size S00 for starter combination rated current 16 A N-release 208 A Spring-type terminal Standard switching capacity Ambient temperature -50 Β°C 500 switching cycles",115.13,"ΤΕΜ",1,"EP",1,"3RV23114AC200BA0","3RV Θερμομαγνητικοί διακόπτες ισχύος"]
["3RV2342-4RC10","Circuit breaker size S3 for starter combination Rated current 84 A N-release 1170 A screw terminal Increased switching capacity 100 kA",450.14,"ΤΕΜ",1,"EP",1,"3RV23424RC10","3RV Θερμομαγνητικοί διακόπτες ισχύος"]
["3RV2411-0GA10","Circuit breaker size S00 for transformer protection A-release 0.45...0.63 A N-release 13 A screw terminal Standard switching capacity",76.36,"ΤΕΜ",1,"EP",1,"3RV24110GA10","3RV Θερμομαγνητικοί διακόπτες ισχύος"]
["3RV2411-1HA10-0BA0","Special type Circuit breaker size S00 for transformer protection A-release 5.8...8 A N-release 163 A screw terminal Standard switching capacity Ambient temperature -50 Β°C 500 switching cycles",113.54,"ΤΕΜ",1,"EP",1,"3RV24111HA100BA0","3RV Θερμομαγνητικοί διακόπτες ισχύος"]
["3RV2711-1CD10","Circuit breaker size S00 for system protection with approval circuit breaker UL 489, CSA C22.2 No.5-02 A-release 2.5 A N-release 33 A screw terminal Standard switching capacity",155.91,"ΤΕΜ",1,"EP",1,"3RV27111CD10","3RV Θερμομαγνητικοί διακόπτες ισχύος"]
["3RV2902-4DF0","Shunt release 90-110 V AC, 50/60 Hz, 100% ON period 70-190 V AC, 50/60 Hz, 5 s ON period 70-190 V AC, 5 s ON period with ring cable lug connection for circuit breaker 3RV2",36.04,"ΤΕΜ",1,"EP",1,"3RV29024DF0","3RV Θερμομαγνητικοί διακόπτες ισχύος"]
["3RV2926-0Q","Tolerance compensation for door-coupling rotary operating mechanism Size S00...S3",40.51,"ΤΕΜ",1,"EP",1,"3RV29260Q","3RV Θερμομαγνητικοί διακόπτες ισχύος"]
["3RV2938-1K","Phase barrier for circuit breaker Size S2",11.17,"ΤΕΜ",1,"EP",1,"3RV29381K","3RV Θερμομαγνητικοί διακόπτες ισχύος"]
["3RW4028-1TB04","SIRIUS soft starter S0 38 A, 18.5 kW/400 V, 40 Β°C 200-480 V AC, 24 V AC/DC Screw terminals Thermistor motor protection",1074.33,"ΤΕΜ",1,"EP",1,"3RW40281TB04","3RW Ομαλοί εκκινητές"]
["3RW4037-1BB05","SIRIUS soft starter S2 63 A, 37 kW/500 V, 40 Β°C 400-600 V AC, 24 V AC/DC Screw terminals",1453.14,"ΤΕΜ",1,"EP",1,"3RW40371BB05","3RW Ομαλοί εκκινητές"]
["3RW4746-0LC00","Power semiconductor module 690 V, for 3RW4446, 356 A two units for each device",1909.14,"ΤΕΜ",1,"EP",1,"3RW47460LC00","3RW Ομαλοί εκκινητές"]
["3RW4766-2HC00","Removable control terminals with spring-type terminals 4 blocks with 6 terminals each",152.97,"ΤΕΜ",1,"EP",1,"3RW47662HC00","3RW Ομαλοί εκκινητές"]
["3RW5072-2AB14","SIRIUS soft starter 200-480 V 210 A, 110-250 V AC Spring-loaded terminals Analog output",3263.38,"ΤΕΜ",1,"EP",1,"3RW50722AB14","3RW Ομαλοί εκκινητές"]
["3RW5074-6TB05","SIRIUS soft starter 200-600 V 315 A, 24 V AC/DC Screw terminals Thermistor input",4326.8900000000003,"ΤΕΜ",1,"EP",1,"3RW50746TB05","3RW Ομαλοί εκκινητές"]
["3RW5214-3AC04","SIRIUS soft starter 200-480 V 18 A, 24 V AC/DC spring-type terminals Analog output",1155.3,"ΤΕΜ",1,"EP",1,"3RW52143AC04","3RW Ομαλοί εκκινητές"]
["3RW5215-3TC05","SIRIUS soft starter 200-600 V 25 A, 24 V AC/DC spring-type terminals Thermistor input",1423.36,"ΤΕΜ",1,"EP",1,"3RW52153TC05","3RW Ομαλοί εκκινητές"]
["3RW5226-3TC05","SIRIUS soft starter 200-600 V 77 A, 24 V AC/DC spring-type terminals Thermistor input",2476.67,"ΤΕΜ",1,"EP",1,"3RW52263TC05","3RW Ομαλοί εκκινητές"]
["3RW5235-2AC14","SIRIUS soft starter 200-480 V 143 A, 110-250 V AC spring-type terminals Analog output",3277.95,"ΤΕΜ",1,"EP",1,"3RW52352AC14","3RW Ομαλοί εκκινητές"]
["3RW5245-6TC05","SIRIUS soft starter 200-600 V 315 A, 24 V AC/DC Screw terminals Thermistor input",6789,"ΤΕΜ",1,"EP",1,"3RW52456TC05","3RW Ομαλοί εκκινητές"]
["3RW5248-6AC04","SIRIUS soft starter 200-480 V 570 A, 24 V AC/DC Screw terminals Analog output",9498.76,"ΤΕΜ",1,"EP",1,"3RW52486AC04","3RW Ομαλοί εκκινητές"]
["3RW5514-1HA05","SIRIUS soft starter 200-600 V 18 A, 24 V AC/DC Screw terminals",1900.26,"ΤΕΜ",1,"EP",1,"3RW55141HA05","3RW Ομαλοί εκκινητές"]
["3RW5527-3HF04","SIRIUS soft starter 200-480 V 93 A, 24 V AC/DC spring-type terminals Fail-safe",3983.51,"ΤΕΜ",1,"EP",1,"3RW55273HF04","3RW Ομαλοί εκκινητές"]
["3RW5535-6HA06","SIRIUS soft starter 200-690 V 143 A, 24 V AC/DC Screw terminals",5391.11,"ΤΕΜ",1,"EP",1,"3RW55356HA06","3RW Ομαλοί εκκινητές"]
["3RW5547-6HA16","SIRIUS soft starter 200-690 V 470 A, 110-250 V AC Screw terminals",13949.32,"ΤΕΜ",1,"EP",1,"3RW55476HA16","3RW Ομαλοί εκκινητές"]
["3RW5556-6HA04","SIRIUS soft starter 200-480 V 1100 A, 24 V AC/DC Screw terminals",21958.560000000001,"ΤΕΜ",1,"EP",1,"3RW55566HA04","3RW Ομαλοί εκκινητές"]
["3RW5951-0VY00","Transport packaging for 3RW55/52, Size 1",47.61,"ΤΕΜ",1,"EP",1,"3RW59510VY00","3RW Ομαλοί εκκινητές"]
["3RW5954-0BP00","Bypass kit for 3RW55/52 Size 4, 210 A to 315 A",361.26,"ΤΕΜ",1,"EP",1,"3RW59540BP00","3RW Ομαλοί εκκινητές"]
["3SB2000-0AH01","Pushbutton, 16 mm, round, plastic, clear, pushbutton, flat",10.47,"ΤΕΜ",1,"EP",1,"3SB20000AH01","3SB μπουτόν 16mm"]
["3SB2000-2HG01","Selector switch, 16 mm, round, plastic, white, 2 switch positions O-I, latching, actuating angle 90 degree",20.84,"ΤΕΜ",1,"EP",1,"3SB20002HG01","3SB μπουτόν 16mm"]
["3SB2202-4LB01","Key-operated switch, 16 mm, round, plastic, CES, 2 switch positions O-I, latching, actuating angle 62 degree, Key removal O+I",80.819999999999993,"ΤΕΜ",1,"EP",1,"3SB22024LB01","3SB μπουτόν 16mm"]
["3SB2901-2BA","Adhesive labeling plate, on label holder, Label size 9.5 x 18.5 mm, silver-colored, black font, with inscription: Manual Auto",123.32,"ΤΕΜ",100,"EP",10,"3SB29012BA","3SB μπουτόν 16mm"]
["3SB2901-4AK","Inscription plate for pushbutton and illuminated pushbutton flat, milky with black font, with inscription: Stop",123.32,"ΤΕΜ",100,"EP",10,"3SB29014AK","3SB μπουτόν 16mm"]
["3SB2908-8AD","Complete connector for connecting contact blocks and lampholder, max. 10 connections",10.36,"ΤΕΜ",1,"EP",1,"3SB29088AD","3SB μπουτόν 16mm"]
["3SB2910-1BH","lens, clear, smooth, for inscription with insert caps",64.87,"ΤΕΜ",100,"EP",10,"3SB29101BH","3SB μπουτόν 16mm"]
["3SE3902-4CB20","Foot switch molded-plastic enclosure Pedal switch 1-pedal without cover, 1 change-over contact",88.19,"ΤΕΜ",1,"EP",1,"3SE39024CB20","3SE Τερματικοί διακόπτες"]
["3SE5000-0AE10-1AJ0","Actuator head for position switch 3SE52 Roller lever made of metal with Plastic roller 13 mm functional at -40 Β°C",15.39,"ΤΕΜ",1,"EP",1,"3SE50000AE101AJ0","3SE Τερματικοί διακόπτες"]
["3SE5112-0BA00","Basic switch for position switch 3SE51 Metal enclosure, according to EN 50041 1x (M20x 1.5) 1 NO/1 NC slow-action contacts without actuator head",39.409999999999997,"ΤΕΜ",1,"EP",1,"3SE51120BA00","3SE Τερματικοί διακόπτες"]
["3SE5112-0KE01","Position switch Metal enclosure 40 mm according to EN 50041 Device connection 1x (M20 x 1.5) 1 NO/2 NC slow-action contacts Roller lever, Metal lever and plastic roller 22 mm",62.95,"ΤΕΜ",1,"EP",1,"3SE51120KE01","3SE Τερματικοί διακόπτες"]
["3SE5122-0BD02","Position switch Metal enclosure 56 mm wide Device connection 3x (M20x 1.5) 1 NO/1 NC slow-action contacts Roller plunger with Stainless steel roller 13 mm",70.63,"ΤΕΜ",1,"EP",1,"3SE51220BD02","3SE Τερματικοί διακόπτες"]
["3SE5122-0PA00-1CA0","Basic switch for position switch 3SE5112 Metal enclosure 56 mm increased corrosion protection (increased corrosion protection) 3x (M20x 1.5) 2 NO/1 NC slow-action contacts without actuator head",44.5,"ΤΕΜ",1,"EP",1,"3SE51220PA001CA0","3SE Τερματικοί διακόπτες"]
["3SE5130-1AA00-1AG0","LED cover yellow for position switch plastic 3SE5132 enclosure, according to EN 50041 2 LEDs, yellow/green, 24 V DC",26.04,"ΤΕΜ",1,"EP",1,"3SE51301AA001AG0","3SE Τερματικοί διακόπτες"]
["3SE5162-0BA00-1CA0","Basic switch for position switch 3SE5162 Metal enclosure XL, 56 mm wide Device connection 3x(M20 x 1.5) IP66/IP67 2 x (1 NO/2 NC) Slow-action contacts without actuator head with increased corrosion protection",112.11,"ΤΕΜ",1,"EP",1,"3SE51620BA001CA0","3SE Τερματικοί διακόπτες"]
["3SE5212-0CH22-1AJ0","Position switch Metal 31 mm, according to EN 50047 Increased corrosion protection Device connection 1 x (M20 x 1.5) 1 NO/1 NC quick action contacts Rotary actuator right/left adjustable Metal lever and Stainless steel roller 19 mm functional at -40 Β°C Shock and vibration test according to EN 61373, Category 1B",94,"ΤΕΜ",1,"EP",1,"3SE52120CH221AJ0","3SE Τερματικοί διακόπτες"]
["3SE5232-0HC05-1AB4","Position switch Plastic enclosure, 31 mm according to EN 50047 Control cabinet type 1 NO/1 NC snap-action contacts integrated (not replaceable) Rounded plunger Degree of protection IP40, with Self-sealing grommet Standard cover, turquoise With accessories: screws and mounting plate without locking sheet metal and seal",25.87,"ΤΕΜ",1,"EP",1,"3SE52320HC051AB4","3SE Τερματικοί διακόπτες"]
["3SE5232-0LK15","Position switch Plastic enclosure according to EN 50047, 31 mm Device connection 1 x (M20 x 1.5) 1 NO/2 NC quick action contacts Twist lever, 35 mm long right/left adjustable with plastic roller 19 mm",43.71,"ΤΕΜ",1,"EP",1,"3SE52320LK15","3SE Τερματικοί διακόπτες"]
["3SE5242-0LC05-1CA0","Position switch with increased corrosion protection Plastic enclosure wide, according to EN 50047, 50 mm 1 NO/2 NC quick action contacts Teflon plunger",37.68,"ΤΕΜ",1,"EP",1,"3SE52420LC051CA0","3SE Τερματικοί διακόπτες"]
["3SE5250-0LC05","Position switch Plastic enclosure open type 30 mm 1 NO/2 NC quick action contacts Metal plunger, IP10",26.9,"ΤΕΜ",1,"EP",1,"3SE52500LC05","3SE Τερματικοί διακόπτες"]
["3SE5312-3SF13","Safety position switch with tumbler Locking force 2600 N 5 directions of approaches Spring-locked Escape release from the front Magnet voltage 230 V AC Monitoring actuator 2 NC/1 NO Monitoring magnet 2 NC/1 NO LED display yellow/green Supplied without actuator. Actuator 3SE5000-0AV0. please order separately",441.52,"ΤΕΜ",1,"EP",1,"3SE53123SF13","3SE Τερματικοί διακόπτες"]
["3SE5423-0CD20-1EB1","Position switch in compact design 40 mm wide with connector plug M12 Snap-action contacts 1 NO+1 NC with roller plunger",77.19,"ΤΕΜ",1,"EP",1,"3SE54230CD201EB1","3SE Τερματικοί διακόπτες"]
["3SE7910-3AH","Steel rope 4 mm, Length 50 m with red plastic sheath",428.12,"ΤΕΜ",1,"EP",1,"3SE79103AH","3SE Τερματικοί διακόπτες"]
["3SF1324-1SD21-1BA1","Safety position switch with tumbler Locking force 1300 N 5 directions of approaches Plastic enclosure, M12 connector ASIsafe integrated Channel 1=actuator 1 NC Channel 2=magnet 1 NC spring-locked Auxiliary release on front Magnet voltage 24 V DC/AC Monitoring actuator 2 NC/1 NO Monitoring magnet 2 NC/1 NO The matching separate Actuator 3SE5000-0AV0 must be ordered separately",884.54,"ΤΕΜ",1,"EP",1,"3SF13241SD211BA1","3SF AS-I τερματικοί διακόπτες"]
["3SK1112-2BB40","SIRIUS safety relay Basic unit Standard series electronic enabling circuits 2 enabling circuits plus 1 signaling circuit Us = 24 V DC Spring-type terminal (push-in)",207.6,"ΤΕΜ",1,"EP",1,"3SK11122BB40","3SK Ρελέ ασφαλείας"]
["3SU1000-0CB50-0AA0","Pushbutton, 22 mm, round, plastic, blue, Front ring, raised momentary contact type",9.48,"ΤΕΜ",1,"EP",1,"3SU10000CB500AA0","3SU Μπουτόν"]
["3SU1000-1HQ20-0AA0","EMERGENCY STOP mushroom pushbutton, 22 mm, round, plastic, red, 40 mm, with O.M.R. lock, lock number 73037, positive latching, acc. to EN ISO 13850, key-operated release",67.5,"ΤΕΜ",1,"EP",1,"3SU10001HQ200AA0","3SU Μπουτόν"]
["3SU1000-5BF01-0AA0","key-operated switch Siemens, 22 mm, round, plastic, lock number SSG10, with 2 keys, 2 switch positions O-I, latching, actuating angle 90Β°, 10:30h/13:30h, key removal O",85.35,"ΤΕΜ",1,"EP",1,"3SU10005BF010AA0","3SU Μπουτόν"]
["3SU1000-5TF01-0AA0","Key-operated switch BKS, 22 mm, round, plastic, Lock No. E9 (VW), without key, 2 switch positions O-I, latching, actuating angle 90Β°, 10:30h/13:30h, Key removal O",127.78,"ΤΕΜ",1,"EP",1,"3SU10005TF010AA0","3SU Μπουτόν"]
["3SU1001-0BB40-0AA0","Illuminated pushbutton, 22 mm, round, plastic, green, pushbutton, raised momentary contact type",10.039999999999999,"ΤΕΜ",1,"EP",1,"3SU10010BB400AA0","3SU Μπουτόν"]
["3SU1002-2BC60-0AA0","Selector switch, illuminable, 22 mm, round, plastic, white, selector switch, short, 2 switch positions O<I, momentary contact type, Actuating angle 45Β°, 10:30h/12h",14.24,"ΤΕΜ",1,"EP",1,"3SU10022BC600AA0","3SU Μπουτόν"]
["3SU1050-0AB10-0AA0","Pushbutton, 22 mm, round, metal, shiny, black, pushbutton, flat momentary contact type",8.6,"ΤΕΜ",1,"EP",1,"3SU10500AB100AA0","3SU Μπουτόν"]
["3SU1050-3AB61-0AK0","Twin pushbutton, 22 mm, round, metal, shiny, white: I, Black: O, pushbuttons, flat",18.14,"ΤΕΜ",1,"EP",1,"3SU10503AB610AK0","3SU Μπουτόν"]
["3SU1050-5BP61-0AA0","key-operated switch Siemens, 22 mm, round, metal, shiny, lock number SSG10, with 2 keys, 3 switch positions I>O<II, momentary contact on the left, latching on the right, actuating angle 2x45Β°, 10:30h/12h/13:30h, key removal O+II",89.93,"ΤΕΜ",1,"EP",1,"3SU10505BP610AA0","3SU Μπουτόν"]
["3SU1051-0AB52-0AS0","Illuminated pushbutton, 22 mm, round, metal, shiny, blue, pushbutton, flat, momentary contact type, with customer-specific symbol, customer material number 38.0459 on packaging",11.7,"ΤΕΜ",1,"EP",1,"3SU10510AB520AS0","3SU Μπουτόν"]
["3SU1051-6AA50-0AA0","Indicator lights, 22 mm, round, metal, shiny, blue, lens, smooth",6.22,"ΤΕΜ",1,"EP",5,"3SU10516AA500AA0","3SU Μπουτόν"]
["3SU1052-2CC10-0AA0","Illuminable selector switch, 22 mm, round, metal shiny, black, Selector switch long, 2 switch positions O<I, momentary contact type, Actuating angle 45Β°, 10:30h/12h",24.39,"ΤΕΜ",1,"EP",1,"3SU10522CC100AA0","3SU Μπουτόν"]
["3SU1052-2CN60-0AA0","Selector switch, illuminable, 22 mm, round, metal, shiny, white, selector switch, long, 3 switch positions I-O<II, left latching, right momentary contact type, actuating angle 2x45Β°, 10:30h/12h/13:30h",22.04,"ΤΕΜ",1,"EP",1,"3SU10522CN600AA0","3SU Μπουτόν"]
["3SU1062-2EC60-0AA0","Selector switch, illuminable, 30 mm, round, metal, matte, white, selector switch, long, front ring for flush installation, 2 switch positions O<I, momentary contact type, Actuating angle 45Β°, 10:30h/12h",47.7,"ΤΕΜ",1,"EP",1,"3SU10622EC600AA0","3SU Μπουτόν"]
["3SU1100-0AB70-1BA0","Pushbutton, 22 mm, round, plastic, clear, pushbutton, flat, momentary contact type, with holder 1 NO, screw terminal",18.829999999999998,"ΤΕΜ",1,"EP",1,"3SU11000AB701BA0","3SU Μπουτόν"]
["3SU1100-7AB10-1NA0","Coordinate switch, 22 mm, round, plastic, black, 2 switch positions, vertical latching, without mechanical interlocking, in O position, with holder, 1 NO, 1 NO, screw terminal,",79.400000000000006,"ΤΕΜ",1,"EP",1,"3SU11007AB101NA0","3SU Μπουτόν"]
["3SU1103-0AB70-1BA0","Illuminated pushbutton, 22 mm, round, plastic, clear, pushbutton, flat, momentary contact type, with holder, 1 NO, LED module with integrated LED 110 V AC, screw terminal",39.6,"ΤΕΜ",1,"EP",1,"3SU11030AB701BA0","3SU Μπουτόν"]
["3SU1150-0AB50-3BA0","Pushbutton, 22 mm, round, metal, shiny, blue, pushbutton, flat, momentary contact type, 1 NO, Spring-type terminal",22.34,"ΤΕΜ",1,"EP",1,"3SU11500AB503BA0","3SU Μπουτόν"]
["3SU1150-1GB20-3CW0","EMERGENCY STOP mushroom pushbutton, 22 mm, round, metal, shiny, red, 30 mm, positive latching, according to DIN EN ISO 13850, rotate-to-unlatch, washer for EMERGENCY STOP, yellow, without inscription, with holder, 1 NC, spring-loaded terminal, front plate mounting",57.55,"ΤΕΜ",1,"EP",1,"3SU11501GB203CW0","3SU Μπουτόν"]
["3SU1150-4BF11-3FA0","RONIS key-operated switch, 22 mm, round, metal, shiny, lock number SB30, with 2 keys, 2 switch positions O-I, latching, actuating angle 90Β°, 10:30h/13:30h, key removal O+I, with holder, 1 NO+1 NC, spring-type terminal, possible special locks: SB31, 421, 455",56.96,"ΤΕΜ",1,"EP",1,"3SU11504BF113FA0","3SU Μπουτόν"]
["3SU1153-0AB50-3FA0","Illuminated pushbutton, 22 mm, round, metal, shiny, blue, pushbutton, flat, momentary contact type, with holder, 1 NO+1 NC, LED module with integrated LED 110 V AC, Spring-type terminal",49.36,"ΤΕΜ",1,"EP",1,"3SU11530AB503FA0","3SU Μπουτόν"]
["3SU1200-2PQ10-1AA0","Potentiometer, compact, 22 mm, round, plastic, black, 1k ohm, with holder, screw terminal",98.52,"ΤΕΜ",1,"EP",1,"3SU12002PQ101AA0","3SU Μπουτόν"]
["3SU1400-1DA10-3AA0","Support terminal, black, spring-type terminal, for front plate mounting",9.9499999999999993,"ΤΕΜ",1,"EP",1,"3SU14001DA103AA0","3SU Μπουτόν"]
["3SU1400-1MA10-1BA1","SIRIUS ACT: terminal module (command module) for front plate mounting",54.92,"ΤΕΜ",1,"EP",1,"3SU14001MA101BA1","3SU Μπουτόν"]
["3SU1401-1BH20-3AA0","LED module with integrated LED, 24-240 V AC/DC, red, spring-type terminal, for front plate mounting",23.5,"ΤΕΜ",1,"EP",1,"3SU14011BH203AA0","3SU Μπουτόν"]
["3SU1401-1ME40-1DA1","SIRIUS ACT: terminal module (LED module), integrated LED green, for front plate mounting",53.26,"ΤΕΜ",1,"EP",1,"3SU14011ME401DA1","3SU Μπουτόν"]
["3SU1401-2BG60-1AA0","LED module with integrated LED 6-24V AC/DC white, screw terminal, for floor mounting",12.98,"ΤΕΜ",1,"EP",1,"3SU14012BG601AA0","3SU Μπουτόν"]
["3SU1501-1AG60-1BA0","holder, 3-way, plastic, 1 NO, LED module, white, 6-24 V AC/DC, screw terminal",22.54,"ΤΕΜ",1,"EP",1,"3SU15011AG601BA0","3SU Μπουτόν"]
["3SU1801-0NL00-1AA2","Enclosure for command devices, 22 mm, round, Enclosure material plastic, Enclosure top part yellow, 1 control point plastic, Control point in center, A=EMERGENCY STOP mushroom pushbutton red, positive latching, 40 mm, rotate-to-unlatch, 2x 2NC, screw terminal, Front plate mounting, with enclosure adapter, 1xM20 each on top and bottom",103.39,"ΤΕΜ",1,"EP",1,"3SU18010NL001AA2","3SU Μπουτόν"]
["3SU1802-0AH00-4AB1","Enclosure for command devices, 22 mm, round, enclosure material plastic, enclosure top part gray, 2 control points plastic, recess for labels, customer-specific equipment, spring-loaded terminal, floor mounting, GΓ¶pfert no. 428640 on rating plate Labels glued in",117.05,"ΤΕΜ",1,"EP",1,"3SU18020AH004AB1","3SU Μπουτόν"]
["3SU1804-0AH20-4VB1","enclosure for command devices, 22 mm, round, enclosure material plastic, enclosure top part gray, 4 control points plastic, recess for labels, customer-specific equipment, electronic module for IO-Link, spring-loaded terminal, floor mounting, M12 5-pole plug on top, PIN assignment: PIN1=21, PIN2=11, PIN3=n.c., PIN4=22, PIN5=12, M12 5-pole plug at bottom, IO-Link wiring: PIN1=L1+, PIN3=L1-, PIN4=C/Q1, without labeling plates CSP ID: 5506810",845.68,"ΤΕΜ",1,"EP",1,"3SU18040AH204VB1","3SU Μπουτόν"]
["3SU1900-0AB71-0DJ0","Inscription plate for illuminated pushbutton, round, milky with black font, with inscription: On",193.14,"ΤΕΜ",100,"EP",10,"3SU19000AB710DJ0","3SU Μπουτόν"]
["3SU1900-0AC16-0DK0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: Off",205.81,"ΤΕΜ",100,"EP",10,"3SU19000AC160DK0","3SU Μπουτόν"]
["3SU1900-0AC81-0AH0","Labeling plate for snapping on or gluing, on label holder, label size 12.5x27 mm, silver label, black font with inscription: Rechts",193.14,"ΤΕΜ",100,"EP",10,"3SU19000AC810AH0","3SU Μπουτόν"]
["3SU1900-0AD16-0QB0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, black label, white font, with graphic symbol: I",205.81,"ΤΕΜ",100,"EP",10,"3SU19000AD160QB0","3SU Μπουτόν"]
["3SU1900-0AE16-0AK0","Labeling plate for snapping on or gluing, on label holder, label size 27x27 mm, black label, white font, with inscription: Halt",220.44,"ΤΕΜ",100,"EP",10,"3SU19000AE160AK0","3SU Μπουτόν"]
["3SU1900-0AE16-0GS0","Labeling plate for snapping on or gluing on label holder, Label size 27x27 mm, black label, white font, with inscription: Sous tension",220.44,"ΤΕΜ",100,"EP",10,"3SU19000AE160GS0","3SU Μπουτόν"]
["3SU1900-0AF81-0DW0","Labeling plate for gluing on enclosure, label size 22x22mm, silver label, black font, with inscription: Open",4.51,"ΤΕΜ",1,"EP",10,"3SU19000AF810DW0","3SU Μπουτόν"]
["3SU1900-0AF81-0QP0","Labeling plate for gluing on enclosure, label size 22x22mm, silver label, black font, with graphic symbol: I O (one below the other)",4.51,"ΤΕΜ",1,"EP",10,"3SU19000AF810QP0","3SU Μπουτόν"]
["3SU1900-0FT30-0AA0","pushbutton, flat, yellow, for pushbutton",151.19,"ΤΕΜ",100,"EP",10,"3SU19000FT300AA0","3SU Μπουτόν"]
["3SU1901-0BD31-0AA0","Washer round for EMERGENCY STOP mushroom pushbutton, yellow, illuminated, thickness 5 mm, outer diameter 60 mm, inside diameter 23 mm, without inscription",133.63,"ΤΕΜ",1,"EP",1,"3SU19010BD310AA0","3SU Μπουτόν"]
["3SX5100-1SS51","Accessory for position switches 3SE51/52; M12 connector 5-pole, for M20 x 1.5; Pin1=Brown cable, Pin2=White cable, Pin3=Yellow-green cable, Pin4=Black cable, Pin5=Gray cable. Suitable for wiring sensors that are to be connected to all SIMATIC ET200 compact block I/O modules .",33.700000000000003,"ΤΕΜ",1,"EP",1,"3SX51001SS51","3SX εξαρτήματα για τερματικούς διακόπτες"]
["3SX9926","Cable gland molded plastic for position switch, M20x 1.5 for cable diameter: 5-13 mm",9.9,"ΤΕΜ",1,"EP",1,"3SX9926","3SX εξαρτήματα για τερματικούς διακόπτες"]
["3TC4417-5KB4","Contactor, Size 2, 2-pole, DC-3 and 5, 32 A Auxiliary switch 22 (2 NO + 2 NC) 24V DC DC operation with integrated varistor",471.1,"ΤΕΜ",1,"EP",1,"3TC44175KB4","3TC 2πολκά ρελέ"]
["3TC5214-0BP0","Contactor, Size 8, 2-pole, DC 4, Rated operating current 220 A Auxiliary switch 44E (4 NO+4 NC) 230V AC 50Hz, 277 V 60 Hz AC operation",2155.87,"ΤΕΜ",1,"EP",1,"3TC52140BP0","3TC 2πολκά ρελέ"]
["3TC7414-5KB","Traction contactor 1-pole 400 A 4 NO+4 NC 24 V DC with integrated varistor",3479.05,"ΤΕΜ",1,"EP",1,"3TC74145KB","3TC 2πολκά ρελέ"]
["3TG1010-1AG2","Power relay, AC-3 8.4 A, 4 kW / 400 V 4 NO, 110 V AC, 45...450 Hz 3 pole, flat connector terminal 6.3 x 0.8mm",27.9,"ΤΕΜ",1,"EP",10,"3TG10101AG2","3TG Ρελέ 4KW"]
["3TH4244-0AP6","Contactor relay, 44E, DIN EN 50011, 4NO + 4NC, screw terminal AC operation 240 V AC 60 Hz/220 V AC 50 Hz",98.33,"ΤΕΜ",1,"EP",1,"3TH42440AP6","3TH βοηθητικά ρελέ"]
["3TH4280-0AM0","Contactor relay, 80E, DIN EN 50011, 8 NO, screw terminal AC operation 220 V 50 Hz",98.33,"ΤΕΜ",1,"EP",1,"3TH42800AM0","3TH βοηθητικά ρελέ"]
["3TH4293-0AH0","Contactor relay, 44E, DIN EN 50011, 4 NO + 4 NC, screw terminal AC operation 48 V AC 50 Hz/58 V AC 60 Hz",116.76,"ΤΕΜ",1,"EP",1,"3TH42930AH0","3TH βοηθητικά ρελέ"]
["3TH4355-0BF4","Contactor relay, 55E, EN 50011, 5 NO + 5 NC, screw terminal, DC operation, 110 V DC",218.51,"ΤΕΜ",1,"EP",1,"3TH43550BF4","3TH βοηθητικά ρελέ"]
["3TH4394-0BB4","Contactor relay, 55E, EN 50011, 5 NO + 5 NC, 1U, screw terminal 24 V DC DC operation,",234.58,"ΤΕΜ",1,"EP",1,"3TH43940BB4","3TH βοηθητικά ρελέ"]
["3TX7402-3L","Surge suppressor Varistor with cable spacer 400-600 V AC for mounting to coil terminal for contactors size S0-S2",21.85,"ΤΕΜ",1,"EP",1,"3TX74023L","3TX εξαρτήματα για ρελέ"]
["3TY1304-0K","Series resistor 0.125 kohm",43.93,"ΤΕΜ",1,"EP",1,"3TY13040K","3TY εξαρτήματα για ρελέ"]
["3TY1304-1X","Series resistor 2.24 kohm",43.93,"ΤΕΜ",1,"EP",1,"3TY13041X","3TY εξαρτήματα για ρελέ"]
["3TY6483-0AU0","Magnet coil for contactor 3TC48, 240 V AC 50 Hz/288 V AC 60 Hz",81.760000000000005,"ΤΕΜ",1,"EP",1,"3TY64830AU0","3TY εξαρτήματα για ρελέ"]
["3TY6523-0BE4","Magnet coil for 3TB52, 3TC52, 60 V DC",431.6,"ΤΕΜ",1,"EP",1,"3TY65230BE4","3TY εξαρτήματα για ρελέ"]
["3TY7680-0B","Vacuum interrupters for 3TF68..-.C.., 3TF68..-.D.. 3TF68..-.Q.., consists of 3 vacuum interrupters with add-on parts",4348.75,"ΤΕΜ",1,"EP",1,"3TY76800B","3TY εξαρτήματα για ρελέ"]
["3UF7011-1AB00-1","Basic unit SIMOCODE pro V PN GP , Ethernet/PROFINET IO, PN system redundancy, OPC UA server, Web server, transmission rate 100 Mbps, 2 x bus connection via RJ45, 4 I/3 Q freely parameterizable, Us: 24 V DC, input for thermistor connection Monostable relay outputs, expandable by 1 extension module(DM, TM, EM)",996.48,"ΤΕΜ",1,"EP",1,"3UF70111AB001","3UF SIMOCODE"]
["3UF7982-0AA30-1","PCS 7 block library SIMOCODE pro migration V7-V9.1 AS blocks and faceplates for integration of SIMOCODE pro in the process control system PCS 7 V9.1 engineering software for an engineering station, (Single License) including runtime software for execution of the AS block in an automation system, Single License German/English type of delivery: OSD; software download, Class A email required for delivery condition of use: license for engineering software V7;",853.43,"ΤΕΜ",1,"EP",1,"3UF79820AA301","3UF SIMOCODE"]
["3UG4583-1CW31","insulation monitoring relay for non-grounded (IT) networks up to 400 V AC, 15-400 Hz and up to 600 V DC measuring range 1-100 / 2-200 kOhm supply voltage 24-240 V AC/DC width 45 mm 1 + 1 or 2 changeover contacts screw terminal",854.49,"ΤΕΜ",1,"EP",1,"3UG45831CW31","3UG Επιτηρητές ηλεκτρικών μεγεθών"]
["3VA1010-2ED32-0AC0","Circuit breaker 3VA1 IEC Frame 100 Switching capacity class B Icu=16 kA @ 415 V 3-pole, system protection TM210, FTFM, In=100 A Overload protection Ir=100 A non-adjustable short-circuit protection Ii = 10 x In Lug terminal 2 auxiliary switches HQ",237.21,"ΤΕΜ",1,"EP",1,"3VA10102ED320AC0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1010-2ED32-0KC0","Circuit breaker 3VA1 IEC Frame 100 Switching capacity class B Icu=16 kA @ 415 V 3-pole, system protection TM210, FTFM, In=100 A Overload protection Ir=100 A non-adjustable short-circuit protection Ii = 10 x In Lug terminal Shunt release (STL) 220-250 V DC, 208-277 V AC 2 auxiliary switches HQ",309.3,"ΤΕΜ",1,"EP",1,"3VA10102ED320KC0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1010-3ED36-0AA0","Circuit breaker 3VA1 IEC Frame 100 Switching capacity class N Icu=25 kA @ 415 V 3-pole, system protection TM210, FTFM, In=100 A Overload protection Ir=100 A non-adjustable short-circuit protection Ii = 10 x In Terminal connection",222.09,"ΤΕΜ",1,"EP",1,"3VA10103ED360AA0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1010-3ED42-0JA0","Circuit breaker 3VA1 IEC Frame 100 Switching capacity class N Icu=25 kA @ 415 V 4-pole, system protection TM210, FTFM, In=100 A Overload protection Ir=100 A non-adjustable short-circuit protection Ii = 10 x In N-conductor unprotected Lug terminal Shunt release (STL) 110-127 V DC, 50/60 Hz AC",336.05,"ΤΕΜ",1,"EP",1,"3VA10103ED420JA0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1010-4ED42-0HH0","circuit breaker 3VA1 IEC frame 100 breaking capacity class S Icu=36kA @ 415V 4-pole, line protection TM210, FTFM, In=100A overload protection Ir=100A fixed short-circuit protection Ii=10 x In N conductor unprotected nut keeper kit shunt trip (STL) 12-30V DC; 24V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",400,"ΤΕΜ",1,"EP",1,"3VA10104ED420HH0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1020-2ED32-0KC0","circuit breaker 3VA1 IEC frame 100 breaking capacity class B Icu=16kA @ 415V 3-pole, line protection TM210, FTFM, In=20A overload protection Ir=20A fixed short-circuit protection Ii=16 x In nut keeper kit shunt trip (STL) 220-250V DC, 208-277V AC 2 auxiliary switches HQ",266.27999999999997,"ΤΕΜ",1,"EP",1,"3VA10202ED320KC0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1020-3ED32-0AE0","circuit breaker 3VA1 IEC frame 100 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM210, FTFM, In=20A overload protection Ir=20A fixed short-circuit protection Ii=16 x In nut keeper kit 4 auxiliary switches HQ",238.96,"ΤΕΜ",1,"EP",1,"3VA10203ED320AE0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1020-4ED36-0AD0","circuit breaker 3VA1 IEC frame 100 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM210, FTFM, In=20A overload protection Ir=20A fixed short-circuit protection Ii=16 x In clamp connection 3 auxiliary switches HQ",240.12,"ΤΕΜ",1,"EP",1,"3VA10204ED360AD0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1025-2ED32-0JC0","circuit breaker 3VA1 IEC frame 100 breaking capacity class B Icu=16kA @ 415V 3-pole, line protection TM210, FTFM, In=25A overload protection Ir=25A fixed short-circuit protection Ii=12.8 x In nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ",266.27999999999997,"ΤΕΜ",1,"EP",1,"3VA10252ED320JC0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1032-2ED32-0CC0","circuit breaker 3VA1 IEC frame 100 breaking capacity class B Icu=16kA @ 415V 3-pole, line protection TM210, FTFM, In=32A overload protection Ir=32A fixed short-circuit protection Ii=10 x In nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ",287.79000000000002,"ΤΕΜ",1,"EP",1,"3VA10322ED320CC0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1032-3ED32-0AE0","circuit breaker 3VA1 IEC frame 100 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM210, FTFM, In=32A overload protection Ir=32A fixed short-circuit protection Ii=10 x In nut keeper kit 4 auxiliary switches HQ",238.96,"ΤΕΜ",1,"EP",1,"3VA10323ED320AE0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1032-4ED36-0BH0","circuit breaker 3VA1 IEC frame 100 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM210, FTFM, In=32A overload protection Ir=32A fixed short-circuit protection Ii=10 x In clamp connection undervoltage release (UVR) 24V DC 2 auxiliary switches HQ 1 trip alarm switch HQ",333.14,"ΤΕΜ",1,"EP",1,"3VA10324ED360BH0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1032-4ED36-0KH0","circuit breaker 3VA1 IEC frame 100 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM210, FTFM, In=32A overload protection Ir=32A fixed short-circuit protection Ii=10 x In clamp connection shunt trip (STL) 220-250V DC, 208-277V AC 2 auxiliary switches HQ 1 trip alarm switch HQ",312.79000000000002,"ΤΕΜ",1,"EP",1,"3VA10324ED360KH0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1040-3ED32-0DA0","circuit breaker 3VA1 IEC frame 100 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM210, FTFM, In=40A overload protection Ir=40A fixed short-circuit protection Ii=10 x In nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz",252.33,"ΤΕΜ",1,"EP",1,"3VA10403ED320DA0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1050-2ED32-0CA0","circuit breaker 3VA1 IEC frame 100 breaking capacity class B Icu=16kA @ 415V 3-pole, line protection TM210, FTFM, In=50A overload protection Ir=50A fixed short-circuit protection Ii=10 x In nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz",248.84,"ΤΕΜ",1,"EP",1,"3VA10502ED320CA0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1050-3ED32-0CC0","circuit breaker 3VA1 IEC frame 100 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM210, FTFM, In=50A overload protection Ir=50A fixed short-circuit protection Ii=10 x In nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ",291.27999999999997,"ΤΕΜ",1,"EP",1,"3VA10503ED320CC0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1050-3ED42-0AF0","circuit breaker 3VA1 IEC frame 100 breaking capacity class N Icu=25kA @ 415V 4-pole, line protection TM210, FTFM, In=50A overload protection Ir=50A fixed short-circuit protection Ii=10 x In N conductor unprotected nut keeper kit 1 auxiliary switch HQ 1 trip alarm switch HQ",247.68,"ΤΕΜ",1,"EP",1,"3VA10503ED420AF0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1050-4ED32-0AA0","circuit breaker 3VA1 IEC frame 100 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM210, FTFM, In=50A overload protection Ir=50A fixed short-circuit protection Ii=10 x In nut keeper kit",162.79,"ΤΕΜ",1,"EP",1,"3VA10504ED320AA0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1063-2ED36-0AA0","circuit breaker 3VA1 IEC frame 100 breaking capacity class B Icu=16kA @ 415V 3-pole, line protection TM210, FTFM, In=63A overload protection Ir=63A fixed short-circuit protection Ii=10 x In clamp connection",175,"ΤΕΜ",1,"EP",1,"3VA10632ED360AA0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1063-2ED36-0JH0","circuit breaker 3VA1 IEC frame 100 breaking capacity class B Icu=16kA @ 415V 3-pole, line protection TM210, FTFM, In=63A overload protection Ir=63A fixed short-circuit protection Ii=10 x In clamp connection shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",305.24,"ΤΕΜ",1,"EP",1,"3VA10632ED360JH0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1063-3ED36-0KA0","circuit breaker 3VA1 IEC frame 100 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM210, FTFM, In=63A overload protection Ir=63A fixed short-circuit protection Ii=10 x In clamp connection shunt trip (STL) 220-250V DC, 208-277V AC",249.42,"ΤΕΜ",1,"EP",1,"3VA10633ED360KA0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1063-4ED32-0HA0","circuit breaker 3VA1 IEC frame 100 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM210, FTFM, In=63A overload protection Ir=63A fixed short-circuit protection Ii=10 x In nut keeper kit shunt trip (STL) 12-30V DC, 24V AC 50/60Hz",233.72,"ΤΕΜ",1,"EP",1,"3VA10634ED320HA0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1063-4ED42-0AF0","circuit breaker 3VA1 IEC frame 100 breaking capacity class S Icu=36kA @ 415V 4-pole, line protection TM210, FTFM, In=63A overload protection Ir=63A fixed short-circuit protection Ii=10 x In N conductor unprotected nut keeper kit 1 auxiliary switch HQ 1 trip alarm switch HQ",252.33,"ΤΕΜ",1,"EP",1,"3VA10634ED420AF0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1080-2ED42-0CH0","circuit breaker 3VA1 IEC frame 100 breaking capacity class B Icu=16kA @ 415V 4-pole, line protection TM210, FTFM, In=80A overload protection Ir=80A fixed short-circuit protection Ii=10 x In N conductor unprotected nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",374.42,"ΤΕΜ",1,"EP",1,"3VA10802ED420CH0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1080-3ED42-0DC0","circuit breaker 3VA1 IEC frame 100 breaking capacity class N Icu=25kA @ 415V 4-pole, line protection TM210, FTFM, In=80A overload protection Ir=80A fixed short-circuit protection Ii=10 x In N conductor unprotected nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ",358.14,"ΤΕΜ",1,"EP",1,"3VA10803ED420DC0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1080-4ED32-0BH0","circuit breaker 3VA1 IEC frame 100 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM210, FTFM, In=80A overload protection Ir=80A fixed short-circuit protection Ii=10 x In nut keeper kit undervoltage release (UVR) 24V DC 2 auxiliary switches HQ 1 trip alarm switch HQ",329.07,"ΤΕΜ",1,"EP",1,"3VA10804ED320BH0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1080-4ED42-0AE0","circuit breaker 3VA1 IEC frame 100 breaking capacity class S Icu=36kA @ 415V 4-pole, line protection TM210, FTFM, In=80A overload protection Ir=80A fixed short-circuit protection Ii=10 x In N conductor unprotected nut keeper kit 4 auxiliary switches HQ",312.20999999999998,"ΤΕΜ",1,"EP",1,"3VA10804ED420AE0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1096-3ED32-0KH0","circuit breaker 3VA1 IEC frame 100 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM210, FTFM, In=16A overload protection Ir=16A fixed short-circuit protection Ii=10 x In nut keeper kit shunt trip (STL) 220-250V DC, 208-277V AC 2 auxiliary switches HQ 1 trip alarm switch HQ",290.7,"ΤΕΜ",1,"EP",1,"3VA10963ED320KH0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1110-1AA32-0BH0","switch disconnector 3VA1 IEC frame 160 3-pole SD100, In=100A without overload protection w/o short-circuit protection nut keeper kit undervoltage release (UVR) 24V DC 2 auxiliary switches HQ 1 trip alarm switch HQ",381.58,"ΤΕΜ",1,"EP",1,"3VA11101AA320BH0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1110-1AA42-0JC0","switch disconnector 3VA1 IEC frame 160 4-pole SD100, In=100A without overload protection w/o short-circuit protection nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ",396.72,"ΤΕΜ",1,"EP",1,"3VA11101AA420JC0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1110-3EE46-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 4-pole, line protection TM220, ATFM, In=100A overload protection Ir=70A...100A short-circuit protection Ii=10 x In N conductor unprotected clamp connection",305.24,"ΤΕΜ",1,"EP",1,"3VA11103EE460AA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1110-4EF32-0BH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=100A overload protection Ir=70A...100A short-circuit protection Ii=5...10 x In nut keeper kit undervoltage release (UVR) 24V DC 2 auxiliary switches HQ 1 trip alarm switch HQ",434.46,"ΤΕΜ",1,"EP",1,"3VA11104EF320BH0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1110-4EF36-0AE0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=100A overload protection Ir=70A...100A short-circuit protection Ii=5...10 x In clamp connection 4 auxiliary switches HQ",376.28,"ΤΕΜ",1,"EP",1,"3VA11104EF360AE0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1110-5ED32-0AE0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM210, FTFM, In=100A overload protection Ir=100A fixed short-circuit protection Ii=10 x In nut keeper kit 4 auxiliary switches HQ",360.47,"ΤΕΜ",1,"EP",1,"3VA11105ED320AE0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1110-5EF32-0CC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=100A overload protection Ir=70A...100A short-circuit protection Ii=5...10 x In nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ",437.62,"ΤΕΜ",1,"EP",1,"3VA11105EF320CC0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1110-5MH32-0HA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, starter protection TM120M, AM, In=100A without overload protection short-circuit protection Ii=5...15 x In nut keeper kit shunt trip (STL) 12-30 V DC; 24 V AC 50/60 Hz",373.12,"ΤΕΜ",1,"EP",1,"3VA11105MH320HA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1110-5MH36-0CC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, starter protection TM120M, AM, In=100A without overload protection short-circuit protection Ii=5...15 x In clamp connection undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ",459.75,"ΤΕΜ",1,"EP",1,"3VA11105MH360CC0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1110-6EF32-0HA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM240, ATAM, In=100A overload protection Ir=70A...100A short-circuit protection Ii=5...10 x In nut keeper kit shunt trip (STL) 12-30V DC, 24V AC 50/60Hz",400.31,"ΤΕΜ",1,"EP",1,"3VA11106EF320HA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1110-6MH32-0KH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, starter protection TM120M, AM, In=100A without overload protection short-circuit protection Ii=5...15 x In nut keeper kit shunt trip (STL) 220-250 V DC; 208-277 V AC 2 auxiliary switches HQ 1 trip alarm switch HQ",464.18,"ΤΕΜ",1,"EP",1,"3VA11106MH320KH0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1112-1AA32-0KC0","switch disconnector 3VA1 IEC frame 160 3-pole SD100, In=125A without overload protection w/o short-circuit protection nut keeper kit shunt trip (STL) 220-250V DC; 208-277V AC 2 auxiliary switches HQ",380.07,"ΤΕΜ",1,"EP",1,"3VA11121AA320KC0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1112-3ED42-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 4-pole, line protection TM210, FTFM, In=125A overload protection Ir=125A fixed short-circuit protection Ii=10 x In N conductor unprotected nut keeper kit",428.04,"ΤΕΜ",1,"EP",1,"3VA11123ED420AA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1112-3EF32-0DC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM240, ATAM, In=125A overload protection Ir=88A...125A short-circuit protection Ii=5...10 x In nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ",480.22,"ΤΕΜ",1,"EP",1,"3VA11123EF320DC0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1112-4EF36-0AE0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=125A overload protection Ir=88A...125A short-circuit protection Ii=5...10 x In clamp connection 4 auxiliary switches HQ",479.66,"ΤΕΜ",1,"EP",1,"3VA11124EF360AE0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1112-4EF36-0KH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=125A overload protection Ir=88A...125A short-circuit protection Ii=5...10 x In clamp connection shunt trip (STL) 220-250V DC, 208-277V AC 2 auxiliary switches HQ 1 trip alarm switch HQ",528.46,"ΤΕΜ",1,"EP",1,"3VA11124EF360KH0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1112-5ED32-0KA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM210, FTFM, In=125A overload protection Ir=125A fixed short-circuit protection Ii=10 x In nut keeper kit shunt trip (STL) 220-250V DC, 208-277V AC",496.49,"ΤΕΜ",1,"EP",1,"3VA11125ED320KA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1112-5MH32-0DH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, starter protection TM120M, AM, In=125A without overload protection short-circuit protection Ii=5...15 x In nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",607.82000000000005,"ΤΕΜ",1,"EP",1,"3VA11125MH320DH0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1112-6EF32-0AE0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM240, ATAM, In=125A overload protection Ir=88A...125A short-circuit protection Ii=5...10 x In nut keeper kit 4 auxiliary switches HQ",606.47,"ΤΕΜ",1,"EP",1,"3VA11126EF320AE0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1112-6EF36-0JC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM240, ATAM, In=125A overload protection Ir=88A...125A short-circuit protection Ii=5...10 x In clamp connection shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ",664.02,"ΤΕΜ",1,"EP",1,"3VA11126EF360JC0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1116-1AA32-0AD0","switch disconnector 3VA1 IEC frame 160 3-pole SD100, In=160A without overload protection w/o short-circuit protection nut keeper kit 3 auxiliary switches HQ",343.39,"ΤΕΜ",1,"EP",1,"3VA11161AA320AD0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1116-1AA32-0KC0","switch disconnector 3VA1 IEC frame 160 3-pole SD100, In=160A without overload protection w/o short-circuit protection nut keeper kit shunt trip (STL) 220-250V DC; 208-277V AC 2 auxiliary switches HQ",399.68,"ΤΕΜ",1,"EP",1,"3VA11161AA320KC0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1116-3ED26-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 2-pole, line protection TM210, FTFM, In=160A overload protection Ir=160A fixed short-circuit protection Ii=10 x In clamp connection",361.17,"ΤΕΜ",1,"EP",1,"3VA11163ED260AA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1116-3EF36-0DA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM240, ATAM, In=160A overload protection Ir=112A...160A short-circuit protection Ii=5...10 x In clamp connection undervoltage release (UVR) 208-230V AC 50/60Hz",549.6,"ΤΕΜ",1,"EP",1,"3VA11163EF360DA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1116-4EF32-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=160A overload protection Ir=112A...160A short-circuit protection Ii=5...10 x In nut keeper kit",420.76,"ΤΕΜ",1,"EP",1,"3VA11164EF320AA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1116-5ED32-0AD0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM210, FTFM, In=160A overload protection Ir=160A fixed short-circuit protection Ii=10 x In nut keeper kit 3 auxiliary switches HQ",530.20000000000005,"ΤΕΜ",1,"EP",1,"3VA11165ED320AD0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1116-5ED32-0KC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM210, FTFM, In=160A overload protection Ir=160A fixed short-circuit protection Ii=10 x In nut keeper kit shunt trip (STL) 220-250V DC, 208-277V AC 2 auxiliary switches HQ",582.05999999999995,"ΤΕΜ",1,"EP",1,"3VA11165ED320KC0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1116-5EF36-0KA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=160A overload protection Ir=112A...160A short-circuit protection Ii=5...10 x In clamp connection shunt trip (STL) 220-250V DC, 208-277V AC",572.58000000000004,"ΤΕΜ",1,"EP",1,"3VA11165EF360KA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1116-6EE42-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 4-pole, line protection TM220, ATFM, In=160A overload protection Ir=112A...160A short-circuit protection Ii=10 x In N conductor unprotected nut keeper kit",764.69,"ΤΕΜ",1,"EP",1,"3VA11166EE420AA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1116-6EF36-0CA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM240, ATAM, In=160A overload protection Ir=112A...160A short-circuit protection Ii=5...10 x In clamp connection undervoltage release (UVR) 120-127V AC 50/60Hz",732.56,"ΤΕΜ",1,"EP",1,"3VA11166EF360CA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1120-3EE46-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 4-pole, line protection TM220, ATFM, In=20A overload protection Ir=14A...20A short-circuit protection Ii=16 x In N conductor unprotected clamp connection",275.27999999999997,"ΤΕΜ",1,"EP",1,"3VA11203EE460AA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1120-4EF32-0AB0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=20A overload protection Ir=14A...20A short-circuit protection Ii=8...16 x In nut keeper kit 2 auxiliary switches HP",283.05,"ΤΕΜ",1,"EP",1,"3VA11204EF320AB0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1120-4EF36-0HC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=20A overload protection Ir=14A...20A short-circuit protection Ii=8...16 x In clamp connection shunt trip (STL) 12-30V DC, 24V AC 50/60Hz 2 auxiliary switches HQ",361.42,"ΤΕΜ",1,"EP",1,"3VA11204EF360HC0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1120-5ED36-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM210, FTFM, In=20A overload protection Ir=20A fixed short-circuit protection Ii=16 x In clamp connection",243.54,"ΤΕΜ",1,"EP",1,"3VA11205ED360AA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1120-6ED46-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 4-pole, line protection TM210, FTFM, In=20A overload protection Ir=20A fixed short-circuit protection Ii=16 x In N conductor unprotected clamp connection",350.73,"ΤΕΜ",1,"EP",1,"3VA11206ED460AA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1120-6EF36-0CH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM240, ATAM, In=20A overload protection Ir=14A...20A short-circuit protection Ii=8...16 x In clamp connection undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",459.46,"ΤΕΜ",1,"EP",1,"3VA11206EF360CH0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1125-4ED32-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM210, FTFM, In=25A overload protection Ir=25A fixed short-circuit protection Ii=12.8 x In nut keeper kit",201.45,"ΤΕΜ",1,"EP",1,"3VA11254ED320AA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1125-4GF46-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 4-pole, line protection TM240, ATAM, In=25A overload protection Ir=18A...25A short-circuit protection Ii=6.4...12.8 x In N conductor protection 100% clamp connection",309.27,"ΤΕΜ",1,"EP",1,"3VA11254GF460AA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1125-5GF42-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection TM240, ATAM, In=25A overload protection Ir=18A...25A short-circuit protection Ii=6.4...12.8 x In N conductor protection 100% nut keeper kit",309.27,"ΤΕΜ",1,"EP",1,"3VA11255GF420AA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1125-6EF32-0AD0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM240, ATAM, In=25A overload protection Ir=18A...25A short-circuit protection Ii=6.4...12.8 x In nut keeper kit 3 auxiliary switches HQ",334.15,"ΤΕΜ",1,"EP",1,"3VA11256EF320AD0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1132-3EF32-0AE0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM240, ATAM, In=32A overload protection Ir=22A...32A short-circuit protection Ii=5...10 x In nut keeper kit 4 auxiliary switches HQ",287.32,"ΤΕΜ",1,"EP",1,"3VA11323EF320AE0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1132-4EF32-0AF0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=32A overload protection Ir=22A...32A short-circuit protection Ii=5...10 x In nut keeper kit 1 auxiliary switch HQ 1 trip alarm switch HQ",258.91000000000003,"ΤΕΜ",1,"EP",1,"3VA11324EF320AF0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1132-5EF32-0AE0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=32A overload protection Ir=22A...32A short-circuit protection Ii=5...10 x In nut keeper kit 4 auxiliary switches HQ",326.06,"ΤΕΜ",1,"EP",1,"3VA11325EF320AE0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1132-5EF36-0JC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=32A overload protection Ir=22A...32A short-circuit protection Ii=5...10 x In clamp connection shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ",381.58,"ΤΕΜ",1,"EP",1,"3VA11325EF360JC0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1132-6EF36-0JH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM240, ATAM, In=32A overload protection Ir=22A...32A short-circuit protection Ii=5...10 x In clamp connection shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",435.59,"ΤΕΜ",1,"EP",1,"3VA11326EF360JH0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1140-3ED26-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 2-pole, line protection TM210, FTFM, In=40A overload protection Ir=40A fixed short-circuit protection Ii=10 x In clamp connection",180.14,"ΤΕΜ",1,"EP",1,"3VA11403ED260AA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1140-3EF36-0BH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM240, ATAM, In=40A overload protection Ir=28A...40A short-circuit protection Ii=5...10 x In clamp connection undervoltage release (UVR) 24V DC 2 auxiliary switches HQ 1 trip alarm switch HQ",387.4,"ΤΕΜ",1,"EP",1,"3VA11403EF360BH0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1140-4EF36-0CC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=40A overload protection Ir=28A...40A short-circuit protection Ii=5...10 x In clamp connection undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ",384.17,"ΤΕΜ",1,"EP",1,"3VA11404EF360CC0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1140-5EF32-0AF0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=40A overload protection Ir=28A...40A short-circuit protection Ii=5...10 x In nut keeper kit 1 auxiliary switch HQ 1 trip alarm switch HQ",282.14999999999998,"ΤΕΜ",1,"EP",1,"3VA11405EF320AF0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1140-6EF32-0BC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM240, ATAM, In=40A overload protection Ir=28A...40A short-circuit protection Ii=5...10 x In nut keeper kit undervoltage release (UVR) 24V DC 2 auxiliary switches HQ",417.03,"ΤΕΜ",1,"EP",1,"3VA11406EF320BC0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1140-6EF42-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 4-pole, line protection TM240, ATAM, In=40A overload protection Ir=28A...40A short-circuit protection Ii=5...10 x In N conductor unprotected nut keeper kit",346.09,"ΤΕΜ",1,"EP",1,"3VA11406EF420AA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1150-3EF36-0HA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM240, ATAM, In=50A overload protection Ir=35A...50A short-circuit protection Ii=5...10 x In clamp connection shunt trip (STL) 12-30V DC, 24V AC 50/60Hz",297.64999999999998,"ΤΕΜ",1,"EP",1,"3VA11503EF360HA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1150-4EF32-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=50A overload protection Ir=35A...50A short-circuit protection Ii=5...10 x In nut keeper kit",216.94,"ΤΕΜ",1,"EP",1,"3VA11504EF320AA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1150-4EF36-0HA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=50A overload protection Ir=35A...50A short-circuit protection Ii=5...10 x In clamp connection shunt trip (STL) 12-30V DC, 24V AC 50/60Hz",316.37,"ΤΕΜ",1,"EP",1,"3VA11504EF360HA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1150-5EF36-0HC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=50A overload protection Ir=35A...50A short-circuit protection Ii=5...10 x In clamp connection shunt trip (STL) 12-30V DC, 24V AC 50/60Hz 2 auxiliary switches HQ",381.58,"ΤΕΜ",1,"EP",1,"3VA11505EF360HC0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1150-6EF36-0KA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM240, ATAM, In=50A overload protection Ir=35A...50A short-circuit protection Ii=5...10 x In clamp connection shunt trip (STL) 220-250V DC, 208-277V AC",369.29,"ΤΕΜ",1,"EP",1,"3VA11506EF360KA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1163-1AA32-0DA0","switch disconnector 3VA1 IEC frame 160 3-pole SD100, In=63A without overload protection w/o short-circuit protection nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz",271.83,"ΤΕΜ",1,"EP",1,"3VA11631AA320DA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1163-1AA36-0KA0","switch disconnector 3VA1 IEC frame 160 3-pole SD100, In=63A without overload protection w/o short-circuit protection clamp connection shunt trip (STL) 220-250V DC; 208-277V AC",268.52,"ΤΕΜ",1,"EP",1,"3VA11631AA360KA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1163-3EF42-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 4-pole, line protection TM240, ATAM, In=63A overload protection Ir=44A...63A short-circuit protection Ii=5...10 x In N conductor unprotected nut keeper kit",255,"ΤΕΜ",1,"EP",1,"3VA11633EF420AA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1163-4EE42-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 4-pole, line protection TM220, ATFM, In=63A overload protection Ir=44A...63A short-circuit protection Ii=10 x In N conductor unprotected nut keeper kit",262.64999999999998,"ΤΕΜ",1,"EP",1,"3VA11634EE420AA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1163-5ED32-0BC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM210, FTFM, In=63A overload protection Ir=63A fixed short-circuit protection Ii=10 x In nut keeper kit undervoltage release (UVR) 24V DC 2 auxiliary switches HQ",361.47,"ΤΕΜ",1,"EP",1,"3VA11635ED320BC0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1163-5EE32-0JC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM220, ATFM, In=63A overload protection Ir=44A...63A short-circuit protection Ii=10 x In nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ",344.89,"ΤΕΜ",1,"EP",1,"3VA11635EE320JC0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1163-5MH32-0AD0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, starter protection TM120M, AM, In=63A without overload protection short-circuit protection Ii=5...15 x In nut keeper kit 3 auxiliary switches HQ",299.63,"ΤΕΜ",1,"EP",1,"3VA11635MH320AD0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1163-5MH32-0JH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, starter protection TM120M, AM, In=63A without overload protection short-circuit protection Ii=5...15 x In nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",379.32,"ΤΕΜ",1,"EP",1,"3VA11635MH320JH0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1163-6EF32-0AF0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM240, ATAM, In=63A overload protection Ir=44A...63A short-circuit protection Ii=5...10 x In nut keeper kit 1 auxiliary switch HQ 1 trip alarm switch HQ",309.62,"ΤΕΜ",1,"EP",1,"3VA11636EF320AF0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1163-6MH32-0HH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, starter protection TM120M, AM, In=63A without overload protection short-circuit protection Ii=5...15 x In nut keeper kit shunt trip (STL) 12-30 V DC; 24 V AC 50/60 Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",415.04,"ΤΕΜ",1,"EP",1,"3VA11636MH320HH0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1180-3EE32-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM220, ATFM, In=80A overload protection Ir=56A...80A short-circuit protection Ii=10 x In nut keeper kit",163.38,"ΤΕΜ",1,"EP",1,"3VA11803EE320AA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1180-4ED36-0AC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM210, FTFM, In=80A overload protection Ir=80A fixed short-circuit protection Ii=10 x In clamp connection circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM210, FTFM, In=80A overload protection Ir=80A fixed short-circuit protection Ii=10 x In clamp connection 2 auxiliary switch changeover H",286.67,"ΤΕΜ",1,"EP",1,"3VA11804ED360AC0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1180-4EF36-0AF0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=80A overload protection Ir=56A...80A short-circuit protection Ii=5...10 x In clamp connection 1 auxiliary switch HQ 1 trip alarm switch HQ",300.24,"ΤΕΜ",1,"EP",1,"3VA11804EF360AF0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1180-5EF36-0BC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=80A overload protection Ir=56A...80A short-circuit protection Ii=5...10 x In clamp connection undervoltage release (UVR) 24V DC 2 auxiliary switches HQ",426.78,"ΤΕΜ",1,"EP",1,"3VA11805EF360BC0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1180-5GE42-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection TM220, ATFM, In=80A overload protection Ir=56A...80A short-circuit protection Ii=10 x In N conductor protection 100% nut keeper kit",322.83,"ΤΕΜ",1,"EP",1,"3VA11805GE420AA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1196-3EE32-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM220, ATFM, In=16A overload protection Ir=11A...16A short-circuit protection Ii=20 x In nut keeper kit",189.18,"ΤΕΜ",1,"EP",1,"3VA11963EE320AA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1196-3EF32-0DH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM240, ATAM, In=16A overload protection Ir=11A...16A short-circuit protection Ii=10...20 x In nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",366.09,"ΤΕΜ",1,"EP",1,"3VA11963EF320DH0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1196-4GD46-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 4-pole, line protection TM210, FTFM, In=16A overload protection Ir=16A fixed short-circuit protection Ii=20 x In N conductor protection 100% clamp connection",288.61,"ΤΕΜ",1,"EP",1,"3VA11964GD460AA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1196-5EF32-0CH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=16A overload protection Ir=11A...16A short-circuit protection Ii=10...20 x In nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",406.77,"ΤΕΜ",1,"EP",1,"3VA11965EF320CH0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1196-6EF32-0HC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM240, ATAM, In=16A overload protection Ir=11A...16A short-circuit protection Ii=10...20 x In nut keeper kit shunt trip (STL) 12-30V DC, 24V AC 50/60Hz 2 auxiliary switches HQ",393.16,"ΤΕΜ",1,"EP",1,"3VA11966EF320HC0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1216-4EF32-0AE0","circuit breaker 3VA1 IEC frame 250 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=160A overload protection Ir=112A...160A short-circuit protection Ii=5...10 x In nut keeper kit 4 auxiliary switches HQ",716.68,"ΤΕΜ",1,"EP",1,"3VA12164EF320AE0","3VA12 Διακότπες ισχύος κλειστού τύπου έως 250Α"]
["3VA1216-5EF32-0CA0","circuit breaker 3VA1 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=160A overload protection Ir=112A...160A short-circuit protection Ii=5...10 x In nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz",800.62,"ΤΕΜ",1,"EP",1,"3VA12165EF320CA0","3VA12 Διακότπες ισχύος κλειστού τύπου έως 250Α"]
["3VA1220-4EF32-0DC0","circuit breaker 3VA1 IEC frame 250 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=200A overload protection Ir=140A...200A short-circuit protection Ii=5...10 x In nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ",682.99,"ΤΕΜ",1,"EP",1,"3VA12204EF320DC0","3VA12 Διακότπες ισχύος κλειστού τύπου έως 250Α"]
["3VA1220-4EF42-0KC0","circuit breaker 3VA1 IEC frame 250 breaking capacity class S Icu=36kA @ 415V 4-pole, line protection TM240, ATAM, In=200A overload protection Ir=140A...200A short-circuit protection Ii=5...10 x In N conductor unprotected nut keeper kit shunt trip (STL) 220-250V DC; 208-277V AC 2 auxiliary switches HQ",831.71,"ΤΕΜ",1,"EP",1,"3VA12204EF420KC0","3VA12 Διακότπες ισχύος κλειστού τύπου έως 250Α"]
["3VA1220-5EF42-0DF0","circuit breaker 3VA1 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection TM240, ATAM, In=200A overload protection Ir=140A...200A short-circuit protection Ii=5...10 x In N conductor unprotected nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 1 auxiliary switch HQ 1 trip alarm switch HQ",911.32,"ΤΕΜ",1,"EP",1,"3VA12205EF420DF0","3VA12 Διακότπες ισχύος κλειστού τύπου έως 250Α"]
["3VA1220-5GF42-0AJ0","circuit breaker 3VA1 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection TM240, ATAM, In=200A overload protection Ir=140A...200A short-circuit protection Ii=5...10 x In N conductor protection 100% nut keeper kit 2 auxiliary switches HP 1 trip alarm switch HP",873.12,"ΤΕΜ",1,"EP",1,"3VA12205GF420AJ0","3VA12 Διακότπες ισχύος κλειστού τύπου έως 250Α"]
["3VA1220-6EF42-0JA0","circuit breaker 3VA1 IEC frame 250 breaking capacity class H Icu=70kA @ 415V 4-pole, line protection TM240, ATAM, In=200A overload protection Ir=140A...200A short-circuit protection Ii=5...10 x In N conductor unprotected nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz",884.65,"ΤΕΜ",1,"EP",1,"3VA12206EF420JA0","3VA12 Διακότπες ισχύος κλειστού τύπου έως 250Α"]
["3VA1220-6MH32-0BH0","circuit breaker 3VA1 IEC frame 250 breaking capacity class H Icu=70kA @ 415V 3-pole, starter protection TM120M, AM, In=200A without overload protection short-circuit protection Ii=6...14 x In nut keeper kit undervoltage release (UVR) 24V DC 2 auxiliary switches HQ 1 trip alarm switch HQ",1007.76,"ΤΕΜ",1,"EP",1,"3VA12206MH320BH0","3VA12 Διακότπες ισχύος κλειστού τύπου έως 250Α"]
["3VA1225-1AA42-0JA0","switch disconnector 3VA1 IEC frame 250 4-pole SD100, In=250A without overload protection w/o short-circuit protection nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz",709.41,"ΤΕΜ",1,"EP",1,"3VA12251AA420JA0","3VA12 Διακότπες ισχύος κλειστού τύπου έως 250Α"]
["3VA1225-4EF42-0CH0","circuit breaker 3VA1 IEC frame 250 breaking capacity class S Icu=36kA @ 415V 4-pole, line protection TM240, ATAM, In=250A overload protection Ir=175A...250A short-circuit protection Ii=5...10 x In N conductor unprotected nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",882.3,"ΤΕΜ",1,"EP",1,"3VA12254EF420CH0","3VA12 Διακότπες ισχύος κλειστού τύπου έως 250Α"]
["3VA1225-5EF32-0DH0","circuit breaker 3VA1 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=250A overload protection Ir=175A...250A short-circuit protection Ii=5...10 x In nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",954.92,"ΤΕΜ",1,"EP",1,"3VA12255EF320DH0","3VA12 Διακότπες ισχύος κλειστού τύπου έως 250Α"]
["3VA1225-5FF42-0AE0","circuit breaker 3VA1 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection TM240, ATAM, In=250A overload protection Ir=175A...250A short-circuit protection Ii=5...10 x In N conductor protection 50% nut keeper kit 4 auxiliary switches HQ",1106.7,"ΤΕΜ",1,"EP",1,"3VA12255FF420AE0","3VA12 Διακότπες ισχύος κλειστού τύπου έως 250Α"]
["3VA1225-5FF42-0KC0","circuit breaker 3VA1 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection TM240, ATAM, In=250A overload protection Ir=175A...250A short-circuit protection Ii=5...10 x In N conductor protection 50% nut keeper kit shunt trip (STL) 220-250V DC; 208-277V AC 2 auxiliary switches HQ",1144.6400000000001,"ΤΕΜ",1,"EP",1,"3VA12255FF420KC0","3VA12 Διακότπες ισχύος κλειστού τύπου έως 250Α"]
["3VA1225-6EF42-0DH0","circuit breaker 3VA1 IEC frame 250 breaking capacity class H Icu=70kA @ 415V 4-pole, line protection TM240, ATAM, In=250A overload protection Ir=175A...250A short-circuit protection Ii=5...10 x In N conductor unprotected nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",1398.93,"ΤΕΜ",1,"EP",1,"3VA12256EF420DH0","3VA12 Διακότπες ισχύος κλειστού τύπου έως 250Α"]
["3VA1332-4EF32-0DG0","circuit breaker 3VA1 IEC frame 400 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=320A overload protection Ir=224A...320A short-circuit protection Ii=5...10 x In nut keeper kit circuit breaker 3VA1 IEC frame 400 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=320A overload protection Ir=224A...320A short-circuit protection Ii=5...10 x In nut UNDERVOLTAGE RELEASE 208-230 V AC 50/60 HZ ACCESSORY FOR 3VA1 1 AUXILIARY SWITCH CHANGEOVER H 1 TRIP ALARM SWITCH CHANGEOVER",1152.82,"ΤΕΜ",1,"EP",1,"3VA13324EF320DG0","3VA13 Διακόπτες ισχύος κλειστού τύπου έως 400Α"]
["3VA1340-4EF32-0KA0","circuit breaker 3VA1 IEC frame 400 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=400A overload protection Ir=280A...400A short-circuit protection Ii=5...10 x In nut keeper kit circuit breaker 3VA1 IEC frame 400 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=400A overload protection Ir=280A...400A short-circuit protection Ii=5...10 x In nut SHUNT TRIP LEFT 208-277 V AC 50/60 HZ 220-250 V DC ACCESSORY",1068.76,"ΤΕΜ",1,"EP",1,"3VA13404EF320KA0","3VA13 Διακόπτες ισχύος κλειστού τύπου έως 400Α"]
["3VA1340-6EF32-0HJ0","circuit breaker 3VA1 IEC frame 400 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM240, ATAM, In=400A overload protection Ir=280A...400A short-circuit protection Ii=5...10 x In nut keeper kit circuit breaker 3VA1 IEC frame 400 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM240, ATAM, In=400A overload protection Ir=280A...400A short-circuit protection Ii=5...10 x In nut SHUNT TRIP LEFT 24 V AC 50/60 HZ / 24-30 V DC ACCESSORY FOR 2 AUXILIARY SWITCH CHANGEOVER H 1 TRIP ALARM SWITCH CHANGEOVER",1391.28,"ΤΕΜ",1,"EP",1,"3VA13406EF320HJ0","3VA13 Διακόπτες ισχύος κλειστού τύπου έως 400Α"]
["3VA1463-4GF42-0AA0","circuit breaker 3VA1 IEC frame 630 breaking capacity class S Icu=36kA @ 415V 4-pole, line protection TM240, ATAM, In=630A overload protection Ir=440A...630A short-circuit protection Ii=4...8 x In N conductor protection 100% nut keeper kit",1814.99,"ΤΕΜ",1,"EP",1,"3VA14634GF420AA0","3VA14 Διακόπτες ισχύος κλειστού τύπου έως 630Α"]
["3VA1463-5GF42-0DB0","circuit breaker 3VA1 IEC frame 630 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection TM240, ATAM, In=630A overload protection Ir=441A...630A short-circuit protection Ii=4...8 x In N conductor protection 100% nut keeper kit circuit breaker 3VA1 IEC frame 630 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection TM240, ATAM, In=630A overload protection Ir=441A...630A short-circuit UNDERVOLTAGE RELEASE 208-230 V AC 50/60 HZ ACCESSORY FOR 3VA1 2 AUXILIARY SWITCH CHANGEOVER H",2150.16,"ΤΕΜ",1,"EP",1,"3VA14635GF420DB0","3VA14 Διακόπτες ισχύος κλειστού τύπου έως 630Α"]
["3VA1580-5EF32-0AF0","circuit breaker 3VA1 IEC frame 1000 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=800A overload protection Ir=560A...800A short-circuit protection Ii=5 x In nut keeper kit 1 auxiliary switch HQ 1 trip alarm switch HQ",2200.75,"ΤΕΜ",1,"EP",1,"3VA15805EF320AF0","3VA15 Διακόπτες ισχύος κλειστού τύπου έως 1000Α"]
["3VA1580-6MH32-0AA0","circuit breaker 3VA1 IEC frame 1000 breaking capacity class H Icu=70kA @ 415V 3-pole, starter protection TM120M, AM, In=800A without overload protection short-circuit protection Ii=6...12 x In nut keeper kit",2371.5,"ΤΕΜ",1,"EP",1,"3VA15806MH320AA0","3VA15 Διακόπτες ισχύος κλειστού τύπου έως 1000Α"]
["3VA2010-5HL36-0BL0","circuit breaker 3VA2 IEC frame 100 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU320, LI, In=100A overload protection Ir=40A...100A short-circuit protection Ii=1.5...12 x In clamp connection undervoltage release (UVR) 24V DC 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",682.99,"ΤΕΜ",1,"EP",1,"3VA20105HL360BL0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2010-5HN32-0BL0","circuit breaker 3VA2 IEC frame 100 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU350, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In nut keeper kit undervoltage release (UVR) 24V DC 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",714.61,"ΤΕΜ",1,"EP",1,"3VA20105HN320BL0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2010-5JQ32-0BA0","circuit breaker 3VA2 IEC frame 100 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU560, LSIG, In=100A overload protection Ir=40A...100A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer gr.-fault prot., can be sw. off Ig=0.2...1 x In, tg=0.05-0.8s nut keeper kit undervoltage release (UVR) 24V DC",1201.56,"ΤΕΜ",1,"EP",1,"3VA20105JQ320BA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2010-5KP32-0CL0","circuit breaker 3VA2 IEC frame 100 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU850, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",1277.45,"ΤΕΜ",1,"EP",1,"3VA20105KP320CL0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2010-5KQ32-0AA0","circuit breaker 3VA2 IEC frame 100 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU860, LSIG, In=100A overload protection Ir=40A...100A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% gr.-fault prot., can be sw. off Ig=0.2...1 x In, tg=0.05-0.8s nut keeper kit",1201.56,"ΤΕΜ",1,"EP",1,"3VA20105KQ320AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2010-6HN32-0CA0","circuit breaker 3VA2 IEC frame 100 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU350, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz",670.34,"ΤΕΜ",1,"EP",1,"3VA20106HN320CA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2010-6JP36-0AA0","circuit breaker 3VA2 IEC frame 100 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU550, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% clamp connection",967.57,"ΤΕΜ",1,"EP",1,"3VA20106JP360AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2010-8KQ36-0AA0","circuit breaker 3VA2 IEC frame 100 breaking capacity class L Icu=150kA @ 415V 3-pole, line protection ETU860, LSIG, In=100A overload protection Ir=40A...100A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% gr.-fault prot., can be sw. off Ig=0.2...1 x In, tg=0.05-0.8s clamp connection",1384.96,"ΤΕΜ",1,"EP",1,"3VA20108KQ360AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2025-6HM46-0AA0","circuit breaker 3VA2 IEC frame 100 breaking capacity class H Icu=85kA @ 415V 4-pole, line protection ETU330, LIG, In=25A overload protection Ir=10A...25A short-circuit protection Ii=1.5...12 x In N conductor protection adjustable (OFF, 100%) ground-fault protection Ig=0.6...1 x In= tg=0.1/0.3s clamp connection",860.06,"ΤΕΜ",1,"EP",1,"3VA20256HM460AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2025-8KP46-0AA0","circuit breaker 3VA2 IEC frame 100 breaking capacity class L Icu=150kA @ 415V 4-pole, line protection ETU850, LSI, In=25A overload protection Ir=10A...25A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection adjustable (OFF, up to 160%) clamp connection",1384.96,"ΤΕΜ",1,"EP",1,"3VA20258KP460AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2040-6JP32-0AA0","circuit breaker 3VA2 IEC frame 100 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU550, LSI, In=40A overload protection Ir=16A...40A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% nut keeper kit",904.33,"ΤΕΜ",1,"EP",1,"3VA20406JP320AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2040-6KP46-0AA0","circuit breaker 3VA2 IEC frame 100 breaking capacity class H Icu=85kA @ 415V 4-pole, line protection ETU850, LSI, In=40A overload protection Ir=16A...40A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection adjustable (OFF, up to 160%) clamp connection",1258.48,"ΤΕΜ",1,"EP",1,"3VA20406KP460AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2063-5HL32-0BH0","circuit breaker 3VA2 IEC frame 100 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU320, LI, In=63A overload protection Ir=25A...63A short-circuit protection Ii=1.5...12 x In nut keeper kit undervoltage release (UVR) 24V DC 2 auxiliary switches HQ 1 trip alarm switch HQ",593.19000000000005,"ΤΕΜ",1,"EP",1,"3VA20635HL320BH0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2063-5HN32-0BA0","circuit breaker 3VA2 IEC frame 100 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU350, LSI, In=63A overload protection Ir=25A...63A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In nut keeper kit undervoltage release (UVR) 24V DC",584.97,"ΤΕΜ",1,"EP",1,"3VA20635HN320BA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2063-5HN36-0DC0","circuit breaker 3VA2 IEC frame 100 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU350, LSI, In=63A overload protection Ir=25A...63A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In clamp connection undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ",645.04999999999995,"ΤΕΜ",1,"EP",1,"3VA20635HN360DC0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2063-5JP46-0AA0","circuit breaker 3VA2 IEC frame 100 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection ETU550, LSI, In=63A overload protection Ir=25A...63A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection adjustable (OFF, up to 160%) clamp connection",999.19,"ΤΕΜ",1,"EP",1,"3VA20635JP460AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2063-5KP32-0HA0","circuit breaker 3VA2 IEC frame 100 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU850, LSI, In=63A overload protection Ir=25A...63A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer nut keeper kit shunt trip (STL) 12-30V DC; 24V AC 50/60Hz",1132,"ΤΕΜ",1,"EP",1,"3VA20635KP320HA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2063-6HN32-0AA0","circuit breaker 3VA2 IEC frame 100 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU350, LSI, In=63A overload protection Ir=25A...63A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In nut keeper kit",531.22,"ΤΕΜ",1,"EP",1,"3VA20636HN320AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2063-7JQ42-0AA0","circuit breaker 3VA2 IEC frame 100 breaking capacity class C Icu=110kA @ 415V 4-pole, line protection ETU560, LSIG, In=63A overload protection Ir=25A...63A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection adjustable (OFF, up to 160%) gr.-fault prot., can be sw. off Ig=0.25...1 x In= tg=0.05-0.8s nut keeper kit",1302.74,"ΤΕΜ",1,"EP",1,"3VA20637JQ420AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2110-0HL46-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class  E Icu=200 kA @ 415 V 4-pole, line protection ETU320,  LI, In=100A overload protection Ir=40A ... 100A short circuit protection Ii=1,5...12 x In neutral protection adjustable(OFF 50% 100%) cable connection",980.22,"ΤΕΜ",1,"EP",1,"3VA21100HL460AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2110-5HL36-0CH0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU320, LI, In=100A overload protection Ir=40A...100A short-circuit protection Ii=1.5...12 x In clamp connection undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",651.37,"ΤΕΜ",1,"EP",1,"3VA21105HL360CH0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2110-5HM36-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU330, LIG, In=100A overload protection Ir=40A...100A short-circuit protection Ii=1.5...12 x In ground-fault protection Ig=0.2...1 x In, tg=0.1/0.3s clamp connection",708.29,"ΤΕΜ",1,"EP",1,"3VA21105HM360AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2110-5HN46-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection ETU350, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In N conductor protection adjustable (OFF, 50%, 100%) clamp connection",670.34,"ΤΕΜ",1,"EP",1,"3VA21105HN460AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2110-5JQ32-0AD0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU560, LSIG, In=100A overload protection Ir=40A...100A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer gr.-fault prot., can be sw. off Ig=0.2...1 x In, tg=0.05-0.8s nut keeper kit 3 auxiliary switches HQ",1176.26,"ΤΕΜ",1,"EP",1,"3VA21105JQ320AD0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2110-5KP32-0BC0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU850, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer nut keeper kit undervoltage release (UVR) 24V DC 2 auxiliary switches HQ",1207.8800000000001,"ΤΕΜ",1,"EP",1,"3VA21105KP320BC0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2110-5MN36-0BH0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, motor protection ETU350M, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=3...15 x Ir, Ii=15 x In clamp connection undervoltage release (UVR) 24V DC 2 auxiliary switches HQ 1 trip alarm switch HQ",676.67,"ΤΕΜ",1,"EP",1,"3VA21105MN360BH0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2110-6HN32-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU350, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In nut keeper kit",571.05999999999995,"ΤΕΜ",1,"EP",1,"3VA21106HN320AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2110-6HN32-0CC0","circuit breaker 3VA2 IEC frame 160 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU350, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ",714.61,"ΤΕΜ",1,"EP",1,"3VA21106HN320CC0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2110-6HN36-0KC0","circuit breaker 3VA2 IEC frame 160 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU350, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In clamp connection shunt trip (STL) 220-250V DC, 208-277V AC 2 auxiliary switches HQ",708.29,"ΤΕΜ",1,"EP",1,"3VA21106HN360KC0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2110-7MN36-0BA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class C Icu=110kA @ 415V 3-pole, motor protection ETU350M, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=3...15 x Ir, Ii=15 x In clamp connection undervoltage release (UVR) 24V DC",695.64,"ΤΕΜ",1,"EP",1,"3VA21107MN360BA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2110-7MN36-0KC0","circuit breaker 3VA2 IEC frame 160 breaking capacity class C Icu=110kA @ 415V 3-pole, motor protection ETU350M, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=3...15 x Ir, Ii=15 x In clamp connection shunt trip (STL) 220-250V DC, 208-277V AC 2 auxiliary switches HQ",714.61,"ΤΕΜ",1,"EP",1,"3VA21107MN360KC0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2110-8HK32-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class L Icu=150kA @ 415V 3-pole, line protection ETU340, ELISA LI, In=100A overload protection Ir=40A...100A short-circuit protection Ii=15 x In nut keeper kit",623.54999999999995,"ΤΕΜ",1,"EP",1,"3VA21108HK320AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2116-0HN42-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class  E Icu=200 kA @ 415 V 4-pole, line protection ETU350,  LSI, In=160A overload protection Ir=63A ... 160A short circuit protection Isd=1,5...10xIr, Ii=12xIn neutral protection adjustable(OFF 50% 100%) busbar connection",1460.84,"ΤΕΜ",1,"EP",1,"3VA21160HN420AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2116-5HL36-0CC0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU320, LI, In=160A overload protection Ir=63A...160A short-circuit protection Ii=1.5...10 x In clamp connection undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ",860.06,"ΤΕΜ",1,"EP",1,"3VA21165HL360CC0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2116-5HN32-0AD0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU350, LSI, In=160A overload protection Ir=63A...160A short-circuit protection Isd=1.5...10 x Ir, Ii=10 x In nut keeper kit 3 auxiliary switches HQ",815.8,"ΤΕΜ",1,"EP",1,"3VA21165HN320AD0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2116-5HN36-0BA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU350, LSI, In=160A overload protection Ir=63A...160A short-circuit protection Isd=1.5...10 x Ir, Ii=10 x In clamp connection undervoltage release (UVR) 24V DC",872.71,"ΤΕΜ",1,"EP",1,"3VA21165HN360BA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2116-5JQ36-0AK0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU560, LSIG, In=160A overload protection Ir=63A...160A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection optionally with external current transformer, up to 160% gr.-fault prot., can be sw. off Ig=0.2...1 x In, tg=0.05-0.8s clamp connection circuit breaker 3VA2 IEC frame 160 breaking capacity class M 1 AUXILIARY SWITCH CHANGEOVER H 1 TRIP ALARM SWITCH CHANGEOVER 1 electrical alarm switch HQ",1448.2,"ΤΕΜ",1,"EP",1,"3VA21165JQ360AK0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2116-5KQ46-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection ETU860, LSIG, In=160A overload protection Ir=63A...160A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection adjustable (OFF, up to 100%) gr.-fault prot., can be sw. off Ig=0.2...1 x In= tg=0.05-0.8s clamp connection",1675.86,"ΤΕΜ",1,"EP",1,"3VA21165KQ460AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2116-6HN32-0JL0","circuit breaker 3VA2 IEC frame 160 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU350, LSI, In=160A overload protection Ir=63A...160A short-circuit protection Isd=1.5...10 x Ir, Ii=10 x In nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",1011.84,"ΤΕΜ",1,"EP",1,"3VA21166HN320JL0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2116-6KQ36-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU860, LSIG, In=160A overload protection Ir=63A...160A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection optionally with external current transformer, up to 160% gr.-fault prot., can be sw. off Ig=0.2...1 x In, tg=0.05-0.8s clamp connection",1555.7,"ΤΕΜ",1,"EP",1,"3VA21166KQ360AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2125-0MS32-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class  E Icu=200 kA @ 415 V 3-pole motor starter protection ETU310M, I, In=25A short circuit protection Ii=3...15 x In busbar connection",445.21,"ΤΕΜ",1,"EP",1,"3VA21250MS320AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2125-5JP46-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection ETU550, LSI, In=25A overload protection Ir=10A...25A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection adjustable (OFF, up to 160%) clamp connection",999.19,"ΤΕΜ",1,"EP",1,"3VA21255JP460AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2125-7MS32-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class C Icu=110kA @ 415V 3-pole, starter protection ETU310M, I, In=25A without overload protection short-circuit protection Ii=3...15 x In nut keeper kit",387.66,"ΤΕΜ",1,"EP",1,"3VA21257MS320AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2125-8JP46-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class L Icu=150kA @ 415V 4-pole, line protection ETU550, LSI, In=25A overload protection Ir=10A...25A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection adjustable (OFF, up to 160%) clamp connection",1195.24,"ΤΕΜ",1,"EP",1,"3VA21258JP460AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2140-5MN32-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, motor protection ETU350M, LSI, In=40A overload protection Ir=16A...40A short-circuit protection Isd=3...15 x Ir, Ii=15 x In nut keeper kit",470.51,"ΤΕΜ",1,"EP",1,"3VA21405MN320AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2140-6HL42-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class H Icu=85kA @ 415V 4-pole, line protection ETU320, LI, In=40A overload protection Ir=16A...40A short-circuit protection Ii=1.5...12 x In N conductor protection adjustable (OFF, 100%) nut keeper kit",606.47,"ΤΕΜ",1,"EP",1,"3VA21406HL420AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2140-8HK36-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class L Icu=150kA @ 415V 3-pole, line protection ETU340, ELISA LI, In=40A overload protection Ir=16A...40A short-circuit protection Ii=15 x In clamp connection",595.72,"ΤΕΜ",1,"EP",1,"3VA21408HK360AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2140-8JQ42-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class L Icu=150kA @ 415V 4-pole, line protection ETU560, LSIG, In=40A overload protection Ir=16A...40A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection adjustable (OFF, up to 160%) gr.-fault prot., can be sw. off Ig=0.4...1 x In= tg=0.05-0.8s nut keeper kit",1391.28,"ΤΕΜ",1,"EP",1,"3VA21408JQ420AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2163-5HL32-0AC0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU320, LI, In=63A overload protection Ir=25A...63A short-circuit protection Ii=1.5...12 x In nut keeper kit 2 auxiliary switches HQ",471.14,"ΤΕΜ",1,"EP",1,"3VA21635HL320AC0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2163-5HN32-0AD0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU350, LSI, In=63A overload protection Ir=25A...63A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In nut keeper kit 3 auxiliary switches HQ",547.03,"ΤΕΜ",1,"EP",1,"3VA21635HN320AD0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2163-5JP32-0BH0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU550, LSI, In=63A overload protection Ir=25A...63A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer nut keeper kit undervoltage release (UVR) 24V DC 2 auxiliary switches HQ 1 trip alarm switch HQ",1024.49,"ΤΕΜ",1,"EP",1,"3VA21635JP320BH0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2163-5JQ32-0CH0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU560, LSIG, In=63A overload protection Ir=25A...63A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer gr.-fault prot., can be sw. off Ig=0.25...1 x In, tg=0.05-0.8s nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",1245.83,"ΤΕΜ",1,"EP",1,"3VA21635JQ320CH0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2163-5KP32-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU850, LSI, In=63A overload protection Ir=25A...63A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% nut keeper kit",1043.46,"ΤΕΜ",1,"EP",1,"3VA21635KP320AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2163-5MN36-0HL0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, motor protection ETU350M, LSI, In=63A overload protection Ir=25A...63A short-circuit protection Isd=3...15 x Ir, Ii=15 x In clamp connection shunt trip (STL) 12-30V DC, 24V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",664.02,"ΤΕΜ",1,"EP",1,"3VA21635MN360HL0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2163-6HL32-0AC0","circuit breaker 3VA2 IEC frame 160 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU320, LI, In=63A overload protection Ir=25A...63A short-circuit protection Ii=1.5...12 x In nut keeper kit 2 auxiliary switches HQ",521.73,"ΤΕΜ",1,"EP",1,"3VA21636HL320AC0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2163-6HN32-0AF0","circuit breaker 3VA2 IEC frame 160 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU350, LSI, In=63A overload protection Ir=25A...63A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In nut keeper kit 1 auxiliary switch HQ 1 trip alarm switch HQ",572.95000000000005,"ΤΕΜ",1,"EP",1,"3VA21636HN320AF0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2163-6HN36-0BL0","circuit breaker 3VA2 IEC frame 160 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU350, LSI, In=63A overload protection Ir=25A...63A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In clamp connection undervoltage release (UVR) 24V DC 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",752.56,"ΤΕΜ",1,"EP",1,"3VA21636HN360BL0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2163-7HN32-0JC0","circuit breaker 3VA2 IEC frame 160 breaking capacity class C Icu=110kA @ 415V 3-pole, line protection ETU350, LSI, In=63A overload protection Ir=25A...63A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ",682.99,"ΤΕΜ",1,"EP",1,"3VA21637HN320JC0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2163-7MN32-0DA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class C Icu=110kA @ 415V 3-pole, motor protection ETU350M, LSI, In=63A overload protection Ir=25A...63A short-circuit protection Isd=3...15 x Ir, Ii=15 x In nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz",645.04999999999995,"ΤΕΜ",1,"EP",1,"3VA21637MN320DA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2163-7MN36-0AF0","circuit breaker 3VA2 IEC frame 160 breaking capacity class C Icu=110kA @ 415V 3-pole, motor protection ETU350M, LSI, In=63A overload protection Ir=25A...63A short-circuit protection Isd=3...15 x Ir, Ii=15 x In clamp connection 1 auxiliary switch HQ 1 trip alarm switch HQ",613.42999999999995,"ΤΕΜ",1,"EP",1,"3VA21637MN360AF0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2163-7MS36-0BC0","circuit breaker 3VA2 IEC frame 160 breaking capacity class C Icu=110kA @ 415V 3-pole, starter protection ETU310M, I, In=63A overload protection Ir=25A...63A short-circuit protection Ii=3...15 x In clamp connection undervoltage release (UVR) 24V DC",552.09,"ΤΕΜ",1,"EP",1,"3VA21637MS360BC0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2163-8HM46-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class L Icu=150kA @ 415V 4-pole, line protection ETU330, LIG, In=63A overload protection Ir=25A...63A short-circuit protection Ii=1.5...12 x In N conductor protection adjustable (OFF, 100%) ground-fault protection Ig=0.25...1 x In= tg=0.1/0.3s clamp connection",992.87,"ΤΕΜ",1,"EP",1,"3VA21638HM460AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2216-5MN32-0AH0","circuit breaker 3VA2 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 3-pole, motor protection ETU350M, LSI, In=160A overload protection Ir=63A...160A short-circuit protection Isd=3...15 x Ir, Ii=15 x In nut keeper kit 2 auxiliary switches HQ 1 trip alarm switch HQ",872.71,"ΤΕΜ",1,"EP",1,"3VA22165MN320AH0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2216-6HN32-0KF0","circuit breaker 3VA2 IEC frame 250 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU350, LSI, In=160A overload protection Ir=63A...160A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In nut keeper kit shunt trip (STL) 220-250V DC, 208-277V AC 1 auxiliary switch HQ 1 trip alarm switch HQ",1195.24,"ΤΕΜ",1,"EP",1,"3VA22166HN320KF0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2216-7MS32-0KC0","circuit breaker 3VA2 IEC frame 250 breaking capacity class C Icu=110kA @ 415V 3-pole, starter protection ETU310M, I, In=160A without overload protection short-circuit protection Ii=3...15 x In nut keeper kit circuit breaker 3VA2 IEC frame 250 breaking capacity class C Icu=110kA @ 415V 3-pole, starter protection ETU310M, I, In=160A without overload protection short-circuit protection Ii=3...15 x In nut SHUNT TRIP LEFT 208-277 V AC 50/60 HZ 220-250 V DC ACCESSORY 2 AUXILIARY SWITCH CHANGEOVER H",898.01,"ΤΕΜ",1,"EP",1,"3VA22167MS320KC0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2220-5MN32-0AA0","circuit breaker 3VA2 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 3-pole, motor protection ETU350M, LSI, In=200A overload protection Ir=80A...200A short-circuit protection Isd=3...15 x Ir, Ii=15 x In nut keeper kit",935.95,"ΤΕΜ",1,"EP",1,"3VA22205MN320AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2220-7MS32-0CC0","circuit breaker 3VA2 IEC frame 250 breaking capacity class C Icu=110kA @ 415V 3-pole, starter protection ETU310M, I, In=200A overload protection Ir=80A...200A short-circuit protection Ii=3...15 x In nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz",1081.4000000000001,"ΤΕΜ",1,"EP",1,"3VA22207MS320CC0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2225-0KQ32-0AA0","circuit breaker 3VA2 IEC frame 250 breaking capacity class  E Icu=200 kA @ 415 V 3-pole, line protection ETU860,  LSIG, In=250A overload protection Ir=100A ... 250A short circuit protection Isd=0,6...10xIn, Ii=1,5...10xIn busbar connection",2131.19,"ΤΕΜ",1,"EP",1,"3VA22250KQ320AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2225-5HL42-0JC0","circuit breaker 3VA2 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection ETU320, LI, In=250A overload protection Ir=100A...250A short-circuit protection Ii=1.5...10 x In N conductor protection adjustable (OFF, 50%, 100%) nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ",1328.04,"ΤΕΜ",1,"EP",1,"3VA22255HL420JC0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2225-5HN32-0KF0","circuit breaker 3VA2 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU350, LSI, In=250A overload protection Ir=100A...250A short-circuit protection Isd=1.5...10 x Ir, Ii=10 x In nut keeper kit circuit breaker 3VA2 IEC frame 250 breaking capacity class M Icu=55kA @ 415V shunt trip left 208-277V AC 50/60Hz 1 auxiliary switch HQ 1 trip alarm switch HQ",1087.73,"ΤΕΜ",1,"EP",1,"3VA22255HN320KF0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2225-5JP42-0AA0","circuit breaker 3VA2 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection ETU550, LSI, In=250A overload protection Ir=100A...250A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection adjustable (OFF, up to 100%) nut keeper kit",1637.92,"ΤΕΜ",1,"EP",1,"3VA22255JP420AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2225-5JQ42-0CH0","circuit breaker 3VA2 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection ETU560, LSIG, In=250A overload protection Ir=100A...250A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection adjustable (OFF, up to 100%) gr.-fault prot., can be sw. off Ig=0.2...1 x In= tg=0.05-0.8s nut keeper kit UNDERVOLTAGE RELEASE 120-127 V AC 50/60 HZ ACCESSORY FOR 3VA1 2 AUXILIARY SWITCH CHANGEOVER H 1 TRIP ALARM SWITCH CHANGEOVER",2011.03,"ΤΕΜ",1,"EP",1,"3VA22255JQ420CH0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2225-5KP32-0CL0","circuit breaker 3VA2 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU850, LSI, In=250A overload protection Ir=100A...250A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection optionally with external current transformer nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",1726.45,"ΤΕΜ",1,"EP",1,"3VA22255KP320CL0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2225-6HN32-0JC0","circuit breaker 3VA2 IEC frame 250 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU350, LSI, In=250A overload protection Ir=100A...250A short-circuit protection Isd=1.5...10 x Ir, Ii=10 x In nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ",1195.24,"ΤΕΜ",1,"EP",1,"3VA22256HN320JC0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2225-6JP32-0AJ0","circuit breaker 3VA2 IEC frame 250 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU550, LSI, In=250A overload protection Ir=100A...250A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection optionally with external current transformer nut keeper kit 2 auxiliary switches HP 1 trip alarm switch HP",1562.03,"ΤΕΜ",1,"EP",1,"3VA22256JP320AJ0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2225-6KP32-0BC0","circuit breaker 3VA2 IEC frame 250 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU850, LSI, In=250A overload protection Ir=100A...250A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection optionally with external current transformer nut keeper kit undervoltage release (UVR) 24V DC 2 auxiliary switches HQ",1796.02,"ΤΕΜ",1,"EP",1,"3VA22256KP320BC0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2225-6KP32-0KH0","circuit breaker 3VA2 IEC frame 250 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU850, LSI, In=250A overload protection Ir=100A...250A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection optionally with external current transformer nut keeper kit shunt trip (STL) 220-250V DC; 208-277V AC 2 auxiliary switches HQ 1 trip alarm switch HQ",1796.02,"ΤΕΜ",1,"EP",1,"3VA22256KP320KH0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2225-7KP32-0AF0","circuit breaker 3VA2 IEC frame 250 breaking capacity class C Icu=110kA @ 415V 3-pole, line protection ETU850, LSI, In=250A overload protection Ir=100A...250A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection optionally with external current transformer nut keeper kit 1 auxiliary switch HQ 1 trip alarm switch HQ",1770.72,"ΤΕΜ",1,"EP",1,"3VA22257KP320AF0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2225-8HL32-0AE0","circuit breaker 3VA2 IEC frame 250 breaking capacity class L Icu=150kA @ 415V 3-pole, line protection ETU320, LI, In=250A overload protection Ir=100A...250A short-circuit protection Ii=1.5...10 x In nut keeper kit 4 auxiliary switches HQ",1353.34,"ΤΕΜ",1,"EP",1,"3VA22258HL320AE0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2225-8HL32-0KA0","circuit breaker 3VA2 IEC frame 250 breaking capacity class L Icu=150kA @ 415V 3-pole, line protection ETU320, LI, In=250A overload protection Ir=100A...250A short-circuit protection Ii=1.5...10 x In nut keeper kit shunt trip (STL) 220-250V DC, 208-277V AC",1347.01,"ΤΕΜ",1,"EP",1,"3VA22258HL320KA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2325-5HN32-0AA0","circuit breaker 3VA2 IEC frame 400 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU350, LSI, In=250A overload protection Ir=100A...250A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In nut keeper kit",1296.42,"ΤΕΜ",1,"EP",1,"3VA23255HN320AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2325-5MN32-0JC0","circuit breaker 3VA2 IEC frame 400 breaking capacity class M Icu=55kA @ 415V 3-pole, motor protection ETU350M, LSI, In=250A overload protection Ir=100A...250A short-circuit protection Isd=3...15 x Ir, Ii=15 x In nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ",1448.2,"ΤΕΜ",1,"EP",1,"3VA23255MN320JC0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2325-6HL32-0JA0","circuit breaker 3VA2 IEC frame 400 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU320, LI, In=250A overload protection Ir=100A...250A short-circuit protection Ii=1.5...12 x In nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz",1441.87,"ΤΕΜ",1,"EP",1,"3VA23256HL320JA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2325-6HN32-0BC0","circuit breaker 3VA2 IEC frame 400 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU350, LSI, In=250A overload protection Ir=100A...250A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In nut keeper kit undervoltage release (UVR) 24V DC 2 auxiliary switches HQ",1599.97,"ΤΕΜ",1,"EP",1,"3VA23256HN320BC0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2325-8HK32-0AA0","circuit breaker 3VA2 IEC frame 400 breaking capacity class L Icu=150kA @ 415V 3-pole, line protection ETU340, ELISA LI, In=250A overload protection Ir=100A...250A short-circuit protection Ii=15 x In nut keeper kit",1688.51,"ΤΕΜ",1,"EP",1,"3VA23258HK320AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2340-0HN32-0AA0","circuit breaker 3VA2 IEC frame 400 breaking capacity class  E Icu=200 kA @ 415 V 3-pole, line protection ETU350,  LSI, In=400A overload protection Ir=160A ... 400A short circuit protection Isd=1,5...10xIr, Ii=12xIn busbar connection",1897.2,"ΤΕΜ",1,"EP",1,"3VA23400HN320AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2340-5HL42-0JH0","circuit breaker 3VA2 IEC frame 400 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection ETU320, LI, In=400A overload protection Ir=160A...400A short-circuit protection Ii=1.5...10 x In N conductor protection adjustable (OFF, 50%, 100%) nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",1707.48,"ΤΕΜ",1,"EP",1,"3VA23405HL420JH0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2340-5HN32-0KA0","circuit breaker 3VA2 IEC frame 400 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU350, LSI, In=400A overload protection Ir=160A...400A short-circuit protection Isd=1.5...10 x Ir, Ii=10 x In nut keeper kit shunt trip (STL) 220-250V DC, 208-277V AC",1372.31,"ΤΕΜ",1,"EP",1,"3VA23405HN320KA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2340-5JP32-0JL0","circuit breaker 3VA2 IEC frame 400 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU550, LSI, In=400A overload protection Ir=160A...400A short-circuit protection Isd=0.6...10 x In, Ii=1.5 x In N conductor protection optionally with external current transformer, up to 160% nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",1846.61,"ΤΕΜ",1,"EP",1,"3VA23405JP320JL0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2340-5JQ32-0CH0","circuit breaker 3VA2 IEC frame 400 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU560, LSIG, In=400A overload protection Ir=160A...400A short-circuit protection Isd=0.6...10 x In, Ii=1.5 x In N conductor protection optionally with external current transformer, up to 160% gr.-fault prot., can be sw. off Ig=0.2...1 x In, tg=0.05-0.8s nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",2055.3000000000002,"ΤΕΜ",1,"EP",1,"3VA23405JQ320CH0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2340-5KP32-0AJ0","circuit breaker 3VA2 IEC frame 400 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU850, LSI, In=400A overload protection Ir=160A...400A short-circuit protection Isd=0.6...10 x In, Ii=1.5 x In N conductor protection optionally with external current transformer, up to 160% nut keeper kit 2 auxiliary switches HP 1 trip alarm switch HP",1960.44,"ΤΕΜ",1,"EP",1,"3VA23405KP320AJ0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2340-6HL32-0HC0","circuit breaker 3VA2 IEC frame 400 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU320, LI, In=400A overload protection Ir=160A...400A short-circuit protection Ii=1.5...10 x In nut keeper kit shunt trip (STL) 12-30V DC, 24V AC 50/60Hz 2 auxiliary switches HQ",1473.49,"ΤΕΜ",1,"EP",1,"3VA23406HL320HC0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2340-6HN32-0HL0","circuit breaker 3VA2 IEC frame 400 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU350, LSI, In=400A overload protection Ir=160A...400A short-circuit protection Isd=1.5...10 x Ir, Ii=10 x In nut keeper kit shunt trip (STL) 12-30V DC, 24V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",1637.92,"ΤΕΜ",1,"EP",1,"3VA23406HN320HL0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2340-6JQ32-0HL0","circuit breaker 3VA2 IEC frame 400 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU560, LSIG, In=400A overload protection Ir=160A...400A short-circuit protection Isd=0.6...10 x In, Ii=1.5 x In N conductor protection, opt. w. ext. curr. transf., up to 160% gr.-fault prot., can be sw. off Ig=0.2...1 x In= tg=0.05-0.8s nut keeper kit shunt trip (STL) 12-30V DC; 24V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",2219.7199999999998,"ΤΕΜ",1,"EP",1,"3VA23406JQ320HL0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2340-7HL32-0JA0","circuit breaker 3VA2 IEC frame 400 breaking capacity class C Icu=110kA @ 415V 3-pole, line protection ETU320, LI, In=400A overload protection Ir=160A...400A short-circuit protection Ii=1.5...10 x In nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz",1543.06,"ΤΕΜ",1,"EP",1,"3VA23407HL320JA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2340-7KP42-0AA0","circuit breaker 3VA2 IEC frame 400 breaking capacity class C Icu=110kA @ 415V 4-pole, line protection ETU850, LSI, In=400A overload protection Ir=160A...400A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection adjustable (OFF, up to 100%) nut keeper kit",2580.19,"ΤΕΜ",1,"EP",1,"3VA23407KP420AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2340-8JP32-0AA0","circuit breaker 3VA2 IEC frame 400 breaking capacity class L Icu=150kA @ 415V 3-pole, line protection ETU550, LSI, In=400A overload protection Ir=160A...400A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection optionally with external current transformer, up to 160% nut keeper kit",2150.16,"ΤΕΜ",1,"EP",1,"3VA23408JP320AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2440-5MN32-0AA0","circuit breaker 3VA2 IEC frame 630 breaking capacity class M Icu=55kA @ 415V 3-pole, motor protection ETU350M, LSI, In=400A overload protection Ir=160A...400A short-circuit protection Isd=3...15 x Ir, Ii=15 x In nut keeper kit",1827.64,"ΤΕΜ",1,"EP",1,"3VA24405MN320AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2440-5MN32-0HA0","circuit breaker 3VA2 IEC frame 630 breaking capacity class M Icu=55kA @ 415V 3-pole, motor protection ETU350M, LSI, In=400A overload protection Ir=160A...400A short-circuit protection Isd=3...15 x Ir, Ii=15 x In nut keeper kit shunt trip (STL) 12-30V DC, 24V AC 50/60Hz",1909.85,"ΤΕΜ",1,"EP",1,"3VA24405MN320HA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2440-6HN32-0CL0","circuit breaker 3VA2 IEC frame 630 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU350, LSI, In=400A overload protection Ir=160A...400A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",2143.84,"ΤΕΜ",1,"EP",1,"3VA24406HN320CL0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2440-7HL32-0CH0","circuit breaker 3VA2 IEC frame 630 breaking capacity class C Icu=110kA @ 415V 3-pole, line protection ETU320, LI, In=400A overload protection Ir=160A...400A short-circuit protection Ii=1.5...12 x In nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",2162.81,"ΤΕΜ",1,"EP",1,"3VA24407HL320CH0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2440-7MS32-0KH0","circuit breaker 3VA2 IEC frame 630 breaking capacity class C Icu=110kA @ 415V 3-pole, starter protection ETU310M, I, In=400A without overload protection short-circuit protection Ii=3...15 x In nut keeper kit shunt trip left 208-277V AC 50/60Hz 2 auxiliary switches 1 trip alarm switch",1745.42,"ΤΕΜ",1,"EP",1,"3VA24407MS320KH0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2450-5MN32-0AD0","circuit breaker 3VA2 IEC frame 630 breaking capacity class M Icu=55kA @ 415V 3-pole, motor protection ETU350M, LSI, In=500A overload protection Ir=200A...500A short-circuit protection Isd=3...15 x Ir, Ii=15 x In nut keeper kit 3 auxiliary switches HQ",2150.16,"ΤΕΜ",1,"EP",1,"3VA24505MN320AD0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2450-6JQ32-0AA0","circuit breaker 3VA2 IEC frame 630 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU560, LSIG, In=500A overload protection Ir=200A...500A short-circuit protection Isd=0.6..10x In, Ii=1.5..14x In N conductor protection optionally with external current transformer, up to 160% gr.-fault prot., can be sw. off Ig=0.2...1 x In, tg=0.05-0.8s nut keeper kit",2535.92,"ΤΕΜ",1,"EP",1,"3VA24506JQ320AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2463-0KP42-0AA0","circuit breaker 3VA2 IEC frame 630 breaking capacity class E Icu=200 kA @ 415 V 4-pole, line protection ETU850, LSI, In=630A overload protection Ir=250A ... 630A short circuit protection Isd=0,6...9xIn, Ii=1,5...9xIn neutral protection adjustable(OFF up to 100%) busbar connection",3952.5,"ΤΕΜ",1,"EP",1,"3VA24630KP420AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2463-5HL32-0KJ0","circuit breaker 3VA2 IEC frame 630 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU320, LI, In=630A overload protection Ir=250A...630A short-circuit protection Ii=1.5...9x In nut keeper kit circuit breaker 3VA2 IEC frame 630 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU320, LI, In=630A overload protection Ir=250A...630A short-circuit protection Ii=1.5...9x In nut SHUNT TRIP LEFT 208-277 V AC 50/60 HZ 220-250 V DC ACCESSORY 2 AUXILIARY SWITCH CHANGEOVER H 1 TRIP ALARM SWITCH CHANGEOVER",1814.99,"ΤΕΜ",1,"EP",1,"3VA24635HL320KJ0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2463-5JP32-0BA0","circuit breaker 3VA2 IEC frame 630 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU550, LSI, In=630A overload protection Ir=250A...630A short-circuit protection Isd=0.6..9 x In, Ii=1.5..9 x In N conductor protection optionally with external current transformer, up to 160% nut keeper kit undervoltage release (UVR) 24V DC",2200.75,"ΤΕΜ",1,"EP",1,"3VA24635JP320BA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2463-5JQ32-0KA0","circuit breaker 3VA2 IEC frame 630 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU560, LSIG, In=630A overload protection Ir=250A...630A short-circuit protection Isd=0.6..9 x In, Ii=1.5..9 x In N conductor protection optionally with external current transformer, up to 160% gr.-fault prot., can be sw. off Ig=0.2...1 x In, tg=0.05-0.8s nut keeper kit shunt trip (STL) 220-250V DC; 208-277V AC",2396.8000000000002,"ΤΕΜ",1,"EP",1,"3VA24635JQ320KA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2463-6HL32-0AG0","circuit breaker 3VA2 IEC frame 630 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU320, LI, In=630A overload protection Ir=250A...630A short-circuit protection Ii=1.5...9 x In nut keeper kit 1 auxiliary switch HP 1 trip alarm switch HP",1916.17,"ΤΕΜ",1,"EP",1,"3VA24636HL320AG0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2463-6HL32-0JC0","circuit breaker 3VA2 IEC frame 630 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU320, LI, In=630A overload protection Ir=250A...630A short-circuit protection Ii=1.5...9 x In nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ",1979.41,"ΤΕΜ",1,"EP",1,"3VA24636HL320JC0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2463-6JP32-0DL0","circuit breaker 3VA2 IEC frame 630 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU550, LSI, In=630A overload protection Ir=250A...630A short-circuit protection Isd=0.6..9 x In, Ii=1.5..9 x In N conductor protection optionally with external current transformer, up to 160% nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",2523.2800000000002,"ΤΕΜ",1,"EP",1,"3VA24636JP320DL0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2463-6JQ32-0JL0","circuit breaker 3VA2 IEC frame 630 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU560, LSIG, In=630A overload protection Ir=250A...630A short-circuit protection Isd=0.6..9 x In, Ii=1.5..9 x In N conductor protection, opt. w. ext. curr. transf., up to 160% gr.-fault prot., can be sw. off Ig=0.2...1 x In= tg=0.05-0.8s nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",2713,"ΤΕΜ",1,"EP",1,"3VA24636JQ320JL0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2463-7HL32-0BC0","circuit breaker 3VA2 IEC frame 630 breaking capacity class C Icu=110kA @ 415V 3-pole, line protection ETU320, LI, In=630A overload protection Ir=250A...630A short-circuit protection Ii=1.5...9 x In nut keeper kit undervoltage release (UVR) 24V DC 2 auxiliary switches HQ",2150.16,"ΤΕΜ",1,"EP",1,"3VA24637HL320BC0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2463-7HN32-0KH0","circuit breaker 3VA2 IEC frame 630 breaking capacity class C Icu=110kA @ 415V 3-pole, line protection ETU350, LSI, In=630A overload protection Ir=250A...630A short-circuit protection Isd=1.5...9 x Ir, Ii=9 x In nut keeper kit shunt trip (STL) 220-250V DC, 208-277V AC 2 auxiliary switches HQ 1 trip alarm switch HQ",2232.37,"ΤΕΜ",1,"EP",1,"3VA24637HN320KH0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2510-5HL42-0KF0","circuit breaker 3VA2 IEC frame 1000 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection ETU320, LI, In=1000A overload protection Ir=400A...1000A short-circuit protection Ii=1.5...10 x In N conductor protection adjustable (OFF, 50%, 100%) nut keeper kit circuit breaker 3VA2 IEC frame 1000 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection ETU320, LI, In=1000A overload protection Ir=400A...1000A short-circuit SHUNT TRIP LEFT 208-277 V AC 50/60 HZ 220-250 V DC ACCESSORY 1 AUXILIARY SWITCH CHANGEOVER H 1 TRIP ALARM SWITCH CHANGEOVER",4312.97,"ΤΕΜ",1,"EP",1,"3VA25105HL420KF0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2510-5HN32-0CH0","circuit breaker 3VA2 IEC frame 1000 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU350, LSI, In=1000A overload protection Ir=400A...1000A short-circuit protection Isd=1.5...10 x Ir, Ii=10 x In nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",3351.72,"ΤΕΜ",1,"EP",1,"3VA25105HN320CH0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2510-5KQ32-0CC0","circuit breaker 3VA2 IEC frame 1000 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU860, LSIG, In=1000A overload protection Ir=400A...1000A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection optionally with external current transformer, up to 160% gr.-fault prot., can be sw. off Ig=0.2...1 x In, tg=0.05-0.8s nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ",4256.05,"ΤΕΜ",1,"EP",1,"3VA25105KQ320CC0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2510-6KQ32-0DD0","circuit breaker 3VA2 IEC frame 1000 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU860, LSIG, In=1000A overload protection Ir=400A...1000A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection optionally with external current transformer, up to 160% gr.-fault prot., can be sw. off Ig=0.2...1 x In, tg=0.05-0.8s nut keeper kit circuit breaker 3VA2 IEC frame 1000 breaking capacity class H UNDERVOLTAGE RELEASE 208-230 V AC 50/60 HZ ACCESSORY FOR 3VA1 3 AUXILIARY SWITCH CHANGEOVER H",4717.7,"ΤΕΜ",1,"EP",1,"3VA25106KQ320DD0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2563-5MN32-0KA0","circuit breaker 3VA2 IEC frame 1000 breaking capacity class M Icu=55kA @ 415V 3-pole, motor protection ETU350M, LSI, In=630A overload protection Ir=250A...630A short-circuit protection Isd=3...15 x Ir, Ii=15 x In nut keeper kit shunt trip (STL) 220-250V DC, 208-277V AC",2226.0500000000002,"ΤΕΜ",1,"EP",1,"3VA25635MN320KA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2580-5HL32-0CA0","circuit breaker 3VA2 IEC frame 1000 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU320, LI, In=800A overload protection Ir=320A...800A short-circuit protection Ii=1.5...12 x In nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz",2384.15,"ΤΕΜ",1,"EP",1,"3VA25805HL320CA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2580-5HL42-0AA0","circuit breaker 3VA2 IEC frame 1000 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection ETU320, LI, In=800A overload protection Ir=320A...800A short-circuit protection Ii=1.5...12 x In N conductor protection adjustable (OFF, 50%, 100%) nut keeper kit",3029.2,"ΤΕΜ",1,"EP",1,"3VA25805HL420AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2580-5KQ32-0AJ0","circuit breaker 3VA2 IEC frame 1000 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU860, LSIG, In=800A overload protection Ir=320A...800A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% gr.-fault prot., can be sw. off Ig=0.2...1 x In, tg=0.05-0.8s nut keeper kit 2 auxiliary switches HP 1 trip alarm switch HP",3351.72,"ΤΕΜ",1,"EP",1,"3VA25805KQ320AJ0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2580-5KQ32-0JL0","circuit breaker 3VA2 IEC frame 1000 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU860, LSIG, In=800A overload protection Ir=320A...800A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection, opt. w. ext. curr. transf., up to 160% gr.-fault prot., can be sw. off Ig=0.2...1 x In= tg=0.05-0.8s nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",3433.93,"ΤΕΜ",1,"EP",1,"3VA25805KQ320JL0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2580-7HN32-0AG0","circuit breaker 3VA2 IEC frame 1000 breaking capacity class C Icu=110kA @ 415V 3-pole, line protection ETU350, LSI, In=800A overload protection Ir=320A...800A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In nut keeper kit circuit breaker 3VA2 IEC frame 1000 breaking capacity class C Icu=110kA @ 415V 3-pole, line protection ETU350, LSI, In=800A overload protection Ir=320A...800A short-circuit protection Isd=1.5...10 x Ir, 1 AUXILIARY SWITCH CHANGEOVER H 1 TRIP ALARM SWITCH CHANGEOVER",2972.28,"ΤΕΜ",1,"EP",1,"3VA25807HN320AG0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2612-5HN32-0AB0","circuit breaker 3VA2 IEC frame 1250 breaking capacity class  M Icu=55kA @ 415 V 3-pole, line protection ETU350,  LSI, In=1250A overload protection Ir=500A ...1250A short circuit protection Isd=1,5... 10 X Ir, Ii=10 x In nut keeper kit circuit breaker 3VA2 IEC frame 1250 breaking capacity class  M Icu=55kA @ 415 V 3-pole, line protection ETU350,  LSI, In=1250A overload protection Ir=500A ...1250A short circuit protection Isd=1,5... 10 X Ir, 2 AUXILIARY SWITCH CHANGEOVER H",3819.7,"ΤΕΜ",1,"EP",1,"3VA26125HN320AB0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA4111-5ED34-0AA0","circuit breaker 3VA4 UL frame 125 breaking capacity class M 35kA @ 480 V 3-pole, line protection TM210,  FTFM, In=110A overload protection Ir=110A fixed short-circuit protection Ii=10 x In clamp connection",561.76,"ΤΕΜ",1,"EP",1,"3VA41115ED340AA0","3VA4 Διακόπτες ισχύος κλειστού τύπου UL"]
["3VA4112-6ED54-0AA0","circuit breaker 3VA4 UL frame 125 breaking capacity class H 65kA @ 277 V 1-pole, line protection TM210,  FTFM, In=125A overload protection Ir=125A fixed short-circuit protection Ii=10 x In clamp connection",623.87,"ΤΕΜ",1,"EP",1,"3VA41126ED540AA0","3VA4 Διακόπτες ισχύος κλειστού τύπου UL"]
["3VA4120-6ED14-0AA0","circuit breaker 3VA4 UL frame 125 breaking capacity class H 65kA @ 277 V 1-pole, line protection TM210,  FTFM, In=20A overload protection Ir=20A fixed short-circuit protection Ii=15 x In clamp connection",196.52,"ΤΕΜ",1,"EP",1,"3VA41206ED140AA0","3VA4 Διακόπτες ισχύος κλειστού τύπου UL"]
["3VA4135-4ED24-3AA0","circuit breaker 3VA4 UL frame 125 breaking capacity class S 25kA @ 480 V 2-pole, line protection TM210, FTFM, In=35A overload protection Ir=35A fixed short circuit protection Ii=10 x In",290.14999999999998,"ΤΕΜ",1,"EP",18,"3VA41354ED243AA0","3VA4 Διακόπτες ισχύος κλειστού τύπου UL"]
["3VA4145-5ED34-3AA0","circuit breaker 3VA4 UL frame 125 breaking capacity class M 35kA @ 480 V 3-pole, line protection TM210, FTFM, In=45A overload protection Ir=45A fixed short circuit protection Ii=10 x In",346.7,"ΤΕΜ",1,"EP",12,"3VA41455ED343AA0","3VA4 Διακόπτες ισχύος κλειστού τύπου UL"]
["3VA4160-4ED14-3AA0","circuit breaker 3VA4 UL frame 125 breaking capacity class S 25kA @ 277 V 1-pole, line protection TM210, FTFM, In=60A overload protection Ir=60A fixed short circuit protection Ii=10 x In",160.37,"ΤΕΜ",1,"EP",36,"3VA41604ED143AA0","3VA4 Διακόπτες ισχύος κλειστού τύπου UL"]
["3VA4170-5ED24-3AA0","circuit breaker 3VA4 UL frame 125 breaking capacity class M 35kA @ 480 V 2-pole, line protection TM210, FTFM, In=70A overload protection Ir=70A fixed short circuit protection Ii=10 x In",353.19,"ΤΕΜ",1,"EP",18,"3VA41705ED243AA0","3VA4 Διακόπτες ισχύος κλειστού τύπου UL"]
["3VA4195-4ED14-0AA0","circuit breaker 3VA4 UL frame 125 breaking capacity class S 25kA @ 277 V 1-pole, line protection TM210,  FTFM, In=15A overload protection Ir=15A fixed short-circuit protection Ii=20 x In clamp connection",160.37,"ΤΕΜ",1,"EP",1,"3VA41954ED140AA0","3VA4 Διακόπτες ισχύος κλειστού τύπου UL"]
["3VA4195-6ED14-1AA0","circuit breaker 3VA4 UL frame 125 breaking capacity class H 65kA @ 277 V 1-pole, line protection TM210,  FTFM, In=15A overload protection Ir=15A fixed short-circuit protection Ii=20 x In UL489 SB (naval), 50 deg. cel. clamp connection",214.14,"ΤΕΜ",1,"EP",1,"3VA41956ED141AA0","3VA4 Διακόπτες ισχύος κλειστού τύπου UL"]
["3VA5110-4GF41-0AA0","circuit breaker 3VA5 UL frame 125 breaking capacity class S 25kA @ 480V 4-pole, line protection TM240, ATAM, In=100A overload protection Ir=80A...100A short-circuit protection Ii=5...10 x In N conductor protection 100% without connection",567.32000000000005,"ΤΕΜ",1,"EP",1,"3VA51104GF410AA0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5111-6GC41-0AA0","circuit breaker 3VA5 UL frame 125 breaking capacity class H 65kA @ 480V 4-pole, line protection TM230, FTAM, In=110A overload protection Ir=110A fixed short-circuit protection Ii=5...10 x In N conductor protection 100% without connection",816.69,"ΤΕΜ",1,"EP",1,"3VA51116GC410AA0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5120-6ED31-0AB0","circuit breaker 3VA5 UL frame 125 breaking capacity class H 65kA @ 480V 3-pole, line protection TM210, FTFM, In=20A overload protection Ir=20A fixed short-circuit protection Ii=15 x In without connection circuit breaker 3VA5 UL frame 125 breaking capacity class H 65kA @ 480V 3-pole, line protection TM210, FTFM, In=20A overload protection Ir=20A fixed short-circuit protection Ii=15 x In without connection",380.07,"ΤΕΜ",1,"EP",1,"3VA51206ED310AB0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5130-4EC41-0AA0","circuit breaker 3VA5 UL frame 125 breaking capacity class S 25kA @ 480V 4-pole, line protection TM230, FTAM, In=30A overload protection Ir=30A fixed short-circuit protection Ii=5...10 x In N conductor unprotected without connection",412.52,"ΤΕΜ",1,"EP",1,"3VA51304EC410AA0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5140-4ED21-1AA0","circuit breaker 3VA5 UL frame 125 breaking capacity class S 25kA @ 480V 2-pole, line protection TM210, FTFM, In=40A overload protection Ir=40A fixed short-circuit protection Ii=10 x In UL 489 SB (naval), 50Β° C without connection",309.62,"ΤΕΜ",1,"EP",1,"3VA51404ED211AA0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5145-5EC31-1AA0","circuit breaker 3VA5 UL frame 125 breaking capacity class M 35kA @ 480 V 3-pole, line protection TM230, FTAM, In=45A overload protection Ir=45A fixed short-circuit protection Ii=5...10 x In UL 489 SB (naval), 50Β° C without connection",372.65,"ΤΕΜ",1,"EP",1,"3VA51455EC311AA0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5150-4EC31-0AA0","circuit breaker 3VA5 UL frame 125 breaking capacity class S 25kA @ 480V 3-pole, line protection TM230, FTAM, In=50A overload protection Ir=50A fixed short-circuit protection Ii=5...10 x In without connection",317.02999999999997,"ΤΕΜ",1,"EP",1,"3VA51504EC310AA0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5170-4ED11-0AA0","circuit breaker 3VA5 UL frame 125 breaking capacity class S 25kA @ 277V 1-pole, line protection TM210, FTFM, In=70A overload protection Ir=70A fixed short-circuit protection Ii=10 x In without connection",176.13,"ΤΕΜ",1,"EP",1,"3VA51704ED110AA0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5170-6EF41-0AA0","circuit breaker 3VA5 UL frame 125 breaking capacity class H 65kA @ 480V 4-pole, line protection TM240, ATAM, In=70A overload protection Ir=56A...70A short-circuit protection Ii=5...10 x In N conductor unprotected without connection",591.42999999999995,"ΤΕΜ",1,"EP",1,"3VA51706EF410AA0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5190-6ED21-1AA0","circuit breaker 3VA5 UL frame 125 breaking capacity class H 65kA @ 480V 2-pole, line protection TM210, FTFM, In=90A overload protection Ir=90A fixed short-circuit protection Ii=10 x In UL 489 SB (naval), 50Β° C without connection",408.81,"ΤΕΜ",1,"EP",1,"3VA51906ED211AA0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5195-4EF31-0AA0","circuit breaker 3VA5 UL frame 125 breaking capacity class S 25kA @ 480V 3-pole, line protection TM240, ATAM, In=15A overload protection Ir=12A...15A short-circuit protection Ii=10β€¦20 x In without connection",339.28,"ΤΕΜ",1,"EP",1,"3VA51954EF310AA0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5211-7ED31-0AA0","circuit breaker 3VA5 UL frame 250 breaking capacity class C 100kA @ 480V 3-pole, line protection TM210, FTFM, In=110A overload protection Ir=110A fixed short-circuit protection Ii=10 x In without connection",1186.56,"ΤΕΜ",1,"EP",1,"3VA52117ED310AA0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5212-6ED31-1AA0","circuit breaker 3VA5 UL frame 250 breaking capacity class H 65kA @ 480V 3-pole, line protection TM210, FTFM, In=125A overload protection Ir=125A fixed short-circuit protection Ii=10 x In UL 489 SB (naval), 50Β° C without connection",1093.8599999999999,"ΤΕΜ",1,"EP",1,"3VA52126ED311AA0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5215-5ED61-0AA0","circuit breaker 3VA5 UL frame 250 breaking capacity class M 35kA @ 480 V 2-pole, line protection TM210, FTFM, In=150A overload protection Ir=150A fixed short-circuit protection Ii=10 x In without connection",973.35,"ΤΕΜ",1,"EP",1,"3VA52155ED610AA0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5220-0MH31-0AA0","circuit breaker 3VA5 UL frame 250 3-pole, starter protection TM120M, AM, In=200A without overload protection short-circuit protection Ii=6...12 x In without connection",1325.61,"ΤΕΜ",1,"EP",1,"3VA52200MH310AA0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5222-7ED61-0AA0","circuit breaker 3VA5 UL frame 250 breaking capacity class C 100kA @ 480V 2-pole, line protection TM210, FTFM, In=225A overload protection Ir=225A fixed short-circuit protection Ii=10 x In without connection",1418.31,"ΤΕΜ",1,"EP",1,"3VA52227ED610AA0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5225-6ED61-0AA0","circuit breaker 3VA5 UL frame 250 breaking capacity class H 65kA @ 480V 2-pole, line protection TM210, FTFM, In=250A overload protection Ir=250A fixed short-circuit protection Ii=10 x In without connection",1279.26,"ΤΕΜ",1,"EP",1,"3VA52256ED610AA0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5240-5ED31-1AA0","Circuit breaker 3VA5 UL Frame 250 Breaking capacity class M 35kA @ 480 V 3-pole, line protection TM210, FTFM, In=40A Overload protection Ir=40A fixed Short-circuit protection Ii=10 x In UL489 SB (naval), 50 deg. Cel Without connection",748.09,"ΤΕΜ",1,"EP",1,"3VA52405ED311AA0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5280-5ED41-0AA0","circuit breaker 3VA5 UL frame 250 breaking capacity class M 35kA @ 480V 4-pole, line protection TM210, FTFM, In=80A overload protection Ir=80A fixed short-circuit protection Ii=10 x In N conductor unprotected without connection",1019.7,"ΤΕΜ",1,"EP",1,"3VA52805ED410AA0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5290-6EC31-0AA0","circuit breaker 3VA5 UL frame 250 breaking capacity class H 65kA @ 480V 3-pole, line protection TM230, FTAM, In=90A overload protection Ir=90A fixed short-circuit protection Ii=5...10 x In without connection",917.73,"ΤΕΜ",1,"EP",1,"3VA52906EC310AA0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5325-5EC61-0AA0","CIRCUIT BREAKER 3VA5 UL Frame 400 BREAKING CAPACITY CLASS  M 35kA @ 480 V 2POLE, LINE PROTECTION TM230,  FTAM, In=250A WITHOUT OVERLOAD PROTECTION IR=250A FIXED SHORT CIRCUIT PROTECTION Ii=5...10 x In W/O CONNECTION",1316.34,"ΤΕΜ",1,"EP",1,"3VA53255EC610AA0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5330-7EC41-0AA0","CIRCUIT BREAKER 3VA5 UL FRAME 400 BREAKING CAPACITY CLASS  C 100kA @ 480 V 4POLE, LINE PROTECTION TM230,  FTAM, In=300A OVERLOAD PROTECTION IR=300A FIXED SHORT CIRCUIT PROTECTION II=5...10 X IN NEUTRAL UNPROTECTED W/O CONNECTION",2781,"ΤΕΜ",1,"EP",1,"3VA53307EC410AA0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5445-5GC41-0AA0","CIRCUIT BREAKER 3VA5 UL Frame 600 BREAKING CAPACITY CLASS  M 35kA @ 480 V 4POLE, LINE PROTECTION TM230,  FTAM, In=450A WITHOUT OVERLOAD PROTECTION IR=450A FIXED SHORT CIRCUIT PROTECTION Ii=5...10 x In NEUTRAL PROTECTION 100% W/O CONNECTION",2975.67,"ΤΕΜ",1,"EP",1,"3VA54455GC410AA0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5450-1MU31-0AA0","CIRCUIT BREAKER 3VA5 UL Frame 600 3POLE,MOTOR STARTER PROTECTION TM120M,  AM, In=500A WITHOUT OVERLOAD PROTECTION SHORT CIRCUIT PROTECTION Ii=3...6 x In W/O CONNECTION",2753.19,"ΤΕΜ",1,"EP",1,"3VA54501MU310AA0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5460-6EC41-0AA0","CIRCUIT BREAKER 3VA5 UL Frame 600 BREAKING CAPACITY CLASS  H 65kA @ 480 V 4POLE, LINE PROTECTION TM230,  FTAM, In=600A WITHOUT OVERLOAD PROTECTION IR=600A FIXED SHORT CIRCUIT PROTECTION Ii=4...8x In NEUTRAL UNPROTECTED W/O CONNECTION",3689.46,"ΤΕΜ",1,"EP",1,"3VA54606EC410AA0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5570-7EC36-0AA0","circuit breaker 3VA5 UL frame 800 breaking capacity class  C 100kA @ 480 V 3-pole, line protection TM230,  FTAM, In=700A overload protection Ir=700A fixed short circuit protection Ii=5...10 x In",4106.6099999999997,"ΤΕΜ",1,"EP",1,"3VA55707EC360AA0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5580-7EC36-1AA0","circuit breaker 3VA5 UL frame 800 breaking capacity class  C 100kA @ 480 V 3-pole, line protection TM230,  FTAM, In=800A overload protection Ir=800A fixed short circuit protection Ii=5...10 x In",4857.4799999999996,"ΤΕΜ",1,"EP",1,"3VA55807EC361AA0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA6110-6JP31-0AA0","circuit breaker 3VA6 UL frame 150 breaking capacity class H 65kA @ 480V 3-pole, line protection ETU550, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% without connection",1632.83,"ΤΕΜ",1,"EP",1,"3VA61106JP310AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6110-7KT41-2AA0","circuit breaker 3VA6 UL frame 150 breaking capacity class C 100kA @ 480V 4-pole, line protection ETU856, LSI, In=100A overload protection, 100% rated Ir=40A...100A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection adjustable (OFF, up to 150%) ground-fault alarm message via EFB300 or COM without connection",2758.28,"ΤΕΜ",1,"EP",1,"3VA61107KT412AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6110-8KQ31-2AA0","circuit breaker 3VA6 UL frame 150 breaking capacity class L 150kA @ 480V 3-pole, line protection ETU860, LSIG, In=100A overload protection, 100% rated Ir=40A...100A short-circuit protection Isd=0.6..10x In,Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% ground-faultprotection Ig=0.2...1 x In,tg=0.05-0.8s without connection",2573.7800000000002,"ΤΕΜ",1,"EP",1,"3VA61108KQ312AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6115-5HM41-2AA0","circuit breaker 3VA6 UL frame 150 breaking capacity class M 35kA @ 480V 4-pole, line protection ETU330, LIG, In=150A overload protection, 100% rated Ir=60A...150A short-circuit protection Ii=1.5...10 x In N conductor protection adjustable (OFF, 100%) ground-fault protection Ig=0.2...1 x In=tg=0.1/0.3s without connection",2112.5300000000002,"ΤΕΜ",1,"EP",1,"3VA61155HM412AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6115-6KQ31-2AA0","circuit breaker 3VA6 UL frame 150 breaking capacity class H 65kA @ 480V 3-pole, line protection ETU860, LSIG, In=150A overload protection, 100% rated Ir=60A...150A short-circuit protection Isd=0.6..10x In,Ii=1.5..10x In N conductor protection optionally with external current transformer, up to 160% ground-faultprotection Ig=0.2...1 x In,tg=0.05-0.8s without connection",2905.88,"ΤΕΜ",1,"EP",1,"3VA61156KQ312AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6115-7KP41-2AA0","circuit breaker 3VA6 UL frame 150 breaking capacity class C 100kA @ 480V 4-pole, line protection ETU850, LSI, In=150A overload protection, 100% rated Ir=60A...150A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection adjustable (OFF, up to 100%) without connection",3237.98,"ΤΕΜ",1,"EP",1,"3VA61157KP412AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6140-5JQ41-0AA0","circuit breaker 3VA6 UL frame 150 breaking capacity class M 35kA @ 480V 4-pole, line protection ETU560, LSIG, In=40A overload protection Ir=16A...40A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection adjustable (OFF, up to 160%) ground-fault protection Ig=0.375...1 x In= tg=0.05-0.8s without connection",2066.4,"ΤΕΜ",1,"EP",1,"3VA61405JQ410AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6140-6JQ31-2AA0","circuit breaker 3VA6 UL frame 150 breaking capacity class H 65kA @ 480V 3-pole, line protection ETU560, LSIG, In=40A overload protection, 100% rated Ir=16A...40A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% ground-fault protection Ig=0.375...1 x In, tg=0.05-0.8s without connection",2140.1999999999998,"ΤΕΜ",1,"EP",1,"3VA61406JQ312AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6140-7HM41-2AA0","circuit breaker 3VA6 UL frame 150 breaking capacity class C 100kA @ 480V 4-pole, line protection ETU330, LIG, In=40A overload protection, 100% rated Ir=16A...40A short-circuit protection Ii=1.5...12 x In N conductor protection adjustable (OFF, 100%) ground-fault protection Ig=0.375...1 x In= tg=0.1/0.3s without connection",1651.28,"ΤΕΜ",1,"EP",1,"3VA61407HM412AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6140-8JT41-2AA0","circuit breaker 3VA6 UL frame 150 breaking capacity class L 150kA @ 480V 4-pole, line protection ETU556, LSI, In=40A overload protection, 100% rated Ir=16A...40A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection adjustable (OFF, up to 160%) ground-fault alarm message via EFB300 or COM without connection",2619.9,"ΤΕΜ",1,"EP",1,"3VA61408JT412AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6210-5HM41-2AA0","circuit breaker 3VA6 UL frame 250 breaking capacity class M 35kA @ 480V 4-pole, line protection ETU330, LIG, In=100A overload protection, 100% rated Ir=40A...100A short-circuit protection Ii=1.5...12 x In N conductor protection adjustable (OFF, 50%, 100%) ground-fault protection Ig=0.2...1 x In= tg=0.1/0.3s without connection",2693.7,"ΤΕΜ",1,"EP",1,"3VA62105HM412AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6210-6KQ31-0AA0","circuit breaker 3VA6 UL frame 250 breaking capacity class H 65kA @ 480V 3-pole, line protection ETU860, LSIG, In=100A overload protection Ir=40A...100A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% ground-fault protection Ig=0.2...1 x In, tg=0.05-0.8s without connection",3099.6,"ΤΕΜ",1,"EP",1,"3VA62106KQ310AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6210-7KP41-2AA0","circuit breaker 3VA6 UL frame 250 breaking capacity class C 100kA @ 480V 4-pole, line protection ETU850, LSI, In=100A overload protection, 100% rated Ir=40A...100A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection adjustable (OFF, up to 160%) without connection",3948.3,"ΤΕΜ",1,"EP",1,"3VA62107KP412AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6225-5HM31-0AA0","circuit breaker 3VA6 UL frame 250 breaking capacity class M 35kA @ 480V 3-pole, line protection ETU330, LIG, In=250A overload protection Ir=100A...250A short-circuit protection Ii=1.5...10 x In ground-fault protection Ig=0.2...1 x In, tg=0.1/0.3s without connection",1964.93,"ΤΕΜ",1,"EP",1,"3VA62255HM310AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6225-6HM31-2AA0","circuit breaker 3VA6 UL frame 250 breaking capacity class H 65kA @ 480V 3-pole, line protection ETU330, LIG, In=250A overload protection, 100% rated Ir=100A...250A short-circuit protection Ii=1.5...10 x In ground-fault protection Ig=0.2...1 x In, tg=0.1/0.3s without connection",2398.5,"ΤΕΜ",1,"EP",1,"3VA62256HM312AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6225-7JT41-2AA0","circuit breaker 3VA6 UL frame 250 breaking capacity class C 100kA @ 480V 4-pole, line protection ETU556, LSI, In=250A overload protection, 100% rated Ir=100A...250A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection adjustable (OFF, up to 100%) ground-fault alarm message via EFB300 or COM without connection",4031.33,"ΤΕΜ",1,"EP",1,"3VA62257JT412AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6225-8HL31-0AA0","circuit breaker 3VA6 UL frame 250 breaking capacity class L 150kA @ 480V 3-pole, line protection ETU320, LI, In=250A overload protection Ir=100A...250A short-circuit protection Ii=1.5...10 x In without connection",2186.33,"ΤΕΜ",1,"EP",1,"3VA62258HL310AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6325-5JQ41-0AA0","circuit breaker 3VA6 UL frame 400 breaking capacity class M 35kA @ 480V 4-pole, line protection ETU560, LSIG, In=250A overload protection Ir=100A...250A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection adjustable (OFF, up to 160%) ground-fault protection Ig=0.2...1 x In= tg=0.05-0.8s without connection",3865.28,"ΤΕΜ",1,"EP",1,"3VA63255JQ410AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6325-6JQ31-2AA0","circuit breaker 3VA6 UL frame 400 breaking capacity class H 65kA @ 480V 3-pole, line protection ETU560, LSIG, In=250A overload protection, 100% rated Ir=100A...250A short-circuit protection Isd=0.6..10x In,Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% ground-faultprotection Ig=0.2...1 x In,tg=0.05-0.8s without connection",3865.28,"ΤΕΜ",1,"EP",1,"3VA63256JQ312AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6325-7JQ31-2AA0","circuit breaker 3VA6 UL frame 400 breaking capacity class C 100kA @ 480V 3-pole, line protection ETU560, LSIG, In=250A overload protection, 100% rated Ir=100A...250A short-circuit protection Isd=0.6..10x In,Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% ground-faultprotection Ig=0.2...1 x In,tg=0.05-0.8s without connection",4068.23,"ΤΕΜ",1,"EP",1,"3VA63257JQ312AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6340-0HL41-0AA0","circuit breaker 3VA6 UL frame 400 breaking capacity class  E 200 kA @ 480 V 4-pole, line protection ETU320,  LI, In=400A overload protection Ir=160A ... 400A short circuit protection Ii=1,5...12 x In neutral protection adjustable(OFF; 50%; 100%) w/o connection",4160.4799999999996,"ΤΕΜ",1,"EP",1,"3VA63400HL410AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6340-5JQ31-0AA0","circuit breaker 3VA6 UL frame 400 breaking capacity class M 35kA @ 480V 3-pole, line protection ETU560, LSIG, In=400A overload protection Ir=160A...400A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection optionally with external current transformer, up to 160% ground-fault protection Ig=0.2...1 x In, tg=0.05-0.8s without connection",3237.98,"ΤΕΜ",1,"EP",1,"3VA63405JQ310AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6340-8JT41-0AA0","circuit breaker 3VA6 UL frame 400 breaking capacity class L 150kA @ 480V 4-pole, line protection ETU556, LSI, In=400A overload protection Ir=160A...400A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection adjustable (OFF, up to 100%) ground-fault alarm message via EFB300 or COM without connection",4621.7299999999996,"ΤΕΜ",1,"EP",1,"3VA63408JT410AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6440-5KL41-0AA0","circuit breaker 3VA6 UL frame 600 breaking capacity class M 35kA @ 480V 4-pole, line protection ETU820, LI, In=400A overload protection Ir=160A...400A short-circuit protection Ii=1.5...12 x In without connection",4649.3999999999996,"ΤΕΜ",1,"EP",1,"3VA64405KL410AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6440-7JP31-0AA0","circuit breaker 3VA6 UL frame 600 breaking capacity class C 100kA @ 480V 3-pole, line protection ETU550, LSI, In=400A overload protection Ir=160A...400A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% without connection",4243.5,"ΤΕΜ",1,"EP",1,"3VA64407JP310AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6440-8JQ31-2AA0","circuit breaker 3VA6 UL frame 600 breaking capacity class L 150kA @ 480V 3-pole, line protection ETU560, LSIG, In=400A overload protection, 100% rated Ir=160A...400A short-circuit protection Isd=0.6..10x In,Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% ground-faultprotection Ig=0.2...1 x In,tg=0.05-0.8s without connection",5682.6,"ΤΕΜ",1,"EP",1,"3VA64408JQ312AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6460-6HM41-0AA0","circuit breaker 3VA6 UL frame 600 breaking capacity class H 65kA @ 480V 4-pole, line protection ETU330, LIG, In=600A overload protection Ir=240A...600A short-circuit protection Ii=1.5...9 x In N conductor protection adjustable (OFF, 50%, 100%) ground-fault protection Ig=0.2...1 x In= tg=0.1/0.3s without connection",4603.28,"ΤΕΜ",1,"EP",1,"3VA64606HM410AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6460-7HL31-0AA0","circuit breaker 3VA6 UL frame 600 breaking capacity class C 100kA @ 480V 3-pole, line protection ETU320, LI, In=600A overload protection Ir=240A...600A short-circuit protection Ii=1.5...9 x In without connection",3431.7,"ΤΕΜ",1,"EP",1,"3VA64607HL310AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6560-5KL36-2AA0","circuit breaker 3VA6 UL frame 800 breaking capacity class  M 35kA @ 480 V 3-pole, line protection ETU820, LI, In=600A overload protection, 100% rated Ir=240A...600A short circuit protection Ii=1,5...10 x In",5258.25,"ΤΕΜ",1,"EP",1,"3VA65605KL362AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6560-6HL32-0AA0","circuit breaker 3VA6 UL frame 800 breaking capacity class  H 65kA @ 480 V 3-pole, line protection ETU320,  LI, In=600A overload protection Ir=240A ...600A short circuit protection Ii=1,5...12 x In",3468.6,"ΤΕΜ",1,"EP",1,"3VA65606HL320AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6560-7HL36-2AA0","circuit breaker 3VA6 UL frame 800 breaking capacity class  C 100kA @ 480 V 3-pole, line protection ETU320, LI, In=600A overload protection, 100% rated Ir=240A...600A short circuit protection Ii=1,5...12 x In",4372.6499999999996,"ΤΕΜ",1,"EP",1,"3VA65607HL362AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6560-7KT42-0AA0","circuit breaker 3VA6 UL frame 800 breaking capacity class  C 100kA @ 480 V 4-pole, line protection ETU856,  LSI, In=600A overload protection Ir=240A ...600A short circuit protection Isd=0,6..12x In, Ii=1,5..12x In",6706.58,"ΤΕΜ",1,"EP",1,"3VA65607KT420AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6580-5JT46-0AA0","circuit breaker 3VA6 UL frame 800 breaking capacity class  M 35kA @ 480 V 4-pole, line protection ETU556,  LSI, In=800A overload protection Ir=320A ...800A short circuit protection Isd=0,6..10x In, Ii=1,5..10x In",7988.85,"ΤΕΜ",1,"EP",1,"3VA65805JT460AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6580-6HN32-2AA0","circuit breaker 3VA6 UL frame 800 breaking capacity class  H 65kA @ 480 V 3-pole, line protection ETU350, LSI, In=800A overload protection, 100% rated Ir=320A...800A short circuit protection Isd=1,5... 10 x Ir, Ii=10 x In",5175.2299999999996,"ΤΕΜ",1,"EP",1,"3VA65806HN322AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6580-6JQ46-0AA0","circuit breaker 3VA6 UL frame 800 breaking capacity class  H 65kA @ 480 V 4-pole, line protection ETU560,  LSIG, In=800A overload protection Ir=320A ...800A short circuit protection Isd=0,6..10x In, Ii=1,5..10x In",9215.7800000000007,"ΤΕΜ",1,"EP",1,"3VA65806JQ460AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6580-7JT32-2AA0","circuit breaker 3VA6 UL frame 800 breaking capacity class  C 100kA @ 480 V 3-pole, line protection ETU556, LSI, In=800A overload protection, 100% rated Ir=320A...800A short circuit protection",7564.5,"ΤΕΜ",1,"EP",1,"3VA65807JT322AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6610-5KL42-0AA0","circuit breaker 3VA6 UL frame 1000 breaking capacity class  M 35kA @ 480 V 4-pole, line protection ETU820,  LI, In=1000A overload protection Ir=400A ...1000A short circuit protection Ii=1,5...10 x In",8874.4500000000007,"ΤΕΜ",1,"EP",1,"3VA66105KL420AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6610-7HN36-0AA0","circuit breaker 3VA6 UL frame 1000 breaking capacity class  C 100kA @ 480 V 3-pole, line protection ETU350,  LSI, In=1000A overload protection Ir=400A ...1000A short circuit protection Isd=1,5... 10 xIr, Ii=12 x In",7444.58,"ΤΕΜ",1,"EP",1,"3VA66107HN360AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6610-7KQ42-0AA0","circuit breaker 3VA6 UL frame 1000 breaking capacity class  C 100kA @ 480 V 4-pole, line protection ETU860,  LSIG, In=1000A overload protection Ir=400A ...1000A short circuit protection Isd=0,6..10x In, Ii=1,5..10x In",10885.5,"ΤΕΜ",1,"EP",1,"3VA66107KQ420AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA9114-0SS10","mounting screw kit consists of 4 screws and nuts, metric thread M4 x 70mm accessory for: circuit breaker, 4-pole 3VA10/11 and for plugin units 3VA1 250, drawout units 3VA1 250,",18.079999999999998,"ΤΕΜ",1,"EP",1,"3VA91140SS10","3VA9 εξαρτήματα για 3VA διακόπτες"]
["3VA9131-0QF10","rear connection stud round short 1 unit accessory for: 3VA4/5 125",17.93,"ΤΕΜ",1,"EP",1,"3VA91310QF10","3VA9 εξαρτήματα για 3VA διακόπτες"]
["3VA9134-0JG10","wire connector with control wire tap 4 units accessory for: 3VA5 125",29.61,"ΤΕΜ",1,"EP",1,"3VA91340JG10","3VA9 εξαρτήματα για 3VA διακόπτες"]
["3VA9138-0VF30","sliding bar accessory for: 3VA5 125",176.05,"ΤΕΜ",1,"EP",1,"3VA91380VF30","3VA9 εξαρτήματα για 3VA διακόπτες"]
["3VA9163-0SB10","cover frame 104.6x 70.7mm (WxH) accessory for: circuit breaker 3-pole without ETU access 3VA2 100/160/250",27.22,"ΤΕΜ",1,"EP",1,"3VA91630SB10","3VA9 εξαρτήματα για 3VA διακόπτες"]
["3VA9211-0WD30","terminal cover 3-pole 1 unit accessory for: 3VA1 250",16.47,"ΤΕΜ",1,"EP",1,"3VA92110WD30","3VA9 εξαρτήματα για 3VA διακόπτες"]
["3VA9213-0QE00","rear connection stud flat 3 units accessory for: 3VA1 250",54.22,"ΤΕΜ",1,"EP",1,"3VA92130QE00","3VA9 εξαρτήματα για 3VA διακόπτες"]
["3VA9237-0VF10","module for Bowden cable sliding bar accessory for: 3VA5 250",73.7,"ΤΕΜ",1,"EP",1,"3VA92370VF10","3VA9 εξαρτήματα για 3VA διακόπτες"]
["3VA9243-0QA00","nut keeper kit 3 units accessory for: 3VA6 150/250",27.61,"ΤΕΜ",1,"EP",1,"3VA92430QA00","3VA9 εξαρτήματα για 3VA διακόπτες"]
["3VA9257-0KP81","autotrip plunger accessory for: plug-in unit 3VA1 250",34.9,"ΤΕΜ",1,"EP",1,"3VA92570KP81","3VA9 εξαρτήματα για 3VA διακόπτες"]
["3VA9267-0GK00","rotary operator with shaft stub for 8UC retrofit accessory for: 3VA2 100/160/250",45.8,"ΤΕΜ",1,"EP",1,"3VA92670GK00","3VA9 εξαρτήματα για 3VA διακόπτες"]
["3VA9277-0VF40","door interlock for side wall mount. rot. operators for the UL market accessory for: 3VA5 250 3VA6 150/250",840.28,"ΤΕΜ",1,"EP",1,"3VA92770VF40","3VA9 εξαρτήματα για 3VA διακόπτες"]
["3VA9307-0NA10","external current transformer for N conductor accessory for: 3VA2 In=400/500/630A",409.28,"ΤΕΜ",1,"EP",1,"3VA93070NA10","3VA9 εξαρτήματα για 3VA διακόπτες"]
["3VA9404-0QA00","nut keeper kit 4 units accessory for: 3VA1 400/630 3VA2 400/630",57.2,"ΤΕΜ",1,"EP",1,"3VA94040QA00","3VA9 εξαρτήματα για 3VA διακόπτες"]
["3VA9447-0EK11","FRONT MOUNTED ROTARY OPERATOR STANDARD IEC IP30/40 ACCESSORY FOR: 3VA5/6 400/600",94.43,"ΤΕΜ",1,"EP",1,"3VA94470EK11","3VA9 εξαρτήματα για 3VA διακόπτες"]
["3VA9467-0HA22","motor operator 230 V AC optimized for long cables accessory for: 3VA1 400/630 3VA2 400/630",699.45,"ΤΕΜ",1,"EP",1,"3VA94670HA22","3VA9 εξαρτήματα για 3VA διακόπτες"]
["3VA9481-0WJ40","insulating plate extended 4-pole 1 unit accessory for: 3VA1 400/630 3VA2 400/630",23.68,"ΤΕΜ",1,"EP",1,"3VA94810WJ40","3VA9 εξαρτήματα για 3VA διακόπτες"]
["3VA9603-0KB00","Position signaling switch accessory for: plug-in unit 3VA9603-0KP00",48.04,"ΤΕΜ",1,"EP",1,"3VA96030KB00","3VA9 εξαρτήματα για 3VA διακόπτες"]
["3VA9674-0JB32","wire connector for 3 cables; 4 pcs. accessory for: 3VA55/3VA65/3VA66",339.31,"ΤΕΜ",1,"EP",1,"3VA96740JB32","3VA9 εξαρτήματα για 3VA διακόπτες"]
["3VA9677-0EK31","Front mounted rotary operator standard IP30 with door interlocking and door open function accessory for: 3VA55/3VA65/3VA66",344.91,"ΤΕΜ",1,"EP",1,"3VA96770EK31","3VA9 εξαρτήματα για 3VA διακόπτες"]
["3VA9978-0AA21","leading changeover switch changeover contacts type HP (14mm) accessory for: 3VA4/5/6",61.29,"ΤΕΜ",1,"EP",1,"3VA99780AA21","3VA9 εξαρτήματα για 3VA διακόπτες"]
["3VA9980-0LF30","adapter cylinder lock accessory for: SEO motor operator",62.26,"ΤΕΜ",1,"EP",1,"3VA99800LF30","3VA9 εξαρτήματα για 3VA διακόπτες"]
["3VW8112-0BA01","guide frame for 3WL10 - 4p rear vertical main circ. conn. equiv. to withdr. circ. breaker without frame accessory for circuit breaker 3WL10",2157.9899999999998,"ΤΕΜ",1,"EP",1,"3VW81120BA01","3VW εξαρτήματα για 3WL10/3VA27 διακόπτες"]
["3VW9011-0AE12","time-delay device (adjustable) for undervoltage release UVR 110/127V AC/DC standard rail mounting accessory for circuit breaker 3WL10 / 3VA27",483.5,"ΤΕΜ",1,"EP",1,"3VW90110AE12","3VW εξαρτήματα για 3WL10/3VA27 διακόπτες"]
["3VW9011-0AT43","Adapter 3VA for TD400",223.48,"ΤΕΜ",1,"EP",1,"3VW90110AT43","3VW εξαρτήματα για 3WL10/3VA27 διακόπτες"]
["3VW9011-0BB18","locking mech to prevent opening in the cabinet door in ON pos. Bowden cable, withdr. circ. br. accessory for circuit breaker 3WL10 / 3VA27",418.85,"ΤΕΜ",1,"EP",1,"3VW90110BB18","3VW εξαρτήματα για 3WL10/3VA27 διακόπτες"]
["3WA9111-0AD22","Accessory 3WA/3WL Shunt trip (ST) 5% OP, 24-30 V DC momentary duty, with cut-off switch, not for continuous duty",258.37,"ΤΕΜ",1,"EP",1,"3WA91110AD22","3WA9 εξαρτήματα για 3WA διακόπτες"]
["3WA9111-0AH11","Accessory Circuit breaker 3WA, Position signalling switch module 3x connected, 2x test, 1x disconnected",425.69,"ΤΕΜ",1,"EP",1,"3WA91110AH11","3WA9 εξαρτήματα για 3WA διακόπτες"]
["3WA9111-0AP07","Accessory Circuit breaker 3WA, Shutter, frame size 3, 3 poles Only for repair. Shutter is included generally in every guide frame.",582.38,"ΤΕΜ",1,"EP",1,"3WA91110AP07","3WA9 εξαρτήματα για 3WA διακόπτες"]
["3WA9111-0AX21","Accessory Circuit breaker 3WA, Rear horizontal main- connection, top or bottom, frame size 2 - up to 2000 A not for breaking capacity C for withdrawable design, 1 piece",47.12,"ΤΕΜ",1,"EP",1,"3WA91110AX21","3WA9 εξαρτήματα για 3WA διακόπτες"]
["3WA9111-0BA71","Accessory Circuit breaker 3WA, Locking provision for Padlock device for charging handle padlocks are not included Spare parts for Z-Option S33",171.77,"ΤΕΜ",1,"EP",1,"3WA91110BA71","3WA9 εξαρτήματα για 3WA διακόπτες"]
["3WA9111-0EK62","Accessory circuit breaker 3WA, Voltage tap Retrofit Kit: V-tap for upper stab contact only for 3WA with breaking capacity N, S, M, H, C, not fΓΌr E, Set for 4-poles Circuit breaker, Frame size 2",358.62,"ΤΕΜ",1,"EP",1,"3WA91110EK62","3WA9 εξαρτήματα για 3WA διακόπτες"]
["3WA9111-0EX20","Accessory circuit breaker 3WA, Option Plug  LSIG GFx  2000 A Basic protective function LT, ST, INST and GF, Rated current 2000 A (Ground fault protection with extended setting range)",858.89,"ΤΕΜ",1,"EP",1,"3WA91110EX20","3WA9 εξαρτήματα για 3WA διακόπτες"]
["3WL9111-0AL11-0AA0","accessories circuit breaker 3WL maine conductor conn. 1 piece fixed-mounted circ.br. size II front conn. top dual hole front accessible up to2000A",111.62,"ΤΕΜ",1,"EP",1,"3WL91110AL110AA0","3WL9 εξαρτήματα για 3WL διακόπτες"]
["3WL9111-0AN27-0AA0","accessories circuit breaker 3WL maine conductor conn. 1 piece withdraw. circ. breaker sz ii connection flange, up to 2500A",131.69,"ΤΕΜ",1,"EP",1,"3WL91110AN270AA0","3WL9 εξαρτήματα για 3WL διακόπτες"]
["3WL9111-0AT66-0AA0","access. f. 3WL air circ. br., COM35 communication module PROFINET IO and Modbus TCP BSS and cable set as retrofit kit",2079.77,"ΤΕΜ",1,"EP",1,"3WL91110AT660AA0","3WL9 εξαρτήματα για 3WL διακόπτες"]
["3WL9111-0BA85-0AA0","accessories circuit breaker 3WL locking device against traversing of circ. breaker In sep. position (cable pULl a. lock In cabinet door) make: profalux",891.33,"ΤΕΜ",1,"EP",1,"3WL91110BA850AA0","3WL9 εξαρτήματα για 3WL διακόπτες"]
["3WL9111-1AT16-0AA0","3WL9 NAFTA accessory WLBSS BSS (breaker status sensor)",5413.18,"ΤΕΜ",1,"EP",1,"3WL91111AT160AA0","3WL9 εξαρτήματα για 3WL διακόπτες"]
["3WL9111-2AA61-0AA0","accessories circuit breaker 3WL rated current ref. module 1600A f. ETU25, 27, 45, 55, 75, 76 approved to UL 489",462.85,"ΤΕΜ",1,"EP",1,"3WL91112AA610AA0","3WL9 εξαρτήματα για 3WL διακόπτες"]
["3ZS1316-4CC10-0YA5","SIRIUS engineering Safety ES V1.0 Basic License key on USB flash drive Software on CD Floating License for one user Engineering software Class A 3 languages (de,en,fr) Executable in: Windows 10 64 bit Pro/Enterprise Windows 7 32/64 bit SP 1 Prof./Ultimate/Enterprise Reference HW: SIRIUS MSS 3RK3 SIRIUS 3SK2 Communications via system interface to PC (serial interface) Content: Set (1xDVD + 1x USB)",188.99,"ΤΕΜ",1,"EP",1,"3ZS13164CC100YA5","3ZS λογισμικα"]
["3ZS2718-2CC00-0YH0","power management software SENTRON powermanager option pack Distributed Systems (5) license on USB flash drive 2 languages (D/E)",4816.68,"ΤΕΜ",1,"EP",1,"3ZS27182CC000YH0","3ZS λογισμικα"]
["4AC3763-0","Safety transformer, 63VA Primary 230 V AC, 50Hz, secondary 2x12 V/24 V AC With PTC fuse, 5 MW++",160.43,"ΤΕΜ",1,"EP",1,"4AC37630","4AC Μετασχηματιστές ράγας"]
["4AM3442-8DD40-0FA0","TRANSFORMER SITAS; PHASES:1; PN/PN(S6)(KVA):0,1 /0,31; UPRI(V):550-525-500-480-460- 440-415-400-380-230-208; USEC(V):2X115; ISEC(A):0,435-0,87; F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0 /0; TA/ISOKL:40 /B; IP00; TYPE OF TERMINALS:SCREW/TAB CONNECTION; INSTALLATION:SCREWS/MOUNTING RAILS; EN 61558-2-1, -2-2, -2-4 >UL/CSA-RECOGNIZED< >CONTROL CIRCUIT TRANSFORMER< >ISOLATION TRANSFORMER<",266.39,"ΤΕΜ",1,"EP",1,"4AM34428DD400FA0","4AM  Μετασχηματιστές τάσης 1φασικοί"]
["4AM3842-8MD40-0FA0","TRANSFORMER SITAS; PHASES:1; PN/PN(S6)(KVA):0,16 /0,49; UPRI(V):440-400-230; USEC(V):230(2X115); ISEC(A):0,70-1,39; F(HZ):50...60; VECTOR GR./SHIELD WNG.:IIII0 /0; TA/ISOKL:40 /B; IP00; TYPE OF TERMINALS:SCREW/TAB CONNECTION; INSTALLATION:SCREWS/MOUNTING RAILS; EN 61558-2-1, -2-2, -2-4 >UL/CSA-RECOGNIZED< >CONTROL CIRCUIT TRANSFORMER< >ISOLATION TRANSFORMER<",264.54000000000002,"ΤΕΜ",1,"EP",1,"4AM38428MD400FA0","4AM  Μετασχηματιστές τάσης 1φασικοί"]
["4AM4642-8DD40-0FC0","TRANSFORMER SITAS; PHASES:1; PN/PN(S6)(KVA):0,34 /1,44; UPRI(V):550-525-500-480-460- 440-415-400-380-230-208; USEC(V):2X115; ISEC(A):2X1,48; F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0 /0; TA/ISOKL:40 /B; IP23; TYPE OF TERMINALS:SCREW/TAB CONNECTION; INSTALLATION:SCREW; EN 61558-2-1, -2-2, -2-4 >UL/CSA-RECOGNIZED< >CONTROL CIRCUIT TRANSFORMER< >ISOLATION TRANSFORMER<",775.11,"ΤΕΜ",1,"EP",1,"4AM46428DD400FC0","4AM  Μετασχηματιστές τάσης 1φασικοί"]
["4AM4842-5AT10-0FA1","TRANSFORMER SITAS; PHASES:1; PN/PN(S6)(KVA):0,5/2 UPRI(V):400+/-5%; USEC(V):230; ISEC(A):2,17; F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0 /0; TA/ISOKL:40 /B; IP00; TYPE OF TERMINALS:CAGE-CLAMP; INSTALLATION:SCREW; EN 61558-2-1, -2-2, -2-4 >UL/CSA-RECOGNIZED<(><<)> >CONT CIRCUIT TRANSFORMER<(><<)> >ISOLATION TRANSFORMER<(><<)>",464.32,"ΤΕΜ",1,"EP",1,"4AM48425AT100FA1","4AM  Μετασχηματιστές τάσης 1φασικοί"]
["4AM5742-4TV00-0EA0","TRANSFORMER SITAS; PHASES:1; PN/PN(S6)(KVA):1 /5; UPRI(V):230+/-5%; USEC(V):42; ISEC(A):23,8; F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0 /0; TA/ISOKL:40 /B; IP00; TYPE OF TERMINALS:SCREW/TAB CONNECTION; INSTALLATION:SCREW; EN 61558-2-2, -2-6 >UL/CSA-RECOGNIZED< >CONTROL CIRCUIT TRANSFORMER< >SAFETY ISOLATING TRANSFORMER<",756.62,"ΤΕΜ",1,"EP",1,"4AM57424TV000EA0","4AM  Μετασχηματιστές τάσης 1φασικοί"]
["4AM6142-5FT10-0FC0","TRANSFORMER SITAS; PHASES:1; PN/PN(S6)(KVA):1,36 /7,3; UPRI(V):500+/-5%; USEC(V):230; ISEC(A):5,91; F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0 /0; TA/ISOKL:40 /B; IP23; TYPE OF TERMINALS:SCREW/TAB CONNECTION; INSTALLATION:SCREW; EN 61558-2-1, -2-2, -2-4 >UL/CSA-RECOGNIZED< >CONTROL CIRCUIT TRANSFORMER< >ISOLATION TRANSFORMER<",1478.09,"ΤΕΜ",1,"EP",1,"4AM61425FT100FC0","4AM  Μετασχηματιστές τάσης 1φασικοί"]
["4AM6442-8JD40-0FA0","SITAS transformer; phases: 1; PN/PN(S6)(KVA):2 / 9.7; UPRI(V): 400-230+/-15; Usec(V):2x115; Isec(A):2x8.7; F(HZ):50...60; Vector gr./shield wng.:II0 /0; TA/ISO Cl:40 /B; IP00; Connection: screw/tab connection; mounting: screws; EN 61558-2-1, -2-2, -2-4 >UL/CSA-recognized< >Control transformer< >Isolating transformer<",1376.33,"ΤΕΜ",1,"EP",1,"4AM64428JD400FA0","4AM  Μετασχηματιστές τάσης 1φασικοί"]
["4AT3932-8ED40-0FA0","TRANSFORMER SITAS; PHASES:1; PN/PN(S6)(KVA):10 /36,4; UPRI(V):600-575-550-525-500- 480-460-440-415-400-240-230; USEC(V):2X115; ISEC(A):2X43,5; F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0 /0; TA/ISOKL:55 /H; IP00; TYPE OF TERMINALS:SCREW CONNECTION; INSTALLATION:SCREW; EN 61558-2-1, -2-2, -2-4 >UL/CSA-RECOGNIZED< >CONTROL CIRCUIT TRANSFORMER< >ISOLATION TRANSFORMER<",5401.76,"ΤΕΜ",1,"EP",1,"4AT39328ED400FA0","4AT  Μετασχηματιστές τάσης 1φασικοί"]
["4AV2200-2EB00-0A","POWER SUPPLY; PHASES:1; PN(KW):0,12; UPRI(V):400-230+/-15; USEC(V DC):24; ISEC(A DC):5/6 (60/40 CEL); F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0 /0; PROTECTION CL.:I; TA/ISOKL:60 /B; W(%):5; IP00; TYPE OF TERMINALS:SCREW/TAB CONNECTION; INSTALLATION:SCREW; EN 61558-2-6, EN61131-2 >SAFETY ISOLATING TRANSFORMER<",644.30999999999995,"ΤΕΜ",1,"EP",1,"4AV22002EB000A","4AV Τροφοδοτικά"]
["4EP3700-2US00","MAINS CHOKE F.FU; PHASES:3; UN1(V):480; ITHMAX 1(A) / F1(HZ):35,5 /60; I LN (A):31,95; UK(%):2; LN(MH):0,397; TA/ISOKL:40 /B; IP00; TYPE OF TERMINALS:SCREW CONNECTION; EN 61558-2-20 >UL/CSA-RECOGNIZED< >CHOKE<",1241.56,"ΤΕΜ",1,"EP",1,"4EP37002US00","4EP CHOKE"]
["4EU3022-2BA00-0AA0","COMMUTATING CHOKE FOR CONVERTER; PHASES:3; UN1(V):400; ITHMAX 1(A) / F1(HZ):400 /50; I LN (A):360; UK(%):4; LN(MH):0,056; TA/ISOKL:40 /H; IP00; TYPE OF TERMINALS:FLAT-TYPE TERMINAL; EN 61558-2-20 >UL/CSA-RECOGNIZED< >CHOKE<",8516.4599999999991,"ΤΕΜ",1,"EP",1,"4EU30222BA000AA0","4EU CHOKE"]
["4NC5431-0CH21","current transformer 800/1 A, 10 VA CL 1.0",123.91,"ΤΕΜ",1,"EP",1,"4NC54310CH21","4NC Μετασχηματιστές έντασης"]
["5SB4311","D-Fuse DIII 63A gG 500V a.c./44 SENTRON fuse-link DIAZED size DIII In 63A gG Un 500V a.c./440V d.c.",3.48,"ΤΕΜ",1,"EP",25,"5SB4311","5SB Ασφάλειες DIAZED"]
["5SD8006","DIAZED fuse link 690 V for cable and line protection Operating class gG Size DIII, E33, 6A",17.88,"ΤΕΜ",1,"EP",5,"5SD8006","5SD Ασφάλειες DIAZED"]
["5SE2310","NEOZED fuse-link, D01, 10 A, gG, Un AC: 400 V, Un DC: 250 V, with tin-coated contact-caps",0.69,"ΤΕΜ",1,"EP",10,"5SE2310","5SE Ασφάλειες NEOZED"]
["5SG7113","MINIZED, Switch disconnector with Fuse, D02, 1-pole, In: 63 A, Un AC: 230 V",36.46,"ΤΕΜ",1,"EP",1,"5SG7113","5SG Ασφαλειοδιακόπτες MINIZED"]
["5SH5327","infeed terminals insulated for 1.5 mm2 to 25 mm2 in pin designs",3.48,"ΤΕΜ",1,"EP",10,"5SH5327","5SH εξαρτήματα ασφαλειών"]
["5SJ4113-8HG40","Miniature circuit breaker 240 V 14kA, 1-pole, D, 13 A, D=70 mm according to UL 489, equal polarity",45.08,"ΤΕΜ",1,"EP",1,"5SJ41138HG40","5SJ Μικροαυτόματοι διακόπτες κατά UL489"]
["5SJ4132-7HG40","Miniature circuit breaker 240 V 14kA, 1-pole, C, 32 A, D=70 mm according to UL 489, equal polarity",47.13,"ΤΕΜ",1,"EP",1,"5SJ41327HG40","5SJ Μικροαυτόματοι διακόπτες κατά UL489"]
["5SJ4210-7HG41","Miniature circuit breaker 240 V 14kA, 2-pole, C, 10A, D=70 mm according to UL 489",130.41,"ΤΕΜ",1,"EP",1,"5SJ42107HG41","5SJ Μικροαυτόματοι διακόπτες κατά UL489"]
["5SJ4232-8HG42","Circuit breaker 10kA, 2-pole, D, 32A according to UL 489-480Y/277V",178.85,"ΤΕΜ",1,"EP",1,"5SJ42328HG42","5SJ Μικροαυτόματοι διακόπτες κατά UL489"]
["5SJ4302-8HG41","Miniature circuit breaker 240 V 14kA, 3-pole, D, 2A, D=70 mm according to UL 489",260.82,"ΤΕΜ",1,"EP",1,"5SJ43028HG41","5SJ Μικροαυτόματοι διακόπτες κατά UL489"]
["5SJ4350-8HG41","Miniature circuit breaker 240 V 10kA, 3-pole, D, 50 A, D=70 mm according to UL 489",388.44,"ΤΕΜ",1,"EP",1,"5SJ43508HG41","5SJ Μικροαυτόματοι διακόπτες κατά UL489"]
["5SL3006-7","CIRCUIT BREAKER 230V 4.5KA, 1+N-POLE/1MW C6",15.66,"ΤΕΜ",1,"EP",1,"5SL30067","5SL30 Μικροαυτόματοι διακόπτες 1P+N 1 στοιχείου 4,5kA"]
["5SL4108-6","Miniature circuit breaker 230/400 V 10kA, 1-pole, B, 8A",14.42,"ΤΕΜ",1,"EP",1,"5SL41086","5SL4 Μικροαυτόματοι διακόπτες 10kA"]
["5SL4125-8","Miniature circuit breaker 230/400 V 10kA, 1-pole, D, 25A",12.44,"ΤΕΜ",1,"EP",1,"5SL41258","5SL4 Μικροαυτόματοι διακόπτες 10kA"]
["5SL4320-6","Miniature circuit breaker 400 V 10kA, 3-pole, B, 20 A",53.99,"ΤΕΜ",1,"EP",1,"5SL43206","5SL4 Μικροαυτόματοι διακόπτες 10kA"]
["5SL4402-6","Miniature circuit breaker 400 V 10kA, 4-pole, B, 2A",90.64,"ΤΕΜ",1,"EP",1,"5SL44026","5SL4 Μικροαυτόματοι διακόπτες 10kA"]
["5SL4450-7","Miniature circuit breaker 400 V 10kA, 4-pole, C, 50 A",112.2,"ΤΕΜ",1,"EP",1,"5SL44507","5SL4 Μικροαυτόματοι διακόπτες 10kA"]
["5SL4625-7","Miniature circuit breaker 400 V 10kA, 3+N-pole, C, 25A",59.16,"ΤΕΜ",1,"EP",1,"5SL46257","5SL4 Μικροαυτόματοι διακόπτες 10kA"]
["5SL6025-6MC","Miniature Circuit Breaker Measuring, Communication AC 230V 6kA, 1+N pole, B, 25A Please consider Radio approval! List of countries: see Certificates",229.79,"ΤΕΜ",1,"EP",1,"5SL60256MC","5SL60 Μικροαυτόματοι διακόπτες 1P+N 1 στοιχείου 6kA COM"]
["5SL6201-7","Miniature circuit breaker 400 V 6kA, 2-pole, C, 1 A",19.38,"ΤΕΜ",1,"EP",1,"5SL62017","5SL6 Μικροαυτόματοι διακόπτες 6kA"]
["5SL6232-7","Miniature circuit breaker 400 V 6kA, 2-pole, C, 32 A",18.36,"ΤΕΜ",1,"EP",1,"5SL62327","5SL6 Μικροαυτόματοι διακόπτες 6kA"]
["5SL6606-7","Miniature circuit breaker 400 V 6kA, 3+N-pole, C, 6A",33.659999999999997,"ΤΕΜ",1,"EP",1,"5SL66067","5SL6 Μικροαυτόματοι διακόπτες 6kA"]
["5SL6663-7","Miniature circuit breaker 400 V 6kA, 3+N-pole, C, 63 A",60.18,"ΤΕΜ",1,"EP",1,"5SL66637","5SL6 Μικροαυτόματοι διακόπτες 6kA"]
["5SM2626-2","RC unit for 5SL4, 2-pole, typeΒ AC, selective, In: 63 A, 300 mA, Un AC: 230 V",185.64,"ΤΕΜ",1,"EP",1,"5SM26262","RC μονάδα διαρροής ρεύματος για 5SL4"]
["5SM6011-1XX02","Arc fault detection device block AFDD, 1-16 A 230 V 1 MW with miniature circuit breaker 1+N 6 kA, B 10 A 1 MW",467.82,"ΤΕΜ",1,"EP",1,"5SM60111XX02","5SM Στοιχεία AFDD"]
["5SP4391-7","Miniature circuit breaker 400 V 10kA, 3-pole, C, 100 A, D=70 mm",117.3,"ΤΕΜ",1,"EP",1,"5SP43917","5SP4 Μικροαυτόματη ασφάλεια 10kA - UL1077"]
["5ST1143","standard mounting rail, 35x 27x 7.3x 1.0 mm 2000 mm long, not perforated galvanized",6.16,"ΤΕΜ",1,"EP",20,"5ST1143","Εξαρτήματα για υλικό ράγας"]
["5ST2528","Connecting cable with connector 6 mm2, 220 mm long Insulation blue",3.45,"ΤΕΜ",1,"EP",10,"5ST2528","Εξαρτήματα για υλικό ράγας"]
["5ST3644","Pin busbar, 16 mm2 connection: 3x 3-phase touch-safe",7.12,"ΤΕΜ",1,"EP",10,"5ST3644","5ST3 μπάρες για υλικό ράγας"]
["5ST3657","Pin busbar, 16 mm2 Range with: 20x 5ST3643+10x 5ST3644+ 50x 5ST3645+10x 5ST3655",584.64,"ΣΕΤ",1,"EP",1,"5ST3657","5ST3 μπάρες για υλικό ράγας"]
["5ST3734","Pin busbar touch-safe, 10 mm2 2-phase, 214 mm long can be cut, with end caps",9,"ΤΕΜ",1,"EP",1,"5ST3734","5ST3 μπάρες για υλικό ράγας"]
["5ST3782-1","Series connector, 1-pole 150mm, 16 mm2, blue 750V, 80 A",5.1100000000000003,"ΤΕΜ",1,"EP",10,"5ST37821","5ST3 μπάρες για υλικό ράγας"]
["5SU1154-6KK06","RCBO, 10 kA, 1P+N, type A, 10 mA, B char., In: 6 A, Un AC: 230 V",134.13999999999999,"ΤΕΜ",1,"EP",1,"5SU11546KK06","5SU RCBO 10kA"]
["5SU1324-6FP10","RCBO, 10 kA, 2P Type A, 30 mA, B-Char, In: 10A Un: 230V",147.80000000000001,"ΤΕΜ",1,"EP",1,"5SU13246FP10","5SU RCBO 10kA"]
["5SU1336-6FP13","RCBO, 6 kA, 3P Type A, 30 mA, B-Char, In: 13A Un: 400V",181.33,"ΤΕΜ",1,"EP",1,"5SU13366FP13","5SU RCBO 6kA"]
["5SU1353-7KK10","RCBO, 4.5 kA, 1P+N, type A, 30 mA, C-Char, In: 10 A, Un AC: 230 V",95,"ΤΕΜ",1,"EP",1,"5SU13537KK10","5SU RCBO 4,5kA"]
["5SU1354-7KK06","RCBO, 10 kA, 1P+N, type A, 30 mA, C-Char, In: 6 A, Un AC: 230 V",130,"ΤΕΜ",1,"EP",1,"5SU13547KK06","5SU RCBO 10kA"]
["5SU1356-6KK32","RCBO, 6 kA, 1P+N, type A, 30 mA, B char., In: 32 A, Un AC: 230 V",109.39,"ΤΕΜ",1,"EP",1,"5SU13566KK32","5SU RCBO 6kA"]
["5SU1653-7KK20","RCBO, 4.5 kA, 1P+N, type A, 300 mA, C-Char, In: 20 A, Un AC: 230 V",90,"ΤΕΜ",1,"EP",1,"5SU16537KK20","5SU RCBO 4,5kA"]
["5SU1654-6KK10","RCBO, 10 kA, 1P+N, type A, 300 mA, B char., In: 10 A, Un AC: 230 V",128.54,"ΤΕΜ",1,"EP",1,"5SU16546KK10","5SU RCBO 10kA"]
["5SU9156-7VK32","RCBO, 6 kA, 1P+N, type A, short-time-delayed K, 10 mA, C-Char, In: 32 A, Un AC: 230 V",161.13999999999999,"ΤΕΜ",1,"EP",1,"5SU91567VK32","5SU RCBO 6kA Voltage Dependend - CY"]
["5SU9356-7KK25","RCBO, 6 kA, 1P+N, type A, 30 mA, C-Char, In: 25 A, Un AC: 230 V",129.56,"ΤΕΜ",1,"EP",1,"5SU93567KK25","5SU RCBO 6kA Voltage Dependend - CY"]
["5SV1316-0KK10","RCBO compact 1P+N 6 kA type AC 30 mA B10",212.38,"ΤΕΜ",1,"EP",1,"5SV13160KK10","5SV RCBO 6kA 1 στοιχείου"]
["5SV1616-7KK02","RCBO compact 1P+N 6 kA type A 300 mA C2",130,"ΤΕΜ",1,"EP",1,"5SV16167KK02","5SV RCBO 6kA 1 στοιχείου"]
["5SV3314-3","Residual current operated circuit breaker, 2-pole, type F, short-time delayed, In: 40 A, 30 mA, Un AC: 230 V",132.6,"ΤΕΜ",1,"EP",1,"5SV33143","5SV3 Ρελέ διαρροής τύπου A/F/B/B+"]
["5SV3346-4KK60","Residual current operated circuit breaker, 4-pole, Type B, In: 63A, 30mA, 6mA DC, Un AC: 400V, Mobile Installations",773.88,"ΤΕΜ",1,"EP",1,"5SV33464KK60","5SV ρελέ διαρροής 6mA DC - Νέο υλικό"]
["5SV3614-6","Residual current operated circuit breaker, 2-pole, type A, In: 40 A, 300 mA, Un AC: 230 V",78.540000000000006,"ΤΕΜ",1,"EP",1,"5SV36146","5SV3 Ρελέ διαρροής τύπου A/F/B/B+"]
["5SV3744-6","Residual current operated circuit breaker, 4-pole, type A, In: 40 A, 500 mA, Un AC: 400 V",76.5,"ΤΕΜ",1,"EP",1,"5SV37446","5SV3 Ρελέ διαρροής τύπου A/F/B/B+"]
["5SV4344-0LA01","Residual current operated circuit breaker, 4-pole, Type AC, short-time delayed, In: 40 A, 30 mA, Un AC: 400 V, with thermal overload protection",159.97,"ΤΕΜ",1,"EP",1,"5SV43440LA01","5SV4 Ρελέ διαρροής τύπου AC"]
["5SV5642-6","Residual current operated circuit breaker, 4-pole, Type A, In: 25A, 300mA, Un AC: 400V Residential",69.36,"ΤΕΜ",1,"EP",1,"5SV56426","5SV5 Ρελέ διαρροής τύπου AC / A - residential offer"]
["5SV6016-7KK40","AFDD-MCB-Combination 230V, 6kA, 1+N, C, 40A Compact (1MW)",316.02,"ΤΕΜ",1,"EP",1,"5SV60167KK40","5SV6 AFDD / Μικροαυτόματος διακόπτης 1 στοιχείου"]
["5SV8900-1KK","SENTRON, holder, for transformer mounting",7.79,"ΤΕΜ",1,"EP",2,"5SV89001KK","5SV8 Επιτηρητες διαροής προς γη"]
["5SW3006","Wall box, gray IP40, for flush mounting for built-in devices 2, 5 MW max. wide",59.62,"ΤΕΜ",1,"EP",1,"5SW3006","5SW εξαρτήματα μικροαυτομάτων"]
["5SY4106-7","Miniature circuit breaker 230/400 V 10kA, 1-pole, C, 6 A, D=70 mm",15.81,"ΤΕΜ",1,"EP",1,"5SY41067","5SY4 Μικροαυτόματοι διακόπτες 10kΑ - multistandard offer"]
["5SY4205-8","Miniature circuit breaker 400 V 10kA, 2-pole, D, 0.5 A, D=70 mm",138.62,"ΤΕΜ",1,"EP",1,"5SY42058","5SY4 Μικροαυτόματοι διακόπτες 10kΑ - multistandard offer"]
["5SY4303-8","Miniature circuit breaker 400 V 10kA, 3-pole, D, 3 A, D=70 mm",184.56,"ΤΕΜ",1,"EP",1,"5SY43038","5SY4 Μικροαυτόματοι διακόπτες 10kΑ - multistandard offer"]
["5SY4325-8","Miniature circuit breaker 400 V 10kA, 3-pole, D, 25A, D=70 mm",151.54,"ΤΕΜ",1,"EP",1,"5SY43258","5SY4 Μικροαυτόματοι διακόπτες 10kΑ - multistandard offer"]
["5SY4363-6","Miniature circuit breaker 400 V 10kA, 3-pole, B, 63A, D=70 mm",181.96,"ΤΕΜ",1,"EP",1,"5SY43636","5SY4 Μικροαυτόματοι διακόπτες 10kΑ - multistandard offer"]
["5SY4508-7","Miniature circuit breaker 230 V 10kA, 1+N-pole, C, 8A, D=70 mm",31.81,"ΤΕΜ",1,"EP",1,"5SY45087","5SY4 Μικροαυτόματοι διακόπτες 10kΑ - multistandard offer"]
["5SY4520-6","Miniature circuit breaker 230 V 10kA, 1+N-pole, B, 20 A, D=70 mm",42.18,"ΤΕΜ",1,"EP",1,"5SY45206","5SY4 Μικροαυτόματοι διακόπτες 10kΑ - multistandard offer"]
["5SY4640-6","Miniature circuit breaker 400 V 10kA, 3+N-pole, B, 40A, D=70 mm",166.17,"ΤΕΜ",1,"EP",1,"5SY46406","5SY4 Μικροαυτόματοι διακόπτες 10kΑ - multistandard offer"]
["5SY5201-7","Circuit breaker Universal current 440 V DC 400 V AC 10kA, 2-pole, C, 01A",79.56,"ΤΕΜ",1,"EP",1,"5SY52017","5SY5 Μικροαυτόματοι διακόπτες 10kA / 220-440 VDC - multistandard offer"]
["5SY6110-6","Miniature circuit breaker 230/400 V 6kA, 1-pole, B, 10A, D=70 mm",15.97,"ΤΕΜ",1,"EP",1,"5SY61106","5SY6 Μικροαυτόματοι διακόπτες 6kA - multistandard offer"]
["5SY6240-6","Miniature circuit breaker 400 V 6kA, 2-pole, B, 40A, D=70 mm",67.61,"ΤΕΜ",1,"EP",1,"5SY62406","5SY6 Μικροαυτόματοι διακόπτες 6kA - multistandard offer"]
["5SY6316-6","Miniature circuit breaker 400 V 6kA, 3-pole, B, 16A, D=70 mm",63.17,"ΤΕΜ",1,"EP",1,"5SY63166","5SY6 Μικροαυτόματοι διακόπτες 6kA - multistandard offer"]
["5SY6604-7","Miniature circuit breaker 400 V 6kA, 3+N-pole C, 4A, D=70 mm",78.59,"ΤΕΜ",1,"EP",1,"5SY66047","5SY6 Μικροαυτόματοι διακόπτες 6kA - multistandard offer"]
["5SY7113-6","Miniature circuit breaker 230/400 V 15kA, 1-pole, B, 13 A, D=70 mm",20.12,"ΤΕΜ",1,"EP",1,"5SY71136","5SY7 Μικροαυτόματοι διακόπτες 15kA - multistandard offer"]
["5SY7301-8","Miniature circuit breaker 400 V 15kA, 3-pole, D, 1 A, D=70 mm",237.78,"ΤΕΜ",1,"EP",1,"5SY73018","5SY7 Μικροαυτόματοι διακόπτες 15kA - multistandard offer"]
["5SY7325-8","Miniature circuit breaker 400 V 15kA, 3-pole, D, 25A, D=70 mm",199.61,"ΤΕΜ",1,"EP",1,"5SY73258","5SY7 Μικροαυτόματοι διακόπτες 15kA - multistandard offer"]
["5SY7516-7","Miniature circuit breaker 230 V 15kA, 1+N-pole, C, 16A, D=70 mm",46.58,"ΤΕΜ",1,"EP",1,"5SY75167","5SY7 Μικροαυτόματοι διακόπτες 15kA - multistandard offer"]
["5SY7601-8","Miniature circuit breaker 400 V 15kA, 3+N-pole, D, 1 A, D=70 mm",299.42,"ΤΕΜ",1,"EP",1,"5SY76018","5SY7 Μικροαυτόματοι διακόπτες 15kA - multistandard offer"]
["5SY7663-7","Miniature circuit breaker 400 V 15kA, 3+N-pole, C, 63 A, D=70 mm",253.58,"ΤΕΜ",1,"EP",1,"5SY76637","5SY7 Μικροαυτόματοι διακόπτες 15kA - multistandard offer"]
["5SY8240-8","Miniature circuit breaker 400 V D=70 mm 25 kA according to EN 60947-2, 2P, D40",236.8,"ΤΕΜ",1,"EP",1,"5SY82408","5SY8 Μικροαυτόματοι διακόπτες 25kA - multistandard offer"]
["5SY8415-8","Miniature circuit breaker 400 V D=70 mm 25 kA according to EN 60947-2, 4P, D1.6",378.68,"ΤΕΜ",1,"EP",1,"5SY84158","5SY8 Μικροαυτόματοι διακόπτες 25kA - multistandard offer"]
["5SY8510-7","Miniature circuit breaker 230 V D=70 mm 25 kA according to EN 60947-2, 1P+N, C10",49.27,"ΤΕΜ",1,"EP",1,"5SY85107","5SY8 Μικροαυτόματοι διακόπτες 25kA - multistandard offer"]
["5SY8603-7","Miniature circuit breaker 400 V D=70 mm 25 kA according to EN 60947-2, 3P+N, C3",155.77000000000001,"ΤΕΜ",1,"EP",1,"5SY86037","5SY8 Μικροαυτόματοι διακόπτες 25kA - multistandard offer"]
["5TC1337-0PM","DELTA style button sys Shutter Platinum metallic",82.84,"ΤΕΜ",1,"EP",1,"5TC13370PM","Διακοπτικό Υλικό"]
["5TC8906","DELTA profil, silver Cover plate for dimmer with rotary knob 65x 65 mm",36.380000000000003,"ΤΕΜ",1,"EP",1,"5TC8906","Διακοπτικό Υλικό"]
["5TE2814-0","Switch 400V 4-pole 125 A",93,"ΤΕΜ",1,"EP",1,"5TE28140","5TE Διακόπτες - μπουτόν - λυχνίες ράγας"]
["5TE5804","Indicator light 1 lamp 230 V red for long supply lines",16.27,"ΤΕΜ",1,"EP",1,"5TE5804","5TE Διακόπτες - μπουτόν - λυχνίες ράγας"]
["5TG1122-0","DELTA miro aluminum Frame 2-fold Authentic material aluminum natural Dimensions 161x 90 mm",119.8,"ΤΕΜ",1,"EP",1,"5TG11220","Διακοπτικό Υλικό"]
["5TG1202-1","DELTA miro glass Frame 2-fold Authentic material white glass 161x 90 mm",119.8,"ΤΕΜ",1,"EP",1,"5TG12021","Διακοπτικό Υλικό"]
["5TG1342-0AC","DELTA style Cover TAE Multimedia Antracite Cosso",18.11,"ΤΕΜ",1,"EP",2,"5TG13420AC","Διακοπτικό Υλικό"]
["5TG1394","DELTA style, titanium white Cover plate UAE connection socket 68x 68 mm for Rutenbeck Cat. 3+5+6 BTR-DAT C6, E-DAT/UAE design TelegΓ¤rtner AMJ45, UMJ45",12.82,"ΤΕΜ",1,"EP",1,"5TG1394","Διακοπτικό Υλικό"]
["5TG1894","DELTA profil, Label \"Heating switch\" Labeling sheet w. 5 labels",2.09,"ΤΕΜ",1,"EP",1,"5TG1894","Διακοπτικό Υλικό"]
["5TG2553-1","DELTA line, titanium white frame 3-fold, 222x 80 mm horizontal, with Labeling field",29.25,"ΤΕΜ",1,"EP",1,"5TG25531","Διακοπτικό Υλικό"]
["5TG4324","DELTA i-system Sealing set IP44 for switch and button rockers for two-circuit switch and Double pushbutton (1 set=4 individual seals)",8.82,"ΣΕΤ",1,"EP",1,"5TG4324","Διακοπτικό Υλικό"]
["5TG6221","DELTA i-system carbon metallic Rocker switch for universal switch Change/off for intermediate and OFF switch for neutral pushbutton, 55x 55 mm",11.92,"ΤΕΜ",1,"EP",1,"5TG6221","Διακοπτικό Υλικό"]
["5TG6251","DELTA i-system aluminum-metallic Rocker switch with window, with label for emergency switch for heating 55x 55 mm",11.18,"ΤΕΜ",1,"EP",1,"5TG6251","Διακοπτικό Υλικό"]
["5TG7151-1","DELTA style, Rocker switch with pull actuation for pushbutton platinum metallic, 68x 68 mm",29.92,"ΤΕΜ",1,"EP",1,"5TG71511","Διακοπτικό Υλικό"]
["5TG7935","DELTA profil, silver Rocker switch with window, with label for emergency switch for heating 65x 65 mm",24.86,"ΤΕΜ",1,"EP",1,"5TG7935","Διακοπτικό Υλικό"]
["5TG9874-1TW","DELTA m-system Modular jack socket CAT3 RJ11 6/4 with shutter titanium white",16.87,"ΤΕΜ",1,"EP",1,"5TG98741TW","Διακοπτικό Υλικό"]
["5TT3461","Fault signaling relay T5570 230 V AC 5 A Additional detector with transparent cap",270.38,"ΤΕΜ",1,"EP",1,"5TT3461","5TT Ρελέ ράγας"]
["5TT4207-2","switching relay with 2 CO contact for 230V AC 16A control 24V AC",73.77,"ΤΕΜ",1,"EP",1,"5TT42072","5TT Ρελέ ράγας"]
["5TT4425-0","Remote control switch Contact for 25 A Voltage 230 V AC 1 NO 1 NC",51.61,"ΤΕΜ",1,"EP",1,"5TT44250","5TT Ρελέ ράγας"]
["5TT4478-2","Remote control switch Contact for 63 A Voltage 24 V AC 2 change-over contacts",120.59,"ΤΕΜ",1,"EP",1,"5TT44782","5TT Ρελέ ράγας"]
["5TT5852-2","INSTA contactor with 2 NO contact and 2 NC contacts Contact for 230 V AC, 400V 63A Control 24 V AC",174.91,"ΤΕΜ",1,"EP",1,"5TT58522","5TT Ρελέ ράγας"]
["5UB1350","DELTA i-system titanium white socket outlet 16 A 250 V with grounding pin 2-pole according to CEE7 cover plate 55 x 55 mm",16.09,"ΤΕΜ",1,"EP",1,"5UB1350","Διακοπτικό Υλικό"]
["5UB1842-0AC01","DELTA style, Antracite cosso SCHUKO socket outlet 10/16 A 250 V with spring flap, increased touch protection cover plate 68 x 68 mm",49.01,"ΤΕΜ",1,"EP",1,"5UB18420AC01","Διακοπτικό Υλικό"]
["5UB1853-1","DELTA style, platinum metallic SCHUKO socket outlet 10/16 A 250 V cover plate 68 x 68 mm",26.03,"ΤΕΜ",1,"EP",1,"5UB18531","Διακοπτικό Υλικό"]
["5UH1065","DELTA style, titanium white cover plate 68 x 68 mm for SCHUKO socket outlet",8.0500000000000007,"ΤΕΜ",1,"EP",1,"5UH1065","Διακοπτικό Υλικό"]
["5UH1213","DELTA i-system electrical white Cover plate with spring flap 55x 55 mm, with label for SCHUKO socket outlet",27.89,"ΤΕΜ",1,"EP",1,"5UH1213","Διακοπτικό Υλικό"]
["6AG1124-1QC02-4AX1","SIPLUS HMI KP1500 Comfort based on 6AV2124-1QC02-0AX1 with conformal coating, 0...+50 Â°C, Comfort Panel, key operation 15\" widescreen TFT display, 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 24 MB configuration memory, WEC 2013, configurable as of WinCC Comfort V14 SP1 with HSP",6950,"ΤΕΜ",1,"SIMATIC",1,"6AG11241QC024AX1","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6AG1155-6AU02-7BN0","SIPLUS ET 200SP IM155-6PN ST based on 6ES7155-6AU02-0BN0 with conformal coating, -40...+70 Â°C interface module IM 155-6 PN ST, max. 32 I/O modules, and 16 ET 200AL modules, multi hot swap, optional PN strain relief, including server module (6AG1193-6PA00-7AA0)",594,"TEM",1,"SIMATIC",1,"6AG11556AU027BN0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6AG1221-1BF32-4XB0","SIPLUS S7-1200 SM 1221 8DI based on 6ES7221-1BF32-0XB0 with conformal coating, -20â€¦+60 Â°C, digital input 8 DI, 24 V DC, sink/source",195,"ΤΕΜ",1,"SIMATIC",1,"6AG12211BF324XB0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6AG1231-5QF32-4XB0","SIPLUS S7-1200 SM 1231 TC 8 AI based on 6ES7231-5QF32-0XB0 with conformal coating, -20â€¦+60 Â°C, analog input, SM 1231 TC 8 AI thermocouples",815,"ΤΕΜ",1,"SIMATIC",1,"6AG12315QF324XB0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6AG1500-0HP00-4AB0","SIPLUS S7-1500 CPU 1517H System Bundle based on 6ES7500-0HP00-0AB0 with conformal coating, 0â€¦+60 Â°C, system bundle consisting of: 2 x CPU 1517H-3 PN, 4 sync modules up to 10 m. 2 x sync cables 1 m without memory card",27589,"ΤΕΜ",1,"SIMATIC",1,"6AG15000HP004AB0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6AG1513-1AM03-2AB0","SIPLUS S7-1500 CPU 1513-1 PN based on 6ES7513-1AM03-0AB0 with conformal coating -40...+60 Â°C . central processing unit with work memory 600 KB for program and 2.5 MB for data, 1st interface: PROFINET IRT with 2-port switch, 25 ns bit performance, SIMATIC Memory Card required",3346,"ΤΕΜ",1,"SIMATIC",1,"6AG15131AM032AB0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6AG1620-0AA00-7AA0","SIPLUS PN/CAN link based on 6BK1620-0AA00-0AA0 with conformal coating, -40â€¦+70 Â°C, from PROFINET to CAN/CANopen networks CAN 2.0 A/B CANopen manager to CiA301/302 CANopen slave to CiA301/302 IP20",1101,"ΤΕΜ",1,"SIMATIC",1,"6AG16200AA007AA0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6AG2134-6GD01-4BA1","SIPLUS ET 200SP AI 4xI 2-/4-wire TX rail based on 6ES7134-6GD01-0BA1 with conformal coating, -40â€¦+70 Â°C, OT4 with ST1/2 (+85 Â°C for 10 minutes), analog input module, suitable for BU type A0, A1, color code CC03, module diagnostics, 16-bit, +/-0.3%",445,"ΤΕΜ",1,"SIMATIC",1,"6AG21346GD014BA1","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6AG2516-3FP03-4AB0","SIPLUS S7-1500 CPU 1516F-3 PN rail based on 6ES7516-3FP03-0AB0 with conformal coating OT4: -40...+70 Â°C ST1/2: 85 Â°C for 10 minutes . central processing unit with work memory 3 MB for program and 7.5 MB for data 1st interface: PROFINET IRT with 2-port switch, 2nd interface: PROFINET RT, 3rd interface: PROFIBUS, 6 ns bit performance, SIMATIC Memory Card required",11816,"ΤΕΜ",1,"SIMATIC",1,"6AG25163FP034AB0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6AT8000-2AB30-1AA1","SIPLUS CMS accessories \"Cable-Power-135-0000;\" \"Length=1.35 m;\" IFN power cable",65.099999999999994,"ST",1,"GMC",1,"6AT80002AB301AA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["6AU1400-1QA20-0AA0","SIMOTION drive-based 2 GB CompactFlash card D410-2; SINAMICS drive runtime software V5.x and SIMOTION Kernel for SIMOTION D410-2; current software version; note: not for SIMOTION D410, D4x5 and D4x5-2; is compatible with 1 GB CF card 6AU1400-1PA23-0AA0",508,"ΤΕΜ",1,"GMC",1,"6AU14001QA200AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6AU1810-1CA55-0XK5","SIMOTION SCOUT stand-alone V5.5 upgrade license license key download floating license for 1 user without software and documentation - - consignee email address required for delivery",995,"ΤΕΜ",1,"GMC",1,"6AU18101CA550XK5","Ρυθμιστές στροφών και συστήματα Motion control"]
["6AV2101-4BB02-3AK5","SIMATIC WinCC Comfort V19, upgrade WinCC flexible 2008 Standard-> WinCC Comfort V19 Combo; engineering software in the TIA Portal; floating license; software, documentation and license key for download; class A; 9 languages: de,en,zh included, fr,es,it,ru,ja,ko as download; for configuration of SIMATIC Panels. please observe product release: support.industry.siemens.com entry ID: 109821219 - - consignee email address required for delivery",357,"ΤΕΜ",1,"SIMATIC",1,"6AV21014BB023AK5","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6AV2103-8XA00-0AP0","EPL master for WinCC V19 Engineering (EPL=Enterprise License) mandatory royalty per 1 installation only valid in connection with Enterprise License contract",672,"ΤΕΜ",1,"SIMATIC",1,"6AV21038XA000AP0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6AV2104-3KK07-0AK0","SIMATIC WinCC Runtime Advanced 8192 or 16384 PowerTags V17, upgrade V11..V16 -> V17; runtime software in TIA Portal; single license; software, documentation and license key for download; class A; 6 languages: de,en,fr,es,it,zh; please observe product release: support.industry.siemens.com entry ID: 109795525 - - consignee email address required for delivery",2036,"ΤΕΜ",1,"SIMATIC",1,"6AV21043KK070AK0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6AV2105-2TV00-0BJ0","SIMATIC WinCC RT Professional, Powerpack 262144 PowerTags -> 500000 PowerTags /+Asia V11..V19 (without version change), runtime software in TIA Portal, single license, without software, without documentation, license key download, class A, - - consignee email address required for delivery",17141,"ΤΕΜ",1,"SIMATIC",1,"6AV21052TV000BJ0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6AV2107-0JA00-0BB0","SIMATIC WinCC Recipes for Runtime Advanced option for WinCC (TIA Portal) runtime software, single license without software, without documentation license key on USB flash drive, class A - - content: 1x USB",359,"ΤΕΜ",1,"SIMATIC",1,"6AV21070JA000BB0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6AV2108-0CH00-0BH0","SIMATIC Energy Suite S7-1500, Single Runtime License download contains license certificate for 10 energy objects (1x10 EnO) as pdf for download, class A; executable on all S7-1500 CPU (without S7-1500S) and ET 200SP CPU Firmware V2.0 or higher - - consignee email address required for delivery",509,"ΤΕΜ",1,"SIMATIC",1,"6AV21080CH000BH0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6AV2124-0MC24-1AX0","SIMATIC HMI TP1200 Comfort Pro for supporting foot (expandable, flange at bottom), Comfort Panel, touch operation, 12\" Widescreen TFT display, 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 12 MB configuration memory, WEC 2013, configurable from WinCC Comfort V14 SP1 with HSP",3452,"ΤΕΜ",1,"SIMATIC",1,"6AV21240MC241AX0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6AV2125-2AE03-0AX0","SIMATIC HMI connection box compact for Mobile Panels, installation in control cabinet, PROFINET and PROFIsafe, connection of safety relay, Connection point detection",190,"ΤΕΜ",1,"SIMATIC",1,"6AV21252AE030AX0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6AV2151-0XA02-3AA5","SIMATIC WinCC Unified V19 Basic Engineering, engineering software in the TIA Portal; floating license; with software and documentation on DVD; license key on USB flash drive; class A; 9 languages: de,en,zh included, fr,es,it,ru,ja,ko as download; please observe product release: support.industry.siemens.com entry ID: 109820987 - - content: set (3x DVD + 1x USB)",152,"ΤΕΜ",1,"SIMATIC",1,"6AV21510XA023AA5","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6AV2153-0XB00-0LR2","WinCC Unified Eng. Maint BMW EPL Maintenance PC ENGINEERING; right to upgrade to the current version BMW - - maintenance for one installation without software and without documentation; only valid in connection with enterprise license agreement; requires EPL Master. purchase via BMW - EPL contract. as download - - consignee email address required for delivery",1184,"TEM",1,"SIMATIC",1,"6AV21530XB000LR2","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6AV2154-1GB20-0AB0","SIMATIC WinCC Unified PC Runtime Powerpack PC 10k -> PC 50k PowerTags (without version change) V16..V19; runtime software in TIA Portal; single license; without software and documentation; license key on USB flash drive; class A; - - content: 1x USB",2793,"ΤΕΜ",1,"SIMATIC",1,"6AV21541GB200AB0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6AV2154-3DB00-0LR0","EPL Maintenance for SIMATIC WinCC Unified PC Runtime 150 PowerTags; only valid in connection with Enterprise License agreement, requires EPL Master - - consignee email address required for delivery",149,"ΤΕΜ",1,"SIMATIC",1,"6AV21543DB000LR0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6AV2155-3DW01-8AA0","WinCC Unified Package for SIMATIC IPC; consists of: WinCC Unified V18 PC Runtime 150 PowerTags and and parameter Ctrl. PC; WinCC Unified 100 LoggingTags; WinCC Unified 2 Operate client; supplied only if the same number of SIMATIC IPCs is ordered simultaneously. Please observe product info: support.industry.siemens.com entry ID: 99860269 - - content: 6AV2154-3DB01-8AA0; 6AV2154-0BP01-8AB0; 6AV2157-2DA00-0AB0; 2x 6AV2157-1JW00-0AB0;",5034,"ΤΕΜ",1,"SIMATIC",1,"6AV21553DW018AA0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6AV2156-0BS01-8LA0","SIMATIC WinCC Unified V18 Sequence Execution; option for WinCC Unified V18; delivery only following special sales release; engineering/runtime software; single license; software, documentation and license certificate for download; please observe product release: support.industry.siemens.com entry ID: 109807125 - - consignee email address required for delivery",2244,"ΤΕΜ",1,"SIMATIC",1,"6AV21560BS018LA0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6AV2157-3JM00-0AB0","SIMATIC WinCC Unified Client, 3 Monitor Clients, option for WinCC Unified PC, runtime software, single license without software and documentation; license key on USB flash drive; class A; - - content: 1x USB",2262,"ΤΕΜ",1,"SIMATIC",1,"6AV21573JM000AB0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6AV2185-8CE01-0AA0","Extension Unit 12\" KP12 PN for mounting on all fully IP65-enclosed 16:9 HMI/IPC devices. For the flexible installation of operator controls, 3 mounting positions, 3 operator controls equippable; Connection via PROFINET (without equipment)",989,"ΤΕΜ",1,"SIMATIC",1,"6AV21858CE010AA0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6AV6362-2BM00-0AH0","SIMATIC WinCC/WebUX Operate, 100 client licenses (countable) option for WinCC V7.3 or higher and WinCC Professional V14 or higher, runtime software, single license, license key download, at the server end Windows 64-bit is required - - consignee email address required for delivery",68661,"ΤΕΜ",1,"SIMATIC",1,"6AV63622BM000AH0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6AV6371-1DG08-0AX3","WinCC/ProAgent upgrade from V7.3/7.4 -> V8.0 for SIMATIC WinCC V8.0, runtime software on CD-ROM, single license on USB flash drive please observe product release: support.industry.siemens.com SIOS entry ID: 109816599 - - content: set (1x DVD + 1x USB)",336,"ΤΕΜ",1,"SIMATIC",1,"6AV63711DG080AX3","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6AV6371-1DV07-5BX4","WinCC/Audit RT upgrade from V7.4 -> V7.5 SP2 for WinCC/Audit RT, runtime software, single license, software and documentation on CD, license key on USB flash drive - - content: set (1x DVD + 1x USB)",161,"ΤΕΜ",1,"SIMATIC",1,"6AV63711DV075BX4","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6AV6371-1KV08-1BX3","WinCC/Audit RT upgrade from V7.4/7.5 -> V8.1, for WinCC/Audit RT, runtime software, single license, software and license key download - - consignee email address required for delivery",195,"TEM",1,"SIMATIC",1,"6AV63711KV081BX3","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6AV6371-2BN17-5AX0","WinCC Powerpack RC 8192/65536 for WinCC V7.5 SP2, runtime/configuration license without version change from 8192 to 65536 PowerTags, floating license, license key on USB flash drive - - content: 1x USB",2246,"ΤΕΜ",1,"SIMATIC",1,"6AV63712BN175AX0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6AV6372-2DF00-0FY0","SIMATIC Energy Manager PRO for systems with up to 500 tags, software update service; within the framework of this contract, you will receive for one year all up-to-date software versions; The contract is extended automatically by 1 year if not canceled 3 months prior to expiration. period of delivery and service: 1 year from date of invoice. requirement for conclusion: current version of the software - - consignee email address required for delivery",4578,"ΤΕΜ",1,"SIMATIC",1,"6AV63722DF000FY0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6AV6372-2DF07-4CH4","SIMATIC Energy Manager upgrade V7.x -> V7.4 for systems with up to 50 tags; engineering/runtime software; single license; software, documentation and license key for download; please observe product release: support.industry.siemens.com entry ID: 109815309 - - consignee email address required for delivery",3052,"ΤΕΜ",1,"SIMATIC",1,"6AV63722DF074CH4","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6AV6381-1KA00-0CX5","WinCC Software Update Service download valid for 10 licenses automatic follow-up deliveries of upgrades and service packs; within the framework of this contract, you will receive for one year all up-to-date software versions. The contract is extended automatically by 1 year if not canceled 3 months prior to expiration. period of delivery and service: 1 year from date of invoice requirement for conclusion: current version of the software - - consignee email address required for delivery",8417,"ΤΕΜ",1,"SIMATIC",1,"6AV63811KA000CX5","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6AV6381-2AB08-0AK3","SIMATIC WinCC RC software upgrade from V7.3/7.4 to V8.0 for SIMATIC WinCC Runtime & Configuration (RC) including options Redundancy, Server, User Archive, Web Navigator, Web NAV Load-Balancing, Web Diagnostics Client/Server, Data Monitor, Connectivity Pack, Connectivity Station, runtime/configuration software, single license, software and license key download - - consignee email address required for delivery",2030,"ΤΕΜ",1,"SIMATIC",1,"6AV63812AB080AK3","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6AV6381-2BJ08-1AX0","WinCC system software V8.1, RT 102400 (102400 PowerTags), runtime software, single license, software and documentation on DVD, license key on USB flash drive, class A, 5 languages (de,en,fr,es,it), please observe product release: support.industry.siemens.com SIOS entry ID: 109973487 - - content: set (2x DVD + 1x USB)",12104,"TEM",1,"SIMATIC",1,"6AV63812BJ081AX0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6AV6381-2CB07-5AH0","WinCC system software V7.5 SP2, WinCC RC Client V7.5 SP2 runtime/configuration software, floating license, software including documentation and license key download, class A, 5 languages (de,en,fr,es,it), please observe product release: support.industry.siemens.com SIOS entry ID: 109783852 - - consignee email address required for delivery",4308,"ΤΕΜ",1,"SIMATIC",1,"6AV63812CB075AH0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6AV6612-0AA00-0AM0","SIMATIC WinCC Comfort Software Update Service Compact for multiple orders on one position, these deliveries are grouped. Minimum order quantity: 3 units within the framework of this contract, you will receive for one year all up-to-date software versions. the contract is extended automatically by 1 year if it is not canceled 3 months prior to expiration. Period of delivery and service: 1 year from date of invoice Requirement for conclusion: current version of the software",213,"ΤΕΜ",1,"SIMATIC",1,"6AV66120AA000AM0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6AV6646-1BA18-0AA1","SIMATIC ITC1900 V3, industrial thin client, 19\" widescreen TFT display, capacitive touch sensor, supported protocols: RDP, VNC, SmartServer HTML5 and others standard design, built-in unit",2235,"ΤΕΜ",1,"SIMATIC",1,"6AV66461BA180AA1","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6AV6646-1BC18-0NA0","SIMATIC ITC1900 V3 PRO, Industrial Thin Client, 19\" widescreen TFT display, capacitive touch sensor Supported protocols: RDP, VNC, Smart Server, HTML5 etc. neutral design, prepared for support arm without expansion elements",2744,"ΤΕΜ",1,"SIMATIC",1,"6AV66461BC180NA0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6AV6881-0AM62-0AE0","icotek cable sleeve, 5-6 mm, color: gray, scope of supply: 5 cable sleeves",29.200000000000003,"ΤΕΜ",1,"SIMATIC",1,"6AV68810AM620AE0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6AV6881-0MJ22-0AA0","protective film 12\"; front type 5, adhesive over the entire surface, no reflection, matte, scope of supply: 5 protective films, including mounting accessories",213,"ΤΕΜ",1,"SIMATIC",1,"6AV68810MJ220AA0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6AV7674-1LA32-0AA0","Extension unit 12\" PROFINET for mounting on all fully IP65-enclosed 16:9 HMI/IPC devices. For the flexible installation of operator controls, 6 mounting positions, 6 operator controls can be equipped; Connection via PROFINET (without equipment)",583,"ΤΕΜ",1,"SIMATIC",1,"6AV76741LA320AA0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6AV7860-3EH00-0AA0","SIMATIC Flat Panel Monitor V2 Extended V2 host module, HDBaseT V2 transceiver DisplayPort,USB to HDBaseT, 24 V power supply",312,"ΤΕΜ",1,"SIMATIC",1,"6AV78603EH000AA0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6AV7863-7MA14-2NA0","SIMATIC IFP2400 V2 PRO, 24 multi-touch display (16:9) with 1920x1080 pixel resolution, PRO variant stand, for 24 V DC, DisplayPort, can be placed up to 100 m away HDBaseT, USB on the rear side, neutral design",2850,"ΤΕΜ",1,"SIMATIC",1,"6AV78637MA142NA0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6BK1000-6AE00-0AA0","SIMATIC BoxPC627E_5Slot ASM, i3, 480 GB SSD, 8 GB, ASM image ASM AS: 00118015-01",3847,"ΤΕΜ",1,"SIMATIC",1,"6BK10006AE000AA0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6DR4004-8J","Iy module plug-in module for analog current output signal for SIPART PS2 electropneumatic positioner, position feedback, signal current 4-20 mA, simple to retrofit, not explosion-proof",329,"ST",1,"PI5",1,"6DR40048J","Όργανα Μέτρησης Πεδίου"]
["6DR5010-0NG01-0AA1","SIPART PS2 Smart, electropneumatic positioner, 4...20mA, Ex/nEx, single-acting, polycarbonate enclosure, for pneumatic linear and part-turn actuators. Non-contacting (wear-free) position detection (NCS). Standard Without explosion protection. Connection thread el.: M20x1.5 / pneu.: G 1/4 Without limit monitor. Analog Output Module (AOM), analog position feedback 4 ... 20 mA. Device plug M12 optionally orderable with -Z D53. Isolating power supply SITRANS I100 separately orderable (7NG4124-1AA00). . Brief instructions English / German / Chinese. Standard / Fail-Safe - Depressurizing the actuator in case of failure of electrical auxiliary power (single acting only). Manometer block aluminum GÂ¼, single-acting with plastic manometer IP31 (MPa, bar)",1619,"ST",1,"PI5",1,"6DR50100NG010AA1","Όργανα Μέτρησης Πεδίου"]
["6DR5120-0NN00-5KA0","SIPART PS2 Smart, electropneumatic positioner, 4...20mA, HART, Ex/nEx, double-acting, polycarbonate enclosure, for pneumatic linear and part-turn actuators. Non-contacting (wear-free) position detection (NCS). Standard Without explosion protection. Connection thread el.: 1/2\" NPT / pneu.: 1/4\" NPT Without limit monitor. Without option module. . Brief instructions English / German / Chinese / Spanish. Standard / Fail-Safe - Depressurizing the actuator in case of failure of electrical auxiliary power (single acting only). Without Manometer block / Venting gauge block / Booster.",1294,"ST",1,"PI5",1,"6DR51200NN005KA0","Όργανα Μέτρησης Πεδίου"]
["6EP1332-5BA00","SITOP PSU100C 24 V/2.5 A stabilized power supply input: 120-230 V AC (110-300 V DC) output: 24 V DC/2.5 A",89.6,"ΤΕΜ",1,"SIMATIC",1,"6EP13325BA00","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6EP3332-7SB00-0AX0","SITOP PSU6200 24 V/2.5 A Stabilized power supply Input: 120 - 230 V AC, (120 - 240 V DC) Output: 24 V DC/2.5 A",90.8,"ΤΕΜ",1,"SIMATIC",1,"6EP33327SB000AX0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6EP3444-7SB00-3AX0","SITOP PSU6200 48 V/5 A Stabilized power supply Input: 400 - 500 V AC Output: 48 V DC/5 A With diagnostic interface",266,"ΤΕΜ",1,"SIMATIC",1,"6EP34447SB003AX0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6EP4136-3AC00-0AY0","SITOP UPS1600 EX 20 A uninterruptible power supply input: 24 V DC output: 24 V DC/20 A",385,"ΤΕΜ",1,"SIMATIC",1,"6EP41363AC000AY0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6ES7132-6FD00-2BB1","SIMATIC ET 200SP, digital output module, DQ 4x 24..230V AC/2A Standard Pack quantity: 10 units, suitable for BU type B1, Color code CC41, Module diagnostics",127,"ΤΕΜ",1,"SIMATIC",10,"6ES71326FD002BB1","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6ES7137-6AA01-0BA0","SIMATIC ET 200SP, CM PTP communication module for serial connection RS-422, RS-485 and RS-232, freeport, 3964 (R), USS, MODBUS RTU master, slave, max. 250 Kbit/s, suitable for BU type A0, pack quantity: 1 unit",366,"ΤΕΜ",1,"SIMATIC",1,"6ES71376AA010BA0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6ES7155-6BA01-0CN0","SIMATIC ET 200SP, PROFIBUS bundle IM, IM 155-6DP HF, max. 32 I/O modules and 16 ET 200AL modules, Multi-hotswap, bundle consists of: Interface module (6ES7155-6BU01-0CN0), Server module (6ES7193-6PA00-0AA0), PROFIBUS connector (6ES7972-0BB70-0XA0)",368,"ΤΕΜ",1,"SIMATIC",1,"6ES71556BA010CN0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6ES7193-6BP00-2DA0","SIMATIC ET 200SP, BaseUnit BU15-P16+A0+2D, BU type A0, Pack quantity: 10 units, Push-in terminals, without AUX terminals, New load group, WxH: 15x 117 mm",31.400000000000002,"ΤΕΜ",1,"SIMATIC",10,"6ES71936BP002DA0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6ES7194-2AB00-0AA0","M8 connector for ET connection, 4-pole, shielded",30.3,"ΤΕΜ",1,"SIMATIC",1,"6ES71942AB000AA0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6ES7194-2LH20-1AC0","Power cable M8, single-sided assembled with M8 socket, 4-pole, Length 2.0 m",13.5,"ΤΕΜ",1,"SIMATIC",1,"6ES71942LH201AC0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6ES7194-2MN10-0AB0","bus cable for ET connection M8, PUR cable assembled on both ends with 2x M8 connectors angled, 4-pole, shielded length 10 m",94.1,"ΤΕΜ",1,"SIMATIC",1,"6ES71942MN100AB0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6ES7195-1GG30-0XA0","SIMATIC DP, mounting rail for ET 200M, 620 mm long, for holding bus modules for removal and insertion function",126,"ΤΕΜ",1,"SIMATIC",1,"6ES71951GG300XA0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6ES7223-1BH32-0XB0","SIMATIC S7-1200, Digital I/O SM 1223, 8 DI/8 DO, 8 DI 24 V DC, Sink/Source, 8 DO, transistor 0.5 A",224,"ΤΕΜ",1,"SIMATIC",1,"6ES72231BH320XB0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6ES7292-2AL40-0XA0","SIMATIC S7-1200, spare part, I/O terminal block tin-coated, in push-in design, coded right, for digital signal module 32CH (4 units with 11 pins each)",47.1,"ΠΑΚ",1,"SIMATIC",1,"6ES72922AL400XA0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6ES7313-5BG04-0AB0","SIMATIC S7-300, CPU 313C, Compact CPU with MPI, 24 DI/16 DO, 4 AI, 2 AO, 1 Pt100, 3 high-speed counters (30 kHz), Integr. power supply 24 V DC, work memory 128 KB, Front connector (2x 40-pole) and Micro Memory Card required",2061,"ΤΕΜ",1,"SIMATIC",1,"6ES73135BG040AB0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6ES7390-1BC00-0AA0","SIMATIC S7-300, mounting rail, length: 2000 mm",180,"ΤΕΜ",1,"SIMATIC",1,"6ES73901BC000AA0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6ES7400-0HA10-4AB0","SIMATIC S7-400H, 416-5H Energy Standard bundle for SPPA-TX000 System bundle contains: 1x rack UR2-H, 2x CPU 416-5H, 2x memory cards 4 MB, 4x sync modules, 2x FOC cables, 2x CP442-1RX00, The SV modules (PS405 or PS407) and the batteries must be ordered separately",34125,"ΤΕΜ",1,"SIMATIC",1,"6ES74000HA104AB0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6ES7468-1BB50-0AA0","SIMATIC S7-400, IM cable with C-bus, 1.5 m",306,"ΤΕΜ",1,"SIMATIC",1,"6ES74681BB500AA0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6ES7505-0RB00-0AB0","SIMATIC S7-1500, System power supply with buffer functionality PS 60W 24/48/60V DC HF, supplies the backplane bus of the S7-1500 with operating voltage and permits the CPU to retain RAM (data) retentively",880,"ΤΕΜ",1,"SIMATIC",1,"6ES75050RB000AB0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6ES7528-0AA00-0AA0","SIMATIC S7-1500, spare part Front door for 25 mm width I/O modules; consisting of: - - front door (unlasered), - - labeling strips (front) - - cabling diagram, 5 units per packing unit",71.699999999999989,"ΠΑΚ",1,"SIMATIC",1,"6ES75280AA000AA0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6ES7590-1AC40-0AA0","SIMATIC S7-1500, mounting rail 245 mm (approx. 9.6 inch); incl. grounding screw, integrated DIN rail for mounting of incidentals such as terminals, automatic circuit breakers and relays",39.200000000000003,"ΤΕΜ",1,"SIMATIC",1,"6ES75901AC400AA0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6ES7648-2BF10-0XK1","SIMATIC CFast memory card, 30 GB, for IPCs and Open Controller with corresponding slot, scope of supply: 1 CFast 30 GB",613,"ΤΕΜ",1,"SIMATIC",1,"6ES76482BF100XK1","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6ES7672-7AC02-0YK0","SIMATIC S7-1500 Software Controller CPU 1507S upgrade for CPU 1507S V2, single license for 1 installation, runtime software class A; runtime software, software, documentation and license key download; 6 languages (de,en,it,fr,es,zh); executable in Windows 10; reference hardware: SIMATIC IPC2x7G, IPC4x7E, BX/PX-39A, IPC6x7E, IPC8x7E - - consignee email address required for delivery",537,"ΤΕΜ",1,"SIMATIC",1,"6ES76727AC020YK0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6ES7677-2WB42-0GK0","SIMATIC ET 200SP Open Controller, CPU 1515SP PC2 TF + HMI 128PT, 8 GB RAM (basic device 6ES7677-2DB40-0AA0), 128 GB CFast with Windows 10 IoT Enterprise LTSC 2019 64-bit, S7-1500 Failsafe Software Controller CPU 1505SP TF V2x and WinCC Runtime Advanced V17 preinstalled, with 128 PowerTags license; interfaces: 1x slot CFast, 1x slot SD/MMC, 1x connection for ET 200SP BusAdapter PROFINET, 1x 10/100/1000 Mbps Ethernet, 2x USB 3.0, 2x USB 2.0, 1x DisplayPort; documentation on CFast,",4823,"ΤΕΜ",1,"SIMATIC",1,"6ES76772WB420GK0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6ES7822-1AE23-0XC5","SIMATIC STEP 7 Professional V19, Powerpack & upgrade STEP 7 V5.7-> V19/2021 SR2; combo floating license DL; engineering software in the TIA Portal; class A; software, documentation and license key for download; 9 languages: de,en,zh included, fr,es,it,ru,ja,ko as download; for configuration of SIMATIC S7-1200/1500, SIMATIC S7-300/400/WinAC, SIMATIC Basic Panels SIMATIC Unified Basic Panels; - - for system requirements specification, see www.siemens.com/compatool consignee email address required for delivery",1500,"ΤΕΜ",1,"SIMATIC",1,"6ES78221AE230XC5","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6ES7823-1TE07-2AE6","TIA Portal Test Suite Advanced V19; upgrade V16..V18 -->V19; UCL download for one installation; option for engineering software in the TIA Portal; software, documentation and master license for download, UCL agreement required - - consignee email address required for delivery",611,"ΤΕΜ",1,"SIMATIC",1,"6ES78231TE072AE6","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6ES7833-1FC02-0YH5","SIMATIC S7, safety programming tool S7 Distributed Safety V5.4, floating license for 1 user, software, documentation and license key for download, class A, 3 languages (de,en,fr), executable in Windows 7 SP1, Windows 10 Professional Windows 10 Enterprise, Windows Server 2008 R2 SP1, Windows Server 2012 R2, Windows Server 2016; 64-bit operating system required; STEP 7 V5.5 SP1 or higher; ref,-HW S7-300F/400F/WinAC F - - consignee email address required for delivery",804,"ΤΕΜ",1,"SIMATIC",1,"6ES78331FC020YH5","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6ES7853-0AE01-0YE5","Siemens Network Planner upgrade V2.0, floating license download; software for simulation of PROFINET networks; software, documentation and license key for download; class A; 3 languages: de, en, zh; executable in Windows 7 (64-bit) and Windows 10 (64-bit) - - consignee email address required for delivery",436,"ΤΕΜ",1,"SIMATIC",1,"6ES78530AE010YE5","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6ES7922-3BC50-5AC0","Front connector for SIMATIC S7-300 40 pole (6ES7392-1AM00-0AA0) with 40 single cores 0.5 mm2, Single cores H05V-K, Screw version VPE=5 units L = 2.5 m",746,"ΠΑΚ",1,"SIMATIC",1,"6ES79223BC505AC0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6ES7922-3BJ00-0AU0","Cable with front connector for SIMATIC S7-300 20-pole (6ES7392-1AJ00-0AA0) on 50-pole D-SUB socket for ET200M; 0.50 mm2 Length = 8 m",312,"ΤΕΜ",1,"SIMATIC",1,"6ES79223BJ000AU0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6ES7923-3BB00-0HC0","connection cable shielded f. SIMATIC ET200 SP HA from 37-pole D-sub to bare ends with wire end sleeve labeled 32 channels L = 1 m, 0.34 mm2",90.8,"TEM",1,"SIMATIC",1,"6ES79233BB000HC0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6ES7924-0AA20-0AC0","Connection module TP1 8 channels u. 2x2 terminals f. Potential supply Type: Push-in terminal without LED, VPE=1 unit 16 pole IDC connector f. cable",20,"ΤΕΜ",1,"SIMATIC",1,"6ES79240AA200AC0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6ES7954-8LC04-0AA0","SIMATIC S7, memory cards for S7-1x 00 CPU/SINAMICS, 3, 3V Flash, 4 MB",66.099999999999994,"ΤΕΜ",1,"SIMATIC",1,"6ES79548LC040AA0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6ES7998-8XC01-8YE2","SIMATIC Manual Collection on DVD, 5 languages, Software Update Service within the framework of this contract, you will receive for one year all up-to-date software versions. the contract is extended automatically by 1 year if it is not canceled 3 months prior to expiration. Period of delivery and service: 1 year from date of invoice",418,"ΤΕΜ",1,"SIMATIC",1,"6ES79988XC018YE2","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6FB1104-0AT05-0AS1","SIDOOR door clutch holder Door clutch holder for Toothed belt width 20 mm, for holding the two toothed belt ends and for connection of the respective Door leaf with the toothed belt",66.899999999999991,"ST",1,"GMC",1,"6FB11040AT050AS1","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX2001-2EA50","INCREM. ENCODER 6FX2001-2EA50 WITH RS 422(TTL), 500 P/R, SYNCHRO-FLANGE SHAFT 6MM OPERATING VOLTAGE: 5 V RADIAL FLANGE CONNECTOR",516,"ST",1,"GMC",1,"6FX20012EA50","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX2001-2MB25","INCREM. ENCODER 6FX2001-2MB25 WITH RS 422 (TTL), 1250 P/R, CLAMP FLANGE SHAFT 10MM OPERATING VOLTAGE 5 V, UNIVERSAL CABLE OUTGOING AXIAL / RADIAL CABLE 1M WITH CONNECTOR",516,"ST",1,"GMC",1,"6FX20012MB25","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX2001-4HA50","INCREM. ENCODER 6FX2001-4HA50 WITH HTL, 500 P/R, OPERATING VOLTAGE 10-30 V, SYNCHRON. FLANGE SHAFT 6MM AXIAL FLANGE CONNECTOR",516,"ST",1,"GMC",1,"6FX20014HA50","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX2001-5FN25","absolute encoder 6FX2001-5FN25 multi-turn 30-bit with PROFINET operating voltage 10-30 V synchronous flange/ shaft 6 mm plug M12 radial FS15 maximum ambient temperature 85 Â°C",1970,"ST",1,"GMC",1,"6FX20015FN25","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX2002-1DC00-1AH3","Signal cable pre-assembled type: 6FX2002-1DC00 (SINAMICS Drive CLiQ) Connector IP20/IP20, without 24 V Length (m)= 0 + 0 + 7 + 0,3",217,"ST",1,"GMC",1,"6FX20021DC001AH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX2002-1DC00-1BD1","Signal cable pre-assembled type: 6FX2002-1DC00 (SINAMICS Drive CLiQ) Connector IP20/IP20, without 24 V Length (m)= 0 + 10 + 3 + 0,1",277,"ST",1,"GMC",1,"6FX20021DC001BD1","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX2002-1DC00-1BF1","Signal cable pre-assembled type: 6FX2002-1DC00 (SINAMICS Drive CLiQ) Connector IP20/IP20, without 24 V Length (m)= 0 + 10 + 5 + 0,1",296,"ST",1,"GMC",1,"6FX20021DC001BF1","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX2002-1DC00-1EG0","Signal cable pre-assembled type: 6FX2002-1DC00 (SINAMICS Drive CLiQ) Connector IP20/IP20, without 24 V Length (m)= 0 + 40 + 6 + 0",591,"ST",1,"GMC",1,"6FX20021DC001EG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX2003-0LA10","power connector 6-pole Sz. 1.5 type: 6FX2003-0LA10 pins, male thread 1x 6-pole insulator 5x pin contacts (1.5-4 mm2) 5x pin contacts (6-16 mm2) 3x brake cont. (1-2.5 mm2) 2x cable terminal Pack=1 unit for cable diameter: 7 - 9 / 9 - 16 / 16 - 25",274,"ST",1,"GMC",1,"6FX20030LA10","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX2003-0SU35","signal connector 17-pole type: 6FX2003-0SU35 SPEED-CONNECT M17 screw cap, socket 1x 12-pole insulator 20xcontacts 0.14-0.5 mm2 1x cable clamp 6-9.5 mm",157,"ST",1,"GMC",1,"6FX20030SU35","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX2003-7KS20","Pin contacts 0.14-0.5 mm2 type: 6FX2003-7KS20 (signal connector M17) Pack=20 units",33.800000000000004,"PAK","PAK","GMC",1,"6FX20037KS20","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX3002-2DB12-1AF0","Pre-assembled signal cable for absolute encoder in S-1FL6 LI SH50 3 x 2 x 0.20 + 2 x 2 x 0.25 C MOTION-CONNECT 300 no UL for connector on the motor s Dmax: 7.2 mm length: 5 m with straight conne",165,"ST",1,"GMC",1,"6FX30022DB121AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX3502-2XB11-1AD0","Encoder cable, Preassembled 3x2x0.25 for motor S-1FL2 SH48/52 with S200, MOTION-CONNECT 350 Length(m)=3m Dmax encoder=7.0mm 1 million bending times",151,"ST",1,"GMC",1,"6FX35022XB111AD0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX3502-7DD01-1CA0","Dual cable pre-assembled 4x0.75+2x0.38/2x2x0.25+2x0.38 for motor S-1FL2 SH20/30/40 with S200, MOTION-CONNECT 350 Length(m)=20m Dmax power=7.5mm Dmax encoder=7.0mm w. brake, Drive End Outlet 1 million bending times",725,"ST",1,"GMC",1,"6FX35027DD011CA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX3802-5CL01-1DA0","Power cable, Preassembled 4x0.75 for motor S-1FL2 SH45/65/90 with S200, MOTION-CONNECT 380 Length(m)=30m Dmax power=7.5mm w.o. brake 5 million bending times",600,"ST",1,"GMC",1,"6FX38025CL011DA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-2AH00-1AK0","Signal cable pre-assembled (HTL in motor 1-ph.) 4x 2x 0.34+4x 0.5 C UL/CSA, DESINA MOTION-CONNECT 500 Dmax=9.3 mm TYPE: 6FX5002-2AH00 LENGTH (M) = +0 +0 +9 +0",179,"ST",1,"GMC",1,"6FX50022AH001AK0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-2AH00-2DF0","Signal cable pre-assembled (HTL in motor 1-ph.) 4x 2x 0.34+4x 0.5 C UL/CSA, DESINA MOTION-CONNECT 500 Dmax=9.3 mm TYPE: 6FX5002-2AH00 LENGTH (M) = +100 +30 +5 +0",1199,"ST",1,"GMC",1,"6FX50022AH002DF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-2CA20-1CA0","signal cable pre-assembled type: 6FX5002-2CA20 (incr. encoder in motor AH20) 3x 2x 0.14+4x 0.14+2x 0.5+4x 0.22C with M17 connector UL/CSA DESINA MOTION-CONNECT 500 Dmax=9.9 mm; Length (m)= +0 +20 +0 +0",484,"ST",1,"GMC",1,"6FX50022CA201CA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-2CA31-1BB0","signal cable pre-assembled (encoder voltage signal) 3x 2x 0.14+4x 0.14+2x0.5+4x 0.23 C UL/CSA, DESINA MOTION-CONNECT 500 Dmax=9.9 mm TYPE: 6FX5002-2CA31 LENGTH (M) = +0 +10 +1 +0",272,"ST",1,"GMC",1,"6FX50022CA311BB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-2CA31-1KA0","signal cable pre-assembled (encoder voltage signal) 3x 2x 0.14+4x 0.14+2x0.5+4x 0.23 C UL/CSA, DESINA MOTION-CONNECT 500 Dmax=9.9 mm TYPE: 6FX5002-2CA31 LENGTH (M) = +0 +90 +0 +0",1095,"ST",1,"GMC",1,"6FX50022CA311KA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-2CD24-1DA0","Signal cable pre-assembled (incremental encoder TTL 24V) 4x 2x 0.34+4x 0.5 C UL/CSA, DESINA MOTION-CONNECT 500 Dmax=9.3 mm TYPE: 6FX5002-2CD24 LENGTH (M) = +0 +30 +0 +0",386,"ST",1,"GMC",1,"6FX50022CD241DA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-2CF04-1AB0","signal cable, pre-assembled Extension (resolver IM 1FK6) 3x 2x 0.14+4x 0.14+2x0.5 C UL/CSA, DESINA MOTION-CONNECT 500 Inner shields also applied on round connector Dmax=9.3 mm TYPE: 6FX5002-2CF04 LENGTH (M) = +0 +0 +1 +0",200,"ST",1,"GMC",1,"6FX50022CF041AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-2CF20-1AF0","Signal cable pre-assembled type: 6FX5002-2CF20 (resolver in motor AH20) 3x 2x 0.14+4x 0.14+2x 0.5 C UL/CSA DESINA MOTION-CONNECT 500 Dmax=9.3 mm Length (m)= +0 +0 +5 +0",275,"ST",1,"GMC",1,"6FX50022CF201AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-2CH00-1EA0","Signal cable pre-assembled (810D/611D to encoder EnDat) 3x 2x 0.14+4x 0.14+2x0.5 C UL/CSA, DESINA MOTION-CONNECT 500 Dmax=9.3 mm TYPE: 6FX5002-2CH00 LENGTH (M) = +0 +40 +0 +0",518,"ST",1,"GMC",1,"6FX50022CH001EA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-2DC00-1BK0","Signal cable pre-assembled type: 6FX5002-2DC00 (SINAMICS Drive CLiQ) connector IP20/IP20, with 24 V MOTION-CONNECT 500 Length (m)= +0 +10 +9 +0",303,"ST",1,"GMC",1,"6FX50022DC001BK0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-2DC10-1AD0","Signal cable pre-assembled type: 6FX5002-2DC10 (SINAMICS DRIVE-CLiQ) plug IP20/IP67, with 24 V MOTION-CONNECT 500 length (m)= +0 +0 +3 +0",177,"ST",1,"GMC",1,"6FX50022DC101AD0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-2DC10-1BF5","Signal cable pre-assembled type: 6FX5002-2DC10 (SINAMICS DRIVE-CLiQ) plug IP20/IP67, with 24 V MOTION-CONNECT 500 length (m)= +0 +10 +5 +0.5",298,"ST",1,"GMC",1,"6FX50022DC101BF5","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-2DC10-1EB0","Signal cable pre-assembled type: 6FX5002-2DC10 (SINAMICS DRIVE-CLiQ) plug IP20/IP67, with 24 V MOTION-CONNECT 500 length (m)= +0 +40 +1 +0",533,"ST",1,"GMC",1,"6FX50022DC101EB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-2DC20-1AC3","Signal cable pre-assembled type: 6FX5002-2DC20 (SINAMICS DRIVE-CLiQ) plug IP67/IP67, with 24 V MOTION-CONNECT 500 length (m)= +0 +0 +2 +0.3",200,"ST",1,"GMC",1,"6FX50022DC201AC3","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-2DC20-1AF2","Signal cable pre-assembled type: 6FX5002-2DC20 (SINAMICS DRIVE-CLiQ) plug IP67/IP67, with 24 V MOTION-CONNECT 500 length (m)= +0 +0 +5 +0.2",228,"ST",1,"GMC",1,"6FX50022DC201AF2","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-2DC20-1HF0","Signal cable pre-assembled type: 6FX5002-2DC20 (SINAMICS DRIVE-CLiQ) plug IP67/IP67, with 24 V MOTION-CONNECT 500 length (m)= +0 +70 +5 +0",874,"ST",1,"GMC",1,"6FX50022DC201HF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-2DC36-1BC0","Signal cable pre-assembled type: 6FX5002-2DC36 DRIVE-CLiQ with 24 V M12 female/ RJ45 IP67 MOTION-CONNECT 500 Dmax=7.1 mm Length (m)=12",298,"ST",1,"GMC",1,"6FX50022DC361BC0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-2DC40-1BF0","Signal cable pre-assembled type: 6FX5002-2DC40 Customer-specific DRIVE-CLiQ with 24 V M17 female SPEED-CONNECT/ RJ45 IP20 MOTION-CONNECT 500 Dmax=7.1 mm Length (m)= +0 +10 +5 +0",317,"ST",1,"GMC",1,"6FX50022DC401BF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-2DC46-1BC0","Signal cable pre-assembled type: 6FX5002-2DC46 DRIVE-CLiQ with 24 V M12 female/ M17 male speed-connect-ready MOTION-CONNECT 500 Dmax=7.1 mm Length (m)=12",346,"ST",1,"GMC",1,"6FX50022DC461BC0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-2EQ10-1AB5","signal cable pre-assembled (absolute encoder in motor) 3x 2x 0.14+4x 0.14+2x0.5+4x 0.23 C UL/CSA, DESINA MOTION-CONNECT 500 Dmax=9.9 mm TYPE: 6FX5002-2EQ10 LENGTH (M) = +0 +0 +1 +0.5",174,"ST",1,"GMC",1,"6FX50022EQ101AB5","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-2EQ10-1DH0","signal cable pre-assembled (absolute encoder in motor) 3x 2x 0.14+4x 0.14+2x0.5+4x 0.23 C UL/CSA, DESINA MOTION-CONNECT 500 Dmax=9.9 mm TYPE: 6FX5002-2EQ10 LENGTH (M) = +0 +30 +7 +0",525,"ST",1,"GMC",1,"6FX50022EQ101DH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-2EQ10-1JA0","signal cable pre-assembled (absolute encoder in motor) 3x 2x 0.14+4x 0.14+2x0.5+4x 0.23 C UL/CSA, DESINA MOTION-CONNECT 500 Dmax=9.9 mm TYPE: 6FX5002-2EQ10 LENGTH (M) = +0 +80 +0 +0",958,"ST",1,"GMC",1,"6FX50022EQ101JA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5CA05-1CF0","power cable, pre-assembled, Extension 4x 1.5 C connector Sz. 1 (1FT/1FK to 611/810D/SIMOVERT) UL/CSA, DESINA MOTION-CONNECT 500 Dmax=11.5 mm TYPE: 6FX5002-5CA05 LENGTH (M) = +0 +20 +5 +0",460,"ST",1,"GMC",1,"6FX50025CA051CF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5CF10-1BA0","power cable type: 6FX5002-5CF10 pre-assembled 4x 1.5 C, SPEED-CONNECT Sz. 1 for SINAMICS S120 Combi MOTION-CONNECT 500 UL/CSA, DESINA Dmax=8.4 mm Length (m)= +0 +10 +0 +0",215,"ST",1,"GMC",1,"6FX50025CF101BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5CG01-1DJ0","Power cable pre-assembled type: 6FX5002-5CG01 4x 1.5 C, Connector Sz. 1 (SINAMICS AC Drive) UL/CSA, DESINA MOTION-CONNECT 500 Dmax=8.4 mm +0 +30 +8 +0",398,"ST",1,"GMC",1,"6FX50025CG011DJ0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5CG10-1CE0","Power cable pre-assembled 4x 1.5 C SPEED-CONNECT connector Sz. 1 (SINAMICS AC Drive) UL/CSA DESINA MOTION-CONNECT 500 Dmax=8.4 mm TYPE: 6FX5002-5CG10 LENGTH (M) = +0 +20 +4 +0",313,"ST",1,"GMC",1,"6FX50025CG101CE0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5CG21-1AE0","Power cable pre-assembled type: 6FX5002-5CG21 4x 1.5 C connector Sz. 1.5 (SINAMICS AC Drive) UL/CSA, DESINA MOTION-CONNECT 500 Dmax=8.4 mm +0 +0 +4 +0",321,"ST",1,"GMC",1,"6FX50025CG211AE0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5CG22-1CJ0","Power cable pre-assembled 4x 1.5 C Speed connect connector Sz. 1.5 (SINAMICS AC Drive) UL/CSA DESINA MOTION-CONNECT 500 Dmax=8.4 mm TYPE: 6FX5002-5CG22 LENGTH (M) = +0 +20 +8 +0",543,"ST",1,"GMC",1,"6FX50025CG221CJ0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5CG32-1AH5","Power cable pre-assembled 4x 2.5 C Speed connect connector Sz. 1.5 (SINAMICS AC Drive) UL/CSA DESINA MOTION-CONNECT 500 Dmax=10 mm TYPE: 6FX5002-5CG32 LENGTH (M) = +0 +0 +7 +0.5",332,"ST",1,"GMC",1,"6FX50025CG321AH5","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5CG52-1DA0","Power cable pre-assembled 4x 6 C Speed connect connector Sz. 1.5 (SINAMICS AC Drive) UL/CSA DESINA MOTION-CONNECT 500 Dmax=13.6 mm TYPE: 6FX5002-5CG52 LENGTH (M) = +0 +30 +0 +0",719,"ST",1,"GMC",1,"6FX50025CG521DA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5CN06-1CB4","Power cable pre-assembled TYPE 6FX5002-5CN06 4X1,5 C, SPEED-CONNECT SIZE 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 500 UL/CSA, DESINA DMAX=8.4 MM LENGTH (M) = +0 +20 +1 + 0.4",378,"ST",1,"GMC",1,"6FX50025CN061CB4","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5CN16-1CA0","Power cable pre-assembled TYPE 6FX5002-5CN16 4X2.5 C CONNECTOR SPEED-CONNECT SIZE 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 500 UL/CSA, DESINA DMAX=11 MM LENGTH (M) = +0 +20 +0 +0",403,"ST",1,"GMC",1,"6FX50025CN161CA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5CN26-1AH4","Power cable pre-assembled TYPE 6FX5002-5CN26 4X1,5C, SPEED-CONNECT SIZE 1.5 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 500 UL/CSA, DESINA DMAX=8.4 MM LENGTH (M) = +0 +0 +7 + 0.4",376,"ST",1,"GMC",1,"6FX50025CN261AH4","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5CN56-1DA0","Power cable pre-assembled TYPE 6FX5002-5CN56 4X6 C CONNECTOR SPEED-CONNECT S. 1.5 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 500 UL/CSA, DESINA DMAX=13.6 MM LENGTH (M) = +0 +30 +0 +0",723,"ST",1,"GMC",1,"6FX50025CN561DA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5CQ58-1BA0","power cable extension 4x 6 C, SPEED-CONNECT Sz. 1.5 MOTION-CONNECT 500 UL/CSA DESINA Dmax=16.6 mm TYPE: 6FX5002-5CQ58 LENGTH (M) = +0 +10 +0 +0",659,"ST",1,"GMC",1,"6FX50025CQ581BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5CS06-1BB5","Power cable pre-assembled TYPE 6FX5002-5CS06 4X1,5 C, CONN. FULL THREAD S. 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 500 UL/CSA, DESINA DMAX=8.4 MM LENGTH (M) = +0 +10 +1 + 0.5",325,"ST",1,"GMC",1,"6FX50025CS061BB5","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5CS14-1CF0","Power cable pre-assembled type: 6FX5002-5CS14 (1FT/1FK/1PH for SINAMICS) 4x 10 C, Connector size 3 Ring cable lug UL/CSA, DESINA MOTION-CONNECT 500 Dmax=20 mm; Length (m)= +0 +20 +5 +0",1283,"ST",1,"GMC",1,"6FX50025CS141CF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5CS54-1AH0","Power cable pre-assembled type: 6FX5002-5CS54 (1FT/1FK/1PH for SINAMICS) 4x 6 C, Connector Sz. 1.5/ Ring cable lug UL/CSA DESINA MOTION-CONNECT 500 Dmax=15.6 mm, Length (m)= +0 +0 +7 +0",395,"ST",1,"GMC",1,"6FX50025CS541AH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5CS66-1FA0","Power cable pre-assembled Type 6FX5002-5CS66 4x 10 C Connector, full thread, Sz. 1.5 for SINAMICS S120 booksize Motor Module C/D types MOTION-CONNECT 500 UL/CSA, DESINA Dmax=20 mm Length (m)= +0 +50 +0 +0",1340,"ST",1,"GMC",1,"6FX50025CS661FA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5DA05-1AB5","power cable, pre-assembled, Extension 4x 1.5+(2x1.5) C, Connector Sz. 1 (1FT/1FK to 611/810D/SIMOVERT) UL/CSA, DESINA MOTION-CONNECT 500 Dmax=13.1 mm TYPE: 6FX5002-5DA05 LENGTH (M) = +0 +0 +1 +0.5",344,"ST",1,"GMC",1,"6FX50025DA051AB5","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5DG01-1AB0","Power cable pre-assembled type: 6FX5002-5DG01 4x 1.5+(2x1.5) C, Connector Sz. 1 (SINAMICS AC Drive) UL/CSA, DESINA MOTION-CONNECT 500 Dmax=10.8 mm +0 +0 +1 +0",204,"ST",1,"GMC",1,"6FX50025DG011AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5DG10-1DH0","Power cable pre-assembled 4x 1.5+(2x1.5) C SPEED-CONNECT connector Sz. 1 (SINAMICS AC Drive) UL/CSA DESINA MOTION-CONNECT 500 Dmax=10.8 mm TYPE: 6FX5002-5DG10 LENGTH (M) = +0 +30 +7 +0",579,"ST",1,"GMC",1,"6FX50025DG101DH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5DG12-1AC0","Power cable pre-assembled 4x 2.5+(2x1.5) C C SPEED-CONNECT Sz. 1 for SINAMICS Power Module MOTION-CONNECT 500 UL/CSA DESINA Dmax=12.4 mm TYPE: 6FX5002-5DG12 LENGTH (M) = +0 +0 +2 +0",220,"ST",1,"GMC",1,"6FX50025DG121AC0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5DG31-1AD0","power cable pre-assembled type: 6FX5002-5DG31 4x 2.5+(2x1.5) C, Connector Sz. 1.5 (SINAMICS AC Drive) UL/CSA, DESINA MOTION-CONNECT 500 Dmax=12.4 mm +0 +0 +3 +0",331,"ST",1,"GMC",1,"6FX50025DG311AD0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5DG42-1AD0","Power cable pre-assembled 4x 4+(2x1.5) C Speed connect connector Sz. 1.5 (SINAMICS AC Drive) UL/CSA DESINA MOTION-CONNECT 500 Dmax=14 mm TYPE: 6FX5002-5DG42 LENGTH (M) = +0 +0 +3 +0",343,"ST",1,"GMC",1,"6FX50025DG421AD0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5DG51-1CG0","Power cable pre-assembled type: 6FX5002-5DG51 4x 6+(2x1.5) C, Connector Sz. 1.5 (SINAMICS AC Drive) UL/CSA, DESINA MOTION-CONNECT 500 Dmax=16.1 mm +0 +20 +6 +0",838,"ST",1,"GMC",1,"6FX50025DG511CG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5DN05-1CF0","power cable, pre-assembled, Extension 4x 1.5+(2x1.5) C SPEED-CONNECT connector Sz. 1 (SIMODRIVE) UL/CSA DESINA MOTION-CONNECT 500 Dmax=13.1 mm TYPE: 6FX5002-5DN05 LENGTH (M) = +0 +20 +5 +0",584,"ST",1,"GMC",1,"6FX50025DN051CF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5DN06-1BE5","Power cable pre-assembled TYPE 6FX5002-5DN06 4X1.5, (2X1.5)C C CONNECTOR SPEED-CONNECT SIZE 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 500 UL/CSA, DESINA DMAX = 10.8 MM LENGTH (M) = +0 +10 +4 + 0.5",410,"ST",1,"GMC",1,"6FX50025DN061BE5","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5DN26-1BF0","Power cable pre-assembled TYPE 6FX5002-5DN26 4X1.5, (2X1.5)C C CONNECTOR SPEED-CONNECT SIZE 1.5 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 500 UL/CSA, DESINA DMAX = 10.8 MM LENGTH (M) = +0 +10 +5 +0",482,"ST",1,"GMC",1,"6FX50025DN261BF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5DN30-1CA0","Power cable pre-assembled 4x 1.5+(2x1.5) C C SPEED-CONNECT Sz. 0.5 for SINAMICS motor Module UL/CSA DESINA MOTION-CONNECT 500 Dmax=10.8 mm TYPE: 6FX5002-5DN30 LENGTH (M) = +0 +20 +0 +0",426,"ST",1,"GMC",1,"6FX50025DN301CA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5DN64-1FH0","Power cable pre-assembled 4x 10+2x1.5 C SPEED-CONNECT connector Sz. 1.5 Ring cable lug (SINAMICS Motor Module) UL/CSA DESINA MOTION-CONNECT 500 Dmax=21.7 mm TYPE: 6FX5002-5DN64 LENGTH (M) = +0 +50 +7 +0",2008,"ST",1,"GMC",1,"6FX50025DN641FH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5DS06-1BE0","Power cable pre-assembled TYPE 6FX5002-5DS06 4X1.5, (2X1.5)C C CONNECTOR FULL THREAD SIZE 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 500 UL/CSA, DESINA DMAX = 10.8 MM LENGTH (M) = +0 +10 +4 +0",401,"ST",1,"GMC",1,"6FX50025DS061BE0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5DS06-1EA0","Power cable pre-assembled TYPE 6FX5002-5DS06 4X1.5, (2X1.5)C C CONNECTOR FULL THREAD SIZE 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 500 UL/CSA, DESINA DMAX = 10.8 MM LENGTH (M) = +0 +40 +0 +0",624,"ST",1,"GMC",1,"6FX50025DS061EA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5DS54-1BA0","Power cable pre-assembled type: 6FX5002-5DS54 (1FT/1FK/1PH for SINAMICS) 4x 6+2x1.0 C, Connector Sz. 1.5/ Ring cable lug UL/CSA, DESINA MOTION-CONNECT 500 Dmax=16.9 mm, Length (m)= +0 +10 +0 +0",520,"ST",1,"GMC",1,"6FX50025DS541BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5DX48-1EB0","Power cable pre-assembled 4x 35+(2x1.5) C, Connector size 3 (1FT/1FK to 611/810D/SIMOVERT) UL/CSA DESINA MOTION-CONNECT 500 Dmax=32.6 mm TYPE: 6FX5002-5DX48 LENGTH (M) = +0 +40 +1 +0",5492,"ST",1,"GMC",1,"6FX50025DX481EB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-8QE21-1CB0","Single cable extension 4G2.5+1Q0,2STC+1P1.5C-C SPEED-CONNECT M23 connector UL/CSA DESINA MOTION-CONNECT 500 Dmax.=13.3 mm Length (m)= +0 +20 +1 +0",1209,"ST",1,"GMC",1,"6FX50028QE211CB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-8QE21-1EC0","Single cable extension 4G2.5+1Q0,2STC+1P1.5C-C SPEED-CONNECT M23 connector UL/CSA DESINA MOTION-CONNECT 500 Dmax.=13.3 mm Length (m)= +0 +40 +2 +0",2013,"ST",1,"GMC",1,"6FX50028QE211EC0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-8QN11-1AF5","Single cable connection prefabricated 4G1.5+1Q0,2STC+1P1.5C-C SPEED-CONNECT connector M23 Cores with end sleeve Data cable with IX connector UL/CSA DESINA MOTION-CONNECT 500 Dmax.=12.3 MM Length(M)= +0 +0 +5 +0.5",380,"ST",1,"GMC",1,"6FX50028QN111AF5","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-8QN21-1BD0","Single cable pre-assembled 4G2,5+1Q0,2STC+1P1,5C-C SPEED-CONNECT connector M23 Cores with end sleeve Data cable with IX connector UL/CSA DESINA Motion-Connect 500 Dmax.=13.3 mm length(M)= +0 +10 +3 +0",786,"ST",1,"GMC",1,"6FX50028QN211BD0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-8QN21-1ED0","Single cable pre-assembled 4G2,5+1Q0,2STC+1P1,5C-C SPEED-CONNECT connector M23 Cores with end sleeve Data cable with IX connector UL/CSA DESINA Motion-Connect 500 Dmax.=13.3 mm length(M)= +0 +40 +3 +0",1936,"ST",1,"GMC",1,"6FX50028QN211ED0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5008-1BA61-1CF0","Power cable sold by the meter type: 6FX5008-1BA61 4x 16+2x 1.5 C UL/CSA, DESINA MOTION-CONNECT 500 Type of delivery: up to 29 m ring from 30 m drum Dmax=25.0 mm, Length (m)= +0 +20 +5 +0",1222,"ST",1,"GMC",1,"6FX50081BA611CF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5008-1BB25-1BJ0","Power cable sold by the meter type: 6FX5008-1BB25 4x 25 C UL/CSA, DESINA MOTION-CONNECT 500 Type of delivery: up to 19 m ring from 20 m drum Dmax=28.0 mm, Length (m)= +0 +10 +8 +0",997,"ST",1,"GMC",1,"6FX50081BB251BJ0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5008-1BB31-1JA0","Power cable sold by the meter type: 6FX5008-1BB31 4x 4.0 C UL/CSA, DESINA MOTION-CONNECT 500 Type of delivery: to 99 m ring from 100 m drum Dmax=11.4 mm, Length (m)= +0 +80 +0 +0",1213,"ST",1,"GMC",1,"6FX50081BB311JA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5008-1BB35-1CF0","Power cable sold by the meter type: 6FX5008-1BB35 4x 35 C UL/CSA, DESINA MOTION-CONNECT 500 Type of delivery: up to 14 m ring from 15 m drum Dmax=31.5 mm, Length (m)= +0 +20 +5 +0",1964,"ST",1,"GMC",1,"6FX50081BB351CF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5008-1BB50-1BA0","Power cable sold by the meter type: 6FX5008-1BB50 4x 50 C UL/CSA, DESINA MOTION-CONNECT 500 Type of delivery: to 9 m ring from 10 m drum Dmax=38.0 mm, Length (m)= +0 +10 +0 +0",1078,"ST",1,"GMC",1,"6FX50081BB501BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5008-1BB51-1AH0","Power cable sold by the meter type: 6FX5008-1BB51 4x 10 C UL/CSA, DESINA MOTION-CONNECT 500 Type of delivery: to 49 m ring from 50 m drum Dmax=20.0 mm, Length (m)= +0 +0 +7 +0",224,"ST",1,"GMC",1,"6FX50081BB511AH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5008-1BB70-1CA0","Power cable sold by the meter type: 6FX5008-1BB70 4x 70 C UL/CSA, DESINA MOTION-CONNECT 500 Dmax=42.6 mm, Length (m)= +0 +20 +0 +0",3786,"ST",1,"GMC",1,"6FX50081BB701CA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5012-2CA31-1DA0","signal cable pre-assembled (encoder voltage signal) 3x 2x 0.14+4x 0.14+2x0.5+4x 0.23 C UL/CSA, DESINA MOTION-CONNECT 500 Dmax=9.9 mm TYPE: 6FX5012-2CA31 MODULE SIDE: CRIMPED CONTACTS, CONNECTOR HOUSING INCLUDED LENGTH (M) = +0 +30 +0 +0",471,"ST",1,"GMC",1,"6FX50122CA311DA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5012-2EQ10-1EG0","signal cable pre-assembled (absolute encoder in motor) 3x 2x 0.14+4x 0.14+2x0.5+4x 0.23 C UL/CSA, DESINA MOTION-CONNECT 500 Dmax=9.9 mm TYPE: 6FX5012-2EQ10 MODULE SIDE: CRIMPED CONTACTS, CONNECTOR HOUSING INCLUDED LENGTH (M) = +0 +40 +6 +0",616,"ST",1,"GMC",1,"6FX50122EQ101EG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5012-5DN06-1AF5","Power cable pre-assembled TYPE 6FX5012-5DN06 4X1.5, (2X1.5)C C CONNECTOR SPEED-CONNECT SIZE 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES PREPARED CONDUCTORS, SINAMICS CONNECTOR INCLUDED MOTION-CONNECT 500 UL/CSA, DESINA DMAX = 10.8 MM LENGTH (M) = +0 +0 +5 + 0.5",333,"ST",1,"GMC",1,"6FX50125DN061AF5","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5022-5DN16-1DC0","Power cable pre-assembled TYPE 6FX5022-5DN16 4X2.5 , (2X1.5)C C CONNECTOR SPEED-CONNECT SIZE 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES PREPARED CONDUCTORS, W/O SINAMICS CONNECTOR MOTION-CONNECT 500 UL/CSA, DESINA DMAX=12.4 MM LENGTH (M) = +0 +30 +2 +0",582,"ST",1,"GMC",1,"6FX50225DN161DC0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5042-2CA31-1FA0","signal cable pre-assembled (encoder voltage signal) 3x 2x 0.14+4x 0.14+2x0.5+4x 0.23 C UL/CSA, DESINA MOTION-CONNECT 500 Dmax=9.9 mm TYPE: 6FX5042-2CA31 MOTOR SIDE: CRIMPED CONTACTS, CONNECTOR HOUSING INCLUDED LENGTH (M) = +0 +50 +0 +0",678,"ST",1,"GMC",1,"6FX50422CA311FA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX7002-5EA31-1BB0","power cable, pre-assembled type: 6FX7002-5EA31 4x 2.5+(4x 0.5) C, Connector Sz. 1.5 (1FN to 611) trailable UL/CSA DESINA MOTION-CONNECT 700 Dmax=15.2 mm, Length (m)= 0 + 10 + 1 + 0",652,"ST",1,"GMC",1,"6FX70025EA311BB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX7002-5EB11-1AJ2","power cable pre-assembled type: 6FX7002-5EB11 4x 2.5+(4x 0.5) C, Connector Sz. 1 (1FN to 611) trailable UL/CSA DESINA MOTION-CONNECT 700 Dmax=15.2 mm, Length (m)= 0 + 0 + 8 + 0,2",502,"ST",1,"GMC",1,"6FX70025EB111AJ2","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX7002-5LM42-1AD0","Power cable pre-assembled type: 6FX7002-5LM42 4x 2.5 C M20/1FN3 screw connection Connector full thread Sz. 1 on the converter side for SIMODRIVE/MASTERDRIVES MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=11 mm Length (m)= 0 + 0 + 3 + 0",346,"ST",1,"GMC",1,"6FX70025LM421AD0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX7008-1BC11-2AA0","Power cable sold by the meter type: 6FX7008-1BC11 4x 1.5+4x 0.5 C for linear motors trailable UL/CSA DESINA MOTION-CONNECT 700 Type of delivery: Ring Dmax=14.0 mm, Length (m)=100",3534,"ST",1,"GMC",1,"6FX70081BC112AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX7008-1BC31-1BG0","Power cable sold by the meter type: 6FX7008-1BC31 4x 4+4x 0.5 C for linear motors trailable UL/CSA DESINA MOTION-CONNECT 700 Type of delivery: Ring Dmax=16.6 mm, Length (m)= 0 + 10 + 6 + 0",707,"ST",1,"GMC",1,"6FX70081BC311BG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2AD04-1AJ0","Signal cable pre-assembled for absolute value encoder SSI and EnDat 5V DC, also extension for base 6FX8002-2AD00-XXXX 3x (2x0.14) C+4x 0.14+2x0.5 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.2 mm TYPE: 6FX8002-2AD04 LENGTH (M) = +0 +0 +8 +0",341,"ST",1,"GMC",1,"6FX80022AD041AJ0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2AH00-1AG0","Signal cable pre-assembled for incr. encoder HTL in motor Connection via SMC30 4x (2x0.34)+4x 0.5 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=9.3 mm Length (m)= LENGTH (M) = +0 +0 +6 +0",188,"ST",1,"GMC",1,"6FX80022AH001AG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2BA00-1DA0","Signal cable pre-assembled SIMODRIVE 611 for modulating valve 4x (2x0.34)+4x 0.5 C MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=9.3 mm Length (m)= TYPE: 6FX8002-2BA00 LENGTH (M) = +0 +30 +0 +0",480,"ST",1,"GMC",1,"6FX80022BA001DA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2CA11-1AG4","Signal cable pre-assembled for incremental encoder sin/cos 1 Vpp 6FX2001-3 4x (2x0.34)+4x 0.5 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=9.3 mm Length (m)= type: 6FX8002-2CA11 length (m)= +0 +0 +6 +0.4",228,"ST",1,"GMC",1,"6FX80022CA111AG4","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2CA31-1AB0","Signal cable pre-assembled for incr. encoder with C/D tracks integrated into the motor 3x (2x0.14) C+4x 0.14+2x0.5 +4x 0.22 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.8 mm Length (m)= TYPE: 6FX8002-2CA31 LENGTH (M) = +0 +0 +1 +0",212,"ST",1,"GMC",1,"6FX80022CA311AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2CA31-1AG5","Signal cable pre-assembled for incr. encoder with C/D tracks integrated into the motor 3x (2x0.14) C+4x 0.14+2x0.5 +4x 0.22 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.8 mm Length (m)= TYPE: 6FX8002-2CA31 LENGTH (M) = +0 +0 +6 +0.5",299,"ST",1,"GMC",1,"6FX80022CA311AG5","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2CA31-1CG0","Signal cable pre-assembled for incr. encoder with C/D tracks integrated into the motor 3x (2x0.14) C+4x 0.14+2x0.5 +4x 0.22 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.8 mm Length (m)= TYPE: 6FX8002-2CA31 LENGTH (M) = +0 +20 +6 +0",573,"ST",1,"GMC",1,"6FX80022CA311CG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2CA34-1AH0","Signal cable extension for base 2CA31-2CA80 or -2CA88 3x (2x0.14) C + 4x 0.14+2x0.5+4x 0.22 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.8 mm Length (m)= TYPE: 6FX8002-2CA34 LENGTH (M) = +0 +0 +7 +0",329,"ST",1,"GMC",1,"6FX80022CA341AH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2CA88-1AB0","signal cable, pre-assembled Extension for incremental encoder SIN/COS 1 VPP without C and D track for SME20 3x (2x0.14) C+4x 0.14+2x0.5 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=9.2 mm Length (m)= TYPE: 6FX8002-2CA88 LENGTH (M) = +0 +0 +1 +0",209,"ST",1,"GMC",1,"6FX80022CA881AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2CB54-1CG0","signal cable, pre-assembled Extension for incremental encoder TTL 5V, 6FX2001-2 4x (2x0.34)+4x 0.5 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=9.3 mm Length (m)= TYPE: 6FX8002-2CB54 LENGTH (M) = +0 +20 +6 +0",445,"ST",1,"GMC",1,"6FX80022CB541CG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2CB54-1EA0","signal cable, pre-assembled Extension for incremental encoder TTL 5V, 6FX2001-2 4x (2x0.34)+4x 0.5 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=9.3 mm Length (m)= TYPE: 6FX8002-2CB54 LENGTH (M) = +0 +40 +0 +0",589,"ST",1,"GMC",1,"6FX80022CB541EA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2CF02-1BE0","Signal cable pre-assembled For resolvers 3x (2x0.14) C+4x 0.14+2x0.5 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=9.2 mm Length (m)= TYPE: 6FX8002-2CF02 LENGTH (M) = +0 +10 +4 +0",394,"ST",1,"GMC",1,"6FX80022CF021BE0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2CF02-1DF0","Signal cable pre-assembled For resolvers 3x (2x0.14) C+4x 0.14+2x0.5 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=9.2 mm Length (m)= TYPE: 6FX8002-2CF02 LENGTH (M) = +0 +30 +5 +0",697,"ST",1,"GMC",1,"6FX80022CF021DF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2CG00-1BG0","Signal cable pre-assembled for incremental encoder SIN/COS 1VPP, 6FX2001-3 4x (2x0.34)+4x 0.5 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.3 mm Length (m)= TYPE: 6FX8002-2CG00 LENGTH (M) = +0 +10 +6 +0",314,"ST",1,"GMC",1,"6FX80022CG001BG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2CH00-1BC0","Signal cable pre-assembled for absolute encoder EnDat 6FX2001-5 3x (2x0.14) C+4x 0.14+2x0.5 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.2 mm Length (m)= TYPE: 6FX8002-2CH00 LENGTH (M) = +0 +10 +2 +0",371,"ST",1,"GMC",1,"6FX80022CH001BC0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2CP00-1AA6","Signal cable pre-assembled type: 6FX8002-2CP00 for handwheel 840D on COM board 4x (2x0.18) C MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=6.7 mm Length (m)= +0 +0 +0 +0.6",124,"ST",1,"GMC",1,"6FX80022CP001AA6","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2CT31-1AE6","Signal cable pre-assembled type: 6FX8002-2CT31 (encoder voltage signal) Basic cable 6FX8002-2CA31-.... Smaller bending radii Dmax=9.9 mm, Length (m)=4.6",719,"ST",1,"GMC",1,"6FX80022CT311AE6","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2DC10-1AA0","signal cable, pre-assembled type: 6FX8002-2DC10 DRIVE-CLiQ with 24 V plug RJ45 IP20 on module side and IP67 on motor side MOTION-CONNECT 800PLUS released only up to 75 m length Dmax=7.1 mm length (m)= +0 +0 +0 +0",171,"ST",1,"GMC",1,"6FX80022DC101AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2DC10-1AD5","signal cable, pre-assembled type: 6FX8002-2DC10 DRIVE-CLiQ with 24 V plug RJ45 IP20 on module side and IP67 on motor side MOTION-CONNECT 800PLUS released only up to 75 m length Dmax=7.1 mm length (m)= +0 +0 +3 +0.5",216,"ST",1,"GMC",1,"6FX80022DC101AD5","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2DC10-1BC5","signal cable, pre-assembled type: 6FX8002-2DC10 DRIVE-CLiQ with 24 V plug RJ45 IP20 on module side and IP67 on motor side MOTION-CONNECT 800PLUS released only up to 75 m length Dmax=7.1 mm length (m)= +0 +10 +2 +0.5",317,"ST",1,"GMC",1,"6FX80022DC101BC5","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2DC10-1CG0","signal cable, pre-assembled type: 6FX8002-2DC10 DRIVE-CLiQ with 24 V plug RJ45 IP20 on module side and IP67 on motor side MOTION-CONNECT 800PLUS released only up to 75 m length Dmax=7.1 mm length (m)= +0 +20 +6 +0",462,"ST",1,"GMC",1,"6FX80022DC101CG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2DC20-1AF4","Signal cable pre-assembled type: 6FX8002-2DC20 DRIVE-CLiQ with 24 V plug RJ45 IP67 on both sides released only up to 75 m length Dmax=7.1 mm length (m)= +0 +0 +5 +0.4",265,"ST",1,"GMC",1,"6FX80022DC201AF4","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2DC20-1BH5","Signal cable pre-assembled type: 6FX8002-2DC20 DRIVE-CLiQ with 24 V plug RJ45 IP67 on both sides released only up to 75 m length Dmax=7.1 mm length (m)= +0 +10 +7 +0.5",399,"ST",1,"GMC",1,"6FX80022DC201BH5","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2DC20-1DH0","Signal cable pre-assembled type: 6FX8002-2DC20 DRIVE-CLiQ with 24 V plug RJ45 IP67 on both sides released only up to 75 m length Dmax=7.1 mm length (m)= +0 +30 +7 +0",611,"ST",1,"GMC",1,"6FX80022DC201DH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2DC36-1DA0","Signal cable pre-assembled type: 6FX8002-2DC36 DRIVE-CLiQ with 24 V M12 female/ RJ45 IP67 MOTION-CONNECT 800PLUS UL/CSA, DESINA, Trailable Dmax=7.1 mm Length (m)=30",560,"ST",1,"GMC",1,"6FX80022DC361DA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2DC38-1BC0","DRIVE-CLiQ adapter cable pre-fabricated type: 6FX8002-2DC38 DRIVE-CLiQ with 24 V M12 male/ RJ45 IP67 MOTION-CONNECT 800PLUS MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=7.1 mm length (m)=12",349,"ST",1,"GMC",1,"6FX80022DC381BC0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2DC42-1AE1","Signal cable pre-assembled type: 6FX8002-2DC42 DRIVE-CLiQ with 24 V RJ45 IP67/M17 male Speed-connect-ready MOTION-CONNECT 800PLUS UL/CSA, DESINA, trailable Dmax=7.1 mm length (m)= +0 +0 +4 +0.1",285,"ST",1,"GMC",1,"6FX80022DC421AE1","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2DC46-1AK0","Signal cable pre-assembled type: 6FX8002-2DC46 DRIVE-CLiQ with 24 V M12 female/ M17 male speed-connect-ready MOTION-CONNECT 800PLUS UL/CSA, DESINA, Trailable Dmax=7.1 mm Length (m)=9",350,"ST",1,"GMC",1,"6FX80022DC461AK0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2DX30-1DF0","Signal cable pre-assembled DRIVE-CLiQ for SINAMICS S210 Connection: Encoder side: M12 8-pole female drive side: IX connector MOTION-CONNECT 800PLUS UL/CSA, DESINA Dmax=7.1 mm, Length(m)=35",581,"ST",1,"GMC",1,"6FX80022DX301DF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2EQ10-1AK5","Signal cable pre-assembled for absolute encoder EnDat integrated into the motor 3x (2x0.14) C+4x 0.14+2x0.5 +4x 0.22 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.8 mm Length (m)= TYPE: 6FX8002-2EQ10 LENGTH (M) = +0 +0 +9 +0.5",342,"ST",1,"GMC",1,"6FX80022EQ101AK5","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2EQ10-1BK0","Signal cable pre-assembled for absolute encoder EnDat integrated into the motor 3x (2x0.14) C+4x 0.14+2x0.5 +4x 0.22 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.8 mm Length (m)= TYPE: 6FX8002-2EQ10 LENGTH (M) = +0 +10 +9 +0",472,"ST",1,"GMC",1,"6FX80022EQ101BK0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2EQ14-1AB5","Signal cable extension for base 6FX8002-2EQ10-.... 3x (2x0.14) C+4x 0.14+2x0.5 +4x 0.22 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.8 mm Length (m)= TYPE: 6FX8002-2EQ14 LENGTH (M) = +0 +0 +1 +0.5",259,"ST",1,"GMC",1,"6FX80022EQ141AB5","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2EQ20-1BA0","Signal cable pre-assembled type: 6FX8002-2EQ20 for absolute encoder EnDat in motor AH20 with connector full thread M17 (3x 2x 0.14) C+4x 0.14+2x 0.5+4x 0.22 C MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.8 mm Length (m)= +0 +10 +0 +0",365,"ST",1,"GMC",1,"6FX80022EQ201BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2SL00-1AK0","Signal cable pre-assembled type: 6FX8002-2SL00 for temperature sensor 3x 2x 0.5+1x 1 C Motor terminals on M17 female VG MOTION-CONNECT 800PLUS UL/CSA, DESINA, Trailable Dmax=11 mm Length (m)= +0 +0 +9 +0",365,"ST",1,"GMC",1,"6FX80022SL001AK0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2SL02-1AG0","Signal cable pre-assembled type: 6FX8002-2SL02 for temperature sensor 3x 2x 0.5+1x 1 C Motor terminals on M17 female VG with screw coupling M20 (G) MOTION-CONNECT 800PLUS UL/CSA, DESINA, Trailable Dmax=11 mm Length (m)= +0 +0 +6 +0",411,"ST",1,"GMC",1,"6FX80022SL021AG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-4AA21-1AG7","Signal cable pre-assembled 840C/CSB I/O device 4x (2x0.18) C MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=6.7 mm Length (m)= TYPE: 6FX8002-4AA21 LENGTH (M) = +0 +0 +6 +0.7",167,"ST",1,"GMC",1,"6FX80024AA211AG7","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-4AA21-1DH0","Signal cable pre-assembled 840C/CSB I/O device 4x (2x0.18) C MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=6.7 mm Length (m)= TYPE: 6FX8002-4AA21 LENGTH (M) = +0 +30 +7 +0",416,"ST",1,"GMC",1,"6FX80024AA211DH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5CA05-1CB0","power cable extension 4x 1.5 C, connector Full-thread, size 1 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.5 mm, Length (m)= TYPE: 6FX8002-5CA05 LENGTH (M) = +0 +20 +1 +0",682,"ST",1,"GMC",1,"6FX80025CA051CB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5CA38-1AH0","power cable extension 4x 2.5 C Connector full thread Sz. 1.5 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=11 mm Length (m)= TYPE: 6FX8002-5CA38 LENGTH (M) = +0 +0 +7 +0",666,"ST",1,"GMC",1,"6FX80025CA381AH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5CA68-1AF8","power cable extension 4x 10 C Connector full thread Sz. 1.5 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=18.2 mm Length (m)= TYPE: 6FX8002-5CA68 LENGTH (M) = +0 +0 +5 +0.8",849,"ST",1,"GMC",1,"6FX80025CA681AF8","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5CF10-1AF5","Power cable pre-assembled type: 6FX8002-5CF10 4x 1.5 C, SPEED-CONNECT Sz. 1 for SINAMICS S120 Combi MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=9.5 mm, Length (m)= Dmax=9.5 mm, Length (m)= +0 +0 +5 +0.5",269,"ST",1,"GMC",1,"6FX80025CF101AF5","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5CG10-1BH5","Power cable pre-assembled 4x 1.5 C, SPEED-CONNECT Sz. 1 for SINAMICS S120 Power Module MOTION-CONNECT 800PLUS Trailable UL/CSA, DESINA Dmax=9.5 mm, Length (m)= TYPE: 6FX8002-5CG10 LENGTH (M) = +0 +10 +7 +0.5",483,"ST",1,"GMC",1,"6FX80025CG101BH5","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5CG10-2AA0","Power cable pre-assembled 4x 1.5 C, SPEED-CONNECT Sz. 1 for SINAMICS S120 Power Module MOTION-CONNECT 800PLUS Trailable UL/CSA, DESINA Dmax=9.5 mm, Length (m)= TYPE: 6FX8002-5CG10 LENGTH (M) = +100 +0 +0 +0",1875,"ST",1,"GMC",1,"6FX80025CG102AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5CG41-1DH0","Power cable pre-assembled type: 6FX8002-5CG41 4x 4 C Connector full thread Sz. 1.5 for SINAMICS S120 Power Module and Motor Module Booksize Compact MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=12.3 mm Length (m)= +0 +30 +7 +0",1213,"ST",1,"GMC",1,"6FX80025CG411DH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5CG52-1BC0","Power cable pre-assembled 4x 6 C SPEED-CONNECT connector Sz. 1.5 for SINAMICS S120 Power Module and Motor Mod. Booksize Compact MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=14.9 mm Length (m)= TYPE: 6FX8002-5CG52 LENGTH (M) = +0 +10 +2 +0",668,"ST",1,"GMC",1,"6FX80025CG521BC0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5CN05-1BB5","power cable extension 4x 1.5 C, SPEED-CONNECT Sz. 1 MOTION-CONNECT 800PLUS Trailable UL/CSA, DESINA Dmax=9.5 mm TYPE: 6FX8002-5CN05 LENGTH (M) = +0 +10 +1 +0.5",530,"ST",1,"GMC",1,"6FX80025CN051BB5","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5CN06-1DB0","Power cable pre-assembled TYPE 6FX8002-5CN06 4X1,5 C, SPEED-CONNECT SIZE 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=9.5 MM LENGTH (M) = +0 +30 +1 +0",712,"ST",1,"GMC",1,"6FX80025CN061DB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5CN16-1BE0","Power cable pre-assembled TYPE 6FX8002-5CN16 4X2.5 C CONNECTOR SPEED-CONNECT SIZE 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=11 MM LENGTH (M) = +0 +10 +4 +0",509,"ST",1,"GMC",1,"6FX80025CN161BE0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5CN36-1EF0","Power cable pre-assembled TYPE 6FX8002-5CN36 4X2.5 C CONNECTOR SPEED-CONNECT S. 1.5 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=11 MM LENGTH (M) = +0 +40 +5 +0",1090,"ST",1,"GMC",1,"6FX80025CN361EF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5CN46-1BF0","Power cable pre-assembled TYPE 6FX8002-5CN46 4X4 C CONNECTOR SPEED-CONNECT S. 1.5 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=12,3 MM LENGTH (M) = +0 +10 +5 +0",672,"ST",1,"GMC",1,"6FX80025CN461BF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5CN54-1CF0","Power cable pre-assembled 4x 6 C SPEED-CONNECT connector Sz. 1.5 Ring cable lugs on module side for SINAMICS S120 Motor Module MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=14.9 mm Length (m)= TYPE: 6FX8002-5CN54 LENGTH (M) = +0 +20 +5 +0",1116,"ST",1,"GMC",1,"6FX80025CN541CF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5CP16-1DA0","Power cable pre-assembled TYPE 6FX8002-5CP16 4x2.5C SCREW GLANDM32/ 1PH810. FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=11 MM LENGTH (M) = +0 +30 +0 +0",761,"ST",1,"GMC",1,"6FX80025CP161DA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5CQ28-1BA0","power cable extension 4x 1.5 C, SPEED-CONNECT Sz. 1.5 MOTION-CONNECT 800PLUS Trailable UL/CSA, DESINA Dmax=9.5 mm, Length (m)= TYPE: 6FX8002-5CQ28 LENGTH (M) = +0 +10 +0 +0",694,"ST",1,"GMC",1,"6FX80025CQ281BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5CQ58-1BA0","power cable extension 4x 6 C SPEED-CONNECT connector Sz. 1.5 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=14.9 mm Length (m)= TYPE: 6FX8002-5CQ58 LENGTH (M) = +0 +10 +0 +0",853,"ST",1,"GMC",1,"6FX80025CQ581BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5CR42-1BD0","Power cable pre-assembled type: 6FX8002-5CR42 4x 10 C, M40 screw connection SINAMICS S120 Power Module MOTION-CONNECT 800 trailable, UL/CSA, DESINA Dmax=19.4 mm, Length (m)= +0 +10 +3 +0",860,"ST",1,"GMC",1,"6FX80025CR421BD0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5CR43-1BE0","Power cable pre-assembled type: 6FX8002-5CR43 4x 10 C, M50 screw connection SINAMICS S120 Power Module MOTION-CONNECT 800 trailable, UL/CSA, DESINA Dmax=19.4 mm, Length (m)= +0 +10 +4 +0",1006,"ST",1,"GMC",1,"6FX80025CR431BE0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5CR53-1DA0","Power cable pre-assembled type: 6FX8002-5CR53 4x 16 C Screw connection M50/1PH813 for SINAMICS S120, with bare core ends at module side MOTION-CONNECT 800PLUS Dmax=22.3 mm Length (m)= +0 +30 +0 +0",2175,"ST",1,"GMC",1,"6FX80025CR531DA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5CS16-1AK0","Power cable pre-assembled TYPE 6FX8002-5CS16 4X2.5 C, CONN. FULL THREAD S. 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=11 MM LENGTH (M) = +0 +0 +9 +0",428,"ST",1,"GMC",1,"6FX80025CS161AK0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5CS23-1CC0","Power cable pre-assembled type: 6FX8002-5CS23 4x 16 C Connector full thread Sz. 3 for SINAMICS S120 Motor Module Booksize MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=22.3 mm Length (m)= +0 +20 +2 +0",2235,"ST",1,"GMC",1,"6FX80025CS231CC0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5CS46-1AJ0","Power cable pre-assembled TYPE 6FX8002-5CS46 4X4C, CONN. FULL THREAD S. 1.5 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=12.3 MM LENGTH (M) = +0 +0 +8 +0",527,"ST",1,"GMC",1,"6FX80025CS461AJ0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5CS54-1BH0","Power cable pre-assembled type: 6FX8002-5CS54 4x 6 C Connector full thread Sz. 1.5 Ring cable lugs on module side for SINAMICS S120 Motor Module MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=14.9 mm Length (m)= +0 +10 +7 +0",857,"ST",1,"GMC",1,"6FX80025CS541BH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5CS64-1AG0","Power cable pre-assembled type: 6FX8002-5CS64 (1FT/1FK/1PH for SINAMICS) 4x 10 C, Connector Sz. 1.5/ Ring cable lug UL/CSA DESINA, Trailable MOTION-CONNECT 800 Dmax=18.4 mm, Length (m)= +0 +0 +6 +0",594,"ST",1,"GMC",1,"6FX80025CS641AG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DA05-1AB5","power cable extension 4x 1.5+(2x1.5) C, connector Full-thread, size 1 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=12 mm, LONGUEUR (m)= TYPE: 6FX8002-5DA05 LENGTH (M) = +0 +0 +1 +0.5",389,"ST",1,"GMC",1,"6FX80025DA051AB5","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DA15-1BB0","power cable extension 4x 2.5+(2x1.5) C C MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=13.8 mm Length (m)= TYPE: 6FX8002-5DA15 LENGTH (M) = +0 +10 +1 +0",628,"ST",1,"GMC",1,"6FX80025DA151BB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DA28-1AJ7","power cable extension 4x 1.5+(2x1.5) C, connector Full thread Sz. 1.5 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=12 mm, LONGUEUR (m)= TYPE: 6FX8002-5DA28 LENGTH (M) = +0 +0 +8 +0.7",739,"ST",1,"GMC",1,"6FX80025DA281AJ7","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DA48-1AK5","power cable extension 4x 4+(2x1.5) C, Connector Sz. 1.5 Connector full thread Sz. 1.5 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=15.2 mm LÃ¤nge (m)= TYPE: 6FX8002-5DA48 LENGTH (M) = +0 +0 +9 +0.5",854,"ST",1,"GMC",1,"6FX80025DA481AK5","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DA58-1AJ5","power cable, pre-assembled Extension 4x 6+(2x1.5) C C Connector full thread Sz. 1.5 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=17.3 mm LÃ¤nge (m)= TYPE: 6FX8002-5DA58 LENGTH (M) = +0 +0 +8 +0.5",920,"ST",1,"GMC",1,"6FX80025DA581AJ5","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DA68-1BA0","power cable extension 4x 10+(2x1.5) C C Connector full thread Sz. 1.5 for SIMODRIVE/MASTERDRIVES MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=20.1 mm LÃ¤nge (m)= TYPE: 6FX8002-5DA68 LENGTH (M) = +0 +10 +0 +0",1146,"ST",1,"GMC",1,"6FX80025DA681BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DG10-1AD0","Power cable pre-assembled 4x 1.5+(2x1.5) C C, connector SPEED-CONNECT Sz. 1 for SINAMICS S120 Power Module MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=12 mm, Length (m)= TYPE: 6FX8002-5DG10 LENGTH (M) = +0 +0 +3 +0",272,"ST",1,"GMC",1,"6FX80025DG101AD0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DG11-1DA0","Power cable pre-assembled type: 6FX8002-5DG11 4x 2.5+(2x1.5) C C Connector full thread Sz. 1 for SINAMICS S120 Power Module and Motor Mod. Booksize Compact MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=13.8 mm Length (m)= +0 +30 +0 +0",972,"ST",1,"GMC",1,"6FX80025DG111DA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DG31-1CA0","Power cable pre-assembled type: 6FX8002-5DG31 4x 2.5+(2x1.5) C C Connector full thread Sz. 1.5 for SINAMICS S120 Power Module and Motor Mod. Booksize Compact MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=13.8 mm Length (m)= +0 +20 +0 +0",817,"ST",1,"GMC",1,"6FX80025DG311CA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DG33-1BA0","Power cable pre-assembled type: 6FX8002-5DG33 4x 25+(2x1.5) C C Connector full thread Sz. 3 Core end cut off Length 300 mm for SINAMICS S120 Motor Module and power modules MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=27.6 mm Accessory kit: 4x cable lugs M8 1x cable lugs M6 1x spring-loaded terminal +0 +10 +0 +0",2727,"ST",1,"GMC",1,"6FX80025DG331BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DG51-1EA0","Power cable pre-assembled type: 6FX8002-5DG51 4x 6+(2x1.5) C C Connector full thread Sz. 1.5 for SINAMICS S120 Power Module and Motor Mod. Booksize Compact MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=17.3 mm Length (m)= +0 +40 +0 +0",1874,"ST",1,"GMC",1,"6FX80025DG511EA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DG62-1BA0","Power cable pre-assembled 4x 10+(2x1.5) C C SPEED-CONNECT connector Sz. 1.5 for SINAMICS S120 Power Module and Motor Mod. Booksize Compact MOTION-CONNECT 800PLUS Trailable UL/CSA, DESINA Dmax=20.1 mm LÃ¤nge (m)= TYPE: 6FX8002-5DG62 LENGTH (M) = +0 +10 +0 +0",1014,"ST",1,"GMC",1,"6FX80025DG621BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DN05-1BB5","power cable extension 4x 1.5+(2x1.5) C C, connector SPEED-CONNECT Sz. 1 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=12 mm, Length (m)= TYPE: 6FX8002-5DN05 LENGTH (M) = +0 +10 +1 +0.5",610,"ST",1,"GMC",1,"6FX80025DN051BB5","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DN06-1BD3","Power cable pre-assembled TYPE 6FX8002-5DN06 4X1,5 , (2X1.5)C C CONNECTOR SPEED-CONNECT SIZE 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=12 MM LENGTH (M) = +0 +10 +3 + 0.3",553,"ST",1,"GMC",1,"6FX80025DN061BD3","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DN16-1EA0","Power cable pre-assembled TYPE 6FX8002-5DN16 4X2.5 , (2X1.5)C C CONNECTOR SPEED-CONNECT SIZE 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=13.8 MM LENGTH (M) = +0 +40 +0 +0",1142,"ST",1,"GMC",1,"6FX80025DN161EA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DN27-1BC0","Power cable pre-assembled TYPE 6FX8002-5DN27 4X1.5, (2X1.5)C C CONNECTOR SPEED-CONNECT S. 0.5 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX = 12 MM LENGTH (M) = +0 +10 +2 +0",484,"ST",1,"GMC",1,"6FX80025DN271BC0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DN30-1CF0","Power cable pre-assembled 4x 1.5+(2x1.5) C C, connector SPEED-CONNECT Sz. 0.5 for SINAMICS S120 Power Module and Motor Module Booksize Compact MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=12 mm, Length (m)= TYPE: 6FX8002-5DN30 LENGTH (M) = +0 +20 +5 +0",808,"ST",1,"GMC",1,"6FX80025DN301CF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DN54-1AH0","Power cable pre-assembled 4x 6+(2x1.5) C C SPEED-CONNECT connector Sz. 1.5 Ring cable lugs on module side for SINAMICS S120 Motor Module MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=17.3 mm LÃ¤nge (m)= TYPE: 6FX8002-5DN54 LENGTH (M) = +0 +0 +7 +0",604,"ST",1,"GMC",1,"6FX80025DN541AH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DN56-1BB0","Power cable pre-assembled TYPE 6FX8002-5DN56 4X6 , (2X1.5)C C CONNECTOR SPEED-CONNECT S. 1.5 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=17.3 MM LENGTH (M) = +0 +10 +1 +0",738,"ST",1,"GMC",1,"6FX80025DN561BB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DQ15-1CA0","power cable extension 4x 2.5+(2x1.5) C C SPEED-CONNECT connector Sz. 1 MOTION-CONNECT 800PLUS trailable; UL/CSA DESINA Dmax=13.8 mm Length (m)= TYPE: 6FX8002-5DQ15 LENGTH (M) = +0 +20 +0 +0",858,"ST",1,"GMC",1,"6FX80025DQ151CA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DQ38-1BC0","power cable extension 4x 2.5+(2x1.5) C C SPEED-CONNECT connector Sz. 1.5 MOTION-CONNECT 800PLUS Trailable UL/CSA, DESINA Dmax=13.9 mm Length (m)= TYPE: 6FX8002-5DQ38 LENGTH (M) = +0 +10 +2 +0",852,"ST",1,"GMC",1,"6FX80025DQ381BC0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DQ48-1CK0","power cable extension 4x 4+(2x1.5) C C SPEED-CONNECT connector Sz. 1.5 MOTION-CONNECT 800PLUS Trailable UL/CSA, DESINA Dmax=15.2 mm LÃ¤nge (m)= TYPE: 6FX8002-5DQ48 LENGTH (M) = +0 +20 +9 +0",1438,"ST",1,"GMC",1,"6FX80025DQ481CK0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DS06-1FA0","Power cable pre-assembled TYPE 6FX8002-5DS06 4X1,5 , (2X1.5)C C CONNECTOR FULL THREAD SIZE 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=12 MM LENGTH (M) = +0 +50 +0 +0",1207,"ST",1,"GMC",1,"6FX80025DS061FA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DS14-1CA0","Power cable pre-assembled type: 6FX8002-5DS14 4x 10+(2x1.5) C C Connector full thread Sz. 3 for SINAMICS S120 Motor Module Booksize MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=20.1 mm LÃ¤nge (m)= +0 +20 +0 +0",1702,"ST",1,"GMC",1,"6FX80025DS141CA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DS23-1CD0","Power cable pre-assembled type: 6FX8002-5DS23 4x 16+(2x1.5) C C Connector full thread Sz. 3 Ring cable lugs on module side for SINAMICS S120 Motor Module MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=23.8 mm Length (m)= +0 +20 +3 +0",2736,"ST",1,"GMC",1,"6FX80025DS231CD0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DS36-1BF0","Power cable pre-assembled TYPE 6FX8002-5DS36 4X2.5 , (2X1.5)C C, CONNECTOR FULL THREAD SIZE 1.5 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=13.8 MM LENGTH (M) = +0 +10 +5 +0",695,"ST",1,"GMC",1,"6FX80025DS361BF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DS64-1BG0","Power cable pre-assembled type: 6FX8002-5DS64 4x 10+(2x1.5) C C Connector full thread Sz. 1.5 for SINAMICS S120 Motor Module Booksize Ring cable lug on module side MOTION-CONNECT 800PLUS trailable, UL/CSA DESINA Dmax=20.1 mm LÃ¤nge (m)= +0 +10 +6 +0",1268,"ST",1,"GMC",1,"6FX80025DS641BG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DX28-1BE0","power cable extension 4x 16+(2x1.5) C C Connector full thread Sz. 3 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=23.8 mm Length (m)= TYPE: 6FX8002-5DX28 LENGTH (M) = +0 +10 +4 +0",3391,"ST",1,"GMC",1,"6FX80025DX281BE0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DX48-1AC0","power cable, pre-assembled Extension 4x 35+(2x1.5) C, Connector size 3 (1FT/1FK to 611/810D/SIMOVERT) trailable UL/CSA DESINA MOTION-CONNECT 800 Dmax=32.0 mm TYPE: 6FX8002-5DX48 LENGTH (M) = +0 +0 +2 +0",3245,"ST",1,"GMC",1,"6FX80025DX481AC0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DX48-1CC0","power cable, pre-assembled Extension 4x 35+(2x1.5) C, Connector size 3 (1FT/1FK to 611/810D/SIMOVERT) trailable UL/CSA DESINA MOTION-CONNECT 800 Dmax=32.0 mm TYPE: 6FX8002-5DX48 LENGTH (M) = +0 +20 +2 +0",6535,"ST",1,"GMC",1,"6FX80025DX481CC0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5YQ35-1AB0","Power cable pre-assembled type: 6FX8002-5YQ35 Customer-specific Length (m)= +0 +0 +1 +0",341,"ST",1,"GMC",1,"6FX80025YQ351AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5YT05-1BF0","Power cable pre-assembled type: 6FX8002-5YT05 Customer-specific Length (m)=15",1179,"ST",1,"GMC",1,"6FX80025YT051BF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-7HY00-1DK5","Pre-assembled hybrid cable type: 6FX8002-7HY00 Power and DRIVE-CLiQ Outlet direction NDE/NDE for SINAMICS S120M MOTION-CONNECT 800PLUS Trailing type, UL/CSA DESINA Dmax=15 mm, Length (m)= +0 +30 +9 +0.5",1787,"ST",1,"GMC",1,"6FX80027HY001DK5","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-7HY11-1DD0","Pre-assembled hybrid cable type: 6FX8002-7HY11 Power and DRIVE-CLiQ Outlet direction NDE/DE for SINAMICS S120M MOTION-CONNECT 800PLUS Trailing type, UL/CSA DESINA Dmax=15 mm, Length (m)= +0 +30 +3 +0",1564,"ST",1,"GMC",1,"6FX80027HY111DD0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-7HY22-1CE7","Pre-assembled hybrid cable type: 6FX8002-7HY22 Power and DRIVE-CLiQ Outlet direction DE/DE for SINAMICS S120M MOTION-CONNECT 800PLUS Trailing type, UL/CSA DESINA Dmax=15 mm, Length (m)= +0 +20 +4 +0.7",1309,"ST",1,"GMC",1,"6FX80027HY221CE7","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-8QE04-1AH0","Single cable extension 4G0.38+2x0.38+4x0.2 C Socket and plug Speed-Connect M12 female / M12 male UL/CSA DESINA Motion-Connect 800PLUS Dmax= 9.7 mm, length (m)= +0 +0 +7 +0",381,"ST",1,"GMC",1,"6FX80028QE041AH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-8QE21-1AG0","Single cable extension 4G2.5+1Q0,2STC+1P1.5C-C SPEED-CONNECT M23 connector UL/CSA DESINA MOTION-CONNECT 800PLUS Dmax.=13.3 mm Length (m)= +0 +0 +6 +0",728,"ST",1,"GMC",1,"6FX80028QE211AG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-8QN04-1CD0","Single cable prefabricated 4G0.38+2x0.38+4x0.2 C SPEED-CONNECT M12 connector Cores with end sleeve Data cable with IX connector UL/CSA DESINA MOTION-CONNECT 800PLUS Dmax.=9.7 mm, length(m)= +0 +20 +3 +0",699,"ST",1,"GMC",1,"6FX80028QN041CD0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-8QN11-1BD0","Single cable pre-assembled 4G1,5+1Q0,2STC+1P1,5C-C SPEED-CONNECT connector M23 Wires with end sleeve Data cable with IX connector UL/CSA DESINA MOTION-CONNECT 800PLUS Dmax.=12.3 mm length(M)= +0 +10 +3 +0",683,"ST",1,"GMC",1,"6FX80028QN111BD0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8008-1BA11-6AA0","Power cable sold by the meter type: 6FX8008-1BA11 4x 1.5+(2x1.5) C C MOTION-CONNECT 800PLUS trailable, UL/CSA DESINA Dmax=12 mm Type of delivery: Disposable drum Length (m)=500",11972,"ST",1,"GMC",1,"6FX80081BA116AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8008-1BA25-1CD0","Power cable sold by the meter type: 6FX8008-1BA25 4x 25+(2x1.5) C C MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=27.6 mm Type of delivery: up to 19 m ring from 20 m drum Length (m)= +0 +20 +3 +0",3276,"ST",1,"GMC",1,"6FX80081BA251CD0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8008-1BA50-1CA0","Power cable sold by the meter type: 6FX8008-1BA50 4x 50+(2x1.5) C C MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=35 mm Type of delivery: to 9 m ring from 10 m drum Length (m)= +0 +20 +0 +0",5067,"ST",1,"GMC",1,"6FX80081BA501CA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8008-1BA50-1GA0","Power cable sold by the meter type: 6FX8008-1BA50 4x 50+(2x1.5) C C MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=35 mm Type of delivery: to 9 m ring from 10 m drum Length (m)= +0 +60 +0 +0",15150,"ST",1,"GMC",1,"6FX80081BA501GA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8008-1BB31-1BA0","Power cable sold by the meter type: 6FX8008-1BB31 4x 4 C MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=12.3 mm Type of delivery: to 99 m ring from 100 m disposable drum Length (m)= +0 +10 +0 +0",291,"ST",1,"GMC",1,"6FX80081BB311BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8008-1BB51-1BB0","Power cable sold by the meter type: 6FX8008-1BB51 4x 10.0 C trailable UL/CSA DESINA MOTION-CONNECT 800PLUS Type of delivery: Disposable drum Dmax=18.2 mm, Length (m)= +0 +10 +1 +0",552,"ST",1,"GMC",1,"6FX80081BB511BB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8008-1BD11-1FA0","Signal cable sold by the meter type: 6FX8008-1BD11 8x (2x0.18) C MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=8.2 mm Type of delivery: Ring Length (m)=50",872,"ST",1,"GMC",1,"6FX80081BD111FA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8008-2DC00-1BA0","Signal cable sold by the meter Type: 6FX8008-2DC00 (DRIVE-CLiQ) 2x2x0.15+2x0.38 C, Trailable UL/CSA DESINA MOTION-CONNECT 800, Type of delivery: ring Dmax=7.0 mm, length (M)=10",173,"ST",1,"GMC",1,"6FX80082DC001BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8012-2CA31-1AG6","Signal cable pre-assembled for incr. encoder with C/D tracks integrated into the motor 3x (2x0.14) C+4x 0.14+2x0.5 +4x 0.22 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.8 mm Length (m)= TYPE: 6FX8012-2CA31 MODULE SIDE: CRIMPED CONTACTS, CONNECTOR HOUSING INCLUDED LENGTH (M) = +0 +0 +6 +0.6",299,"ST",1,"GMC",1,"6FX80122CA311AG6","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8012-2EQ10-1BJ0","Signal cable pre-assembled for absolute encoder EnDat integrated into the motor 3x (2x0.14) C+4x 0.14+2x0.5 +4x 0.22 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.8 mm Length (m)= TYPE: 6FX8012-2EQ10 MODULE SIDE: CRIMPED CONTACTS, CONNECTOR HOUSING INCLUDED LENGTH (M) = +0 +10 +8 +0",458,"ST",1,"GMC",1,"6FX80122EQ101BJ0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8012-5CN06-1CA0","Power cable pre-assembled TYPE 6FX8012-5CN06 4X1,5 C, SPEED-CONNECT SIZE 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES PREPARED CONDUCTORS, SINAMICS CONNECTOR INCLUDED MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=9.5 MM LENGTH (M) = +0 +20 +0 +0",559,"ST",1,"GMC",1,"6FX80125CN061CA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8012-5CS36-1BF0","Power cable pre-assembled TYPE 6FX8012-5CS36 4X2.5C, CONN. FULL THR. S. 1.5 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES PREPARED CONDUCTORS, SINAMICS CONNECTOR INCLUDED MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=11 MM LENGTH (M) = +0 +10 +5 +0",602,"ST",1,"GMC",1,"6FX80125CS361BF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8012-5DN05-1BC6","power cable extension 4x 1.5+(2x1.5) C C, connector SPEED-CONNECT Sz. 1 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=12 mm, Length (m)= TYPE: 6FX8012-5DN05 MODULE SIDE: CRIMPED CONTACTS, CONNECTOR HOUSING INCLUDED LENGTH (M) = +0 +10 +2 +0.6",632,"ST",1,"GMC",1,"6FX80125DN051BC6","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8012-5DN46-1BB5","Power cable pre-assembled TYPE 6FX8012-5DN46 4X4, (2X1.5)C C CONNECTOR SPEED-CONNECT S 1.5 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES PREPARED CONDUCTORS, SINAMICS CONNECTOR INCLUDED MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=15.2 MM LENGTH (M) = +0 +10 +1 + 0.5",685,"ST",1,"GMC",1,"6FX80125DN461BB5","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8012-5DN56-2AA0","Power cable pre-assembled TYPE 6FX8012-5DN56 4X6 , (2X1.5)C C CONNECTOR SPEED-CONNECT S 1.5 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES PREPARED CONDUCTORS, SINAMICS CONNECTOR INCLUDED MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=17.3 MM LENGTH (M) = +100 +0 +0 +0",3580,"ST",1,"GMC",1,"6FX80125DN562AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8022-5CS06-1CE5","Power cable pre-assembled TYPE 6FX8022-5CS06 4X1,5 C, FULL THREAD SIZE 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES PREPARED CONDUCTORS, W/O SINAMICS CONNECTOR MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=9.5 MM LENGTH (M) = +0 +20 +4 + 0.5",588,"ST",1,"GMC",1,"6FX80225CS061CE5","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8022-5CS16-1AG0","Power cable pre-assembled TYPE 6FX8022-5CS16 4X2.5 C, CONN. FULL THREAD S. 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES PREPARED CONDUCTORS, W/O SINAMICS CONNECTOR MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=11 MM +0 +0 +6 +0",338,"ST",1,"GMC",1,"6FX80225CS161AG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8042-2CA80-1CF0","Signal cable pre-assembled type: 6FX8042-2CA80 (incr. encoder ECOSpindle) Basis 2CA31; trailable UL/CSA DESINA MOTION-CONNECT 800 Motor side: contacts crimped Connector housing enclosed Length (m)= +0 +20 +5 +0",565,"ST",1,"GMC",1,"6FX80422CA801CF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6GF3540-8AC41","MV500 protective lens barrel IR degree of protection IP67 for MV500 devices face plate: IR /glass enclosure: metal for lens length without/with built-in ring light 48.5 mm/23.9 mm for lens width without/with built-in ring light 60.4 mm/41.6 mm suitable for lenses (MLFB): 6GF9001-1BL01,..-1BF01, ...- 1BG01 ,...- 1BH01,...- 1BJ01 6GF3540-8EA03-0LL0; suitable luminaires (MLFB): 6GF3540-8DA33, â€¦8DA41, â€¦8D42; WxHxD (outer, mm) 65x65x65 scope of delivery: protective barrel with mounted O-ring and pane;",718,"ΤΕΜ",1,"SIMATIC",1,"6GF35408AC41","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6GK1571-1AA00-0AH0","DIN rail support for communications processor CP 5711, rack unit for CP 5711 enclosure; Mechanical Mounting on 35 mm DIN rail .",65.599999999999994,"ΤΕΜ",1,"SIMATIC",1,"6GK15711AA000AH0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6GK1704-1CW23-0AK1","PowerPack SOFTNET-IE S7 V19 extension SOFTNET-IE S7 Lean to SOFTNET-IE S7 V19; floating license; license key for download; class A; 3 languages (de, en, zh-CHS); for WindowsÂ® 10 Professional/Enterprise version 21H2, 22H2; WindowsÂ® 11 Professional/Enterprise version 21H2, 22H2; WindowsÂ® Server 2019, 2022 (Standard Edition, Datacenter); WindowsÂ® 10(IoT) Enterprise 2019 LTSC WindowsÂ® 10(IoT) Enterprise 2021 LTSC",972,"TEM",1,"SIMATIC",1,"6GK17041CW230AK1","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6GK1706-1NW00-3AP0","Industrial Ethernet SNMP OPC Server Basic software Update service download for 1 year with automatic extension Requirement: current Software version.",604,"ΤΕΜ",1,"SIMATIC",1,"6GK17061NW003AP0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6GK1713-5CB17-0AA0","HARDNET-PB S7 V17 SP1 software for S7 communication including PG, FDL OPC server and configuration software; floating license R-SW, software + electronic manual on DVD; license key on USB flash drive, class A; 2 languages (de, en) for WindowsÂ® 10 Professional/Enterprise (64 bit) version 1909, 2004, 20H2; WindowsÂ® Server 2016 (Standard Edition, Datacenter); WindowsÂ® Server 2019 (Standard Edition, Enterprise) WindowsÂ® 10(IoT) Enterprise 2016 LTSB WindowsÂ® 10(IoT) Enterprise 2019 LTSC .",713,"ΤΕΜ",1,"SIMATIC",1,"6GK17135CB170AA0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6GK1716-1CB18-0AA0","SIMATIC NET HARDNET-IE S7 V18 SW for S7-, open communication,: OPC, PG/OP communication, configuration software; up to 120 connections; floating license R-SW, software + electronic manual; license key on USB flash drive; class A; 3 languages (de, en, zh-CHS); for WindowsÂ® 10 Professional/Enterprise version 21H2, 22H2; WindowsÂ® 11 Professional/Enterprise version 21H2, 22H2; WindowsÂ® Server 2016, 2019, 2022 (Standard Edition, Datacenter); WindowsÂ® 10(IoT) Enterprise 2016 LTSB WindowsÂ® 10(IoT) Enterprise 2019 LTSC WindowsÂ® 10(IoT)(*)",1585,"ΤΕΜ",1,"SIMATIC",1,"6GK17161CB180AA0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6GK1901-1BB30-0AA0","Industrial Ethernet FastConnect RJ45 plug 145 2x 2, RJ45 plug-in connector (10/100 Mbit/s) with rugged metal enclosure and FC connection system, for IE FC TP cable 2x 2; 145Â° cable outlet 1 pack = 1 unit.",21,"ΤΕΜ",1,"SIMATIC",1,"6GK19011BB300AA0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6GK1905-6PB00","PROFIBUS Plastic Fiber Optic, BFOC crimping tool.",510,"ΤΕΜ",1,"SIMATIC",1,"6GK19056PB00","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6GK5204-2BC00-2AF2","SCALANCE XF204-2, flat, Managed IE switch, 4x 10/100 Mbit/s RJ45 ports, 2x 100 Mbit/s FO ports, Error signaling contact with set pushbutton, redundant power supply, PROFINET IO device, network management, Redundancy Manager integrated, incl. electron. manual on CD-ROM, C-PLUG optional.",1218,"ΤΕΜ",1,"SIMATIC",1,"6GK52042BC002AF2","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6GK5206-2GS00-2AC2","SCALANCE XC206-2SFP G manageable Layer 2 IE switch; IEC 62443-4-2 certified; 6x 10/100/1000 Mbps RJ45 ports; 2x 1000 Mbps SFP; 1x console port; diagnostics LED; redundant power supply; temperature range -40 Â°C to +70 Â°C; assembly: DIN rail/S7 mounting rail/wall; redundancy functions; office features (RSTP, VLAN,...); PROFINET IO device; Ethernet/IP-compliant; C-PLUG slot; IEEE 1588v2 PTP",1069,"ΤΕΜ",1,"SIMATIC",1,"6GK52062GS002AC2","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6GK5224-4GS00-2FC2","SCALANCE XC224-4C G EEC managed Layer 2 IE switch; IEC 62443-4-2 certified; Full Gigabit; 20x 10/100/1000 Mbps RJ45 ports; 4x 1000 Mbps combo ports (either 1000 Mbps/ SFPs or 10/100/1000 Mbps RJ45 ports can be used); 1x console port; diagnostics LED; redundant power supply; with painted printed circuit boards NAMUR NE21-compliant; temp. range -40 Â°C to +70 Â°C; mounting: DIN rail/S7 mounting rail/wall; redundancy functions; Office features (RSTP, VLAN,â€¦); PROFINET IO device; Ethernet/IP-compliant;",3031,"ΤΕΜ",1,"SIMATIC",1,"6GK52244GS002FC2","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6GK5534-5TR00-4AR3","SCALANCE XR502-32; managed layer 3 IE switch, 19\" rack; 2x 1G/2.5G/5G/10 Gbps RJ45 port 24x 100M/1G SFP port; 8x 1G/10G SFP+ port; LED diagnostics; error signaling contact; select/ set button; PROFINET I/O device; network management; integrated redundancy manager; office; features (RSTP, VLAN, IGMP,..); CLP included in scope of supply; power supply 2x 230 V AC",5740,"ΤΕΜ",1,"SIMATIC",1,"6GK55345TR004AR3","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6GK5795-4MA00-0AA3","ANT795-4MA IWLAN antenna with omnidirectional Characteristic, Radially rotatable, with additional joint, incl. RSMA connector: 3/5 dBi, IP30 (-20-+60 Â°C), 2.4/5 GHz; Wi-Fi compliance and Observe national approvals; Direct mounting on SCALANCE W with RSMA connection system; scope of delivery: 1x ANT795-4MA, compact instructions as hard copy German/English.",36.700000000000003,"ΤΕΜ",1,"SIMATIC",1,"6GK57954MA000AA3","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6GK5896-4MA00-0AA3","ANT896-4MA mobile wireless antenna for GSM (2G), UMTS (3G) and LTE(4G) networks; Omnidirectional Characteristic, Radially rotatable, with additional joint, Antenna gain: 2 dBi, incl. SMA plug, IP54, (-40-+85 Â°C), observe national approvals; for direct installation with SMA connection system; scope of delivery: 1x ANT 896-4MA, compact instructions as hard copy German/English.",50.2,"ΤΕΜ",1,"SIMATIC",1,"6GK58964MA000AA3","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6GK5908-0PB00","KEY-PLUG SINEMA RC, Removable data storage medium for enabling of the connection to SINEMA Remote Connect for S615 and SCALANCE M for simple device replacement in event of fault and for Recording of configuration data.",162,"ΤΕΜ",1,"SIMATIC",1,"6GK59080PB00","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6GK6000-8CG01-1BA0","RUGGEDCOM MDEDIA MODULE Gigabit Copper Media Module 1CG01 (1x10/100/1000TX RJ45). Only for RSG2100. Equivalent to 1CG01",432,"ΤΕΜ",1,"SIMATIC",1,"6GK60008CG011BA0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6GK6000-8FE60-1AA0","RUGGEDCOM Accessory, SFP with active transceiver, 1 X 100MBIT/S, 100BASE-LX, LC-Interface, Optical: Single-mode Fiber Optic up to max. 10km, 1310nm, -40...+85 Degrees Celcius.",314,"ΤΕΜ",1,"SIMATIC",1,"6GK60008FE601AA0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6GK6000-8FG54-2EA1","Media Module for RUGGEDCOM RSG 2488, 2 x SFP-slot, Optical: E quipped with 2 x SFP1132-1LX70 , 1000Mbit/s, Single Mode fibe r optic up to 70 kilometer, 15 50nm with Conformal Coating",3596,"ΤΕΜ",1,"SIMATIC",1,"6GK60008FG542EA1","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6GK6000-8FX06-2CA0","Media Module for RUGGEDCOM RSG2200, RSG2288, RSG2300, and RSG2300P, 2 x 100MBit/s LC-interface, Optical: 100BASE-FX, Single Mode fiber optic up to 20 kilometer, 1310nm (FXA06). Requires the in-field modification kit, 6GK6000-1BC50-0AA1.",980,"ΤΕΜ",1,"SIMATIC",1,"6GK60008FX062CA0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6GK6000-8MK12-1EA0","RUGGEDCOM MOUNTING KIT RSG2488 DP Equivalent to DP, DIN and Panel Mount Kit for RSG2488",101,"ΤΕΜ",1,"SIMATIC",1,"6GK60008MK121EA0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6GK6000-8NT01-0AA0","Mobile radio antenna with omnidirectional characteristics for GSM (2G), UMTS (3G) and LTE(4G), for direct mounting with SMA connector, radially rotatable with additional joint, antenna gain 2 dBi,  -40 to +75 Â°C",68.399999999999991,"ΤΕΜ",1,"SIMATIC",1,"6GK60008NT010AA0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6GK6015-0AL20-0FC1","RUGGEDCOM RX1500PN LM CG01 Line Module 2 x 10/100/1000 TX RJ45 Conformal Coating",672,"ΤΕΜ",1,"SIMATIC",1,"6GK60150AL200FC1","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6GK6015-0AL20-0LB1","RUGGEDCOM RX1500PN LM D02 Line Module 56K Master/Slave, 64K Slave DDS Conformal Coating non-RoHS",1176,"ΤΕΜ",1,"SIMATIC",1,"6GK60150AL200LB1","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6GK6050-0AB00-0AP0","RUGGEDCOM RX5000 empty chassis: Rack Rear Mount, Fan Controller and Power Blocks on Front Panel",5746,"ΤΕΜ",1,"SIMATIC",1,"6GK60500AB000AP0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6GK6050-0AR00-8SM0","RUGGEDCOM REPN-8FSM1 8 x Single Mode Military Circular Fiber Connectors with LC connectors",11637,"ΤΕΜ",1,"SIMATIC",1,"6GK60500AR008SM0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6GK6490-7RB00-3CN0","RUGGEDCOM RSG907R is a 7 port industrially hardened, fully managed Ethernet switch featuring an integrated HSR/PRP RedBox for use in harsh industrial environments. The product has 3x 1Gbit/s SFP slots and 4x 100Mbit/s multimode LC ports (max 2km). -40Â°C to +85Â°C operating temperature (fanless). . . DIN Rail and Panel HI . none",3056,"ΤΕΜ",1,"SIMATIC",1,"6GK64907RB003CN0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6GK7277-1AA10-0AA0","Compact Switch Module CSM 1277 for connecting SIMATIC S7-1200 and up to 3 further nodes to Industrial Ethernet with 10/100 Mbit/s; unmanaged switch, 4 RJ45 ports, ext. 24 V DC power supply LED diagnostics, S7-1200 module incl. electronic Equipment Manual on CD-ROM.",202,"ΤΕΜ",1,"SIMATIC",1,"6GK72771AA100AA0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6GK8751-1UA01-0BA0","SINEC INS Basic 1000 DVD Type of delivery DVD network Services for management of industrial networks, RADIUS, syslog, NTP, DHCP, TFTP, SFTP, DNS Server, license type single monitorable IP devices 1000 DVD: USB stick;",3909,"ΤΕΜ",1,"SIMATIC",1,"6GK87511UA010BA0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6GT2090-4AT12","RFID systems connecting cable ASM reader without connector, loose PUR, trailing, 120 m.",577,"ΤΕΜ",1,"SIMATIC",1,"6GT20904AT12","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6GT2390-0AA00","MOBY D/E/RF600; Support for MDS D100, D200/MDS E600/ RF610T.",3.1,"ΤΕΜ",1,"SIMATIC",50,"6GT23900AA00","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6GT2700-6DE33","SIMATIC RTLS transponder RTLS4060T, ISED, UWB, phase.",404,"ΤΕΜ",1,"SIMATIC",1,"6GT27006DE33","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6GT2790-0DE40","SIMATIC RTLS accessory power clip holder for RTLS transponder, RTLS4083T, plus, with supply connection 116.0 x 87.0 x 23.2 mm Production documentation is included in the manual for the compatible devices 6GT2700-5DC05, 6GT2700-5DC15.",101,"ΤΕΜ",1,"SIMATIC",1,"6GT27900DE40","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6GT2811-6BC10-1AA0","SIMATIC RF600 Reader RF610R FCC; interfaces: 1 Ethernet / PROFINET M12; 1 integrated antenna; 24 V DC; IP67;-25 to +55 Â°C without accessories.",2028,"ΤΕΜ",1,"SIMATIC",1,"6GT28116BC101AA0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6GT2812-1GA08","SIMATIC RF600 antenna RF642A linear (broadband) frequency range 865 to 928 MHz Dimensions 185x 185x 45 mm (LxWxH) IP65, -25 to +75 Â°C.",526,"ΤΕΜ",1,"SIMATIC",1,"6GT28121GA08","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6GT2881-1AB04-2AB0","SIMATIC IDENT CB 4H Gate CMIIT for Tire. RFID UHF system with four antennas for the detection of tires with integrated RFID transponder on a conveyor belt. The system includes special acquisition software for tire detection incl. side detection, and the necessary RFID and automation components incl. HMI panel, control cabinet and metal structure.",24150,"ΤΕΜ",1,"SIMATIC",1,"6GT28811AB042AB0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6NH7997-5DA10-0AA0","ST7 ScadaConnect basic license for connection of RTUs with SINAUT ST7 to HMI/SCADA applications via OPC UA, single license f. 1 installation engineering software, online software delivery (OSD).",689,"ΤΕΜ",1,"SIMATIC",1,"6NH79975DA100AA0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6RA8025-6GV62-0AA0","SINAMICS DCM DC converter for 4-quadrant drives Circuit (B6) A (B6) C Input: 575V 3AC, 50 A controllable: Field rectifier D600/60 MREQ-GEG6V62 Output: 600 V DC, 60A",5444,"ST",1,"GMC",1,"6RA80256GV620AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6RX1800-0LF14","RFI suppression filter 250A and 40Â°C  50/60Hz 760V 3AC TN/TT network 560V 3AC IT network EPCOS  B84143 B0250 S081 Armature circuit",2898,"ST",1,"GMC",1,"6RX18000LF14","Ρυθμιστές στροφών και συστήματα Motion control"]
["6RX1800-4DK12","Commutating reactor for converter; Phases: 3 F(Hz): 50/60; ILN=Ithmax(A): 996 UN(V): 400 (50Hz)/480 (60 Hz) UK (%): 4; Lrated (mH): 0.030 tA/insulating material class: 40Â°/B; IP00 connection: Terminal connection EN 61558-2-20",9461,"ST",1,"GMC",1,"6RX18004DK12","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3000-0BE35-0AA0","SINAMICS line filter Input: 380-480V 3AC, 50/60 Hz 600A",6680,"ST",1,"GMC",1,"6SL30000BE350AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3000-0CE37-7AA0","SINAMICS line reactor Input: 380-480V 3AC, 50/60 Hz 773 A NMA: A5E00125732",3181,"ST",1,"GMC",1,"6SL30000CE377AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3000-2DH32-2CA0","SINAMICS du/dt line reactor Spare part for Power Module/Motor Module 200 kW, 500-690V 3AC max. cable length 300/450 m",4305,"ST",1,"GMC",1,"6SL30002DH322CA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3040-1GA00-1AA0","SINAMICS G130 6SL30401GA001AA0 Control Unit Kit PROFIBUS busbar 6SL3040-1MA00-0AA0 Control Unit 6SL3054-3FC30-1BA0 CompactFlash 6SL3072-0AA00-0AG0 MICROMASTER",1575,"ST",1,"GMC",1,"6SL30401GA001AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3060-4AF10-0AA0","SINAMICS DRIVE-CLIQ CABLE IP20/IP20 LENGTH: 1.45 M",70.199999999999989,"ST",1,"GMC",1,"6SL30604AF100AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3126-1TE28-5AA3","SINAMICS S120 SINGLE MOTOR MODULE INPUT: DC 600V OUTPUT: 3AC 400V, 85A FRAME SIZE: BOOKSIZE COLD-PLATE-COOLING OPTIMIZED PULSE SAMPLE AND SUPPORT OF THE EXTENDED SAFETY INTEGRATED FUNCTIONS INCL. DRIVE-CLIQ CABLE",12606,"ST",1,"GMC",1,"6SL31261TE285AA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3162-8AD00-0AA0","SINAMICS S120 Terminal Kit Double Motor Module 50mm C-/D-TYPE",122,"ST",1,"GMC",1,"6SL31628AD000AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3200-0SK02-0AA0","SINAMICS G120P Small parts mounting set for Power Modul PM230 IP55/UL type 12, FSA or IP20",149,"ST",1,"GMC",1,"6SL32000SK020AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3202-0AE31-5SA0","SINAMICS Sinus filter for Power Module FSF Stand-alone 380-480V 3AC 150.0A",4818,"ST",1,"GMC",1,"6SL32020AE315SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3210-1KE21-3UB1","SINAMICS G120C rated power 3AC380-480V +10/-20%  47-63Hz low overload: 5,5kW at 150% 3s, 110% 57s, 100% 240s high overload: 4,0kW at 200% 3s, 150% 57s, 100% 240s unfiltered external 24V I/O interface: 6DI, 2DO,1AI,1AO, 1Mot_t Safe Torque Off integrated Fieldbus: USS/ MODBUS RTU Protection: IP20/ UL OPEN TYPE Size: FSB 196X100X203(HXWXD)",1366,"ST",1,"GMC",1,"6SL32101KE213UB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3210-1KE31-7UF1","SINAMICS G120C rated power: 90.0 kW with 150% overload for 3 s. 380-480 V 3AC +10/-20% 47-63 Hz unfiltered I/O interface: 6 DI, 2 DO, 1 AI, 1 AO Safe Torque Off integrated fieldbus integrated: PROFINET-PN degree of protection IP20/UL open type size: FSF 708x 305x 357 (HxWxD) external 24 V",12318,"ST",1,"GMC",1,"6SL32101KE317UF1","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3210-1PE34-8AL0","SINAMICS G120/S120 POWER MODULE PM240-2 FSG C2 WITH BUILT IN BRAKING CHOPPER 3AC380-480V+10/-10% 47-63Hz OUTPUT HIGH OVERLOAD: 200kW FOR 200% 3S,150% 57S,100% 240S AMBIENT TEMP -20 bis +50 DEG C (HO) OUTPUT LOW OVERLOAD: 250kW FOR 150% 3S,110% 57S,100% 240S AMBIENT TEMP -20 bis +40 DEG C (LO) 1000x305x357 (HXWXD), FSG PROTECTION IP20 WITHOUT CONTROL UNIT AND PANEL APPROVED FOR CU FIRMWARE- Version V4.7 SP9 AND V5.1",28742,"ST",1,"GMC",1,"6SL32101PE348AL0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3210-1PH31-0UL0","SINAMICS G120 Power Module PM240-2 Unfiltered SINAMICS G120 Power Module PM 240-2 Unfiltered with integrated braking chopper 500-690 V 3 AC +10/-20% 47-63 Hz Power high overload: 75 kW at 200% 3 s, 150% 57 s, 100% 240 s; Ambient temperature -20 to +50 Â°C (HO); Power Low overload: 90 kW at 150% 3 s, 110% 57 s, 100% 240 s; Ambient temperature -20 to +40 Â°C (LO) 708x 305x 357 (HxWxD), FSF Degree of protection IP20 without control Unit and operating unit Released as of CU firmware version V4.7 HF8",14604,"ST",1,"GMC",1,"6SL32101PH310UL0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-1YC10-0UB0","SINAMICS G120X Rated power: 0.75 kW At 110% 60s, 100% 240 s Unfiltered 200-240 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSA Degree of protection IP20 / UL open type painting 3C2 without operator panel Without IO expansion Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",629,"ST",1,"GMC",1,"6SL32201YC100UB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-1YC16-1UB0","SINAMICS G120X Rated power: 2.2 kW At 110% 60s, 100% 240 s Unfiltered 200-240 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSB Degree of protection IP20 / UL open type painting 3C2 without operator panel with IO expansions Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",861,"ST",1,"GMC",1,"6SL32201YC161UB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-1YE12-0AB0","SINAMICS G120X Rated power: 1.1 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSA Degree of protection IP20 / UL open type painting 3C2 without operator panel Without IO expansion Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",835,"ST",1,"GMC",1,"6SL32201YE120AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-1YE16-1AB0","SINAMICS G120X Rated power: 2.2 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSA Degree of protection IP20 / UL open type painting 3C2 without operator panel with IO expansions Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",1089,"ST",1,"GMC",1,"6SL32201YE161AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-1YE28-1UB0","SINAMICS G120X Rated power: 15 kW At 110% 60s, 100% 240 s Unfiltered 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSC Degree of protection IP20 / UL open type painting 3C2 without operator panel with IO expansions Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",2502,"ST",1,"GMC",1,"6SL32201YE281UB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-1YE36-0UF0","SINAMICS G120X Rated power: 37 kW At 110% 60s, 100% 240 s Unfiltered 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSD Degree of protection IP20 / UL open type painting 3C2 without operator panel Without IO expansion Fieldbus integrated: PROFINET PN, Ethernet IP",5177,"ST",1,"GMC",1,"6SL32201YE360UF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-1YE40-0AF0","SINAMICS G120X Rated power: 55 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSE Degree of protection IP20 / UL open type painting 3C2 without operator panel Without IO expansion Fieldbus integrated: PROFINET PN, Ethernet IP",7911,"ST",1,"GMC",1,"6SL32201YE400AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-1YE52-0CF0","SINAMICS G120X Rated power: 200 kW At 110% 60s, 100% 240 s Radio interference suppression filter For category C3 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSG Degree of protection IP20 / UL open type painting 3C2 without operator panel Without IO expansion Fieldbus integrated: PROFINET PN, Ethernet IP",17616,"ST",1,"GMC",1,"6SL32201YE520CF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-1YH20-1AB0","SINAMICS G120X Rated power: 4 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSD Degree of protection IP20 / UL open type painting 3C2 without operator panel with IO expansions Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",1692,"ST",1,"GMC",1,"6SL32201YH201AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-1YH32-0AF0","SINAMICS G120X Rated power: 22 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSD Degree of protection IP20 / UL open type painting 3C2 without operator panel Without IO expansion Fieldbus integrated: PROFINET PN, Ethernet IP",4379,"ST",1,"GMC",1,"6SL32201YH320AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-1YH38-1AP0","SINAMICS G120X Rated power: 45 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSE Degree of protection IP20 / UL open type painting 3C2 without operator panel with IO expansions Fieldbus integrated: PROFIBUS DP",7567,"ST",1,"GMC",1,"6SL32201YH381AP0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-1YH52-1CP0","SINAMICS G120X Rated power: 200 kW At 110% 60s, 100% 240 s Radio interference suppression filter For category C3 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSG Degree of protection IP20 / UL open type painting 3C2 without operator panel with IO expansions Fieldbus integrated: PROFIBUS DP",20354,"ST",1,"GMC",1,"6SL32201YH521CP0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-2YC12-0UP0","SINAMICS G120X Rated power: 1.1 kW At 110% 60s, 100% 240 s Unfiltered 200-240 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSA Degree of protection IP20 / UL open type painting 3C2 with Basic Operator Panel Without IO expansion Fieldbus integrated: PROFIBUS DP",842,"ST",1,"GMC",1,"6SL32202YC120UP0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-2YE10-1UB0","SINAMICS G120X Rated power: 0.75 kW At 110% 60s, 100% 240 s Unfiltered 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSA Degree of protection IP20 / UL open type painting 3C2 with Basic Operator Panel with IO expansions Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",921,"ST",1,"GMC",1,"6SL32202YE101UB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-2YE18-0UP0","SINAMICS G120X Rated power: 3 kW At 110% 60s, 100% 240 s Unfiltered 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSA Degree of protection IP20 / UL open type painting 3C2 with Basic Operator Panel Without IO expansion Fieldbus integrated: PROFIBUS DP",1194,"ST",1,"GMC",1,"6SL32202YE180UP0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-2YE26-1AP0","SINAMICS G120X Rated power: 11 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSC Degree of protection IP20 / UL open type painting 3C2 with Basic Operator Panel with IO expansions Fieldbus integrated: PROFIBUS DP",2452,"ST",1,"GMC",1,"6SL32202YE261AP0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-2YE34-0UB0","SINAMICS G120X Rated power: 30 kW At 110% 60s, 100% 240 s Unfiltered 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSD Degree of protection IP20 / UL open type painting 3C2 with Basic Operator Panel Without IO expansion Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",4262,"ST",1,"GMC",1,"6SL32202YE340UB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-2YE46-1AB0","SINAMICS G120X Rated power: 110 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSF Degree of protection IP20 / UL open type painting 3C2 with Basic Operator Panel with IO expansions Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",12647,"ST",1,"GMC",1,"6SL32202YE461AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-2YE54-0AF0","SINAMICS G120X Rated power: 250 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSG Degree of protection IP20 / UL open type painting 3C2 with Basic Operator Panel Without IO expansion Fieldbus integrated: PROFINET PN, Ethernet IP",24909,"ST",1,"GMC",1,"6SL32202YE540AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-2YH20-0UB0","SINAMICS G120X Rated power: 4 kW At 110% 60s, 100% 240 s Unfiltered 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSD Degree of protection IP20 / UL open type painting 3C2 with Basic Operator Panel Without IO expansion Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",1481,"ST",1,"GMC",1,"6SL32202YH200UB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-2YH30-0AB0","SINAMICS G120X Rated power: 18.5 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSD Degree of protection IP20 / UL open type painting 3C2 with Basic Operator Panel Without IO expansion Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",3630,"ST",1,"GMC",1,"6SL32202YH300AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-2YH36-1AF0","SINAMICS G120X Rated power: 37 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSD Degree of protection IP20 / UL open type painting 3C2 with Basic Operator Panel with IO expansions Fieldbus integrated: PROFINET PN, Ethernet IP",6579,"ST",1,"GMC",1,"6SL32202YH361AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-2YH48-1UF0","SINAMICS G120X Rated power: 132 kW At 110% 60s, 100% 240 s Unfiltered 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSF Degree of protection IP20 / UL open type painting 3C2 with Basic Operator Panel with IO expansions Fieldbus integrated: PROFINET PN, Ethernet IP",15063,"ST",1,"GMC",1,"6SL32202YH481UF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-3YC14-1UP0","SINAMICS G120X Rated power: 1.5 kW At 110% 60s, 100% 240 s Unfiltered 200-240 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSA Degree of protection IP20 / UL open type painting 3C2 With Intelligent Operator Panel with IO expansions Fieldbus integrated: PROFIBUS DP",1124,"ST",1,"GMC",1,"6SL32203YC141UP0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-3YC40-0UP0","SINAMICS G120X rated power: 55 kW at 110% 60s, 100% 240s unfiltered 200-240V3AC+10/-20% 47-63Hz ambient temperature -20 to +45 Â°C frame size: FSF degree of protection IP20 / UL open type painting 3C2 with Intelligent Operator Panel without IO expansion fieldbus integrated: PROFIBUS DP",8152,"ST",1,"GMC",1,"6SL32203YC400UP0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-3YE18-0AP0","SINAMICS G120X Rated power: 3 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSA Degree of protection IP20 / UL open type painting 3C2 With Intelligent Operator Panel Without IO expansion Fieldbus integrated: PROFIBUS DP",1424,"ST",1,"GMC",1,"6SL32203YE180AP0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-3YE18-1UP0","SINAMICS G120X Rated power: 3 kW At 110% 60s, 100% 240 s Unfiltered 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSA Degree of protection IP20 / UL open type painting 3C2 With Intelligent Operator Panel with IO expansions Fieldbus integrated: PROFIBUS DP",1430,"ST",1,"GMC",1,"6SL32203YE181UP0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-3YE32-0AP0","SINAMICS G120X Rated power: 22 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSD Degree of protection IP20 / UL open type painting 3C2 With Intelligent Operator Panel Without IO expansion Fieldbus integrated: PROFIBUS DP",4037,"ST",1,"GMC",1,"6SL32203YE320AP0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-3YE44-0UP0","SINAMICS G120X Rated power: 90 kW At 110% 60s, 100% 240 s Unfiltered 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSF Degree of protection IP20 / UL open type painting 3C2 With Intelligent Operator Panel Without IO expansion Fieldbus integrated: PROFIBUS DP",10375,"ST",1,"GMC",1,"6SL32203YE440UP0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-3YE52-0AB0","SINAMICS G120X Rated power: 200 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSG Degree of protection IP20 / UL open type painting 3C2 With Intelligent Operator Panel Without IO expansion Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",19875,"ST",1,"GMC",1,"6SL32203YE520AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-3YE54-1CB0","SINAMICS G120X Rated power: 250 kW At 110% 60s, 100% 240 s Radio interference suppression filter For category C3 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSG Degree of protection IP20 / UL open type painting 3C2 With Intelligent Operator Panel with IO expansions Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",22186,"ST",1,"GMC",1,"6SL32203YE541CB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-3YH24-1UB0","SINAMICS G120X Rated power: 7.5 kW At 110% 60s, 100% 240 s Unfiltered 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSD Degree of protection IP20 / UL open type painting 3C2 With Intelligent Operator Panel with IO expansions Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",2045,"ST",1,"GMC",1,"6SL32203YH241UB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-3YH34-1AB0","SINAMICS G120X Rated power: 30 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSD Degree of protection IP20 / UL open type painting 3C2 With Intelligent Operator Panel with IO expansions Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",5523,"ST",1,"GMC",1,"6SL32203YH341AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-3YH46-1UB0","SINAMICS G120X Rated power: 110 kW At 110% 60s, 100% 240 s Unfiltered 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSF Degree of protection IP20 / UL open type painting 3C2 With Intelligent Operator Panel with IO expansions Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",13454,"ST",1,"GMC",1,"6SL32203YH461UB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3223-0DE17-5AG1","SINAMICS G120P Power Module PM230 with integrated Class A filter Degree of protection IP55/UL Type 12 380-480 V 3 AC +10/-10% 47-63 Hz Power low overload: 0.75kW at 150% 3s, 110% 57s, 100% 240 s; Ambient temperature -10 to +40 Â°C (LO) 460x 154x 249 (HxWxD), FSA without Control Unit and operating unit released for CU230P-2 Firmware version V4.3.2 or higher",612,"ST",1,"GMC",1,"6SL32230DE175AG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-1YC16-0UP0","SINAMICS G120X Rated power: 2.2 kW At 110% 60s, 100% 240 s Unfiltered 200-240 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSB Degree of protection IP20 / UL open type Paint finish 3C3 without operator panel Without IO expansion Fieldbus integrated: PROFIBUS DP",1079,"ST",1,"GMC",1,"6SL32301YC160UP0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-1YC20-0UF0","SINAMICS G120X Rated power: 4 kW At 110% 60s, 100% 240 s Unfiltered 200-240 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSB Degree of protection IP20 / UL open type Paint finish 3C3 without operator panel Without IO expansion Fieldbus integrated: PROFINET PN, Ethernet IP",1327,"ST",1,"GMC",1,"6SL32301YC200UF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-1YE16-0UP0","SINAMICS G120X Rated power: 2.2 kW At 110% 60s, 100% 240 s Unfiltered 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSA Degree of protection IP20 / UL open type Paint finish 3C3 without operator panel Without IO expansion Fieldbus integrated: PROFIBUS DP",1211,"ST",1,"GMC",1,"6SL32301YE160UP0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-1YE20-0AP0","SINAMICS G120X Rated power: 4 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSB Degree of protection IP20 / UL open type Paint finish 3C3 without operator panel Without IO expansion Fieldbus integrated: PROFIBUS DP",1634,"ST",1,"GMC",1,"6SL32301YE200AP0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-1YE26-1UB0","SINAMICS G120X Rated power: 11 kW At 110% 60s, 100% 240 s Unfiltered 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSC Degree of protection IP20 / UL open type Paint finish 3C3 without operator panel with IO expansions Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",2302,"ST",1,"GMC",1,"6SL32301YE261UB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-1YE40-0AB0","SINAMICS G120X Rated power: 55 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSE Degree of protection IP20 / UL open type Paint finish 3C3 without operator panel Without IO expansion Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",8287,"ST",1,"GMC",1,"6SL32301YE400AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-1YE52-0CB0","SINAMICS G120X Rated power: 200 kW At 110% 60s, 100% 240 s Radio interference suppression filter For category C3 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSG Degree of protection IP20 / UL open type Paint finish 3C3 without operator panel Without IO expansion Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",18156,"ST",1,"GMC",1,"6SL32301YE520CB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-1YE54-1AF0","SINAMICS G120X Rated power: 250 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSG Degree of protection IP20 / UL open type Paint finish 3C3 without operator panel with IO expansions Fieldbus integrated: PROFINET PN, Ethernet IP",25689,"ST",1,"GMC",1,"6SL32301YE541AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-1YH24-1AB0","SINAMICS G120X Rated power: 7.5 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSD Degree of protection IP20 / UL open type Paint finish 3C3 without operator panel with IO expansions Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",2393,"ST",1,"GMC",1,"6SL32301YH241AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-1YH40-1AF0","SINAMICS G120X Rated power: 55 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSE Degree of protection IP20 / UL open type Paint finish 3C3 without operator panel with IO expansions Fieldbus integrated: PROFINET PN, Ethernet IP",9624,"ST",1,"GMC",1,"6SL32301YH401AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-1YH44-0UF0","SINAMICS G120X Rated power: 90 kW At 110% 60s, 100% 240 s Unfiltered 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSF Degree of protection IP20 / UL open type Paint finish 3C3 without operator panel Without IO expansion Fieldbus integrated: PROFINET PN, Ethernet IP",12298,"ST",1,"GMC",1,"6SL32301YH440UF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-2YC18-0UF0","SINAMICS G120X Rated power: 3 kW At 110% 60s, 100% 240 s Unfiltered 200-240 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSB Degree of protection IP20 / UL open type Paint finish 3C3 with Basic Operator Panel Without IO expansion Fieldbus integrated: PROFINET PN, Ethernet IP",1272,"ST",1,"GMC",1,"6SL32302YC180UF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-2YC32-0UP0","SINAMICS G120X Rated power: 22 kW At 110% 60s, 100% 240 s Unfiltered 200-240 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSE Degree of protection IP20 / UL open type Paint finish 3C3 with Basic Operator Panel Without IO expansion Fieldbus integrated: PROFIBUS DP",4233,"ST",1,"GMC",1,"6SL32302YC320UP0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-2YE16-0AB0","SINAMICS G120X Rated power: 2.2 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSA Degree of protection IP20 / UL open type Paint finish 3C3 with Basic Operator Panel Without IO expansion Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",1221,"ST",1,"GMC",1,"6SL32302YE160AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-2YE20-1AF0","SINAMICS G120X Rated power: 4 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSB Degree of protection IP20 / UL open type Paint finish 3C3 with Basic Operator Panel with IO expansions Fieldbus integrated: PROFINET PN, Ethernet IP",1819,"ST",1,"GMC",1,"6SL32302YE201AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-2YE28-0AP0","SINAMICS G120X Rated power: 15 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSC Degree of protection IP20 / UL open type Paint finish 3C3 with Basic Operator Panel Without IO expansion Fieldbus integrated: PROFIBUS DP",3236,"ST",1,"GMC",1,"6SL32302YE280AP0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-2YE40-0UP0","SINAMICS G120X Rated power: 55 kW At 110% 60s, 100% 240 s Unfiltered 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSE Degree of protection IP20 / UL open type Paint finish 3C3 with Basic Operator Panel Without IO expansion Fieldbus integrated: PROFIBUS DP",7832,"ST",1,"GMC",1,"6SL32302YE400UP0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-2YE48-0AB0","SINAMICS G120X Rated power: 132 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSF Degree of protection IP20 / UL open type Paint finish 3C3 with Basic Operator Panel Without IO expansion Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",14692,"ST",1,"GMC",1,"6SL32302YE480AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-2YH18-1UF0","SINAMICS G120X Rated power: 3 kW At 110% 60s, 100% 240 s Unfiltered 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSD Degree of protection IP20 / UL open type Paint finish 3C3 with Basic Operator Panel with IO expansions Fieldbus integrated: PROFINET PN, Ethernet IP",1846,"ST",1,"GMC",1,"6SL32302YH181UF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-2YH24-1UP0","SINAMICS G120X Rated power: 7.5 kW At 110% 60s, 100% 240 s Unfiltered 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSD Degree of protection IP20 / UL open type Paint finish 3C3 with Basic Operator Panel with IO expansions Fieldbus integrated: PROFIBUS DP",2380,"ST",1,"GMC",1,"6SL32302YH241UP0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-2YH42-0CB0","SINAMICS G120X Rated power: 75 kW At 110% 60s, 100% 240 s Radio interference suppression filter For category C3 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSF Degree of protection IP20 / UL open type Paint finish 3C3 with Basic Operator Panel Without IO expansion Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",10826,"ST",1,"GMC",1,"6SL32302YH420CB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-2YH44-1UB0","SINAMICS G120X Rated power: 90 kW At 110% 60s, 100% 240 s Unfiltered 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSF Degree of protection IP20 / UL open type Paint finish 3C3 with Basic Operator Panel with IO expansions Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",12328,"ST",1,"GMC",1,"6SL32302YH441UB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-2YH54-1CF0","SINAMICS G120X Rated power: 250 kW At 110% 60s, 100% 240 s Radio interference suppression filter For category C3 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSG Degree of protection IP20 / UL open type Paint finish 3C3 with Basic Operator Panel with IO expansions Fieldbus integrated: PROFINET PN, Ethernet IP",26222,"ST",1,"GMC",1,"6SL32302YH541CF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-3YC34-0UF0","SINAMICS G120X Rated power: 30 kW At 110% 60s, 100% 240 s Unfiltered 200-240 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSE Degree of protection IP20 / UL open type Paint finish 3C3 With Intelligent Operator Panel Without IO expansion Fieldbus integrated: PROFINET PN, Ethernet IP",5262,"ST",1,"GMC",1,"6SL32303YC340UF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-3YE18-0UB0","SINAMICS G120X Rated power: 3 kW At 110% 60s, 100% 240 s Unfiltered 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSA Degree of protection IP20 / UL open type Paint finish 3C3 With Intelligent Operator Panel Without IO expansion Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",1389,"ST",1,"GMC",1,"6SL32303YE180UB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-3YE24-1UF0","SINAMICS G120X Rated power: 7.5 kW At 110% 60s, 100% 240 s Unfiltered 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSB Degree of protection IP20 / UL open type Paint finish 3C3 With Intelligent Operator Panel with IO expansions Fieldbus integrated: PROFINET PN, Ethernet IP",2206,"ST",1,"GMC",1,"6SL32303YE241UF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-3YE38-0AF0","SINAMICS G120X Rated power: 45 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSE Degree of protection IP20 / UL open type Paint finish 3C3 With Intelligent Operator Panel Without IO expansion Fieldbus integrated: PROFINET PN, Ethernet IP",7238,"ST",1,"GMC",1,"6SL32303YE380AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-3YE40-1UF0","SINAMICS G120X Rated power: 55 kW At 110% 60s, 100% 240 s Unfiltered 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSE Degree of protection IP20 / UL open type Paint finish 3C3 With Intelligent Operator Panel with IO expansions Fieldbus integrated: PROFINET PN, Ethernet IP",8074,"ST",1,"GMC",1,"6SL32303YE401UF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-3YE48-0UP0","SINAMICS G120X Rated power: 132 kW At 110% 60s, 100% 240 s Unfiltered 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSF Degree of protection IP20 / UL open type Paint finish 3C3 With Intelligent Operator Panel Without IO expansion Fieldbus integrated: PROFIBUS DP",13761,"ST",1,"GMC",1,"6SL32303YE480UP0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-3YH22-1AP0","SINAMICS G120X Rated power: 5.5 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSD Degree of protection IP20 / UL open type Paint finish 3C3 With Intelligent Operator Panel with IO expansions Fieldbus integrated: PROFIBUS DP",2405,"ST",1,"GMC",1,"6SL32303YH221AP0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-3YH26-1UF0","SINAMICS G120X Rated power: 11 kW At 110% 60s, 100% 240 s Unfiltered 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSD Degree of protection IP20 / UL open type Paint finish 3C3 With Intelligent Operator Panel with IO expansions Fieldbus integrated: PROFINET PN, Ethernet IP",2938,"ST",1,"GMC",1,"6SL32303YH261UF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-3YH42-0UP0","SINAMICS G120X Rated power: 75 kW At 110% 60s, 100% 240 s Unfiltered 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSF Degree of protection IP20 / UL open type Paint finish 3C3 With Intelligent Operator Panel Without IO expansion Fieldbus integrated: PROFIBUS DP",10576,"ST",1,"GMC",1,"6SL32303YH420UP0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-3YH46-0CP0","SINAMICS G120X Rated power: 110 kW At 110% 60s, 100% 240 s Radio interference suppression filter For category C3 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSF Degree of protection IP20 / UL open type Paint finish 3C3 With Intelligent Operator Panel Without IO expansion Fieldbus integrated: PROFIBUS DP",14769,"ST",1,"GMC",1,"6SL32303YH460CP0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3262-1AD00-0DA0","SINAMICS shield connection kit for Power Module FSD and FSE PM230, PM240 and PM250",159,"ST",1,"GMC",1,"6SL32621AD000DA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3266-1ER00-0VA0","SINAMICS V20 FSAA/FSAB migration mounting Size: 90x150x5 (WxHxD)",6.3,"ST",1,"GMC",1,"6SL32661ER000VA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3420-2HX00-0AA0","SINAMICS S120 HYDRAULIC LINEAR ACTOR 2 AXIS-CONTROLLER",5578,"ST",1,"GMC",1,"6SL34202HX000AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-0XA20-7AF0","SINAMICS G115D wall-mounted Rated power: 0.75 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 180 V DC without operation option with cable gland with communication Fieldbus integrated: PROFINET PN, Ethernet IP",1325,"ST",1,"GMC",1,"6SL35200XA207AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-0XB40-3AB0","SINAMICS G115D wall-mounted rated power: 0.37 kW for 3s 200%, 57s 150%, 240s 87%, RFI suppression filter for category C2 3AC380-480V+10/-10% 45-66Hz ambient temperature -30 to +40 Â°C frame size: FSA degree of protection IP65/66 / UL type 4X brake voltage 180 V DC without operation option Q4/2 for 400 V AC and Power M12 for 24 V DC and M12 for I/O and communication without looping through Q8/0 for motor connection without fieldbus",1030,"ST",1,"GMC",1,"6SL35200XB403AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-0XC04-0AF0","SINAMICS G115D wall-mounted Rated power: 4 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSB Protection class IP65/66 / UL Type 4X brake voltage 180 V DC without operation option with Quickon for 400 V AC and Power M12 for 24 V DC and M12 for I/O and communication without looping through Q8/0 for motor connection Fieldbus integrated: PROFINET PN, Ethernet IP",2544,"ST",1,"GMC",1,"6SL35200XC040AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-0XD01-5AF0","SINAMICS G115D wall-mounted Rated power: 1.5kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 180 V DC without operation option with MQ(X)15 for 400 V AC and Power M12 for 24 V DC and M12 for I/O and communication without looping through Q8/0 for motor connection Fieldbus integrated: PROFINET PN, Ethernet IP",1795,"ST",1,"GMC",1,"6SL35200XD015AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-0XH07-5AB0","SINAMICS G115D wall-mounted Rated power: 7.5 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSC Protection class IP65/66 / UL Type 4X brake voltage 180 V DC without operation option with cable gland without communication with integrated 24 V DC PSU without fieldbus",3163,"ST",1,"GMC",1,"6SL35200XH075AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-0XH62-2AA0","SINAMICS G115D wall-mounted Rated power: 2.2 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSB Protection class IP65/66 / UL Type 4X brake voltage 180 V DC without operation option with cable gland for 400 V AC and 24 V DC and M12 for I/O and communication with integrated 24 V DC PSU fieldbus integrated: AS-Interface",1871,"ST",1,"GMC",1,"6SL35200XH622AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-0XM00-7AA0","SINAMICS G115D wall-mounted Rated power: 0.75 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 180 V DC without operation option MQ(X)15 for 400 V AC and M12 for I/O and communication with integrated 24 V DC PSU without looping through fieldbus integrated: AS-Interface",1566,"ST",1,"GMC",1,"6SL35200XM007AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-0XN03-0AB0","SINAMICS G115D wall-mounted Rated power: 3 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSB Protection class IP65/66 / UL Type 4X brake voltage 180 V DC without operation option Q4/2 for 400 V AC and M12 for I/O and communication with integrated 24 V DC PSU with looping through without fieldbus",1985,"ST",1,"GMC",1,"6SL35200XN030AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-1XA24-0AA0","SINAMICS G115D wall-mounted Rated power: 4 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSB Protection class IP65/66 / UL Type 4X brake voltage 180 V DC repair switch with cable gland with communication fieldbus integrated: AS-Interface",2194,"ST",1,"GMC",1,"6SL35201XA240AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-1XA62-2AA0","SINAMICS G115D wall-mounted Rated power: 2.2 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSB Protection class IP65/66 / UL Type 4X brake voltage 180 V DC repair switch with cable gland for 400 V AC and 24 V DC and M12 for I/O and communication fieldbus integrated: AS-Interface",1751,"ST",1,"GMC",1,"6SL35201XA622AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-1XB07-5AB0","SINAMICS G115D wall-mounted Rated power: 7.5 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSC Protection class IP65/66 / UL Type 4X brake voltage 180 V DC repair switch Q4/2 for 400 V AC and 7/8\" for 24 V DC and M12 for I/O and communication without looping through Q8/0 for motor connection without fieldbus",3293,"ST",1,"GMC",1,"6SL35201XB075AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-1XE00-3AF0","SINAMICS G115D wall-mounted rated power: 0.37 kW for 3s 200%, 57s 150%, 240s 87%, RFI suppression filter for category C2 3AC380-480V+10/-10% 45-66Hz ambient temperature -30 to +40 Â°C frame size: FSA degree of protection IP65/66 / UL type 4X brake voltage 180 V DC repair switch Q4/2 for 400 V AC and 7/8\" for 24 V DC and M12 for I/O and communication with looping through Q8/0 for motor connection Fieldbus integrated: PROFINET PN, Ethernet IP",1711,"ST",1,"GMC",1,"6SL35201XE003AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-1XH21-1AF0","SINAMICS G115D wall-mounted Rated power: 1.1 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 180 V DC repair switch with cable gland with communication with integrated 24 V DC PSU Fieldbus integrated: PROFINET PN, Ethernet IP",1793,"ST",1,"GMC",1,"6SL35201XH211AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-1XK00-3AA0","SINAMICS G115D wall-mounted rated power: 0.37 kW for 3s 200%, 57s 150%, 240s 87%, RFI suppression filter for category C2 3AC380-480V+10/-10% 45-66Hz ambient temperature -30 to +40 Â°C frame size: FSA degree of protection IP65/66 / UL type 4X brake voltage 180 V DC repair switch Q4/2 for 400 V AC and M12 for I/O and communication with integrated 24 V DC PSU without looping through fieldbus integrated: AS-Interface",1634,"ST",1,"GMC",1,"6SL35201XK003AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-1XM02-2AA0","SINAMICS G115D wall-mounted Rated power: 2.2 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSB Protection class IP65/66 / UL Type 4X brake voltage 180 V DC repair switch MQ(X)15 for 400 V AC and M12 for I/O and communication with integrated 24 V DC PSU without looping through fieldbus integrated: AS-Interface",2144,"ST",1,"GMC",1,"6SL35201XM022AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-1XN07-5AB0","SINAMICS G115D wall-mounted Rated power: 7.5 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSC Protection class IP65/66 / UL Type 4X brake voltage 180 V DC repair switch Q4/2 for 400 V AC and M12 for I/O and communication with integrated 24 V DC PSU with looping through without fieldbus",3542,"ST",1,"GMC",1,"6SL35201XN075AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-1XR10-5AB0","SINAMICS G115D wall-mounted Rated power: 0.55 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 180 V DC repair switch with cable gland for 400 V AC Power M12 for 24 V DC with looping through M12 for I/O and communication without fieldbus",1044,"ST",1,"GMC",1,"6SL35201XR105AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-2XA64-0AF0","SINAMICS G115D wall-mounted Rated power: 4 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSB Protection class IP65/66 / UL Type 4X brake voltage 180 V DC local remote control with cable gland for 400 V AC and 24 V DC and M12 for I/O and communication Fieldbus integrated: PROFINET PN, Ethernet IP",2557,"ST",1,"GMC",1,"6SL35202XA640AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-2XB41-1AB0","SINAMICS G115D wall-mounted Rated power: 1.1 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 180 V DC local remote control Q4/2 for 400 V AC and Power M12 for 24 V DC and M12 for I/O and communication without looping through Q8/0 for motor connection without fieldbus",1386,"ST",1,"GMC",1,"6SL35202XB411AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-2XE00-3AB0","SINAMICS G115D wall-mounted rated power: 0.37 kW for 3s 200%, 57s 150%, 240s 87%, RFI suppression filter for category C2 3AC380-480V+10/-10% 45-66Hz ambient temperature -30 to +40 Â°C frame size: FSA degree of protection IP65/66 / UL type 4X brake voltage 180 V DC local remote control Q4/2 for 400 V AC and 7/8\" for 24 V DC and M12 for I/O and communication with looping through Q8/0 for motor connection without fieldbus",1293,"ST",1,"GMC",1,"6SL35202XE003AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-2XE44-0AB0","SINAMICS G115D wall-mounted Rated power: 4 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSB Protection class IP65/66 / UL Type 4X brake voltage 180 V DC local remote control Q4/2 for 400 V AC and Power M12 for 24 V DC and M12 for I/O and communication with looping through Q8/0 for motor connection without fieldbus",2314,"ST",1,"GMC",1,"6SL35202XE440AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-2XK01-1AA0","SINAMICS G115D wall-mounted Rated power: 1.1 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 180 V DC local remote control Q4/2 for 400 V AC and M12 for I/O and communication with integrated 24 V DC PSU without looping through fieldbus integrated: AS-Interface",1871,"ST",1,"GMC",1,"6SL35202XK011AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-2XL03-0AB0","SINAMICS G115D wall-mounted Rated power: 3 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSB Protection class IP65/66 / UL Type 4X brake voltage 180 V DC local remote control Quickon for 400 V AC and M12 for I/O and communication with integrated 24 V DC PSU without looping through without fieldbus",2143,"ST",1,"GMC",1,"6SL35202XL030AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-2XM01-5AA0","SINAMICS G115D wall-mounted Rated power: 1.5kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 180 V DC local remote control MQ(X)15 for 400 V AC and M12 for I/O and communication with integrated 24 V DC PSU without looping through fieldbus integrated: AS-Interface",1981,"ST",1,"GMC",1,"6SL35202XM015AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-2XR11-1AF0","SINAMICS G115D wall-mounted Rated power: 1.1 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 180 V DC local remote control with cable gland for 400 V AC Power M12 for 24 V DC with looping through M12 for I/O and communication Fieldbus integrated: PROFINET PN, Ethernet IP",1756,"ST",1,"GMC",1,"6SL35202XR111AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-3XB00-3AF0","SINAMICS G115D wall-mounted rated power: 0.37 kW for 3s 200%, 57s 150%, 240s 87%, RFI suppression filter for category C2 3AC380-480V+10/-10% 45-66Hz ambient temperature -30 to +40 Â°C frame size: FSA degree of protection IP65/66 / UL type 4X brake voltage 180 V DC repair switch local remote control Q4/2 for 400 V AC and 7/8\" for 24 V DC and M12 for I/O and communication without looping through Q8/0 for motor connection Fieldbus integrated: PROFINET PN, Ethernet IP",1836,"ST",1,"GMC",1,"6SL35203XB003AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-3XB44-0AF0","SINAMICS G115D wall-mounted Rated power: 4 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSB Protection class IP65/66 / UL Type 4X brake voltage 180 V DC repair switch local remote control Q4/2 for 400 V AC and Power M12 for 24 V DC and M12 for I/O and communication without looping through Q8/0 for motor connection Fieldbus integrated: PROFINET PN, Ethernet IP",2856,"ST",1,"GMC",1,"6SL35203XB440AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-3XC02-2AB0","SINAMICS G115D wall-mounted Rated power: 2.2 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSB Protection class IP65/66 / UL Type 4X brake voltage 180 V DC repair switch local remote control with Quickon for 400 V AC and Power M12 for 24 V DC and M12 for I/O and communication without looping through Q8/0 for motor connection without fieldbus",1853,"ST",1,"GMC",1,"6SL35203XC022AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-3XH02-2AB0","SINAMICS G115D wall-mounted Rated power: 2.2 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSB Protection class IP65/66 / UL Type 4X brake voltage 180 V DC repair switch local remote control with cable gland without communication with integrated 24 V DC PSU without fieldbus",1843,"ST",1,"GMC",1,"6SL35203XH022AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-3XH23-0AF0","SINAMICS G115D wall-mounted Rated power: 3 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSB Protection class IP65/66 / UL Type 4X brake voltage 180 V DC repair switch local remote control with cable gland with communication with integrated 24 V DC PSU Fieldbus integrated: PROFINET PN, Ethernet IP",2531,"ST",1,"GMC",1,"6SL35203XH230AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-3XL00-7AF0","SINAMICS G115D wall-mounted Rated power: 0.75 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 180 V DC repair switch local remote control Quickon for 400 V AC and M12 for I/O and communication with integrated 24 V DC PSU without looping through Fieldbus integrated: PROFINET PN, Ethernet IP",2099,"ST",1,"GMC",1,"6SL35203XL007AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-3XM04-0AA0","SINAMICS G115D wall-mounted Rated power: 4 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSB Protection class IP65/66 / UL Type 4X brake voltage 180 V DC repair switch local remote control MQ(X)15 for 400 V AC and M12 for I/O and communication with integrated 24 V DC PSU without looping through fieldbus integrated: AS-Interface",2849,"ST",1,"GMC",1,"6SL35203XM040AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-3XR15-5AB0","SINAMICS G115D wall-mounted Rated power: 5.5 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSC Protection class IP65/66 / UL Type 4X brake voltage 180 V DC repair switch local remote control with cable gland for 400 V AC Power M12 for 24 V DC with looping through M12 for I/O and communication without fieldbus",2735,"ST",1,"GMC",1,"6SL35203XR155AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-0XA60-5AB0","SINAMICS G115D wall-mounted Rated power: 0.55 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 400 V AC without operation option with cable gland for 400 V AC and 24 V DC and M12 for I/O and communication without fieldbus",1139,"ST",1,"GMC",1,"6SL35210XA605AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-0XA62-2AF0","SINAMICS G115D wall-mounted Rated power: 2.2 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSB Protection class IP65/66 / UL Type 4X brake voltage 400 V AC without operation option with cable gland for 400 V AC and 24 V DC and M12 for I/O and communication Fieldbus integrated: PROFINET PN, Ethernet IP",2125,"ST",1,"GMC",1,"6SL35210XA622AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-0XC01-5AA0","SINAMICS G115D wall-mounted Rated power: 1.5kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 400 V AC without operation option with Quickon for 400 V AC and M12 for I/O and communication without looping through Q8/0 for motor connection fieldbus integrated: AS-Interface",1847,"ST",1,"GMC",1,"6SL35210XC015AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-0XD05-5AB0","SINAMICS G115D wall-mounted Rated power: 5.5 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSC Protection class IP65/66 / UL Type 4X brake voltage 400 V AC without operation option with MQ(X)15 for 400 V AC and Power M12 for 24 V DC and M12 for I/O and communication without looping through Q8/0 for motor connection without fieldbus",2816,"ST",1,"GMC",1,"6SL35210XD055AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-0XH22-2AA0","SINAMICS G115D wall-mounted Rated power: 2.2 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSB Protection class IP65/66 / UL Type 4X brake voltage 400 V AC without operation option with cable gland with communication with integrated 24 V DC PSU fieldbus integrated: AS-Interface",2074,"ST",1,"GMC",1,"6SL35210XH222AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-0XL00-5AF0","SINAMICS G115D wall-mounted Rated power: 0.55 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 400 V AC without operation option Quickon for 400 V AC and M12 for I/O and communication with integrated 24 V DC PSU without looping through Fieldbus integrated: PROFINET PN, Ethernet IP",2025,"ST",1,"GMC",1,"6SL35210XL005AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-0XL00-7AB0","SINAMICS G115D wall-mounted Rated power: 0.75 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 400 V AC without operation option Quickon for 400 V AC and M12 for I/O and communication with integrated 24 V DC PSU without looping through without fieldbus",1566,"ST",1,"GMC",1,"6SL35210XL007AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-0XN00-7AF0","SINAMICS G115D wall-mounted Rated power: 0.75 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 400 V AC without operation option Q4/2 for 400 V AC and M12 for I/O and communication with integrated 24 V DC PSU with looping through Fieldbus integrated: PROFINET PN, Ethernet IP",2095,"ST",1,"GMC",1,"6SL35210XN007AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-1XA60-5AF0","SINAMICS G115D wall-mounted Rated power: 0.55 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 400 V AC repair switch with cable gland for 400 V AC and 24 V DC and M12 for I/O and communication Fieldbus integrated: PROFINET PN, Ethernet IP",1750,"ST",1,"GMC",1,"6SL35211XA605AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-1XA65-5AF0","SINAMICS G115D wall-mounted Rated power: 5.5 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSC Protection class IP65/66 / UL Type 4X brake voltage 400 V AC repair switch with cable gland for 400 V AC and 24 V DC and M12 for I/O and communication Fieldbus integrated: PROFINET PN, Ethernet IP",3247,"ST",1,"GMC",1,"6SL35211XA655AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-1XC04-0AA0","SINAMICS G115D wall-mounted Rated power: 4 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSB Protection class IP65/66 / UL Type 4X brake voltage 400 V AC repair switch with Quickon for 400 V AC and M12 for I/O and communication without looping through Q8/0 for motor connection fieldbus integrated: AS-Interface",2714,"ST",1,"GMC",1,"6SL35211XC040AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-1XE00-5AB0","SINAMICS G115D wall-mounted Rated power: 0.55 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 400 V AC repair switch Q4/2 for 400 V AC and 7/8\" for 24 V DC and M12 for I/O and communication with looping through Q8/0 for motor connection without fieldbus",1507,"ST",1,"GMC",1,"6SL35211XE005AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-1XH01-5AB0","SINAMICS G115D wall-mounted Rated power: 1.5kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 400 V AC repair switch with cable gland without communication with integrated 24 V DC PSU without fieldbus",1683,"ST",1,"GMC",1,"6SL35211XH015AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-1XH63-0AB0","SINAMICS G115D wall-mounted Rated power: 3 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSB Protection class IP65/66 / UL Type 4X brake voltage 400 V AC repair switch with cable gland for 400 V AC and 24 V DC and M12 for I/O and communication with integrated 24 V DC PSU without fieldbus",2185,"ST",1,"GMC",1,"6SL35211XH630AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-1XL00-3AF0","SINAMICS G115D wall-mounted rated power: 0.37 kW for 3s 200%, 57s 150%, 240s 87%, RFI suppression filter for category C2 3AC380-480V+10/-10% 45-66Hz ambient temperature -30 to +40 Â°C frame size: FSA degree of protection IP65/66 / UL type 4X brake voltage 400 V AC repair switch Quickon for 400 V AC and M12 for I/O and communication with integrated 24 V DC PSU without looping through Fieldbus integrated: PROFINET PN, Ethernet IP",2127,"ST",1,"GMC",1,"6SL35211XL003AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-1XN02-2AF0","SINAMICS G115D wall-mounted Rated power: 2.2 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSB Protection class IP65/66 / UL Type 4X brake voltage 400 V AC repair switch Q4/2 for 400 V AC and M12 for I/O and communication with integrated 24 V DC PSU with looping through Fieldbus integrated: PROFINET PN, Ethernet IP",2673,"ST",1,"GMC",1,"6SL35211XN022AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-1XR12-2AB0","SINAMICS G115D wall-mounted Rated power: 2.2 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSB Protection class IP65/66 / UL Type 4X brake voltage 400 V AC repair switch with cable gland for 400 V AC Power M12 for 24 V DC with looping through M12 for I/O and communication without fieldbus",1809,"ST",1,"GMC",1,"6SL35211XR122AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-2XA60-3AA0","SINAMICS G115D wall-mounted rated power: 0.37 kW for 3s 200%, 57s 150%, 240s 87%, RFI suppression filter for category C2 3AC380-480V+10/-10% 45-66Hz ambient temperature -30 to +40 Â°C frame size: FSA degree of protection IP65/66 / UL type 4X brake voltage 400 V AC local remote control with cable gland for 400 V AC and 24 V DC and M12 for I/O and communication fieldbus integrated: AS-Interface",1588,"ST",1,"GMC",1,"6SL35212XA603AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-2XB04-0AA0","SINAMICS G115D wall-mounted Rated power: 4 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSB Protection class IP65/66 / UL Type 4X brake voltage 400 V AC local remote control Q4/2 for 400 V AC and M12 for I/O and communication without looping through Q8/0 for motor connection fieldbus integrated: AS-Interface",2789,"ST",1,"GMC",1,"6SL35212XB040AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-2XE00-7AF0","SINAMICS G115D wall-mounted Rated power: 0.75 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 400 V AC local remote control Q4/2 for 400 V AC and 7/8\" for 24 V DC and M12 for I/O and communication with looping through Q8/0 for motor connection Fieldbus integrated: PROFINET PN, Ethernet IP",2109,"ST",1,"GMC",1,"6SL35212XE007AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-2XE07-5AF0","SINAMICS G115D wall-mounted Rated power: 7.5 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSC Protection class IP65/66 / UL Type 4X brake voltage 400 V AC local remote control Q4/2 for 400 V AC and 7/8\" for 24 V DC and M12 for I/O and communication with looping through Q8/0 for motor connection Fieldbus integrated: PROFINET PN, Ethernet IP",4201,"ST",1,"GMC",1,"6SL35212XE075AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-2XH65-5AA0","SINAMICS G115D wall-mounted Rated power: 5.5 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSC Protection class IP65/66 / UL Type 4X brake voltage 400 V AC local remote control with cable gland for 400 V AC and 24 V DC and M12 for I/O and communication with integrated 24 V DC PSU fieldbus integrated: AS-Interface",3340,"ST",1,"GMC",1,"6SL35212XH655AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-2XL00-7AB0","SINAMICS G115D wall-mounted Rated power: 0.75 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 400 V AC local remote control Quickon for 400 V AC and M12 for I/O and communication with integrated 24 V DC PSU without looping through without fieldbus",1760,"ST",1,"GMC",1,"6SL35212XL007AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-2XN00-7AB0","SINAMICS G115D wall-mounted Rated power: 0.75 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 400 V AC local remote control Q4/2 for 400 V AC and M12 for I/O and communication with integrated 24 V DC PSU with looping through without fieldbus",1796,"ST",1,"GMC",1,"6SL35212XN007AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-2XR14-0AB0","SINAMICS G115D wall-mounted Rated power: 4 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSB Protection class IP65/66 / UL Type 4X brake voltage 400 V AC local remote control with cable gland for 400 V AC Power M12 for 24 V DC with looping through M12 for I/O and communication without fieldbus",2394,"ST",1,"GMC",1,"6SL35212XR140AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-3XA20-7AF0","SINAMICS G115D wall-mounted Rated power: 0.75 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 400 V AC repair switch local remote control with cable gland with communication Fieldbus integrated: PROFINET PN, Ethernet IP",1910,"ST",1,"GMC",1,"6SL35213XA207AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-3XB40-3AB0","SINAMICS G115D wall-mounted rated power: 0.37 kW for 3s 200%, 57s 150%, 240s 87%, RFI suppression filter for category C2 3AC380-480V+10/-10% 45-66Hz ambient temperature -30 to +40 Â°C frame size: FSA degree of protection IP65/66 / UL type 4X brake voltage 400 V AC repair switch local remote control Q4/2 for 400 V AC and Power M12 for 24 V DC and M12 for I/O and communication without looping through Q8/0 for motor connection without fieldbus",1615,"ST",1,"GMC",1,"6SL35213XB403AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-3XC04-0AF0","SINAMICS G115D wall-mounted Rated power: 4 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSB Protection class IP65/66 / UL Type 4X brake voltage 400 V AC repair switch local remote control with Quickon for 400 V AC and Power M12 for 24 V DC and M12 for I/O and communication without looping through Q8/0 for motor connection Fieldbus integrated: PROFINET PN, Ethernet IP",3128,"ST",1,"GMC",1,"6SL35213XC040AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-3XE41-5AB0","SINAMICS G115D wall-mounted Rated power: 1.5kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 400 V AC repair switch local remote control Q4/2 for 400 V AC and Power M12 for 24 V DC and M12 for I/O and communication with looping through Q8/0 for motor connection without fieldbus",1956,"ST",1,"GMC",1,"6SL35213XE415AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-3XH64-0AF0","SINAMICS G115D wall-mounted Rated power: 4 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSB Protection class IP65/66 / UL Type 4X brake voltage 400 V AC repair switch local remote control with cable gland for 400 V AC and 24 V DC and M12 for I/O and communication with integrated 24 V DC PSU Fieldbus integrated: PROFINET PN, Ethernet IP",3186,"ST",1,"GMC",1,"6SL35213XH640AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-3XL02-2AA0","SINAMICS G115D wall-mounted Rated power: 2.2 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSB Protection class IP65/66 / UL Type 4X brake voltage 400 V AC repair switch local remote control Quickon for 400 V AC and M12 for I/O and communication with integrated 24 V DC PSU without looping through fieldbus integrated: AS-Interface",2610,"ST",1,"GMC",1,"6SL35213XL022AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-3XM00-7AA0","SINAMICS G115D wall-mounted Rated power: 0.75 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 400 V AC repair switch local remote control MQ(X)15 for 400 V AC and M12 for I/O and communication with integrated 24 V DC PSU without looping through fieldbus integrated: AS-Interface",2151,"ST",1,"GMC",1,"6SL35213XM007AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3525-0PE24-0AA1","SINAMICS G120D Power Module PM250D with integrated Class A filter capable of energy recovery. 380-480 V 3 AC+10/-10% 47-63Hz Power high overload: 4.0kW at 200% 3s, 150% 60S, 100% 300S Ambient temperature -10 to +55 Â°C 210x 450x 220 (HxWxD), FSC Degree of protection IP65 without Control Unit",2278,"ST",1,"GMC",1,"6SL35250PE240AA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3544-0FB21-1FA0","SINAMICS G120D Control Unit CU240D-2 PN-F PROFINET and Safety Integrated 6 DI/3 F-DI, 2 DO/1 F-DO, 2 AI USB interface SD/MMC card interface HTL encoder interface Degree of protection IP65 Ambient temperature 0 to +50 Â°C without Power Module",1191,"ST",1,"GMC",1,"6SL35440FB211FA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3760-8CV00-0DA0","Rittal VX25 protection kit - Active Interface Modules FS2/FS4/FS4+ - standard - 600mm/800mm",1442,"ST",1,"GMC",1,"6SL37608CV000DA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL4112-0JA08-0FF0","SINAMICS G220 200-240 V 3AC +10/-20% 47-63 Hz power low overload: 1.1 kW 150% 3 s, 110% 57 s power high overload: 0.75 kW 200% 3 s, 150% 57 s 415x 220x 225 (HxWxD) frame size: FSB degree of protection IP55 / UL type 12 safety SIL3 painting 3C2 with integrated braking chopper basic version unfiltered with SMTO (ATEX) module PROFINET PN, Modbus TCP",2592,"ST",1,"GMC",1,"6SL41120JA080FF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL4112-0JQ10-0FF0","SINAMICS G220 200-240 V 3AC +10/-20% 47-63 Hz power low overload: 1.5 kW 150% 3 s, 110% 57 s power high overload: 1.1 kW 200% 3 s, 150% 57 s 415x 220x 225 (HxWxD) frame size: FSB degree of protection IP55 / UL type 12 safety SIL3 painting 3C2 with integrated braking chopper NEC type cable gland of UL type 12 unfiltered with SMTO (ATEX) module PROFINET PN, Modbus TCP",2770,"ST",1,"GMC",1,"6SL41120JQ100FF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL4113-0CA11-0AF0","SINAMICS G220 380-500 V 3AC + 10/-20% 47-63 Hz power low overload: 2.2 kW 150% 3 s, 110% 57 s power high overload: 1.5 kW 200% 3 s, 150% 57 s 250x 73x 209 (HxWxD) frame size: FSA degree of protection IP20 / UL open type Safety SIL3 with integrated braking chopper basic version unfiltered communication PROFINET PN, MODBUS TCP",1570,"ST",1,"GMC",1,"6SL41130CA110AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL4113-0CA15-2AF0","SINAMICS G220 380-500 V 3AC + 10/-20% 47-63 Hz power low overload: 5.5 kW 150% 3 s, 110% 57 s power high overload: 4 kW 200% 3 s, 150% 57 s 355x 85x 209 (HxWxD) frame size: FSB degree of protection IP20 / UL open type Safety SIL3 with integrated braking chopper basic version radio interference suppression filter category C2 communication PROFINET PN, MODBUS TCP",2453,"ST",1,"GMC",1,"6SL41130CA152AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL4113-0JA12-0AF0","SINAMICS G220 380-500 V 3AC + 10/-20% 47-63 Hz power low overload: 3 kW 150% 3 s, 110% 57 s power high overload: 2.2 kW 200% 3 s, 150% 57 s 415x 220x 225 (HxWxD) frame size: FSB degree of protection IP55 / UL type 12 safety SIL3 painting 3C2 with integrated braking chopper basic version unfiltered communication PROFINET PN, Modbus TCP",2349,"ST",1,"GMC",1,"6SL41130JA120AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL4113-0JP08-2AF0","SINAMICS G220 380-500 V 3AC + 10/-20% 47-63 Hz power low overload: 1.1 kW 150% 3 s, 110% 57 s power high overload: 0.75 kW 200% 3 s, 150% 57 s 415x 220x 225 (HxWxD) frame size: FSB degree of protection IP55 / UL type 12 safety SIL3 painting 3C2 with integrated braking chopper IEC type cable gland, IP55 (basic version) radio interference suppression filter category C2 communication PROFINET PN, Modbus TCP",2036,"ST",1,"GMC",1,"6SL41130JP082AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL4113-0JP17-2AF0","SINAMICS G220 380-500 V 3AC + 10/-20% 47-63 Hz power low overload: 11 kW 150% 3 s, 110% 57 s power high overload: 7.5 kW 200% 3 s, 150% 57 s 460x 240x 250 (HxWxD) frame size: FSC degree of protection IP55 / UL type 12 safety SIL3 painting 3C2 with integrated braking chopper IEC type cable gland, IP55 (basic version) radio interference suppression filter category C2 communication PROFINET PN, Modbus TCP",4295,"ST",1,"GMC",1,"6SL41130JP172AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL4113-0JP27-2BF0","SINAMICS G220 380-500 V 3AC + 10/-20% 47-63 Hz power low overload: 55 kW 150% 3 s, 110% 57 s power high overload: 45 kW 200% 3 s, 150% 57 s 778x 327x 314 (HxWxD) frame size: FSE degree of protection IP55 / UL type 12 safety SIL3 painting 3C2 with integrated braking chopper IEC type cable gland, IP55 (basic version) radio interference suppression filter category C2 with DRIVE-CLiQ module PROFINET PN, Modbus TCP",12595,"ST",1,"GMC",1,"6SL41130JP272BF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL4113-0JQ24-0BF0","SINAMICS G220 380-500 V 3AC + 10/-20% 47-63 Hz power low overload: 37 kW 150% 3 s, 110% 57 s power high overload: 30 kW 200% 3 s, 150% 57 s 650x 270x 283 (HxWxD) frame size: FSD2 degree of protection IP55 / UL type 12 safety SIL3 painting 3C2 with integrated braking chopper NEC type cable gland of UL type 12 unfiltered with DRIVE-CLiQ module PROFINET PN, Modbus TCP",9009,"ST",1,"GMC",1,"6SL41130JQ240BF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL4113-2CA17-2BF0","SINAMICS G220 Clean Power 380-500 V 3AC + 10/-20% 47-63 Hz power low overload: 11 kW 150% 3 s, 110% 57 s power high overload: 7.5 kW 200% 3 s, 150% 57 s 400x 150x 245 (HxWxD) frame size: FSD1 degree of protection IP20 / UL open type safety SIL3 with integrated braking chopper basic version radio interference suppression filter category C2 with DRIVE-CLiQ module PROFINET PN, Modbus TCP",6392,"ST",1,"GMC",1,"6SL41132CA172BF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL4113-2DA24-2FF0","SINAMICS G220 Clean Power 380-500 V 3AC + 10/-20% 47-63 Hz power low overload: 37 kW 150% 3 s, 110% 57 s power high overload: 30 kW 200% 3 s, 150% 57 s 460x 200x 245 (HxWxD) frame size: FSD2 degree of protection IP20 / UL open type safety SIL3 painting 3C3 with integrated braking chopper basic version radio interference suppression filter category C2 with SMTO (ATEX) module PROFINET PN, Modbus TCP",13343,"ST",1,"GMC",1,"6SL41132DA242FF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL5510-1BE10-2AF0","SINAMICS S200, with PROFINET Input voltage: 380-480 V 3AC; -15%/+10%; 1.3A; 50/60Hz; Output voltage: 0-inpu 1.3A; 0-550Hz; Motor: 0.2kW Degree of protection: IP20 FSA, 50x180x200 (WxHxD)",1184,"ST",1,"GMC",1,"6SL55101BE102AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6XV1801-5AH50","Robust Power Connecting Cable M12-180/M12-180, IP69, for Power supply of the ET 200, pre-assembled cable with M12 plug and M12 socket, A-coded, 4-pole, 5.0 m.",90.8,"ΤΕΜ",1,"SIMATIC",1,"6XV18015AH50","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6XV1812-8A","Energy cable, 2-wire power line, stranded wire, 2x 0.75 mm2, trailable Delivery unit max. 2000 m minimum order quantity 20 m sold by the meter",3,"M",1,"SIMATIC",20,"6XV18128A","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6XV1820-5BT13","fiber optic cable (62.5/125), standard cable, splittable, pre-assembled with 4 BFOC connectors, length 130 m.",874,"ΤΕΜ",1,"SIMATIC",1,"6XV18205BT13","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6XV1830-5EH10","PB FC Process Cable GP/ Ethernet-APL cable GP, bus cable for IEC 61158-2 (PB) and IEC TS 60079-47 (2-WISE) sheath color blue for Ex applications 2-core shielded, sold by the meter delivery unit max. 1000 m minimum order quantity 20 m.",3.5,"M",1,"SIMATIC",20,"6XV18305EH10","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6XV1830-7BN10","PROFIBUS ECOFAST Hybrid Cable, 2xCu 0.64 mm, 4x Cu 1.5 mm2, Cable pre-assembled with ECOFAST plug and socket, trailable, length 10 m.",165,"ΤΕΜ",1,"SIMATIC",1,"6XV18307BN10","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6XV1861-3CT15","PCF Trailing Cable, pre-assembled with 2x2 BFOC plugs, insertion aid, length 150 m.",2106,"ΤΕΜ",1,"SIMATIC",1,"6XV18613CT15","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6XV1870-4GH40","Industrial Ethernet TP Cord RJ45/RJ45, CAT 6A, TP cable 4x2 (yellow), pre-assembled with 2 x RJ45 plugs, length 4 m.",30.700000000000003,"ΤΕΜ",1,"SIMATIC",1,"6XV18704GH40","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6XV1871-8AH15","IE connecting cable M12 push pull 180 / M12 push pull 180, only for ET200SP BusAdapter, preassembled with IE FC trailing cable GP, M12 plugs (D-coded, push-pull), length 1.5 m.",58.8,"ΤΕΜ",1,"SIMATIC",1,"6XV18718AH15","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6XV1873-3AN20","FO Standard Cable 50/125, pre-assembled with 2x2 BFOC connectors, length 20 m.",157,"ΤΕΜ",1,"SIMATIC",1,"6XV18733AN20","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6XV1875-5LE30","N-Connect/SMA male/ male flexible connection cable pre-assembled, Length 0.3 m, flexible connecting cable SCALANCE M antenna.",41,"ΤΕΜ",1,"SIMATIC",1,"6XV18755LE30","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6XV1878-5BH30","IE connecting cable IE FC RJ45 Plug-180/IE FC RJ45 Plug-180; IE FC flexible GP 4x2 cable Pre-assembled with 2x IE FC RJ45 plug 180 4 x 2; Length 3.0 m.",75.8,"ΤΕΜ",1,"SIMATIC",1,"6XV18785BH30","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["6XV1878-5TH15","IE TP Cord M12-180/RJ45-180 pre-assembled IE Flexible Cable, with 1x M12 plug (X-coded) 180 degrees cable outlet and 1x RJ45 plug; 180-degree cable outlet; length 1.5 m.",68.8,"ΤΕΜ",1,"SIMATIC",1,"6XV18785TH15","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["7KN2715-3CE40-0YC0","SENTRON powermanager system package including SENTRON powermanager license and including 3 x PAC3220",5517.96,"ΤΕΜ",1,"EP",1,"7KN27153CE400YC0","Sentron PAC μετρητές / αναλυτές ενέργειας"]
["7KT5821","electronic time counter 12-150V DC, 24-240V, 50Hz",151.11000000000001,"ΤΕΜ",1,"EP",1,"7KT5821","Sentron Χρονικά - χρονοδιακόπτες"]
["7ME3400-1CE00-2BA2","SITRANS FUS380 Mains or battery-operated ultrasonic In-Line flowmeter, diameter DN 50 to DN 1200 (2\" to 48\"). Suitable for volume flow measurement of liquids , for applications in district heating plants, local networks, boiler stations, chiller plants and water applications Siemens DN50 Die-cast bronze, qp=15m3/h. qs=45m3/h. qi=0.15m3/h. EN1092-1   PN40 Compact version, max. 120 Â°C (248 Â°F) . Pulse value: 1 L/p Power supply 115 - 230V AC . Pulse Width: 5 ms",2309,"ST",1,"PI1",1,"7ME34001CE002BA2","Όργανα Μέτρησης Πεδίου"]
["7ME3411-3CC31-5ER2","SITRANS FUE380 Mains or battery-operated ultrasonic In-Line flowmeter, diameter DN 50 to DN 1200 (2\" to 48\"), custody transfer approved. Suitable for volume flow and thermal energy measurement of liquids, for use in custody transfer meteringÂ in district heating plants, local networks, boiler stations, chiller plants. DANFOSS \"DN400 (16\"\") Carbon Steel,\" EN 1434, qp=950m3/h, qs=2660m3/h, qi=19m3/h EN1092-1   PN16 Remote version, Sensor link cabel (SSL) 10 m, with gland, DN50 to DN80: max. 150Â°C (302Â°F), DN100 to DN800 max. 200Â°C (392Â°F) Without EU type approval suitable for billing measurements outside Europe where national approvals exist Calibration according to selection pipe size / flow range Impulswert: 50 L/p (not suitable for FUE950 with nominal size 3L up to 5V) Power supply 115 - 230V AC, Backup: 3.6V DC Lithium battery, single pack is included Marking for Standard device with EU type examination certificate (MI004) Language on nameplate English Pulse width: 5 ms",9153,"ST",1,"PI1",1,"7ME34113CC315ER2","Όργανα Μέτρησης Πεδίου"]
["7ME3950-5LC21","Ultrasonic transit time Sensor Clamp-On, Universal Size B2 paired, dediziert, Ex Zone 0,1,2, Class 1, Div 1,2, any pipe materials, Liquid, Pipe Diameter range 12.7 - 50 mm (0.5 - 2 in), Temperature -40C - +121C (-40F - +250F) Housing Polyetherimide/StSt corrosion resistant, incl. Couplant 7ME39600UC20 and sanding block for FST020, FST030 (FUS1010)",1869,"ST",1,"PI1",1,"7ME39505LC21","Όργανα Μέτρησης Πεδίου"]
["7ME3950-5LR00","Ultrasonic transit time Sensor Clamp-On, High Precision, Size D4H, paired, dedicated, Ex Zone 0,1,2, Class 1, Div 1,2, for steel pipe, Liquid, Pipe wall thickness from 15,7 - 31,8 mm (0.62 - 1.25 in), Best Temperature <80C (<176F) max. -40C - +121C/-40F - +250F Housing Polyetherimide/StSt corrosion resistant, incl. Couplant 7ME39600UC20 and sanding block for FST020, FST030 (FUS1010)",3170,"ST",1,"PI1",1,"7ME39505LR00","Όργανα Μέτρησης Πεδίου"]
["7ME3960-0MS10","Dedicated spacer bar for pipes to DN 200 (liquid), DN 600 (gas) Legacy Part Number: 1012BN-1",193,"ST",1,"PI1",1,"7ME39600MS10","Όργανα Μέτρησης Πεδίου"]
["7ME5930-5CA00-0AA0","SITRANS FM Transmitter Intermag Cable kit for Transmag 911/E sensor, Coil cable 3 x 1.0 mm2, electrode cable7 x 0.5 mm2 shielded, PVC coatedLength: 10 m (32.8 ft) . . . without junction box . . .",558,"ST",1,"PI1",1,"7ME59305CA000AA0","Όργανα Μέτρησης Πεδίου"]
["7ME6140-2DB10-1AA1","SITRANS FM MAG 1100 F Full-bore electromagnetic flow sensor, sanitary design, diameter DN 10 to DN 100 (3/8\" to 4\"). Suitable for volume flow measurement of liquids (conductive) , for applications in F&B, pharmaceutical industry. . DN25, 1 Inch Weld in connection fittings: DIN11850 PFA (no ATEX) EPDM (FDA) Hastelloy C22 / 2.4602 Sensor for remote transmitter (Order transmitter separately) No bus Communication Metric cable glands, Polyamid terminal box or MAG 6000i integral mount",2082,"ST",1,"PI4",1,"7ME61402DB101AA1","Όργανα Μέτρησης Πεδίου"]
["7ME6140-3MA20-2AA1","SITRANS FM MAG 1100 F Full-bore electromagnetic flow sensor, sanitary design, diameter DN 10 to DN 100 (3/8\" to 4\"). Suitable for volume flow measurement of liquids (conductive) , for applications in F&B, pharmaceutical industry. . DN80, 3 Inch None (not 3A approved) Ceramic EPDM (FDA) Electrode material: Platinum Sensor for remote transmitter (Order transmitter separately) No bus Communication Metric cable glands, Polyamid terminal box or MAG 6000i integral mount",2473,"ST",1,"PI4",1,"7ME61403MA202AA1","Όργανα Μέτρησης Πεδίου"]
["7ME6310-3MC11-1AA1","SITRANS FM MAG 3100 Full-bore electromagnetic flow sensor, flanged, diameter DN 15 to DN 2000 (1/2\" to 78\"). Suitable for volume flow measurement of liquids (conductive), main applications in process industry, chemical industry, steel industry, mining, utility, power generation and distribution, O&G/HPI. . DN80, 3 Inch EN1092-1, PN16 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 Soft Rubber Stainless steel AISI 316Ti / 1.4571 (not for PFA) Sensor for remote transmitter (Order transmitter separately) No bus communication Metric cable glands, Polyamid terminal box or MAG 6000i integral mount",1829,"ST",1,"PI4",1,"7ME63103MC111AA1","Όργανα Μέτρησης Πεδίου"]
["7ME6340-3TJ17-2AA2","SITRANS FM MAG 3100 P Full-bore electromagnetic flow sensor, flanged, diameter DN 15 to DN 300 (1/2\" to 12\"). Suitable for volume flow measurement of liquids (conductive), main applications in chemical industry, process industry, pulp & paper, industrial wastewater. . DN100, 4 Inch ANSI B16.5, Class 150 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 PFA max 150 deg.C Hastelloy C without grounding electrodes Sensor for remote transmitter (order transmitter separately) No bus communication 1/2 inch NPT cable glands, Polyamid terminal box or MAG 6000i integral mount",2595,"ST",1,"PI4",1,"7ME63403TJ172AA2","Όργανα Μέτρησης Πεδίου"]
["7ME6520-2YC12-2AA1","SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. Successor product available. Please consider ordering the product SITRANS FMS500. If you need assistance please contact your Siemens sales representative. . DN50, 2 Inch EN 1092-1, PN 16 Carbon steel ASTM A 105, corrosion-resistant coating of category C4 Liner Material: EPDM Hastelloy C-276 incl. grounding electrodes Sensor for remote transmitter (order transmitter separately) No bus communication Metric cable glands, Polyamid terminal box or MAG 6000i integral mount",1402,"ST",1,"PI4",1,"7ME65202YC122AA1","Όργανα Μέτρησης Πεδίου"]
["7ME6520-4PB13-2HA1","SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. Successor product available. Please consider ordering the product SITRANS FMS500. If you need assistance please contact your Siemens sales representative. . DN200, 8 Inch EN 1092-1, PN 10 Carbon steel ASTM A 105, corrosion-resistant coating of category C4 Liner Material: NBR Hastelloy C-276 incl. grounding electrodes MAG 6000, IP67 / NEMA 4X/6, Polyamid enclosure, With display, 11-30V DC/11-24V AC 50/60 Hz No bus communication Metric cable glands, Polyamid terminal box or MAG 6000i integral mount",4061,"ST",1,"PI4",1,"7ME65204PB132HA1","Όργανα Μέτρησης Πεδίου"]
["7ME6520-4VB13-2AA1","SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. Successor product available. Please consider ordering the product SITRANS FMS500. If you need assistance please contact your Siemens sales representative. . DN250, 10 Inch EN 1092-1, PN 10 Carbon steel ASTM A 105, corrosion-resistant coating of category C4 Liner Material: NBR Hastelloy C-276 incl. grounding electrodes Sensor for remote transmitter (order transmitter separately) No bus communication Metric cable glands, Polyamid terminal box or MAG 6000i integral mount",2732,"ST",1,"PI4",1,"7ME65204VB132AA1","Όργανα Μέτρησης Πεδίου"]
["7ME6520-6FB12-2AA1","SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. Successor product available. Please consider ordering the product SITRANS FMS500. If you need assistance please contact your Siemens sales representative. . DN500, 20 Inch EN 1092-1, PN 10 Carbon steel ASTM A 105, corrosion-resistant coating of category C4 Liner Material: EPDM Hastelloy C-276 incl. grounding electrodes Sensor for remote transmitter (order transmitter separately) No bus communication Metric cable glands, Polyamid terminal box or MAG 6000i integral mount",7782,"ST",1,"PI4",1,"7ME65206FB122AA1","Όργανα Μέτρησης Πεδίου"]
["7ME6520-6PB12-2JA1","SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. Successor product available. Please consider ordering the product SITRANS FMS500. If you need assistance please contact your Siemens sales representative. . DN600, 24 Inch EN 1092-1, PN 10 Carbon steel ASTM A 105, corrosion-resistant coating of category C4 Liner Material: EPDM Hastelloy C-276 incl. grounding electrodes MAG 6000, IP67 / NEMA 4X/6, Polyamid enclosure, With display, 115-230V AC 50/60 Hz No bus communication Metric cable glands, Polyamid terminal box or MAG 6000i integral mount",10509,"ST",1,"PI4",1,"7ME65206PB122JA1","Όργανα Μέτρησης Πεδίου"]
["7ME6530-2YC03-1AA0-Z A02","SITRANS FMS500 sensor No transmitter (sensor only) DN 50, 2 inch EN 1092-1 PN16 flanges Carbon steel ASTM A 105 with corrosion-resistant coating acc. to EN ISO 12944 grade C4 NBR (soft rubber) Hastelloy C276 / 2.4819 No transmitter (sensor only) . No transmitter (sensor only) M20x1.5, material polyamide",1367,"ST",1,"PI4",1,"7ME65302YC031AA0Z A02","Όργανα Μέτρησης Πεδίου"]
["7ME6530-5RC02-1AA0-Z A02+D02","SITRANS FMS500 sensor No transmitter (sensor only) DN 500, 20 inch EN 1092-1 PN16 flanges Carbon steel ASTM A 105 with corrosion-resistant coating acc. to EN ISO 12944 grade C4 EPDM (soft rubber) Hastelloy C276 / 2.4819 No transmitter (sensor only) . No transmitter (sensor only) M20x1.5, material polyamide High accuracy factory calibration 0.2% DN 250… 600, 10 inch… 24 inch",8871,"ST",1,"PI4",1,"7ME65305RC021AA0Z A02+D02","Όργανα Μέτρησης Πεδίου"]
["7ME6532-4PB02-1GA2-Z A02","SITRANS FMS500 sensor Transmitter SITRANS FMT020 DN 200, 8 inch EN 1092-1 PN10 flanges Carbon steel ASTM A 105 with corrosion-resistant coating acc. to EN ISO 12944 grade C4 EPDM (soft rubber) Hastelloy C276 / 2.4819 Compact design (integral mount), plastic enclosure . 24 V DC M20x1.5, material polyamide",4003,"ST",1,"PI4",1,"7ME65324PB021GA2Z A02","Όργανα Μέτρησης Πεδίου"]
["7ME6532-5BC02-1GA3-Z A02+D02","SITRANS FMS500 sensor Transmitter SITRANS FMT020 DN 300, 12 inch EN 1092-1 PN16 flanges Carbon steel ASTM A 105 with corrosion-resistant coating acc. to EN ISO 12944 grade C4 EPDM (soft rubber) Hastelloy C276 / 2.4819 Compact design (integral mount), plastic enclosure . 100...240 V AC, 50/60 Hz M20x1.5, material polyamide High accuracy factory calibration 0.2% DN 250… 600, 10 inch… 24 inch",6536,"ST",1,"PI4",1,"7ME65325BC021GA3Z A02+D02","Όργανα Μέτρησης Πεδίου"]
["7ME6532-5HC03-1GA3-Z A02+D02","SITRANS FMS500 sensor Transmitter SITRANS FMT020 DN 400, 16 inch EN 1092-1 PN16 flanges Carbon steel ASTM A 105 with corrosion-resistant coating acc. to EN ISO 12944 grade C4 NBR (soft rubber) Hastelloy C276 / 2.4819 Compact design (integral mount), plastic enclosure . 100...240 V AC, 50/60 Hz M20x1.5, material polyamide High accuracy factory calibration 0.2% DN 250… 600, 10 inch… 24 inch",8590,"ST",1,"PI4",1,"7ME65325HC031GA3Z A02+D02","Όργανα Μέτρησης Πεδίου"]
["7ME6810-3MC31-1AB1","SITRANS FM MAG 8000 Battery-operated electromagnetic flowmeter, flanged, diameter DN 25 to DN 1200 (1\" to 48\"). Suitable for volume flow measurement of liquids (conductive) and water applications within abstraction, distribution network, revenue metering and irrigation. . DN80 / Qmx  160 m3/h(m3), 3 Inch / Qmx 704 GPM(Gx100), DN80 / Qmx 3.84 Ml/d(Ml) EN 1092-1, PN 16, Conforms to PED EPDM liner and Hastelloy Electrodes, corrosion-resistant coating of category C4 Standard calibration w. max. 0,4% of rate +/- 2mm/s with certificate Region version: Europe Display: m3 based 50 Hz filter Basic version compact Transmitter on sensor Communication: Serial RS 485 interface module Modbus  RTU Internal 2 D-cell battery pack installed and disconnected inside meter",3934,"ST",1,"PI7",1,"7ME68103MC311AB1","Όργανα Μέτρησης Πεδίου"]
["7ME6810-4PC32-1CA1","SITRANS FM MAG 8000 Battery-operated electromagnetic flowmeter, flanged, diameter DN 25 to DN 1200 (1\" to 48\"). Suitable for volume flow measurement of liquids (conductive) and water applications within abstraction, distribution network, revenue metering and irrigation. . DN200 / Qmx  997 m3/h(m3), 8 Inch / Qmx 4389 GPM(Gx100) , DN200 / Qmx 24 Ml/d(Ml) EN 1092-1, PN 16, Conforms to PED EPDM liner and Hastelloy Electrodes, corrosion-resistant coating of category C4 Extended calibration 0,2% of rate +/- 2mm/s with certificate Region version: Europe Display: m3 based 50 Hz filter Basic version remote 10m Mounted sensor cables w. plugs No additional communication, Standard IrDA interface Internal 2 D-cell battery pack installed and disconnected inside meter",5753,"ST",1,"PI7",1,"7ME68104PC321CA1","Όργανα Μέτρησης Πεδίου"]
["7ME6820-3MC00-1DS1","SITRANS FM MAG 8000 CT Battery-operated electromagnetic flowmeter, flanged, custody transfer approved. Suitable for volume flow measurement of liquids (conductive) and water applications within abstraction, distribution network, revenue metering and custody transfer metering. . DN 80, 3 Inch EN 1092-1, PN 16, Conforms to PED EPDM liner and Hastelloy electrodes, corrosion-resistant coating of category C4 Without initial verification (standard calibration) Region version: Europe Display: m3, m3/h based 50 Hz filter Basic version remote 20m Mounted sensor cables w. plugs 3G/UMTS module for MAG8000 with remote antenna cable(5m) Internal 2 D-cell battery pack installed and disconnected inside meter",6020,"ST",1,"PI7",1,"7ME68203MC001DS1","Όργανα Μέτρησης Πεδίου"]
["7ME6940-1CM10","Accessory SITRANS FMT020 HART communication add-on module with 4â€¦20 mA output, active or passive",272,"ST",1,"PI4",1,"7ME69401CM10","Όργανα Μέτρησης Πεδίου"]
["7MF1565-5BA01-1AA1","SITRANS P200 Transmitters for pressure and absolute pressure for general applications Non-linearity: 0,25 percent (typically) wetted parts material:ceramics, stainless steel plus sealing material; non-wetted parts material: stainless steel Measuring range for absolute: 0 to 1 bar abs., Overload- pressure 2,5 bar abs. Output signal: 4 to 20 mA two-wire connection, power supply DC 7 to 33 V Explosion protection: EEx ia Electrical connection: plug to DIN EN 175301-803-A, threat for packed gland M16 (with connector) Process connection: G1/2\" male to EN 837-1 (1/2\" BSP male) (standard for metric pressure ranges mbar, bar) Sealing material between sensor and housing: Viton (FPM, Standard) Standard version",258,"ST",1,"PI2",1,"7MF15655BA011AA1","Όργανα Μέτρησης Πεδίου"]
["7MF1565-5BE10-1AA1","SITRANS P200 Transmitters for pressure and absolute pressure for general applications Non-linearity: 0,25 percent (typically) wetted parts material:ceramics, stainless steel plus sealing material; non-wetted parts material: stainless steel Measuring range for absolute: 0 to 4 bar abs., Overload- pressure 10 bar abs. Output signal: 0 to 10 V; three-wire connection, power supply DC 12 to 33 V without explosion protection Electrical connection: plug to DIN EN 175301-803-A, threat for packed gland M16 (with connector) Process connection: G1/2\" male to EN 837-1 (1/2\" BSP male) (standard for metric pressure ranges mbar, bar) Sealing material between sensor and housing: Viton (FPM, Standard) Standard version",214,"ST",1,"PI2",1,"7MF15655BE101AA1","Όργανα Μέτρησης Πεδίου"]
["7MF1567-3DE00-2QA1","SITRANS P220 Transmitters for pressure and absolute pressure fully welded version for high-pressure and refrigerant applications Non-linearity: 0,25 Percent (typically) wetted parts material: stainless steel;  non-wetted parts material: stainless steel Measuring range for gauge: 0 to 400 bar, Overload- pressure 1000 bar Output signal: 4 to 20 mA two-wire connection, power supply DC 7 to 33 V without explosion protection Electrical connection: round plug M12 to IEC 61076-2-101 Process Connection: G1/4\" to DIN3852, form E Standard version Standard version",209,"ST",1,"PI2",1,"7MF15673DE002QA1","Όργανα Μέτρησης Πεδίου"]
["7MF1572-1FA11","Transmitters SITRANS LH100 for hydrostatic level measurement, submersible transmitter, two-wire connection, 4...20 mA housing material 316L (1.4404) measuring cell ceramics (96%) with fixed mounted LD-PE cable Measuring range: 0 - 6 mH2O Cable lenght: 10 m . . Sealing material between sensor and housing: FPM (standard) with ATEX II1 G Ex ia IIC T4 Ga and IECEx Ex ia IIC T4 Ga",724,"ST",1,"PI2",1,"7MF15721FA11","Όργανα Μέτρησης Πεδίου"]
["7MF7903-1BB","Transmitter electronics, PROFIBUS PA, Ex i",699,"ST",1,"PI1",1,"7MF79031BB","Όργανα Μέτρησης Πεδίου"]
["7MF7906-2EQ","Plug Han 8D, metal, blue, straight",163,"ST",1,"PI1",1,"7MF79062EQ","Όργανα Μέτρησης Πεδίου"]
["7MF8010-1AD31-1CE1","SITRANS P Transmitter Compact for pressure and absolut pressure for food, pharmaceu- ticals and biotechnology, with diaphragm flush at front. 2-wire system, process tempera- ture up to 140 deg. Cel., accuracy 0.2 % of f.s.v. output signal: 4...20 mA, Process connection: quick-release connection: connection o.cc.according DIN 11851 with slotted union nut: DN 25 Filling liquid: liquid FDA approved Output signal : 4-20 mA Housing(stainless steel1.4404)/ electrical connection: housing with angeld plug according DIN 43650, IP65 Measuring range: 0...6 bar overload pressure: 60 bar Without explosion protection",531,"ST",1,"PI2",1,"7MF80101AD311CE1","Όργανα Μέτρησης Πεδίου"]
["7MF9007-7AA","Sealing ring acc. EN837-1, threat G1/2 copper (1 set = 100 pieces)",102,"SZ",1,"PI2",1,"7MF90077AA","Όργανα Μέτρησης Πεδίου"]
["7MF9401-7BA","SHUT-OFF VALVE DESIGN B, DIN 16271, WITH TEST AND CONNECTION COLLARS, MAX. OPERATING PRESSURE 250 BAR MAT. NO. 2.0402 PRESSURE EQUIPMENT DIREKTIVE F. GAS 1/LIQUIDS 1 ART. 3.3 SEP",72,"ST",1,"PI2",1,"7MF94017BA","Όργανα Μέτρησης Πεδίου"]
["7MH4138-6AA00-0BA0","SIMATIC ET 200SP, TM SIWAREX WP321 ST, single-channel weighing module for platform or hopper scales with analog load cells, 1xRS485, 1xLC load cell interface (1-4mV/V), suitable for BU type A0, packing quantity: 1 unit",647,"ST",1,"PI1",1,"7MH41386AA000BA0","Όργανα Μέτρησης Πεδίου"]
["7MH5103-3PD00","Siwarex WL 260 Load Cell SP-S AB 500kg C3 - Rated Load 500kg - Accuracy class C3 - no legal-for-trade - 3m Cable length, 6 Conductor - Material Aluminium - Degree of protection IP65",506,"ST",1,"PI1",1,"7MH51033PD00","Όργανα Μέτρησης Πεδίου"]
["7MH5108-3PD01","Load Cell Siwarex WL 270 CP-S SA 0.5t C3, Rated Load 0.5t, Accuracy class C3, not legal for trade, 15m Cable length, 4 Conductor, Material Stainless steel, Type of protection IP68, with explosion protection",830,"ST",1,"PI1",1,"7MH51083PD01","Όργανα Μέτρησης Πεδίου"]
["7MH5113-4LD01","SIWAREX WL280 Load Cell RN-S SA 3.5t C3 Ex - Rated Load 3.5t - Accuracy class C3 according to OIML R60, - 6 m Cable length, 4 Wires - Made of Stainless steel - protection class IP68 Explosion protection",1408,"ST",1,"PI1",1,"7MH51134LD01","Όργανα Μέτρησης Πεδίου"]
["7MH5118-2AD00","Siwarex WL260 Load Cell SP-S SC 10kg C3 - Rated Load 10kg - Accuracy class C3 acc. to OIML R60 - 3m Cable length, 6 wires - Made of Stainless steel - protection class IP68 / IP69K",749,"ST",1,"PI1",1,"7MH51182AD00","Όργανα Μέτρησης Πεδίου"]
["7MH5118-3PD00","Siwarex WL260 Load Cell SP-S SC 500kg C3 - Rated Load 500kg - Accuracy class C3 acc. to OIML R60 - 3m Cable length, 4 wires - Made of Stainless steel - protection class IP68 / IP69K",1035,"ST",1,"PI1",1,"7MH51183PD00","Όργανα Μέτρησης Πεδίου"]
["7MH5121-5AF00","SIWAREX WL230 LOAD CELL SB-S CA 10T C5 - NOMINAL LOAD 10 T - ACCURACY C5 - 6 M CABLE, 4 WIRE - MATERIAL NICKEL PLATED STEEL - TYPE OF PROTECTION IP67",670,"ST",1,"PI1",1,"7MH51215AF00","Όργανα Μέτρησης Πεδίου"]
["7MH5721-4PH10","SIWAREX WL230 SB-S CA load foot - rated load 2.5 to 5t - steel, nickel plated - NBR - height-adjustable",73,"ST",1,"PI1",1,"7MH57214PH10","Όργανα Μέτρησης Πεδίου"]
["7MH7560-1AA05","Sitrans AS100: acoustic sensor for flow detection. It can warn of changes to material flow to prevent costly damage or downtime. Sensor: Standard temperature range (-20 C to +80 C) Cable length: 4 meters (13.12 ft) Sensor mounting: none . Approvals: FM/CSA Class II, Div. 1, Groups E, F, & G; ATEX II 3D, Ex tc IIIC T100Â°C Dc, Ta = -20Â°C to +80Â°C, IP68 (includes M20 female fitting); UKEX II 3D, Ex tc IIIC T100Â°C Dc, Ta = -20Â°C to +80Â°C, IP68 (includes M20 female fitting); EAC Ex Ex tc IIIC T100Â°C Dc; CE, UKCA, RCM",1699,"ST",1,"PI1",1,"7MH75601AA05","Όργανα Μέτρησης Πεδίου"]
["7MH7723-1DQ","SILICONE INNER DIAPHRAGM, WFS320/ILE-61,SPARE",196,"ST",1,"PI1",1,"7MH77231DQ","Όργανα Μέτρησης Πεδίου"]
["7MH7723-1JA","WW100 START STOP CONTROLLER",866,"ST",1,"PI1",1,"7MH77231JA","Όργανα Μέτρησης Πεδίου"]
["7MH7723-1LP","WF100 LOADCELL SPARE 2 LBS",2447,"ST",1,"PI1",1,"7MH77231LP","Όργανα Μέτρησης Πεδίου"]
["7MH7723-1NA","CONDUIT REPLACEMENT KIT 6 meters of flexible conduit with conduit fittings For MLC, MUS, MUS, MSI/MMI belt scales and RBSS, TASS speed sensors.",416,"ST",1,"PI1",1,"7MH77231NA","Όργανα Μέτρησης Πεδίου"]
["7MH7724-1BK","MLC Calibration weight, (Stainless Steel 304(1.4301)) For scales with belt width of 48\", 1200mm, 6.06 lbs (2.75 kg)",263,"ST",1,"PI1",1,"7MH77241BK","Όργανα Μέτρησης Πεδίου"]
["7MH7725-1DX","LOAD CELL PBD-23900250, With Hardware,MSI,750LB, Stainless Steel, CSA/FM/ATEX, F, SPARE",2221,"ST",1,"PI1",1,"7MH77251DX","Όργανα Μέτρησης Πεδίου"]
["7ML1115-3BA40","EchoMax XPS-10 Ultrasonic level transducer: continuous, non-contact, 10 m (32.80 ft), for liquids and solids. Mounting thread and facing: R 1\" ((BSPT) EN 10226-1) Cable length: 5 m (16.40 ft) Mounting flange: None Approvals: CSA Class 1 Div. 1 .",752,"ST",1,"PI3",1,"7ML11153BA40","Όργανα Μέτρησης Πεδίου"]
["7ML1123-0EA50","EchoMax XPS-30 Ultrasonic level transducer: continuous, non-contact, 30 m (98.42 ft) for liquids and solids. Mounting thread and facing: 1 1/2\" universal thread Cable length: 30 m (98.43 ft) Flange: Without mounting flange Approvals: ATEX II 1D, 2G Ex mb IIC T4 Gb, ATEX II 1D, 2G Ex tb IIIC T135Â°C Da, Ta = -40Â°C to +95Â°C; UKEX II 1D, 2G Ex mb IIC T4 Gb, UKEX II 1D, 2G Ex tb IIIC T135Â°C Da, Ta = -40Â°C to +95Â°C; IECEx SIR 13.0009X Ex mb IIC T4 Gb, IECEx SIR 13.0009X Ex tb IIIC T135Â°C Da, Ta = -40Â°C to +95Â°C Instruction Manual: Multi-Language Quick Start",1826,"ST",1,"PI3",1,"7ML11230EA50","Όργανα Μέτρησης Πεδίου"]
["7ML1930-1BQ","RD100 2\"(5.08cm) Pipe Mounting Kit for Stainless",117,"ST",1,"PI1",1,"7ML19301BQ","Όργανα Μέτρησης Πεδίου"]
["7ML1930-1CY","Steel Enclosure for 5 RD Display",904,"ST",1,"PI1",1,"7ML19301CY","Όργανα Μέτρησης Πεδίου"]
["7ML1930-6AF","RD300 RS-232 Serial Adapter",199,"ST",1,"PI1",1,"7ML19306AF","Όργανα Μέτρησης Πεδίου"]
["7ML5320-1AA06-0AP0","SITRANS LR120 Radar level transmitter, continuous, non-contact, 30 m (98.4 ft) range, for liquids slurries, and solids, integrated cable connection. Communications: HART (4 ... 20 mA) Bluetooth function: With Cable length: 5m . . . . Type of protection: Non Ex (ordinary locations) cFMus, cCSAus,CE, RCM Electrical connection of the cable entry: 1\" NPT .",1258,"ST",1,"PI1",1,"7ML53201AA060AP0","Όργανα Μέτρησης Πεδίου"]
["7ML5731-1AB11-1AA0","SITRANS LVS200 Vibrating fork point level switch, standard design: level and material detection in dry bulk solids. Extension options to 4 m (13.12 ft). With advanced testing, output, and durability options, including low bulk densities. Power supply: 19 to 230 V AC, 19 to 55 V DC, one relay output (SPDT) Process temperature: Without temperature isolator Process connection Threaded: 1-1/2 inch NPT ((Taper), ANSI/ASME B1.20.1) Extension length: Stainless steel 304 (1.4301): Standard length, 235 mm (9.25 inch) Material process connection/ extension: Stainless steel threads 304 (1.4301) flanges 321 (1.4541), triclamp 304 (1.4301) Approvals: CSA/FM Dust Ignition Proof, RCM . .",949,"ST",1,"PI1",1,"7ML57311AB111AA0","Όργανα Μέτρησης Πεδίου"]
["7ML5744-1CA00-0A","SITRANS RD300 Display: remote digital panel mount process display with current or voltage inputs. Two input, multi-line display, totalizer and pump control. Input voltage: 85 ... 265 V AC,50/60 Hz; 90 ... 265 V DC, 20 W max Output: 4 Relays Type: Single input process and flow rate totalizer Meter Display: Standard Approvals: UL & C-UL & CE . .",794,"ST",1,"PI1",1,"7ML57441CA000A","Όργανα Μέτρησης Πεδίου"]
["7ML5745-1AA02-1AA0","SITRANS LVL100 Vibrating point level switch. Detects level and material in liquids and slurries. Compact, with 40 mm (1.6 inch) insertion. Approvals: ordinary location, CE Version/Process Temperature: Standard -40 to 100 C Process connection: Thread G 3/4\" A PN64 / 316L Electronics: Transistor output PNP 10...55 V DC Housing: 316L Electrical connection / Protection: M12x1 / IP67 . .",331,"ST",1,"PI1",1,"7ML57451AA021AA0","Όργανα Μέτρησης Πεδίου"]
["7ND4801-7CK","Internal Memory  512Mb for SIREC D300/400",537,"ST",1,"PI1",1,"7ND48017CK","Όργανα Μέτρησης Πεδίου"]
["7NG0320-0HA10-0AA0","SITRANS TR320 Temperature transmitter for rail mounting, with one configurable input and a galvanically isolated 2-wire output. HART (4 â€¦ 20 mA) Input 1 TC Type J None Internal CJC Without enclosure (head mounted and rail mounted transmitter) . General purpose (CE, RCM, FM, KC, EAC, CSA) None (head mounted and rail mounted transmitter) Without local operation",423,"ST",1,"PI1",1,"7NG03200HA100AA0","Όργανα Μέτρησης Πεδίου"]
["7VV3002-3BD20","overvoltage protection module for max. permissible supply voltage 550 V and rated operate voltage 1500 V NMA: 449411910100",16651,"ST",1,"GMC",1,"7VV30023BD20","Ρυθμιστές στροφών και συστήματα Motion control"]
["8GB4563","SIMBOX 63 intermediate frame 3-R for 70 mm devices in N distribution board",81.73,"ΤΕΜ",1,"EP",1,"8GB4563","Simbox πίνακες διανομής"]
["8GF7147","Stab/SIKUS Universal Section cover without cutouts Fixed, H=1000 mm W=250 mm",90.49,"ΤΕΜ",1,"EP",1,"8GF7147","8GF εξαρτήματα πινάκων"]
["8GF9320-1","ISO pedestal high N/PE for 2 busbars 6x 6 mm (1 set = 2 units)",5.17,"ΣΕΤ",1,"EP",10,"8GF93201","8GF εξαρτήματα πινάκων"]
["8GK1031-3KK10","ALPHA 160 DIN flush-mounted board SK2, h=800 w=300 d=120",314.43,"ΤΕΜ",1,"EP",1,"8GK10313KK10","Alpha πίνακες διανομής"]
["8GK1052-4KK41","ALPHA 160, wall-mounted cabinet, Surface mounting, with distribution board panel, IP44, Protection class 2, H: 950 mm, W: 1050 mm, T: 140 mm, RAL 9016",1381.76,"ΤΕΜ",1,"EP",1,"8GK10524KK41","Alpha πίνακες διανομής"]
["8GK1081-4KK30","ALPHA 160 DIN flush-mounted board with mounting kit for modular devices, and terminal blocks RAL 9016, IP31, row distance 150mm SK2, h=950 w=800 d=120",1316.48,"ΤΕΜ",1,"EP",1,"8GK10814KK30","Alpha πίνακες διανομής"]
["8GK1121-4KK22","ALPHA 400, wall-mounted cabinet, Flush-mounting, IP31, type of protection 1, H: 950 mm, W: 550 mm, T: 210 mm, RAL 9016",410.31,"ΤΕΜ",1,"EP",1,"8GK11214KK22","Alpha πίνακες διανομής"]
["8GK1132-6KA22","ALPHA 400, wall-mounted cabinet, IP44, Protection class 2, H: 1250 mm, W: 550 mm, T: 210 mm, RAL 9016",626.14,"ΤΕΜ",1,"EP",1,"8GK11326KA22","Alpha πίνακες διανομής"]
["8GK1322-8KA52","ALPHA 630, Floor-mounted cabinet, IP44, Protection class 1, H: 1950 mm, W: 1300 mm, T: 210 mm, RAL 7035, incl. flange in roof",1587.07,"ΤΕΜ",1,"EP",1,"8GK13228KA52","Alpha πίνακες διανομής"]
["8GK1332-8KA12","ALPHA 630, Floor-mounted cabinet, IP44, Protection class 2, H: 1950 mm, W: 300 mm, T: 210 mm, RAL 7035",1045.1400000000001,"ΤΕΜ",1,"EP",1,"8GK13328KA12","Alpha πίνακες διανομής"]
["8GK1483-8KP35","Transformer cabinet safety class 1, IP30 h=1950 w=800 d=400 sheet metal door open sidewalls",7067.04,"ΤΕΜ",1,"EP",1,"8GK14838KP35","Alpha πίνακες διανομής"]
["8GK2325-5KK43","ALPHA 630 UNIVERSAL, Floor-mounted cabinet, IP55, Protection class 1, H: 1600 mm, W: 900 mm, T: 250 mm, RAL 7035, without door",1054.82,"ΤΕΜ",1,"EP",1,"8GK23255KK43","Alpha πίνακες διανομής"]
["8GK4351-2KK21","ALPHA 160 DIN, Mounting kit for modular installation devices, Clearance between rows 150 mm, H=300 W=500",80.33,"ΤΕΜ",1,"EP",1,"8GK43512KK21","Alpha πίνακες διανομής"]
["8GK4451-4KK22","ALPHA 400/630 DIN, Assembly kit Mounting plate with Section cover closed, H=600 W=500",204.19,"ΤΕΜ",1,"EP",1,"8GK44514KK22","Alpha πίνακες διανομής"]
["8GK4652-3KK12","ALPHA 400/630 assembly kit H=450 W=250 1x 3NP1153 (NH2) on busbar 60 mm (without busbar holder) for busbar holder 8GK9711-0KK03 busbar holder separate order",134.94999999999999,"ΤΕΜ",1,"EP",1,"8GK46523KK12","Alpha πίνακες διανομής"]
["8GK4704-4KK13","ALPHA 630 DIN Assembly kit for 3 and 4-pole Circuit breaker 3VL630, H=600 W=500",233.57,"ΤΕΜ",1,"EP",1,"8GK47044KK13","Alpha πίνακες διανομής"]
["8GK4733-2KK22","Assembly kit Molded case circuit breaker 3VA 3 x 3VA10 and 3VA11 to 160 A with front rotary operating mechanism H=300, W=500",171.28,"ΤΕΜ",1,"EP",1,"8GK47332KK22","Alpha πίνακες διανομής"]
["8GK6430-4KK23","ALPHA NF assembly kit for 3KD Switch disconnector Size 1 to 4 H=400 mm, W=600 mm 2x 3KD size 1 and 2 or 1x 3KD size 3 and 4 for door-coupling rotary operating mechanism in section cover",248.43,"ΤΕΜ",1,"EP",1,"8GK64304KK23","Alpha πίνακες διανομής"]
["8GK6712-2KK23","ALPHA 630 Universal, Circuit breaker kit 1x 3VL160X, 3+4-pole H=200 mm W=600 mm, horizontal Installation, with RCD module",166.71,"ΤΕΜ",1,"EP",1,"8GK67122KK23","Alpha πίνακες διανομής"]
["8GK6735-6KK33","ALPHA 630 Universal Circuit breaker kit 5x 3VA10-11/100A/160A 3+4-pole H=600 mm W=900 mm, horizontal Installation for RCD module infeed side",343.22,"ΤΕΜ",1,"EP",1,"8GK67356KK33","Alpha πίνακες διανομής"]
["8GK6750-4KK33","ALPHA 630 Universal Circuit breaker kit 7x 3VT1 3+4-pole H=400 mm W=900 mm Vertical installation",203.48,"ΤΕΜ",1,"EP",1,"8GK67504KK33","Alpha πίνακες διανομής"]
["8GK9126-7KK00","Connection kit for ALPHA 630 Universal, IP43, H=1200",86.07,"ΤΕΜ",1,"EP",1,"8GK91267KK00","Alpha πίνακες διανομής"]
["8GK9505-6KK33","ALPHA 630 Universal, Door IP55, Transparent (simple version), RAL 7035, H=1000, W=900",334.26,"ΤΕΜ",1,"EP",1,"8GK95056KK33","Alpha πίνακες διανομής"]
["8GK9511-8KK38","ALPHA, door half, on the right, IP31, H: 1400 mm, W: 275 mm, RAL 9016, type of protection 1 and 2",129.85,"ΤΕΜ",1,"EP",1,"8GK95118KK38","Alpha πίνακες διανομής"]
["8GK9520-0KK30","ALPHA AS side panel horizontal Sheet steel",31.14,"ΤΕΜ",1,"EP",1,"8GK95200KK30","Alpha πίνακες διανομής"]
["8GK9601-1KK10","ALPHA 630 DIN, cover Height=150 mm, Width=250 mm, Closed Minimum order quantity 10 units",19.329999999999998,"ΤΕΜ",1,"EP",10,"8GK96011KK10","Alpha πίνακες διανομής"]
["8GK9607-2KK10","ALPHA 630 Universal, Section cover without cutouts H=400 mm, W=300 mm",63,"ΤΕΜ",1,"EP",1,"8GK96072KK10","Alpha πίνακες διανομής"]
["8GK9613-1KK30","ALPHA 630 Universal, Section cover for 4 measuring instruments 96x 96+1 changeover H=200 mm W=900 mm",111.14,"ΤΕΜ",1,"EP",1,"8GK96131KK30","Alpha πίνακες διανομής"]
["8GK9900-0KK43","ALPHA, Base, H: 100 mm, W: 1050 mm, T: 250 mm, RAL 7035",236.48,"ΤΕΜ",1,"EP",1,"8GK99000KK43","Alpha πίνακες διανομής"]
["8GK9910-0KK30","ALPHA 160/400 DIN, Support for section cover 1 set=4 supports Minimum order quantity=5 sets",13.06,"ΣΕΤ",1,"EP",5,"8GK99100KK30","Alpha πίνακες διανομής"]
["8GK9920-0KK43","ALPHA 630 Universal, Transport rail kit H1200 vertical",137.77000000000001,"ΤΕΜ",1,"EP",1,"8GK99200KK43","Alpha πίνακες διανομής"]
["8MF1000-2CD00","SIVACON, trim strip, W: 1000 mm, Petrol",151.72999999999999,"ΤΕΜ",1,"EP",1,"8MF10002CD00","8MF Sivacon Πίνακες"]
["8MF1000-2VE","SIVACON, Rotary handle insert, Daimler",70.34,"ΤΕΜ",1,"EP",1,"8MF10002VE","8MF Sivacon Πίνακες"]
["8MF1004-2AF20","SIVACON, compartment bottom, D: 400 mm, W: 1000 mm, zinc-plated",262.86,"ΤΕΜ",1,"EP",1,"8MF10042AF20","8MF Sivacon Πίνακες"]
["8MF1008-2HN","SIVACON, bar for improving the EMC, Installation in the cabinet depth, EMC, T: 800 mm, zinc-plated",92.99,"ΤΕΜ",1,"EP",1,"8MF10082HN","8MF Sivacon Πίνακες"]
["8MF1008-3BR4","SIVACON, Control panel Empty enclosure, without side panels, according to IEC 62208, IP40, H: 2000 mm, W: 1000 mm, T: 800 mm",3679.98,"ΤΕΜ",1,"EP",1,"8MF10083BR4","8MF Sivacon Πίνακες"]
["8MF1025-2GS30","SIVACON, Supporting structure, for standard Empty enclosure, H: 2000 mm, W: 1200 mm, T: 500 mm, zinc-plated",855.64,"ΤΕΜ",1,"EP",1,"8MF10252GS30","8MF Sivacon Πίνακες"]
["8MF1028-2GS40","SIVACON, Supporting structure, for standard Empty enclosure, H: 2000 mm, W: 1200 mm, T: 800 mm, RAL 7035",1249.02,"ΤΕΜ",1,"EP",1,"8MF10282GS40","8MF Sivacon Πίνακες"]
["8MF1036-2AS30","SIVACON, mounting rail, compact for door width 500 mm, L: 366 mm, zinc-plated",37.880000000000003,"ΤΕΜ",1,"EP",1,"8MF10362AS30","8MF Sivacon Πίνακες"]
["8MF1045-2UB32-0","SIVACON, base, with cable entry, IPXX, T: 500 mm, W: 400 mm, zinc-plated",116.93,"ΤΕΜ",1,"EP",1,"8MF10452UB320","8MF Sivacon Πίνακες"]
["8MF1046-2UB32-0","SIVACON, base, with cable entry, IPXX, T: 600 mm, W: 400 mm, zinc-plated",131.25,"ΤΕΜ",1,"EP",1,"8MF10462UB320","8MF Sivacon Πίνακες"]
["8MF1060-2GS30","SIVACON, Supporting structure, for standard Empty enclosure, H: 2000 mm, W: 600 mm, T: 1000 mm, zinc-plated",861.08,"ΤΕΜ",1,"EP",1,"8MF10602GS30","8MF Sivacon Πίνακες"]
["8MF1060-2UW70-3C","SIVACON, partition, for side-by-side housing, H: 2000 mm, D: 600 mm, zinc-plated",237.48,"ΤΕΜ",1,"EP",1,"8MF10602UW703C","8MF Sivacon Πίνακες"]
["8MF1068-2AF20","SIVACON, compartment bottom, D: 800 mm, W: 600 mm, zinc-plated",373.44,"ΤΕΜ",1,"EP",1,"8MF10682AF20","8MF Sivacon Πίνακες"]
["8MF1080-2AF20","SIVACON, compartment bottom, D: 1000 mm, W: 800 mm, zinc-plated",326.3,"ΤΕΜ",1,"EP",1,"8MF10802AF20","8MF Sivacon Πίνακες"]
["8MF1084-2AF20","SIVACON, compartment bottom, D: 400 mm, W: 800 mm, zinc-plated",155.36000000000001,"ΤΕΜ",1,"EP",1,"8MF10842AF20","8MF Sivacon Πίνακες"]
["8MF1085-2AS30","SIVACON, mounting rail, universal, suitable for cabinet depth 1000 mm, L: 850 mm, zinc-plated",55.84,"ΤΕΜ",1,"EP",1,"8MF10852AS30","8MF Sivacon Πίνακες"]
["8MF1086-3VR4","SIVACON, Control panel Empty enclosure, without side panels, according to IEC 62208, with Ventilation openings IP20, H: 2000 mm, W: 800 mm, T: 600 mm",2846.1,"ΤΕΜ",1,"EP",1,"8MF10863VR4","8MF Sivacon Πίνακες"]
["8MF1090-2UT25-2BA2","SIVACON, door half, left, with ventilation openings, IP40, H: 2000 mm, W: 900 mm, RAL 7035, Protection class 1",636.29,"ΤΕΜ",1,"EP",1,"8MF10902UT252BA2","8MF Sivacon Πίνακες"]
["8MF1095-2UD12-0A","SIVACON, Roof, EMC, EMC, IP40, W: 900 mm, T: 500 mm, zinc-plated",295.49,"ΤΕΜ",1,"EP",1,"8MF10952UD120A","8MF Sivacon Πίνακες"]
["8MF1111-0AA00-0AC0","SIVACON 1800mm x 600mm x 400mm",3081.76,"ΤΕΜ",1,"EP",1,"8MF11110AA000AC0","8MF Sivacon Πίνακες"]
["8MF1111-0AA00-0AE3","SIVACON 1800mm x 600mm x 600mm",3299.3,"ΤΕΜ",1,"EP",1,"8MF11110AA000AE3","8MF Sivacon Πίνακες"]
["8MF1111-0AA00-0AR1","SIVACON 2000mm x 800mm x 600mm",2284.13,"ΤΕΜ",1,"EP",1,"8MF11110AA000AR1","8MF Sivacon Πίνακες"]
["8MF1111-0AA00-0AT4","SIVACON 2000mm x 600mm x 500mm",2791.71,"ΤΕΜ",1,"EP",1,"8MF11110AA000AT4","8MF Sivacon Πίνακες"]
["8MF1111-0AA00-0BC7","SIVACON 2000mm x 800mm x 500mm",3770.62,"ΤΕΜ",1,"EP",1,"8MF11110AA000BC7","8MF Sivacon Πίνακες"]
["8MF1111-0AA00-0BJ0","SIVACON 1800mm x 800mm x 600mm",4368.8500000000004,"ΤΕΜ",1,"EP",1,"8MF11110AA000BJ0","8MF Sivacon Πίνακες"]
["8MF1111-0AA00-0BS8","SIVACON 2000mm x 800mm x 500mm",3571.22,"ΤΕΜ",1,"EP",1,"8MF11110AA000BS8","8MF Sivacon Πίνακες"]
["8MF1111-0AA00-0BW2","SIVACON 1800mm x 800mm x 400mm",3607.47,"ΤΕΜ",1,"EP",1,"8MF11110AA000BW2","8MF Sivacon Πίνακες"]
["8MF1111-0AA00-0CJ5","SIVACON 2000mm x 800mm x 800mm",3933.78,"ΤΕΜ",1,"EP",1,"8MF11110AA000CJ5","8MF Sivacon Πίνακες"]
["8MF1111-0AA00-0CL8","SIVACON 2000mm x 800mm x 600mm",3462.45,"ΤΕΜ",1,"EP",1,"8MF11110AA000CL8","8MF Sivacon Πίνακες"]
["8MF1111-0AA00-0CR6","SIVACON 1800mm x 1000mm x 400mm",4133.18,"ΤΕΜ",1,"EP",1,"8MF11110AA000CR6","8MF Sivacon Πίνακες"]
["8MF1111-0AA00-0DD8","SIVACON 2000mm x 600mm x 500mm",3172.4,"ΤΕΜ",1,"EP",1,"8MF11110AA000DD8","8MF Sivacon Πίνακες"]
["8MF1111-0AA00-0DK8","SIVACON 2000mm x 900mm x 600mm",5039.58,"ΤΕΜ",1,"EP",1,"8MF11110AA000DK8","8MF Sivacon Πίνακες"]
["8MF1111-0AA00-0DR6","SIVACON 2000mm x 800mm x 400mm",3571.22,"ΤΕΜ",1,"EP",1,"8MF11110AA000DR6","8MF Sivacon Πίνακες"]
["8MF1111-0AA00-0DU5","SIVACON 2000mm x 1000mm x 800mm",5184.6099999999997,"ΤΕΜ",1,"EP",1,"8MF11110AA000DU5","8MF Sivacon Πίνακες"]
["8MF1111-0AA00-0EG6","SIVACON 1800mm x 600mm x 1000mm",4024.42,"ΤΕΜ",1,"EP",1,"8MF11110AA000EG6","8MF Sivacon Πίνακες"]
["8MF1111-0AA00-0EM2","SIVACON 2000mm x 1200mm x 500mm",4677.0200000000004,"ΤΕΜ",1,"EP",1,"8MF11110AA000EM2","8MF Sivacon Πίνακες"]
["8MF1111-0AA00-0EU0","SIVACON 2200mm x 1000mm x 600mm",4840.18,"ΤΕΜ",1,"EP",1,"8MF11110AA000EU0","8MF Sivacon Πίνακες"]
["8MF1111-0AA00-0EY7","SIVACON 2000mm x 800mm x 500mm",3353.68,"ΤΕΜ",1,"EP",1,"8MF11110AA000EY7","8MF Sivacon Πίνακες"]
["8MF1111-0AA00-0FJ4","SIVACON 2200mm x 600mm x 400mm",4006.29,"ΤΕΜ",1,"EP",1,"8MF11110AA000FJ4","8MF Sivacon Πίνακες"]
["8MF1111-0AA00-0FL7","SIVACON 1800mm x 800mm x 600mm",4169.4399999999996,"ΤΕΜ",1,"EP",1,"8MF11110AA000FL7","8MF Sivacon Πίνακες"]
["8MF1111-0AA00-0FR5","SIVACON 2000mm x 800mm x 800mm",4060.67,"ΤΕΜ",1,"EP",1,"8MF11110AA000FR5","8MF Sivacon Πίνακες"]
["8MF1111-0AA00-0GA8","SIVACON 2200mm x 900mm x 400mm",4006.29,"ΤΕΜ",1,"EP",1,"8MF11110AA000GA8","8MF Sivacon Πίνακες"]
["8MF1111-0AA00-0GJ1","SIVACON 2000mm x 600mm x 500mm",3190.53,"ΤΕΜ",1,"EP",1,"8MF11110AA000GJ1","8MF Sivacon Πίνακες"]
["8MF1111-0AA00-0GU7","SIVACON 2200mm x 800mm x 600mm",4622.6400000000003,"ΤΕΜ",1,"EP",1,"8MF11110AA000GU7","8MF Sivacon Πίνακες"]
["8MF1111-0AA00-0GX1","SIVACON 2000mm x 600mm x 500mm",3788.75,"ΤΕΜ",1,"EP",1,"8MF11110AA000GX1","8MF Sivacon Πίνακες"]
["8MF1111-0AA00-0HJ8","SIVACON 2000mm x 400mm x 400mm",2465.41,"ΤΕΜ",1,"EP",1,"8MF11110AA000HJ8","8MF Sivacon Πίνακες"]
["8MF1111-0AA00-0HM2","SIVACON 2200mm x 1200mm x 600mm",4677.0200000000004,"ΤΕΜ",1,"EP",1,"8MF11110AA000HM2","8MF Sivacon Πίνακες"]
["8MF1200-2AN30","SIVACON, 19\" fixed mounting, for the installation of 19\" devices, H: 600 mm, zinc-plated",105.14,"ΤΕΜ",1,"EP",1,"8MF12002AN30","8MF Sivacon Πίνακες"]
["8MF1206-2AK13-0","SIVACON, mounting plate, for cabinet side, perforated, D: 600 mm, H: 2200 mm, zinc-plated",380.69,"ΤΕΜ",1,"EP",1,"8MF12062AK130","8MF Sivacon Πίνακες"]
["8MF1228-3VS4","SIVACON, Control panel Empty enclosure, according to IEC 62208, with ventilation openings, IP20, H: 2200 mm, W: 1200 mm, T: 800 mm",5093.97,"ΤΕΜ",1,"EP",1,"8MF12283VS4","8MF Sivacon Πίνακες"]
["8MF1240-3BR4","SIVACON, Control panel Empty enclosure, without side panels, according to IEC 62208, IP40, H: 2200 mm, W: 400 mm, T: 1000 mm",2501.66,"ΤΕΜ",1,"EP",1,"8MF12403BR4","8MF Sivacon Πίνακες"]
["8MF1260-2UT14-1BA2","SIVACON, door, on the right, ventilated, IP20, H: 2200 mm, W: 600 mm, RAL 7035, Protection class 1",714.24,"ΤΕΜ",1,"EP",1,"8MF12602UT141BA2","8MF Sivacon Πίνακες"]
["8MF1260-2UT15-3BA2","SIVACON, door, left, with cutout for filter fan, with ventilation openings H: 2200 mm, W: 600 mm, RAL 7035, Protection class 1",714.24,"ΤΕΜ",1,"EP",1,"8MF12602UT153BA2","8MF Sivacon Πίνακες"]
["8MF1270-2UT14-0CA1","SIVACON, door, right, EMC, IP40, H: 2200 mm, W: 450 mm, RAL 7035, Protection class 1",1283.46,"ΤΕΜ",1,"EP",1,"8MF12702UT140CA1","8MF Sivacon Πίνακες"]
["8MF1286-3BS4","SIVACON, Control panel Empty enclosure, according to IEC 62208, IP40, H: 2200 mm, W: 800 mm, T: 600 mm",3679.98,"ΤΕΜ",1,"EP",1,"8MF12863BS4","8MF Sivacon Πίνακες"]
["8MF1290-3BR5","SIVACON, Control panel Empty enclosure, without side panels, according to IEC 62208, IP55, H: 2200 mm, W: 900 mm, T: 1000 mm",3951.9,"ΤΕΜ",1,"EP",1,"8MF12903BR5","8MF Sivacon Πίνακες"]
["8MF1408-2HH","SIVACON, cable propping bar, D: 800 mm, H: 40 mm, zinc-plated",69.97,"ΤΕΜ",1,"EP",1,"8MF14082HH","8MF Sivacon Πίνακες"]
["8MF1500-2HS","SIVACON, standard mounting rail, L: 1000 mm, H: 7.5 mm, zinc-plated",42.06,"ΤΕΜ",1,"EP",1,"8MF15002HS","8MF Sivacon Πίνακες"]
["8MF1804-3VS4","SIVACON, Control panel Empty enclosure, according to IEC 62208, with ventilation openings, IP20, H: 1800 mm, W: 1000 mm, T: 400 mm",3825.01,"ΤΕΜ",1,"EP",1,"8MF18043VS4","8MF Sivacon Πίνακες"]
["8MF1824-2GS30","SIVACON, Supporting structure, for standard Empty enclosure, H: 1800 mm, W: 1200 mm, T: 400 mm, zinc-plated",817.57,"ΤΕΜ",1,"EP",1,"8MF18242GS30","8MF Sivacon Πίνακες"]
["8MF1840-3BS5","SIVACON, Control panel Empty enclosure, according to IEC 62208, IP55, H: 1800 mm, W: 400 mm, T: 1000 mm",3516.83,"ΤΕΜ",1,"EP",1,"8MF18403BS5","8MF Sivacon Πίνακες"]
["8MF1850-2UT15-0BA2","SIVACON, door, left, IP55, H: 1800 mm, W: 500 mm, RAL 7035, Protection class 1",645.36,"ΤΕΜ",1,"EP",1,"8MF18502UT150BA2","8MF Sivacon Πίνακες"]
["8MF1866-3VS4","SIVACON, Control panel Empty enclosure, according to IEC 62208, with ventilation openings, IP20, H: 1800 mm, W: 600 mm, T: 600 mm",3063.63,"ΤΕΜ",1,"EP",1,"8MF18663VS4","8MF Sivacon Πίνακες"]
["8MF1880-2UT15-0BA2","SIVACON, door, left, IP55, H: 1800 mm, W: 800 mm, RAL 7035, Protection class 1",746.87,"ΤΕΜ",1,"EP",1,"8MF18802UT150BA2","8MF Sivacon Πίνακες"]
["8MF1890-2AM12-0","SIVACON, mounting plate, mounting with bracket, perforated, H: 800 mm, W: 900 mm, zinc-plated",264.67,"ΤΕΜ",1,"EP",1,"8MF18902AM120","8MF Sivacon Πίνακες"]
["8MF1894-3BS4","SIVACON, Control panel Empty enclosure, according to IEC 62208, IP40, H: 1800 mm, W: 900 mm, T: 400 mm",3571.22,"ΤΕΜ",1,"EP",1,"8MF18943BS4","8MF Sivacon Πίνακες"]
["8MF2008-3RB","standard cabinet 8MF2 HxWxD=2000x 1000x 800 Installation: Side-by-side ventilated, mounted, welded IP30",4760.7700000000004,"ΤΕΜ",1,"EP",1,"8MF20083RB","8MF Sivacon Πίνακες"]
["8MF2094-4ES","EMC cabinet IP40 HxWxD=2000x 900x 400 for stand-alone installation with side panels, IP40",5216.8999999999996,"ΤΕΜ",1,"EP",1,"8MF20944ES","8MF Sivacon Πίνακες"]
["8MF2224-5E","standard cabinet 8MF2 HxWxD=2200x 1200x 400 Installation: single non-ventilated, assembled, welded IP54,",6357.2,"ΤΕΜ",1,"EP",1,"8MF22245E","8MF Sivacon Πίνακες"]
["8MF2286-4RL2","SICUBE 8MF 2000 Switchgear cabinet HxWxD=2200x 800x 600 mm For inline installation without side panels, IP40",6186.15,"ΤΕΜ",1,"EP",1,"8MF22864RL2","8MF Sivacon Πίνακες"]
["8MF2804-5R","standard cabinet 8MF2 HxWxD=1800x 1000x 400 Installation: Side-by-side non-ventilated, assembled, welded IP54,",4760.7700000000004,"ΤΕΜ",1,"EP",1,"8MF28045R","8MF Sivacon Πίνακες"]
["8MF2898-4EN","SICUBE 8MF 2000 EMC cabinet, welding version NI HxWxD=1800x 900x 800 mm for stand-alone installation with side panels, IP40",9664.08,"ΤΕΜ",1,"EP",1,"8MF28984EN","8MF Sivacon Πίνακες"]
["8MF3035","Instrument cover, hinged with locking device and protective stay instead of standard door HxW=400x 600 Price is an additional price for Standard version",553.04,"ΤΕΜ",1,"EP",1,"8MF3035","8MF Sivacon Πίνακες"]
["8MF3151","Trim strip with Siemens logo, Petrol Indicator light cutout left Price is an additional price for Standard version",57.02,"ΤΕΜ",1,"EP",1,"8MF3151","8MF Sivacon Πίνακες"]
["8MF3240","Symmetrically divided double-wing door instead of rear panel HxW=1800x 800 IP40 Price is an additional price for Standard version",840.97,"ΤΕΜ",1,"EP",1,"8MF3240","8MF Sivacon Πίνακες"]
["8MF3414","SIVACON, roof, with ventilation openings IP20, W: 1000 mm, D: 600 mm, RAL 7032",161.07,"ΤΕΜ",1,"EP",1,"8MF3414","8MF Sivacon Πίνακες"]
["8MF3475","SIVACON, roof, with ventilation openings IP40, W: 1000 mm, D: 800 mm, RAL 7032",915.09,"ΤΕΜ",1,"EP",1,"8MF3475","8MF Sivacon Πίνακες"]
["8MF3511","SIVACON, roof, for busbar mounting, IP20, W: 600 mm, D: 730 mm, RAL 7032",401.96,"ΤΕΜ",1,"EP",1,"8MF3511","8MF Sivacon Πίνακες"]
["8MF4047","Socket HxWxD=200x 1200x 600",801.06,"ΤΕΜ",1,"EP",1,"8MF4047","8MF Sivacon Πίνακες"]
["8MF4118","Base plate subdivided multiple times WxD=1200x 800",937.9,"ΤΕΜ",1,"EP",1,"8MF4118","8MF Sivacon Πίνακες"]
["8MF4400","C-section mounting rail Cable propping bar C30 W=600",96.07,"ΤΕΜ",1,"EP",1,"8MF4400","8MF Sivacon Πίνακες"]
["8MF4513","Mounting plate incl. mounting bracket HxW=2000x 1000",644.27,"ΤΕΜ",1,"EP",1,"8MF4513","8MF Sivacon Πίνακες"]
["8MF4816","Perforated compartment bottom mounted stationary HxD=800x 600",322.13,"ΤΕΜ",1,"EP",1,"8MF4816","8MF Sivacon Πίνακες"]
["8MF4842","Compartment bottom with telescopic rails Extract HxD=600x 800",618.61,"ΤΕΜ",1,"EP",1,"8MF4842","8MF Sivacon Πίνακες"]
["8MF4921","Support",48.18,"ΤΕΜ",1,"EP",1,"8MF4921","8MF Sivacon Πίνακες"]
["8MF5224-5E","Standard cabinet 8MF5 HxWxD=2200x 1200x 400 Installation: single non-ventilated, not mounted, screwed IP54,",6927.35,"ΤΕΜ",1,"EP",1,"8MF52245E","8MF Sivacon Πίνακες"]
["8MF5868-5R","Standard cabinet 8MF5 HxWxD=1800x 600x 800 Installation: Side-by-side non-ventilated, not mounted, screwed IP54,",4019.58,"ΤΕΜ",1,"EP",1,"8MF58685R","8MF Sivacon Πίνακες"]
["8MF5910-1C","SlimLine lamp with Motion detector SL 025 Socket outlet with magnet (approx. 30 N)",540.74,"ΤΕΜ",1,"EP",1,"8MF59101C","8MF Sivacon Πίνακες"]
["8MF6066-4ES","EMC cabinet IP40 HxWxD=2000x 600x 600",5530.47,"ΤΕΜ",1,"EP",1,"8MF60664ES","8MF Sivacon Πίνακες"]
["8MF6298-4R","Standard cabinet 8MF6 HxWxD=2200x 900x 800 Installation: Side-by-side non-ventilated, assembled, welded IP40",4447.1899999999996,"ΤΕΜ",1,"EP",1,"8MF62984R","8MF Sivacon Πίνακες"]
["8MF6866-4ES","EMC cabinet IP40 HxWxD=1800x 600x 600",5359.43,"ΤΕΜ",1,"EP",1,"8MF68664ES","8MF Sivacon Πίνακες"]
["8MF9212","8MF system cabinets Mounting plate HxW=200x 900 mm for 8MF system cabinet",182.73,"ΤΕΜ",1,"EP",1,"8MF9212","8MF Sivacon Πίνακες"]
["8MR2110-0C","Heater 110-120V, 10W; UL-APP. HGK 047-04700.9-00",101.4,"ΤΕΜ",1,"EP",3,"8MR21100C","8MR εξαρτήματα πινάκων"]
["8MR2170-1KB","small compact thermostat NC (heating) -10 bis +50 Â°C",59.74,"ΤΕΜ",1,"EP",1,"8MR21701KB","ΝΕΟ υλικό 8MR θερμοστάτες πινάκων"]
["8MR2172-1AB","NO contact+NO contact, 50Β°, 122 Β°F FTD011, 01164.0-00",77.44,"ΤΕΜ",1,"EP",1,"8MR21721AB","8MR εξαρτήματα πινάκων"]
["8MR6423-5LE25","Filter fan, Extract: W: 125 mm, H: 125 mm, RAL 7035, IP54, Airflow: 62 m3/h, Ue AC: 230 V, ECO version",448.07,"ΤΕΜ",1,"EP",1,"8MR64235LE25","8MR εξαρτήματα πινάκων"]
["8MR6423-6LV41","Filter fan, Extract: W: 223 mm, H: 223 mm, RAL 7035, IP54, EMC, Airflow: 250 m3/h, Ue AC: 230 V",852.91,"ΤΕΜ",1,"EP",1,"8MR64236LV41","8MR εξαρτήματα πινάκων"]
["8PQ1011-1BA01","SIVACON S4 base reinforcement H: 100mm W:, D:=1000mm",133.6,"ΤΕΜ",1,"EP",1,"8PQ10111BA01","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ2005-4BA03","SIVACON S4 cover IP40, H: 50mm W: 400mm",78.959999999999994,"ΤΕΜ",1,"EP",1,"8PQ20054BA03","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ2020-8BA08","SIVACON S4 protect. upgr. degr. IP55, H: 200mm W: 800mm",84.37,"ΤΕΜ",1,"EP",1,"8PQ20208BA08","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ2025-8BA10","SIVACON S4 cover 3NP1123 (NH000 up to 160 A), H: 250mmW: 800mm",149.25,"ΤΕΜ",1,"EP",1,"8PQ20258BA10","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ2030-6BA26","SIVACON S4 cover 3VA20 (100A), 3VA21 (160A), 3VA22 (250A), 4-pole, withdrawable,H:300mm W: 600mm",173.32,"ΤΕΜ",1,"EP",1,"8PQ20306BA26","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ2045-8BA11","SIVACON S4 cover 3VA20 (100A), 3VA21 (160A), 3VA22 (250A), 3-pole, fixed-mounted, plug-in tech, 8US setup, H: 450mm W: 800mm",196.19,"ΤΕΜ",1,"EP",1,"8PQ20458BA11","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ2055-6BA08","SIVACON S4, mod door, IP40, H: 550 mm, W: 600 mm",252.76,"ΤΕΜ",1,"EP",1,"8PQ20556BA08","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ2075-8BA02","SIVACON S4 protect. upgr. degr. IP55, H: 750mm W: 800mm",109.17,"ΤΕΜ",1,"EP",1,"8PQ20758BA02","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ2197-1BA10","SIVACON S4 Giugiaro glass door, IP55, H: 2000 mm, W: 1000 mm, double-bit key, left",1178.32,"ΤΕΜ",1,"EP",1,"8PQ21971BA10","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ2300-6BA20","SIVACON S4 base plate IP55 W: 350mm D: 600mm",84.14,"ΤΕΜ",1,"EP",1,"8PQ23006BA20","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ2301-4BA03","SIVACON S4 top plate upgr. kit IPX1, W: 1000 mm D: 400mm",207.02,"ΤΕΜ",1,"EP",1,"8PQ23014BA03","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ2304-4BA04","SIVACON S4 top plate upgr. kit IPX1, W: 400mm D: 400mm",119.99,"ΤΕΜ",1,"EP",1,"8PQ23044BA04","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ2420-2BA02","SIVACON S4 rear wall, IP40, W: 1200mm",587.36,"ΤΕΜ",1,"EP",1,"8PQ24202BA02","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ3000-0BA38","SIVACON S4 cable brackets, profile C30,D: 400mm, 1 pack =5 unit(s)",87.86,"ΤΕΜ",1,"EP",1,"8PQ30000BA38","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ3000-1BA61","SIVACON S4 mounting panel, H: 400mm W: 600mm",122.77,"ΤΕΜ",1,"EP",1,"8PQ30001BA61","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ3000-2BA35","SIVACON S4 cable brackets, profile C30, W: 850mm, 1 pack=5 units",237.11,"ΤΕΜ",1,"EP",1,"8PQ30002BA35","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ4000-0BA32","SIVACON S4 field distrib. busbar support cascaded, 2x 30x10mm",58.85,"ΤΕΜ",1,"EP",1,"8PQ40000BA32","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ4000-2BA25","SIVACON S4 field distrib. busbar support non-cascaded, W: 200mm, 1 set =2 units",349.04,"ΣΕΤ",1,"EP",1,"8PQ40002BA25","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ5000-3BA41","SIVACON S4 compartment ID strip H: 17 mm, W: 1100mm",103.51,"ΤΕΜ",1,"EP",1,"8PQ50003BA41","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ5000-4BA52","SIVACON S4 separation, rear W: 800mm H: 400mm",225.07,"ΤΕΜ",1,"EP",1,"8PQ50004BA52","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ6000-2BA65","SIVACON S4 mounting panel 3KL5 up to 125A, 3- or 4-pole, H: 300mm W: 600mm",139.02000000000001,"ΤΕΜ",1,"EP",1,"8PQ60002BA65","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ6000-5BA68","SIVACONΒ S4 connection vertical busbar 3NP 1143 (NH1 up to 250A)",340.62,"ΤΕΜ",1,"EP",1,"8PQ60005BA68","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ6000-8BA55","SIVACON S4 mounting panel 3VA23 (400A), 3VA24 (630A), 3-pole, fixed-mounted, H: 500mm W:600mm",181.74,"ΤΕΜ",1,"EP",1,"8PQ60008BA55","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ9400-0BA10","SIVACON S4 Torx screwdriver insert L=200 mm, 1 pack =2 units",250.35,"ΤΕΜ",1,"EP",1,"8PQ94000BA10","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ9400-0BA71","SIVACON S4 bellows for connecting terminal, 1 pack =4 unit(s)",67.28,"ΤΕΜ",1,"EP",1,"8PQ94000BA71","Sivacon S4 υλικά - εξαρτήματα"]
["8UC6014","Spare part for rotary operating mechanism 8UC6 Coupling driver for shaft 12 mm",95.99,"ΤΕΜ",1,"EP",1,"8UC6014","8UC εξαρτήματα για χειριστήρια"]
["8UC7210-6BD","Spare part for 8UC7212-6BD26 for door-coupling rotary operating mechanism for circuit breaker 3VL 8UC7 design Handle ti-gray, Masking frame light gray",146.76,"ΤΕΜ",1,"EP",1,"8UC72106BD","8UC εξαρτήματα για χειριστήρια"]
["8UD1741-0AB11","Handle with masking frame standard without tolerance compensation Accessory for: 3VA1/2 1000",104.92,"ΤΕΜ",1,"EP",1,"8UD17410AB11","8UD χειριστήρια για 3KC/3KD/3KF"]
["8UD1841-2AF05","handle with masking plate EMERGENCY-STOP size 100 x 100, for shaft 8 x 8, test-0-I handle size 100mm accessory for 3KD size 3 3KF size 2 and 3",79.180000000000007,"ΤΕΜ",1,"EP",1,"8UD18412AF05","8UD χειριστήρια για 3KC/3KD/3KF"]
["8UD1900-2DA00","adapter 8x 8 mm Accessory for: Door-coupling rotary mechanism 3VA",12.72,"ΤΕΜ",1,"EP",1,"8UD19002DA00","8UD χειριστήρια για 3KC/3KD/3KF"]
["8US1620-5AK02","device holder, 1-pole 18x 160 mm",11.92,"ΤΕΜ",1,"EP",6,"8US16205AK02","8US Busbar system"]
["8US1998-1AA00","Busbar system, accessories Busbar center-to-center spacing 40, 60 mm Connecting wedges for connecting the device adapter and device holder",69,"ΤΕΜ",100,"EP",100,"8US19981AA00","8US Busbar system"]
["8WA1822-7EF85","G fuse link DIN 41662 slow-response Low breaking capacity Rated continuous current 6.3 A",2.34,"ΤΕΜ",1,"EP",10,"8WA18227EF85","8WA εξαρτήματα κλεμμών"]
["8WD4220-0CE","Single-flash light element, clear, 24 V DC, diameter 50 mm",240.7,"ΤΕΜ",1,"EP",1,"8WD42200CE","8WD Βιομηχανικοί Φανοί"]
["8WD4308-0DF","adapter for pipe mounting, according to NPT, accessory for signaling columns, with diameter 70 mm",35.659999999999997,"ΤΕΜ",1,"EP",1,"8WD43080DF","8WD Βιομηχανικοί Φανοί"]
["8WD4423-5AK05-0AE0","Complete unit signaling column, top: continuous light, yellow, center: continuous light, blue, bottom: continuous light, green, integrated LED 24 V AC/DC, connection element for pipe mounting, pipe, 250 mm, base, plastic",508.39,"ΤΕΜ",1,"EP",1,"8WD44235AK050AE0","8WD Βιομηχανικοί Φανοί"]
["8WD4450-5BF","Flashlight element, with integrated LED, blue, 230 V AC, Diameter 70 mm",139.47,"ΤΕΜ",1,"EP",1,"8WD44505BF","8WD Βιομηχανικοί Φανοί"]
["8WD5340-0CB","Integrated signal lamp, single flash light, w. built-in electronic flash, red, 115 V AC, Diameter 70 mm",199.08,"ΤΕΜ",1,"EP",1,"8WD53400CB","8WD Βιομηχανικοί Φανοί"]
["8WH1020-5LF00","Two-tier terminals for components, 2.5 mm2 Screw mounting gray for component connection",5.51,"ΤΕΜ",1,"EP",50,"8WH10205LF00","8WH Κλέμμες"]
["8WH2000-0AE08","Through-type terminals with spring-loaded connection, Cross-section: 1.5 mm2, Width: 4.2mm, Color: black",0.98,"ΤΕΜ",1,"EP",50,"8WH20000AE08","8WH Κλέμμες"]
["8WH2004-0AE01","Through-type terminals with spring-loaded connection, 4 connection points, Cross-section: 0.14-1.5 mm2, Width: 4.2mm, Color: blue",1.38,"ΤΕΜ",1,"EP",50,"8WH20040AE01","8WH Κλέμμες"]
["8WH3000-6AE00","Isolating terminal with quick-connect technology Cross-section: 0.25-1.5 mm2, Width: 5.2mm, Color: gray",3.26,"ΤΕΜ",1,"EP",50,"8WH30006AE00","8WH Κλέμμες"]
["8WH6000-0CF07","IPO terminals, Through-type terminals 2.5 mm2",4.03,"ΤΕΜ",1,"EP",50,"8WH60000CF07","8WH Κλέμμες"]
["8WH8110-7AA05","Labeling plate, front, horizontal und vertical, Terminal width: 16.2 mm, H: 10.5 mm, white",7.08,"ΤΕΜ",100,"EP",100,"8WH81107AA05","8WH Κλέμμες"]
["8WH8121-0XA05","Labeling plates 3.5 mm flat, longitudinal customer-specific inscription",24.72,"ΤΕΜ",100,"EP",100,"8WH81210XA05","8WH Κλέμμες"]
["8WH8140-1AB15","Labeling plate, front, with 11-20, horizontal, Terminal width: 4.2 mm, H: 6.4 mm, white",9.58,"ΤΕΜ",100,"EP",100,"8WH81401AB15","8WH Κλέμμες"]
["8WH8141-2AB75","Labeling plate, flat, with 71-80, horizontal, Terminal width: 5.2 mm, H: 6.4 mm, white",9.02,"ΤΕΜ",100,"EP",100,"8WH81412AB75","8WH Κλέμμες"]
["8WH9002-8HC10","Reducing comb from 35 mm2 to 2.5 mm2 and 4 mm2 from screw to spring-type",2.96,"ΤΕΜ",1,"EP",10,"8WH90028HC10","8WH Κλέμμες"]
["8WH9005-3PB00","Cover for Insta -Terminal block for screw mounting",0.81,"ΤΕΜ",1,"EP",1,"8WH90053PB00","8WH Κλέμμες"]
["8WH9020-6JF00","5 conn. combs 3.5Β mm gray",2.15,"ΤΕΜ",1,"EP",50,"8WH90206JF00","8WH Κλέμμες"]
["8WH9050-2AA04","Latch without strain relief for all connectors",63.22,"ΤΕΜ",100,"EP",50,"8WH90502AA04","8WH Κλέμμες"]
["9AE7107-1SH13-0AA0","PM-OPEN PI V7, Software CD, upgrade package for system package Standard for increasing the number of tags from 1024 to > 1024, executable in WinCC system (V6/7), R-SW incl. config. system German/English, Single License, new copy protection (dongle), return of the dongle from initial delivery required, software ID number and dongle serial number for order must be specified. Only for subsequent orders.",3967,"ΤΕΜ",1,"SIMATIC",1,"9AE71071SH130AA0","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["9AE7110-4SU06-8AA3","PM-CONTROL migration service service, delivery by email, for Professional variant, service package of the WinCC Competence Centers for migration of a user project from V8-11 to V12 ****download product****",4904,"ΤΕΜ",1,"SIMATIC",1,"9AE71104SU068AA3","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["9AE7130-1CS06-1AS1","BATCH.21 CONNECT SIMATIC BATCH SUS SUS extension for one year for every 100 EUR list price delivery by email.",24.6,"ΤΕΜ",1,"SIMATIC",1,"9AE71301CS061AS1","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["A5E00078031","NCS magnet holder (aluminum) for non-contacting position detection at linear actuators up to 14 mm stroke. For NCS sensors: 6DR4004-.N.20",115,"ST",1,"PI1",1,"A5E00078031","Όργανα Μέτρησης Πεδίου"]
["A5E00822478","Accessory - Terminal Box M20  - 3A",183,"ST",1,"PI1",1,"A5E00822478","Όργανα Μέτρησης Πεδίου"]
["A5E01150883","SITRANS F M Accessory MAG 3100 Grounding ring Type Flat ring, DN 25 (1\"), EN 1092-1 PN 40, in tantalum, for all liners (PTFE max. 130 Â°C (266 Â°F)), 1 pc.",1679,"ST",1,"PI4",1,"A5E01150883","Όργανα Μέτρησης Πεδίου"]
["A5E01163702","Kit, 316 stainless steel PFA cable extension, 20 METER, CLS300",3269,"ST",1,"PI6",1,"A5E01163702","Όργανα Μέτρησης Πεδίου"]
["A5E01191960","SITRANS F M Accessory MAG 3100 Grounding ring Type Flat ring, DN 300 (12\"), EN 1092-1 PN 40, in stainless steel AISI 316 14.436,00 for all liners (PTFE max. 130 Â°C (266 Â°F)), 1 pc.",430,"ST",1,"PI4",1,"A5E01191960","Όργανα Μέτρησης Πεδίου"]
["A5E01191983","SITRANS F M Accessory MAG 3100 Grounding ring Type Flat ring, DN 65 (2 1/2\"), EN 1092-1 PN 40, in alloy C-276 2.4819, for all liners (PTFE max. 130 Â°C (266 Â°F)), 1 pc.",327,"ST",1,"PI4",1,"A5E01191983","Όργανα Μέτρησης Πεδίου"]
["A5E02212428","Sitrans LR460 enclosure with board stack, HART communication, DC power, NPT cable inlet, approval option A, no process connection",5447,"ST",1,"PI1",1,"A5E02212428","Όργανα Μέτρησης Πεδίου"]
["A5E02218297","SITRANS F M Accessory MAG 1100F Threaded type connection fitting (P-gaskets for EHEDG), DN 32, for sensor DN 25, DIN 11851, in stainless steel AISI 316L 1.4404, for PFA liner, 2 pcs.",735,"ST",1,"PI4",1,"A5E02218297","Όργανα Μέτρησης Πεδίου"]
["A5E02574152","7ML57462AA005AA0,2.2 Cert. (Instrument) Standard vibrating level switch for use in liquid and liquid hazardous applications such as overflow, high, low and demand applications, as well as pump protection. For use in SIL-2 applications.",1183,"ST",1,"PI1",1,"A5E02574152","Όργανα Μέτρησης Πεδίου"]
["A5E02611793","SITRANS FUE950 spare part: Stainless steel pocket (1 pcs.), 210 mm, G1/2B (PN25). For 2-wire Pt500 sensor 6 mm types only.",135,"ST",1,"PI1",1,"A5E02611793","Όργανα Μέτρησης Πεδίου"]
["A5E03461719","SITRANS FUE950 spare part: FUE950 24 V AC supply module, incl. back-up battery (7ME348 versions only).",127,"ST",1,"PI1",1,"A5E03461719","Όργανα Μέτρησης Πεδίου"]
["A5E03617087","7ML5423XXXXX2CCX,HART SU<3.6mA,NPT LR200 enclosure with board stack, LUI display, 5.8 GHz, LR200 enclosure with board NPT cable inlet approval option C, HART communication no process connection",2202,"ST",1,"PI1",1,"A5E03617087","Όργανα Μέτρησης Πεδίου"]
["A5E03915074","Siemens Sensor Link cable 75 m (246 ft) (Ex) with 2 x M12 plugs, PO insulation and PUR sleeve, blue, -40 ... +80 Â°C (-40 ... +176 Â°F).",1221,"ST",1,"PI1",1,"A5E03915074","Όργανα Μέτρησης Πεδίου"]
["A5E33035287","Accessory SITRANS FCS400 Heating Jacket DN15 electric including HT41 Controller 230 V AC",6625,"ST",1,"PI1",1,"A5E33035287","Όργανα Μέτρησης Πεδίου"]
["A5E35345074","Add-on module Profibus DP profile 3.",522,"ST",1,"PI4",1,"A5E35345074","Όργανα Μέτρησης Πεδίου"]
["A5E38014726","Electronic cassette for Wall Box, Sensor input (Internal DSL)",2079,"ST",1,"PI1",1,"A5E38014726","Όργανα Μέτρησης Πεδίου"]
["A5E39669934023","5m(16.4') High temp /Submersible coax sensor cable pair with Nickel Plated Brass glands",430,"ST",1,"PI1",1,"A5E39669934023","Όργανα Μέτρησης Πεδίου"]
["A5E42824563","LUT420,ASSY,AC BOARDSTACK w/CRADLE,HAZ Spare electronics assembly in polycarbonate cradle for use in SITRANS LUT400 Model: LUT420 Level Controller Input Voltage: AC Approvals: Hazardous Locations",1102,"ST",1,"PI3",1,"A5E42824563","Όργανα Μέτρησης Πεδίου"]
["A5E44082453","FUS/FUE380 TRIAX sensor cable pair DN900-1200 spare part",1365,"ST",1,"PI1",1,"A5E44082453","Όργανα Μέτρησης Πεδίου"]
["A5E50369945","FCT030 Compact / TCE 9100 CH 1 HART Ex active ''E06'', M20",2754,"ST",1,"PI1",1,"A5E50369945","Όργανα Μέτρησης Πεδίου"]
["A5E50618139","7ML54401XB000AA2,NO FLANGE A 2-wire, 78 GHz FMCW radar level transmitter for continuous monitoring of solids and liquids to a range of 100 m (329ft) Order hand programmer separately!",4450,"ST",1,"PI1",1,"A5E50618139","Όργανα Μέτρησης Πεδίου"]
["A5E51358415","SIMATIC IPC, spare part PCB assembly - riser 1xPCIe X8 IPC PX-39A PRO",50.4,"ΤΕΜ",1,"SIMATIC",1,"A5E51358415","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["A5E51626981","SIMATIC IPC, spare part; Solid state drive M.2; 256 GB Eco; SSD_2100AI_256GB_M.2 for SIMATIC IPC",213,"TEM",1,"SIMATIC",1,"A5E51626981","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["A5E53339360006","Blades for belt plow, 2 pc., PE-HD, for WW200 with 42in/1067mm belt width, w/o hardware",373,"ST",1,"PI1",1,"A5E53339360006","Όργανα Μέτρησης Πεδίου"]
["C73451-A3000-C31","Gasket for front panel for SIPART DR20/21/22/24",5,"ST",10,"PI1",10,"C73451A3000C31","Όργανα Μέτρησης Πεδίου"]
["C79301-A3000-A2","Recording unit for fan-fold and roll paper for 7ND3590",687,"ST",1,"PI1",1,"C79301A3000A2","Όργανα Μέτρησης Πεδίου"]
["FDK:083G0117","SITRANS F M Accessory MAG 1100 Graphite gasket, DN 15 (1/2\"), conductive (can also be used as grounding ring), graphite, 2 pcs.",87,"ST",1,"PI4",1,"FDK:083G0117","Όργανα Μέτρησης Πεδίου"]
["FDK:083G2121","SITRANS F M Accessory MAG 1100F Weld-in connection fitting (flat gaskets for 3A), DN 40, for sensor DN 40, DIN 11850, in stainless steel AISI 316L 1.4404, for ceramic and PFA liner, 2 pcs.",503,"ST",1,"PI4",1,"FDK:083G2121","Όργανα Μέτρησης Πεδίου"]
["FDK:083G3117","Accessories for MAG 1100 EPDM gasket set for DN15 2 x EPDM-gaskets 2 x earthing wires 3 x M6 screws",58,"ST",1,"PI4",1,"FDK:083G3117","Όργανα Μέτρησης Πεδίου"]
["FDK:083H0235","MASS 6000 Ex d Assembled Display",764,"ST",1,"PI1",1,"FDK:083H0235","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8171","FLANSCHE E FUER MAG 3100, 450MM PN25,  AISI 316",2840,"ST",1,"PI4",1,"FDK:083N8171","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8272","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type E, DN 25 (1\"), ANSI B16.5 Class 300, AS 2129 Table E, in stainless steel AISI 316 14.436,00 for PTFE liners, 1 pc.",474,"ST",1,"PI4",1,"FDK:083N8272","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8366","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type C, DN 750 (30\"), AWWA C-207 Class D, in stainless steel AISI 304 14.301,00 for all liners except PTFE & PFA, 1 pc.",1050,"ST",1,"PI4",1,"FDK:083N8366","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8367","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type C, DN 1100 (44\"), EN 1092-1 PN 16, AS 2129 Table E, in stainless steel AISI 304 14.301,00 for all liners except PTFE & PFA, 1 pc.",2088,"ST",1,"PI4",1,"FDK:083N8367","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8370","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type E, DN 200 (8\"), ANSI B16.5 Class 150, JIS K20, in stainless steel AISI 316 14.436,00 for PTFE liners, 1 pc.",958,"ST",1,"PI4",1,"FDK:083N8370","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8372","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type C, DN 700 (28\"), AS 2129 Table E, in stainless steel AISI 304 14.301,00 for all liners except PTFE & PFA, 1 pc.",939,"ST",1,"PI4",1,"FDK:083N8372","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8373","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type C, DN 800 (32\"), AS 2129 Table E, in stainless steel AISI 304 14.301,00 for all liners except PTFE & PFA, 1 pc.",1112,"ST",1,"PI4",1,"FDK:083N8373","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8394","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type C, DN 1050 (42\"), AWWA C-207 Class D, in stainless steel AISI 304 14.301,00 for all liners except PTFE & PFA, 1 pc.",1808,"ST",1,"PI4",1,"FDK:083N8394","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8395","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type C, DN 1100 (44\"), AWWA C-207 Class D, in stainless steel AISI 304 14.301,00 for all liners except PTFE & PFA, 1 pc.",2123,"ST",1,"PI4",1,"FDK:083N8395","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8396","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type C, DN 900 (36\"), AS 2129 Table E, in stainless steel AISI 304 14.301,00 for all liners except PTFE & PFA, 1 pc.",1360,"ST",1,"PI4",1,"FDK:083N8396","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8397","FLANGE C FOR MAG 3100,  1000MM, AS2129 E AISI 304",1474,"ST",1,"PI4",1,"FDK:083N8397","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8467","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type C, DN 1400 (54\"), EN 1092-1 PN 6, in stainless steel AISI 304 14.301,00 for all liners except PTFE & PFA, 1 pc.",6362,"ST",1,"PI4",1,"FDK:083N8467","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8468","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type C, DN 1400 (54\"), EN 1092-1 PN 10, in stainless steel AISI 304 14.301,00 for all liners except PTFE & PFA, 1 pc.",6370,"ST",1,"PI4",1,"FDK:083N8468","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8469","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type C, DN 1400 (54\"), EN 1092-1 PN 16, in stainless steel AISI 304 14.301,00 for all liners except PTFE & PFA, 1 pc.",6362,"ST",1,"PI4",1,"FDK:083N8469","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8470","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type C, DN 1400 (54\"), AWWA C-207 Class D, in stainless steel AISI 304 14.301,00 for all liners except PTFE & PFA, 1 pc.",6031,"ST",1,"PI4",1,"FDK:083N8470","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8471","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type C, DN 1500 (60\"), EN 1092-1 PN 6, in stainless steel AISI 304 14.301,00 for all liners except PTFE & PFA, 1 pc.",6667,"ST",1,"PI4",1,"FDK:083N8471","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8472","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type C, DN 1500 (60\"), EN 1092-1 PN 10, in stainless steel AISI 304 14.301,00 for all liners except PTFE & PFA, 1 pc.",6738,"ST",1,"PI4",1,"FDK:083N8472","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8473","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type C, DN 1500 (60\"), EN 1092-1 PN 16, in stainless steel AISI 304 14.301,00 for all liners except PTFE & PFA, 1 pc.",6738,"ST",1,"PI4",1,"FDK:083N8473","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8474","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type C, DN 1500 (60\"), AWWA C-207 Class D, in stainless steel AISI 304 14.301,00 for all liners except PTFE & PFA, 1 pc.",6317,"ST",1,"PI4",1,"FDK:083N8474","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8475","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type C, DN 1600 (66\"), EN 1092-1 PN 6, in stainless steel AISI 304 14.301,00 for all liners except PTFE & PFA, 1 pc.",7039,"ST",1,"PI4",1,"FDK:083N8475","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8476","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type C, DN 1600 (66\"), EN 1092-1 PN 10, in stainless steel AISI 304 14.301,00 for all liners except PTFE & PFA, 1 pc.",7190,"ST",1,"PI4",1,"FDK:083N8476","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8477","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type C, DN 1600 (66\"), EN 1092-1 PN 16, in stainless steel AISI 304 14.301,00 for all liners except PTFE & PFA, 1 pc.",7190,"ST",1,"PI4",1,"FDK:083N8477","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8478","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type C, DN 1600 (66\"), AWWA C-207 Class D, in stainless steel AISI 304 14.301,00 for all liners except PTFE & PFA, 1 pc.",7024,"ST",1,"PI4",1,"FDK:083N8478","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8479","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type C, DN 1800 (72\"), EN 1092-1 PN 6, in stainless steel AISI 304 14.301,00 for all liners except PTFE & PFA, 1 pc.",7515,"ST",1,"PI4",1,"FDK:083N8479","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8480","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type C, DN 1800 (72\"), EN 1092-1 PN 10, in stainless steel AISI 304 14.301,00 for all liners except PTFE & PFA, 1 pc.",7722,"ST",1,"PI4",1,"FDK:083N8480","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8481","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type C, DN 1800 (72\"), EN 1092-1 PN 16, in stainless steel AISI 304 14.301,00 for all liners except PTFE & PFA, 1 pc.",7695,"ST",1,"PI4",1,"FDK:083N8481","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8482","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type C, DN 1800 (72\"), AWWA C-207 Class D, in stainless steel AISI 304 14.301,00 for all liners except PTFE & PFA, 1 pc.",7330,"ST",1,"PI4",1,"FDK:083N8482","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8483","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type C, DN 2000 (78\"), EN 1092-1 PN 6, in stainless steel AISI 304 14.301,00 for all liners except PTFE & PFA, 1 pc.",8058,"ST",1,"PI4",1,"FDK:083N8483","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8484","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type C, DN 2000 (78\"), EN 1092-1 PN 10, in stainless steel AISI 304 14.301,00 for all liners except PTFE & PFA, 1 pc.",8327,"ST",1,"PI4",1,"FDK:083N8484","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8485","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type C, DN 2000 (78\"), EN 1092-1 PN 16, in stainless steel AISI 304 14.301,00 for all liners except PTFE & PFA, 1 pc.",8199,"ST",1,"PI4",1,"FDK:083N8485","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8486","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type C, DN 2000 (78\"), AWWA C-207 Class D, in stainless steel AISI 304 14.301,00 for all liners except PTFE & PFA, 1 pc.",7617,"ST",1,"PI4",1,"FDK:083N8486","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8487","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type E, DN 15 (1/2\"), EN 1092-1 PN 40, ANSI B16.5 Class 300, in alloy C-276 2.4819, for PTFE liners, 1 pc.",885,"ST",1,"PI4",1,"FDK:083N8487","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8488","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type E, DN 25 (1\"), EN 1092-1 PN 40, in alloy C-276 2.4819, for PTFE liners, 1 pc.",968,"ST",1,"PI4",1,"FDK:083N8488","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8489","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type E, DN 25 (1\"), ANSI B16.5 Class 300, in alloy C-276 2.4819, for PTFE liners, 1 pc.",968,"ST",1,"PI4",1,"FDK:083N8489","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8490","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type E, DN 40 (1 1/2\"), EN 1092-1 PN 40, in alloy C-276 2.4819, for PTFE liners, 1 pc.",1151,"ST",1,"PI4",1,"FDK:083N8490","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8491","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type E, DN 40 (1 1/2\"), ANSI B16.5 Class 300, in alloy C-276 2.4819, for PTFE liners, 1 pc.",1109,"ST",1,"PI4",1,"FDK:083N8491","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8492","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type E, DN 50 (2\"), EN 1092-1 PN 40, in alloy C-276 2.4819, for PTFE liners, 1 pc.",1415,"ST",1,"PI4",1,"FDK:083N8492","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8493","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type E, DN 50 (2\"), ANSI B16.5 Class 300, in alloy C-276 2.4819, for PTFE liners, 1 pc.",1332,"ST",1,"PI4",1,"FDK:083N8493","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8494","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type E, DN 65 (2 1/2\"), EN 1092-1 PN 6, in alloy C-276 2.4819, for PTFE liners, 1 pc.",1476,"ST",1,"PI4",1,"FDK:083N8494","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8495","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type E, DN 65 (2 1/2\"), EN 1092-1 PN 16, in alloy C-276 2.4819, for PTFE liners, 1 pc.",1558,"ST",1,"PI4",1,"FDK:083N8495","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8496","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type E, DN 65 (2 1/2\"), EN 1092-1 PN 40, in alloy C-276 2.4819, for PTFE liners, 1 pc.",1681,"ST",1,"PI4",1,"FDK:083N8496","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8497","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type E, DN 65 (2 1/2\"), ANSI B16.5 Class 300, in alloy C-276 2.4819, for PTFE liners, 1 pc.",1558,"ST",1,"PI4",1,"FDK:083N8497","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8498","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type E, DN 80 (3\"), EN 1092-1 PN 6, in alloy C-276 2.4819, for PTFE liners, 1 pc.",1617,"ST",1,"PI4",1,"FDK:083N8498","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8499","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type E, DN 80 (3\"), EN 1092-1 PN 16, in alloy C-276 2.4819, for PTFE liners, 1 pc.",1738,"ST",1,"PI4",1,"FDK:083N8499","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8500","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type E, DN 80 (3\"), EN 1092-1 PN 40, in alloy C-276 2.4819, for PTFE liners, 1 pc.",1944,"ST",1,"PI4",1,"FDK:083N8500","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8501","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type E, DN 80 (3\"), ANSI B16.5 Class 150, in alloy C-276 2.4819, for PTFE liners, 1 pc.",1779,"ST",1,"PI4",1,"FDK:083N8501","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8502","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type E, DN 80 (3\"), ANSI B16.5 Class 300, in alloy C-276 2.4819, for PTFE liners, 1 pc.",1900,"ST",1,"PI4",1,"FDK:083N8502","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8503","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type E, DN 100 (4\"), EN 1092-1 PN 6, in alloy C-276 2.4819, for PTFE liners, 1 pc.",1800,"ST",1,"PI4",1,"FDK:083N8503","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8504","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type E, DN 100 (4\"), EN 1092-1 PN 16, in alloy C-276 2.4819, for PTFE liners, 1 pc.",1962,"ST",1,"PI4",1,"FDK:083N8504","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8505","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type E, DN 100 (4\"), EN 1092-1 PN 40, in alloy C-276 2.4819, for PTFE liners, 1 pc.",2209,"ST",1,"PI4",1,"FDK:083N8505","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8506","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type E, DN 100 (4\"), ANSI B16.5 Class 150, in alloy C-276 2.4819, for PTFE liners, 1 pc.",2003,"ST",1,"PI4",1,"FDK:083N8506","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8507","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type E, DN 100 (4\"), ANSI B16.5 Class 300, in alloy C-276 2.4819, for PTFE liners, 1 pc.",2184,"ST",1,"PI4",1,"FDK:083N8507","Όργανα Μέτρησης Πεδίου"]
["FDK:083X16044","SmartPlug replacement for 911-E",675,"ST",1,"PI1",1,"FDK:083X16044","Όργανα Μέτρησης Πεδίου"]
["FDK:085B1089","SITRANS FSS100 spare parts: Gaskets o-ring for FSS100 o-ring transducer type (1 bag with 3 pieces)",292,"ST",1,"PI1",1,"FDK:085B1089","Όργανα Μέτρησης Πεδίου"]
["FDK:085B1360","Coaxial Mountingbox IP65, 4*PG13.5",767,"ST",1,"PI1",1,"FDK:085B1360","Όργανα Μέτρησης Πεδίου"]
["FDK:085B1362","Coaxial EEx-e plasticbox IP65, 4*PG13.5",691,"ST",1,"PI1",1,"FDK:085B1362","Όργανα Μέτρησης Πεδίου"]
["FDK:085B1373","Coaxial Cable 15m (100grd, 75ohm), without connector",89,"ST",1,"PI1",1,"FDK:085B1373","Όργανα Μέτρησης Πεδίου"]
["FDK:085B1374","Coaxial Cable 30m (100grd, 75ohm )",129,"ST",1,"PI1",1,"FDK:085B1374","Όργανα Μέτρησης Πεδίου"]
["FDK:085B1375","Coaxial Cable 60m (100grd, 75ohm )",221,"ST",1,"PI1",1,"FDK:085B1375","Όργανα Μέτρησης Πεδίου"]
["FDK:085B1376","Coaxial Cable 100m (100grd, 75ohm )",356,"ST",1,"PI1",1,"FDK:085B1376","Όργανα Μέτρησης Πεδίου"]
["FDK:085B1378","Coaxial Cable 5m (200grd, 75ohm) PTFE",148,"ST",1,"PI1",1,"FDK:085B1378","Όργανα Μέτρησης Πεδίου"]
["FDK:085B1379","Coaxial Cable 15m (200grd, 75ohm) PTFE",440,"ST",1,"PI1",1,"FDK:085B1379","Όργανα Μέτρησης Πεδίου"]
["FDK:085B1406","SITRANS FSS100 spare part: FSS100 body, O-ring type, with transducer insert element, O-ring gasket in FFKM, body dedicated for Ex-versions, liquid temperature: -20 to +200 deg.C, PN 40, insert length 160 mm.",1324,"ST",1,"PI1",1,"FDK:085B1406","Όργανα Μέτρησης Πεδίου"]
["FDK:085B1411","SONO 3200 Spare Insert L=50mm",386,"ST",1,"PI1",1,"FDK:085B1411","Όργανα Μέτρησης Πεδίου"]
["FDK:085B1419","SONO 3200 Spare Insert (L=160)",468,"ST",1,"PI1",1,"FDK:085B1419","Όργανα Μέτρησης Πεδίου"]
["FDK:085B1420","SONO 3200 Spare Insert (L=230)",452,"ST",1,"PI1",1,"FDK:085B1420","Όργανα Μέτρησης Πεδίου"]
["FDK:085B5330","SITRANS FSS100 Angle measurement tool for sensor mounting FSS100 transducers",8154,"ST",1,"PI1",1,"FDK:085B5330","Όργανα Μέτρησης Πεδίου"]
["FDK:085B5333","SITRANS FSS100 Extraction tool for 160mm FSS100 o-ring transducer types (1 box with tool set)",9886,"ST",1,"PI1",1,"FDK:085B5333","Όργανα Μέτρησης Πεδίου"]
["FDK:085B5335","SITRANS FSS100 Extraction tool for 230mm FSS100 o-ring transducer types(1 box with tool set).",10185,"ST",1,"PI1",1,"FDK:085B5335","Όργανα Μέτρησης Πεδίου"]
["FDK:085B5392","SITRANS FSS100 Hot-tap drill system for FSS100",2640,"ST",1,"PI1",1,"FDK:085B5392","Όργανα Μέτρησης Πεδίου"]
["FDK:085B5393","SITRANS FSS100 FSS100 Alignment tool hot-tap installation for pipes DN300-1200",6298,"ST",1,"PI1",1,"FDK:085B5393","Όργανα Μέτρησης Πεδίου"]
["FDK:085B5452","FSS100 complete transducer, O-ring gasket in FFKM, Liquid temperature: -20 to +200deg.C, PN 40, Length 160 mm, Terminal housing in SS, M20 cable gland and ATEX EExd approval.",3052,"ST",1,"PI1",1,"FDK:085B5452","Όργανα Μέτρησης Πεδίου"]
["FDK:085B5454","FSS100 complete transducer, O-ring gasket in FKM 602, Liquid temperature: -20 to +100deg.C, PN 40, Length 160 mm, Terminal housing in Plastic PA 6.6, M20 cable gland.",1674,"ST",1,"PI1",1,"FDK:085B5454","Όργανα Μέτρησης Πεδίου"]
["FDK:085B5455","FSS100 complete transducer, O-ring gasket in FKM 602, Liquid temperature: -20 to +200deg.C, PN 40, Length 160 mm, Terminal housing in SS, M20 cable gland.",2589,"ST",1,"PI1",1,"FDK:085B5455","Όργανα Μέτρησης Πεδίου"]
["FDK:085B5458","FSS100 complete transducer, O-ring gasket in FKM 602, Liquid temperature: -20 to +100deg.C, PN 40, Length 230 mm, Terminal housing in plastic M20 cable gland.",1771,"ST",1,"PI1",1,"FDK:085B5458","Όργανα Μέτρησης Πεδίου"]
["FDK:085B5459","FSS100 complete transducer, O-ring gasket in FKM 602, Liquid temperature: -20 to +200deg.C, PN 40, Length 230 mm, Terminal housing in SS, M20 cable gland.",2414,"ST",1,"PI1",1,"FDK:085B5459","Όργανα Μέτρησης Πεδίου"]
["FDK:085B5501","Terminal housing in Plastic PA 6.6, Liquid temperature: -20 to +100deg.C, M20 cable gland.",551,"ST",1,"PI1",1,"FDK:085B5501","Όργανα Μέτρησης Πεδίου"]
["FDK:085B5504","Terminal housing in SS, Liquid temperature: -20 to +200deg.C, M20 cable gland.",1884,"ST",1,"PI1",1,"FDK:085B5504","Όργανα Μέτρησης Πεδίου"]
["FDK:085B5505","Terminal housing in SS, Liquid temperature: -20 to +200deg.C, M20 cable gland and ATEX Ex.d.",2164,"ST",1,"PI1",1,"FDK:085B5505","Όργανα Μέτρησης Πεδίου"]
["FDK:085B5510","FSS100 transducer body, O-ring gasket in FKM 602, Liquid temperature: -20 to +200deg.C, PN 40, Length 160 mm.",1182,"ST",1,"PI1",1,"FDK:085B5510","Όργανα Μέτρησης Πεδίου"]
["FDK:085B5511","FSS100 transducer body, O-ring gasket in FKM 602, Liquid temperature: -20 to +200deg.C, PN 40, Length 230 mm.",1420,"ST",1,"PI1",1,"FDK:085B5511","Όργανα Μέτρησης Πεδίου"]
["FDK:085L1102","Transducerholder center track carbon steel 45deg. FSS100 DN100 - DN150, L=160mm",474,"ST",1,"PI1",1,"FDK:085L1102","Όργανα Μέτρησης Πεδίου"]
["FDK:085L1103","Transducerholder center track stainless steel 45deg. FSS100 DN100 - DN150, L=160mm",868,"ST",1,"PI1",1,"FDK:085L1103","Όργανα Μέτρησης Πεδίου"]
["FDK:085L1104","Transducerholder center track carbon steel 60deg. FSS!00 DN200 - DN2400, L=160mm",710,"ST",1,"PI1",1,"FDK:085L1104","Όργανα Μέτρησης Πεδίου"]
["FDK:085L1105","Transducerholder center stainless steel 60deg. FSS100 DN200 - DN2400, L=160mm",853,"ST",1,"PI1",1,"FDK:085L1105","Όργανα Μέτρησης Πεδίου"]
["FDK:085L1107","Transducerholder center stainless steel 60 deg. FSS100 DN600 - DN2400, L=230mm",1829,"ST",1,"PI1",1,"FDK:085L1107","Όργανα Μέτρησης Πεδίου"]
["FDK:085L1108","Transducerholder non-central carbon steel 60deg. FSS100 DN200 - DN4000, L=160mm",871,"ST",1,"PI1",1,"FDK:085L1108","Όργανα Μέτρησης Πεδίου"]
["FDK:085L1109","Transducerholder 2-Track stainless steel 60deg.  SONOKIT DN200 - DN4000,  L=160mm",734,"ST",1,"PI1",1,"FDK:085L1109","Όργανα Μέτρησης Πεδίου"]
["FDK:085L1111","Transducerholder 2-Track stainless steel 60deg.  SONOKIT DN200 - DN4000,  L=230mm",1124,"ST",1,"PI1",1,"FDK:085L1111","Όργανα Μέτρησης Πεδίου"]
["FDK:085L1112","FSS100 monting plate for sensor holder, carbon steel, monting angle 45, plate for 1,3 path sensor sizes DN100 - DN150(4\" - 6\"), 1 PC",175,"ST",1,"PI1",1,"FDK:085L1112","Όργανα Μέτρησης Πεδίου"]
["FDK:085L1113","FSS100  monting plate for sensor holder, stainless steel, monting angle 45, plate for 1,3 path sensor DN100 - DN150(4\" - 6\"), 1 pc.",371,"ST",1,"PI1",1,"FDK:085L1113","Όργανα Μέτρησης Πεδίου"]
["FDK:085L1114","FSS100 Mounting plate 1-track Mild steel",134,"ST",1,"PI1",1,"FDK:085L1114","Όργανα Μέτρησης Πεδίου"]
["FDK:085L1115","FSS100 Mounting plate 1-track AISI316",212,"ST",1,"PI1",1,"FDK:085L1115","Όργανα Μέτρησης Πεδίου"]
["FDK:085L1118","FSS100 Mounting plate 2-track Mild steel",160,"ST",1,"PI1",1,"FDK:085L1118","Όργανα Μέτρησης Πεδίου"]
["FDK:085L1119","FSS100 Mounting plate 2-track AISI316",467,"ST",1,"PI1",1,"FDK:085L1119","Όργανα Μέτρησης Πεδίου"]
["FDK:085U0192","SENSOREPROM 2KB FOR MAG3000/3100",195,"ST",1,"PI4",1,"FDK:085U0192","Όργανα Μέτρησης Πεδίου"]
["FDK:085U0220","Accessory SITRANS FM Potting kit for IP68/NEMA 6P sealing of sensor terminal box",168,"ST",1,"PI4",1,"FDK:085U0220","Όργανα Μέτρησης Πεδίου"]
["FDK:085U0221","Acc.bag USM Sealing Screws",59,"ST",1,"PI4",1,"FDK:085U0221","Όργανα Μέτρησης Πεδίου"]
["FDK:085U0226","USM II, HART MODUL",260,"ST",1,"PI4",1,"FDK:085U0226","Όργανα Μέτρησης Πεδίου"]
["FDK:085U0228","USM II, Can Open Modul",291,"ST",1,"PI4",1,"FDK:085U0228","Όργανα Μέτρησης Πεδίου"]
["FDK:085U0234","USM II, MODBUS RTU modul",260,"ST",1,"PI4",1,"FDK:085U0234","Όργανα Μέτρησης Πεδίου"]
["FDK:085U0235","USM II, Profibus DP modul BOSCH",513,"ST",1,"PI4",1,"FDK:085U0235","Όργανα Μέτρησης Πεδίου"]
["FDK:085U0236","Add-on module Profibus PA profile 3.",534,"ST",1,"PI4",1,"FDK:085U0236","Όργανα Μέτρησης Πεδίου"]
["FDK:085U0237","Add-on module Profibus DP profile 3.",534,"ST",1,"PI4",1,"FDK:085U0237","Όργανα Μέτρησης Πεδίου"]
["FDK:085U0321","HART MODUL INDUSTRY MAG",265,"ST",1,"PI4",1,"FDK:085U0321","Όργανα Μέτρησης Πεδίου"]
["FDK:085U1000","Accessory USM terminal box AISI316 w.Lid",344,"ST",1,"PI1",1,"FDK:085U1000","Όργανα Μέτρησης Πεδίου"]
["FDK:085U1003","Accessory USM Ass. Terminal box lid",110,"ST",1,"PI1",1,"FDK:085U1003","Όργανα Μέτρησης Πεδίου"]
["FDK:085U1005","SITRANS F M Spare part MAG SENSORPROM 2KB (1 Stk.) Required information: Complete MLFB and serial number of original unit",56,"ST",1,"PI1",1,"FDK:085U1005","Όργανα Μέτρησης Πεδίου"]
["FDK:085U1006","DN10 INCLUDING 2 EPDM GASKETS WITH COLLAR",23,"ST",1,"PI1",1,"FDK:085U1006","Όργανα Μέτρησης Πεδίου"]
["FDK:085U1007","DN15 INCLUDING 2 EPDM GASKETS WITH COLLAR",23,"ST",1,"PI1",1,"FDK:085U1007","Όργανα Μέτρησης Πεδίου"]
["FDK:085U1008","Prog. SENSORPROM 256b QUOTE SENSOR CODE NO., SERIAL NO. AND CAL.FACTOR",213,"ST",1,"PI1",1,"FDK:085U1008","Όργανα Μέτρησης Πεδίου"]
["FDK:085U1009","DN25 INCLUDING 2 EPDM GASKETS WITH COLLAR",19,"ST",1,"PI1",1,"FDK:085U1009","Όργανα Μέτρησης Πεδίου"]
["FDK:085U1010","DN32 INCLUDING 2 EPDM GASKETS WITH COLLAR",35,"ST",1,"PI1",1,"FDK:085U1010","Όργανα Μέτρησης Πεδίου"]
["FDK:085U1011","DN40 INCLUDING 2 EPDM GASKETS WITH COLLAR",20,"ST",1,"PI1",1,"FDK:085U1011","Όργανα Μέτρησης Πεδίου"]
["FDK:085U1012","DN50 INCLUDING 2 EPDM GASKETS WITH COLLAR",36,"ST",1,"PI1",1,"FDK:085U1012","Όργανα Μέτρησης Πεδίου"]
["FDK:085U1013","DN65 INCLUDING 2 EPDM GASKETS WITH COLLAR",43,"ST",1,"PI1",1,"FDK:085U1013","Όργανα Μέτρησης Πεδίου"]
["FDK:085U1016","COUNTERPIECES FOR HYGIENE SCREWED CONNECTION DN10 DIN11851",125,"ST",1,"PI4",1,"FDK:085U1016","Όργανα Μέτρησης Πεδίου"]
["FDK:085U1017","Mating part for hygienic fitting DN15 DIN11851",120,"ST",1,"PI4",1,"FDK:085U1017","Όργανα Μέτρησης Πεδίου"]
["FDK:085U1018","Wall mounting unit, 4x M20 cable glands",275,"ST",1,"PI4",1,"FDK:085U1018","Όργανα Μέτρησης Πεδίου"]
["FDK:085U1019","Mating part for hygienic fitting DN25 DIN11851",120,"ST",1,"PI4",1,"FDK:085U1019","Όργανα Μέτρησης Πεδίου"]
["FDK:085U1020","Mating part for hygienic fitting DN32 DIN11851",120,"ST",1,"PI4",1,"FDK:085U1020","Όργανα Μέτρησης Πεδίου"]
["FDK:085U1021","Mating part for hygienic fitting DN40 DIN11851",120,"ST",1,"PI4",1,"FDK:085U1021","Όργανα Μέτρησης Πεδίου"]
["FDK:085U1022","Mating part for hygienic fitting DN50 DIN11851",175,"ST",1,"PI4",1,"FDK:085U1022","Όργανα Μέτρησης Πεδίου"]
["FDK:085U1023","Mating part for hygienic fitting DN65  DIN11851",242,"ST",1,"PI4",1,"FDK:085U1023","Όργανα Μέτρησης Πεδίου"]
["FDK:085U1029","Mating part for hygienic clamp DN25 ISO2852",252,"ST",1,"PI4",1,"FDK:085U1029","Όργανα Μέτρησης Πεδίου"]
["FDK:085U1031","Mating part for hygienic clamp DN40 ISO2852",252,"ST",1,"PI4",1,"FDK:085U1031","Όργανα Μέτρησης Πεδίου"]
["FDK:085U1032","Mating part for hygienic clamp DN50 ISO2852",308,"ST",1,"PI4",1,"FDK:085U1032","Όργανα Μέτρησης Πεδίου"]
["FDK:085U1038","Keypad/Display Unit MAG5000/6000 IP67",205,"ST",1,"PI1",1,"FDK:085U1038","Όργανα Μέτρησης Πεδίου"]
["FDK:085U1039","Keypad/Display Unit MAG5000/6000 IP67",205,"ST",1,"PI1",1,"FDK:085U1039","Όργανα Μέτρησης Πεδίου"]
["FDK:085U1050","Terminalbox with lid, Polyamid, M20 cable glands. The Kit is not approved  for Hazardous locations",177,"ST",1,"PI1",1,"FDK:085U1050","Όργανα Μέτρησης Πεδίου"]
["FDK:085U1052","Terminalbox with lid, Polyamid, 1/2 NPT cable glands",177,"ST",1,"PI1",1,"FDK:085U1052","Όργανα Μέτρησης Πεδίου"]
["FDK:085U1053","Wall mounting unit, 4x 1/2 NPT cable glands",275,"ST",1,"PI4",1,"FDK:085U1053","Όργανα Μέτρησης Πεδίου"]
["FDK:085U1514","FRAME FOR INDICATING DEVICE, IP67, MKIII AND IV",23,"ST",1,"PI1",1,"FDK:085U1514","Όργανα Μέτρησης Πεδίου"]
["FDK:085U2374","MASS 6000 screws & sealing, Ex piedestal",98,"ST",1,"PI1",1,"FDK:085U2374","Όργανα Μέτρησης Πεδίου"]
["FDK:085U3122","MAG INDUSTRY ACC. DISPLAY",181,"ST",1,"PI1",1,"FDK:085U3122","Όργανα Μέτρησης Πεδίου"]
["FDK:085U3123","MAG 6000 I standard (non-Ex) 18...30 VDC; 115...230/24 VAC Spare PCBA unit (not for use with Ex sensors)",1220,"ST",1,"PI1",1,"FDK:085U3123","Όργανα Μέτρησης Πεδίου"]
["FDK:085U3144","MAG 6000I Accessory bag",56,"ST",1,"PI1",1,"FDK:085U3144","Όργανα Μέτρησης Πεδίου"]
["FDK:087H3007","Sparepart SITRANS F US: Transducer spare part set for SITRANS FUS880 retrofit system, with 2 pcs. transducer.",454,"ST",1,"PI1",1,"FDK:087H3007","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4080","MAG8000 Accessories Demo and training package",2508,"ST",1,"PI7",1,"FDK:087L4080","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4142","Alkaline battery for  MAG 8000 demo transmitter  (3 V 13 Ah) (No dangerous goods limitations)",35,"ST",1,"PI1",1,"FDK:087L4142","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4150","SITRANS F M Accessory MAG 8000 Internal Battery with connector, 2 D-cell (3.6 V, 34 Ah), incl. accessories for replacement and NBR O-ring.",275,"ST",1,"PI7",1,"FDK:087L4150","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4151","MAG8000 Accessories, External Battery pack IP68/NEMA 6P with connector, 4 D-Cell (3.6 V 68 Ah) Without power cable.",386,"ST",1,"PI7",1,"FDK:087L4151","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4152","MAG8000 Accessories, Power cable, 1,5 m (4.9 ft) with IP68/NEMA 6P plugs for external battery. PE jacket, ambient temperature - 20 Cel. ... +60 Cel. (-4 ... +140 F)",159,"ST",1,"PI7",1,"FDK:087L4152","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4154","MAG8000 Accessories Cable entry M20 brass, one entry 2-5mm,10pcs.",205,"ST",1,"PI7",1,"FDK:087L4154","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4155","MAG8000 Accessories Cable entry M20 brass, one 6-8mm, 10pcs.",161,"ST",1,"PI7",1,"FDK:087L4155","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4156","MAG8000 Accessories Cable entry M20 brass, one 8-11mm,10pcs.",161,"ST",1,"PI7",1,"FDK:087L4156","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4157","MAG8000 Accessories Cable entry M20 brass, one 11-15mm,10pcs.",177,"ST",1,"PI7",1,"FDK:087L4157","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4158","MAG8000  Accessories Cable entry M20 brass, two entries 3.5-5mm,10pcs",215,"ST",1,"PI7",1,"FDK:087L4158","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4159","MAG8000 Accessories Cable entry M20brass, two 5.5-7.5mm,10pcs.",221,"ST",1,"PI7",1,"FDK:087L4159","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4162","MAG8000 Servicetool Kit",402,"ST",1,"PI1",1,"FDK:087L4162","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4163","MAG8000 Accessories USB Irda adapter",499,"ST",1,"PI7",1,"FDK:087L4163","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4165","MAG8000 Hardware Key",67,"ST",1,"PI7",1,"FDK:087L4165","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4166","MAG8000 Transmitter Compact replacement kit. No battery included. Mandatory requirements: Complete MLFB and serial number of original unit and Not programmed version FDK-087L4203",1485,"ST",1,"PI1",1,"FDK:087L4166","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4167","MAG 8000 Accessories Enclosure top including plastic lid, screws and blank product label.",454,"ST",1,"PI7",1,"FDK:087L4167","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4168","MAG 8000 (Advanced version) transmitter PCB replacement kit. No system number required.",1467,"ST",1,"PI1",1,"FDK:087L4168","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4196","MAG8000 Accessories Cable entry M20 brass, one 6-8mm,1pcs",32,"ST",1,"PI7",1,"FDK:087L4196","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4202","MAG8000 Transmitter Remote replacement kit Mandatory requirements: Complete MLFB and serial number of original unit and Not programmed version FDK-087L4204",1848,"ST",1,"PI1",1,"FDK:087L4202","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4203","MAG8000 (Advanced Version) transmitter compact replacement kit. No battery included. No system number required.",1546,"ST",1,"PI1",1,"FDK:087L4203","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4204","MAG8000 (Advanced version) Transmitter remote replacement kit No battery included. No system number required.",1893,"ST",1,"PI1",1,"FDK:087L4204","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4210","SITRANS FM Accessory  MAG 8000 Mains power supply  12...24 V AC/DC with battery  backup and 3 m (9.8 ft)  power cable for external  connection (no battery  included)",639,"ST",1,"PI7",1,"FDK:087L4210","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4211","SITRANS FM Accessory  MAG 8000 Mains power supply  115 ... 230 VAC with battery  backup up and 3 m (9.8 ft)  power cable for external  connection (no battery  included)",634,"ST",1,"PI7",1,"FDK:087L4211","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4212","SITRANS FM Accessory  MAG 8000 RS 232 add-on module  point to point communication  interface with Modbus  RTU protocol",438,"ST",1,"PI7",1,"FDK:087L4212","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4213","SITRANS FM Accessory  MAG 8000 RS485 add-on module  multidrop communication  interface with Modbus RTU  protocol",438,"ST",1,"PI7",1,"FDK:087L4213","Όργανα Μέτρησης Πεδίου"]
["FDK:087L6001","MAG8000 Accessories Flow Tool Configuration Software CD",265,"ST",1,"PI7",1,"FDK:087L6001","Όργανα Μέτρησης Πεδίου"]
["FDK:521H0552","LITERATURE - SFIDKPS029V201 ISSUER OF LITERATURE : SIEMENS FLOW INSTRUMENTS A/S DENMARK LITERATURE CATEGORY : PRINT/PAPER LITERATURE SUBCATEGORY : HANDBOOKS MAIN PRODUCT GROUP : SONO ISSUE : V VERSION : 2 LANGUAGE CODE : DANISH",13,"ST",1,"PI1",1,"FDK:521H0552","Όργανα Μέτρησης Πεδίου"]
["FDK:521H0553","LITERATURE - SFIDKPS029V202 ISSUER OF LITERATURE : SIEMENS FLOW INSTRUMENTS A/S DENMARK LITERATURE CATEGORY : PRINT/PAPER LITERATURE SUBCATEGORY : HANDBOOKS MAIN PRODUCT GROUP : SONO ISSUE : V VERSION : 2 LANGUAGE CODE : ENGLISH",13,"ST",1,"PI1",1,"FDK:521H0553","Όργανα Μέτρησης Πεδίου"]
["FDK:521H1189","Literature - SFIDKPS023C102 Issuer of literature : Siemens Flow Instruments A/S Denmark Literature category : Print/paper Literature subcategory : Handbooks Main product group : USM Issue : C Version : 1 Language code : English",7,"ST",1,"PI1",1,"FDK:521H1189","Όργανα Μέτρησης Πεδίου"]
["JJY:023146720008","Fa. Heine Breaking resistor FOR POWERMODULE FSA P_MAX=750W/12S/5% ED R=200 OHM P_DAUER=37,5W",123,"ST",1,"GMC",1,"JJY:023146720008","Ρυθμιστές στροφών και συστήματα Motion control"]
["JJY:023151720007","Fa. Heine Breaking resistor FOR POWERMODULE FSB P_MAX=2200W/12S/5% ED R=68 OHM P_DAUER=110W",170,"ST",1,"GMC",1,"JJY:023151720007","Ρυθμιστές στροφών και συστήματα Motion control"]
["JJY:023163720018","Fa. Heine Breaking resistor FOR POWERMODULE FSC1 P_MAX=4000W/12S/5% ED R=37 OHM P_DAUER=200W",236,"ST",1,"GMC",1,"JJY:023163720018","Ρυθμιστές στροφών και συστήματα Motion control"]
["JJY:023422620001","Fa. Heine Breaking resistor FOR POWERMODULE PM240-2 FSD P_MAX=22kW/12S/5% ED R=25 OHM P_DAUER=1100W",661,"ST",1,"GMC",1,"JJY:023422620001","Ρυθμιστές στροφών και συστήματα Motion control"]
["JJY:023422620002","Fa. Heine Breaking resistor FOR POWERMODULE PM240-2 FSD P_MAX=18,5kW/12S/5% ED R=7,5 OHM P_DAUER=930W",755,"ST",1,"GMC",1,"JJY:023422620002","Ρυθμιστές στροφών και συστήματα Motion control"]
["JJY:023423320001","Fa. Heine Breaking resistor FOR POWERMODULE PM240-2 FSE P_MAX=30kW/12S/5% ED R=4,5 OHM P_DAUER=1500W",1038,"ST",1,"GMC",1,"JJY:023423320001","Ρυθμιστές στροφών και συστήματα Motion control"]
["JJY:023424020001","Fa. Heine Breaking resistor FOR POWERMODULE PM240-2 FSD P_MAX=37kW/12S/5% ED R=15 OHM P_DAUER=1850W",944,"ST",1,"GMC",1,"JJY:023424020001","Ρυθμιστές στροφών και συστήματα Motion control"]
["JJY:023424020002","Fa. Heine Breaking resistor FOR POWERMODULE PM240-2 FSD P_MAX=37kW/12S/5% ED R=31 OHM P_DAUER=1850W",1085,"ST",1,"GMC",1,"JJY:023424020002","Ρυθμιστές στροφών και συστήματα Motion control"]
["JJY:023433720001","Heine company braking resistor for power module FSC2 P_max=7500 W/12 s/5% on-load factor R=20 Ohm P_duration=375 W",349,"ST",1,"GMC",1,"JJY:023433720001","Ρυθμιστές στροφών και συστήματα Motion control"]
["JJY:023434020001","Fa. Heine Breaking resistor FOR POWERMODULE PM240-2 FSE P_MAX=55kW/12S/5% ED R=10 OHM P_DAUER=2750W",1415,"ST",1,"GMC",1,"JJY:023434020001","Ρυθμιστές στροφών και συστήματα Motion control"]
["JJY:023434020002","Fa. Heine Breaking resistor FOR POWERMODULE PM240-2 FSE P_MAX=55kW/12S/5% ED R=21 OHM P_DAUER=2750W",1736,"ST",1,"GMC",1,"JJY:023434020002","Ρυθμιστές στροφών και συστήματα Motion control"]
["JJY:023434020003","Fa. Heine Breaking resistor FOR POWERMODULE PM240-2 FSF P_MAX=55kW/12S/5% ED R=2,5 OHM P_DAUER=2750W",1698,"ST",1,"GMC",1,"JJY:023434020003","Ρυθμιστές στροφών και συστήματα Motion control"]
["JJY:023454020001","Fa. Heine Breaking resistor FOR POWERMODULE PM240-2 FSF P_MAX=77kW/12S/5% ED R=7,1 OHM P_DAUER=3850W This braking resistor consists of the 2 braking resistors: JJY:023422620001 and JJY:023434020001, which must be connected in parallel on plant.",2150,"ST",1,"GMC",1,"JJY:023454020001","Ρυθμιστές στροφών και συστήματα Motion control"]
["JJY:023464020001","Fa. Heine Breaking resistor FOR POWERMODULE PM240-2 FSF P_MAX=110kW/12S/5% ED R=5 OHM P_DAUER=5500W This braking resistor consists of 2x JJY:023434020001 braking resistors, which must be connected in parallel on the plant",2904,"ST",1,"GMC",1,"JJY:023464020001","Ρυθμιστές στροφών και συστήματα Motion control"]
["JJY:023464020002","Fa. Heine Breaking resistor FOR POWERMODULE PM240-2 FSF P_MAX=110kW/12S/5% ED R=10,5 OHM P_DAUER=5500W This braking resistor consists of 2x JJY:023434020002 braking resistors, which must be connected in parallel on plant.",3546,"ST",1,"GMC",1,"JJY:023464020002","Ρυθμιστές στροφών και συστήματα Motion control"]
["JTA:TEF1203-0GB","Mdexx dv/dt filter with VPL for SINAMICS G120 voltage peak limit 690 V <(><<)>= 18.5 kW 400 V <(><<)>= 7.5 kW SINAMICS Pool Software V4.7 SP10 or higher is required for G120 application SINAMICS Pool Software V5.1 SP1 or higher is required for S120 application",1983,"ST",1,"GMC",1,"JTA:TEF12030GB","Ρυθμιστές στροφών και συστήματα Motion control"]
["JTA:TEF1203-0HB","Mdexx dv/dt filter with VPL for SINAMICS G120 voltage peak limit 690V 22 - 37 kW 400 V 11 kW - 18.5 kW SINAMICS Pool Software V4.7 SP10 or higher is required for G120 application SINAMICS Pool Software V5.1 SP1 or higher is required for S120 application",3540,"ST",1,"GMC",1,"JTA:TEF12030HB","Ρυθμιστές στροφών και συστήματα Motion control"]
["JTA:TEF1203-0JB","Mdexx dv/dt filter with VPL for SINAMICS G120 voltage peak limit 690 V 45 - 55 kW 400 V 22 kW - 30 kW SINAMICS Pool Software V4.7 SP10 or higher is required for G120 application SINAMICS Pool Software V5.1 SP1 or higher is required for S120 application",4536,"ST",1,"GMC",1,"JTA:TEF12030JB","Ρυθμιστές στροφών και συστήματα Motion control"]
["JTA:TEF1203-0KB","Mdexx dv/dt filter with VPL for SINAMICS G120 voltage peak limit 690 V 75 - 90 kW 400 V 37 kW - 45 kW SINAMICS Pool Software V4.7 SP10 or higher is required for G120 application SINAMICS Pool Software V5.1 SP1 or higher is required for S120 application",5988,"ST",1,"GMC",1,"JTA:TEF12030KB","Ρυθμιστές στροφών και συστήματα Motion control"]
["JTA:TEF1203-0LB","Mdexx dv/dt filter with VPL for SINAMICS G120 voltage peak limit 690 V 110 - 132 kW 400 V 55 kW - 75 kW SINAMICS Pool Software V4.7 SP10 or higher is required for G120 application SINAMICS Pool Software V5.1 SP1 or higher is required for S120 application",7122,"ST",1,"GMC",1,"JTA:TEF12030LB","Ρυθμιστές στροφών και συστήματα Motion control"]
["JTA:TEF1203-0MB","Mdexx dv/dt filter with VPL for SINAMICS G120 voltage peak limit 690 V 160 - 250 kW 400 V 90 kW - 132 kW SINAMICS Pool Software V4.7 SP10 or higher is required for G120 application SINAMICS Pool Software V5.1 SP1 or higher is required for S120 application",9150,"ST",1,"GMC",1,"JTA:TEF12030MB","Ρυθμιστές στροφών και συστήματα Motion control"]
["JTA:TEU2532-0FP00-4EA0","Output Choke 690V 3 -18.5 kW",927,"ST",1,"GMC",1,"JTA:TEU25320FP004EA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["JTA:TEU4732-0FA00-0BA0","Output Choke 690V 160 -250 kW",4885,"ST",1,"GMC",1,"JTA:TEU47320FA000BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["JTA:TEU9932-0FP00-4EA0","Output Choke 690V 22 -37 kW",1769,"ST",1,"GMC",1,"JTA:TEU99320FP004EA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["JTA:TEU9932-0FS00-0EA0","Output Choke 690V 45 -55 kW",2275,"ST",1,"GMC",1,"JTA:TEU99320FS000EA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["JTA:TEU9932-0FV00-1BA0","Output Choke 690V 110 -132 kW",4464,"ST",1,"GMC",1,"JTA:TEU99320FV001BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["JTA:TEU9932-1FC00-1BA0","Output Choke 690V 75 -90 kW",3285,"ST",1,"GMC",1,"JTA:TEU99321FC001BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["KRH:16000100","Sparepart SITRANS FXT030 Electronic for SITRANS FX330 non-Ex/Ex-i in compact design with HART",3923,"ST",1,"PI1",1,"KRH:16000100","Όργανα Μέτρησης Πεδίου"]
["KRH:16000300","Cover gasket O-ring",58,"ST",1,"PI1",1,"KRH:16000300","Όργανα Μέτρησης Πεδίου"]
["KRH:16000400","Converter housing gasket 59,35,5-2-N",63,"ST",1,"PI1",1,"KRH:16000400","Όργανα Μέτρησης Πεδίου"]
["KRH:16000500","Cable feed through, 10 pole (non Ex)",473,"ST",1,"PI1",1,"KRH:16000500","Όργανα Μέτρησης Πεδίου"]
["KRH:16002000","Front Cover (non Ex)",320,"ST",1,"PI1",1,"KRH:16002000","Όργανα Μέτρησης Πεδίου"]
["KRH:16002500","Front Cover (Ex)",768,"ST",1,"PI1",1,"KRH:16002500","Όργανα Μέτρησης Πεδίου"]
["KRH:16003000","Back Cover",163,"ST",1,"PI1",1,"KRH:16003000","Όργανα Μέτρησης Πεδίου"]
["KRH:16111100","Sparepart SITRANS FXS300 Sensor replacement kit DN15 including seal disc, socket, pickup and O-rings (for pickup and pressure screw)",2174,"ST",1,"PI1",1,"KRH:16111100","Όργανα Μέτρησης Πεδίου"]
["KRH:16111110","Sparepart SITRANS FXS300 Sensor replacement kit DN15 Conical including seal disc, socket, pickup and O-rings (for pickup and pressure screw)",2174,"ST",1,"PI1",1,"KRH:16111110","Όργανα Μέτρησης Πεδίου"]
["KRH:16111150","Sparepart SITRANS FXS300 Sensor replacement kit DN25 including seal disc, socket, pickup and O-rings (for pickup and pressure screw)",2174,"ST",1,"PI1",1,"KRH:16111150","Όργανα Μέτρησης Πεδίου"]
["KRH:16111160","Sparepart SITRANS FXS300 Sensor replacement kit DN25 Conical including seal disc, socket, pickup and O-rings (for pickup and pressure screw)",2174,"ST",1,"PI1",1,"KRH:16111160","Όργανα Μέτρησης Πεδίου"]
["KRH:16111200","Sparepart SITRANS FXS300 Sensor replacement kit DN40 including seal disc, socket, pickup and O-rings (for pickup and pressure screw)",2174,"ST",1,"PI1",1,"KRH:16111200","Όργανα Μέτρησης Πεδίου"]
["KRH:16111210","Sparepart SITRANS FXS300 Sensor replacement kit DN50 including seal disc, socket, pickup and O-rings (for pickup and pressure screw)",2174,"ST",1,"PI1",1,"KRH:16111210","Όργανα Μέτρησης Πεδίου"]
["KRH:16111220","Sparepart SITRANS FXS300 Sensor replacement kit DN80 including seal disc, socket, pickup and O-rings (for pickup and pressure screw)",2174,"ST",1,"PI1",1,"KRH:16111220","Όργανα Μέτρησης Πεδίου"]
["KRH:16111230","Sparepart SITRANS FXS300 Sensor replacement kit DN100 including seal disc, socket, pickup and O-rings (for pickup and pressure screw)",2174,"ST",1,"PI1",1,"KRH:16111230","Όργανα Μέτρησης Πεδίου"]
["KRH:16111300","Sparepart SITRANS FXS300 Sensor replacement kit DN150-300 including seal disc, socket, pickup and O-rings (for pickup and pressure screw)",2174,"ST",1,"PI1",1,"KRH:16111300","Όργανα Μέτρησης Πεδίου"]
["KRH:16111350","Sparepart SITRANS FX330 Pressure sensor replacement kit 1 bar, including pressure sensor 1 bar with calibration certificate,DUBOX plug and 2x O-ring DIN 3771-20x1-FPM",2428,"ST",1,"PI1",1,"KRH:16111350","Όργανα Μέτρησης Πεδίου"]
["KRH:16111370","Sparepart SITRANS FX330 Pressure sensor replacement kit 2 bar, including pressure sensor 2 bar with calibration certificate,DUBOX plug and 2x O-ring DIN 3771-20x1-FPM",2428,"ST",1,"PI1",1,"KRH:16111370","Όργανα Μέτρησης Πεδίου"]
["KRH:16111400","Sparepart SITRANS FX330 Pressure sensor replacement kit 4 bar, including pressure sensor 4 bar with calibration certificate,DUBOX plug and 2x O-ring DIN 3771-20x1-FPM",2428,"ST",1,"PI1",1,"KRH:16111400","Όργανα Μέτρησης Πεδίου"]
["KRH:16111401","Sparepart SITRANS FX330 Pressure sensor replacement kit 6 bar, including pressure sensor 6 bar with calibration certificate,DUBOX plug and 2x O-ring DIN 3771-20x1-FPM",2428,"ST",1,"PI1",1,"KRH:16111401","Όργανα Μέτρησης Πεδίου"]
["KRH:16111402","Sparepart SITRANS FX330 Pressure sensor replacement kit 10 bar, including pressure sensor 10 bar with calibration certificate,DUBOX plug and 2x O-ring DIN 3771-20x1-FPM",2428,"ST",1,"PI1",1,"KRH:16111402","Όργανα Μέτρησης Πεδίου"]
["KRH:16111403","Sparepart SITRANS FX330 Pressure sensor replacement kit 16 bar, including pressure sensor 16 bar with calibration certificate,DUBOX plug and 2x O-ring DIN 3771-20x1-FPM",2428,"ST",1,"PI1",1,"KRH:16111403","Όργανα Μέτρησης Πεδίου"]
["KRH:16111404","Sparepart SITRANS FX330 Pressure sensor replacement kit 25 bar, including pressure sensor 25 bar with calibration certificate,DUBOX plug and 2x O-ring DIN 3771-20x1-FPM",2428,"ST",1,"PI1",1,"KRH:16111404","Όργανα Μέτρησης Πεδίου"]
["KRH:16111405","Sparepart SITRANS FX330 Pressure sensor replacement kit 40 bar, including pressure sensor 40 bar with calibration certificate,DUBOX plug and 2x O-ring DIN 3771-20x1-FPM",2428,"ST",1,"PI1",1,"KRH:16111405","Όργανα Μέτρησης Πεδίου"]
["KRH:16111406","Sparepart SITRANS FX330 Pressure sensor replacement kit 60 bar, including pressure sensor 60 bar with calibration certificate,DUBOX plug and 2x O-ring DIN 3771-20x1-FPM",2428,"ST",1,"PI1",1,"KRH:16111406","Όργανα Μέτρησης Πεδίου"]
["KRH:16111407","Sparepart SITRANS FX330 Pressure sensor replacement kit 100 bar, including pressure sensor 100 bar with calibration certificate,DUBOX plug and 2x O-ring DIN 3771-20x1-FPM",2428,"ST",1,"PI1",1,"KRH:16111407","Όργανα Μέτρησης Πεδίου"]
["KRH:16112000","Converter housing for compact or remote version with front and back cover Aluminium Type Plate attached to housing Non Ex/Ex-i Cable gland: 1pc. M20 x 1,5 (plastic-grey),2pc. Blind plug",1506,"ST",1,"PI1",1,"KRH:16112000","Όργανα Μέτρησης Πεδίου"]
["KRH:16112002","Wall housing incl. Neck (incl. Screws, Gaskets and cable glands)",1106,"ST",1,"PI1",1,"KRH:16112002","Όργανα Μέτρησης Πεδίου"]
["KRH:17000700","Seal disc 21,8-12-0,1",63,"ST",1,"PI1",1,"KRH:17000700","Όργανα Μέτρησης Πεδίου"]
["KRH:17000800","SITRANS FX300 DUBOX plug , 5-pole-ger-RM2",8,"ST",1,"PI1",1,"KRH:17000800","Όργανα Μέτρησης Πεδίου"]
["KRH:17001000","O-Ring 10x2-NBR",12,"ST",1,"PI1",1,"KRH:17001000","Όργανα Μέτρησης Πεδίου"]
["KRH:17001100","O-Ring DIN 3771-20x1-FPM",6,"ST",1,"PI1",1,"KRH:17001100","Όργανα Μέτρησης Πεδίου"]
["KRH:17001200","O-ring for pressure screw 17,13x2,62-FPM-70",8,"ST",1,"PI1",1,"KRH:17001200","Όργανα Μέτρησης Πεδίου"]
["KRH:17001400","O-ring pickup",6,"ST",1,"PI1",1,"KRH:17001400","Όργανα Μέτρησης Πεδίου"]
["KRH:17004000","Shut-off valve",2054,"ST",1,"PI1",1,"KRH:17004000","Όργανα Μέτρησης Πεδίου"]
["KRH:17006000","Centering rings for Sandwich-Version, DN15",70,"ST",1,"PI1",1,"KRH:17006000","Όργανα Μέτρησης Πεδίου"]
["KRH:17006001","Centering rings for Sandwich-Version, DN25",123,"ST",1,"PI1",1,"KRH:17006001","Όργανα Μέτρησης Πεδίου"]
["KRH:17006002","Centering rings for Sandwich-Version, DN40",143,"ST",1,"PI1",1,"KRH:17006002","Όργανα Μέτρησης Πεδίου"]
["KRH:17006003","Centering rings for Sandwich-Version, DN50",156,"ST",1,"PI1",1,"KRH:17006003","Όργανα Μέτρησης Πεδίου"]
["KRH:17006004","Centering rings for Sandwich-Version, DN50 (300lbs, 600lbs)",171,"ST",1,"PI1",1,"KRH:17006004","Όργανα Μέτρησης Πεδίου"]
["KRH:17006005","Centering rings forSandwich-Version, DN50 (JIS 10K, 16K, 20K)",247,"ST",1,"PI1",1,"KRH:17006005","Όργανα Μέτρησης Πεδίου"]
["KRH:17006006","Centering rings for Sandwich-Version, DN80",225,"ST",1,"PI1",1,"KRH:17006006","Όργανα Μέτρησης Πεδίου"]
["KRH:17006007","Centering rings for Sandwich-Version, DN100",442,"ST",1,"PI1",1,"KRH:17006007","Όργανα Μέτρησης Πεδίου"]
["KRH:TAGPLATE120X46","TAG name plate in stainless steel SITRANS FX330, 120 x 46 mm (Add plain text to order)",80,"ST",1,"PI1",1,"KRH:TAGPLATE120X46","Όργανα Μέτρησης Πεδίου"]
["KRH:TAGPLATE40X20","TAG name plate in stainless steel SITRANS FX330, 40 x 20 mm (Add plain text to order)",53,"ST",1,"PI1",1,"KRH:TAGPLATE40X20","Όργανα Μέτρησης Πεδίου"]
["LZS:PT17021","Fixing/reject bracket for plug-in relay RT series and PT screw terminals logical and PT spring-loaded terminal socket logical disconnection",42.54,"ΤΕΜ",100,"EP",10,"LZS:PT17021","LZS Μίνι Ρελέ"]
["LZS:PT17024","Fixing/reject bracket for plug-in relay RT series and PT screw terminal base not logical",43.1,"ΤΕΜ",100,"EP",10,"LZS:PT17024","LZS Μίνι Ρελέ"]
["LZS:PT17040","Labeling plate 26 mm for PT relay",30.56,"ΤΕΜ",100,"EP",10,"LZS:PT17040","LZS Μίνι Ρελέ"]
["LZS:PT170P1","fanning strip 2-pole for PT push-in terminal sockets",1.44,"ΤΕΜ",1,"EP",10,"LZS:PT170P1","LZS Μίνι Ρελέ"]
["LZS:PT170R6","Fanning strip 6-pole for PT screw-type terminal",8.3000000000000007,"ΤΕΜ",1,"EP",10,"LZS:PT170R6","LZS Μίνι Ρελέ"]
["LZS:PT2D5L24","Plug-in relay complete unit 2 W, 24 V DC LED module red Socket with logic isolation Spring-type terminal (push-in)",25.3,"ΤΕΜ",1,"EP",5,"LZS:PT2D5L24","LZS Μίνι Ρελέ"]
["LZS:PT2D5T30","Plug-in relay complete unit 2 W, 230 V AC LED module red Socket with logic isolation Spring-type terminal (push-in)",29.11,"ΤΕΜ",1,"EP",5,"LZS:PT2D5T30","LZS Μίνι Ρελέ"]
["LZS:PT3A5L24","Plug-in relay complete unit 3 W, 24 V DC LED module red Standard plug-in socket screw terminal 3.5 mm pinning",21.16,"ΤΕΜ",1,"EP",5,"LZS:PT3A5L24","LZS Μίνι Ρελέ"]
["LZS:PT3A5R24","Plug-in relay complete unit 3 W, 24 V AC LED module red Standard plug-in socket screw terminal 3.5 mm pinning",21.16,"ΤΕΜ",1,"EP",5,"LZS:PT3A5R24","LZS Μίνι Ρελέ"]
["LZS:PT3A5S15","Plug-in relay complete unit 3 W, 115 V AC LED module red Standard plug-in socket screw terminal 3.5 mm pinning",22.5,"ΤΕΜ",1,"EP",5,"LZS:PT3A5S15","LZS Μίνι Ρελέ"]
["LZS:PT3A5T30","Plug-in relay complete unit 3 W, 230 V AC LED module red Standard plug-in socket screw terminal 3.5 mm pinning",22.5,"ΤΕΜ",1,"EP",5,"LZS:PT3A5T30","LZS Μίνι Ρελέ"]
["LZS:PT5A5L24","Plug-in relay complete unit 4 W, 24 V DC LED module red Standard plug-in socket screw terminal 3.5 mm pinning",21.16,"ΤΕΜ",1,"EP",5,"LZS:PT5A5L24","LZS Μίνι Ρελέ"]
["LZS:PT5A5R24","Plug-in relay complete unit 4 W, 24 V AC LED module red Standard plug-in socket screw terminal 3.5 mm pinning",21.16,"ΤΕΜ",1,"EP",5,"LZS:PT5A5R24","LZS Μίνι Ρελέ"]
["LZS:PT5A5S15","Plug-in relay complete unit 4 W, 115 V AC LED module red Standard plug-in socket screw terminal 3.5 mm pinning",22.5,"ΤΕΜ",1,"EP",5,"LZS:PT5A5S15","LZS Μίνι Ρελέ"]
["LZS:PT5A5T30","Plug-in relay complete unit 4 W, 230 V AC LED module red Standard plug-in socket screw terminal 3.5 mm pinning",22.5,"ΤΕΜ",1,"EP",5,"LZS:PT5A5T30","LZS Μίνι Ρελέ"]
["LZS:PT5B5L24","Plug-in relay complete unit 4 W, 24 V DC LED module red Socket with logic isolation screw terminal 3.5 mm pinning",21.16,"ΤΕΜ",1,"EP",5,"LZS:PT5B5L24","LZS Μίνι Ρελέ"]
["LZS:PT5B5R24","Plug-in relay complete unit 4 W, 24 V AC LED module red Socket with logic isolation screw terminal 3.5 mm pinning",21.16,"ΤΕΜ",1,"EP",5,"LZS:PT5B5R24","LZS Μίνι Ρελέ"]
["LZS:PT5B5S15","Plug-in relay complete unit 4 W, 115 V AC LED module red Socket with logic isolation screw terminal 3.5 mm pinning",22.5,"ΤΕΜ",1,"EP",5,"LZS:PT5B5S15","LZS Μίνι Ρελέ"]
["LZS:PT5B5T30","Plug-in relay complete unit 4 W, 230 V AC LED module red Socket with logic isolation screw terminal 3.5 mm pinning",22.5,"ΤΕΜ",1,"EP",5,"LZS:PT5B5T30","LZS Μίνι Ρελέ"]
["LZS:PT5D5L24","Plug-in relay complete unit 4 W, 24 V DC LED module red Socket with logic isolation Spring-type terminal (push-in)",21.94,"ΤΕΜ",1,"EP",5,"LZS:PT5D5L24","LZS Μίνι Ρελέ"]
["LZS:PT5D5R24","Plug-in relay complete unit 4 W, 24 V AC LED module red Socket with logic isolation Spring-type terminal (push-in)",21.94,"ΤΕΜ",1,"EP",5,"LZS:PT5D5R24","LZS Μίνι Ρελέ"]
["LZS:PT5D5S15","Plug-in relay complete unit 4 W, 115 V AC LED module red Socket with logic isolation Spring-type terminal (push-in)",23.5,"ΤΕΜ",1,"EP",5,"LZS:PT5D5S15","LZS Μίνι Ρελέ"]
["LZS:PT5D5T30","Plug-in relay complete unit 4 W, 230 V AC LED module red Socket with logic isolation Spring-type terminal (push-in)",23.5,"ΤΕΜ",1,"EP",5,"LZS:PT5D5T30","LZS Μίνι Ρελέ"]
["LZS:PT78720","Plug-in socket for PT relay 2 change-over contacts screw terminal",5.93,"ΤΕΜ",1,"EP",1,"LZS:PT78720","LZS Μίνι Ρελέ"]
["LZS:PT78722","Plug-in socket for PT relay 2 change-over contacts with logic isolation screw terminal",5.93,"ΤΕΜ",1,"EP",1,"LZS:PT78722","LZS Μίνι Ρελέ"]
["LZS:PT7872P","Plug-in socket for PT relay 2 change-over contacts with logic isolation Spring-type terminal (push-in)",6.54,"ΤΕΜ",1,"EP",1,"LZS:PT7872P","LZS Μίνι Ρελέ"]
["LZS:PT78730","Plug-in socket for PT relay 3 changeover contacts screw terminal",5.93,"ΤΕΜ",1,"EP",1,"LZS:PT78730","LZS Μίνι Ρελέ"]
["LZS:PT78740","Plug-in socket for PT relay 4 changeover contacts screw terminal",5.93,"ΤΕΜ",1,"EP",1,"LZS:PT78740","LZS Μίνι Ρελέ"]
["LZS:PT78742","Plug-in socket for PT relay 4 changeover contacts with logic isolation screw terminal",5.93,"ΤΕΜ",1,"EP",1,"LZS:PT78742","LZS Μίνι Ρελέ"]
["LZS:PT7874P","Plug-in socket for PT relay 4 changeover contacts with logic isolation Spring-type terminal (push-in)",7.13,"ΤΕΜ",1,"EP",1,"LZS:PT7874P","LZS Μίνι Ρελέ"]
["LZS:PTMG0024","LED module, green, 24 V DC",4.1500000000000004,"ΤΕΜ",1,"EP",1,"LZS:PTMG0024","LZS Μίνι Ρελέ"]
["LZS:PTMG0524","LED module green without freewheeling diode 24 V AC/DC",4.1500000000000004,"ΤΕΜ",1,"EP",1,"LZS:PTMG0524","LZS Μίνι Ρελέ"]
["LZS:PTMG0730","LED module, green, 110-230 V AC",4.1500000000000004,"ΤΕΜ",1,"EP",1,"LZS:PTMG0730","LZS Μίνι Ρελέ"]
["LZS:PTML0024","LED module, red for plug-in relay, PT and RT series, for DC 24 V with freewheeling diode",3.93,"ΤΕΜ",1,"EP",1,"LZS:PTML0024","LZS Μίνι Ρελέ"]
["LZS:PTML0524","LED module, red for plug-in relay, PT and RT series, for 24 V AC/DC without freewheeling diode",3.93,"ΤΕΜ",1,"EP",1,"LZS:PTML0524","LZS Μίνι Ρελέ"]
["LZS:PTML0730","LED module, red for plug-in relay, PT and RT series, 110-230 V AC without freewheeling diode",3.93,"ΤΕΜ",1,"EP",1,"LZS:PTML0730","LZS Μίνι Ρελέ"]
["LZS:PTMT00A0","Freewheeling diode with connection to A1 6-230 V DC",2.65,"ΤΕΜ",1,"EP",1,"LZS:PTMT00A0","LZS Μίνι Ρελέ"]
["LZS:PTMU0524","RC element, 24-48 V AC",6.25,"ΤΕΜ",1,"EP",1,"LZS:PTMU0524","LZS Μίνι Ρελέ"]
["LZS:PTMU0730","RC element, 110-230 V AC",6.25,"ΤΕΜ",1,"EP",1,"LZS:PTMU0730","LZS Μίνι Ρελέ"]
["LZS:RT17016","Fixing/reject bracket for plug-in relay RT series",70.98,"ΤΕΜ",100,"EP",10,"LZS:RT17016","LZS Μίνι Ρελέ"]
["LZS:RT17040","Label 15 mm for RT and RY relay",25.75,"ΤΕΜ",100,"EP",10,"LZS:RT17040","LZS Μίνι Ρελέ"]
["LZS:RT170P1","fanning strip 2-pole for RT push-in terminal sockets",108.13,"ΤΕΜ",100,"EP",10,"LZS:RT170P1","LZS Μίνι Ρελέ"]
["LZS:RT170R8","Fanning strip 8-pole for RT screw-type terminal",7.7,"ΤΕΜ",1,"EP",10,"LZS:RT170R8","LZS Μίνι Ρελέ"]
["LZS:RT3A4L24","Plug-in relay complete unit 1 W, 24 V DC LED module red Standard plug-in socket screw terminal",21.5,"ΤΕΜ",1,"EP",5,"LZS:RT3A4L24","LZS Μίνι Ρελέ"]
["LZS:RT3A4R24","Plug-in relay complete unit 1 W, 24 V AC LED module red Standard plug-in socket screw terminal",21.5,"ΤΕΜ",1,"EP",5,"LZS:RT3A4R24","LZS Μίνι Ρελέ"]
["LZS:RT3A4S15","Plug-in relay complete unit 1 W, 115 V AC LED module red Standard plug-in socket screw terminal",24.85,"ΤΕΜ",1,"EP",5,"LZS:RT3A4S15","LZS Μίνι Ρελέ"]
["LZS:RT3A4T30","Plug-in relay complete unit 1 W, 230 V AC LED module red Standard plug-in socket screw terminal",24.85,"ΤΕΜ",1,"EP",5,"LZS:RT3A4T30","LZS Μίνι Ρελέ"]
["LZS:RT3B4L24","Plug-in relay complete unit 1 W, 24 V DC LED module red Socket with logic isolation screw terminal",21.5,"ΤΕΜ",1,"EP",5,"LZS:RT3B4L24","LZS Μίνι Ρελέ"]
["LZS:RT3B4R24","Plug-in relay complete unit 1 W, 24 V AC LED module red Socket with logic isolation screw terminal",21.5,"ΤΕΜ",1,"EP",5,"LZS:RT3B4R24","LZS Μίνι Ρελέ"]
["LZS:RT3B4S15","Plug-in relay complete unit 1 W, 115 V AC LED module red Socket with logic isolation screw terminal",24.85,"ΤΕΜ",1,"EP",5,"LZS:RT3B4S15","LZS Μίνι Ρελέ"]
["LZS:RT3B4T30","Plug-in relay complete unit 1 W, 230 V AC LED module red Socket with logic isolation screw terminal",24.85,"ΤΕΜ",1,"EP",5,"LZS:RT3B4T30","LZS Μίνι Ρελέ"]
["LZS:RT3D4L24","Plug-in relay complete unit 1 W, 24 V DC LED module red Socket with logic isolation Spring-type terminal (push-in)",22.62,"ΤΕΜ",1,"EP",5,"LZS:RT3D4L24","LZS Μίνι Ρελέ"]
["LZS:RT3D4R24","Plug-in relay complete unit 1 W, 24 V AC LED module red Socket with logic isolation Spring-type terminal (push-in)",22.62,"ΤΕΜ",1,"EP",5,"LZS:RT3D4R24","LZS Μίνι Ρελέ"]
["LZS:RT3D4S15","Plug-in relay complete unit 1 W, 115 V AC LED module red Socket with logic isolation Spring-type terminal (push-in)",25.98,"ΤΕΜ",1,"EP",5,"LZS:RT3D4S15","LZS Μίνι Ρελέ"]
["LZS:RT3D4T30","Plug-in relay complete unit 1 W, 230 V AC LED module red Socket with logic isolation Spring-type terminal (push-in)",25.98,"ΤΕΜ",1,"EP",5,"LZS:RT3D4T30","LZS Μίνι Ρελέ"]
["LZS:RT4A4L24","Plug-in relay complete unit 2 W, 24 V DC LED module red Standard plug-in socket screw terminal",22.62,"ΤΕΜ",1,"EP",5,"LZS:RT4A4L24","LZS Μίνι Ρελέ"]
["LZS:RT4A4R24","Plug-in relay complete unit 2 W, 24 V AC LED module red Standard plug-in socket screw terminal",22.62,"ΤΕΜ",1,"EP",5,"LZS:RT4A4R24","LZS Μίνι Ρελέ"]
["LZS:RT4A4S15","Plug-in relay complete unit 2 W, 115 V AC LED module red Standard plug-in socket screw terminal",25.75,"ΤΕΜ",1,"EP",5,"LZS:RT4A4S15","LZS Μίνι Ρελέ"]
["LZS:RT4A4T30","Plug-in relay complete unit 2 W, 230 V AC LED module red Standard plug-in socket screw terminal",25.75,"ΤΕΜ",1,"EP",5,"LZS:RT4A4T30","LZS Μίνι Ρελέ"]
["LZS:RT4B4L24","Plug-in relay complete unit 2 W, 24 V DC LED module red Socket with logic isolation screw terminal",22.62,"ΤΕΜ",1,"EP",5,"LZS:RT4B4L24","LZS Μίνι Ρελέ"]
["LZS:RT4B4R24","Plug-in relay complete unit 2 W, 24 V AC LED module red Socket with logic isolation screw terminal",22.62,"ΤΕΜ",1,"EP",5,"LZS:RT4B4R24","LZS Μίνι Ρελέ"]
["LZS:RT4B4S15","Plug-in relay complete unit 2 W, 115 V AC LED module red Socket with logic isolation screw terminal",25.75,"ΤΕΜ",1,"EP",5,"LZS:RT4B4S15","LZS Μίνι Ρελέ"]
["LZS:RT4B4T30","Plug-in relay complete unit 2 W, 230 V AC LED module red Socket with logic isolation screw terminal",25.75,"ΤΕΜ",1,"EP",5,"LZS:RT4B4T30","LZS Μίνι Ρελέ"]
["LZS:RT4D4L24","Plug-in relay complete unit 2 W, 24 V DC LED module red Socket with logic isolation Spring-type terminal (push-in)",23.62,"ΤΕΜ",1,"EP",5,"LZS:RT4D4L24","LZS Μίνι Ρελέ"]
["LZS:RT4D4R24","Plug-in relay complete unit 2 W, 24 V AC LED module red Socket with logic isolation Spring-type terminal (push-in)",23.62,"ΤΕΜ",1,"EP",5,"LZS:RT4D4R24","LZS Μίνι Ρελέ"]
["LZS:RT4D4S15","Plug-in relay complete unit 2 W, 115 V AC LED module red Socket with logic isolation Spring-type terminal (push-in)",26.98,"ΤΕΜ",1,"EP",5,"LZS:RT4D4S15","LZS Μίνι Ρελέ"]
["LZS:RT4D4T30","Plug-in relay complete unit 2 W, 230 V AC LED module red Socket with logic isolation Spring-type terminal (push-in)",26.98,"ΤΕΜ",1,"EP",5,"LZS:RT4D4T30","LZS Μίνι Ρελέ"]
["LZS:RT78725","Plug-in socket for RT relay Standard plug-in socket screw terminal",7.13,"ΤΕΜ",1,"EP",1,"LZS:RT78725","LZS Μίνι Ρελέ"]
["LZS:RT78726","Plug-in socket for RT relay Socket with logic isolation screw terminal",7.13,"ΤΕΜ",1,"EP",1,"LZS:RT78726","LZS Μίνι Ρελέ"]
["LZS:RT7872P","Plug-in socket for RT relay Socket with logic isolation Socket with logic isolation Spring-type terminal (push-in)",7.89,"ΤΕΜ",1,"EP",1,"LZS:RT7872P","LZS Μίνι Ρελέ"]
["LZX:PT270024","Plug-in relay, 2 change-over contacts 24 V DC, also for LZS sockets",8.3000000000000007,"ΤΕΜ",1,"EP",1,"LZX:PT270024","LZX Μίνι Ρελέ"]
["LZX:PT270524","Plug-in relay, 2 change-over contacts 24 V AC, also for LZS sockets",8.3000000000000007,"ΤΕΜ",1,"EP",1,"LZX:PT270524","LZX Μίνι Ρελέ"]
["LZX:PT270615","Plug-in relay, 2 change-over contacts 115 V AC, also for LZS sockets",9.6999999999999993,"ΤΕΜ",1,"EP",1,"LZX:PT270615","LZX Μίνι Ρελέ"]
["LZX:PT270730","Plug-in relay, 2 change-over contacts 230 V AC, also for LZS sockets",9.6999999999999993,"ΤΕΜ",1,"EP",1,"LZX:PT270730","LZX Μίνι Ρελέ"]
["LZX:PT370024","Plug-in relay, 3 changeover contacts 24 V DC, 10 A, Width 22.5 mm for LZS sockets",8.3000000000000007,"ΤΕΜ",1,"EP",1,"LZX:PT370024","LZX Μίνι Ρελέ"]
["LZX:PT370125","Plug-in relay, 3 changeover contacts 125 V DC, 10 A, Width 22.5 mm for LZS sockets",9.6999999999999993,"ΤΕΜ",1,"EP",1,"LZX:PT370125","LZX Μίνι Ρελέ"]
["LZX:PT370524","Plug-in relay, 3 changeover contacts 24 V AC, 10 A, Width 22.5 mm  for LZS sockets",8.3000000000000007,"ΤΕΜ",1,"EP",1,"LZX:PT370524","LZX Μίνι Ρελέ"]
["LZX:PT370615","Plug-in relay, 3 changeover contacts 115 V AC, 10 A, Width 22.5 mm  for LZS sockets",9.6999999999999993,"ΤΕΜ",1,"EP",1,"LZX:PT370615","LZX Μίνι Ρελέ"]
["LZX:PT370730","Plug-in relay, 3 changeover contacts 230 V AC, 10 A, Width 22.5 mm  for LZS sockets",9.6999999999999993,"ΤΕΜ",1,"EP",1,"LZX:PT370730","LZX Μίνι Ρελέ"]
["LZX:PT520024","Plug-in relay 4 changeover contacts, without test bracket 24 V DC,  for LZS sockets",8.3000000000000007,"ΤΕΜ",1,"EP",1,"LZX:PT520024","LZX Μίνι Ρελέ"]
["LZX:PT520730","Plug-in relay 4 changeover contacts, without test bracket 230 V AC,  for LZS sockets",9.6999999999999993,"ΤΕΜ",1,"EP",1,"LZX:PT520730","LZX Μίνι Ρελέ"]
["LZX:PT570024","Plug-in relay, 4 changeover contacts 24 V DC, 6 A, Width 22.5 mm  for LZS sockets",8.3000000000000007,"ΤΕΜ",1,"EP",1,"LZX:PT570024","LZX Μίνι Ρελέ"]
["LZX:PT570125","Plug-in relay, 4 changeover contacts 125 V DC, 6 A, Width 22.5 mm  for LZS sockets",9.6999999999999993,"ΤΕΜ",1,"EP",1,"LZX:PT570125","LZX Μίνι Ρελέ"]
["LZX:PT570524","Plug-in relay, 4 changeover contacts 24 V AC, 6 A, Width 22.5 mm  for LZS sockets",8.3000000000000007,"ΤΕΜ",1,"EP",1,"LZX:PT570524","LZX Μίνι Ρελέ"]
["LZX:PT570615","Plug-in relay, 4 changeover contacts 115 V AC, 6 A, Width 22.5 mm  for LZS sockets",9.6999999999999993,"ΤΕΜ",1,"EP",1,"LZX:PT570615","LZX Μίνι Ρελέ"]
["LZX:PT570730","Plug-in relay, 4 changeover contacts 230 V AC, 6 A, Width 22.5 mm  for LZS sockets",9.6999999999999993,"ΤΕΜ",1,"EP",1,"LZX:PT570730","LZX Μίνι Ρελέ"]
["LZX:PT580024","Plug-in relay 4 changeover contacts, hard gold-plated 24 V DC,  for LZS sockets",10.72,"ΤΕΜ",1,"EP",1,"LZX:PT580024","LZX Μίνι Ρελέ"]
["LZX:PT580730","Plug-in relay 4 changeover contacts, hard gold-plated 230 V AC,  for LZS sockets",13.88,"ΤΕΜ",1,"EP",1,"LZX:PT580730","LZX Μίνι Ρελέ"]
["LZX:RT314024","Plug-in relay 1 W, Width 15 mm, 24 V DC  for LZS sockets",5.58,"ΤΕΜ",1,"EP",1,"LZX:RT314024","LZX Μίνι Ρελέ"]
["LZX:RT314524","Plug-in relay, 1 change-over contact 24 V AC, 16 A, Width 15.5 mm  for LZS sockets",5.58,"ΤΕΜ",1,"EP",1,"LZX:RT314524","LZX Μίνι Ρελέ"]
["LZX:RT314615","Plug-in relay, 1 change-over contact 115 V AC, 16 A, Width 15.5 mm  for LZS sockets",9.4,"ΤΕΜ",1,"EP",1,"LZX:RT314615","LZX Μίνι Ρελέ"]
["LZX:RT314730","Plug-in relay 1 W, Width 15 mm, 230 V AC  for LZS sockets",9.4,"ΤΕΜ",1,"EP",1,"LZX:RT314730","LZX Μίνι Ρελέ"]
["LZX:RT315024","Plug-in relay 1 change-over contact, hard gold-plated 24 V DC,  for LZS sockets",6.54,"ΤΕΜ",1,"EP",1,"LZX:RT315024","LZX Μίνι Ρελέ"]
["LZX:RT315730","Plug-in relay 1 change-over contact, hard gold-plated 230 V AC,  for LZS sockets",9.9,"ΤΕΜ",1,"EP",1,"LZX:RT315730","LZX Μίνι Ρελέ"]
["LZX:RT424012","Plug-in relay 2 W, Width 15 mm, 12 V DC  for LZS sockets",6.65,"ΤΕΜ",1,"EP",1,"LZX:RT424012","LZX Μίνι Ρελέ"]
["LZX:RT424024","Plug-in relay 2 W, Width 15 mm, 24 V DC  for LZS sockets",6.65,"ΤΕΜ",1,"EP",1,"LZX:RT424024","LZX Μίνι Ρελέ"]
["LZX:RT424110","Plug-in relay 2 W, Width 15 mm, 125 V DC  for LZS sockets",10.57,"ΤΕΜ",1,"EP",1,"LZX:RT424110","LZX Μίνι Ρελέ"]
["LZX:RT424524","Plug-in relay, 2 change-over contacts 24 V AC, 8 A, Width 15.5 mm  for LZS sockets",6.65,"ΤΕΜ",1,"EP",1,"LZX:RT424524","LZX Μίνι Ρελέ"]
["LZX:RT424615","Plug-in relay, 2 change-over contacts 115 V AC, 16 A, Width 15.5 mm  for LZS sockets",10.57,"ΤΕΜ",1,"EP",1,"LZX:RT424615","LZX Μίνι Ρελέ"]
["LZX:RT424730","Plug-in relay 2 W, Width 15 mm, 230 V AC  for LZS sockets",10.57,"ΤΕΜ",1,"EP",1,"LZX:RT424730","LZX Μίνι Ρελέ"]
["M56340-A0001","NIPPLE CONNECTION G 1/2 MAX. 400 BAR, MAT. NO.2.0401.26",11,"ST",1,"PI2",1,"M56340A0001","Όργανα Μέτρησης Πεδίου"]
["M56340-A0002","NIPPLE CONNECTION G 1/2 MAX. 400 BAR, MAT.NO. 1.0715/ 1.0037",5,"ST",1,"PI2",1,"M56340A0002","Όργανα Μέτρησης Πεδίου"]
["M56340-A0003","NIPPLE CONNECTION G 1/2 MAX. 400 BAR, MAT. NO. 1.43305/ 1.4571",20,"ST",1,"PI2",1,"M56340A0003","Όργανα Μέτρησης Πεδίου"]
["M56340-A0004","CLAMPING SLEEVE G 1/2 MAX. 400 BAR, MAT.NO. 2.0402.26",3,"ST",1,"PI2",1,"M56340A0004","Όργανα Μέτρησης Πεδίου"]
["M56340-A0005","CLAMPING SLEEVE G 1/2 MAX. 400 BAR, MAT.NO. 1.0715",2,"ST",1,"PI2",1,"M56340A0005","Όργανα Μέτρησης Πεδίου"]
["M56340-A0006","COLLAR CEONNECTION PIECE G 1/2 MAX. 400 BAR, MAT.NO. 2.0401.26",19,"ST",1,"PI2",1,"M56340A0006","Όργανα Μέτρησης Πεδίου"]
["M56340-A0007","COLLAR CONNECTION PIECE G 1/2 MAX. 400 BAR, MAT.NO. 1.0715",21,"ST",1,"PI2",1,"M56340A0007","Όργανα Μέτρησης Πεδίου"]
["M56340-A0027","SINGLE SHUT-OFF VALVE TYPE A TO DIN 16270 MAX.OPERAT.PRESSURE 250BAR BRASS",20,"ST",1,"PI2",1,"M56340A0027","Όργανα Μέτρησης Πεδίου"]
["M56340-A0028","SINGLE SHUT-OFF VALVE TYPE A TO DIN 16270 MAX.OPERAT.PRESSURE 400BAR STEEL",22,"ST",1,"PI2",1,"M56340A0028","Όργανα Μέτρησης Πεδίου"]
["M56340-A0030","SINGLE SHUT-OFF VALVE TYPE A TO DIN 16271 W/ TEST PEG MAX.OP.RESS.250BAR BRASS",26,"ST",1,"PI2",1,"M56340A0030","Όργανα Μέτρησης Πεδίου"]
["M56340-A0031","SINGLE SHUT-OFF VALVE TYPE A TO DIN 16271 W/ TEST PEG MAX.OP.RESS.400BAR STEEL",27,"ST",1,"PI2",1,"M56340A0031","Όργανα Μέτρησης Πεδίου"]
["M56340-A0032","SINGLE SHUT-OFF VALVE TYPE A TO DIN 16271 W/ TEST PEG MAX.OP.RESS.400BAR STAINL. STEEL",69,"ST",1,"PI2",1,"M56340A0032","Όργανα Μέτρησης Πεδίου"]
["M56340-A0033","DOUBLE SHUT-OFF VALVE TYPE A TEST CONNECT.SIMIL.TO DIN 16272 W/ NARROW TEST FLANGE MAX.OPER. PRESS. 250BAR BRASS",43,"ST",1,"PI2",1,"M56340A0033","Όργανα Μέτρησης Πεδίου"]
["M56340-A0036","DOUBLE SHUT-OFF VALVE TYPE A TEST CONNECT.SIMIL.TO DIN 16272 W/ TEST PEG MAX.OPER. PRESS. 250BAR BRASS",37,"ST",1,"PI2",1,"M56340A0036","Όργανα Μέτρησης Πεδίου"]
["M56340-A0037","DOUBLE SHUT-OFF VALVE TYPE A TEST CONNECT.SIMIL.TO DIN 16272 W/ TEST PEG MAX.OPER. PRESS. 400BAR STEEL",41,"ST",1,"PI2",1,"M56340A0037","Όργανα Μέτρησης Πεδίου"]
["M56340-A0038","DOUBLE SHUT-OFF VALVE TYPE A TEST CONNECT.SIMIL.TO DIN 16272 W/ TEST PEG MAX.OPER. PRESS. 400BAR STAINLESS STEEL",98,"ST",1,"PI2",1,"M56340A0038","Όργανα Μέτρησης Πεδίου"]
["M56340-A0043","WATER TRAP B TO DIN 16282 120 CEL/100 BAR, 400 CEL/63 BAR MAT. NO. 1.0305",17,"ST",1,"PI2",1,"M56340A0043","Όργανα Μέτρησης Πεδίου"]
["M56340-A0045","WATER TRAP D TO DIN 16282 120 CEL/100 BAR, 400 CEL/63 BAR MAT. NO. 1.0305",17,"ST",1,"PI2",1,"M56340A0045","Όργανα Μέτρησης Πεδίου"]
["M56340-A0046","INSTRUMENT BRACKET, DESIGN H TO DIN 16281, MADE OF ALUMINUM ALLOY, PROJECTION LENGTH 60 MM",40,"ST",1,"PI2",1,"M56340A0046","Όργανα Μέτρησης Πεδίου"]
["M56340-A0047","INSTRUMENT BRACKET, DESIGN H TO DIN 16281, MADE OF ALUMINUM ALLOY, PROJECTION LENGTH 100 MM",14,"ST",1,"PI2",1,"M56340A0047","Όργανα Μέτρησης Πεδίου"]
["M56340-A0048","INSTRUMENT BRACKET, DESIGN H TO DIN 16281, MADE OF ALUMINUM ALLOY, PROJECTION LENGTH 160 MM",19,"ST",1,"PI2",1,"M56340A0048","Όργανα Μέτρησης Πεδίου"]
["M56340-A0053","INSTRUMENT BRACKET, DESIGN TO DIN 16281, MADE OF ANNEALED CAST IRON, PROJECTION LENGTH 100 MM",29,"ST",1,"PI2",1,"M56340A0053","Όργανα Μέτρησης Πεδίου"]
["M56340-A0054","PRESSURE IMPACT REDUCER BRASS",8,"ST",1,"PI2",1,"M56340A0054","Όργανα Μέτρησης Πεδίου"]
["M56340-A0059","PRESSURE IMPACT REDUCER STAINLESS STEEL",49,"ST",1,"PI2",1,"M56340A0059","Όργανα Μέτρησης Πεδίου"]
["M56340-A0061","WATER TRAP B TO DIN 16282 120 CEL/100 BAR, 400 CEL/63 BAR MAT. NO. 1.4571",36,"ST",1,"PI2",1,"M56340A0061","Όργανα Μέτρησης Πεδίου"]
["M56340-A0063","WATER TRAP D TO DIN 16282 120 CEL/100 BAR, 400 CEL/63 BAR MAT. NO. 1.4571",36,"ST",1,"PI2",1,"M56340A0063","Όργανα Μέτρησης Πεδίου"]
["M56340-A0079","INSTRUMENT BRACKET, DSIGN A TO DIN 16281, MADE OF ANNEALED CAST IRON, FOR MOUNTING ON A HORIZONTAL OR VERTICAL PIPE * INCLUSIVE S006.03.003",36,"ST",1,"PI2",1,"M56340A0079","Όργανα Μέτρησης Πεδίου"]
["PBD:00000158","Siemens Canada - BID_McGinnis Cement Approval Drawing 1",697,"ST",1,"PI1",1,"PBD:00000158","Όργανα Μέτρησης Πεδίου"]
["PBD:00000159","Siemens Canada - BID_McGinnis Cement Approval Drawing 1",697,"ST",1,"PI1",1,"PBD:00000159","Όργανα Μέτρησης Πεδίου"]
["PBD:00000160","Siemens Canada - BID_McGinnis Cement Approval Drawing 1",697,"ST",1,"PI1",1,"PBD:00000160","Όργανα Μέτρησης Πεδίου"]
["PBD:22475K2A","Kit,horn antenna, long, for SITRANS LR,stainless steel",439,"ST",1,"PI1",1,"PBD:22475K2A","Όργανα Μέτρησης Πεδίου"]
["PBD:22475K3A","Kit,horn antenna,short,LR400, PURG",514,"ST",1,"PI1",1,"PBD:22475K3A","Όργανα Μέτρησης Πεδίου"]
["PBD:22475K4A","KIT,horn ant,long,purge, GP approval only",550,"ST",1,"PI1",1,"PBD:22475K4A","Όργανα Μέτρησης Πεδίου"]
["PBD:23311020","WINDOW,DAMPER,E37,LUCITE",96,"ST",1,"PI1",1,"PBD:23311020","Όργανα Μέτρησης Πεδίου"]
["PBD:23900005","LOAD CELL, 50LB,COMP, 2mM/V,C462,CS",2238,"ST",1,"PI1",1,"PBD:23900005","Όργανα Μέτρησης Πεδίου"]
["PBD:23900010","LOAD CELL, 100LB,COMP, 2mM/V,C462,SS",1941,"ST",1,"PI1",1,"PBD:23900010","Όργανα Μέτρησης Πεδίου"]
["PBD:23900012","LOAD CELL, 250LB, COMP,2mM/V,C462,SS",1941,"ST",1,"PI1",1,"PBD:23900012","Όργανα Μέτρησης Πεδίου"]
["PBD:23900176","LOAD CELL,MLC/MILLFLO,2LB,SS,F LOAD CELL 2 LB FOR MILLFLO FLOWMETER",2413,"ST",1,"PI1",1,"PBD:23900176","Όργανα Μέτρησης Πεδίου"]
["PBD:23900177","LOAD CELL, 5 LB FOR MILLFLO FLOWMETER",2413,"ST",1,"PI1",1,"PBD:23900177","Όργανα Μέτρησης Πεδίου"]
["PBD:23900223","LOAD CELL 'Weighfeeder' 6KG, Stainless steel",1434,"ST",1,"PI1",1,"PBD:23900223","Όργανα Μέτρησης Πεδίου"]
["PBD:23900224","LOAD CELL 'Weighfeeder' 25LB, stainless steel",1883,"ST",1,"PI1",1,"PBD:23900224","Όργανα Μέτρησης Πεδίου"]
["PBD:23900225","LOAD CELL 'Weighfeeder' 50LB, stainless steel",1932,"ST",1,"PI1",1,"PBD:23900225","Όργανα Μέτρησης Πεδίου"]
["PBD:23900244","LOAD CELL 10 LB, FOR MLC BELT SCALE, MILLFLO FLOWMETER",2413,"ST",1,"PI1",1,"PBD:23900244","Όργανα Μέτρησης Πεδίου"]
["PBD:23900245","LOAD CELL 20 LB FOR MLC BELT SCALE",2413,"ST",1,"PI1",1,"PBD:23900245","Όργανα Μέτρησης Πεδίου"]
["PBD:23900246","LOAD CELL, 50 LB, STAINLESS STEEL, FOR MSI BELT SCALE, MILLFLO FLOWMETER",1904,"ST",1,"PI1",1,"PBD:23900246","Όργανα Μέτρησης Πεδίου"]
["PBD:23900247","LOAD CELL, 100 LB, STAINLESS STEEL, FOR MSI BELT SCALE, MILLFLO FLOWMETER",1904,"ST",1,"PI1",1,"PBD:23900247","Όργανα Μέτρησης Πεδίου"]
["PBD:23900248","LOAD CELL,MSI,250LB,SS,F",1904,"ST",1,"PI1",1,"PBD:23900248","Όργανα Μέτρησης Πεδίου"]
["PBD:23900249","LOAD CELL, 500 LB, STAINLESS STEEL, FOR MSI BELT SCALE",1904,"ST",1,"PI1",1,"PBD:23900249","Όργανα Μέτρησης Πεδίου"]
["PBD:23900250","LOAD CELL, 750 LB, STAINLESS STEEL, FOR MSI BELT SCALE",1904,"ST",1,"PI1",1,"PBD:23900250","Όργανα Μέτρησης Πεδίου"]
["PBD:23900251","LOAD CELL, 1000 LB, STAINLESS STEEL, FOR MSI BELT SCALE",1904,"ST",1,"PI1",1,"PBD:23900251","Όργανα Μέτρησης Πεδίου"]
["PBD:23900261","LOAD CELL,NTEP,OIML, 100LB,SS",3165,"ST",1,"PI1",1,"PBD:23900261","Όργανα Μέτρησης Πεδίου"]
["PBD:23900262","LOAD CELL,NTEP,OIML, 250LB,SS",3165,"ST",1,"PI1",1,"PBD:23900262","Όργανα Μέτρησης Πεδίου"]
["PBD:23900263","LOAD CELL,NTEP,OIML,  500LB,SS",3165,"ST",1,"PI1",1,"PBD:23900263","Όργανα Μέτρησης Πεδίου"]
["PBD:23900264","LOAD CELL,NTEP,OIML,  750LB,SS",3165,"ST",1,"PI1",1,"PBD:23900264","Όργανα Μέτρησης Πεδίου"]
["PBD:23900265","LOAD CELL,NTEP,OIML,1000LB,SS",3074,"ST",1,"PI1",1,"PBD:23900265","Όργανα Μέτρησης Πεδίου"]
["PBD:23900268","LOAD CELL, 500 LB,G4-CD500-S, HI-TEMP",2155,"ST",1,"PI1",1,"PBD:23900268","Όργανα Μέτρησης Πεδίου"]
["PBD:24250393","J-BOX CAUTION TAG,LOCKOUT",2,"ST",1,"PI1",1,"PBD:24250393","Όργανα Μέτρησης Πεδίου"]
["PBD:25500K02A","KIT,SPARE,RADAR,ANTENNA HORN, 80mm,316SS",687,"ST",1,"PI1",1,"PBD:25500K02A","Όργανα Μέτρησης Πεδίου"]
["PBD:25500K03A","KIT,SPARE,RADAR,ANTENNA HORN, 100mm,316SS",687,"ST",1,"PI1",1,"PBD:25500K03A","Όργανα Μέτρησης Πεδίου"]
["PBD:25500K05A","KIT,SPARE,RADAR,antenna horn, 150mm,316SS",687,"ST",1,"PI1",1,"PBD:25500K05A","Όργανα Μέτρησης Πεδίου"]
["PBD:25501K0100A","100MM (4\") horn antenna extension kit",498,"ST",1,"PI1",1,"PBD:25501K0100A","Όργανα Μέτρησης Πεδίου"]
["PBD:25501K0150A","150 mm (6\") horn antenna extension kit",512,"ST",1,"PI1",1,"PBD:25501K0150A","Όργανα Μέτρησης Πεδίου"]
["PBD:25501K0200A","200 mm (8\") horn antenna extension kit",525,"ST",1,"PI1",1,"PBD:25501K0200A","Όργανα Μέτρησης Πεδίου"]
["PBD:25501K0500A","7ML14100AA00-Z,Y01=0500MM",672,"ST",1,"PI1",1,"PBD:25501K0500A","Όργανα Μέτρησης Πεδίου"]
["PBD:25501K1000A","1000 mm (40\") horn antenna extension kit",878,"ST",1,"PI1",1,"PBD:25501K1000A","Όργανα Μέτρησης Πεδίου"]
["PBD:45000673","TAG, PAPER WITH HOLE, 100 X 50MM,MULTIPLE TEXT LINES",49,"ST",1,"PI3",1,"PBD:45000673","Όργανα Μέτρησης Πεδίου"]
["PBD:51002K0100AAA","KIT,IQ,ROD,SHLD,2\"NPT,100mm, 316,PTFE,FKM",1028,"ST",1,"PI1",1,"PBD:51002K0100AAA","Όργανα Μέτρησης Πεδίου"]
["PBD:51002K0100BAA","KIT,IQ,ROD,SHLD,2\"BSP,100mm, 316,PTFE,FKM",1028,"ST",1,"PI1",1,"PBD:51002K0100BAA","Όργανα Μέτρησης Πεδίου"]
["PBD:51002K0100CAA","KIT,IQ,ROD,SHLD,2\"G,100mm,316, PTFE,FKM",1173,"ST",1,"PI1",1,"PBD:51002K0100CAA","Όργανα Μέτρησης Πεδίου"]
["PBD:51002K0150CAA","KIT,LR,Rod,Shield,2G,150mm, 316,PTFE,VITON. PTFE rod antenna shielded kit, 2\"G 316 Stainless Steel Process Connection, FKM O-ring, 150 mm 316 Stainless Steel  shield",1105,"ST",1,"PI1",1,"PBD:51002K0150CAA","Όργανα Μέτρησης Πεδίου"]
["PBD:51002K0200CAA","KIT,LR,Rod,Shield,2G,200mm, 316,PTFE,VITON. PTFE rod antenna shielded kit, 2\"G 316 Stainless Steel Process Connection, FKM O-ring, 200 mm 316 Stainless Steel  shield",1547,"ST",1,"PI1",1,"PBD:51002K0200CAA","Όργανα Μέτρησης Πεδίου"]
["PBD:51002K0250CAA","KIT,LR,Rod,Shield,2G,250mm, 316,PTFE,VITON. PTFE rod antenna shielded kit, 2\"G 316 Stainless Steel Process Connection, FKM O-ring, 250 mm 316 Stainless Steel  shield",1849,"ST",1,"PI1",1,"PBD:51002K0250CAA","Όργανα Μέτρησης Πεδίου"]
["PBD:51002K0350CAA","KIT,LR,Rod,Shield,2G,350mm, 316,PTFE,VITON. PTFE rod antenna shielded kit, 2\"G 316 Stainless Steel Process Connection, FKM O-ring, 350 mm 316 Stainless Steel  shield",2299,"ST",1,"PI1",1,"PBD:51002K0350CAA","Όργανα Μέτρησης Πεδίου"]
["PBD:51003K020AAAA","KIT,IQ,ROD/GSKT,22452 2\"/150, 316,PTFE",880,"ST",1,"PI1",1,"PBD:51003K020AAAA","Όργανα Μέτρησης Πεδίου"]
["PBD:51003K050AJAA","KIT, Assembly flange PTFE rod with gasket,DIN50 PN16,316L",880,"ST",1,"PI1",1,"PBD:51003K050AJAA","Όργανα Μέτρησης Πεδίου"]
["PBD:51003K050AOAA","KIT,ROD/GSKT,22452 JIS10K50A, 316,PTFE",1173,"ST",1,"PI1",1,"PBD:51003K050AOAA","Όργανα Μέτρησης Πεδίου"]
["PBD:51004K2AAA","KIT,IQ,ROD,1.5\"NPT,PTFE,316, FKM",1269,"ST",1,"PI1",1,"PBD:51004K2AAA","Όργανα Μέτρησης Πεδίου"]
["PBD:51004K3AAA","KIT,RADAR ROD,2\"NPT,PTFE,316, FKM",1269,"ST",1,"PI1",1,"PBD:51004K3AAA","Όργανα Μέτρησης Πεδίου"]
["PBD:51005K1AAA","IQ,ROD, PROCESS CONNECTION THREAD SERIES: 2\"NPT, ANTENNA MATERIAL: PTFE, WETTED METALLIC MATERIAL: 316 STAINLESS STEEL, O-RING MATERIAL: FKM",979,"ST",1,"PI1",1,"PBD:51005K1AAA","Όργανα Μέτρησης Πεδίου"]
["PBD:51005K2AAA","IQ,ROD,PROCESS CONNECTION THREAD SERIES: 2\"BSP, ANTENNA MATERIAL: PTFE, WETTED METALLIC MATERIAL: 316 STAINLESS STEEL, O-RING MATERIAL: FKM",979,"ST",1,"PI1",1,"PBD:51005K2AAA","Όργανα Μέτρησης Πεδίου"]
["PBD:51005K3AAA","KIT,RADAR ROD,2\"G,PTFE,316, FKM",979,"ST",1,"PI1",1,"PBD:51005K3AAA","Όργανα Μέτρησης Πεδίου"]
["PBD:51006K020AAAA","KIT,IQ HN 3\",22452 2/150 316, PTFE,FKM,NP",1368,"ST",1,"PI1",1,"PBD:51006K020AAAA","Όργανα Μέτρησης Πεδίου"]
["PBD:51006K020AABA","KIT,IQ HN 4\",22452 2/150 316, PTFE,FKM,No,Pressure",1368,"ST",1,"PI1",1,"PBD:51006K020AABA","Όργανα Μέτρησης Πεδίου"]
["PBD:51006K020AACA","KIT,IQ HN 6\",22452 2/150 316, PTFE,FKM,No Pressure",1368,"ST",1,"PI1",1,"PBD:51006K020AACA","Όργανα Μέτρησης Πεδίου"]
["PBD:51006K020AADA","KIT,IQ HN 8\",22452 2/150 316, PTFE,FKM,No Pressure",1368,"ST",1,"PI1",1,"PBD:51006K020AADA","Όργανα Μέτρησης Πεδίου"]
["PBD:51006K050AJAA","Kit for IQ Radar with Horn 80MM,22452,50/16,316,PTFE,NP",1368,"ST",1,"PI1",1,"PBD:51006K050AJAA","Όργανα Μέτρησης Πεδίου"]
["PBD:51006K050AJBA","KIT,IQ HORN 4\",22452,50/16, 316,PTFE,FKM,NP",1368,"ST",1,"PI1",1,"PBD:51006K050AJBA","Όργανα Μέτρησης Πεδίου"]
["PBD:51006K050AJCA","KIT,IQ HORN 4\",22452,50/16, 316,PTFE,FKM,No Pressure",1368,"ST",1,"PI1",1,"PBD:51006K050AJCA","Όργανα Μέτρησης Πεδίου"]
["PBD:51006K050AJDA","KIT,IQ HORN 8\",22452, 50/16,316, PTFE,FKM,NP",1368,"ST",1,"PI1",1,"PBD:51006K050AJDA","Όργανα Μέτρησης Πεδίου"]
["PBD:51010K1AA","KIT,IQ Rod SAN 3A,2\",PTFE,PR",3222,"ST",1,"PI1",1,"PBD:51010K1AA","Όργανα Μέτρησης Πεδίου"]
["PBD:51010K1AB","KIT,IQ Rod SAN 3A 2\" SANITARY CLAMP UHMW-PE,PR",1896,"ST",1,"PI1",1,"PBD:51010K1AB","Όργανα Μέτρησης Πεδίου"]
["PBD:51010K3AA","KIT,IQ Rod SAN 3A 4\" SANITARY CLAMP PTFE,PR",3983,"ST",1,"PI1",1,"PBD:51010K3AA","Όργανα Μέτρησης Πεδίου"]
["PBD:51010K3AB","KIT,IQ Rod SAN 3A 4\"SANITARY CLAMP UHMW-PE,PR",2655,"ST",1,"PI1",1,"PBD:51010K3AB","Όργανα Μέτρησης Πεδίου"]
["PBD:51014K0100AAA","KIT,IQ,ROD,SHLD,3/150,100MM, 316,PTFE,FKM",1173,"ST",1,"PI1",1,"PBD:51014K0100AAA","Όργανα Μέτρησης Πεδίου"]
["PBD:51014K0100EJA","KIT,LR,FLNG SHLD ROD,80PN16, 100MM,SS,T,V",1225,"ST",1,"PI1",1,"PBD:51014K0100EJA","Όργανα Μέτρησης Πεδίου"]
["PBD:51014K0150AAA","KIT,LR,FLNG SHLD ROD,3/150, 150MM,SS,T,V",1417,"ST",1,"PI1",1,"PBD:51014K0150AAA","Όργανα Μέτρησης Πεδίου"]
["PBD:51014K0150EJA","KIT,LR,FLNG SHLD ROD,80PN16, 150MM,SS,T,V",1463,"ST",1,"PI1",1,"PBD:51014K0150EJA","Όργανα Μέτρησης Πεδίου"]
["PBD:51014K0200AAA","PTFE shielded rod antenna kit, flanged, 3\" ASME 150 lb 316L SS flange, 200 mm 316L SS shield.",1463,"ST",1,"PI1",1,"PBD:51014K0200AAA","Όργανα Μέτρησης Πεδίου"]
["PBD:51014K0200EJA","PTFE shielded rod antenna kit, flanged, DN 80 PN 16 316L SS flange, 200 mm 316L SS shield.",1517,"ST",1,"PI1",1,"PBD:51014K0200EJA","Όργανα Μέτρησης Πεδίου"]
["PBD:51014K0250AAA","KIT,LR,FLNG SHLD ROD,80PN16, 250MM,SS,T,V",1563,"ST",1,"PI1",1,"PBD:51014K0250AAA","Όργανα Μέτρησης Πεδίου"]
["PBD:51014K0250EJA","KIT,LR,FLNG SHLD ROD, DN80PN16, 250MM,SS,T,V",1615,"ST",1,"PI1",1,"PBD:51014K0250EJA","Όργανα Μέτρησης Πεδίου"]
["PBD:51014K0450EJA","Kit, Flanged shielded rod, DN80 PN16, 450 MM, PTFE",1598,"ST",1,"PI1",1,"PBD:51014K0450EJA","Όργανα Μέτρησης Πεδίου"]
["PBD:51035410","KIT,display,SITRANS LR 400, B&B",332,"ST",1,"PI1",1,"PBD:51035410","Όργανα Μέτρησης Πεδίου"]
["PBD:51035813","Kit,universal flange 3\"/80mm, no pressure",280,"ST",1,"PI1",1,"PBD:51035813","Όργανα Μέτρησης Πεδίου"]
["PBD:51035814","Kit,universal flange 4\"/100mm,no pressure",363,"ST",1,"PI1",1,"PBD:51035814","Όργανα Μέτρησης Πεδίου"]
["PBD:51035815","Kit,universal flange 6\"/150mm, no pressure",571,"ST",1,"PI1",1,"PBD:51035815","Όργανα Μέτρησης Πεδίου"]
["PBD:51035816","Kit,universal flange 8\"/200mm, no pressure",951,"ST",1,"PI1",1,"PBD:51035816","Όργανα Μέτρησης Πεδίου"]
["PBD:51036252","7ML56715GA001XA0, SOLAR 1064829-1, 508MM SITRANS LC 300, Stilling Well Version with Flanged Process Connection: An inverse frequency shift capacitance transmitter for continuous level measuring in liquids and solids applications.",3074,"ST",1,"PI6",1,"PBD:51036252","Όργανα Μέτρησης Πεδίου"]
["PBD:51036253","7ML56715GA001XA0, SOLAR 1064829-2, 578MM SITRANS LC 300, Stilling Well Version with Flanged Process Connection: An inverse frequency shift capacitance transmitter for continuous level measuring in liquids and solids applications.",3085,"ST",1,"PI6",1,"PBD:51036253","Όργανα Μέτρησης Πεδίου"]
["PBD:51036254","7ML56715GA001XA0, SOLAR 1064829-3, 482MM SITRANS LC 300, Stilling Well Version with Flanged Process Connection: An inverse frequency shift capacitance transmitter for continuous level measuring in liquids and solids applications.",3059,"ST",1,"PI6",1,"PBD:51036254","Όργανα Μέτρησης Πεδίου"]
["PBD:51036255","7ML56715KA001XA0, SOLAR 1064829-4, 482MM SITRANS LC 300, Stilling Well Version with Flanged Process Connection: An inverse frequency shift capacitance transmitter for continuous level measuring in liquids and solids applications.",2993,"ST",1,"PI6",1,"PBD:51036255","Όργανα Μέτρησης Πεδίου"]
["PBD:51040483","CERTIFICATE C11",326,"ST",1,"PI6",1,"PBD:51040483","Όργανα Μέτρησης Πεδίου"]
["PBD:51040484","CERTIFICATE TEST",234,"ST",1,"PI3",1,"PBD:51040484","Όργανα Μέτρησης Πεδίου"]
["PBD:51041448","Sitrans LG Mounting eye M12x20",61,"ST",1,"PI1",1,"PBD:51041448","Όργανα Μέτρησης Πεδίου"]
["PBD:51041449","Sitrans LG Mounting spring",95,"ST",1,"PI1",1,"PBD:51041449","Όργανα Μέτρησης Πεδίου"]
["PBD:51110KC2","KIT,horn antenna,2\"/50,solid",374,"ST",1,"PI1",1,"PBD:51110KC2","Όργανα Μέτρησης Πεδίου"]
["PBD:51110KC3","KIT,horn antenna,3\"/80,solid",421,"ST",1,"PI1",1,"PBD:51110KC3","Όργανα Μέτρησης Πεδίου"]
["PBD:51110KC4","KIT,horn antenna,4\"/100,solid",514,"ST",1,"PI1",1,"PBD:51110KC4","Όργανα Μέτρησης Πεδίου"]
["PBD:54000141","RING,MCH.ILE37CA DIAP 10C881-2A",82,"ST",1,"PI1",1,"PBD:54000141","Όργανα Μέτρησης Πεδίου"]
["PBD:61009731","Load cell asembly,tension, 100lb (45.4 kg)",2352,"ST",1,"PI1",1,"PBD:61009731","Όργανα Μέτρησης Πεδίου"]
["PBD:61009732","Load cell assembly, tension, 250 lb (113.4 kg)",2352,"ST",1,"PI1",1,"PBD:61009732","Όργανα Μέτρησης Πεδίου"]
["PBD:61009733","Load cell assembly, tension, 500 lb (226.8 kg)",2352,"ST",1,"PI1",1,"PBD:61009733","Όργανα Μέτρησης Πεδίου"]
["PBD:61009734","Load cell asembly, tension, 1000 lb (453.6 kg) ,GR1",2352,"ST",1,"PI1",1,"PBD:61009734","Όργανα Μέτρησης Πεδίου"]
["PBD:61009735","Load cell assembly, tension, 50lb (22.7 kg)",2352,"ST",1,"PI1",1,"PBD:61009735","Όργανα Μέτρησης Πεδίου"]
["PBD:61010081","Kit,2 IDLER CABLE SUSPENSION",230,"ST",1,"PI1",1,"PBD:61010081","Όργανα Μέτρησης Πεδίου"]
["PBD:61010082","KIT,2 IDLER CABLE SUSPN.HEAVY DUTY",291,"ST",1,"PI1",1,"PBD:61010082","Όργανα Μέτρησης Πεδίου"]
["PBD:61010741","Kit,4 idler cable suspension standard",579,"ST",1,"PI1",1,"PBD:61010741","Όργανα Μέτρησης Πεδίου"]
["PBD:61010742","Kit,4 Idler cable suspension heavy duty",657,"ST",1,"PI1",1,"PBD:61010742","Όργανα Μέτρησης Πεδίου"]
["PBD:61010743","Kit,4 idler cable suspension magnum",741,"ST",1,"PI1",1,"PBD:61010743","Όργανα Μέτρησης Πεδίου"]
["PMF:ZERTIFIKATE","Zertificate SITRANS P",97,"ST",1,"PI2",1,"PMF:ZERTIFIKATE","Όργανα Μέτρησης Πεδίου"]
["S79220-B8655-P","SIMATIC WINCC V7.5 Data carrier without license, Use only in connection with valid license",35.9,"ΤΕΜ",1,"SIMATIC",1,"S79220B8655P","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["S79220-B9194-P","SIMATIC WINCC V7.5 SP1 Data carrier without license, Use only in connection with valid license",35.9,"ΤΕΜ",1,"SIMATIC",1,"S79220B9194P","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["S79220-C2163-F888","SIMATIC STEP 7 Professional V18 engineering software,Trial365 license software and documentation on DVD class A license key on USB flash drive 9 languages: de,en,zh included, fr,es,it,ru,ja,ko as download; executable on Windows 10; Windows 11; Windows Server 2016/2019/2022; for configuration of SIMATIC S7-1200/1500 SIMATIC S7-300/400/WinAC SIMATIC Basic Panels - - content: set (4x DVD + 1x USB)",2594,"ΤΕΜ",1,"SIMATIC",1,"S79220C2163F888","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["UAC:FN3440110118E2FAJRX","G120 LINE HARMONICS FILTER 400V 110 kW 50 Hz",10486,"ST",1,"GMC",1,"UAC:FN3440110118E2FAJRX","Ρυθμιστές στροφών και συστήματα Motion control"]
["UAC:FN344011113E2FAJRX","Schaffner Line harmonics filter 400V 11 kW 50 Hz",2822,"ST",1,"GMC",1,"UAC:FN344011113E2FAJRX","Ρυθμιστές στροφών και συστήματα Motion control"]
["UAC:FN3440132118E2FAJXX","G120 LINE HARMONICS FILTER 400V 132 kW 50 Hz",11236,"ST",1,"GMC",1,"UAC:FN3440132118E2FAJXX","Ρυθμιστές στροφών και συστήματα Motion control"]
["UAC:FN344015113E2FAJRX","G120 LINE HARMONICS FILTER 400V 15 kW",3378,"ST",1,"GMC",1,"UAC:FN344015113E2FAJRX","Ρυθμιστές στροφών και συστήματα Motion control"]
["UAC:FN3440160118E2FAJXX","G120 LINE HARMONICS FILTER 400V 160 kW 50 Hz",12297,"ST",1,"GMC",1,"UAC:FN3440160118E2FAJXX","Ρυθμιστές στροφών και συστήματα Motion control"]
["UAC:FN344019113E2FAJRX","G120 LINE HARMONICS FILTER 400V 18.5 kW",3378,"ST",1,"GMC",1,"UAC:FN344019113E2FAJRX","Ρυθμιστές στροφών και συστήματα Motion control"]
["UAC:FN3440200118E2FAJXX","G120 LINE HARMONICS FILTER 400V 200 kW 50 Hz",14655,"ST",1,"GMC",1,"UAC:FN3440200118E2FAJXX","Ρυθμιστές στροφών και συστήματα Motion control"]
["UAC:FN344022115E2FAJRX","G120 LINE HARMONICS FILTER 400V 22 kW 50 Hz",3900,"ST",1,"GMC",1,"UAC:FN344022115E2FAJRX","Ρυθμιστές στροφών και συστήματα Motion control"]
["UAC:FN344030115E2FAJRX","G120 LINE HARMONICS FILTER 400V 30 kW 50 Hz",4464,"ST",1,"GMC",1,"UAC:FN344030115E2FAJRX","Ρυθμιστές στροφών και συστήματα Motion control"]
["UAC:FN344037115E2FAJRX","G120 LINE HARMONICS FILTER 400V 37 kW 50 Hz",5231,"ST",1,"GMC",1,"UAC:FN344037115E2FAJRX","Ρυθμιστές στροφών και συστήματα Motion control"]
["UAC:FN344045115E2FAJRX","G120 LINE HARMONICS FILTER 400V 45 kW 50 Hz",5963,"ST",1,"GMC",1,"UAC:FN344045115E2FAJRX","Ρυθμιστές στροφών και συστήματα Motion control"]
["UAC:FN344055115E2FAJRX","G120 LINE HARMONICS FILTER 400V 55 kW 50 Hz",6907,"ST",1,"GMC",1,"UAC:FN344055115E2FAJRX","Ρυθμιστές στροφών και συστήματα Motion control"]
["UAC:FN34406112E2XXJRX","Schaffner Line harmonics filter 400V 5.5 kW 50 Hz",2081,"ST",1,"GMC",1,"UAC:FN34406112E2XXJRX","Ρυθμιστές στροφών και συστήματα Motion control"]
["UAC:FN344075116E2FAJRX","G120 LINE HARMONICS FILTER 400V 75 kW 50 Hz",8515,"ST",1,"GMC",1,"UAC:FN344075116E2FAJRX","Ρυθμιστές στροφών και συστήματα Motion control"]
["UAC:FN34408112E2XXJRX","Schaffner Line harmonics filter 400V 7.5 KW 50 Hz",2359,"ST",1,"GMC",1,"UAC:FN34408112E2XXJRX","Ρυθμιστές στροφών και συστήματα Motion control"]
["UAC:FN344090116E2FAJRX","G120 LINE HARMONICS FILTER 400V 90 kW 50 Hz",9585,"ST",1,"GMC",1,"UAC:FN344090116E2FAJRX","Ρυθμιστές στροφών και συστήματα Motion control"]
["W73078-B1001-A703","3-pin terminal for relay (6DR2804-8A/8B) MODULES",58,"ST",2,"PI1",2,"W73078B1001A703","Όργανα Μέτρησης Πεδίου"]
["W73078-B1001-A705","5-pin terminal for option modules 6DR2801-8A,B,C and 6DR2802-8A MODULES",60,"ST",2,"PI1",2,"W73078B1001A705","Όργανα Μέτρησης Πεδίου"]
["W73078-B1001-A706","6-pin terminal for option module 6DR2804-8A/8B MODULES",62,"ST",2,"PI1",2,"W73078B1001A706","Όργανα Μέτρησης Πεδίου"]
["W73078-B1001-A710","10-pin terminal (main board) for SIPART DR22/24",77,"ST",1,"PI1",1,"W73078B1001A710","Όργανα Μέτρησης Πεδίου"]
["W73078-B1001-A714","14-pin terminal (main board) for SIPART DR22/24",85,"ST",2,"PI1",2,"W73078B1001A714","Όργανα Μέτρησης Πεδίου"]
["W73078-B1001-A904","4-pin terminal for module I/U, R, P (6DR2800-8J / -8R / -8P) MODULES",63,"ST",2,"PI1",2,"W73078B1001A904","Όργανα Μέτρησης Πεδίου"]
["W73078-B1001-A906","6-pin terminal for option modules for 6DR2801-8D and 6DR2800-8A MODULES",62,"ST",2,"PI1",2,"W73078B1001A906","Όργανα Μέτρησης Πεδίου"]
["W73078-B1003-A904","4-pin terminal (6DR2800-8V) for SIPART DR19/21 and SITRANS T",9,"ST",1,"PI1",1,"W73078B1003A904","Όργανα Μέτρησης Πεδίου"]
["W73078-B1017-A908","8-pin terminal for SIPART DR19/21",16,"ST",1,"PI1",1,"W73078B1017A908","Όργανα Μέτρησης Πεδίου"]
["W73078-B1018-A903","3-pin terminal for SIPART DR19/21",5,"ST",1,"PI1",1,"W73078B1018A903","Όργανα Μέτρησης Πεδίου"]
["W73078-B3001-A705","5POL. TERMINAL FOR MODULE",14,"ST",2,"PI1",2,"W73078B3001A705","Όργανα Μέτρησης Πεδίου"]
["W79084-E1001-B2","lithium battery SIMATIC HMI and C7, scope of supply: 1 lithium battery, with 235 mm connection cable",38.1,"ΤΕΜ",1,"SIMATIC",1,"W79084E1001B2","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["ZNX:EIP200PRO","SIMATIC DP, Ethernet/IP head assembly for ET 200 PRO, max. 12 I/O modules incl. motor starter no F modules integrated 2-port switch incl. configuration tool (DVD)",562,"ΤΕΜ",1,"SIMATIC",1,"ZNX:EIP200PRO","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]
["ZNX:EIP200PROCM1","SIMATIC DP, Connection module for Ethernet/IP head assembly ET 200 PRO; M12/7/8\", 2x M12 and 2x 7/8\"",96.399999999999991,"ΤΕΜ",1,"SIMATIC",1,"ZNX:EIP200PROCM1","Βιομηχανικός αυτομ. SIMATIC, Υλικά Δικτύου, Τροφοδοτικά SITOP"]

{"sheet":"Sheet1","index":1,"n_rows":13,"n_cols":2,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["PA","PMD Data available"]
[""]
["VF","Sales Release"]
[""]
["LF","Delivery Release"]
[""]
["AE","Phase Out Announce"]
[""]
["TS","Prod. Cancellation"]
[""]
["MH","Prod. Discont."]
[""]
["AK","End Prod.Lifecycl."]