{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Price List January 2024","Sheet2","Sheet1"],"not_rendered":{"charts":0,"images":5,"macros":1,"external_links":0,"defined_names":3,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Price List January 2024","index":0,"n_rows":111138,"n_cols":9,"rows_kept":4500,"cut":true,"hidden":false,"merged":[[0,1,0,2],[1,0,1,6],[2,2,2,6],[2,0,2,1],[0,3,0,8]],"bounds":{"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0}}
[null,"Siemens Digital Industries\nΤιμοκατάλογος Προϊόντων Βιομηχανίας 2024",null,"Ισχύει από την 01.01.2024 και καταργεί κάθε προηγούμενο. Οι τιμές και τα τεχνικά χαρακτηριστικά των υλικών υπόκεινται σε οποιαδήποτε αλλαγή χωρίς προηγούμενη ειδοποίηση και δεν περιλαμβάνουν ΦΠΑ. "]
["Περιλαμβάνει τις παρακάτω κατηγορίες υλικών:"]
["Βιομηχανικός αυτοματισμός SIMATIC (SIMATIC)\nΒιομηχανικός αυτοματισμός SIMATIC S7-1200 (S7-1200)\nLOGO!, τροφοδοτικά LOGO! Power (LOGO!)\n\n",null,"Βιομηχανικό / Ηλεκτρολογικό Υλικό Χαμηλής Τάσης (EP) \nΡυθμιστές στροφών και συστήματα Motion control (GMC) \nΌργανα Μέτρησης Πεδίου (PI1…PI7)"]
["Αναζήτηση υλικού","Αναζήτηση με:"]
["Κωδικός","Περιγραφή","Τιμή καταλόγου \n(€)","Μον. \nΜέτρησης","Ποσ. μονάδας μέτρησης","Κατηγορία \nυλικού","Ελάχιστη ποσότητα παραγγελίας",null,"Γρήγορη επιλογή κατηγορίας"]
["1FK2102-0AG00-0MA0","SIMOTICS S-1FK2 HD servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D8x25mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1321,"ΤΕΜ",1,"GMC",1,"1FK21020AG000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-0AG00-0SA0","SIMOTICS S-1FK2 HD servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D8x25mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",932,"ΤΕΜ",1,"GMC",1,"1FK21020AG000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-0AG00-1MA0","SIMOTICS S-1FK2 HD servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D8x25mm with fitted key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1321,"ΤΕΜ",1,"GMC",1,"1FK21020AG001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-0AG00-1SA0","SIMOTICS S-1FK2 HD servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D8x25mm with fitted key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",932,"ΤΕΜ",1,"GMC",1,"1FK21020AG001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-0AG01-0MA0","SIMOTICS S-1FK2 HD servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D8x25mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1430,"ΤΕΜ",1,"GMC",1,"1FK21020AG010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-0AG01-0SA0","SIMOTICS S-1FK2 HD servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D8x25mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1040,"ΤΕΜ",1,"GMC",1,"1FK21020AG010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-0AG01-1MA0","SIMOTICS S-1FK2 HD servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D8x25mm with fitted key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1430,"ΤΕΜ",1,"GMC",1,"1FK21020AG011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-0AG01-1SA0","SIMOTICS S-1FK2 HD servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D8x25mm with fitted key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1040,"ΤΕΜ",1,"GMC",1,"1FK21020AG011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-0AG10-0MA0","SIMOTICS S-1FK2 HD servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D8x25mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1581,"ΤΕΜ",1,"GMC",1,"1FK21020AG100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-0AG10-0SA0","SIMOTICS S-1FK2 HD servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D8x25mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1192,"ΤΕΜ",1,"GMC",1,"1FK21020AG100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-0AG10-1MA0","SIMOTICS S-1FK2 HD servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D8x25mm with fitted key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1581,"ΤΕΜ",1,"GMC",1,"1FK21020AG101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-0AG10-1SA0","SIMOTICS S-1FK2 HD servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D8x25mm with fitted key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1192,"ΤΕΜ",1,"GMC",1,"1FK21020AG101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-0AG11-0MA0","SIMOTICS S-1FK2 HD servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D8x25mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1690,"ΤΕΜ",1,"GMC",1,"1FK21020AG110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-0AG11-0SA0","SIMOTICS S-1FK2 HD servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D8x25mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1300,"ΤΕΜ",1,"GMC",1,"1FK21020AG110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-0AG11-1MA0","SIMOTICS S-1FK2 HD servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D8x25mm with fitted key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1690,"ΤΕΜ",1,"GMC",1,"1FK21020AG111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-0AG11-1SA0","SIMOTICS S-1FK2 HD servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D8x25mm with fitted key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1300,"ΤΕΜ",1,"GMC",1,"1FK21020AG111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-1AG00-0MA0","SIMOTICS S-1FK2 HD servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D8x25mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1347,"ΤΕΜ",1,"GMC",1,"1FK21021AG000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-1AG00-0SA0","SIMOTICS S-1FK2 HD servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D8x25mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",958,"ΤΕΜ",1,"GMC",1,"1FK21021AG000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-1AG00-1MA0","SIMOTICS S-1FK2 HD servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D8x25mm with fitted key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1347,"ΤΕΜ",1,"GMC",1,"1FK21021AG001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-1AG00-1SA0","SIMOTICS S-1FK2 HD servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D8x25mm with fitted key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",958,"ΤΕΜ",1,"GMC",1,"1FK21021AG001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-1AG01-0MA0","SIMOTICS S-1FK2 HD servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D8x25mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1455,"ΤΕΜ",1,"GMC",1,"1FK21021AG010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-1AG01-0SA0","SIMOTICS S-1FK2 HD servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D8x25mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1066,"ΤΕΜ",1,"GMC",1,"1FK21021AG010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-1AG01-1MA0","SIMOTICS S-1FK2 HD servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D8x25mm with fitted key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1455,"ΤΕΜ",1,"GMC",1,"1FK21021AG011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-1AG01-1SA0","SIMOTICS S-1FK2 HD servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D8x25mm with fitted key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1066,"ΤΕΜ",1,"GMC",1,"1FK21021AG011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-1AG10-0MA0","SIMOTICS S-1FK2 HD servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D8x25mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1607,"ΤΕΜ",1,"GMC",1,"1FK21021AG100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-1AG10-0SA0","SIMOTICS S-1FK2 HD servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D8x25mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1218,"ΤΕΜ",1,"GMC",1,"1FK21021AG100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-1AG10-1MA0","SIMOTICS S-1FK2 HD servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D8x25mm with fitted key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1607,"ΤΕΜ",1,"GMC",1,"1FK21021AG101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-1AG10-1SA0","SIMOTICS S-1FK2 HD servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D8x25mm with fitted key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1218,"ΤΕΜ",1,"GMC",1,"1FK21021AG101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-1AG11-0MA0","SIMOTICS S-1FK2 HD servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D8x25mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1715,"ΤΕΜ",1,"GMC",1,"1FK21021AG110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-1AG11-0SA0","SIMOTICS S-1FK2 HD servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D8x25mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1326,"ΤΕΜ",1,"GMC",1,"1FK21021AG110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-1AG11-1MA0","SIMOTICS S-1FK2 HD servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D8x25mm with fitted key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1715,"ΤΕΜ",1,"GMC",1,"1FK21021AG111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2102-1AG11-1SA0","SIMOTICS S-1FK2 HD servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D8x25mm with fitted key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1326,"ΤΕΜ",1,"GMC",1,"1FK21021AG111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AG00-0MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1424,"ΤΕΜ",1,"GMC",1,"1FK21032AG000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AG00-0SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1035,"ΤΕΜ",1,"GMC",1,"1FK21032AG000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AG00-1MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1424,"ΤΕΜ",1,"GMC",1,"1FK21032AG001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AG00-1SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1035,"ΤΕΜ",1,"GMC",1,"1FK21032AG001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AG00-2MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1424,"ΤΕΜ",1,"GMC",1,"1FK21032AG002MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AG00-2SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1035,"ΤΕΜ",1,"GMC",1,"1FK21032AG002SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AG01-0MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1533,"ΤΕΜ",1,"GMC",1,"1FK21032AG010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AG01-0SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1144,"ΤΕΜ",1,"GMC",1,"1FK21032AG010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AG01-1MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1533,"ΤΕΜ",1,"GMC",1,"1FK21032AG011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AG01-1SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1144,"ΤΕΜ",1,"GMC",1,"1FK21032AG011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AG01-2MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M12, rotatable; .",1533,"ΤΕΜ",1,"GMC",1,"1FK21032AG012MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AG01-2SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M12, rotatable; .",1144,"ΤΕΜ",1,"GMC",1,"1FK21032AG012SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AG10-0MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1736,"ΤΕΜ",1,"GMC",1,"1FK21032AG100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AG10-0SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1347,"ΤΕΜ",1,"GMC",1,"1FK21032AG100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AG10-1MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1736,"ΤΕΜ",1,"GMC",1,"1FK21032AG101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AG10-1SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1347,"ΤΕΜ",1,"GMC",1,"1FK21032AG101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AG10-2MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1736,"ΤΕΜ",1,"GMC",1,"1FK21032AG102MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AG10-2SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1347,"ΤΕΜ",1,"GMC",1,"1FK21032AG102SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AG11-0MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1845,"ΤΕΜ",1,"GMC",1,"1FK21032AG110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AG11-0SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1456,"ΤΕΜ",1,"GMC",1,"1FK21032AG110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AG11-1MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1845,"ΤΕΜ",1,"GMC",1,"1FK21032AG111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AG11-1SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1456,"ΤΕΜ",1,"GMC",1,"1FK21032AG111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AG11-2MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M12, rotatable; .",1845,"ΤΕΜ",1,"GMC",1,"1FK21032AG112MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AG11-2SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M12, rotatable; .",1456,"ΤΕΜ",1,"GMC",1,"1FK21032AG112SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH00-0MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1424,"ΤΕΜ",1,"GMC",1,"1FK21032AH000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH00-0MB0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1424,"ΤΕΜ",1,"GMC",1,"1FK21032AH000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH00-0SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1035,"ΤΕΜ",1,"GMC",1,"1FK21032AH000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH00-0SB0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1035,"ΤΕΜ",1,"GMC",1,"1FK21032AH000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH00-1MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1424,"ΤΕΜ",1,"GMC",1,"1FK21032AH001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH00-1MB0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1424,"ΤΕΜ",1,"GMC",1,"1FK21032AH001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH00-1SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1035,"ΤΕΜ",1,"GMC",1,"1FK21032AH001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH00-1SB0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1035,"ΤΕΜ",1,"GMC",1,"1FK21032AH001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH00-2MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1424,"ΤΕΜ",1,"GMC",1,"1FK21032AH002MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH00-2MB0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1424,"ΤΕΜ",1,"GMC",1,"1FK21032AH002MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH00-2SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1035,"ΤΕΜ",1,"GMC",1,"1FK21032AH002SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH00-2SB0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1035,"ΤΕΜ",1,"GMC",1,"1FK21032AH002SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH01-0MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1533,"ΤΕΜ",1,"GMC",1,"1FK21032AH010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH01-0MB0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1533,"ΤΕΜ",1,"GMC",1,"1FK21032AH010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH01-0SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1144,"ΤΕΜ",1,"GMC",1,"1FK21032AH010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH01-0SB0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1144,"ΤΕΜ",1,"GMC",1,"1FK21032AH010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH01-1MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1533,"ΤΕΜ",1,"GMC",1,"1FK21032AH011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH01-1MB0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1533,"ΤΕΜ",1,"GMC",1,"1FK21032AH011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH01-1SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1144,"ΤΕΜ",1,"GMC",1,"1FK21032AH011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH01-1SB0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1144,"ΤΕΜ",1,"GMC",1,"1FK21032AH011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH01-2MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable; .",1533,"ΤΕΜ",1,"GMC",1,"1FK21032AH012MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH01-2MB0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17; .",1533,"ΤΕΜ",1,"GMC",1,"1FK21032AH012MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH01-2SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable; .",1144,"ΤΕΜ",1,"GMC",1,"1FK21032AH012SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH01-2SB0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17; .",1144,"ΤΕΜ",1,"GMC",1,"1FK21032AH012SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH10-0MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1736,"ΤΕΜ",1,"GMC",1,"1FK21032AH100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH10-0MB0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1736,"ΤΕΜ",1,"GMC",1,"1FK21032AH100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH10-0SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1347,"ΤΕΜ",1,"GMC",1,"1FK21032AH100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH10-0SB0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1347,"ΤΕΜ",1,"GMC",1,"1FK21032AH100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH10-1MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1736,"ΤΕΜ",1,"GMC",1,"1FK21032AH101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH10-1MB0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1736,"ΤΕΜ",1,"GMC",1,"1FK21032AH101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH10-1SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1347,"ΤΕΜ",1,"GMC",1,"1FK21032AH101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH10-1SB0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1347,"ΤΕΜ",1,"GMC",1,"1FK21032AH101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH10-2MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1736,"ΤΕΜ",1,"GMC",1,"1FK21032AH102MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH10-2MB0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1736,"ΤΕΜ",1,"GMC",1,"1FK21032AH102MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH10-2SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1347,"ΤΕΜ",1,"GMC",1,"1FK21032AH102SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH10-2SB0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1347,"ΤΕΜ",1,"GMC",1,"1FK21032AH102SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH11-0MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1845,"ΤΕΜ",1,"GMC",1,"1FK21032AH110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH11-0MB0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1845,"ΤΕΜ",1,"GMC",1,"1FK21032AH110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH11-0SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1456,"ΤΕΜ",1,"GMC",1,"1FK21032AH110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH11-0SB0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1456,"ΤΕΜ",1,"GMC",1,"1FK21032AH110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH11-1MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1845,"ΤΕΜ",1,"GMC",1,"1FK21032AH111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH11-1MB0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1845,"ΤΕΜ",1,"GMC",1,"1FK21032AH111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH11-1SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1456,"ΤΕΜ",1,"GMC",1,"1FK21032AH111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH11-1SB0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1456,"ΤΕΜ",1,"GMC",1,"1FK21032AH111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH11-2MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable; .",1845,"ΤΕΜ",1,"GMC",1,"1FK21032AH112MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH11-2MB0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1845,"ΤΕΜ",1,"GMC",1,"1FK21032AH112MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH11-2SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable; .",1456,"ΤΕΜ",1,"GMC",1,"1FK21032AH112SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-2AH11-2SB0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.28 kW at nN=4500 rpm (380-480 V); PN = 0.167 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1456,"ΤΕΜ",1,"GMC",1,"1FK21032AH112SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AG00-0MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1580,"ΤΕΜ",1,"GMC",1,"1FK21034AG000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AG00-0SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1190,"ΤΕΜ",1,"GMC",1,"1FK21034AG000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AG00-1MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1580,"ΤΕΜ",1,"GMC",1,"1FK21034AG001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AG00-1SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1190,"ΤΕΜ",1,"GMC",1,"1FK21034AG001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AG00-2MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1580,"ΤΕΜ",1,"GMC",1,"1FK21034AG002MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AG00-2SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1190,"ΤΕΜ",1,"GMC",1,"1FK21034AG002SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AG01-0MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1688,"ΤΕΜ",1,"GMC",1,"1FK21034AG010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AG01-0SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1299,"ΤΕΜ",1,"GMC",1,"1FK21034AG010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AG01-1MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1688,"ΤΕΜ",1,"GMC",1,"1FK21034AG011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AG01-1SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1299,"ΤΕΜ",1,"GMC",1,"1FK21034AG011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AG01-2MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M12, rotatable; .",1688,"ΤΕΜ",1,"GMC",1,"1FK21034AG012MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AG01-2SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M12, rotatable; .",1299,"ΤΕΜ",1,"GMC",1,"1FK21034AG012SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AG10-0MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1892,"ΤΕΜ",1,"GMC",1,"1FK21034AG100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AG10-0SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1502,"ΤΕΜ",1,"GMC",1,"1FK21034AG100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AG10-1MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1892,"ΤΕΜ",1,"GMC",1,"1FK21034AG101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AG10-1SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1502,"ΤΕΜ",1,"GMC",1,"1FK21034AG101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AG10-2MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1892,"ΤΕΜ",1,"GMC",1,"1FK21034AG102MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AG10-2SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1502,"ΤΕΜ",1,"GMC",1,"1FK21034AG102SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AG11-0MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",2000,"ΤΕΜ",1,"GMC",1,"1FK21034AG110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AG11-0SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1611,"ΤΕΜ",1,"GMC",1,"1FK21034AG110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AG11-1MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",2000,"ΤΕΜ",1,"GMC",1,"1FK21034AG111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AG11-1SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1611,"ΤΕΜ",1,"GMC",1,"1FK21034AG111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AG11-2MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M12, rotatable; .",2000,"ΤΕΜ",1,"GMC",1,"1FK21034AG112MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AG11-2SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M12, rotatable; .",1611,"ΤΕΜ",1,"GMC",1,"1FK21034AG112SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH00-0MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1580,"ΤΕΜ",1,"GMC",1,"1FK21034AH000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH00-0MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1580,"ΤΕΜ",1,"GMC",1,"1FK21034AH000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH00-0SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1190,"ΤΕΜ",1,"GMC",1,"1FK21034AH000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH00-0SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1190,"ΤΕΜ",1,"GMC",1,"1FK21034AH000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH00-1MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1580,"ΤΕΜ",1,"GMC",1,"1FK21034AH001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH00-1MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1580,"ΤΕΜ",1,"GMC",1,"1FK21034AH001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH00-1SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1190,"ΤΕΜ",1,"GMC",1,"1FK21034AH001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH00-1SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1190,"ΤΕΜ",1,"GMC",1,"1FK21034AH001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH00-2MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1580,"ΤΕΜ",1,"GMC",1,"1FK21034AH002MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH00-2MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1580,"ΤΕΜ",1,"GMC",1,"1FK21034AH002MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH00-2SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1190,"ΤΕΜ",1,"GMC",1,"1FK21034AH002SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH00-2SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1190,"ΤΕΜ",1,"GMC",1,"1FK21034AH002SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH01-0MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1688,"ΤΕΜ",1,"GMC",1,"1FK21034AH010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH01-0MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1688,"ΤΕΜ",1,"GMC",1,"1FK21034AH010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH01-0SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1299,"ΤΕΜ",1,"GMC",1,"1FK21034AH010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH01-0SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1299,"ΤΕΜ",1,"GMC",1,"1FK21034AH010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH01-1MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1688,"ΤΕΜ",1,"GMC",1,"1FK21034AH011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH01-1MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1688,"ΤΕΜ",1,"GMC",1,"1FK21034AH011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH01-1SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1299,"ΤΕΜ",1,"GMC",1,"1FK21034AH011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH01-1SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1299,"ΤΕΜ",1,"GMC",1,"1FK21034AH011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH01-2MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable; .",1688,"ΤΕΜ",1,"GMC",1,"1FK21034AH012MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH01-2MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17; .",1688,"ΤΕΜ",1,"GMC",1,"1FK21034AH012MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH01-2SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable; .",1299,"ΤΕΜ",1,"GMC",1,"1FK21034AH012SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH01-2SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17; .",1299,"ΤΕΜ",1,"GMC",1,"1FK21034AH012SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH10-0MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1892,"ΤΕΜ",1,"GMC",1,"1FK21034AH100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH10-0MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1892,"ΤΕΜ",1,"GMC",1,"1FK21034AH100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH10-0SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1502,"ΤΕΜ",1,"GMC",1,"1FK21034AH100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH10-0SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1502,"ΤΕΜ",1,"GMC",1,"1FK21034AH100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH10-1MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1892,"ΤΕΜ",1,"GMC",1,"1FK21034AH101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH10-1MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1892,"ΤΕΜ",1,"GMC",1,"1FK21034AH101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH10-1SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1502,"ΤΕΜ",1,"GMC",1,"1FK21034AH101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH10-1SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1502,"ΤΕΜ",1,"GMC",1,"1FK21034AH101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH10-2MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1892,"ΤΕΜ",1,"GMC",1,"1FK21034AH102MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH10-2MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1892,"ΤΕΜ",1,"GMC",1,"1FK21034AH102MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH10-2SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1502,"ΤΕΜ",1,"GMC",1,"1FK21034AH102SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH10-2SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1502,"ΤΕΜ",1,"GMC",1,"1FK21034AH102SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH11-0MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2000,"ΤΕΜ",1,"GMC",1,"1FK21034AH110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH11-0MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2000,"ΤΕΜ",1,"GMC",1,"1FK21034AH110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH11-0SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1611,"ΤΕΜ",1,"GMC",1,"1FK21034AH110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH11-0SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1611,"ΤΕΜ",1,"GMC",1,"1FK21034AH110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH11-1MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2000,"ΤΕΜ",1,"GMC",1,"1FK21034AH111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH11-1MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2000,"ΤΕΜ",1,"GMC",1,"1FK21034AH111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH11-1SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1611,"ΤΕΜ",1,"GMC",1,"1FK21034AH111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH11-1SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1611,"ΤΕΜ",1,"GMC",1,"1FK21034AH111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH11-2MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable; .",2000,"ΤΕΜ",1,"GMC",1,"1FK21034AH112MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH11-2MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",2000,"ΤΕΜ",1,"GMC",1,"1FK21034AH112MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH11-2SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable; .",1611,"ΤΕΜ",1,"GMC",1,"1FK21034AH112SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2103-4AH11-2SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.48 kW at nN=4500 rpm (380-480 V); PN = 0.3 kW at nN=2500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1611,"ΤΕΜ",1,"GMC",1,"1FK21034AH112SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF00-0MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1580,"ΤΕΜ",1,"GMC",1,"1FK21044AF000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF00-0MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1580,"ΤΕΜ",1,"GMC",1,"1FK21044AF000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF00-0SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1190,"ΤΕΜ",1,"GMC",1,"1FK21044AF000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF00-0SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1190,"ΤΕΜ",1,"GMC",1,"1FK21044AF000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF00-1MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1580,"ΤΕΜ",1,"GMC",1,"1FK21044AF001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF00-1MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1580,"ΤΕΜ",1,"GMC",1,"1FK21044AF001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF00-1SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1190,"ΤΕΜ",1,"GMC",1,"1FK21044AF001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF00-1SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1190,"ΤΕΜ",1,"GMC",1,"1FK21044AF001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF00-2MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1580,"ΤΕΜ",1,"GMC",1,"1FK21044AF002MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF00-2MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1580,"ΤΕΜ",1,"GMC",1,"1FK21044AF002MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF00-2SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1190,"ΤΕΜ",1,"GMC",1,"1FK21044AF002SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF00-2SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1190,"ΤΕΜ",1,"GMC",1,"1FK21044AF002SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF01-0MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1688,"ΤΕΜ",1,"GMC",1,"1FK21044AF010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF01-0MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1688,"ΤΕΜ",1,"GMC",1,"1FK21044AF010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF01-0SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1299,"ΤΕΜ",1,"GMC",1,"1FK21044AF010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF01-0SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1299,"ΤΕΜ",1,"GMC",1,"1FK21044AF010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF01-1MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1688,"ΤΕΜ",1,"GMC",1,"1FK21044AF011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF01-1MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1688,"ΤΕΜ",1,"GMC",1,"1FK21044AF011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF01-1SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1299,"ΤΕΜ",1,"GMC",1,"1FK21044AF011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF01-1SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1299,"ΤΕΜ",1,"GMC",1,"1FK21044AF011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF01-2MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480V); PN = 0.2 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M17, rotatable; .",1688,"ΤΕΜ",1,"GMC",1,"1FK21044AF012MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF01-2MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480V); PN = 0.2 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1688,"ΤΕΜ",1,"GMC",1,"1FK21044AF012MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF01-2SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480V); PN = 0.2 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M17, rotatable; .",1299,"ΤΕΜ",1,"GMC",1,"1FK21044AF012SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF01-2SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480V); PN = 0.2 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1299,"ΤΕΜ",1,"GMC",1,"1FK21044AF012SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF10-0MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1892,"ΤΕΜ",1,"GMC",1,"1FK21044AF100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF10-0MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1892,"ΤΕΜ",1,"GMC",1,"1FK21044AF100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF10-0SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1502,"ΤΕΜ",1,"GMC",1,"1FK21044AF100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF10-0SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1502,"ΤΕΜ",1,"GMC",1,"1FK21044AF100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF10-1MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1892,"ΤΕΜ",1,"GMC",1,"1FK21044AF101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF10-1MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1892,"ΤΕΜ",1,"GMC",1,"1FK21044AF101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF10-1SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1502,"ΤΕΜ",1,"GMC",1,"1FK21044AF101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF10-1SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1502,"ΤΕΜ",1,"GMC",1,"1FK21044AF101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF10-2MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1892,"ΤΕΜ",1,"GMC",1,"1FK21044AF102MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF10-2MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1892,"ΤΕΜ",1,"GMC",1,"1FK21044AF102MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF10-2SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1502,"ΤΕΜ",1,"GMC",1,"1FK21044AF102SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF10-2SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1502,"ΤΕΜ",1,"GMC",1,"1FK21044AF102SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF11-0MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2000,"ΤΕΜ",1,"GMC",1,"1FK21044AF110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF11-0MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2000,"ΤΕΜ",1,"GMC",1,"1FK21044AF110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF11-0SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1611,"ΤΕΜ",1,"GMC",1,"1FK21044AF110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF11-0SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1611,"ΤΕΜ",1,"GMC",1,"1FK21044AF110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF11-1MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2000,"ΤΕΜ",1,"GMC",1,"1FK21044AF111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF11-1MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2000,"ΤΕΜ",1,"GMC",1,"1FK21044AF111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF11-1SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1611,"ΤΕΜ",1,"GMC",1,"1FK21044AF111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF11-1SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1611,"ΤΕΜ",1,"GMC",1,"1FK21044AF111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF11-2MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480V); PN = 0.2 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M17, rotatable; .",2000,"ΤΕΜ",1,"GMC",1,"1FK21044AF112MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF11-2MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480V); PN = 0.2 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",2000,"ΤΕΜ",1,"GMC",1,"1FK21044AF112MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF11-2SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480V); PN = 0.2 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M17, rotatable; .",1611,"ΤΕΜ",1,"GMC",1,"1FK21044AF112SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AF11-2SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480V); PN = 0.2 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1611,"ΤΕΜ",1,"GMC",1,"1FK21044AF112SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK00-0MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1580,"ΤΕΜ",1,"GMC",1,"1FK21044AK000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK00-0MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1580,"ΤΕΜ",1,"GMC",1,"1FK21044AK000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK00-0SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1190,"ΤΕΜ",1,"GMC",1,"1FK21044AK000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK00-0SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1190,"ΤΕΜ",1,"GMC",1,"1FK21044AK000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK00-1MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1580,"ΤΕΜ",1,"GMC",1,"1FK21044AK001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK00-1MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1580,"ΤΕΜ",1,"GMC",1,"1FK21044AK001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK00-1SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1190,"ΤΕΜ",1,"GMC",1,"1FK21044AK001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK00-1SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1190,"ΤΕΜ",1,"GMC",1,"1FK21044AK001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK00-2MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1580,"ΤΕΜ",1,"GMC",1,"1FK21044AK002MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK00-2MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1580,"ΤΕΜ",1,"GMC",1,"1FK21044AK002MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK00-2SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1190,"ΤΕΜ",1,"GMC",1,"1FK21044AK002SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK00-2SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1190,"ΤΕΜ",1,"GMC",1,"1FK21044AK002SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK01-0MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1688,"ΤΕΜ",1,"GMC",1,"1FK21044AK010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK01-0MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1688,"ΤΕΜ",1,"GMC",1,"1FK21044AK010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK01-0SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1299,"ΤΕΜ",1,"GMC",1,"1FK21044AK010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK01-0SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1299,"ΤΕΜ",1,"GMC",1,"1FK21044AK010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK01-1MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1688,"ΤΕΜ",1,"GMC",1,"1FK21044AK011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK01-1MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1688,"ΤΕΜ",1,"GMC",1,"1FK21044AK011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK01-1SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1299,"ΤΕΜ",1,"GMC",1,"1FK21044AK011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK01-1SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1299,"ΤΕΜ",1,"GMC",1,"1FK21044AK011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK01-2MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480V); PN = 0.4 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M17, rotatable; .",1688,"ΤΕΜ",1,"GMC",1,"1FK21044AK012MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK01-2MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1688,"ΤΕΜ",1,"GMC",1,"1FK21044AK012MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK01-2SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480V); PN = 0.4 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M17, rotatable; .",1299,"ΤΕΜ",1,"GMC",1,"1FK21044AK012SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK01-2SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1299,"ΤΕΜ",1,"GMC",1,"1FK21044AK012SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK10-0MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1892,"ΤΕΜ",1,"GMC",1,"1FK21044AK100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK10-0MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1892,"ΤΕΜ",1,"GMC",1,"1FK21044AK100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK10-0SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1502,"ΤΕΜ",1,"GMC",1,"1FK21044AK100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK10-0SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1502,"ΤΕΜ",1,"GMC",1,"1FK21044AK100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK10-1MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1892,"ΤΕΜ",1,"GMC",1,"1FK21044AK101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK10-1MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1892,"ΤΕΜ",1,"GMC",1,"1FK21044AK101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK10-1SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1502,"ΤΕΜ",1,"GMC",1,"1FK21044AK101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK10-1SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1502,"ΤΕΜ",1,"GMC",1,"1FK21044AK101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK10-2MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1892,"ΤΕΜ",1,"GMC",1,"1FK21044AK102MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK10-2MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1892,"ΤΕΜ",1,"GMC",1,"1FK21044AK102MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK10-2SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1502,"ΤΕΜ",1,"GMC",1,"1FK21044AK102SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK10-2SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1502,"ΤΕΜ",1,"GMC",1,"1FK21044AK102SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK11-0MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2000,"ΤΕΜ",1,"GMC",1,"1FK21044AK110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK11-0MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2000,"ΤΕΜ",1,"GMC",1,"1FK21044AK110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK11-0SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1611,"ΤΕΜ",1,"GMC",1,"1FK21044AK110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK11-0SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1611,"ΤΕΜ",1,"GMC",1,"1FK21044AK110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK11-1MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2000,"ΤΕΜ",1,"GMC",1,"1FK21044AK111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK11-1MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2000,"ΤΕΜ",1,"GMC",1,"1FK21044AK111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK11-1SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1611,"ΤΕΜ",1,"GMC",1,"1FK21044AK111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK11-1SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1611,"ΤΕΜ",1,"GMC",1,"1FK21044AK111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK11-2MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480V); PN = 0.4 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M17, rotatable; .",2000,"ΤΕΜ",1,"GMC",1,"1FK21044AK112MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK11-2MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",2000,"ΤΕΜ",1,"GMC",1,"1FK21044AK112MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK11-2SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480V); PN = 0.4 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M17, rotatable; .",1611,"ΤΕΜ",1,"GMC",1,"1FK21044AK112SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-4AK11-2SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1611,"ΤΕΜ",1,"GMC",1,"1FK21044AK112SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF00-0MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1709,"ΤΕΜ",1,"GMC",1,"1FK21045AF000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF00-0MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1709,"ΤΕΜ",1,"GMC",1,"1FK21045AF000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF00-0SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1320,"ΤΕΜ",1,"GMC",1,"1FK21045AF000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF00-0SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1320,"ΤΕΜ",1,"GMC",1,"1FK21045AF000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF00-1MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1709,"ΤΕΜ",1,"GMC",1,"1FK21045AF001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF00-1MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1709,"ΤΕΜ",1,"GMC",1,"1FK21045AF001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF00-1SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1320,"ΤΕΜ",1,"GMC",1,"1FK21045AF001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF00-1SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1320,"ΤΕΜ",1,"GMC",1,"1FK21045AF001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF00-2MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1709,"ΤΕΜ",1,"GMC",1,"1FK21045AF002MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF00-2MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1709,"ΤΕΜ",1,"GMC",1,"1FK21045AF002MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF00-2SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1320,"ΤΕΜ",1,"GMC",1,"1FK21045AF002SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF00-2SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1320,"ΤΕΜ",1,"GMC",1,"1FK21045AF002SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF01-0MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1818,"ΤΕΜ",1,"GMC",1,"1FK21045AF010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF01-0MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1818,"ΤΕΜ",1,"GMC",1,"1FK21045AF010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF01-0SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1428,"ΤΕΜ",1,"GMC",1,"1FK21045AF010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF01-0SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1428,"ΤΕΜ",1,"GMC",1,"1FK21045AF010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF01-1MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1818,"ΤΕΜ",1,"GMC",1,"1FK21045AF011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF01-1MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1818,"ΤΕΜ",1,"GMC",1,"1FK21045AF011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF01-1SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1428,"ΤΕΜ",1,"GMC",1,"1FK21045AF011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF01-1SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1428,"ΤΕΜ",1,"GMC",1,"1FK21045AF011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF01-2MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480V); PN = 0.375 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M17, rotatable; .",1818,"ΤΕΜ",1,"GMC",1,"1FK21045AF012MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF01-2MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480V); PN = 0.375 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1818,"ΤΕΜ",1,"GMC",1,"1FK21045AF012MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF01-2SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480V); PN = 0.375 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M17, rotatable; .",1428,"ΤΕΜ",1,"GMC",1,"1FK21045AF012SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF01-2SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480V); PN = 0.375 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1428,"ΤΕΜ",1,"GMC",1,"1FK21045AF012SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF10-0MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2021,"ΤΕΜ",1,"GMC",1,"1FK21045AF100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF10-0MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2021,"ΤΕΜ",1,"GMC",1,"1FK21045AF100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF10-0SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1632,"ΤΕΜ",1,"GMC",1,"1FK21045AF100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF10-0SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1632,"ΤΕΜ",1,"GMC",1,"1FK21045AF100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF10-1MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2021,"ΤΕΜ",1,"GMC",1,"1FK21045AF101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF10-1MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2021,"ΤΕΜ",1,"GMC",1,"1FK21045AF101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF10-1SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1632,"ΤΕΜ",1,"GMC",1,"1FK21045AF101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF10-1SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1632,"ΤΕΜ",1,"GMC",1,"1FK21045AF101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF10-2MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2021,"ΤΕΜ",1,"GMC",1,"1FK21045AF102MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF10-2MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2021,"ΤΕΜ",1,"GMC",1,"1FK21045AF102MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF10-2SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1632,"ΤΕΜ",1,"GMC",1,"1FK21045AF102SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF10-2SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1632,"ΤΕΜ",1,"GMC",1,"1FK21045AF102SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF11-0MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2130,"ΤΕΜ",1,"GMC",1,"1FK21045AF110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF11-0MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2130,"ΤΕΜ",1,"GMC",1,"1FK21045AF110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF11-0SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1740,"ΤΕΜ",1,"GMC",1,"1FK21045AF110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF11-0SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1740,"ΤΕΜ",1,"GMC",1,"1FK21045AF110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF11-1MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2130,"ΤΕΜ",1,"GMC",1,"1FK21045AF111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF11-1MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2130,"ΤΕΜ",1,"GMC",1,"1FK21045AF111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF11-1SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1740,"ΤΕΜ",1,"GMC",1,"1FK21045AF111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF11-1SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1740,"ΤΕΜ",1,"GMC",1,"1FK21045AF111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF11-2MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480V); PN = 0.375 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M17, rotatable; .",2130,"ΤΕΜ",1,"GMC",1,"1FK21045AF112MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF11-2MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480V); PN = 0.375 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",2130,"ΤΕΜ",1,"GMC",1,"1FK21045AF112MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF11-2SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480V); PN = 0.375 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M17, rotatable; .",1740,"ΤΕΜ",1,"GMC",1,"1FK21045AF112SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AF11-2SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480V); PN = 0.375 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1740,"ΤΕΜ",1,"GMC",1,"1FK21045AF112SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK00-0MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1709,"ΤΕΜ",1,"GMC",1,"1FK21045AK000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK00-0MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1709,"ΤΕΜ",1,"GMC",1,"1FK21045AK000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK00-0SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1320,"ΤΕΜ",1,"GMC",1,"1FK21045AK000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK00-0SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1320,"ΤΕΜ",1,"GMC",1,"1FK21045AK000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK00-1MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1709,"ΤΕΜ",1,"GMC",1,"1FK21045AK001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK00-1MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1709,"ΤΕΜ",1,"GMC",1,"1FK21045AK001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK00-1SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1320,"ΤΕΜ",1,"GMC",1,"1FK21045AK001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK00-1SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1320,"ΤΕΜ",1,"GMC",1,"1FK21045AK001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK00-2MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1709,"ΤΕΜ",1,"GMC",1,"1FK21045AK002MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK00-2MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1709,"ΤΕΜ",1,"GMC",1,"1FK21045AK002MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK00-2SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1320,"ΤΕΜ",1,"GMC",1,"1FK21045AK002SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK00-2SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1320,"ΤΕΜ",1,"GMC",1,"1FK21045AK002SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK01-0MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1818,"ΤΕΜ",1,"GMC",1,"1FK21045AK010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK01-0MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1818,"ΤΕΜ",1,"GMC",1,"1FK21045AK010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK01-0SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1428,"ΤΕΜ",1,"GMC",1,"1FK21045AK010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK01-0SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1428,"ΤΕΜ",1,"GMC",1,"1FK21045AK010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK01-1MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1818,"ΤΕΜ",1,"GMC",1,"1FK21045AK011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK01-1MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1818,"ΤΕΜ",1,"GMC",1,"1FK21045AK011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK01-1SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1428,"ΤΕΜ",1,"GMC",1,"1FK21045AK011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK01-1SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1428,"ΤΕΜ",1,"GMC",1,"1FK21045AK011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK01-2MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480V); PN = 0.75 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M17, rotatable; .",1818,"ΤΕΜ",1,"GMC",1,"1FK21045AK012MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK01-2MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1818,"ΤΕΜ",1,"GMC",1,"1FK21045AK012MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK01-2SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480V); PN = 0.75 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M17, rotatable; .",1428,"ΤΕΜ",1,"GMC",1,"1FK21045AK012SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK01-2SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1428,"ΤΕΜ",1,"GMC",1,"1FK21045AK012SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK10-0MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2021,"ΤΕΜ",1,"GMC",1,"1FK21045AK100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK10-0MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2021,"ΤΕΜ",1,"GMC",1,"1FK21045AK100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK10-0SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1632,"ΤΕΜ",1,"GMC",1,"1FK21045AK100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK10-0SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1632,"ΤΕΜ",1,"GMC",1,"1FK21045AK100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK10-1MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2021,"ΤΕΜ",1,"GMC",1,"1FK21045AK101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK10-1MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2021,"ΤΕΜ",1,"GMC",1,"1FK21045AK101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK10-1SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1632,"ΤΕΜ",1,"GMC",1,"1FK21045AK101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK10-1SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1632,"ΤΕΜ",1,"GMC",1,"1FK21045AK101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK10-2MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2021,"ΤΕΜ",1,"GMC",1,"1FK21045AK102MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK10-2MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2021,"ΤΕΜ",1,"GMC",1,"1FK21045AK102MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK10-2SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1632,"ΤΕΜ",1,"GMC",1,"1FK21045AK102SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK10-2SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1632,"ΤΕΜ",1,"GMC",1,"1FK21045AK102SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK11-0MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2130,"ΤΕΜ",1,"GMC",1,"1FK21045AK110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK11-0MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2130,"ΤΕΜ",1,"GMC",1,"1FK21045AK110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK11-0SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1740,"ΤΕΜ",1,"GMC",1,"1FK21045AK110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK11-0SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1740,"ΤΕΜ",1,"GMC",1,"1FK21045AK110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK11-1MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2130,"ΤΕΜ",1,"GMC",1,"1FK21045AK111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK11-1MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2130,"ΤΕΜ",1,"GMC",1,"1FK21045AK111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK11-1SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1740,"ΤΕΜ",1,"GMC",1,"1FK21045AK111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK11-1SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1740,"ΤΕΜ",1,"GMC",1,"1FK21045AK111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK11-2MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480V); PN = 0.75 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M17, rotatable; .",2130,"ΤΕΜ",1,"GMC",1,"1FK21045AK112MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK11-2MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",2130,"ΤΕΜ",1,"GMC",1,"1FK21045AK112MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK11-2SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480V); PN = 0.75 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M17, rotatable; .",1740,"ΤΕΜ",1,"GMC",1,"1FK21045AK112SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-5AK11-2SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1740,"ΤΕΜ",1,"GMC",1,"1FK21045AK112SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF00-0MA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1787,"ΤΕΜ",1,"GMC",1,"1FK21046AF000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF00-0MB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1787,"ΤΕΜ",1,"GMC",1,"1FK21046AF000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF00-0SA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1397,"ΤΕΜ",1,"GMC",1,"1FK21046AF000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF00-0SB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1397,"ΤΕΜ",1,"GMC",1,"1FK21046AF000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF00-1MA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1787,"ΤΕΜ",1,"GMC",1,"1FK21046AF001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF00-1MB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1787,"ΤΕΜ",1,"GMC",1,"1FK21046AF001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF00-1SA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1397,"ΤΕΜ",1,"GMC",1,"1FK21046AF001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF00-1SB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1397,"ΤΕΜ",1,"GMC",1,"1FK21046AF001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF00-2MA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1787,"ΤΕΜ",1,"GMC",1,"1FK21046AF002MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF00-2MB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1787,"ΤΕΜ",1,"GMC",1,"1FK21046AF002MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF00-2SA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1397,"ΤΕΜ",1,"GMC",1,"1FK21046AF002SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF00-2SB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1397,"ΤΕΜ",1,"GMC",1,"1FK21046AF002SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF01-0MA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1895,"ΤΕΜ",1,"GMC",1,"1FK21046AF010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF01-0MB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1895,"ΤΕΜ",1,"GMC",1,"1FK21046AF010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF01-0SA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1506,"ΤΕΜ",1,"GMC",1,"1FK21046AF010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF01-0SB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1506,"ΤΕΜ",1,"GMC",1,"1FK21046AF010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF01-1MA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1895,"ΤΕΜ",1,"GMC",1,"1FK21046AF011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF01-1MB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1895,"ΤΕΜ",1,"GMC",1,"1FK21046AF011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF01-1SA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1506,"ΤΕΜ",1,"GMC",1,"1FK21046AF011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF01-1SB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1506,"ΤΕΜ",1,"GMC",1,"1FK21046AF011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF01-2MA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480V); PN = 0.5 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M17, rotatable; .",1895,"ΤΕΜ",1,"GMC",1,"1FK21046AF012MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF01-2MB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480V); PN = 0.5 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1895,"ΤΕΜ",1,"GMC",1,"1FK21046AF012MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF01-2SA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480V); PN = 0.5 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M17, rotatable; .",1506,"ΤΕΜ",1,"GMC",1,"1FK21046AF012SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF01-2SB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480V); PN = 0.5 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1506,"ΤΕΜ",1,"GMC",1,"1FK21046AF012SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF10-0MA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2099,"ΤΕΜ",1,"GMC",1,"1FK21046AF100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF10-0MB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2099,"ΤΕΜ",1,"GMC",1,"1FK21046AF100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF10-0SA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1709,"ΤΕΜ",1,"GMC",1,"1FK21046AF100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF10-0SB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1709,"ΤΕΜ",1,"GMC",1,"1FK21046AF100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF10-1MA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2099,"ΤΕΜ",1,"GMC",1,"1FK21046AF101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF10-1MB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2099,"ΤΕΜ",1,"GMC",1,"1FK21046AF101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF10-1SA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1709,"ΤΕΜ",1,"GMC",1,"1FK21046AF101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF10-1SB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1709,"ΤΕΜ",1,"GMC",1,"1FK21046AF101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF10-2MA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2099,"ΤΕΜ",1,"GMC",1,"1FK21046AF102MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF10-2MB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2099,"ΤΕΜ",1,"GMC",1,"1FK21046AF102MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF10-2SA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1709,"ΤΕΜ",1,"GMC",1,"1FK21046AF102SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF10-2SB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1709,"ΤΕΜ",1,"GMC",1,"1FK21046AF102SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF11-0MA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2207,"ΤΕΜ",1,"GMC",1,"1FK21046AF110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF11-0MB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2207,"ΤΕΜ",1,"GMC",1,"1FK21046AF110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF11-0SA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1818,"ΤΕΜ",1,"GMC",1,"1FK21046AF110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF11-0SB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1818,"ΤΕΜ",1,"GMC",1,"1FK21046AF110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF11-1MA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2207,"ΤΕΜ",1,"GMC",1,"1FK21046AF111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF11-1MB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2207,"ΤΕΜ",1,"GMC",1,"1FK21046AF111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF11-1SA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1818,"ΤΕΜ",1,"GMC",1,"1FK21046AF111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF11-1SB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1818,"ΤΕΜ",1,"GMC",1,"1FK21046AF111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF11-2MA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480V); PN = 0.5 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M17, rotatable; .",2207,"ΤΕΜ",1,"GMC",1,"1FK21046AF112MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF11-2MB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480V); PN = 0.5 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",2207,"ΤΕΜ",1,"GMC",1,"1FK21046AF112MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF11-2SA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480V); PN = 0.5 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M17, rotatable; .",1818,"ΤΕΜ",1,"GMC",1,"1FK21046AF112SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2104-6AF11-2SB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480V); PN = 0.5 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1818,"ΤΕΜ",1,"GMC",1,"1FK21046AF112SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF00-0MA0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1989,"ΤΕΜ",1,"GMC",1,"1FK21054AF000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF00-0MB0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1989,"ΤΕΜ",1,"GMC",1,"1FK21054AF000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF00-0SA0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1599,"ΤΕΜ",1,"GMC",1,"1FK21054AF000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF00-0SB0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1599,"ΤΕΜ",1,"GMC",1,"1FK21054AF000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF00-1MA0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1989,"ΤΕΜ",1,"GMC",1,"1FK21054AF001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF00-1MB0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1989,"ΤΕΜ",1,"GMC",1,"1FK21054AF001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF00-1SA0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1599,"ΤΕΜ",1,"GMC",1,"1FK21054AF001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF00-1SB0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1599,"ΤΕΜ",1,"GMC",1,"1FK21054AF001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF01-0MA0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2097,"ΤΕΜ",1,"GMC",1,"1FK21054AF010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF01-0MB0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2097,"ΤΕΜ",1,"GMC",1,"1FK21054AF010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF01-0SA0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1708,"ΤΕΜ",1,"GMC",1,"1FK21054AF010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF01-0SB0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1708,"ΤΕΜ",1,"GMC",1,"1FK21054AF010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF01-1MA0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2097,"ΤΕΜ",1,"GMC",1,"1FK21054AF011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF01-1MB0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2097,"ΤΕΜ",1,"GMC",1,"1FK21054AF011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF01-1SA0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1708,"ΤΕΜ",1,"GMC",1,"1FK21054AF011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF01-1SB0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1708,"ΤΕΜ",1,"GMC",1,"1FK21054AF011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF10-0MA0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2353,"ΤΕΜ",1,"GMC",1,"1FK21054AF100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF10-0MB0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2353,"ΤΕΜ",1,"GMC",1,"1FK21054AF100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF10-0SA0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1963,"ΤΕΜ",1,"GMC",1,"1FK21054AF100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF10-0SB0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1963,"ΤΕΜ",1,"GMC",1,"1FK21054AF100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF10-1MA0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2353,"ΤΕΜ",1,"GMC",1,"1FK21054AF101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF10-1MB0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2353,"ΤΕΜ",1,"GMC",1,"1FK21054AF101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF10-1SA0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1963,"ΤΕΜ",1,"GMC",1,"1FK21054AF101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF10-1SB0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1963,"ΤΕΜ",1,"GMC",1,"1FK21054AF101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF11-0MA0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2461,"ΤΕΜ",1,"GMC",1,"1FK21054AF110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF11-0MB0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2461,"ΤΕΜ",1,"GMC",1,"1FK21054AF110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF11-0SA0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",2072,"ΤΕΜ",1,"GMC",1,"1FK21054AF110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF11-0SB0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2072,"ΤΕΜ",1,"GMC",1,"1FK21054AF110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF11-1MA0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2461,"ΤΕΜ",1,"GMC",1,"1FK21054AF111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF11-1MB0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2461,"ΤΕΜ",1,"GMC",1,"1FK21054AF111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF11-1SA0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",2072,"ΤΕΜ",1,"GMC",1,"1FK21054AF111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-4AF11-1SB0","SIMOTICS S-1FK2 HD servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2072,"ΤΕΜ",1,"GMC",1,"1FK21054AF111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF00-0MA0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2304,"ΤΕΜ",1,"GMC",1,"1FK21056AF000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF00-0MB0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2304,"ΤΕΜ",1,"GMC",1,"1FK21056AF000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF00-0SA0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1915,"ΤΕΜ",1,"GMC",1,"1FK21056AF000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF00-0SB0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1915,"ΤΕΜ",1,"GMC",1,"1FK21056AF000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF00-1MA0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2304,"ΤΕΜ",1,"GMC",1,"1FK21056AF001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF00-1MB0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2304,"ΤΕΜ",1,"GMC",1,"1FK21056AF001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF00-1SA0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1915,"ΤΕΜ",1,"GMC",1,"1FK21056AF001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF00-1SB0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1915,"ΤΕΜ",1,"GMC",1,"1FK21056AF001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF01-0MA0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2413,"ΤΕΜ",1,"GMC",1,"1FK21056AF010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF01-0MB0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2413,"ΤΕΜ",1,"GMC",1,"1FK21056AF010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF01-0SA0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",2023,"ΤΕΜ",1,"GMC",1,"1FK21056AF010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF01-0SB0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2023,"ΤΕΜ",1,"GMC",1,"1FK21056AF010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF01-1MA0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2413,"ΤΕΜ",1,"GMC",1,"1FK21056AF011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF01-1MB0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2413,"ΤΕΜ",1,"GMC",1,"1FK21056AF011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF01-1SA0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",2023,"ΤΕΜ",1,"GMC",1,"1FK21056AF011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF01-1SB0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2023,"ΤΕΜ",1,"GMC",1,"1FK21056AF011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF10-0MA0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2668,"ΤΕΜ",1,"GMC",1,"1FK21056AF100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF10-0MB0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2668,"ΤΕΜ",1,"GMC",1,"1FK21056AF100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF10-0SA0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",2279,"ΤΕΜ",1,"GMC",1,"1FK21056AF100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF10-0SB0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2279,"ΤΕΜ",1,"GMC",1,"1FK21056AF100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF10-1MA0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2668,"ΤΕΜ",1,"GMC",1,"1FK21056AF101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF10-1MB0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2668,"ΤΕΜ",1,"GMC",1,"1FK21056AF101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF10-1SA0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",2279,"ΤΕΜ",1,"GMC",1,"1FK21056AF101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF10-1SB0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2279,"ΤΕΜ",1,"GMC",1,"1FK21056AF101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF11-0MA0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2777,"ΤΕΜ",1,"GMC",1,"1FK21056AF110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF11-0MB0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2777,"ΤΕΜ",1,"GMC",1,"1FK21056AF110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF11-0SA0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",2387,"ΤΕΜ",1,"GMC",1,"1FK21056AF110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF11-0SB0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2387,"ΤΕΜ",1,"GMC",1,"1FK21056AF110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF11-1MA0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2777,"ΤΕΜ",1,"GMC",1,"1FK21056AF111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF11-1MB0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2777,"ΤΕΜ",1,"GMC",1,"1FK21056AF111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF11-1SA0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",2387,"ΤΕΜ",1,"GMC",1,"1FK21056AF111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2105-6AF11-1SB0","SIMOTICS S-1FK2 HD servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2387,"ΤΕΜ",1,"GMC",1,"1FK21056AF111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF00-0MA0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2376,"ΤΕΜ",1,"GMC",1,"1FK21063AF000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF00-0MB0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2376,"ΤΕΜ",1,"GMC",1,"1FK21063AF000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF00-0SA0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",1987,"ΤΕΜ",1,"GMC",1,"1FK21063AF000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF00-0SB0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",1987,"ΤΕΜ",1,"GMC",1,"1FK21063AF000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF00-1MA0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2376,"ΤΕΜ",1,"GMC",1,"1FK21063AF001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF00-1MB0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2376,"ΤΕΜ",1,"GMC",1,"1FK21063AF001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF00-1SA0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",1987,"ΤΕΜ",1,"GMC",1,"1FK21063AF001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF00-1SB0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",1987,"ΤΕΜ",1,"GMC",1,"1FK21063AF001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF01-0MA0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2485,"ΤΕΜ",1,"GMC",1,"1FK21063AF010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF01-0MB0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2485,"ΤΕΜ",1,"GMC",1,"1FK21063AF010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF01-0SA0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2096,"ΤΕΜ",1,"GMC",1,"1FK21063AF010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF01-0SB0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2096,"ΤΕΜ",1,"GMC",1,"1FK21063AF010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF01-1MA0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2485,"ΤΕΜ",1,"GMC",1,"1FK21063AF011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF01-1MB0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2485,"ΤΕΜ",1,"GMC",1,"1FK21063AF011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF01-1SA0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2096,"ΤΕΜ",1,"GMC",1,"1FK21063AF011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF01-1SB0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2096,"ΤΕΜ",1,"GMC",1,"1FK21063AF011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF10-0MA0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2792,"ΤΕΜ",1,"GMC",1,"1FK21063AF100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF10-0MB0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2792,"ΤΕΜ",1,"GMC",1,"1FK21063AF100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF10-0SA0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2403,"ΤΕΜ",1,"GMC",1,"1FK21063AF100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF10-0SB0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2403,"ΤΕΜ",1,"GMC",1,"1FK21063AF100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF10-1MA0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2792,"ΤΕΜ",1,"GMC",1,"1FK21063AF101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF10-1MB0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2792,"ΤΕΜ",1,"GMC",1,"1FK21063AF101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF10-1SA0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2403,"ΤΕΜ",1,"GMC",1,"1FK21063AF101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF10-1SB0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2403,"ΤΕΜ",1,"GMC",1,"1FK21063AF101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF11-0MA0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2901,"ΤΕΜ",1,"GMC",1,"1FK21063AF110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF11-0MB0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2901,"ΤΕΜ",1,"GMC",1,"1FK21063AF110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF11-0SA0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2512,"ΤΕΜ",1,"GMC",1,"1FK21063AF110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF11-0SB0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2512,"ΤΕΜ",1,"GMC",1,"1FK21063AF110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF11-1MA0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2901,"ΤΕΜ",1,"GMC",1,"1FK21063AF111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF11-1MB0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2901,"ΤΕΜ",1,"GMC",1,"1FK21063AF111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF11-1SA0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2512,"ΤΕΜ",1,"GMC",1,"1FK21063AF111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-3AF11-1SB0","SIMOTICS S-1FK2 HD servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2512,"ΤΕΜ",1,"GMC",1,"1FK21063AF111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF00-0MA0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2555,"ΤΕΜ",1,"GMC",1,"1FK21064AF000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF00-0MB0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2555,"ΤΕΜ",1,"GMC",1,"1FK21064AF000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF00-0SA0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2166,"ΤΕΜ",1,"GMC",1,"1FK21064AF000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF00-0SB0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2166,"ΤΕΜ",1,"GMC",1,"1FK21064AF000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF00-1MA0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2555,"ΤΕΜ",1,"GMC",1,"1FK21064AF001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF00-1MB0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2555,"ΤΕΜ",1,"GMC",1,"1FK21064AF001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF00-1SA0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2166,"ΤΕΜ",1,"GMC",1,"1FK21064AF001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF00-1SB0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2166,"ΤΕΜ",1,"GMC",1,"1FK21064AF001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF01-0MA0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2664,"ΤΕΜ",1,"GMC",1,"1FK21064AF010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF01-0MB0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2664,"ΤΕΜ",1,"GMC",1,"1FK21064AF010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF01-0SA0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2275,"ΤΕΜ",1,"GMC",1,"1FK21064AF010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF01-0SB0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2275,"ΤΕΜ",1,"GMC",1,"1FK21064AF010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF01-1MA0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2664,"ΤΕΜ",1,"GMC",1,"1FK21064AF011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF01-1MB0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2664,"ΤΕΜ",1,"GMC",1,"1FK21064AF011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF01-1SA0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2275,"ΤΕΜ",1,"GMC",1,"1FK21064AF011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF01-1SB0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2275,"ΤΕΜ",1,"GMC",1,"1FK21064AF011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF10-0MA0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2971,"ΤΕΜ",1,"GMC",1,"1FK21064AF100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF10-0MB0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2971,"ΤΕΜ",1,"GMC",1,"1FK21064AF100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF10-0SA0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2582,"ΤΕΜ",1,"GMC",1,"1FK21064AF100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF10-0SB0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2582,"ΤΕΜ",1,"GMC",1,"1FK21064AF100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF10-1MA0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2971,"ΤΕΜ",1,"GMC",1,"1FK21064AF101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF10-1MB0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2971,"ΤΕΜ",1,"GMC",1,"1FK21064AF101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF10-1SA0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2582,"ΤΕΜ",1,"GMC",1,"1FK21064AF101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF10-1SB0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2582,"ΤΕΜ",1,"GMC",1,"1FK21064AF101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF11-0MA0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3080,"ΤΕΜ",1,"GMC",1,"1FK21064AF110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF11-0MB0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3080,"ΤΕΜ",1,"GMC",1,"1FK21064AF110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF11-0SA0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2691,"ΤΕΜ",1,"GMC",1,"1FK21064AF110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF11-0SB0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2691,"ΤΕΜ",1,"GMC",1,"1FK21064AF110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF11-1MA0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3080,"ΤΕΜ",1,"GMC",1,"1FK21064AF111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF11-1MB0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3080,"ΤΕΜ",1,"GMC",1,"1FK21064AF111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF11-1SA0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2691,"ΤΕΜ",1,"GMC",1,"1FK21064AF111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-4AF11-1SB0","SIMOTICS S-1FK2 HD servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2691,"ΤΕΜ",1,"GMC",1,"1FK21064AF111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF00-0MA0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2939,"ΤΕΜ",1,"GMC",1,"1FK21066AF000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF00-0MB0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2939,"ΤΕΜ",1,"GMC",1,"1FK21066AF000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF00-0SA0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2549,"ΤΕΜ",1,"GMC",1,"1FK21066AF000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF00-0SB0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2549,"ΤΕΜ",1,"GMC",1,"1FK21066AF000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF00-1MA0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2939,"ΤΕΜ",1,"GMC",1,"1FK21066AF001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF00-1MB0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2939,"ΤΕΜ",1,"GMC",1,"1FK21066AF001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF00-1SA0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2549,"ΤΕΜ",1,"GMC",1,"1FK21066AF001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF00-1SB0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2549,"ΤΕΜ",1,"GMC",1,"1FK21066AF001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF01-0MA0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3047,"ΤΕΜ",1,"GMC",1,"1FK21066AF010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF01-0MB0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3047,"ΤΕΜ",1,"GMC",1,"1FK21066AF010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF01-0SA0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2658,"ΤΕΜ",1,"GMC",1,"1FK21066AF010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF01-0SB0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2658,"ΤΕΜ",1,"GMC",1,"1FK21066AF010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF01-1MA0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3047,"ΤΕΜ",1,"GMC",1,"1FK21066AF011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF01-1MB0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3047,"ΤΕΜ",1,"GMC",1,"1FK21066AF011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF01-1SA0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2658,"ΤΕΜ",1,"GMC",1,"1FK21066AF011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF01-1SB0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2658,"ΤΕΜ",1,"GMC",1,"1FK21066AF011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF10-0MA0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3355,"ΤΕΜ",1,"GMC",1,"1FK21066AF100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF10-0MB0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3355,"ΤΕΜ",1,"GMC",1,"1FK21066AF100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF10-0SA0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2965,"ΤΕΜ",1,"GMC",1,"1FK21066AF100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF10-0SB0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2965,"ΤΕΜ",1,"GMC",1,"1FK21066AF100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF10-1MA0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3355,"ΤΕΜ",1,"GMC",1,"1FK21066AF101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF10-1MB0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3355,"ΤΕΜ",1,"GMC",1,"1FK21066AF101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF10-1SA0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2965,"ΤΕΜ",1,"GMC",1,"1FK21066AF101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF10-1SB0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2965,"ΤΕΜ",1,"GMC",1,"1FK21066AF101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF11-0MA0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3463,"ΤΕΜ",1,"GMC",1,"1FK21066AF110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF11-0MB0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3463,"ΤΕΜ",1,"GMC",1,"1FK21066AF110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF11-0SA0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3074,"ΤΕΜ",1,"GMC",1,"1FK21066AF110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF11-0SB0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3074,"ΤΕΜ",1,"GMC",1,"1FK21066AF110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF11-1MA0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3463,"ΤΕΜ",1,"GMC",1,"1FK21066AF111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF11-1MB0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3463,"ΤΕΜ",1,"GMC",1,"1FK21066AF111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF11-1SA0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3074,"ΤΕΜ",1,"GMC",1,"1FK21066AF111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2106-6AF11-1SB0","SIMOTICS S-1FK2 HD servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3074,"ΤΕΜ",1,"GMC",1,"1FK21066AF111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AG00-0MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1424,"ΤΕΜ",1,"GMC",1,"1FK22032AG000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AG00-0SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1035,"ΤΕΜ",1,"GMC",1,"1FK22032AG000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AG00-1MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1424,"ΤΕΜ",1,"GMC",1,"1FK22032AG001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AG00-1SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1035,"ΤΕΜ",1,"GMC",1,"1FK22032AG001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AG00-2MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1424,"ΤΕΜ",1,"GMC",1,"1FK22032AG002MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AG00-2SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1035,"ΤΕΜ",1,"GMC",1,"1FK22032AG002SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AG01-0MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1533,"ΤΕΜ",1,"GMC",1,"1FK22032AG010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AG01-0SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1144,"ΤΕΜ",1,"GMC",1,"1FK22032AG010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AG01-1MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1533,"ΤΕΜ",1,"GMC",1,"1FK22032AG011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AG01-1SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1144,"ΤΕΜ",1,"GMC",1,"1FK22032AG011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AG01-2MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M12, rotatable; .",1533,"ΤΕΜ",1,"GMC",1,"1FK22032AG012MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AG01-2SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M12, rotatable; .",1144,"ΤΕΜ",1,"GMC",1,"1FK22032AG012SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AG10-0MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1736,"ΤΕΜ",1,"GMC",1,"1FK22032AG100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AG10-0SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1347,"ΤΕΜ",1,"GMC",1,"1FK22032AG100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AG10-1MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1736,"ΤΕΜ",1,"GMC",1,"1FK22032AG101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AG10-1SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1347,"ΤΕΜ",1,"GMC",1,"1FK22032AG101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AG10-2MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1736,"ΤΕΜ",1,"GMC",1,"1FK22032AG102MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AG10-2SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1347,"ΤΕΜ",1,"GMC",1,"1FK22032AG102SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AG11-0MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1845,"ΤΕΜ",1,"GMC",1,"1FK22032AG110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AG11-0SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1456,"ΤΕΜ",1,"GMC",1,"1FK22032AG110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AG11-1MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1845,"ΤΕΜ",1,"GMC",1,"1FK22032AG111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AG11-1SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1456,"ΤΕΜ",1,"GMC",1,"1FK22032AG111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AG11-2MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M12, rotatable; .",1845,"ΤΕΜ",1,"GMC",1,"1FK22032AG112MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AG11-2SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M12, rotatable; .",1456,"ΤΕΜ",1,"GMC",1,"1FK22032AG112SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK00-0MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1424,"ΤΕΜ",1,"GMC",1,"1FK22032AK000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK00-0MB0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1424,"ΤΕΜ",1,"GMC",1,"1FK22032AK000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK00-0SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1035,"ΤΕΜ",1,"GMC",1,"1FK22032AK000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK00-0SB0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1035,"ΤΕΜ",1,"GMC",1,"1FK22032AK000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK00-1MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1424,"ΤΕΜ",1,"GMC",1,"1FK22032AK001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK00-1MB0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1424,"ΤΕΜ",1,"GMC",1,"1FK22032AK001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK00-1SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1035,"ΤΕΜ",1,"GMC",1,"1FK22032AK001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK00-1SB0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1035,"ΤΕΜ",1,"GMC",1,"1FK22032AK001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK00-2MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1424,"ΤΕΜ",1,"GMC",1,"1FK22032AK002MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK00-2MB0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1424,"ΤΕΜ",1,"GMC",1,"1FK22032AK002MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK00-2SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1035,"ΤΕΜ",1,"GMC",1,"1FK22032AK002SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK00-2SB0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1035,"ΤΕΜ",1,"GMC",1,"1FK22032AK002SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK01-0MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1533,"ΤΕΜ",1,"GMC",1,"1FK22032AK010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK01-0MB0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1533,"ΤΕΜ",1,"GMC",1,"1FK22032AK010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK01-0SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1144,"ΤΕΜ",1,"GMC",1,"1FK22032AK010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK01-0SB0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1144,"ΤΕΜ",1,"GMC",1,"1FK22032AK010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK01-1MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1533,"ΤΕΜ",1,"GMC",1,"1FK22032AK011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK01-1MB0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1533,"ΤΕΜ",1,"GMC",1,"1FK22032AK011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK01-1SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1144,"ΤΕΜ",1,"GMC",1,"1FK22032AK011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK01-1SB0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1144,"ΤΕΜ",1,"GMC",1,"1FK22032AK011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK01-2MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable; .",1533,"ΤΕΜ",1,"GMC",1,"1FK22032AK012MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK01-2MB0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17; .",1533,"ΤΕΜ",1,"GMC",1,"1FK22032AK012MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK01-2SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable; .",1144,"ΤΕΜ",1,"GMC",1,"1FK22032AK012SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK01-2SB0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17; .",1144,"ΤΕΜ",1,"GMC",1,"1FK22032AK012SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK10-0MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1736,"ΤΕΜ",1,"GMC",1,"1FK22032AK100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK10-0MB0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1736,"ΤΕΜ",1,"GMC",1,"1FK22032AK100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK10-0SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1347,"ΤΕΜ",1,"GMC",1,"1FK22032AK100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK10-0SB0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1347,"ΤΕΜ",1,"GMC",1,"1FK22032AK100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK10-1MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1736,"ΤΕΜ",1,"GMC",1,"1FK22032AK101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK10-1MB0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1736,"ΤΕΜ",1,"GMC",1,"1FK22032AK101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK10-1SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1347,"ΤΕΜ",1,"GMC",1,"1FK22032AK101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK10-1SB0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1347,"ΤΕΜ",1,"GMC",1,"1FK22032AK101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK10-2MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1736,"ΤΕΜ",1,"GMC",1,"1FK22032AK102MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK10-2MB0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1736,"ΤΕΜ",1,"GMC",1,"1FK22032AK102MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK10-2SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1347,"ΤΕΜ",1,"GMC",1,"1FK22032AK102SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK10-2SB0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1347,"ΤΕΜ",1,"GMC",1,"1FK22032AK102SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK11-0MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1845,"ΤΕΜ",1,"GMC",1,"1FK22032AK110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK11-0MB0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1845,"ΤΕΜ",1,"GMC",1,"1FK22032AK110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK11-0SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1456,"ΤΕΜ",1,"GMC",1,"1FK22032AK110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK11-0SB0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1456,"ΤΕΜ",1,"GMC",1,"1FK22032AK110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK11-1MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1845,"ΤΕΜ",1,"GMC",1,"1FK22032AK111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK11-1MB0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1845,"ΤΕΜ",1,"GMC",1,"1FK22032AK111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK11-1SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1456,"ΤΕΜ",1,"GMC",1,"1FK22032AK111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK11-1SB0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1456,"ΤΕΜ",1,"GMC",1,"1FK22032AK111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK11-2MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable; .",1845,"ΤΕΜ",1,"GMC",1,"1FK22032AK112MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK11-2MB0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1845,"ΤΕΜ",1,"GMC",1,"1FK22032AK112MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK11-2SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable; .",1456,"ΤΕΜ",1,"GMC",1,"1FK22032AK112SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-2AK11-2SB0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.255 kW at nN=6000 rpm (380-480 V); PN = 0.2 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1456,"ΤΕΜ",1,"GMC",1,"1FK22032AK112SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AG00-0MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1580,"ΤΕΜ",1,"GMC",1,"1FK22034AG000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AG00-0SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1190,"ΤΕΜ",1,"GMC",1,"1FK22034AG000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AG00-1MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1580,"ΤΕΜ",1,"GMC",1,"1FK22034AG001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AG00-1SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1190,"ΤΕΜ",1,"GMC",1,"1FK22034AG001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AG00-2MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1580,"ΤΕΜ",1,"GMC",1,"1FK22034AG002MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AG00-2SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1190,"ΤΕΜ",1,"GMC",1,"1FK22034AG002SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AG01-0MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1688,"ΤΕΜ",1,"GMC",1,"1FK22034AG010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AG01-0SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1299,"ΤΕΜ",1,"GMC",1,"1FK22034AG010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AG01-1MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1688,"ΤΕΜ",1,"GMC",1,"1FK22034AG011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AG01-1SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1299,"ΤΕΜ",1,"GMC",1,"1FK22034AG011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AG01-2MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M12, rotatable; .",1688,"ΤΕΜ",1,"GMC",1,"1FK22034AG012MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AG01-2SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M12, rotatable; .",1299,"ΤΕΜ",1,"GMC",1,"1FK22034AG012SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AG10-0MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1892,"ΤΕΜ",1,"GMC",1,"1FK22034AG100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AG10-0SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1502,"ΤΕΜ",1,"GMC",1,"1FK22034AG100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AG10-1MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1892,"ΤΕΜ",1,"GMC",1,"1FK22034AG101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AG10-1SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1502,"ΤΕΜ",1,"GMC",1,"1FK22034AG101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AG10-2MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",1892,"ΤΕΜ",1,"GMC",1,"1FK22034AG102MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AG10-2SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1502,"ΤΕΜ",1,"GMC",1,"1FK22034AG102SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AG11-0MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",2000,"ΤΕΜ",1,"GMC",1,"1FK22034AG110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AG11-0SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1611,"ΤΕΜ",1,"GMC",1,"1FK22034AG110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AG11-1MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M12, rotatable;",2000,"ΤΕΜ",1,"GMC",1,"1FK22034AG111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AG11-1SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M12, rotatable;",1611,"ΤΕΜ",1,"GMC",1,"1FK22034AG111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AG11-2MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M12, rotatable; .",2000,"ΤΕΜ",1,"GMC",1,"1FK22034AG112MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AG11-2SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M12, rotatable; .",1611,"ΤΕΜ",1,"GMC",1,"1FK22034AG112SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK00-0MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1580,"ΤΕΜ",1,"GMC",1,"1FK22034AK000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK00-0MB0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1580,"ΤΕΜ",1,"GMC",1,"1FK22034AK000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK00-0SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1190,"ΤΕΜ",1,"GMC",1,"1FK22034AK000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK00-0SB0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1190,"ΤΕΜ",1,"GMC",1,"1FK22034AK000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK00-1MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1580,"ΤΕΜ",1,"GMC",1,"1FK22034AK001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK00-1MB0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1580,"ΤΕΜ",1,"GMC",1,"1FK22034AK001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK00-1SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1190,"ΤΕΜ",1,"GMC",1,"1FK22034AK001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK00-1SB0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1190,"ΤΕΜ",1,"GMC",1,"1FK22034AK001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK00-2MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1580,"ΤΕΜ",1,"GMC",1,"1FK22034AK002MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK00-2MB0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1580,"ΤΕΜ",1,"GMC",1,"1FK22034AK002MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK00-2SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1190,"ΤΕΜ",1,"GMC",1,"1FK22034AK002SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK00-2SB0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1190,"ΤΕΜ",1,"GMC",1,"1FK22034AK002SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK01-0MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1688,"ΤΕΜ",1,"GMC",1,"1FK22034AK010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK01-0MB0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1688,"ΤΕΜ",1,"GMC",1,"1FK22034AK010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK01-0SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1299,"ΤΕΜ",1,"GMC",1,"1FK22034AK010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK01-0SB0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1299,"ΤΕΜ",1,"GMC",1,"1FK22034AK010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK01-1MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1688,"ΤΕΜ",1,"GMC",1,"1FK22034AK011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK01-1MB0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1688,"ΤΕΜ",1,"GMC",1,"1FK22034AK011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK01-1SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1299,"ΤΕΜ",1,"GMC",1,"1FK22034AK011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK01-1SB0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17;",1299,"ΤΕΜ",1,"GMC",1,"1FK22034AK011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK01-2MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable; .",1688,"ΤΕΜ",1,"GMC",1,"1FK22034AK012MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK01-2MB0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17; .",1688,"ΤΕΜ",1,"GMC",1,"1FK22034AK012MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK01-2SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable; .",1299,"ΤΕΜ",1,"GMC",1,"1FK22034AK012SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK01-2SB0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; power connector size M17; .",1299,"ΤΕΜ",1,"GMC",1,"1FK22034AK012SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK10-0MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1892,"ΤΕΜ",1,"GMC",1,"1FK22034AK100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK10-0MB0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1892,"ΤΕΜ",1,"GMC",1,"1FK22034AK100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK10-0SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1502,"ΤΕΜ",1,"GMC",1,"1FK22034AK100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK10-0SB0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1502,"ΤΕΜ",1,"GMC",1,"1FK22034AK100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK10-1MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1892,"ΤΕΜ",1,"GMC",1,"1FK22034AK101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK10-1MB0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1892,"ΤΕΜ",1,"GMC",1,"1FK22034AK101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK10-1SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1502,"ΤΕΜ",1,"GMC",1,"1FK22034AK101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK10-1SB0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1502,"ΤΕΜ",1,"GMC",1,"1FK22034AK101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK10-2MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1892,"ΤΕΜ",1,"GMC",1,"1FK22034AK102MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK10-2MB0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1892,"ΤΕΜ",1,"GMC",1,"1FK22034AK102MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK10-2SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1502,"ΤΕΜ",1,"GMC",1,"1FK22034AK102SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK10-2SB0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1502,"ΤΕΜ",1,"GMC",1,"1FK22034AK102SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK11-0MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2000,"ΤΕΜ",1,"GMC",1,"1FK22034AK110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK11-0MB0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2000,"ΤΕΜ",1,"GMC",1,"1FK22034AK110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK11-0SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1611,"ΤΕΜ",1,"GMC",1,"1FK22034AK110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK11-0SB0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1611,"ΤΕΜ",1,"GMC",1,"1FK22034AK110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK11-1MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2000,"ΤΕΜ",1,"GMC",1,"1FK22034AK111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK11-1MB0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2000,"ΤΕΜ",1,"GMC",1,"1FK22034AK111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK11-1SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1611,"ΤΕΜ",1,"GMC",1,"1FK22034AK111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK11-1SB0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D14x30 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1611,"ΤΕΜ",1,"GMC",1,"1FK22034AK111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK11-2MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable; .",2000,"ΤΕΜ",1,"GMC",1,"1FK22034AK112MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK11-2MB0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",2000,"ΤΕΜ",1,"GMC",1,"1FK22034AK112MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK11-2SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable; .",1611,"ΤΕΜ",1,"GMC",1,"1FK22034AK112SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2203-4AK11-2SB0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.43 kW at nN=6000 rpm (380-480 V); PN = 0.375 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1611,"ΤΕΜ",1,"GMC",1,"1FK22034AK112SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF00-0MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1709,"ΤΕΜ",1,"GMC",1,"1FK22045AF000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF00-0MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1709,"ΤΕΜ",1,"GMC",1,"1FK22045AF000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF00-0SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1320,"ΤΕΜ",1,"GMC",1,"1FK22045AF000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF00-0SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1320,"ΤΕΜ",1,"GMC",1,"1FK22045AF000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF00-1MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1709,"ΤΕΜ",1,"GMC",1,"1FK22045AF001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF00-1MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1709,"ΤΕΜ",1,"GMC",1,"1FK22045AF001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF00-1SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1320,"ΤΕΜ",1,"GMC",1,"1FK22045AF001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF00-1SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1320,"ΤΕΜ",1,"GMC",1,"1FK22045AF001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF00-2MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1709,"ΤΕΜ",1,"GMC",1,"1FK22045AF002MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF00-2MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1709,"ΤΕΜ",1,"GMC",1,"1FK22045AF002MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF00-2SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1320,"ΤΕΜ",1,"GMC",1,"1FK22045AF002SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF00-2SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1320,"ΤΕΜ",1,"GMC",1,"1FK22045AF002SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF01-0MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1818,"ΤΕΜ",1,"GMC",1,"1FK22045AF010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF01-0MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1818,"ΤΕΜ",1,"GMC",1,"1FK22045AF010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF01-0SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1428,"ΤΕΜ",1,"GMC",1,"1FK22045AF010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF01-0SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1428,"ΤΕΜ",1,"GMC",1,"1FK22045AF010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF01-1MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1818,"ΤΕΜ",1,"GMC",1,"1FK22045AF011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF01-1MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1818,"ΤΕΜ",1,"GMC",1,"1FK22045AF011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF01-1SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1428,"ΤΕΜ",1,"GMC",1,"1FK22045AF011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF01-1SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1428,"ΤΕΜ",1,"GMC",1,"1FK22045AF011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF01-2MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480V); PN = 0.375 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M17, rotatable; .",1818,"ΤΕΜ",1,"GMC",1,"1FK22045AF012MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF01-2MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480V); PN = 0.375 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1818,"ΤΕΜ",1,"GMC",1,"1FK22045AF012MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF01-2SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480V); PN = 0.375 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M17, rotatable; .",1428,"ΤΕΜ",1,"GMC",1,"1FK22045AF012SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF01-2SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480V); PN = 0.375 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1428,"ΤΕΜ",1,"GMC",1,"1FK22045AF012SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF10-0MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2021,"ΤΕΜ",1,"GMC",1,"1FK22045AF100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF10-0MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2021,"ΤΕΜ",1,"GMC",1,"1FK22045AF100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF10-0SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1632,"ΤΕΜ",1,"GMC",1,"1FK22045AF100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF10-0SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1632,"ΤΕΜ",1,"GMC",1,"1FK22045AF100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF10-1MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2021,"ΤΕΜ",1,"GMC",1,"1FK22045AF101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF10-1MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2021,"ΤΕΜ",1,"GMC",1,"1FK22045AF101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF10-1SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1632,"ΤΕΜ",1,"GMC",1,"1FK22045AF101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF10-1SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1632,"ΤΕΜ",1,"GMC",1,"1FK22045AF101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF10-2MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2021,"ΤΕΜ",1,"GMC",1,"1FK22045AF102MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF10-2MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2021,"ΤΕΜ",1,"GMC",1,"1FK22045AF102MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF10-2SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1632,"ΤΕΜ",1,"GMC",1,"1FK22045AF102SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF10-2SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1632,"ΤΕΜ",1,"GMC",1,"1FK22045AF102SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF11-0MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2130,"ΤΕΜ",1,"GMC",1,"1FK22045AF110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF11-0MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2130,"ΤΕΜ",1,"GMC",1,"1FK22045AF110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF11-0SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1740,"ΤΕΜ",1,"GMC",1,"1FK22045AF110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF11-0SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1740,"ΤΕΜ",1,"GMC",1,"1FK22045AF110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF11-1MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2130,"ΤΕΜ",1,"GMC",1,"1FK22045AF111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF11-1MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2130,"ΤΕΜ",1,"GMC",1,"1FK22045AF111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF11-1SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1740,"ΤΕΜ",1,"GMC",1,"1FK22045AF111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF11-1SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1740,"ΤΕΜ",1,"GMC",1,"1FK22045AF111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF11-2MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480V); PN = 0.375 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M17, rotatable; .",2130,"ΤΕΜ",1,"GMC",1,"1FK22045AF112MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF11-2MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480V); PN = 0.375 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",2130,"ΤΕΜ",1,"GMC",1,"1FK22045AF112MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF11-2SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480V); PN = 0.375 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M17, rotatable; .",1740,"ΤΕΜ",1,"GMC",1,"1FK22045AF112SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AF11-2SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480V); PN = 0.375 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1740,"ΤΕΜ",1,"GMC",1,"1FK22045AF112SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK00-0MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1709,"ΤΕΜ",1,"GMC",1,"1FK22045AK000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK00-0MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Âµs;",1709,"ΤΕΜ",1,"GMC",1,"1FK22045AK000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK00-0SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1320,"ΤΕΜ",1,"GMC",1,"1FK22045AK000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK00-0SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Âµs;",1320,"ΤΕΜ",1,"GMC",1,"1FK22045AK000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK00-1MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1709,"ΤΕΜ",1,"GMC",1,"1FK22045AK001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK00-1MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Âµs;",1709,"ΤΕΜ",1,"GMC",1,"1FK22045AK001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK00-1SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1320,"ΤΕΜ",1,"GMC",1,"1FK22045AK001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK00-1SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Âµs;",1320,"ΤΕΜ",1,"GMC",1,"1FK22045AK001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK00-2MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1709,"ΤΕΜ",1,"GMC",1,"1FK22045AK002MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK00-2MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Âµs;",1709,"ΤΕΜ",1,"GMC",1,"1FK22045AK002MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK00-2SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1320,"ΤΕΜ",1,"GMC",1,"1FK22045AK002SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK00-2SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Âµs;",1320,"ΤΕΜ",1,"GMC",1,"1FK22045AK002SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK01-0MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1818,"ΤΕΜ",1,"GMC",1,"1FK22045AK010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK01-0MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Âµs;",1818,"ΤΕΜ",1,"GMC",1,"1FK22045AK010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK01-0SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1428,"ΤΕΜ",1,"GMC",1,"1FK22045AK010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK01-0SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Âµs;",1428,"ΤΕΜ",1,"GMC",1,"1FK22045AK010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK01-1MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1818,"ΤΕΜ",1,"GMC",1,"1FK22045AK011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK01-1MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Âµs;",1818,"ΤΕΜ",1,"GMC",1,"1FK22045AK011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK01-1SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1428,"ΤΕΜ",1,"GMC",1,"1FK22045AK011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK01-1SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Âµs;",1428,"ΤΕΜ",1,"GMC",1,"1FK22045AK011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK01-2MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480V); PN = 0.75 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M17, rotatable; .",1818,"ΤΕΜ",1,"GMC",1,"1FK22045AK012MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK01-2MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480V); PN = 0.75 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Âµs; .",1818,"ΤΕΜ",1,"GMC",1,"1FK22045AK012MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK01-2SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480V); PN = 0.75 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M17, rotatable; .",1428,"ΤΕΜ",1,"GMC",1,"1FK22045AK012SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK01-2SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480V); PN = 0.75 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Âµs; .",1428,"ΤΕΜ",1,"GMC",1,"1FK22045AK012SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK10-0MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2021,"ΤΕΜ",1,"GMC",1,"1FK22045AK100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK10-0MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Âµs;",2021,"ΤΕΜ",1,"GMC",1,"1FK22045AK100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK10-0SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1632,"ΤΕΜ",1,"GMC",1,"1FK22045AK100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK10-0SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Âµs;",1632,"ΤΕΜ",1,"GMC",1,"1FK22045AK100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK10-1MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2021,"ΤΕΜ",1,"GMC",1,"1FK22045AK101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK10-1MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Âµs;",2021,"ΤΕΜ",1,"GMC",1,"1FK22045AK101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK10-1SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1632,"ΤΕΜ",1,"GMC",1,"1FK22045AK101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK10-1SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Âµs;",1632,"ΤΕΜ",1,"GMC",1,"1FK22045AK101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK10-2MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2021,"ΤΕΜ",1,"GMC",1,"1FK22045AK102MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK10-2MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Âµs;",2021,"ΤΕΜ",1,"GMC",1,"1FK22045AK102MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK10-2SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1632,"ΤΕΜ",1,"GMC",1,"1FK22045AK102SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK10-2SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Âµs;",1632,"ΤΕΜ",1,"GMC",1,"1FK22045AK102SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK11-0MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2130,"ΤΕΜ",1,"GMC",1,"1FK22045AK110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK11-0MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Âµs;",2130,"ΤΕΜ",1,"GMC",1,"1FK22045AK110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK11-0SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1740,"ΤΕΜ",1,"GMC",1,"1FK22045AK110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK11-0SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Âµs;",1740,"ΤΕΜ",1,"GMC",1,"1FK22045AK110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK11-1MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2130,"ΤΕΜ",1,"GMC",1,"1FK22045AK111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK11-1MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Âµs;",2130,"ΤΕΜ",1,"GMC",1,"1FK22045AK111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK11-1SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1740,"ΤΕΜ",1,"GMC",1,"1FK22045AK111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK11-1SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW at nN=3000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Âµs;",1740,"ΤΕΜ",1,"GMC",1,"1FK22045AK111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK11-2MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480V); PN = 0.75 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M17, rotatable; .",2130,"ΤΕΜ",1,"GMC",1,"1FK22045AK112MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK11-2MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480V); PN = 0.75 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Âµs; .",2130,"ΤΕΜ",1,"GMC",1,"1FK22045AK112MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK11-2SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480V); PN = 0.75 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M17, rotatable; .",1740,"ΤΕΜ",1,"GMC",1,"1FK22045AK112SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-5AK11-2SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480V); PN = 0.75 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Âµs; .",1740,"ΤΕΜ",1,"GMC",1,"1FK22045AK112SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF00-0MA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1787,"ΤΕΜ",1,"GMC",1,"1FK22046AF000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF00-0MB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1787,"ΤΕΜ",1,"GMC",1,"1FK22046AF000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF00-0SA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1397,"ΤΕΜ",1,"GMC",1,"1FK22046AF000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF00-0SB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1397,"ΤΕΜ",1,"GMC",1,"1FK22046AF000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF00-1MA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1787,"ΤΕΜ",1,"GMC",1,"1FK22046AF001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF00-1MB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1787,"ΤΕΜ",1,"GMC",1,"1FK22046AF001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF00-1SA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1397,"ΤΕΜ",1,"GMC",1,"1FK22046AF001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF00-1SB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1397,"ΤΕΜ",1,"GMC",1,"1FK22046AF001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF00-2MA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1787,"ΤΕΜ",1,"GMC",1,"1FK22046AF002MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF00-2MB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1787,"ΤΕΜ",1,"GMC",1,"1FK22046AF002MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF00-2SA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1397,"ΤΕΜ",1,"GMC",1,"1FK22046AF002SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF00-2SB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1397,"ΤΕΜ",1,"GMC",1,"1FK22046AF002SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF01-0MA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1895,"ΤΕΜ",1,"GMC",1,"1FK22046AF010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF01-0MB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1895,"ΤΕΜ",1,"GMC",1,"1FK22046AF010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF01-0SA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1506,"ΤΕΜ",1,"GMC",1,"1FK22046AF010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF01-0SB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1506,"ΤΕΜ",1,"GMC",1,"1FK22046AF010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF01-1MA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1895,"ΤΕΜ",1,"GMC",1,"1FK22046AF011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF01-1MB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1895,"ΤΕΜ",1,"GMC",1,"1FK22046AF011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF01-1SA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1506,"ΤΕΜ",1,"GMC",1,"1FK22046AF011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF01-1SB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1506,"ΤΕΜ",1,"GMC",1,"1FK22046AF011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF01-2MA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480V); PN = 0.5 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M17, rotatable; .",1895,"ΤΕΜ",1,"GMC",1,"1FK22046AF012MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF01-2MB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480V); PN = 0.5 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1895,"ΤΕΜ",1,"GMC",1,"1FK22046AF012MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF01-2SA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480V); PN = 0.5 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M17, rotatable; .",1506,"ΤΕΜ",1,"GMC",1,"1FK22046AF012SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF01-2SB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480V); PN = 0.5 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1506,"ΤΕΜ",1,"GMC",1,"1FK22046AF012SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF10-0MA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2099,"ΤΕΜ",1,"GMC",1,"1FK22046AF100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF10-0MB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2099,"ΤΕΜ",1,"GMC",1,"1FK22046AF100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF10-0SA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1709,"ΤΕΜ",1,"GMC",1,"1FK22046AF100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF10-0SB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1709,"ΤΕΜ",1,"GMC",1,"1FK22046AF100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF10-1MA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2099,"ΤΕΜ",1,"GMC",1,"1FK22046AF101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF10-1MB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2099,"ΤΕΜ",1,"GMC",1,"1FK22046AF101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF10-1SA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1709,"ΤΕΜ",1,"GMC",1,"1FK22046AF101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF10-1SB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1709,"ΤΕΜ",1,"GMC",1,"1FK22046AF101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF10-2MA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2099,"ΤΕΜ",1,"GMC",1,"1FK22046AF102MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF10-2MB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2099,"ΤΕΜ",1,"GMC",1,"1FK22046AF102MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF10-2SA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1709,"ΤΕΜ",1,"GMC",1,"1FK22046AF102SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF10-2SB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1709,"ΤΕΜ",1,"GMC",1,"1FK22046AF102SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF11-0MA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2207,"ΤΕΜ",1,"GMC",1,"1FK22046AF110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF11-0MB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2207,"ΤΕΜ",1,"GMC",1,"1FK22046AF110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF11-0SA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1818,"ΤΕΜ",1,"GMC",1,"1FK22046AF110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF11-0SB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1818,"ΤΕΜ",1,"GMC",1,"1FK22046AF110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF11-1MA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2207,"ΤΕΜ",1,"GMC",1,"1FK22046AF111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF11-1MB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2207,"ΤΕΜ",1,"GMC",1,"1FK22046AF111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF11-1SA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1818,"ΤΕΜ",1,"GMC",1,"1FK22046AF111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF11-1SB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1818,"ΤΕΜ",1,"GMC",1,"1FK22046AF111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF11-2MA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480V); PN = 0.5 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M17, rotatable; .",2207,"ΤΕΜ",1,"GMC",1,"1FK22046AF112MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF11-2MB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480V); PN = 0.5 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",2207,"ΤΕΜ",1,"GMC",1,"1FK22046AF112MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF11-2SA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480V); PN = 0.5 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M17, rotatable; .",1818,"ΤΕΜ",1,"GMC",1,"1FK22046AF112SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2204-6AF11-2SB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480V); PN = 0.5 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1818,"ΤΕΜ",1,"GMC",1,"1FK22046AF112SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF00-0MA0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1814,"ΤΕΜ",1,"GMC",1,"1FK22052AF000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF00-0MB0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1814,"ΤΕΜ",1,"GMC",1,"1FK22052AF000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF00-0SA0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1425,"ΤΕΜ",1,"GMC",1,"1FK22052AF000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF00-0SB0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1425,"ΤΕΜ",1,"GMC",1,"1FK22052AF000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF00-1MA0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1814,"ΤΕΜ",1,"GMC",1,"1FK22052AF001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF00-1MB0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1814,"ΤΕΜ",1,"GMC",1,"1FK22052AF001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF00-1SA0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1425,"ΤΕΜ",1,"GMC",1,"1FK22052AF001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF00-1SB0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1425,"ΤΕΜ",1,"GMC",1,"1FK22052AF001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF01-0MA0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1923,"ΤΕΜ",1,"GMC",1,"1FK22052AF010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF01-0MB0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1923,"ΤΕΜ",1,"GMC",1,"1FK22052AF010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF01-0SA0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1534,"ΤΕΜ",1,"GMC",1,"1FK22052AF010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF01-0SB0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1534,"ΤΕΜ",1,"GMC",1,"1FK22052AF010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF01-1MA0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",1923,"ΤΕΜ",1,"GMC",1,"1FK22052AF011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF01-1MB0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1923,"ΤΕΜ",1,"GMC",1,"1FK22052AF011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF01-1SA0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1534,"ΤΕΜ",1,"GMC",1,"1FK22052AF011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF01-1SB0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1534,"ΤΕΜ",1,"GMC",1,"1FK22052AF011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF10-0MA0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2178,"ΤΕΜ",1,"GMC",1,"1FK22052AF100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF10-0MB0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2178,"ΤΕΜ",1,"GMC",1,"1FK22052AF100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF10-0SA0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1789,"ΤΕΜ",1,"GMC",1,"1FK22052AF100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF10-0SB0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1789,"ΤΕΜ",1,"GMC",1,"1FK22052AF100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF10-1MA0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2178,"ΤΕΜ",1,"GMC",1,"1FK22052AF101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF10-1MB0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2178,"ΤΕΜ",1,"GMC",1,"1FK22052AF101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF10-1SA0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1789,"ΤΕΜ",1,"GMC",1,"1FK22052AF101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF10-1SB0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1789,"ΤΕΜ",1,"GMC",1,"1FK22052AF101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF11-0MA0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2287,"ΤΕΜ",1,"GMC",1,"1FK22052AF110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF11-0MB0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2287,"ΤΕΜ",1,"GMC",1,"1FK22052AF110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF11-0SA0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1898,"ΤΕΜ",1,"GMC",1,"1FK22052AF110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF11-0SB0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1898,"ΤΕΜ",1,"GMC",1,"1FK22052AF110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF11-1MA0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2287,"ΤΕΜ",1,"GMC",1,"1FK22052AF111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF11-1MB0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2287,"ΤΕΜ",1,"GMC",1,"1FK22052AF111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF11-1SA0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1898,"ΤΕΜ",1,"GMC",1,"1FK22052AF111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-2AF11-1SB0","SIMOTICS S-1FK2 CT servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1898,"ΤΕΜ",1,"GMC",1,"1FK22052AF111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF00-0MA0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2071,"ΤΕΜ",1,"GMC",1,"1FK22054AF000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF00-0MB0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2071,"ΤΕΜ",1,"GMC",1,"1FK22054AF000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF00-0SA0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1682,"ΤΕΜ",1,"GMC",1,"1FK22054AF000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF00-0SB0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1682,"ΤΕΜ",1,"GMC",1,"1FK22054AF000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF00-1MA0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2071,"ΤΕΜ",1,"GMC",1,"1FK22054AF001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF00-1MB0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2071,"ΤΕΜ",1,"GMC",1,"1FK22054AF001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF00-1SA0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1682,"ΤΕΜ",1,"GMC",1,"1FK22054AF001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF00-1SB0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1682,"ΤΕΜ",1,"GMC",1,"1FK22054AF001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF01-0MA0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2180,"ΤΕΜ",1,"GMC",1,"1FK22054AF010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF01-0MB0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2180,"ΤΕΜ",1,"GMC",1,"1FK22054AF010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF01-0SA0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1791,"ΤΕΜ",1,"GMC",1,"1FK22054AF010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF01-0SB0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1791,"ΤΕΜ",1,"GMC",1,"1FK22054AF010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF01-1MA0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2180,"ΤΕΜ",1,"GMC",1,"1FK22054AF011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF01-1MB0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2180,"ΤΕΜ",1,"GMC",1,"1FK22054AF011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF01-1SA0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",1791,"ΤΕΜ",1,"GMC",1,"1FK22054AF011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF01-1SB0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",1791,"ΤΕΜ",1,"GMC",1,"1FK22054AF011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF10-0MA0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2435,"ΤΕΜ",1,"GMC",1,"1FK22054AF100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF10-0MB0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2435,"ΤΕΜ",1,"GMC",1,"1FK22054AF100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF10-0SA0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",2046,"ΤΕΜ",1,"GMC",1,"1FK22054AF100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF10-0SB0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2046,"ΤΕΜ",1,"GMC",1,"1FK22054AF100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF10-1MA0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2435,"ΤΕΜ",1,"GMC",1,"1FK22054AF101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF10-1MB0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2435,"ΤΕΜ",1,"GMC",1,"1FK22054AF101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF10-1SA0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",2046,"ΤΕΜ",1,"GMC",1,"1FK22054AF101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF10-1SB0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2046,"ΤΕΜ",1,"GMC",1,"1FK22054AF101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF11-0MA0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2544,"ΤΕΜ",1,"GMC",1,"1FK22054AF110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF11-0MB0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2544,"ΤΕΜ",1,"GMC",1,"1FK22054AF110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF11-0SA0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",2155,"ΤΕΜ",1,"GMC",1,"1FK22054AF110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF11-0SB0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D19x40mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2155,"ΤΕΜ",1,"GMC",1,"1FK22054AF110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF11-1MA0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M17, rotatable;",2544,"ΤΕΜ",1,"GMC",1,"1FK22054AF111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF11-1MB0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2544,"ΤΕΜ",1,"GMC",1,"1FK22054AF111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF11-1SA0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M17, rotatable;",2155,"ΤΕΜ",1,"GMC",1,"1FK22054AF111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2205-4AF11-1SB0","SIMOTICS S-1FK2 CT servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D19x40 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17;",2155,"ΤΕΜ",1,"GMC",1,"1FK22054AF111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF00-0MA0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2118,"ΤΕΜ",1,"GMC",1,"1FK22062AF000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF00-0MB0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2118,"ΤΕΜ",1,"GMC",1,"1FK22062AF000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF00-0SA0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",1729,"ΤΕΜ",1,"GMC",1,"1FK22062AF000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF00-0SB0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",1729,"ΤΕΜ",1,"GMC",1,"1FK22062AF000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF00-1MA0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2118,"ΤΕΜ",1,"GMC",1,"1FK22062AF001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF00-1MB0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2118,"ΤΕΜ",1,"GMC",1,"1FK22062AF001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF00-1SA0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",1729,"ΤΕΜ",1,"GMC",1,"1FK22062AF001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF00-1SB0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",1729,"ΤΕΜ",1,"GMC",1,"1FK22062AF001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF01-0MA0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2227,"ΤΕΜ",1,"GMC",1,"1FK22062AF010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF01-0MB0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2227,"ΤΕΜ",1,"GMC",1,"1FK22062AF010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF01-0SA0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",1838,"ΤΕΜ",1,"GMC",1,"1FK22062AF010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF01-0SB0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",1838,"ΤΕΜ",1,"GMC",1,"1FK22062AF010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF01-1MA0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2227,"ΤΕΜ",1,"GMC",1,"1FK22062AF011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF01-1MB0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2227,"ΤΕΜ",1,"GMC",1,"1FK22062AF011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF01-1SA0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",1838,"ΤΕΜ",1,"GMC",1,"1FK22062AF011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF01-1SB0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",1838,"ΤΕΜ",1,"GMC",1,"1FK22062AF011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF10-0MA0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2534,"ΤΕΜ",1,"GMC",1,"1FK22062AF100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF10-0MB0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2534,"ΤΕΜ",1,"GMC",1,"1FK22062AF100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF10-0SA0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2145,"ΤΕΜ",1,"GMC",1,"1FK22062AF100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF10-0SB0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2145,"ΤΕΜ",1,"GMC",1,"1FK22062AF100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF10-1MA0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2534,"ΤΕΜ",1,"GMC",1,"1FK22062AF101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF10-1MB0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2534,"ΤΕΜ",1,"GMC",1,"1FK22062AF101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF10-1SA0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2145,"ΤΕΜ",1,"GMC",1,"1FK22062AF101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF10-1SB0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2145,"ΤΕΜ",1,"GMC",1,"1FK22062AF101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF11-0MA0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2643,"ΤΕΜ",1,"GMC",1,"1FK22062AF110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF11-0MB0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2643,"ΤΕΜ",1,"GMC",1,"1FK22062AF110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF11-0SA0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2254,"ΤΕΜ",1,"GMC",1,"1FK22062AF110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF11-0SB0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2254,"ΤΕΜ",1,"GMC",1,"1FK22062AF110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF11-1MA0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2643,"ΤΕΜ",1,"GMC",1,"1FK22062AF111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF11-1MB0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2643,"ΤΕΜ",1,"GMC",1,"1FK22062AF111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF11-1SA0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2254,"ΤΕΜ",1,"GMC",1,"1FK22062AF111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-2AF11-1SB0","SIMOTICS S-1FK2 CT servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2254,"ΤΕΜ",1,"GMC",1,"1FK22062AF111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF00-0MA0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2640,"ΤΕΜ",1,"GMC",1,"1FK22064AF000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF00-0MB0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2640,"ΤΕΜ",1,"GMC",1,"1FK22064AF000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF00-0SA0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2251,"ΤΕΜ",1,"GMC",1,"1FK22064AF000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF00-0SB0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2251,"ΤΕΜ",1,"GMC",1,"1FK22064AF000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF00-1MA0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2640,"ΤΕΜ",1,"GMC",1,"1FK22064AF001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF00-1MB0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2640,"ΤΕΜ",1,"GMC",1,"1FK22064AF001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF00-1SA0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2251,"ΤΕΜ",1,"GMC",1,"1FK22064AF001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF00-1SB0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2251,"ΤΕΜ",1,"GMC",1,"1FK22064AF001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF01-0MA0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2749,"ΤΕΜ",1,"GMC",1,"1FK22064AF010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF01-0MB0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2749,"ΤΕΜ",1,"GMC",1,"1FK22064AF010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF01-0SA0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2360,"ΤΕΜ",1,"GMC",1,"1FK22064AF010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF01-0SB0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2360,"ΤΕΜ",1,"GMC",1,"1FK22064AF010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF01-1MA0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",2749,"ΤΕΜ",1,"GMC",1,"1FK22064AF011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF01-1MB0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2749,"ΤΕΜ",1,"GMC",1,"1FK22064AF011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF01-1SA0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2360,"ΤΕΜ",1,"GMC",1,"1FK22064AF011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF01-1SB0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2360,"ΤΕΜ",1,"GMC",1,"1FK22064AF011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF10-0MA0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3056,"ΤΕΜ",1,"GMC",1,"1FK22064AF100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF10-0MB0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3056,"ΤΕΜ",1,"GMC",1,"1FK22064AF100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF10-0SA0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2667,"ΤΕΜ",1,"GMC",1,"1FK22064AF100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF10-0SB0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2667,"ΤΕΜ",1,"GMC",1,"1FK22064AF100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF10-1MA0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3056,"ΤΕΜ",1,"GMC",1,"1FK22064AF101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF10-1MB0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3056,"ΤΕΜ",1,"GMC",1,"1FK22064AF101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF10-1SA0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2667,"ΤΕΜ",1,"GMC",1,"1FK22064AF101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF10-1SB0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2667,"ΤΕΜ",1,"GMC",1,"1FK22064AF101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF11-0MA0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3165,"ΤΕΜ",1,"GMC",1,"1FK22064AF110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF11-0MB0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3165,"ΤΕΜ",1,"GMC",1,"1FK22064AF110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF11-0SA0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2776,"ΤΕΜ",1,"GMC",1,"1FK22064AF110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF11-0SB0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2776,"ΤΕΜ",1,"GMC",1,"1FK22064AF110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF11-1MA0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3165,"ΤΕΜ",1,"GMC",1,"1FK22064AF111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF11-1MB0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3165,"ΤΕΜ",1,"GMC",1,"1FK22064AF111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF11-1SA0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2776,"ΤΕΜ",1,"GMC",1,"1FK22064AF111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2206-4AF11-1SB0","SIMOTICS S-1FK2 CT servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2776,"ΤΕΜ",1,"GMC",1,"1FK22064AF111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC00-0MA0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3094,"ΤΕΜ",1,"GMC",1,"1FK22083AC000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC00-0MB0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3094,"ΤΕΜ",1,"GMC",1,"1FK22083AC000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC00-0SA0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2705,"ΤΕΜ",1,"GMC",1,"1FK22083AC000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC00-0SB0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2705,"ΤΕΜ",1,"GMC",1,"1FK22083AC000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC00-1MA0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3094,"ΤΕΜ",1,"GMC",1,"1FK22083AC001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC00-1MB0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3094,"ΤΕΜ",1,"GMC",1,"1FK22083AC001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC00-1SA0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2705,"ΤΕΜ",1,"GMC",1,"1FK22083AC001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC00-1SB0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2705,"ΤΕΜ",1,"GMC",1,"1FK22083AC001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC01-0MA0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3203,"ΤΕΜ",1,"GMC",1,"1FK22083AC010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC01-0MB0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3203,"ΤΕΜ",1,"GMC",1,"1FK22083AC010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC01-0SA0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2814,"ΤΕΜ",1,"GMC",1,"1FK22083AC010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC01-0SB0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2814,"ΤΕΜ",1,"GMC",1,"1FK22083AC010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC01-1MA0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3203,"ΤΕΜ",1,"GMC",1,"1FK22083AC011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC01-1MB0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3203,"ΤΕΜ",1,"GMC",1,"1FK22083AC011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC01-1SA0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",2814,"ΤΕΜ",1,"GMC",1,"1FK22083AC011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC01-1SB0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2814,"ΤΕΜ",1,"GMC",1,"1FK22083AC011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC10-0MA0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3614,"ΤΕΜ",1,"GMC",1,"1FK22083AC100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC10-0MB0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3614,"ΤΕΜ",1,"GMC",1,"1FK22083AC100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC10-0SA0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3225,"ΤΕΜ",1,"GMC",1,"1FK22083AC100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC10-0SB0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3225,"ΤΕΜ",1,"GMC",1,"1FK22083AC100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC10-1MA0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3614,"ΤΕΜ",1,"GMC",1,"1FK22083AC101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC10-1MB0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3614,"ΤΕΜ",1,"GMC",1,"1FK22083AC101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC10-1SA0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3225,"ΤΕΜ",1,"GMC",1,"1FK22083AC101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC10-1SB0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3225,"ΤΕΜ",1,"GMC",1,"1FK22083AC101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC11-0MA0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3723,"ΤΕΜ",1,"GMC",1,"1FK22083AC110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC11-0MB0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3723,"ΤΕΜ",1,"GMC",1,"1FK22083AC110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC11-0SA0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3334,"ΤΕΜ",1,"GMC",1,"1FK22083AC110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC11-0SB0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3334,"ΤΕΜ",1,"GMC",1,"1FK22083AC110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC11-1MA0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3723,"ΤΕΜ",1,"GMC",1,"1FK22083AC111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC11-1MB0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3723,"ΤΕΜ",1,"GMC",1,"1FK22083AC111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC11-1SA0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3334,"ΤΕΜ",1,"GMC",1,"1FK22083AC111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-3AC11-1SB0","SIMOTICS S-1FK2 CT servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3334,"ΤΕΜ",1,"GMC",1,"1FK22083AC111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC00-0MA0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3404,"ΤΕΜ",1,"GMC",1,"1FK22084AC000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC00-0MB0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3404,"ΤΕΜ",1,"GMC",1,"1FK22084AC000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC00-0SA0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3015,"ΤΕΜ",1,"GMC",1,"1FK22084AC000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC00-0SB0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3015,"ΤΕΜ",1,"GMC",1,"1FK22084AC000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC00-1MA0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3404,"ΤΕΜ",1,"GMC",1,"1FK22084AC001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC00-1MB0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3404,"ΤΕΜ",1,"GMC",1,"1FK22084AC001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC00-1SA0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3015,"ΤΕΜ",1,"GMC",1,"1FK22084AC001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC00-1SB0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3015,"ΤΕΜ",1,"GMC",1,"1FK22084AC001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC01-0MA0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3513,"ΤΕΜ",1,"GMC",1,"1FK22084AC010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC01-0MB0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3513,"ΤΕΜ",1,"GMC",1,"1FK22084AC010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC01-0SA0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3123,"ΤΕΜ",1,"GMC",1,"1FK22084AC010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC01-0SB0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3123,"ΤΕΜ",1,"GMC",1,"1FK22084AC010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC01-1MA0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3513,"ΤΕΜ",1,"GMC",1,"1FK22084AC011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC01-1MB0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3513,"ΤΕΜ",1,"GMC",1,"1FK22084AC011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC01-1SA0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3123,"ΤΕΜ",1,"GMC",1,"1FK22084AC011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC01-1SB0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3123,"ΤΕΜ",1,"GMC",1,"1FK22084AC011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC10-0MA0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3924,"ΤΕΜ",1,"GMC",1,"1FK22084AC100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC10-0MB0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3924,"ΤΕΜ",1,"GMC",1,"1FK22084AC100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC10-0SA0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3535,"ΤΕΜ",1,"GMC",1,"1FK22084AC100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC10-0SB0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3535,"ΤΕΜ",1,"GMC",1,"1FK22084AC100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC10-1MA0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3924,"ΤΕΜ",1,"GMC",1,"1FK22084AC101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC10-1MB0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3924,"ΤΕΜ",1,"GMC",1,"1FK22084AC101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC10-1SA0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3535,"ΤΕΜ",1,"GMC",1,"1FK22084AC101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC10-1SB0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3535,"ΤΕΜ",1,"GMC",1,"1FK22084AC101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC11-0MA0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4033,"ΤΕΜ",1,"GMC",1,"1FK22084AC110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC11-0MB0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4033,"ΤΕΜ",1,"GMC",1,"1FK22084AC110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC11-0SA0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3643,"ΤΕΜ",1,"GMC",1,"1FK22084AC110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC11-0SB0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3643,"ΤΕΜ",1,"GMC",1,"1FK22084AC110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC11-1MA0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4033,"ΤΕΜ",1,"GMC",1,"1FK22084AC111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC11-1MB0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4033,"ΤΕΜ",1,"GMC",1,"1FK22084AC111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC11-1SA0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3643,"ΤΕΜ",1,"GMC",1,"1FK22084AC111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-4AC11-1SB0","SIMOTICS S-1FK2 CT servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3643,"ΤΕΜ",1,"GMC",1,"1FK22084AC111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC00-0MA0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3793,"ΤΕΜ",1,"GMC",1,"1FK22085AC000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC00-0MB0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3793,"ΤΕΜ",1,"GMC",1,"1FK22085AC000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC00-0SA0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3404,"ΤΕΜ",1,"GMC",1,"1FK22085AC000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC00-0SB0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3404,"ΤΕΜ",1,"GMC",1,"1FK22085AC000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC00-1MA0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3793,"ΤΕΜ",1,"GMC",1,"1FK22085AC001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC00-1MB0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3793,"ΤΕΜ",1,"GMC",1,"1FK22085AC001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC00-1SA0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3404,"ΤΕΜ",1,"GMC",1,"1FK22085AC001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC00-1SB0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3404,"ΤΕΜ",1,"GMC",1,"1FK22085AC001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC01-0MA0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3902,"ΤΕΜ",1,"GMC",1,"1FK22085AC010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC01-0MB0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3902,"ΤΕΜ",1,"GMC",1,"1FK22085AC010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC01-0SA0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3513,"ΤΕΜ",1,"GMC",1,"1FK22085AC010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC01-0SB0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3513,"ΤΕΜ",1,"GMC",1,"1FK22085AC010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC01-1MA0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",3902,"ΤΕΜ",1,"GMC",1,"1FK22085AC011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC01-1MB0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3902,"ΤΕΜ",1,"GMC",1,"1FK22085AC011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC01-1SA0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3513,"ΤΕΜ",1,"GMC",1,"1FK22085AC011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC01-1SB0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3513,"ΤΕΜ",1,"GMC",1,"1FK22085AC011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC10-0MA0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4313,"ΤΕΜ",1,"GMC",1,"1FK22085AC100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC10-0MB0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4313,"ΤΕΜ",1,"GMC",1,"1FK22085AC100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC10-0SA0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3924,"ΤΕΜ",1,"GMC",1,"1FK22085AC100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC10-0SB0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3924,"ΤΕΜ",1,"GMC",1,"1FK22085AC100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC10-1MA0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4313,"ΤΕΜ",1,"GMC",1,"1FK22085AC101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC10-1MB0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4313,"ΤΕΜ",1,"GMC",1,"1FK22085AC101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC10-1SA0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3924,"ΤΕΜ",1,"GMC",1,"1FK22085AC101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC10-1SB0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3924,"ΤΕΜ",1,"GMC",1,"1FK22085AC101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC11-0MA0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4422,"ΤΕΜ",1,"GMC",1,"1FK22085AC110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC11-0MB0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4422,"ΤΕΜ",1,"GMC",1,"1FK22085AC110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC11-0SA0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",4033,"ΤΕΜ",1,"GMC",1,"1FK22085AC110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC11-0SB0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4033,"ΤΕΜ",1,"GMC",1,"1FK22085AC110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC11-1MA0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4422,"ΤΕΜ",1,"GMC",1,"1FK22085AC111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC11-1MB0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4422,"ΤΕΜ",1,"GMC",1,"1FK22085AC111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC11-1SA0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",4033,"ΤΕΜ",1,"GMC",1,"1FK22085AC111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2208-5AC11-1SB0","SIMOTICS S-1FK2 CT servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4033,"ΤΕΜ",1,"GMC",1,"1FK22085AC111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB00-0MA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4001,"ΤΕΜ",1,"GMC",1,"1FK22103AB000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB00-0MB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4001,"ΤΕΜ",1,"GMC",1,"1FK22103AB000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB00-0SA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3612,"ΤΕΜ",1,"GMC",1,"1FK22103AB000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB00-0SB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3612,"ΤΕΜ",1,"GMC",1,"1FK22103AB000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB00-1MA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4001,"ΤΕΜ",1,"GMC",1,"1FK22103AB001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB00-1MB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4001,"ΤΕΜ",1,"GMC",1,"1FK22103AB001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB00-1SA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3612,"ΤΕΜ",1,"GMC",1,"1FK22103AB001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB00-1SB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3612,"ΤΕΜ",1,"GMC",1,"1FK22103AB001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB01-0MA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4109,"ΤΕΜ",1,"GMC",1,"1FK22103AB010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB01-0MB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4109,"ΤΕΜ",1,"GMC",1,"1FK22103AB010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB01-0SA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3720,"ΤΕΜ",1,"GMC",1,"1FK22103AB010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB01-0SB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3720,"ΤΕΜ",1,"GMC",1,"1FK22103AB010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB01-1MA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4109,"ΤΕΜ",1,"GMC",1,"1FK22103AB011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB01-1MB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4109,"ΤΕΜ",1,"GMC",1,"1FK22103AB011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB01-1SA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3720,"ΤΕΜ",1,"GMC",1,"1FK22103AB011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB01-1SB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3720,"ΤΕΜ",1,"GMC",1,"1FK22103AB011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB10-0MA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4573,"ΤΕΜ",1,"GMC",1,"1FK22103AB100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB10-0MB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4573,"ΤΕΜ",1,"GMC",1,"1FK22103AB100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB10-0SA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",4184,"ΤΕΜ",1,"GMC",1,"1FK22103AB100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB10-0SB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4184,"ΤΕΜ",1,"GMC",1,"1FK22103AB100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB10-1MA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4573,"ΤΕΜ",1,"GMC",1,"1FK22103AB101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB10-1MB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4573,"ΤΕΜ",1,"GMC",1,"1FK22103AB101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB10-1SA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",4184,"ΤΕΜ",1,"GMC",1,"1FK22103AB101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB10-1SB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4184,"ΤΕΜ",1,"GMC",1,"1FK22103AB101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB11-0MA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4682,"ΤΕΜ",1,"GMC",1,"1FK22103AB110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB11-0MB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4682,"ΤΕΜ",1,"GMC",1,"1FK22103AB110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB11-0SA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",4292,"ΤΕΜ",1,"GMC",1,"1FK22103AB110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB11-0SB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4292,"ΤΕΜ",1,"GMC",1,"1FK22103AB110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB11-1MA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4682,"ΤΕΜ",1,"GMC",1,"1FK22103AB111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB11-1MB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4682,"ΤΕΜ",1,"GMC",1,"1FK22103AB111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB11-1SA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",4292,"ΤΕΜ",1,"GMC",1,"1FK22103AB111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AB11-1SB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4292,"ΤΕΜ",1,"GMC",1,"1FK22103AB111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC00-0MA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4001,"ΤΕΜ",1,"GMC",1,"1FK22103AC000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC00-0MB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4001,"ΤΕΜ",1,"GMC",1,"1FK22103AC000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC00-0SA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3612,"ΤΕΜ",1,"GMC",1,"1FK22103AC000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC00-0SB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3612,"ΤΕΜ",1,"GMC",1,"1FK22103AC000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC00-1MA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4001,"ΤΕΜ",1,"GMC",1,"1FK22103AC001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC00-1MB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4001,"ΤΕΜ",1,"GMC",1,"1FK22103AC001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC00-1SA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3612,"ΤΕΜ",1,"GMC",1,"1FK22103AC001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC00-1SB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3612,"ΤΕΜ",1,"GMC",1,"1FK22103AC001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC01-0MA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4109,"ΤΕΜ",1,"GMC",1,"1FK22103AC010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC01-0MB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4109,"ΤΕΜ",1,"GMC",1,"1FK22103AC010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC01-0SA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3720,"ΤΕΜ",1,"GMC",1,"1FK22103AC010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC01-0SB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3720,"ΤΕΜ",1,"GMC",1,"1FK22103AC010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC01-1MA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4109,"ΤΕΜ",1,"GMC",1,"1FK22103AC011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC01-1MB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4109,"ΤΕΜ",1,"GMC",1,"1FK22103AC011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC01-1SA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",3720,"ΤΕΜ",1,"GMC",1,"1FK22103AC011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC01-1SB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3720,"ΤΕΜ",1,"GMC",1,"1FK22103AC011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC10-0MA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4573,"ΤΕΜ",1,"GMC",1,"1FK22103AC100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC10-0MB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4573,"ΤΕΜ",1,"GMC",1,"1FK22103AC100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC10-0SA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",4184,"ΤΕΜ",1,"GMC",1,"1FK22103AC100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC10-0SB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4184,"ΤΕΜ",1,"GMC",1,"1FK22103AC100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC10-1MA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4573,"ΤΕΜ",1,"GMC",1,"1FK22103AC101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC10-1MB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4573,"ΤΕΜ",1,"GMC",1,"1FK22103AC101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC10-1SA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",4184,"ΤΕΜ",1,"GMC",1,"1FK22103AC101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC10-1SB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4184,"ΤΕΜ",1,"GMC",1,"1FK22103AC101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC11-0MA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4682,"ΤΕΜ",1,"GMC",1,"1FK22103AC110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC11-0MB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4682,"ΤΕΜ",1,"GMC",1,"1FK22103AC110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC11-0SA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",4292,"ΤΕΜ",1,"GMC",1,"1FK22103AC110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC11-0SB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4292,"ΤΕΜ",1,"GMC",1,"1FK22103AC110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC11-1MA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4682,"ΤΕΜ",1,"GMC",1,"1FK22103AC111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC11-1MB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4682,"ΤΕΜ",1,"GMC",1,"1FK22103AC111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC11-1SA0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",4292,"ΤΕΜ",1,"GMC",1,"1FK22103AC111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-3AC11-1SB0","SIMOTICS S-1FK2 CT servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4292,"ΤΕΜ",1,"GMC",1,"1FK22103AC111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB00-0MA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4811,"ΤΕΜ",1,"GMC",1,"1FK22104AB000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB00-0MB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4811,"ΤΕΜ",1,"GMC",1,"1FK22104AB000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB00-0SA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",4421,"ΤΕΜ",1,"GMC",1,"1FK22104AB000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB00-0SB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4421,"ΤΕΜ",1,"GMC",1,"1FK22104AB000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB00-1MA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4811,"ΤΕΜ",1,"GMC",1,"1FK22104AB001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB00-1MB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4811,"ΤΕΜ",1,"GMC",1,"1FK22104AB001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB00-1SA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",4421,"ΤΕΜ",1,"GMC",1,"1FK22104AB001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB00-1SB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4421,"ΤΕΜ",1,"GMC",1,"1FK22104AB001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB01-0MA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4919,"ΤΕΜ",1,"GMC",1,"1FK22104AB010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB01-0MB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4919,"ΤΕΜ",1,"GMC",1,"1FK22104AB010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB01-0SA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",4530,"ΤΕΜ",1,"GMC",1,"1FK22104AB010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB01-0SB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4530,"ΤΕΜ",1,"GMC",1,"1FK22104AB010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB01-1MA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4919,"ΤΕΜ",1,"GMC",1,"1FK22104AB011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB01-1MB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4919,"ΤΕΜ",1,"GMC",1,"1FK22104AB011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB01-1SA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",4530,"ΤΕΜ",1,"GMC",1,"1FK22104AB011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB01-1SB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4530,"ΤΕΜ",1,"GMC",1,"1FK22104AB011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB10-0MA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",5382,"ΤΕΜ",1,"GMC",1,"1FK22104AB100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB10-0MB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",5382,"ΤΕΜ",1,"GMC",1,"1FK22104AB100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB10-0SA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",4993,"ΤΕΜ",1,"GMC",1,"1FK22104AB100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB10-0SB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4993,"ΤΕΜ",1,"GMC",1,"1FK22104AB100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB10-1MA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",5382,"ΤΕΜ",1,"GMC",1,"1FK22104AB101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB10-1MB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",5382,"ΤΕΜ",1,"GMC",1,"1FK22104AB101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB10-1SA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",4993,"ΤΕΜ",1,"GMC",1,"1FK22104AB101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB10-1SB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4993,"ΤΕΜ",1,"GMC",1,"1FK22104AB101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB11-0MA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",5491,"ΤΕΜ",1,"GMC",1,"1FK22104AB110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB11-0MB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",5491,"ΤΕΜ",1,"GMC",1,"1FK22104AB110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB11-0SA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",5102,"ΤΕΜ",1,"GMC",1,"1FK22104AB110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB11-0SB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",5102,"ΤΕΜ",1,"GMC",1,"1FK22104AB110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB11-1MA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",5491,"ΤΕΜ",1,"GMC",1,"1FK22104AB111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB11-1MB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",5491,"ΤΕΜ",1,"GMC",1,"1FK22104AB111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB11-1SA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",5102,"ΤΕΜ",1,"GMC",1,"1FK22104AB111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AB11-1SB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",5102,"ΤΕΜ",1,"GMC",1,"1FK22104AB111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC00-0MA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4811,"ΤΕΜ",1,"GMC",1,"1FK22104AC000MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC00-0MB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4811,"ΤΕΜ",1,"GMC",1,"1FK22104AC000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC00-0SA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",4421,"ΤΕΜ",1,"GMC",1,"1FK22104AC000SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC00-0SB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4421,"ΤΕΜ",1,"GMC",1,"1FK22104AC000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC00-1MA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4811,"ΤΕΜ",1,"GMC",1,"1FK22104AC001MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC00-1MB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4811,"ΤΕΜ",1,"GMC",1,"1FK22104AC001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC00-1SA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",4421,"ΤΕΜ",1,"GMC",1,"1FK22104AC001SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC00-1SB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4421,"ΤΕΜ",1,"GMC",1,"1FK22104AC001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC01-0MA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4919,"ΤΕΜ",1,"GMC",1,"1FK22104AC010MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC01-0MB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4919,"ΤΕΜ",1,"GMC",1,"1FK22104AC010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC01-0SA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",4530,"ΤΕΜ",1,"GMC",1,"1FK22104AC010SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC01-0SB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4530,"ΤΕΜ",1,"GMC",1,"1FK22104AC010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC01-1MA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",4919,"ΤΕΜ",1,"GMC",1,"1FK22104AC011MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC01-1MB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4919,"ΤΕΜ",1,"GMC",1,"1FK22104AC011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC01-1SA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",4530,"ΤΕΜ",1,"GMC",1,"1FK22104AC011SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC01-1SB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4530,"ΤΕΜ",1,"GMC",1,"1FK22104AC011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC10-0MA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",5382,"ΤΕΜ",1,"GMC",1,"1FK22104AC100MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC10-0MB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",5382,"ΤΕΜ",1,"GMC",1,"1FK22104AC100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC10-0SA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",4993,"ΤΕΜ",1,"GMC",1,"1FK22104AC100SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC10-0SB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4993,"ΤΕΜ",1,"GMC",1,"1FK22104AC100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC10-1MA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",5382,"ΤΕΜ",1,"GMC",1,"1FK22104AC101MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC10-1MB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",5382,"ΤΕΜ",1,"GMC",1,"1FK22104AC101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC10-1SA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",4993,"ΤΕΜ",1,"GMC",1,"1FK22104AC101SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC10-1SB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4993,"ΤΕΜ",1,"GMC",1,"1FK22104AC101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC11-0MA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",5491,"ΤΕΜ",1,"GMC",1,"1FK22104AC110MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC11-0MB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",5491,"ΤΕΜ",1,"GMC",1,"1FK22104AC110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC11-0SA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",5102,"ΤΕΜ",1,"GMC",1,"1FK22104AC110SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC11-0SB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",5102,"ΤΕΜ",1,"GMC",1,"1FK22104AC110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC11-1MA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with OCC interface; plug size M23, rotatable;",5491,"ΤΕΜ",1,"GMC",1,"1FK22104AC111MA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC11-1MB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",5491,"ΤΕΜ",1,"GMC",1,"1FK22104AC111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC11-1SA0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; plug size M23, rotatable;",5102,"ΤΕΜ",1,"GMC",1,"1FK22104AC111SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-4AC11-1SB0","SIMOTICS S-1FK2 CT servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",5102,"ΤΕΜ",1,"GMC",1,"1FK22104AC111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-5AC00-0MB0","SIMOTICS S-1FK2 CT servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M40;",5601,"ΤΕΜ",1,"GMC",1,"1FK22105AC000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-5AC00-0SB0","SIMOTICS S-1FK2 CT servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M40;",5212,"ΤΕΜ",1,"GMC",1,"1FK22105AC000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-5AC00-1MB0","SIMOTICS S-1FK2 CT servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M40;",5601,"ΤΕΜ",1,"GMC",1,"1FK22105AC001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-5AC00-1SB0","SIMOTICS S-1FK2 CT servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M40;",5212,"ΤΕΜ",1,"GMC",1,"1FK22105AC001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-5AC01-0MB0","SIMOTICS S-1FK2 CT servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M40;",5710,"ΤΕΜ",1,"GMC",1,"1FK22105AC010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-5AC01-0SB0","SIMOTICS S-1FK2 CT servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M40;",5320,"ΤΕΜ",1,"GMC",1,"1FK22105AC010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-5AC01-1MB0","SIMOTICS S-1FK2 CT servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M40;",5710,"ΤΕΜ",1,"GMC",1,"1FK22105AC011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-5AC01-1SB0","SIMOTICS S-1FK2 CT servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M40;",5320,"ΤΕΜ",1,"GMC",1,"1FK22105AC011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-5AC10-0MB0","SIMOTICS S-1FK2 CT servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M40;",6173,"ΤΕΜ",1,"GMC",1,"1FK22105AC100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-5AC10-0SB0","SIMOTICS S-1FK2 CT servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M40;",5784,"ΤΕΜ",1,"GMC",1,"1FK22105AC100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-5AC10-1MB0","SIMOTICS S-1FK2 CT servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M40;",6173,"ΤΕΜ",1,"GMC",1,"1FK22105AC101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-5AC10-1SB0","SIMOTICS S-1FK2 CT servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP64; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M40;",5784,"ΤΕΜ",1,"GMC",1,"1FK22105AC101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-5AC11-0MB0","SIMOTICS S-1FK2 CT servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M40;",6282,"ΤΕΜ",1,"GMC",1,"1FK22105AC110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-5AC11-0SB0","SIMOTICS S-1FK2 CT servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; cylindrical shaft D38x80 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M40;",5893,"ΤΕΜ",1,"GMC",1,"1FK22105AC110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-5AC11-1MB0","SIMOTICS S-1FK2 CT servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M40;",6282,"ΤΕΜ",1,"GMC",1,"1FK22105AC111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2210-5AC11-1SB0","SIMOTICS S-1FK2 CT servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); with holding brake; degree of protection IP65; shaft D38x80 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M40;",5893,"ΤΕΜ",1,"GMC",1,"1FK22105AC111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-2AC00-0MB0","SIMOTICS S-1FK2 HI servo motor M0=6 Nm; PN = 1.15 kW at NN=2000 rpm, (380-480 V); degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2071,"ΤΕΜ",1,"GMC",1,"1FK23062AC000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-2AC00-0SB0","SIMOTICS S-1FK2 HI servo motor M0=6 Nm; PN = 1.15 kW at NN=2000 rpm, (380-480 V); degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",1682,"ΤΕΜ",1,"GMC",1,"1FK23062AC000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-2AC00-1MB0","SIMOTICS S-1FK2 HI servo motor M0=6 Nm; PN = 1.15 kW at NN=2000 rpm, (380-480 V); degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2071,"ΤΕΜ",1,"GMC",1,"1FK23062AC001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-2AC00-1SB0","SIMOTICS S-1FK2 HI servo motor M0=6 Nm; PN = 1.15 kW at NN=2000 rpm, (380-480 V); degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",1682,"ΤΕΜ",1,"GMC",1,"1FK23062AC001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-2AC01-0MB0","SIMOTICS S-1FK2 HI servo motor M0=6 Nm; PN = 1.15 kW at NN=2000 rpm, (380-480 V); degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2180,"ΤΕΜ",1,"GMC",1,"1FK23062AC010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-2AC01-0SB0","SIMOTICS S-1FK2 HI servo motor M0=6 Nm; PN = 1.15 kW at NN=2000 rpm, (380-480 V); degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",1791,"ΤΕΜ",1,"GMC",1,"1FK23062AC010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-2AC01-1MB0","SIMOTICS S-1FK2 HI servo motor M0=6 Nm; PN = 1.15 kW at NN=2000 rpm, (380-480 V); degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2180,"ΤΕΜ",1,"GMC",1,"1FK23062AC011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-2AC01-1SB0","SIMOTICS S-1FK2 HI servo motor M0=6 Nm; PN = 1.15 kW at NN=2000 rpm, (380-480 V); degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",1791,"ΤΕΜ",1,"GMC",1,"1FK23062AC011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-2AC10-0MB0","SIMOTICS S-1FK2 HI servo motor M0=6 Nm; PN = 1.15 kW at NN=2000 rpm, (380-480 V); with holding brake; degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2487,"ΤΕΜ",1,"GMC",1,"1FK23062AC100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-2AC10-0SB0","SIMOTICS S-1FK2 HI servo motor M0=6 Nm; PN = 1.15 kW at NN=2000 rpm, (380-480 V); with holding brake; degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2098,"ΤΕΜ",1,"GMC",1,"1FK23062AC100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-2AC10-1MB0","SIMOTICS S-1FK2 HI servo motor M0=6 Nm; PN = 1.15 kW at NN=2000 rpm, (380-480 V); with holding brake; degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2487,"ΤΕΜ",1,"GMC",1,"1FK23062AC101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-2AC10-1SB0","SIMOTICS S-1FK2 HI servo motor M0=6 Nm; PN = 1.15 kW at NN=2000 rpm, (380-480 V); with holding brake; degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2098,"ΤΕΜ",1,"GMC",1,"1FK23062AC101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-2AC11-0MB0","SIMOTICS S-1FK2 HI servo motor M0=6 Nm; PN = 1.15 kW at NN=2000 rpm, (380-480 V); with holding brake; degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2596,"ΤΕΜ",1,"GMC",1,"1FK23062AC110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-2AC11-0SB0","SIMOTICS S-1FK2 HI servo motor M0=6 Nm; PN = 1.15 kW at NN=2000 rpm, (380-480 V); with holding brake; degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2207,"ΤΕΜ",1,"GMC",1,"1FK23062AC110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-2AC11-1MB0","SIMOTICS S-1FK2 HI servo motor M0=6 Nm; PN = 1.15 kW at NN=2000 rpm, (380-480 V); with holding brake; degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2596,"ΤΕΜ",1,"GMC",1,"1FK23062AC111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-2AC11-1SB0","SIMOTICS S-1FK2 HI servo motor M0=6 Nm; PN = 1.15 kW at NN=2000 rpm, (380-480 V); with holding brake; degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2207,"ΤΕΜ",1,"GMC",1,"1FK23062AC111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-4AC00-0MB0","SIMOTICS S-1FK2 HI servo motor M0=12 Nm; PN = 2.2 kW at NN=2000 rpm, (380-480 V); degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2640,"ΤΕΜ",1,"GMC",1,"1FK23064AC000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-4AC00-0SB0","SIMOTICS S-1FK2 HI servo motor M0=12 Nm; PN = 2.2 kW at NN=2000 rpm, (380-480 V); degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2251,"ΤΕΜ",1,"GMC",1,"1FK23064AC000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-4AC00-1MB0","SIMOTICS S-1FK2 HI servo motor M0=12 Nm; PN = 2.2 kW at NN=2000 rpm, (380-480 V); degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2640,"ΤΕΜ",1,"GMC",1,"1FK23064AC001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-4AC00-1SB0","SIMOTICS S-1FK2 HI servo motor M0=12 Nm; PN = 2.2 kW at NN=2000 rpm, (380-480 V); degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2251,"ΤΕΜ",1,"GMC",1,"1FK23064AC001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-4AC01-0MB0","SIMOTICS S-1FK2 HI servo motor M0=12 Nm; PN = 2.2 kW at NN=2000 rpm, (380-480 V); degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2749,"ΤΕΜ",1,"GMC",1,"1FK23064AC010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-4AC01-0SB0","SIMOTICS S-1FK2 HI servo motor M0=12 Nm; PN = 2.2 kW at NN=2000 rpm, (380-480 V); degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2360,"ΤΕΜ",1,"GMC",1,"1FK23064AC010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-4AC01-1MB0","SIMOTICS S-1FK2 HI servo motor M0=12 Nm; PN = 2.2 kW at NN=2000 rpm, (380-480 V); degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2749,"ΤΕΜ",1,"GMC",1,"1FK23064AC011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-4AC01-1SB0","SIMOTICS S-1FK2 HI servo motor M0=12 Nm; PN = 2.2 kW at NN=2000 rpm, (380-480 V); degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2360,"ΤΕΜ",1,"GMC",1,"1FK23064AC011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-4AC10-0MB0","SIMOTICS S-1FK2 HI servo motor M0=12 Nm; PN = 2.2 kW at NN=2000 rpm, (380-480 V); with holding brake; degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3056,"ΤΕΜ",1,"GMC",1,"1FK23064AC100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-4AC10-0SB0","SIMOTICS S-1FK2 HI servo motor M0=12 Nm; PN = 2.2 kW at NN=2000 rpm, (380-480 V); with holding brake; degree of protection IP64; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2667,"ΤΕΜ",1,"GMC",1,"1FK23064AC100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-4AC10-1MB0","SIMOTICS S-1FK2 HI servo motor M0=12 Nm; PN = 2.2 kW at NN=2000 rpm, (380-480 V); with holding brake; degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3056,"ΤΕΜ",1,"GMC",1,"1FK23064AC101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-4AC10-1SB0","SIMOTICS S-1FK2 HI servo motor M0=12 Nm; PN = 2.2 kW at NN=2000 rpm, (380-480 V); with holding brake; degree of protection IP64; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2667,"ΤΕΜ",1,"GMC",1,"1FK23064AC101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-4AC11-0MB0","SIMOTICS S-1FK2 HI servo motor M0=12 Nm; PN = 2.2 kW at NN=2000 rpm, (380-480 V); with holding brake; degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3165,"ΤΕΜ",1,"GMC",1,"1FK23064AC110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-4AC11-0SB0","SIMOTICS S-1FK2 HI servo motor M0=12 Nm; PN = 2.2 kW at NN=2000 rpm, (380-480 V); with holding brake; degree of protection IP65; cylindrical shaft D24x50 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2776,"ΤΕΜ",1,"GMC",1,"1FK23064AC110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-4AC11-1MB0","SIMOTICS S-1FK2 HI servo motor M0=12 Nm; PN = 2.2 kW at NN=2000 rpm, (380-480 V); with holding brake; degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3165,"ΤΕΜ",1,"GMC",1,"1FK23064AC111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2306-4AC11-1SB0","SIMOTICS S-1FK2 HI servo motor M0=12 Nm; PN = 2.2 kW at NN=2000 rpm, (380-480 V); with holding brake; degree of protection IP65; shaft D24x50 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2776,"ΤΕΜ",1,"GMC",1,"1FK23064AC111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-3AB00-0MB0","SIMOTICS S-1FK2 HI servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3094,"ΤΕΜ",1,"GMC",1,"1FK23083AB000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-3AB00-0SB0","SIMOTICS S-1FK2 HI servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2705,"ΤΕΜ",1,"GMC",1,"1FK23083AB000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-3AB00-1MB0","SIMOTICS S-1FK2 HI servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3094,"ΤΕΜ",1,"GMC",1,"1FK23083AB001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-3AB00-1SB0","SIMOTICS S-1FK2 HI servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2705,"ΤΕΜ",1,"GMC",1,"1FK23083AB001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-3AB01-0MB0","SIMOTICS S-1FK2 HI servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3203,"ΤΕΜ",1,"GMC",1,"1FK23083AB010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-3AB01-0SB0","SIMOTICS S-1FK2 HI servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2814,"ΤΕΜ",1,"GMC",1,"1FK23083AB010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-3AB01-1MB0","SIMOTICS S-1FK2 HI servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3203,"ΤΕΜ",1,"GMC",1,"1FK23083AB011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-3AB01-1SB0","SIMOTICS S-1FK2 HI servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",2814,"ΤΕΜ",1,"GMC",1,"1FK23083AB011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-3AB10-0MB0","SIMOTICS S-1FK2 HI servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); with holding brake; degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3614,"ΤΕΜ",1,"GMC",1,"1FK23083AB100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-3AB10-0SB0","SIMOTICS S-1FK2 HI servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); with holding brake; degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3225,"ΤΕΜ",1,"GMC",1,"1FK23083AB100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-3AB10-1MB0","SIMOTICS S-1FK2 HI servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); with holding brake; degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3614,"ΤΕΜ",1,"GMC",1,"1FK23083AB101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-3AB10-1SB0","SIMOTICS S-1FK2 HI servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); with holding brake; degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3225,"ΤΕΜ",1,"GMC",1,"1FK23083AB101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-3AB11-0MB0","SIMOTICS S-1FK2 HI servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); with holding brake; degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3723,"ΤΕΜ",1,"GMC",1,"1FK23083AB110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-3AB11-0SB0","SIMOTICS S-1FK2 HI servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); with holding brake; degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3334,"ΤΕΜ",1,"GMC",1,"1FK23083AB110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-3AB11-1MB0","SIMOTICS S-1FK2 HI servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); with holding brake; degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3723,"ΤΕΜ",1,"GMC",1,"1FK23083AB111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-3AB11-1SB0","SIMOTICS S-1FK2 HI servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); with holding brake; degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3334,"ΤΕΜ",1,"GMC",1,"1FK23083AB111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-4AB00-0MB0","SIMOTICS S-1FK2 HI servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3404,"ΤΕΜ",1,"GMC",1,"1FK23084AB000MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-4AB00-0SB0","SIMOTICS S-1FK2 HI servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3015,"ΤΕΜ",1,"GMC",1,"1FK23084AB000SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-4AB00-1MB0","SIMOTICS S-1FK2 HI servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3404,"ΤΕΜ",1,"GMC",1,"1FK23084AB001MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-4AB00-1SB0","SIMOTICS S-1FK2 HI servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3015,"ΤΕΜ",1,"GMC",1,"1FK23084AB001SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-4AB01-0MB0","SIMOTICS S-1FK2 HI servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3513,"ΤΕΜ",1,"GMC",1,"1FK23084AB010MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-4AB01-0SB0","SIMOTICS S-1FK2 HI servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3123,"ΤΕΜ",1,"GMC",1,"1FK23084AB010SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-4AB01-1MB0","SIMOTICS S-1FK2 HI servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3513,"ΤΕΜ",1,"GMC",1,"1FK23084AB011MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-4AB01-1SB0","SIMOTICS S-1FK2 HI servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3123,"ΤΕΜ",1,"GMC",1,"1FK23084AB011SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-4AB10-0MB0","SIMOTICS S-1FK2 HI servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); with holding brake; degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3924,"ΤΕΜ",1,"GMC",1,"1FK23084AB100MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-4AB10-0SB0","SIMOTICS S-1FK2 HI servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); with holding brake; degree of protection IP64; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3535,"ΤΕΜ",1,"GMC",1,"1FK23084AB100SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-4AB10-1MB0","SIMOTICS S-1FK2 HI servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); with holding brake; degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3924,"ΤΕΜ",1,"GMC",1,"1FK23084AB101MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-4AB10-1SB0","SIMOTICS S-1FK2 HI servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); with holding brake; degree of protection IP64; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3535,"ΤΕΜ",1,"GMC",1,"1FK23084AB101SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-4AB11-0MB0","SIMOTICS S-1FK2 HI servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); with holding brake; degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4033,"ΤΕΜ",1,"GMC",1,"1FK23084AB110MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-4AB11-0SB0","SIMOTICS S-1FK2 HI servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); with holding brake; degree of protection IP65; cylindrical shaft D32x58 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3643,"ΤΕΜ",1,"GMC",1,"1FK23084AB110SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-4AB11-1MB0","SIMOTICS S-1FK2 HI servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); with holding brake; degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder 22-bit + 12-bit multiturn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",4033,"ΤΕΜ",1,"GMC",1,"1FK23084AB111MB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK2308-4AB11-1SB0","SIMOTICS S-1FK2 HI servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); with holding brake; degree of protection IP65; shaft D32x58 mm with feather key; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M23;",3643,"ΤΕΜ",1,"GMC",1,"1FK23084AB111SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK24-1AA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1826,"ΤΕΜ",1,"GMC",1,"1FK70115AK241AA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK24-1AB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",2146,"ΤΕΜ",1,"GMC",1,"1FK70115AK241AB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK24-1AG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1765,"ΤΕΜ",1,"GMC",1,"1FK70115AK241AG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK24-1AH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",2017,"ΤΕΜ",1,"GMC",1,"1FK70115AK241AH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK24-1JA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor absolute encoder 16 S/R (encoder A-16); derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1635,"ΤΕΜ",1,"GMC",1,"1FK70115AK241JA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK24-1JB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor absolute encoder 16 S/R (encoder A-16); derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1955,"ΤΕΜ",1,"GMC",1,"1FK70115AK241JB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK24-1JG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor absolute encoder 16 S/R (encoder A-16); derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1574,"ΤΕΜ",1,"GMC",1,"1FK70115AK241JG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK24-1JH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor absolute encoder 16 S/R (encoder A-16); derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1826,"ΤΕΜ",1,"GMC",1,"1FK70115AK241JH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK24-1SA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",994,"ΤΕΜ",1,"GMC",1,"1FK70115AK241SA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK24-1SB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1313,"ΤΕΜ",1,"GMC",1,"1FK70115AK241SB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK24-1SG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",932,"ΤΕΜ",1,"GMC",1,"1FK70115AK241SG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK24-1SH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1184,"ΤΕΜ",1,"GMC",1,"1FK70115AK241SH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK24-1TA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",994,"ΤΕΜ",1,"GMC",1,"1FK70115AK241TA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK24-1TB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1313,"ΤΕΜ",1,"GMC",1,"1FK70115AK241TB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK24-1TG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",932,"ΤΕΜ",1,"GMC",1,"1FK70115AK241TG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK24-1TH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1184,"ΤΕΜ",1,"GMC",1,"1FK70115AK241TH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK74-1AA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1826,"ΤΕΜ",1,"GMC",1,"1FK70115AK741AA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK74-1AB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",2146,"ΤΕΜ",1,"GMC",1,"1FK70115AK741AB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK74-1AG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1765,"ΤΕΜ",1,"GMC",1,"1FK70115AK741AG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK74-1AH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",2017,"ΤΕΜ",1,"GMC",1,"1FK70115AK741AH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK74-1JA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor absolute encoder 16 S/R (encoder A-16); derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1635,"ΤΕΜ",1,"GMC",1,"1FK70115AK741JA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK74-1JB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor absolute encoder 16 S/R (encoder A-16); derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1955,"ΤΕΜ",1,"GMC",1,"1FK70115AK741JB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK74-1JG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor absolute encoder 16 S/R (encoder A-16); derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1574,"ΤΕΜ",1,"GMC",1,"1FK70115AK741JG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK74-1JH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor absolute encoder 16 S/R (encoder A-16); derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1826,"ΤΕΜ",1,"GMC",1,"1FK70115AK741JH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK74-1SA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",994,"ΤΕΜ",1,"GMC",1,"1FK70115AK741SA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK74-1SB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1313,"ΤΕΜ",1,"GMC",1,"1FK70115AK741SB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK74-1SG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",932,"ΤΕΜ",1,"GMC",1,"1FK70115AK741SG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK74-1SH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1184,"ΤΕΜ",1,"GMC",1,"1FK70115AK741SH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK74-1TA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",994,"ΤΕΜ",1,"GMC",1,"1FK70115AK741TA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK74-1TB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1313,"ΤΕΜ",1,"GMC",1,"1FK70115AK741TB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK74-1TG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",932,"ΤΕΜ",1,"GMC",1,"1FK70115AK741TG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7011-5AK74-1TH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1184,"ΤΕΜ",1,"GMC",1,"1FK70115AK741TH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK24-1AA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1943,"ΤΕΜ",1,"GMC",1,"1FK70155AK241AA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK24-1AB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",2263,"ΤΕΜ",1,"GMC",1,"1FK70155AK241AB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK24-1AG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1882,"ΤΕΜ",1,"GMC",1,"1FK70155AK241AG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK24-1AH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",2134,"ΤΕΜ",1,"GMC",1,"1FK70155AK241AH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK24-1JA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor absolute encoder 16 S/R (encoder A-16); derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1753,"ΤΕΜ",1,"GMC",1,"1FK70155AK241JA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK24-1JB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor absolute encoder 16 S/R (encoder A-16); derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",2072,"ΤΕΜ",1,"GMC",1,"1FK70155AK241JB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK24-1JG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor absolute encoder 16 S/R (encoder A-16); derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1691,"ΤΕΜ",1,"GMC",1,"1FK70155AK241JG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK24-1JH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor absolute encoder 16 S/R (encoder A-16); derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1943,"ΤΕΜ",1,"GMC",1,"1FK70155AK241JH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK24-1SA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1111,"ΤΕΜ",1,"GMC",1,"1FK70155AK241SA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK24-1SB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1431,"ΤΕΜ",1,"GMC",1,"1FK70155AK241SB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK24-1SG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1049,"ΤΕΜ",1,"GMC",1,"1FK70155AK241SG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK24-1SH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1301,"ΤΕΜ",1,"GMC",1,"1FK70155AK241SH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK24-1TA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1111,"ΤΕΜ",1,"GMC",1,"1FK70155AK241TA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK24-1TB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1431,"ΤΕΜ",1,"GMC",1,"1FK70155AK241TB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK24-1TG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1049,"ΤΕΜ",1,"GMC",1,"1FK70155AK241TG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK24-1TH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1301,"ΤΕΜ",1,"GMC",1,"1FK70155AK241TH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK74-1AA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1943,"ΤΕΜ",1,"GMC",1,"1FK70155AK741AA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK74-1AB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",2263,"ΤΕΜ",1,"GMC",1,"1FK70155AK741AB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK74-1AG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1882,"ΤΕΜ",1,"GMC",1,"1FK70155AK741AG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK74-1AH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",2134,"ΤΕΜ",1,"GMC",1,"1FK70155AK741AH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK74-1JA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor absolute encoder 16 S/R (encoder A-16); derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1753,"ΤΕΜ",1,"GMC",1,"1FK70155AK741JA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK74-1JB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor absolute encoder 16 S/R (encoder A-16); derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",2072,"ΤΕΜ",1,"GMC",1,"1FK70155AK741JB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK74-1JG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor absolute encoder 16 S/R (encoder A-16); derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1691,"ΤΕΜ",1,"GMC",1,"1FK70155AK741JG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK74-1JH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor absolute encoder 16 S/R (encoder A-16); derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1943,"ΤΕΜ",1,"GMC",1,"1FK70155AK741JH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK74-1SA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1111,"ΤΕΜ",1,"GMC",1,"1FK70155AK741SA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK74-1SB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1431,"ΤΕΜ",1,"GMC",1,"1FK70155AK741SB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK74-1SG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1049,"ΤΕΜ",1,"GMC",1,"1FK70155AK741SG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK74-1SH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1301,"ΤΕΜ",1,"GMC",1,"1FK70155AK741SH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK74-1TA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1111,"ΤΕΜ",1,"GMC",1,"1FK70155AK741TA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK74-1TB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1431,"ΤΕΜ",1,"GMC",1,"1FK70155AK741TB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK74-1TG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1049,"ΤΕΜ",1,"GMC",1,"1FK70155AK741TG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7015-5AK74-1TH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1301,"ΤΕΜ",1,"GMC",1,"1FK70155AK741TH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1DA0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2618,"ΤΕΜ",1,"GMC",1,"1FK70225AK211DA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1DA2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2755,"ΤΕΜ",1,"GMC",1,"1FK70225AK211DA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1DA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2685,"ΤΕΜ",1,"GMC",1,"1FK70225AK211DA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1DA5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2821,"ΤΕΜ",1,"GMC",1,"1FK70225AK211DA5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1DA8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2967,"ΤΕΜ",1,"GMC",1,"1FK70225AK211DA8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1DB0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2938,"ΤΕΜ",1,"GMC",1,"1FK70225AK211DB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1DB2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",3075,"ΤΕΜ",1,"GMC",1,"1FK70225AK211DB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1DB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",3004,"ΤΕΜ",1,"GMC",1,"1FK70225AK211DB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1DB5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",3141,"ΤΕΜ",1,"GMC",1,"1FK70225AK211DB5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1DB8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3287,"ΤΕΜ",1,"GMC",1,"1FK70225AK211DB8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1DG0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2492,"ΤΕΜ",1,"GMC",1,"1FK70225AK211DG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1DG2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2629,"ΤΕΜ",1,"GMC",1,"1FK70225AK211DG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1DG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2559,"ΤΕΜ",1,"GMC",1,"1FK70225AK211DG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1DG5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2695,"ΤΕΜ",1,"GMC",1,"1FK70225AK211DG5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1DG8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2841,"ΤΕΜ",1,"GMC",1,"1FK70225AK211DG8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1DH0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2809,"ΤΕΜ",1,"GMC",1,"1FK70225AK211DH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1DH2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2945,"ΤΕΜ",1,"GMC",1,"1FK70225AK211DH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1DH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2875,"ΤΕΜ",1,"GMC",1,"1FK70225AK211DH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1DH5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",3012,"ΤΕΜ",1,"GMC",1,"1FK70225AK211DH5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1DH8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3158,"ΤΕΜ",1,"GMC",1,"1FK70225AK211DH8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1LA0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",3158,"ΤΕΜ",1,"GMC",1,"1FK70225AK211LA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1LA2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",3294,"ΤΕΜ",1,"GMC",1,"1FK70225AK211LA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1LA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",3224,"ΤΕΜ",1,"GMC",1,"1FK70225AK211LA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1LA5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",3361,"ΤΕΜ",1,"GMC",1,"1FK70225AK211LA5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1LA8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3507,"ΤΕΜ",1,"GMC",1,"1FK70225AK211LA8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1LB0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",3478,"ΤΕΜ",1,"GMC",1,"1FK70225AK211LB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1LB2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",3614,"ΤΕΜ",1,"GMC",1,"1FK70225AK211LB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1LB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",3544,"ΤΕΜ",1,"GMC",1,"1FK70225AK211LB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1LB5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",3681,"ΤΕΜ",1,"GMC",1,"1FK70225AK211LB5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1LB8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3826,"ΤΕΜ",1,"GMC",1,"1FK70225AK211LB8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1LG0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",3032,"ΤΕΜ",1,"GMC",1,"1FK70225AK211LG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1LG2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",3169,"ΤΕΜ",1,"GMC",1,"1FK70225AK211LG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1LG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",3098,"ΤΕΜ",1,"GMC",1,"1FK70225AK211LG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1LG5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",3235,"ΤΕΜ",1,"GMC",1,"1FK70225AK211LG5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1LG8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3381,"ΤΕΜ",1,"GMC",1,"1FK70225AK211LG8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1LH0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",3348,"ΤΕΜ",1,"GMC",1,"1FK70225AK211LH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1LH2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",3485,"ΤΕΜ",1,"GMC",1,"1FK70225AK211LH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1LH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",3414,"ΤΕΜ",1,"GMC",1,"1FK70225AK211LH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1LH5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",3551,"ΤΕΜ",1,"GMC",1,"1FK70225AK211LH5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1LH8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3697,"ΤΕΜ",1,"GMC",1,"1FK70225AK211LH8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1PA0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1762,"ΤΕΜ",1,"GMC",1,"1FK70225AK211PA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1PA2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1899,"ΤΕΜ",1,"GMC",1,"1FK70225AK211PA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1PA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1829,"ΤΕΜ",1,"GMC",1,"1FK70225AK211PA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1PA5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1965,"ΤΕΜ",1,"GMC",1,"1FK70225AK211PA5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1PA8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2111,"ΤΕΜ",1,"GMC",1,"1FK70225AK211PA8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1PB0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2082,"ΤΕΜ",1,"GMC",1,"1FK70225AK211PB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1PB2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2219,"ΤΕΜ",1,"GMC",1,"1FK70225AK211PB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1PB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2148,"ΤΕΜ",1,"GMC",1,"1FK70225AK211PB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1PB5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2285,"ΤΕΜ",1,"GMC",1,"1FK70225AK211PB5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1PB8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2431,"ΤΕΜ",1,"GMC",1,"1FK70225AK211PB8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1PG0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1636,"ΤΕΜ",1,"GMC",1,"1FK70225AK211PG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1PG2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1773,"ΤΕΜ",1,"GMC",1,"1FK70225AK211PG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1PG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1703,"ΤΕΜ",1,"GMC",1,"1FK70225AK211PG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1PG5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1839,"ΤΕΜ",1,"GMC",1,"1FK70225AK211PG5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1PG8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1985,"ΤΕΜ",1,"GMC",1,"1FK70225AK211PG8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1PH0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1953,"ΤΕΜ",1,"GMC",1,"1FK70225AK211PH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1PH2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2089,"ΤΕΜ",1,"GMC",1,"1FK70225AK211PH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1PH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2019,"ΤΕΜ",1,"GMC",1,"1FK70225AK211PH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1PH5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2156,"ΤΕΜ",1,"GMC",1,"1FK70225AK211PH5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1PH8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2302,"ΤΕΜ",1,"GMC",1,"1FK70225AK211PH8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1UA0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1720,"ΤΕΜ",1,"GMC",1,"1FK70225AK211UA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1UA2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1857,"ΤΕΜ",1,"GMC",1,"1FK70225AK211UA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1UA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1787,"ΤΕΜ",1,"GMC",1,"1FK70225AK211UA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1UA5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1923,"ΤΕΜ",1,"GMC",1,"1FK70225AK211UA5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1UA8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2069,"ΤΕΜ",1,"GMC",1,"1FK70225AK211UA8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1UB0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2040,"ΤΕΜ",1,"GMC",1,"1FK70225AK211UB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1UB2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2177,"ΤΕΜ",1,"GMC",1,"1FK70225AK211UB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1UB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2106,"ΤΕΜ",1,"GMC",1,"1FK70225AK211UB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1UB5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2243,"ΤΕΜ",1,"GMC",1,"1FK70225AK211UB5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1UB8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2389,"ΤΕΜ",1,"GMC",1,"1FK70225AK211UB8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1UG0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1594,"ΤΕΜ",1,"GMC",1,"1FK70225AK211UG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1UG2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1731,"ΤΕΜ",1,"GMC",1,"1FK70225AK211UG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1UG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1661,"ΤΕΜ",1,"GMC",1,"1FK70225AK211UG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1UG5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1797,"ΤΕΜ",1,"GMC",1,"1FK70225AK211UG5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1UG8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1943,"ΤΕΜ",1,"GMC",1,"1FK70225AK211UG8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1UH0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1911,"ΤΕΜ",1,"GMC",1,"1FK70225AK211UH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1UH2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2047,"ΤΕΜ",1,"GMC",1,"1FK70225AK211UH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1UH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1977,"ΤΕΜ",1,"GMC",1,"1FK70225AK211UH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1UH5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2114,"ΤΕΜ",1,"GMC",1,"1FK70225AK211UH5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK21-1UH8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2260,"ΤΕΜ",1,"GMC",1,"1FK70225AK211UH8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK24-1AA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2309,"ΤΕΜ",1,"GMC",1,"1FK70225AK241AA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK24-1AA5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2446,"ΤΕΜ",1,"GMC",1,"1FK70225AK241AA5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK24-1AB0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2563,"ΤΕΜ",1,"GMC",1,"1FK70225AK241AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1DA0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2618,"ΤΕΜ",1,"GMC",1,"1FK70225AK711DA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1DA2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2755,"ΤΕΜ",1,"GMC",1,"1FK70225AK711DA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1DA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2685,"ΤΕΜ",1,"GMC",1,"1FK70225AK711DA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1DA5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2821,"ΤΕΜ",1,"GMC",1,"1FK70225AK711DA5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1DA8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2967,"ΤΕΜ",1,"GMC",1,"1FK70225AK711DA8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1DB0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2938,"ΤΕΜ",1,"GMC",1,"1FK70225AK711DB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1DB2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",3075,"ΤΕΜ",1,"GMC",1,"1FK70225AK711DB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1DB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",3004,"ΤΕΜ",1,"GMC",1,"1FK70225AK711DB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1DB5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",3141,"ΤΕΜ",1,"GMC",1,"1FK70225AK711DB5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1DB8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3287,"ΤΕΜ",1,"GMC",1,"1FK70225AK711DB8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1DG0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2492,"ΤΕΜ",1,"GMC",1,"1FK70225AK711DG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1DG2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2629,"ΤΕΜ",1,"GMC",1,"1FK70225AK711DG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1DG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2559,"ΤΕΜ",1,"GMC",1,"1FK70225AK711DG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1DG5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2695,"ΤΕΜ",1,"GMC",1,"1FK70225AK711DG5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1DG8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2841,"ΤΕΜ",1,"GMC",1,"1FK70225AK711DG8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1DH0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2809,"ΤΕΜ",1,"GMC",1,"1FK70225AK711DH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1DH2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2945,"ΤΕΜ",1,"GMC",1,"1FK70225AK711DH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1DH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2875,"ΤΕΜ",1,"GMC",1,"1FK70225AK711DH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1DH5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",3012,"ΤΕΜ",1,"GMC",1,"1FK70225AK711DH5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1DH8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3158,"ΤΕΜ",1,"GMC",1,"1FK70225AK711DH8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1LA0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",3158,"ΤΕΜ",1,"GMC",1,"1FK70225AK711LA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1LA2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",3294,"ΤΕΜ",1,"GMC",1,"1FK70225AK711LA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1LA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",3224,"ΤΕΜ",1,"GMC",1,"1FK70225AK711LA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1LA5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",3361,"ΤΕΜ",1,"GMC",1,"1FK70225AK711LA5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1LA8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3507,"ΤΕΜ",1,"GMC",1,"1FK70225AK711LA8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1LB0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",3478,"ΤΕΜ",1,"GMC",1,"1FK70225AK711LB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1LB2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",3614,"ΤΕΜ",1,"GMC",1,"1FK70225AK711LB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1LB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",3544,"ΤΕΜ",1,"GMC",1,"1FK70225AK711LB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1LB5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",3681,"ΤΕΜ",1,"GMC",1,"1FK70225AK711LB5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1LB8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3826,"ΤΕΜ",1,"GMC",1,"1FK70225AK711LB8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1LG0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",3032,"ΤΕΜ",1,"GMC",1,"1FK70225AK711LG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1LG2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",3169,"ΤΕΜ",1,"GMC",1,"1FK70225AK711LG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1LG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",3098,"ΤΕΜ",1,"GMC",1,"1FK70225AK711LG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1LG5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",3235,"ΤΕΜ",1,"GMC",1,"1FK70225AK711LG5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1LG8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3381,"ΤΕΜ",1,"GMC",1,"1FK70225AK711LG8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1LH0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",3348,"ΤΕΜ",1,"GMC",1,"1FK70225AK711LH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1LH2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",3485,"ΤΕΜ",1,"GMC",1,"1FK70225AK711LH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1LH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",3414,"ΤΕΜ",1,"GMC",1,"1FK70225AK711LH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1LH5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",3551,"ΤΕΜ",1,"GMC",1,"1FK70225AK711LH5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1LH8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3697,"ΤΕΜ",1,"GMC",1,"1FK70225AK711LH8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1PA0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1762,"ΤΕΜ",1,"GMC",1,"1FK70225AK711PA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1PA2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1899,"ΤΕΜ",1,"GMC",1,"1FK70225AK711PA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1PA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1829,"ΤΕΜ",1,"GMC",1,"1FK70225AK711PA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1PA5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1965,"ΤΕΜ",1,"GMC",1,"1FK70225AK711PA5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1PA8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2111,"ΤΕΜ",1,"GMC",1,"1FK70225AK711PA8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1PB0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2082,"ΤΕΜ",1,"GMC",1,"1FK70225AK711PB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1PB2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2219,"ΤΕΜ",1,"GMC",1,"1FK70225AK711PB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1PB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2148,"ΤΕΜ",1,"GMC",1,"1FK70225AK711PB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1PB5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2285,"ΤΕΜ",1,"GMC",1,"1FK70225AK711PB5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1PB8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2431,"ΤΕΜ",1,"GMC",1,"1FK70225AK711PB8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1PG0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1636,"ΤΕΜ",1,"GMC",1,"1FK70225AK711PG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1PG2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1773,"ΤΕΜ",1,"GMC",1,"1FK70225AK711PG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1PG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1703,"ΤΕΜ",1,"GMC",1,"1FK70225AK711PG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1PG5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1839,"ΤΕΜ",1,"GMC",1,"1FK70225AK711PG5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1PG8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1985,"ΤΕΜ",1,"GMC",1,"1FK70225AK711PG8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1PH0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1953,"ΤΕΜ",1,"GMC",1,"1FK70225AK711PH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1PH2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2089,"ΤΕΜ",1,"GMC",1,"1FK70225AK711PH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1PH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2019,"ΤΕΜ",1,"GMC",1,"1FK70225AK711PH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1PH5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2156,"ΤΕΜ",1,"GMC",1,"1FK70225AK711PH5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1PH8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2302,"ΤΕΜ",1,"GMC",1,"1FK70225AK711PH8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1UA0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1762,"ΤΕΜ",1,"GMC",1,"1FK70225AK711UA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1UA2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1899,"ΤΕΜ",1,"GMC",1,"1FK70225AK711UA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1UA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1829,"ΤΕΜ",1,"GMC",1,"1FK70225AK711UA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1UA5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1965,"ΤΕΜ",1,"GMC",1,"1FK70225AK711UA5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1UA8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2111,"ΤΕΜ",1,"GMC",1,"1FK70225AK711UA8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1UB0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2082,"ΤΕΜ",1,"GMC",1,"1FK70225AK711UB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1UB2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2219,"ΤΕΜ",1,"GMC",1,"1FK70225AK711UB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1UB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2148,"ΤΕΜ",1,"GMC",1,"1FK70225AK711UB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1UB5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2285,"ΤΕΜ",1,"GMC",1,"1FK70225AK711UB5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1UB8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2431,"ΤΕΜ",1,"GMC",1,"1FK70225AK711UB8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1UG0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1636,"ΤΕΜ",1,"GMC",1,"1FK70225AK711UG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1UG2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1773,"ΤΕΜ",1,"GMC",1,"1FK70225AK711UG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1UG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1703,"ΤΕΜ",1,"GMC",1,"1FK70225AK711UG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1UG5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1839,"ΤΕΜ",1,"GMC",1,"1FK70225AK711UG5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1UG8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1985,"ΤΕΜ",1,"GMC",1,"1FK70225AK711UG8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1UH0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1953,"ΤΕΜ",1,"GMC",1,"1FK70225AK711UH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1UH2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2089,"ΤΕΜ",1,"GMC",1,"1FK70225AK711UH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1UH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2019,"ΤΕΜ",1,"GMC",1,"1FK70225AK711UH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1UH5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2156,"ΤΕΜ",1,"GMC",1,"1FK70225AK711UH5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK71-1UH8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2302,"ΤΕΜ",1,"GMC",1,"1FK70225AK711UH8","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1AA0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2243,"ΤΕΜ",1,"GMC",1,"1FK70225AK741AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1AA2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2379,"ΤΕΜ",1,"GMC",1,"1FK70225AK741AA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1AA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2309,"ΤΕΜ",1,"GMC",1,"1FK70225AK741AA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1AA5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2446,"ΤΕΜ",1,"GMC",1,"1FK70225AK741AA5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1AB0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2563,"ΤΕΜ",1,"GMC",1,"1FK70225AK741AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1AB2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2699,"ΤΕΜ",1,"GMC",1,"1FK70225AK741AB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1AB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2629,"ΤΕΜ",1,"GMC",1,"1FK70225AK741AB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1AB5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2765,"ΤΕΜ",1,"GMC",1,"1FK70225AK741AB5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1AG0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2117,"ΤΕΜ",1,"GMC",1,"1FK70225AK741AG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1AG2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2253,"ΤΕΜ",1,"GMC",1,"1FK70225AK741AG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1AG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2183,"ΤΕΜ",1,"GMC",1,"1FK70225AK741AG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1AG5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2320,"ΤΕΜ",1,"GMC",1,"1FK70225AK741AG5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1AH0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2433,"ΤΕΜ",1,"GMC",1,"1FK70225AK741AH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1AH2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2570,"ΤΕΜ",1,"GMC",1,"1FK70225AK741AH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1AH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2499,"ΤΕΜ",1,"GMC",1,"1FK70225AK741AH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1AH5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2636,"ΤΕΜ",1,"GMC",1,"1FK70225AK741AH5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1HA0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2809,"ΤΕΜ",1,"GMC",1,"1FK70225AK741HA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1HA2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2946,"ΤΕΜ",1,"GMC",1,"1FK70225AK741HA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1HA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2875,"ΤΕΜ",1,"GMC",1,"1FK70225AK741HA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1HA5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",3012,"ΤΕΜ",1,"GMC",1,"1FK70225AK741HA5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1HB0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",3129,"ΤΕΜ",1,"GMC",1,"1FK70225AK741HB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1HB2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",3265,"ΤΕΜ",1,"GMC",1,"1FK70225AK741HB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1HB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",3195,"ΤΕΜ",1,"GMC",1,"1FK70225AK741HB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1HB5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",3332,"ΤΕΜ",1,"GMC",1,"1FK70225AK741HB5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1HG0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2683,"ΤΕΜ",1,"GMC",1,"1FK70225AK741HG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1HG2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2820,"ΤΕΜ",1,"GMC",1,"1FK70225AK741HG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1HG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2749,"ΤΕΜ",1,"GMC",1,"1FK70225AK741HG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1HG5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2886,"ΤΕΜ",1,"GMC",1,"1FK70225AK741HG5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1HH0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2999,"ΤΕΜ",1,"GMC",1,"1FK70225AK741HH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1HH2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",3136,"ΤΕΜ",1,"GMC",1,"1FK70225AK741HH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1HH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",3066,"ΤΕΜ",1,"GMC",1,"1FK70225AK741HH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1HH5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",3202,"ΤΕΜ",1,"GMC",1,"1FK70225AK741HH5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1SA0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1410,"ΤΕΜ",1,"GMC",1,"1FK70225AK741SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1SA2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1547,"ΤΕΜ",1,"GMC",1,"1FK70225AK741SA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1SA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1477,"ΤΕΜ",1,"GMC",1,"1FK70225AK741SA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1SA5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1613,"ΤΕΜ",1,"GMC",1,"1FK70225AK741SA5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1SB0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1730,"ΤΕΜ",1,"GMC",1,"1FK70225AK741SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1SB2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1867,"ΤΕΜ",1,"GMC",1,"1FK70225AK741SB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1SB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1796,"ΤΕΜ",1,"GMC",1,"1FK70225AK741SB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1SB5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1933,"ΤΕΜ",1,"GMC",1,"1FK70225AK741SB5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1SG0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1284,"ΤΕΜ",1,"GMC",1,"1FK70225AK741SG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1SG2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1421,"ΤΕΜ",1,"GMC",1,"1FK70225AK741SG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1SG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1351,"ΤΕΜ",1,"GMC",1,"1FK70225AK741SG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1SG5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1487,"ΤΕΜ",1,"GMC",1,"1FK70225AK741SG5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1SH0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1601,"ΤΕΜ",1,"GMC",1,"1FK70225AK741SH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1SH2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1737,"ΤΕΜ",1,"GMC",1,"1FK70225AK741SH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1SH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1667,"ΤΕΜ",1,"GMC",1,"1FK70225AK741SH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1SH5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1803,"ΤΕΜ",1,"GMC",1,"1FK70225AK741SH5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1TA0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1410,"ΤΕΜ",1,"GMC",1,"1FK70225AK741TA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1TA2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1547,"ΤΕΜ",1,"GMC",1,"1FK70225AK741TA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1TA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1477,"ΤΕΜ",1,"GMC",1,"1FK70225AK741TA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1TA5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1613,"ΤΕΜ",1,"GMC",1,"1FK70225AK741TA5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1TB0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1730,"ΤΕΜ",1,"GMC",1,"1FK70225AK741TB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1TB2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1867,"ΤΕΜ",1,"GMC",1,"1FK70225AK741TB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1TB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1796,"ΤΕΜ",1,"GMC",1,"1FK70225AK741TB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1TB5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1933,"ΤΕΜ",1,"GMC",1,"1FK70225AK741TB5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1TG0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1284,"ΤΕΜ",1,"GMC",1,"1FK70225AK741TG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1TG2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1421,"ΤΕΜ",1,"GMC",1,"1FK70225AK741TG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1TG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1351,"ΤΕΜ",1,"GMC",1,"1FK70225AK741TG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1TG5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1487,"ΤΕΜ",1,"GMC",1,"1FK70225AK741TG5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1TH0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1601,"ΤΕΜ",1,"GMC",1,"1FK70225AK741TH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1TH2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1737,"ΤΕΜ",1,"GMC",1,"1FK70225AK741TH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1TH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1667,"ΤΕΜ",1,"GMC",1,"1FK70225AK741TH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-1TH5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Â° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1803,"ΤΕΜ",1,"GMC",1,"1FK70225AK741TH5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-8HG0","SIMOTICS S Synchronous servo motor 1FK7 Compact, 0.85Nm 100K, 6000rpm, 0.38kW Naturally cooled Bare cable end 0.5m Outlet directions DE with connector size 1 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2986,"ΤΕΜ",1,"GMC",1,"1FK70225AK748HG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7022-5AK74-8HH2","SIMOTICS S Synchronous servo motor 1FK7 Compact, 0.85Nm 100K, 6000rpm, 0.38kW Naturally cooled Bare cable end 0.5m Outlet directions DE with connector size 1 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",3439,"ΤΕΜ",1,"GMC",1,"1FK70225AK748HH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7024-5AK71-1LB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, 1.1Nm 100K, 6000rpm, 0.50kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Â° absolute encoder 512 S/R (encoder A-512) with DRIVE-CLiQ interface Derating 10% due to absolute encoder Shaft with feather key tolerance N with holding brake Degree of protection IP64 paint finish RAL7016",3762,"ΤΕΜ",1,"GMC",1,"1FK70245AK711LB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7024-5AK71-1LG0","SIMOTICS S Synchronous servo motor 1FK7 Compact, 1.1Nm 100K, 6000rpm, 0.50kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Â° absolute encoder 512 S/R (encoder A-512) with DRIVE-CLiQ interface Derating 10% due to absolute encoder Smooth shaft Tolerance N without holding brake Degree of protection IP65",3250,"ΤΕΜ",1,"GMC",1,"1FK70245AK711LG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7024-5AK71-1LG2","SIMOTICS S Synchronous servo motor 1FK7 Compact, 1.1Nm 100K, 6000rpm, 0.50kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Â° absolute encoder 512 S/R (encoder A-512) with DRIVE-CLiQ interface Derating 10% due to absolute encoder Smooth shaft Tolerance N without holding brake Degree of protection IP65 DE flange IP67",3387,"ΤΕΜ",1,"GMC",1,"1FK70245AK711LG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1BA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) shaft with feather key, tolerance N without holding brake degree of protection IP64",2551,"ΤΕΜ",1,"GMC",1,"1FK70322AF211BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1BA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65",2681,"ΤΕΜ",1,"GMC",1,"1FK70322AF211BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1BA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65, DE flange IP67",2681,"ΤΕΜ",1,"GMC",1,"1FK70322AF211BA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1BB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) shaft with feather key, tolerance N with holding brake degree of protection IP64",2856,"ΤΕΜ",1,"GMC",1,"1FK70322AF211BB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1BB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65",2986,"ΤΕΜ",1,"GMC",1,"1FK70322AF211BB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1BB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65, DE flange IP67",2986,"ΤΕΜ",1,"GMC",1,"1FK70322AF211BB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1BG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N without holding brake degree of protection IP64",2431,"ΤΕΜ",1,"GMC",1,"1FK70322AF211BG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1BG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N without holding brake degree of protection IP65",2561,"ΤΕΜ",1,"GMC",1,"1FK70322AF211BG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1BG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N without holding brake degree of protection IP65, DE flange IP67",2561,"ΤΕΜ",1,"GMC",1,"1FK70322AF211BG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1BH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N with holding brake degree of protection IP64",2732,"ΤΕΜ",1,"GMC",1,"1FK70322AF211BH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1BH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N with holding brake degree of protection IP65",2863,"ΤΕΜ",1,"GMC",1,"1FK70322AF211BH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1BH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N with holding brake degree of protection IP65, DE flange IP67",2863,"ΤΕΜ",1,"GMC",1,"1FK70322AF211BH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1CA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N without holding brake degree of protection IP64",3065,"ΤΕΜ",1,"GMC",1,"1FK70322AF211CA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1CA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65",3195,"ΤΕΜ",1,"GMC",1,"1FK70322AF211CA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1CA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65, DE flange IP67",3195,"ΤΕΜ",1,"GMC",1,"1FK70322AF211CA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1CB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N with holding brake degree of protection IP64",3370,"ΤΕΜ",1,"GMC",1,"1FK70322AF211CB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1CB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65",3500,"ΤΕΜ",1,"GMC",1,"1FK70322AF211CB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1CB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65, DE flange IP67",3500,"ΤΕΜ",1,"GMC",1,"1FK70322AF211CB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1CG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N without holding brake degree of protection IP64",2945,"ΤΕΜ",1,"GMC",1,"1FK70322AF211CG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1CG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N without holding brake degree of protection IP65",3075,"ΤΕΜ",1,"GMC",1,"1FK70322AF211CG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1CG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N without holding brake degree of protection IP65, DE flange IP67",3075,"ΤΕΜ",1,"GMC",1,"1FK70322AF211CG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1CH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N with holding brake degree of protection IP64",3246,"ΤΕΜ",1,"GMC",1,"1FK70322AF211CH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1CH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N with holding brake degree of protection IP65",3376,"ΤΕΜ",1,"GMC",1,"1FK70322AF211CH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1CH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N with holding brake degree of protection IP65, DE flange IP67",3376,"ΤΕΜ",1,"GMC",1,"1FK70322AF211CH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1DA0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.31kW; UDC=300V; M0=1.2Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2663,"ΤΕΜ",1,"GMC",1,"1FK70322AF211DA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1DA1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.31kW; UDC=300V; M0=1.2Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2790,"ΤΕΜ",1,"GMC",1,"1FK70322AF211DA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1DB0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.31kW; UDC=300V; M0=1.2Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2967,"ΤΕΜ",1,"GMC",1,"1FK70322AF211DB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1DG0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.31kW; UDC=300V; M0=1.2Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2543,"ΤΕΜ",1,"GMC",1,"1FK70322AF211DG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1DH0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.31kW; UDC=300V; M0=1.2Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2844,"ΤΕΜ",1,"GMC",1,"1FK70322AF211DH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1FA0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.31kW; UDC=300V; M0=1.2Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",3177,"ΤΕΜ",1,"GMC",1,"1FK70322AF211FA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1FB0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.31kW; UDC=300V; M0=1.2Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",3481,"ΤΕΜ",1,"GMC",1,"1FK70322AF211FB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1FB1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.31kW; UDC=300V; M0=1.2Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",3609,"ΤΕΜ",1,"GMC",1,"1FK70322AF211FB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1FG0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.31kW; UDC=300V; M0=1.2Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",3057,"ΤΕΜ",1,"GMC",1,"1FK70322AF211FG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1FH0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.31kW; UDC=300V; M0=1.2Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",3358,"ΤΕΜ",1,"GMC",1,"1FK70322AF211FH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1FH2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.31kW; UDC=300V; M0=1.2Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",3485,"ΤΕΜ",1,"GMC",1,"1FK70322AF211FH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1PA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, type of protection IP64",1736,"ΤΕΜ",1,"GMC",1,"1FK70322AF211PA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1PA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, type of protection IP65",1866,"ΤΕΜ",1,"GMC",1,"1FK70322AF211PA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1PA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, degree of protection IP65 DE flange IP67",1866,"ΤΕΜ",1,"GMC",1,"1FK70322AF211PA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1PB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, type of protection IP64",2041,"ΤΕΜ",1,"GMC",1,"1FK70322AF211PB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1PB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, type of protection IP65",2171,"ΤΕΜ",1,"GMC",1,"1FK70322AF211PB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1PB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, degree of protection IP65 DE flange IP67",2171,"ΤΕΜ",1,"GMC",1,"1FK70322AF211PB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1PG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, type of protection IP64",1616,"ΤΕΜ",1,"GMC",1,"1FK70322AF211PG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1PG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, type of protection IP65",1746,"ΤΕΜ",1,"GMC",1,"1FK70322AF211PG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1PG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, degree of protection IP65 DE flange IP67",1746,"ΤΕΜ",1,"GMC",1,"1FK70322AF211PG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1PH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, type of protection IP64",1917,"ΤΕΜ",1,"GMC",1,"1FK70322AF211PH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1PH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, type of protection IP65",2047,"ΤΕΜ",1,"GMC",1,"1FK70322AF211PH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1PH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, degree of protection IP65 DE flange IP67",2047,"ΤΕΜ",1,"GMC",1,"1FK70322AF211PH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1QA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N without holding brake degree of protection IP64",1879,"ΤΕΜ",1,"GMC",1,"1FK70322AF211QA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1QA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65",2009,"ΤΕΜ",1,"GMC",1,"1FK70322AF211QA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1QA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65, DE flange IP67",2009,"ΤΕΜ",1,"GMC",1,"1FK70322AF211QA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1QB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N with holding brake degree of protection IP64",2184,"ΤΕΜ",1,"GMC",1,"1FK70322AF211QB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1QB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65",2314,"ΤΕΜ",1,"GMC",1,"1FK70322AF211QB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1QB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65, DE flange IP67",2314,"ΤΕΜ",1,"GMC",1,"1FK70322AF211QB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1QG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UZK=300V M0=1.2Nm (100K); NN=3000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 power connector rotatable absolute encoder single-turn 20-bit with Drive-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N without holding brake degree of protection IP64",1759,"ΤΕΜ",1,"GMC",1,"1FK70322AF211QG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1QG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N without holding brake degree of protection IP65",1889,"ΤΕΜ",1,"GMC",1,"1FK70322AF211QG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1QG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N without holding brake degree of protection IP65, DE flange IP67",1889,"ΤΕΜ",1,"GMC",1,"1FK70322AF211QG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1QH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N with holding brake degree of protection IP64",2061,"ΤΕΜ",1,"GMC",1,"1FK70322AF211QH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1QH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N with holding brake degree of protection IP65",2191,"ΤΕΜ",1,"GMC",1,"1FK70322AF211QH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1QH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N with holding brake degree of protection IP65, DE flange IP67",2191,"ΤΕΜ",1,"GMC",1,"1FK70322AF211QH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1RA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N without holding brake degree of protection IP64",2400,"ΤΕΜ",1,"GMC",1,"1FK70322AF211RA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1RA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65",2530,"ΤΕΜ",1,"GMC",1,"1FK70322AF211RA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1RA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65, DE flange IP67",2530,"ΤΕΜ",1,"GMC",1,"1FK70322AF211RA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1RB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N with holding brake degree of protection IP64",2704,"ΤΕΜ",1,"GMC",1,"1FK70322AF211RB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1RB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65",2834,"ΤΕΜ",1,"GMC",1,"1FK70322AF211RB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1RB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65, DE flange IP67",2834,"ΤΕΜ",1,"GMC",1,"1FK70322AF211RB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1RG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N without holding brake degree of protection IP64",2280,"ΤΕΜ",1,"GMC",1,"1FK70322AF211RG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1RG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N without holding brake degree of protection IP65",2410,"ΤΕΜ",1,"GMC",1,"1FK70322AF211RG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1RG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N without holding brake degree of protection IP65, DE flange IP67",2410,"ΤΕΜ",1,"GMC",1,"1FK70322AF211RG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1RH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N with holding brake degree of protection IP64",2581,"ΤΕΜ",1,"GMC",1,"1FK70322AF211RH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1RH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N with holding brake degree of protection IP65",2711,"ΤΕΜ",1,"GMC",1,"1FK70322AF211RH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1RH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N with holding brake degree of protection IP65, DE flange IP67",2711,"ΤΕΜ",1,"GMC",1,"1FK70322AF211RH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1UA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, type of protection IP64",1736,"ΤΕΜ",1,"GMC",1,"1FK70322AF211UA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1UA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, type of protection IP65",1866,"ΤΕΜ",1,"GMC",1,"1FK70322AF211UA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1UA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, degree of protection IP65 DE flange IP67",1866,"ΤΕΜ",1,"GMC",1,"1FK70322AF211UA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1UB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, type of protection IP64",2041,"ΤΕΜ",1,"GMC",1,"1FK70322AF211UB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1UB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, type of protection IP65",2171,"ΤΕΜ",1,"GMC",1,"1FK70322AF211UB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1UB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, degree of protection IP65 DE flange IP67",2171,"ΤΕΜ",1,"GMC",1,"1FK70322AF211UB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1UG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, type of protection IP64",1616,"ΤΕΜ",1,"GMC",1,"1FK70322AF211UG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1UG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, type of protection IP65",1746,"ΤΕΜ",1,"GMC",1,"1FK70322AF211UG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1UG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, degree of protection IP65 DE flange IP67",1746,"ΤΕΜ",1,"GMC",1,"1FK70322AF211UG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1UH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, type of protection IP64",1917,"ΤΕΜ",1,"GMC",1,"1FK70322AF211UH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1UH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, type of protection IP65",2047,"ΤΕΜ",1,"GMC",1,"1FK70322AF211UH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF21-1UH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, degree of protection IP65 DE flange IP67",2047,"ΤΕΜ",1,"GMC",1,"1FK70322AF211UH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1EH2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.31kW; UDC=300V; M0=1.2Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",3042,"ΤΕΜ",1,"GMC",1,"1FK70322AF241EH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1SA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N without holding brake degree of protection IP64",1400,"ΤΕΜ",1,"GMC",1,"1FK70322AF241SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1SA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N without holding brake degree of protection IP65",1531,"ΤΕΜ",1,"GMC",1,"1FK70322AF241SA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1SA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N without holding brake degree of protection IP65, DE flange IP67",1531,"ΤΕΜ",1,"GMC",1,"1FK70322AF241SA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1SB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N with holding brake degree of protection IP64",1705,"ΤΕΜ",1,"GMC",1,"1FK70322AF241SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1SB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N with holding brake degree of protection IP65",1835,"ΤΕΜ",1,"GMC",1,"1FK70322AF241SB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1SB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N with holding brake degree of protection IP65, DE flange IP67",1835,"ΤΕΜ",1,"GMC",1,"1FK70322AF241SB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1SG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N without holding brake, type of protection IP64",1280,"ΤΕΜ",1,"GMC",1,"1FK70322AF241SG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1SG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N without holding brake, type of protection IP65",1411,"ΤΕΜ",1,"GMC",1,"1FK70322AF241SG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1SG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N without holding brake, type of protection IP65 DE flange IP67",1411,"ΤΕΜ",1,"GMC",1,"1FK70322AF241SG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1SH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N with holding brake, type of protection IP64",1582,"ΤΕΜ",1,"GMC",1,"1FK70322AF241SH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1SH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N with holding brake, type of protection IP65",1712,"ΤΕΜ",1,"GMC",1,"1FK70322AF241SH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1SH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N with holding brake, degree of protection IP65 DE Flange IP67",1712,"ΤΕΜ",1,"GMC",1,"1FK70322AF241SH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1TA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N without holding brake degree of protection IP64",1400,"ΤΕΜ",1,"GMC",1,"1FK70322AF241TA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1TA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N without holding brake degree of protection IP65",1531,"ΤΕΜ",1,"GMC",1,"1FK70322AF241TA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1TA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N without holding brake degree of protection IP65, DE flange IP67",1531,"ΤΕΜ",1,"GMC",1,"1FK70322AF241TA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1TB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N with holding brake degree of protection IP64",1705,"ΤΕΜ",1,"GMC",1,"1FK70322AF241TB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1TB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N with holding brake degree of protection IP65",1835,"ΤΕΜ",1,"GMC",1,"1FK70322AF241TB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1TB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N with holding brake degree of protection IP65, DE flange IP67",1835,"ΤΕΜ",1,"GMC",1,"1FK70322AF241TB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1TG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N without holding brake, type of protection IP64",1280,"ΤΕΜ",1,"GMC",1,"1FK70322AF241TG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1TG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N without holding brake, type of protection IP65",1411,"ΤΕΜ",1,"GMC",1,"1FK70322AF241TG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1TG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N without holding brake, type of protection IP65 DE flange IP67",1411,"ΤΕΜ",1,"GMC",1,"1FK70322AF241TG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1TH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N with holding brake, type of protection IP64",1582,"ΤΕΜ",1,"GMC",1,"1FK70322AF241TH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1TH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N with holding brake, type of protection IP65",1712,"ΤΕΜ",1,"GMC",1,"1FK70322AF241TH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AF24-1TH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N with holding brake, degree of protection IP65 DE Flange IP67",1712,"ΤΕΜ",1,"GMC",1,"1FK70322AF241TH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1BA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) Shaft with feather key, tolerance N without Holding brake, degree of protection IP64",2551,"ΤΕΜ",1,"GMC",1,"1FK70322AK711BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1BA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) Shaft with feather key, tolerance N without Holding brake, degree of protection IP65",2681,"ΤΕΜ",1,"GMC",1,"1FK70322AK711BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1BA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) Shaft with feather key, tolerance N without Holding brake, degree of protection IP65 DE flange IP67",2681,"ΤΕΜ",1,"GMC",1,"1FK70322AK711BA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1BB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) Shaft with feather key, tolerance N with Holding brake, degree of protection IP64",2856,"ΤΕΜ",1,"GMC",1,"1FK70322AK711BB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1BB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) Shaft with feather key, tolerance N with Holding brake, degree of protection IP65",2986,"ΤΕΜ",1,"GMC",1,"1FK70322AK711BB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1BB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) Shaft with feather key, tolerance N with Holding brake, degree of protection IP65 DE flange IP67",2986,"ΤΕΜ",1,"GMC",1,"1FK70322AK711BB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1BG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N without Holding brake, degree of protection IP64",2431,"ΤΕΜ",1,"GMC",1,"1FK70322AK711BG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1BG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N without Holding brake, degree of protection IP65",2561,"ΤΕΜ",1,"GMC",1,"1FK70322AK711BG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1BG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N without Holding brake, degree of protection IP65 DE flange IP67",2561,"ΤΕΜ",1,"GMC",1,"1FK70322AK711BG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1BH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N with Holding brake, degree of protection IP64",2732,"ΤΕΜ",1,"GMC",1,"1FK70322AK711BH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1BH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N with Holding brake, degree of protection IP65",2863,"ΤΕΜ",1,"GMC",1,"1FK70322AK711BH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1BH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N with Holding brake, degree of protection IP65 DE flange IP67",2863,"ΤΕΜ",1,"GMC",1,"1FK70322AK711BH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1CA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 24 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) Shaft with feather key, tolerance N without Holding brake, degree of protection IP64",3065,"ΤΕΜ",1,"GMC",1,"1FK70322AK711CA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1CA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 24 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) Shaft with feather key, tolerance N without Holding brake, degree of protection IP65",3195,"ΤΕΜ",1,"GMC",1,"1FK70322AK711CA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1CA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 24 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) Shaft with feather key, tolerance N without Holding brake, degree of protection IP65 DE flange IP67",3195,"ΤΕΜ",1,"GMC",1,"1FK70322AK711CA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1CB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 24 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) Shaft with feather key, tolerance N with Holding brake, degree of protection IP64",3370,"ΤΕΜ",1,"GMC",1,"1FK70322AK711CB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1CB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 24 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) Shaft with feather key, tolerance N with Holding brake, degree of protection IP65",3500,"ΤΕΜ",1,"GMC",1,"1FK70322AK711CB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1CB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 24 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) Shaft with feather key, tolerance N with Holding brake, degree of protection IP65 DE flange IP67",3500,"ΤΕΜ",1,"GMC",1,"1FK70322AK711CB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1CG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 24 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N without Holding brake, degree of protection IP64",2945,"ΤΕΜ",1,"GMC",1,"1FK70322AK711CG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1CG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 24 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N without Holding brake, degree of protection IP65",3075,"ΤΕΜ",1,"GMC",1,"1FK70322AK711CG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1CG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 24 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N without Holding brake, degree of protection IP65 DE flange IP67",3075,"ΤΕΜ",1,"GMC",1,"1FK70322AK711CG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1CH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 24 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N with Holding brake, degree of protection IP64",3246,"ΤΕΜ",1,"GMC",1,"1FK70322AK711CH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1CH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 24 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N with Holding brake, degree of protection IP65",3376,"ΤΕΜ",1,"GMC",1,"1FK70322AK711CH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1CH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 24 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N with Holding brake, degree of protection IP65 DE flange IP67",3376,"ΤΕΜ",1,"GMC",1,"1FK70322AK711CH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1DA0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2663,"ΤΕΜ",1,"GMC",1,"1FK70322AK711DA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1DA1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2790,"ΤΕΜ",1,"GMC",1,"1FK70322AK711DA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1DB0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2967,"ΤΕΜ",1,"GMC",1,"1FK70322AK711DB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1DG0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2543,"ΤΕΜ",1,"GMC",1,"1FK70322AK711DG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1DG1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2670,"ΤΕΜ",1,"GMC",1,"1FK70322AK711DG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1DG2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2670,"ΤΕΜ",1,"GMC",1,"1FK70322AK711DG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1DH0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2844,"ΤΕΜ",1,"GMC",1,"1FK70322AK711DH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1DH1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2971,"ΤΕΜ",1,"GMC",1,"1FK70322AK711DH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1FA0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",3177,"ΤΕΜ",1,"GMC",1,"1FK70322AK711FA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1FA2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",3304,"ΤΕΜ",1,"GMC",1,"1FK70322AK711FA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1FB0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",3481,"ΤΕΜ",1,"GMC",1,"1FK70322AK711FB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1FB1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",3609,"ΤΕΜ",1,"GMC",1,"1FK70322AK711FB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1FG0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",3057,"ΤΕΜ",1,"GMC",1,"1FK70322AK711FG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1FG1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",3184,"ΤΕΜ",1,"GMC",1,"1FK70322AK711FG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1FH0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",3358,"ΤΕΜ",1,"GMC",1,"1FK70322AK711FH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1FH1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",3485,"ΤΕΜ",1,"GMC",1,"1FK70322AK711FH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1PA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, type of protection IP64",1736,"ΤΕΜ",1,"GMC",1,"1FK70322AK711PA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1PA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, type of protection IP65",1866,"ΤΕΜ",1,"GMC",1,"1FK70322AK711PA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1PA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, degree of protection IP65 DE flange IP67",1866,"ΤΕΜ",1,"GMC",1,"1FK70322AK711PA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1PB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, type of protection IP64",2041,"ΤΕΜ",1,"GMC",1,"1FK70322AK711PB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1PB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, type of protection IP65",2171,"ΤΕΜ",1,"GMC",1,"1FK70322AK711PB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1PB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, degree of protection IP65 DE flange IP67",2171,"ΤΕΜ",1,"GMC",1,"1FK70322AK711PB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1PG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, type of protection IP64",1616,"ΤΕΜ",1,"GMC",1,"1FK70322AK711PG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1PG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, type of protection IP65",1746,"ΤΕΜ",1,"GMC",1,"1FK70322AK711PG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1PG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, degree of protection IP65 DE flange IP67",1746,"ΤΕΜ",1,"GMC",1,"1FK70322AK711PG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1PH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, type of protection IP64",1917,"ΤΕΜ",1,"GMC",1,"1FK70322AK711PH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1PH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, type of protection IP65",2047,"ΤΕΜ",1,"GMC",1,"1FK70322AK711PH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1PH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, degree of protection IP65 DE flange IP67",2047,"ΤΕΜ",1,"GMC",1,"1FK70322AK711PH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1QA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) Shaft with feather key, tolerance N without Holding brake, degree of protection IP64",1879,"ΤΕΜ",1,"GMC",1,"1FK70322AK711QA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1QA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) Shaft with feather key, tolerance N without Holding brake, degree of protection IP65",2009,"ΤΕΜ",1,"GMC",1,"1FK70322AK711QA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1QA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) Shaft with feather key, tolerance N without Holding brake, degree of protection IP65 DE flange IP67",2009,"ΤΕΜ",1,"GMC",1,"1FK70322AK711QA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1QB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) Shaft with feather key, tolerance N with Holding brake, degree of protection IP64",2184,"ΤΕΜ",1,"GMC",1,"1FK70322AK711QB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1QB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) Shaft with feather key, tolerance N with Holding brake, degree of protection IP65",2314,"ΤΕΜ",1,"GMC",1,"1FK70322AK711QB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1QB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) Shaft with feather key, tolerance N with Holding brake, degree of protection IP65 DE flange IP67",2314,"ΤΕΜ",1,"GMC",1,"1FK70322AK711QB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1QG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N without Holding brake, degree of protection IP64",1759,"ΤΕΜ",1,"GMC",1,"1FK70322AK711QG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1QG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N without Holding brake, degree of protection IP65",1889,"ΤΕΜ",1,"GMC",1,"1FK70322AK711QG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1QG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N without Holding brake, degree of protection IP65 DE flange IP67",1889,"ΤΕΜ",1,"GMC",1,"1FK70322AK711QG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1QH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N with Holding brake, degree of protection IP64",2061,"ΤΕΜ",1,"GMC",1,"1FK70322AK711QH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1QH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N with Holding brake, degree of protection IP65",2191,"ΤΕΜ",1,"GMC",1,"1FK70322AK711QH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1QH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N with Holding brake, degree of protection IP65 DE flange IP67",2191,"ΤΕΜ",1,"GMC",1,"1FK70322AK711QH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1RA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 20 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) Shaft with feather key, tolerance N without Holding brake, degree of protection IP64",2400,"ΤΕΜ",1,"GMC",1,"1FK70322AK711RA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1RA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 20 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) Shaft with feather key, tolerance N without Holding brake, degree of protection IP65",2530,"ΤΕΜ",1,"GMC",1,"1FK70322AK711RA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1RA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 20 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) Shaft with feather key, tolerance N without Holding brake, degree of protection IP65 DE flange IP67",2530,"ΤΕΜ",1,"GMC",1,"1FK70322AK711RA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1RB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 20 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) Shaft with feather key, tolerance N with Holding brake, degree of protection IP64",2704,"ΤΕΜ",1,"GMC",1,"1FK70322AK711RB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1RB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 20 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) Shaft with feather key, tolerance N with Holding brake, degree of protection IP65",2834,"ΤΕΜ",1,"GMC",1,"1FK70322AK711RB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1RB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 20 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) Shaft with feather key, tolerance N with Holding brake, degree of protection IP65 DE flange IP67",2834,"ΤΕΜ",1,"GMC",1,"1FK70322AK711RB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1RG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 20 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N without Holding brake, degree of protection IP64",2280,"ΤΕΜ",1,"GMC",1,"1FK70322AK711RG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1RG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 20 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N without Holding brake, degree of protection IP65",2410,"ΤΕΜ",1,"GMC",1,"1FK70322AK711RG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1RG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 20 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N without Holding brake, degree of protection IP65 DE flange IP67",2410,"ΤΕΜ",1,"GMC",1,"1FK70322AK711RG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1RH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 20 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N with Holding brake, degree of protection IP64",2581,"ΤΕΜ",1,"GMC",1,"1FK70322AK711RH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1RH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 20 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N with Holding brake, degree of protection IP65",2711,"ΤΕΜ",1,"GMC",1,"1FK70322AK711RH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1RH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 20 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N with Holding brake, degree of protection IP65 DE flange IP67",2711,"ΤΕΜ",1,"GMC",1,"1FK70322AK711RH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1UA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, type of protection IP64",1736,"ΤΕΜ",1,"GMC",1,"1FK70322AK711UA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1UA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, type of protection IP65",1866,"ΤΕΜ",1,"GMC",1,"1FK70322AK711UA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1UA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, degree of protection IP65 DE flange IP67",1866,"ΤΕΜ",1,"GMC",1,"1FK70322AK711UA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1UB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, type of protection IP64",2041,"ΤΕΜ",1,"GMC",1,"1FK70322AK711UB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1UB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, type of protection IP65",2171,"ΤΕΜ",1,"GMC",1,"1FK70322AK711UB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1UB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, degree of protection IP65 DE flange IP67",2171,"ΤΕΜ",1,"GMC",1,"1FK70322AK711UB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1UG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, type of protection IP64",1616,"ΤΕΜ",1,"GMC",1,"1FK70322AK711UG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1UG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, type of protection IP65",1746,"ΤΕΜ",1,"GMC",1,"1FK70322AK711UG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1UG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, degree of protection IP65 DE flange IP67",1746,"ΤΕΜ",1,"GMC",1,"1FK70322AK711UG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1UH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, type of protection IP64",1917,"ΤΕΜ",1,"GMC",1,"1FK70322AK711UH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1UH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, type of protection IP65",2047,"ΤΕΜ",1,"GMC",1,"1FK70322AK711UH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK71-1UH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, degree of protection IP65 DE flange IP67",2047,"ΤΕΜ",1,"GMC",1,"1FK70322AK711UH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1AA0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2216,"ΤΕΜ",1,"GMC",1,"1FK70322AK741AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1AA1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2343,"ΤΕΜ",1,"GMC",1,"1FK70322AK741AA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1AA2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2343,"ΤΕΜ",1,"GMC",1,"1FK70322AK741AA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1AB0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2520,"ΤΕΜ",1,"GMC",1,"1FK70322AK741AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1AB1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2648,"ΤΕΜ",1,"GMC",1,"1FK70322AK741AB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1AB2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2648,"ΤΕΜ",1,"GMC",1,"1FK70322AK741AB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1AG0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2096,"ΤΕΜ",1,"GMC",1,"1FK70322AK741AG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1AG1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2223,"ΤΕΜ",1,"GMC",1,"1FK70322AK741AG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1AG2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2223,"ΤΕΜ",1,"GMC",1,"1FK70322AK741AG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1AH0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2397,"ΤΕΜ",1,"GMC",1,"1FK70322AK741AH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1AH1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2525,"ΤΕΜ",1,"GMC",1,"1FK70322AK741AH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1AH2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2525,"ΤΕΜ",1,"GMC",1,"1FK70322AK741AH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1EA0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2733,"ΤΕΜ",1,"GMC",1,"1FK70322AK741EA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1EA1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2860,"ΤΕΜ",1,"GMC",1,"1FK70322AK741EA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1EA2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2860,"ΤΕΜ",1,"GMC",1,"1FK70322AK741EA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1EB0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",3037,"ΤΕΜ",1,"GMC",1,"1FK70322AK741EB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1EB1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",3165,"ΤΕΜ",1,"GMC",1,"1FK70322AK741EB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1EB2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",3165,"ΤΕΜ",1,"GMC",1,"1FK70322AK741EB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1EG0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2613,"ΤΕΜ",1,"GMC",1,"1FK70322AK741EG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1EG1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2740,"ΤΕΜ",1,"GMC",1,"1FK70322AK741EG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1EG2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2740,"ΤΕΜ",1,"GMC",1,"1FK70322AK741EG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1EH0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2914,"ΤΕΜ",1,"GMC",1,"1FK70322AK741EH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1EH1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",3042,"ΤΕΜ",1,"GMC",1,"1FK70322AK741EH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1EH2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",3042,"ΤΕΜ",1,"GMC",1,"1FK70322AK741EH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1SA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N without holding brake degree of protection IP64",1400,"ΤΕΜ",1,"GMC",1,"1FK70322AK741SA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1SA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N without holding brake degree of protection IP65",1531,"ΤΕΜ",1,"GMC",1,"1FK70322AK741SA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1SA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N without holding brake degree of protection IP65, DE flange IP67",1531,"ΤΕΜ",1,"GMC",1,"1FK70322AK741SA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1SB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N with holding brake degree of protection IP64",1705,"ΤΕΜ",1,"GMC",1,"1FK70322AK741SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1SB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N with holding brake degree of protection IP65",1835,"ΤΕΜ",1,"GMC",1,"1FK70322AK741SB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1SB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N with holding brake degree of protection IP65, DE flange IP67",1835,"ΤΕΜ",1,"GMC",1,"1FK70322AK741SB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1SG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N without holding brake, type of protection IP64",1280,"ΤΕΜ",1,"GMC",1,"1FK70322AK741SG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1SG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N without holding brake, type of protection IP65",1411,"ΤΕΜ",1,"GMC",1,"1FK70322AK741SG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1SG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N without holding brake, type of protection IP65 DE flange IP67",1411,"ΤΕΜ",1,"GMC",1,"1FK70322AK741SG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1SH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N with holding brake, type of protection IP64",1582,"ΤΕΜ",1,"GMC",1,"1FK70322AK741SH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1SH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N with holding brake, type of protection IP65",1712,"ΤΕΜ",1,"GMC",1,"1FK70322AK741SH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1SH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N with holding brake, degree of protection IP65 DE flange IP67",1712,"ΤΕΜ",1,"GMC",1,"1FK70322AK741SH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1TA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N without holding brake degree of protection IP64",1400,"ΤΕΜ",1,"GMC",1,"1FK70322AK741TA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1TA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N without holding brake degree of protection IP65",1531,"ΤΕΜ",1,"GMC",1,"1FK70322AK741TA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1TA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N without holding brake degree of protection IP65, DE flange IP67",1531,"ΤΕΜ",1,"GMC",1,"1FK70322AK741TA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1TB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N with holding brake degree of protection IP64",1705,"ΤΕΜ",1,"GMC",1,"1FK70322AK741TB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1TB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N with holding brake degree of protection IP65",1835,"ΤΕΜ",1,"GMC",1,"1FK70322AK741TB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1TB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N with holding brake degree of protection IP65, DE flange IP67",1835,"ΤΕΜ",1,"GMC",1,"1FK70322AK741TB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1TG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N without holding brake, type of protection IP64",1280,"ΤΕΜ",1,"GMC",1,"1FK70322AK741TG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1TG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N without holding brake, type of protection IP65",1411,"ΤΕΜ",1,"GMC",1,"1FK70322AK741TG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1TG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N without holding brake, type of protection IP65 DE flange IP67",1411,"ΤΕΜ",1,"GMC",1,"1FK70322AK741TG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1TH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N with holding brake, type of protection IP64",1582,"ΤΕΜ",1,"GMC",1,"1FK70322AK741TH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1TH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N with holding brake, type of protection IP65",1712,"ΤΕΜ",1,"GMC",1,"1FK70322AK741TH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7032-2AK74-1TH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N with holding brake, degree of protection IP65 DE flange IP67",1712,"ΤΕΜ",1,"GMC",1,"1FK70322AK741TH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1BA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2613,"ΤΕΜ",1,"GMC",1,"1FK70334CF211BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1BA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2740,"ΤΕΜ",1,"GMC",1,"1FK70334CF211BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1BA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2740,"ΤΕΜ",1,"GMC",1,"1FK70334CF211BA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1BB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2917,"ΤΕΜ",1,"GMC",1,"1FK70334CF211BB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1BB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",3045,"ΤΕΜ",1,"GMC",1,"1FK70334CF211BB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1BB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",3045,"ΤΕΜ",1,"GMC",1,"1FK70334CF211BB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1BG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2493,"ΤΕΜ",1,"GMC",1,"1FK70334CF211BG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1BG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2620,"ΤΕΜ",1,"GMC",1,"1FK70334CF211BG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1BG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2620,"ΤΕΜ",1,"GMC",1,"1FK70334CF211BG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1BH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2794,"ΤΕΜ",1,"GMC",1,"1FK70334CF211BH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1BH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2922,"ΤΕΜ",1,"GMC",1,"1FK70334CF211BH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1BH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2922,"ΤΕΜ",1,"GMC",1,"1FK70334CF211BH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1CA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",3127,"ΤΕΜ",1,"GMC",1,"1FK70334CF211CA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1CA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",3254,"ΤΕΜ",1,"GMC",1,"1FK70334CF211CA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1CA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",3254,"ΤΕΜ",1,"GMC",1,"1FK70334CF211CA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1CB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",3431,"ΤΕΜ",1,"GMC",1,"1FK70334CF211CB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1CB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",3559,"ΤΕΜ",1,"GMC",1,"1FK70334CF211CB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1CB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",3559,"ΤΕΜ",1,"GMC",1,"1FK70334CF211CB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1CG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",3007,"ΤΕΜ",1,"GMC",1,"1FK70334CF211CG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1CG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",3134,"ΤΕΜ",1,"GMC",1,"1FK70334CF211CG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1CG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",3134,"ΤΕΜ",1,"GMC",1,"1FK70334CF211CG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1CH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",3308,"ΤΕΜ",1,"GMC",1,"1FK70334CF211CH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1CH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",3435,"ΤΕΜ",1,"GMC",1,"1FK70334CF211CH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1CH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",3435,"ΤΕΜ",1,"GMC",1,"1FK70334CF211CH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1DA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2724,"ΤΕΜ",1,"GMC",1,"1FK70334CF211DA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1DA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2852,"ΤΕΜ",1,"GMC",1,"1FK70334CF211DA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1DH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",3033,"ΤΕΜ",1,"GMC",1,"1FK70334CF211DH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1PA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1797,"ΤΕΜ",1,"GMC",1,"1FK70334CF211PA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1PA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1925,"ΤΕΜ",1,"GMC",1,"1FK70334CF211PA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1PA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1925,"ΤΕΜ",1,"GMC",1,"1FK70334CF211PA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1PB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2102,"ΤΕΜ",1,"GMC",1,"1FK70334CF211PB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1PB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2230,"ΤΕΜ",1,"GMC",1,"1FK70334CF211PB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1PB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2230,"ΤΕΜ",1,"GMC",1,"1FK70334CF211PB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1PG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1677,"ΤΕΜ",1,"GMC",1,"1FK70334CF211PG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1PG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1805,"ΤΕΜ",1,"GMC",1,"1FK70334CF211PG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1PG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1805,"ΤΕΜ",1,"GMC",1,"1FK70334CF211PG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1PH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",1979,"ΤΕΜ",1,"GMC",1,"1FK70334CF211PH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1PH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2106,"ΤΕΜ",1,"GMC",1,"1FK70334CF211PH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1PH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2106,"ΤΕΜ",1,"GMC",1,"1FK70334CF211PH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1QA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1941,"ΤΕΜ",1,"GMC",1,"1FK70334CF211QA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1QA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2068,"ΤΕΜ",1,"GMC",1,"1FK70334CF211QA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1QA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2068,"ΤΕΜ",1,"GMC",1,"1FK70334CF211QA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1QB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2245,"ΤΕΜ",1,"GMC",1,"1FK70334CF211QB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1QB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2373,"ΤΕΜ",1,"GMC",1,"1FK70334CF211QB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1QB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2373,"ΤΕΜ",1,"GMC",1,"1FK70334CF211QB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1QG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1821,"ΤΕΜ",1,"GMC",1,"1FK70334CF211QG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1QG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1948,"ΤΕΜ",1,"GMC",1,"1FK70334CF211QG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1QG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1948,"ΤΕΜ",1,"GMC",1,"1FK70334CF211QG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1QH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2122,"ΤΕΜ",1,"GMC",1,"1FK70334CF211QH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1QH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2250,"ΤΕΜ",1,"GMC",1,"1FK70334CF211QH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1QH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2250,"ΤΕΜ",1,"GMC",1,"1FK70334CF211QH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1RA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2461,"ΤΕΜ",1,"GMC",1,"1FK70334CF211RA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1RA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2589,"ΤΕΜ",1,"GMC",1,"1FK70334CF211RA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1RA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2589,"ΤΕΜ",1,"GMC",1,"1FK70334CF211RA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1RB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2766,"ΤΕΜ",1,"GMC",1,"1FK70334CF211RB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1RB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2893,"ΤΕΜ",1,"GMC",1,"1FK70334CF211RB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1RB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2893,"ΤΕΜ",1,"GMC",1,"1FK70334CF211RB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1RG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2341,"ΤΕΜ",1,"GMC",1,"1FK70334CF211RG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1RG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2469,"ΤΕΜ",1,"GMC",1,"1FK70334CF211RG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1RG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2469,"ΤΕΜ",1,"GMC",1,"1FK70334CF211RG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1RH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2643,"ΤΕΜ",1,"GMC",1,"1FK70334CF211RH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1RH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2770,"ΤΕΜ",1,"GMC",1,"1FK70334CF211RH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1RH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2770,"ΤΕΜ",1,"GMC",1,"1FK70334CF211RH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1UA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1797,"ΤΕΜ",1,"GMC",1,"1FK70334CF211UA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1UA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1925,"ΤΕΜ",1,"GMC",1,"1FK70334CF211UA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1UA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1925,"ΤΕΜ",1,"GMC",1,"1FK70334CF211UA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1UB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2102,"ΤΕΜ",1,"GMC",1,"1FK70334CF211UB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1UB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2230,"ΤΕΜ",1,"GMC",1,"1FK70334CF211UB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1UB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2230,"ΤΕΜ",1,"GMC",1,"1FK70334CF211UB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1UG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1677,"ΤΕΜ",1,"GMC",1,"1FK70334CF211UG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1UG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1805,"ΤΕΜ",1,"GMC",1,"1FK70334CF211UG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1UG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1805,"ΤΕΜ",1,"GMC",1,"1FK70334CF211UG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1UH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",1979,"ΤΕΜ",1,"GMC",1,"1FK70334CF211UH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1UH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2106,"ΤΕΜ",1,"GMC",1,"1FK70334CF211UH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF21-1UH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2106,"ΤΕΜ",1,"GMC",1,"1FK70334CF211UH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF24-1AA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2405,"ΤΕΜ",1,"GMC",1,"1FK70334CF241AA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF24-1AH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2459,"ΤΕΜ",1,"GMC",1,"1FK70334CF241AH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CF24-1EG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2674,"ΤΕΜ",1,"GMC",1,"1FK70334CF241EG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1BA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2613,"ΤΕΜ",1,"GMC",1,"1FK70334CK711BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1BA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2740,"ΤΕΜ",1,"GMC",1,"1FK70334CK711BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1BA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2740,"ΤΕΜ",1,"GMC",1,"1FK70334CK711BA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1BB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2917,"ΤΕΜ",1,"GMC",1,"1FK70334CK711BB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1BB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",3045,"ΤΕΜ",1,"GMC",1,"1FK70334CK711BB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1BB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",3045,"ΤΕΜ",1,"GMC",1,"1FK70334CK711BB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1BG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2493,"ΤΕΜ",1,"GMC",1,"1FK70334CK711BG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1BG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2620,"ΤΕΜ",1,"GMC",1,"1FK70334CK711BG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1BG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2620,"ΤΕΜ",1,"GMC",1,"1FK70334CK711BG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1BH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2794,"ΤΕΜ",1,"GMC",1,"1FK70334CK711BH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1BH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2922,"ΤΕΜ",1,"GMC",1,"1FK70334CK711BH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1BH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2922,"ΤΕΜ",1,"GMC",1,"1FK70334CK711BH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1CA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",3127,"ΤΕΜ",1,"GMC",1,"1FK70334CK711CA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1CA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",3254,"ΤΕΜ",1,"GMC",1,"1FK70334CK711CA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1CA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",3254,"ΤΕΜ",1,"GMC",1,"1FK70334CK711CA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1CB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",3431,"ΤΕΜ",1,"GMC",1,"1FK70334CK711CB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1CB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",3559,"ΤΕΜ",1,"GMC",1,"1FK70334CK711CB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1CB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",3559,"ΤΕΜ",1,"GMC",1,"1FK70334CK711CB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1CG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",3007,"ΤΕΜ",1,"GMC",1,"1FK70334CK711CG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1CG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",3134,"ΤΕΜ",1,"GMC",1,"1FK70334CK711CG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1CG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",3134,"ΤΕΜ",1,"GMC",1,"1FK70334CK711CG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1CH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",3308,"ΤΕΜ",1,"GMC",1,"1FK70334CK711CH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1CH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",3435,"ΤΕΜ",1,"GMC",1,"1FK70334CK711CH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1CH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",3435,"ΤΕΜ",1,"GMC",1,"1FK70334CK711CH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1DA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2724,"ΤΕΜ",1,"GMC",1,"1FK70334CK711DA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1DA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2852,"ΤΕΜ",1,"GMC",1,"1FK70334CK711DA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1DG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2604,"ΤΕΜ",1,"GMC",1,"1FK70334CK711DG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1PA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1797,"ΤΕΜ",1,"GMC",1,"1FK70334CK711PA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1PA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1925,"ΤΕΜ",1,"GMC",1,"1FK70334CK711PA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1PA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1925,"ΤΕΜ",1,"GMC",1,"1FK70334CK711PA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1PB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2102,"ΤΕΜ",1,"GMC",1,"1FK70334CK711PB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1PB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2230,"ΤΕΜ",1,"GMC",1,"1FK70334CK711PB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1PB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2230,"ΤΕΜ",1,"GMC",1,"1FK70334CK711PB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1PG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1677,"ΤΕΜ",1,"GMC",1,"1FK70334CK711PG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1PG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1805,"ΤΕΜ",1,"GMC",1,"1FK70334CK711PG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1PG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1805,"ΤΕΜ",1,"GMC",1,"1FK70334CK711PG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1PH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",1979,"ΤΕΜ",1,"GMC",1,"1FK70334CK711PH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1PH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2106,"ΤΕΜ",1,"GMC",1,"1FK70334CK711PH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1PH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2106,"ΤΕΜ",1,"GMC",1,"1FK70334CK711PH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1QA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1941,"ΤΕΜ",1,"GMC",1,"1FK70334CK711QA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1QA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2068,"ΤΕΜ",1,"GMC",1,"1FK70334CK711QA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1QA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2068,"ΤΕΜ",1,"GMC",1,"1FK70334CK711QA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1QB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2245,"ΤΕΜ",1,"GMC",1,"1FK70334CK711QB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1QB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2373,"ΤΕΜ",1,"GMC",1,"1FK70334CK711QB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1QB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2373,"ΤΕΜ",1,"GMC",1,"1FK70334CK711QB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1QG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1821,"ΤΕΜ",1,"GMC",1,"1FK70334CK711QG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1QG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1948,"ΤΕΜ",1,"GMC",1,"1FK70334CK711QG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1QG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1948,"ΤΕΜ",1,"GMC",1,"1FK70334CK711QG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1QH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2122,"ΤΕΜ",1,"GMC",1,"1FK70334CK711QH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1QH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2250,"ΤΕΜ",1,"GMC",1,"1FK70334CK711QH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1QH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2250,"ΤΕΜ",1,"GMC",1,"1FK70334CK711QH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1RA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2461,"ΤΕΜ",1,"GMC",1,"1FK70334CK711RA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1RA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2589,"ΤΕΜ",1,"GMC",1,"1FK70334CK711RA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1RA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2589,"ΤΕΜ",1,"GMC",1,"1FK70334CK711RA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1RB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2766,"ΤΕΜ",1,"GMC",1,"1FK70334CK711RB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1RB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2893,"ΤΕΜ",1,"GMC",1,"1FK70334CK711RB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1RB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2893,"ΤΕΜ",1,"GMC",1,"1FK70334CK711RB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1RG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2341,"ΤΕΜ",1,"GMC",1,"1FK70334CK711RG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1RG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2469,"ΤΕΜ",1,"GMC",1,"1FK70334CK711RG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1RG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2469,"ΤΕΜ",1,"GMC",1,"1FK70334CK711RG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1RH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2643,"ΤΕΜ",1,"GMC",1,"1FK70334CK711RH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1RH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2770,"ΤΕΜ",1,"GMC",1,"1FK70334CK711RH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1RH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2770,"ΤΕΜ",1,"GMC",1,"1FK70334CK711RH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1UA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1797,"ΤΕΜ",1,"GMC",1,"1FK70334CK711UA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1UA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1925,"ΤΕΜ",1,"GMC",1,"1FK70334CK711UA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1UA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1925,"ΤΕΜ",1,"GMC",1,"1FK70334CK711UA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1UB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2102,"ΤΕΜ",1,"GMC",1,"1FK70334CK711UB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1UB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2230,"ΤΕΜ",1,"GMC",1,"1FK70334CK711UB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1UB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2230,"ΤΕΜ",1,"GMC",1,"1FK70334CK711UB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1UG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1677,"ΤΕΜ",1,"GMC",1,"1FK70334CK711UG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1UG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1805,"ΤΕΜ",1,"GMC",1,"1FK70334CK711UG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1UG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1805,"ΤΕΜ",1,"GMC",1,"1FK70334CK711UG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1UH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",1979,"ΤΕΜ",1,"GMC",1,"1FK70334CK711UH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1UH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2106,"ΤΕΜ",1,"GMC",1,"1FK70334CK711UH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK71-1UH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2106,"ΤΕΜ",1,"GMC",1,"1FK70334CK711UH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK74-1AA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2277,"ΤΕΜ",1,"GMC",1,"1FK70334CK741AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK74-1AA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2405,"ΤΕΜ",1,"GMC",1,"1FK70334CK741AA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK74-1AA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2405,"ΤΕΜ",1,"GMC",1,"1FK70334CK741AA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK74-1AB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2582,"ΤΕΜ",1,"GMC",1,"1FK70334CK741AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK74-1AB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2710,"ΤΕΜ",1,"GMC",1,"1FK70334CK741AB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK74-1AB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2710,"ΤΕΜ",1,"GMC",1,"1FK70334CK741AB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7033-4CK74-1TB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",1767,"ΤΕΜ",1,"GMC",1,"1FK70334CK741TB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7034-2AF21-1FH0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.47kW; UDC=300V; M0=1.6Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",3490,"ΤΕΜ",1,"GMC",1,"1FK70342AF211FH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7034-2AK71-1BA0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 24-bit with Drive-CLiQ interface (encoder AS24DQI) shaft with feather key, Tolerance N without holding brake Degree of protection IP64",2684,"ΤΕΜ",1,"GMC",1,"1FK70342AK711BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7034-2AK71-1CG0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 24-bit +12-bit multi-turn with Drive-CLiQ interface (encoder AM24DQI) smooth shaft, Tolerance N without holding brake Degree of protection IP64",3077,"ΤΕΜ",1,"GMC",1,"1FK70342AK711CG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7034-2AK74-1SG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.63 kW; UDC=600V M0=1.6 Nm (100K); NN=6000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N without holding brake, type of protection IP64",1413,"ΤΕΜ",1,"GMC",1,"1FK70342AK741SG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7040-2AK71-1BB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.69 kW; UDC=600V M0=1.6 Nm (100K); NN=6000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) shaft with feather key, tolerance N with holding brake degree of protection IP64",3004,"ΤΕΜ",1,"GMC",1,"1FK70402AK711BB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7040-2AK71-1QG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.69 kW; UDC=600V M0=1.6 Nm (100K); NN=6000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N without holding brake degree of protection IP65",1979,"ΤΕΜ",1,"GMC",1,"1FK70402AK711QG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7040-2AK74-1TA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.69 kW; UDC=600V M0=1.6 Nm (100K); NN=6000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N without holding brake degree of protection IP65, DE flange IP67",1620,"ΤΕΜ",1,"GMC",1,"1FK70402AK741TA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7042-2AC71-1FA2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.59kW; UDC=600V M0=3Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",3483,"ΤΕΜ",1,"GMC",1,"1FK70422AC711FA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7042-2AC74-1AB2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.59kW; UDC=600V M0=3Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2885,"ΤΕΜ",1,"GMC",1,"1FK70422AC741AB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7042-2AC74-1TA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.59 kW; UDC=600V M0=3Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N without holding brake degree of protection IP65, DE flange IP67",1709,"ΤΕΜ",1,"GMC",1,"1FK70422AC741TA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7042-2AF24-1SH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.82 kW; UDC=300 V M0=3Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=4) smooth shaft, tolerance N with holding brake, type of protection IP64",1819,"ΤΕΜ",1,"GMC",1,"1FK70422AF241SH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7042-2AF71-1DG0","SIMOTICS S SIMOTICS S-1FK7 Synchronous motor 1FK7-CT PN=0.82kW; UDC=600V M0=3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2721,"ΤΕΜ",1,"GMC",1,"1FK70422AF711DG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7042-2AF71-1UA0","SIMOTICS S SIMOTICS S-1FK7 synchronous motor 1FK7-CT PN=0.82 kW; UDC=600 V M0=3 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake degree of protection IP64",1914,"ΤΕΜ",1,"GMC",1,"1FK70422AF711UA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7042-2AF74-1SB0","SIMOTICS S SIMOTICS S-1FK7 synchronous motor 1FK7-CT PN=0.82 kW; UDC=600 V M0=3 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=4) shaft with feather key, tolerance N with holding brake degree of protection IP64",1942,"ΤΕΜ",1,"GMC",1,"1FK70422AF741SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7042-2AK71-1QG1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.94kW; UDC=600V M0=3Nm (100K); NN=6000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 20-bit with Drive-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N without holding brake IP65 degree of protection",2068,"ΤΕΜ",1,"GMC",1,"1FK70422AK711QG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7042-2AK74-1AH2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.94kW; UDC=600V M0=3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2762,"ΤΕΜ",1,"GMC",1,"1FK70422AK741AH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7042-2AK74-1SG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.94 kW; UDC=600V M0=3Nm (100K); NN=6000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=4) smooth shaft, tolerance N without holding brake, type of protection IP65",1589,"ΤΕΜ",1,"GMC",1,"1FK70422AK741SG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7042-3BK71-1QB1","SIMOTICS S synchronous motor 1FK7-HI PN=0.94 kW; UDC=600 V M0=3 Nm (100K); NN=6000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65",2551,"ΤΕΜ",1,"GMC",1,"1FK70423BK711QB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7043-4CF21-1CG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.94kW; UDC=300V; M0=3. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",3185,"ΤΕΜ",1,"GMC",1,"1FK70434CF211CG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7043-4CH71-1CB2","SIMOTICS S Synchronous motor 1FK7-HD PN=1.2kW; UDC=600V M0=3.5Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",3796,"ΤΕΜ",1,"GMC",1,"1FK70434CH711CB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7043-4CH74-1AG0","SIMOTICS S Synchronous motor 1FK7-HD PN=1.2kW; UDC=600V M0=3.5Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2336,"ΤΕΜ",1,"GMC",1,"1FK70434CH741AG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7043-4CK71-1CA2","SIMOTICS S Synchronous motor 1FK7-HD PN=1.3kW; UDC=600V M0=3.5Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",3433,"ΤΕΜ",1,"GMC",1,"1FK70434CK711CA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7043-4CK71-1PH0","SIMOTICS S Synchronous motor 1FK7-HD PN=1.3kW; UDC=600V M0=3.5Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2216,"ΤΕΜ",1,"GMC",1,"1FK70434CK711PH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7043-4CK74-1AB1","SIMOTICS S Synchronous motor 1FK7-HD PN=1.3kW; UDC=600V M0=3.5Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2946,"ΤΕΜ",1,"GMC",1,"1FK70434CK741AB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7044-4CF71-1QH0","SIMOTICS S Synchronous motor 1FK7-HD PN=1.2kW; UDC=600V M0=4.5Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2458,"ΤΕΜ",1,"GMC",1,"1FK70444CF711QH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7044-4CF74-1EH0","SIMOTICS S Synchronous motor 1FK7-HD PN=1.2kW; UDC=600V M0=4.5Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",3311,"ΤΕΜ",1,"GMC",1,"1FK70444CF741EH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7044-4CH71-1CB1","SIMOTICS S Synchronous motor 1FK7-HD PN=1.4kW; UDC=600V M0=4.5Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",3894,"ΤΕΜ",1,"GMC",1,"1FK70444CH711CB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7044-4CH71-1QB1","SIMOTICS S Synchronous motor 1FK7-HD PN=1.4kW; UDC=600V M0=4.5Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2708,"ΤΕΜ",1,"GMC",1,"1FK70444CH711QB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7060-2AC71-1BH2","SIMOTICS S Synchronous motor 1FK7-CT PN=1.1kW; UDC=600V M0=6Nm (100K); NN=2000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 24-bit with Drive-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N with holding brake IP65 degree of protection DE flange IP67",3463,"ΤΕΜ",1,"GMC",1,"1FK70602AC711BH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7060-2AC71-1DG2","SIMOTICS S Synchronous motor 1FK7-CT PN=1.1kW; UDC=600V M0=6Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",3147,"ΤΕΜ",1,"GMC",1,"1FK70602AC711DG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7060-2AC74-1AB0","SIMOTICS S Synchronous motor 1FK7-CT PN=1.1kW; UDC=600V M0=6Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",3114,"ΤΕΜ",1,"GMC",1,"1FK70602AC741AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7060-2AF71-1CA0","SIMOTICS S synchronous motor 1FK7-CT PN=1.5kW; UDC=600V M0=6Nm (100K); NN=3000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 24-bit + 12-bit multiturn with DRIVE-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N without holding brake, degree of protection IP64",3542,"ΤΕΜ",1,"GMC",1,"1FK70602AF711CA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7060-2AF71-1UG1","SIMOTICS S synchronous motor 1FK7-CT PN=1.5 kW; UDC=600 V M0=6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake degree of protection IP65",2223,"ΤΕΜ",1,"GMC",1,"1FK70602AF711UG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7060-2AF74-1SH1","SIMOTICS S synchronous motor 1FK7-CT PN=1.5 kW; UDC=600V M0=6Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=4) smooth shaft, tolerance N with holding brake, type of protection IP65",2312,"ΤΕΜ",1,"GMC",1,"1FK70602AF741SH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7060-2AH71-1RB1","SIMOTICS S synchronous motor 1FK7-CT PN=1.7 kW; UDC=600 V M0=6 Nm (100K); NN=4500 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 20-bit +12- bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65",3428,"ΤΕΜ",1,"GMC",1,"1FK70602AH711RB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7060-2AH74-1AA1","SIMOTICS S Synchronous motor 1FK7-CT PN=1.7kW; UDC=600V M0=6Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2823,"ΤΕΜ",1,"GMC",1,"1FK70602AH741AA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7060-2AH74-1TH2","SIMOTICS S synchronous motor 1FK7-CT PN=1.7 kW; UDC=600V M0=6Nm (100K); NN=4500rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N with holding brake, degree of protection IP65 DE Flange IP67",2312,"ΤΕΜ",1,"GMC",1,"1FK70602AH741TH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7060-3BF74-1AH0","SIMOTICS S Synchronous motor 1FK7-HI PN=1.5kW; UDC=600V M0=6Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VP 2048 S/R WITH C- AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2997,"ΤΕΜ",1,"GMC",1,"1FK70603BF741AH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7061-4CF71-1RB0","SIMOTICS S Synchronous motor 1FK7-HD PN=1.7kW; UDC=600V M0=6.4Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",3452,"ΤΕΜ",1,"GMC",1,"1FK70614CF711RB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7061-4CF74-1AG0","SIMOTICS S Synchronous motor 1FK7-HD PN=1.7kW; UDC=600V M0=6.4Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2727,"ΤΕΜ",1,"GMC",1,"1FK70614CF741AG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7061-4CF74-1TG2","SIMOTICS S Synchronous motor 1FK7-HD PN=1.7kW; UDC=600V M0=6.4Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2039,"ΤΕΜ",1,"GMC",1,"1FK70614CF741TG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7061-4CH74-1EH0","SIMOTICS S Synchronous motor 1FK7-HD PN=2kW; UDC=600V M0=6.4Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",3668,"ΤΕΜ",1,"GMC",1,"1FK70614CH741EH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7062-2AC71-1CA0","SIMOTICS S synchronous motor 1FK7-CT PN=1.5kW; UDC=600V M0=8.5Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 24-bit + 12-bit multiturn with DRIVE-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N without holding brake, degree of protection IP64",3722,"ΤΕΜ",1,"GMC",1,"1FK70622AC711CA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7062-2AC71-1RG2","SIMOTICS S synchronous motor 1FK7-CT PN=1.5kW; UDC=600V M0=8.5Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 20-bit + 12-bit multiturn with DRIVE-CLiQ interface (encoder AM20DQI) Smooth shaft, tolerance N without holding brake, degree of protection IP65 DE Flange, IP67",3067,"ΤΕΜ",1,"GMC",1,"1FK70622AC711RG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7062-2AC74-1SB0","SIMOTICS S synchronous motor 1FK7-CT PN=1.5 kW; UDC=600V M0=8.5Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=4) shaft with feather key, tolerance N with holding brake degree of protection IP64",2479,"ΤΕΜ",1,"GMC",1,"1FK70622AC741SB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7062-2AF71-1QG1","SIMOTICS S synchronous motor 1FK7-CT PN=1.9 kW; UDC=600 V M0=8.5 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N without holding brake degree of protection IP65",2547,"ΤΕΜ",1,"GMC",1,"1FK70622AF711QG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7062-2AF74-1EG0","SIMOTICS S Synchronous motor 1FK7-CT PN=1.9kW; UDC=600V M0=8.5Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",3270,"ΤΕΜ",1,"GMC",1,"1FK70622AF741EG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7062-2AF74-1TA0","SIMOTICS S synchronous motor 1FK7-CT PN=1.9 kW; UDC=600V M0=8.5Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N without holding brake degree of protection IP64",2058,"ΤΕΜ",1,"GMC",1,"1FK70622AF741TA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7062-2AH71-1RG2","SIMOTICS S synchronous motor 1FK7-CT PN=1.4 kW; UDC=600V M0=8.5Nm (100K); NN=4500rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N without holding brake degree of protection IP65, DE flange IP67",3067,"ΤΕΜ",1,"GMC",1,"1FK70622AH711RG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7062-2AH74-1TA0","SIMOTICS S synchronous motor 1FK7-CT PN=1.4 kW; UDC=600V M0=8.5Nm (100K); NN=4500rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N without holding brake degree of protection IP64",2058,"ΤΕΜ",1,"GMC",1,"1FK70622AH741TA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7062-3BF71-1RB0","SIMOTICS S synchronous motor 1FK7-HI PN=1.9 kW; UDC=600 V M0=8.5 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 20-bit +12- bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N with holding brake degree of protection IP64",3479,"ΤΕΜ",1,"GMC",1,"1FK70623BF711RB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7063-2AC71-1PB2","SIMOTICS S synchronous motor 1FK7-CT PN=1.9 kW; UDC=600 V M0=11 Nm (100K); NN=2000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake degree of protection IP65 DE flange IP67",3075,"ΤΕΜ",1,"GMC",1,"1FK70632AC711PB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7063-2AC71-1UA1","SIMOTICS S synchronous motor 1FK7-CT PN=1.9 kW; UDC=600 V M0=11 Nm (100K); NN=2000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake degree of protection IP65",2654,"ΤΕΜ",1,"GMC",1,"1FK70632AC711UA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7063-2AC74-1EH1","SIMOTICS S Synchronous motor 1FK7-CT PN=1.9kW; UDC=600V M0=11Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",3953,"ΤΕΜ",1,"GMC",1,"1FK70632AC741EH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7063-2AF71-1RA2","SIMOTICS S synchronous motor 1FK7-CT PN=2.3kW; UDC=600V M0=11Nm (100K); NN=3000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 20-bit + 12-bit multiturn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N without holding brake, degree of protection IP65 DE Flange, IP67",3317,"ΤΕΜ",1,"GMC",1,"1FK70632AF711RA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7063-2AF74-1EH0","SIMOTICS S Synchronous motor 1FK7-CT PN=2.3kW; UDC=600V M0=11Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",3825,"ΤΕΜ",1,"GMC",1,"1FK70632AF741EH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7063-2AH71-1DG2","SIMOTICS S Synchronous motor 1FK7-CT PN=1.4kW; UDC=600V M0=11Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",3458,"ΤΕΜ",1,"GMC",1,"1FK70632AH711DG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7063-2AH71-1UA0","SIMOTICS S synchronous motor 1FK7-CT PN=1.4 kW; UDC=600 V M0=11 Nm (100K); NN=4500 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake degree of protection IP64",2524,"ΤΕΜ",1,"GMC",1,"1FK70632AH711UA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7064-4CC71-1CG0","SIMOTICS S Synchronous motor 1FK7-HD PN=2.1kW; UDC=600V M0=12Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",3954,"ΤΕΜ",1,"GMC",1,"1FK70644CC711CG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7064-4CC71-1PH2","SIMOTICS S Synchronous motor 1FK7-HD PN=2.1kW; UDC=600V M0=12Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",3177,"ΤΕΜ",1,"GMC",1,"1FK70644CC711PH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7064-4CC74-1AG0","SIMOTICS S Synchronous motor 1FK7-HD PN=2.1kW; UDC=600V M0=12Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",3105,"ΤΕΜ",1,"GMC",1,"1FK70644CC741AG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7064-4CF71-1CB0","SIMOTICS S Synchronous motor 1FK7-HD PN=2.5kW; UDC=600V M0=12Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",4496,"ΤΕΜ",1,"GMC",1,"1FK70644CF711CB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7064-4CF71-1UH0","SIMOTICS S Synchronous motor 1FK7-HD PN=2.5kW; UDC=600V M0=12Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",3050,"ΤΕΜ",1,"GMC",1,"1FK70644CF711UH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7064-4CH71-1DA1","SIMOTICS S Synchronous motor 1FK7-HD PN=2.4kW; UDC=600V M0=12Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",3799,"ΤΕΜ",1,"GMC",1,"1FK70644CH711DA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7064-4CH71-1RG2","SIMOTICS S Synchronous motor 1FK7-HD PN=2.4kW; UDC=600V M0=12Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",3416,"ΤΕΜ",1,"GMC",1,"1FK70644CH711RG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7080-2AF71-1CG0","SIMOTICS S synchronous motor 1FK7-CT PN=2.1 kW; UDC=600 V M0=8 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12- bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N without holding brake degree of protection IP64",3659,"ΤΕΜ",1,"GMC",1,"1FK70802AF711CG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7080-2AF71-1PB0","SIMOTICS S synchronous motor 1FK7-CT PN=2.1 kW; UDC=600 V M0=8 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake degree of protection IP64",3022,"ΤΕΜ",1,"GMC",1,"1FK70802AF711PB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7080-2AF74-1SA2","SIMOTICS S synchronous motor 1FK7-CT PN=2.1 kW; UDC=600V M0=8Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=4) shaft with feather key, tolerance N without holding brake degree of protection IP65, DE flange IP67",2244,"ΤΕΜ",1,"GMC",1,"1FK70802AF741SA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7080-2AH71-1DH0","SIMOTICS S Synchronous motor 1FK7-CT PN=2.1kW; UDC=600V M0=8Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",3829,"ΤΕΜ",1,"GMC",1,"1FK70802AH711DH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7080-2AH74-1SA1","SIMOTICS S synchronous motor 1FK7-CT PN=2.1 kW; UDC=600V M0=8Nm (100K); NN=4500rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=4) shaft with feather key, tolerance N without holding brake degree of protection IP65",2244,"ΤΕΜ",1,"GMC",1,"1FK70802AH741SA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7081-2AC71-1CG2","SIMOTICS S synchronous motor 1FK7-CT PN=2.1 kW; UDC=600V M0=12Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N without holding brake degree of protection IP65, DE flange IP67",4091,"ΤΕΜ",1,"GMC",1,"1FK70812AC711CG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7081-2AC71-1QB0","SIMOTICS S synchronous motor 1FK7-CT PN=2.1 kW; UDC=600V M0=12Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N with holding brake degree of protection IP64",3468,"ΤΕΜ",1,"GMC",1,"1FK70812AC711QB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7081-2AC74-1TA0","SIMOTICS S synchronous motor 1FK7-CT PN=2.1 kW; UDC=600V M0=12Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N without holding brake degree of protection IP64",2417,"ΤΕΜ",1,"GMC",1,"1FK70812AC741TA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7081-2AF71-1FB0","SIMOTICS S Synchronous motor 1FK7-CT PN=2.7kW; UDC=600V M0=12Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",4765,"ΤΕΜ",1,"GMC",1,"1FK70812AF711FB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7081-2AF74-1EA0","SIMOTICS S Synchronous motor 1FK7-CT PN=2.7kW; UDC=600V M0=12Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",3749,"ΤΕΜ",1,"GMC",1,"1FK70812AF741EA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7081-2AH71-1CH0","SIMOTICS S synchronous motor 1FK7-CT PN=1.8 kW; UDC=600V M0=12Nm (100K); NN=4500rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N with holding brake degree of protection IP64",4534,"ΤΕΜ",1,"GMC",1,"1FK70812AH711CH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7081-2AH74-1EH0","SIMOTICS S Synchronous motor 1FK7-CT PN=1.8kW; UDC=600V M0=12Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) Smooth shaft, tolerance N With holding brake PROTECTION CLASS IP64;",4201,"ΤΕΜ",1,"GMC",1,"1FK70812AH741EH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7081-3BF71-1CB0","SIMOTICS S synchronous motor 1FK7-HI PN=2.7kW; UDC=600V M0=12Nm (100K); NN=3000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 24-bit + 12-bit multiturn with DRIVE-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N with holding brake, degree of protection IP64",4654,"ΤΕΜ",1,"GMC",1,"1FK70813BF711CB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7083-2AC71-1BB1","SIMOTICS S synchronous motor 1FK7-CT PN=2.6kW; UDC=600V M0=16Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 24-bit with Drive-CLiQ interface (encoder AS24DQI) shaft with feather key, tolerance N with holding brake, degree of protection IP65",4420,"ΤΕΜ",1,"GMC",1,"1FK70832AC711BB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7083-2AC71-1DA1","SIMOTICS S Synchronous motor 1FK7-CT PN=2.6kW; UDC=600V M0=16Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",3956,"ΤΕΜ",1,"GMC",1,"1FK70832AC711DA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7083-2AC74-1EG1","SIMOTICS S Synchronous motor 1FK7-CT PN=2.6kW; UDC=600V M0=16Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",3906,"ΤΕΜ",1,"GMC",1,"1FK70832AC741EG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7083-2AF71-1CA2","SIMOTICS S synchronous motor 1FK7-CT PN=3.3kW; UDC=600V M0=16Nm (100K); NN=3000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 24-bit + 12-bit multiturn with DRIVE-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N without holding brake, degree of protection IP65 DE Flange, IP67",4361,"ΤΕΜ",1,"GMC",1,"1FK70832AF711CA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7083-2AF71-1UG2","SIMOTICS S synchronous motor 1FK7-CT PN=3.3 kW; UDC=600 V M0=16 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake degree of protection IP65 DE flange IP67",2912,"ΤΕΜ",1,"GMC",1,"1FK70832AF711UG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7083-2AF74-1EH1","SIMOTICS S Synchronous motor 1FK7-CT PN=3.3kW; UDC=600V M0=16Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",4479,"ΤΕΜ",1,"GMC",1,"1FK70832AF741EH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7083-2AH71-1CA0","SIMOTICS S synchronous motor 1FK7-CT PN=1.4 kW; UDC=600 V M0=16 Nm (100K); NN=4500 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12- bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N without holding brake degree of protection IP64",4231,"ΤΕΜ",1,"GMC",1,"1FK70832AH711CA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7083-2AH74-1AA2","SIMOTICS S Synchronous motor 1FK7-CT PN=1.4kW; UDC=600V M0=16Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",3512,"ΤΕΜ",1,"GMC",1,"1FK70832AH741AA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7084-2AC71-1CB0","SIMOTICS S synchronous motor 1FK7-CT PN=3.1 kW; UDC=600 V M0=20 Nm (100K); NN=2000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12- bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N with holding brake degree of protection IP64",5218,"ΤΕΜ",1,"GMC",1,"1FK70842AC711CB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7084-2AC71-1RH0","SIMOTICS S synchronous motor 1FK7-CT PN=3.1 kW; UDC=600 V M0=20 Nm (100K); NN=2000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 20-bit +12- bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N with holding brake degree of protection IP64",4432,"ΤΕΜ",1,"GMC",1,"1FK70842AC711RH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7084-2AC74-1AG0","SIMOTICS S Synchronous motor 1FK7-CT PN=3.1kW; UDC=600V M0=20Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",3676,"ΤΕΜ",1,"GMC",1,"1FK70842AC741AG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7084-2AF71-1QG0","SIMOTICS S synchronous motor 1FK7-CT PN=3.1kW; UDC=600V M0=20Nm (100K); NN=3000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 20-bit with Drive-CLiQ interface (encoder AS20DQI) Smooth shaft, tolerance N without holding brake, degree of protection IP64",3340,"ΤΕΜ",1,"GMC",1,"1FK70842AF711QG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7084-2AF71-1UG0","SIMOTICS S synchronous motor 1FK7-CT PN=3.1 kW; UDC=600 V M0=20 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake degree of protection IP64",3196,"ΤΕΜ",1,"GMC",1,"1FK70842AF711UG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7084-2AF74-1TA1","SIMOTICS S synchronous motor 1FK7-CT PN=3.1 kW; UDC=600V M0=20Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N without holding brake degree of protection IP65",3111,"ΤΕΜ",1,"GMC",1,"1FK70842AF741TA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7084-3BC71-1RH0","SIMOTICS S synchronous motor 1FK7-HI PN=3.1kW; UDC=600V M0=20Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 20-bit + 12-bit multiturn with DRIVE-CLiQ interface (encoder AM20DQI) Smooth shaft, tolerance N with holding brake, degree of protection IP64",4432,"ΤΕΜ",1,"GMC",1,"1FK70843BC711RH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7084-3BF71-1QH0","SIMOTICS S synchronous motor 1FK7-HI PN=3.1 kW; UDC=600 V M0=20 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N with holding brake degree of protection IP64",3912,"ΤΕΜ",1,"GMC",1,"1FK70843BF711QH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7084-3BF74-1EH2","SIMOTICS S Synchronous motor 1FK7-HI PN=3.1kW; UDC=600V M0=20Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) Smooth shaft, tolerance N With holding brake PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",4896,"ΤΕΜ",1,"GMC",1,"1FK70843BF741EH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7085-4CC71-1CG2","SIMOTICS S Synchronous motor 1FK7-HD PN=3.1kW; UDC=600V M0=22Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",4848,"ΤΕΜ",1,"GMC",1,"1FK70854CC711CG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7085-4CC74-1SH1","SIMOTICS S Synchronous motor 1FK7-HD PN=3.1kW; UDC=600V M0=22Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",3756,"ΤΕΜ",1,"GMC",1,"1FK70854CC741SH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7085-4CF71-1CG1","SIMOTICS S Synchronous motor 1FK7-HD PN=2kW; UDC=600V M0=22Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",4848,"ΤΕΜ",1,"GMC",1,"1FK70854CF711CG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7085-4CF74-1EB0","SIMOTICS S Synchronous motor 1FK7-HD PN=2kW; UDC=600V M0=22Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",5080,"ΤΕΜ",1,"GMC",1,"1FK70854CF741EB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7086-4CC71-1PG1","SIMOTICS S Synchronous motor 1FK7-HD PN=3.8kW; UDC=600V M0=28Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",4073,"ΤΕΜ",1,"GMC",1,"1FK70864CC711PG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7086-4CC74-1EA0","SIMOTICS S Synchronous motor 1FK7-HD PN=3.8kW; UDC=600V M0=28Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",5062,"ΤΕΜ",1,"GMC",1,"1FK70864CC741EA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7086-4CC74-1SH0","SIMOTICS S Synchronous motor 1FK7-HD PN=3.8kW; UDC=600V M0=28Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",4182,"ΤΕΜ",1,"GMC",1,"1FK70864CC741SH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7086-4CF71-1PA2","SIMOTICS S Synchronous motor 1FK7-HD PN=2kW; UDC=600V M0=28Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",4193,"ΤΕΜ",1,"GMC",1,"1FK70864CF711PA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7086-4CF74-1SB1","SIMOTICS S Synchronous motor 1FK7-HD PN=2kW; UDC=600V M0=28Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",4429,"ΤΕΜ",1,"GMC",1,"1FK70864CF741SB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7086-4SF71-1UG1","SIMOTICS S Synchronous motor 1FK7 High Dynamic, 38Nm 100K; NN=3000rpm; 7.50kW Forced ventilation FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",5981,"ΤΕΜ",1,"GMC",1,"1FK70864SF711UG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7100-2AC71-1RA0","SIMOTICS S synchronous motor 1FK7-CT PN=3 kW; UDC=600V M0=18Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N without holding brake degree of protection IP64",3911,"ΤΕΜ",1,"GMC",1,"1FK71002AC711RA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7100-2AF71-1CH1","SIMOTICS S Synchronous motor 1FK7-CT PN=3.8kW; UDC=600V M0=18Nm (100K); NN=3000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 24-bit +12-bit multi-turn with Drive-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N with holding brake IP65 degree of protection",5158,"ΤΕΜ",1,"GMC",1,"1FK71002AF711CH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7100-2AF71-1RB1","SIMOTICS S Synchronous motor 1FK7-CT PN=3.8kW; UDC=600V M0=18Nm (100K); NN=3000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 20-bit +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N with holding brake IP65 degree of protection",4613,"ΤΕΜ",1,"GMC",1,"1FK71002AF711RB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7100-2AF74-1EB2","SIMOTICS S Synchronous motor 1FK7-CT PN=3.8kW; UDC=600V M0=18Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",4943,"ΤΕΜ",1,"GMC",1,"1FK71002AF741EB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7100-3BC74-1AB0","SIMOTICS S Synchronous motor 1FK7-HI PN=3kW; UDC=600V M0=18Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VP 2048 S/R WITH C- AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",4287,"ΤΕΜ",1,"GMC",1,"1FK71003BC741AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7101-2AC71-1BA0","SIMOTICS S Synchronous motor 1FK7-CT PN=4.3kW; UDC=600V M0=27Nm (100K); NN=2000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 24-bit with Drive-CLiQ interface (encoder AS24DQI) shaft with feather key, tolerance N without holding brake IP64 degree of protection",4508,"ΤΕΜ",1,"GMC",1,"1FK71012AC711BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7101-2AC71-1RG2","SIMOTICS S Synchronous motor 1FK7-CT PN=4.3kW; UDC=600V M0=27Nm (100K); NN=2000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 20-bit +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N without holding brake IP65 degree of protection DE flange IP67",4367,"ΤΕΜ",1,"GMC",1,"1FK71012AC711RG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7101-2AC74-1SG1","SIMOTICS S synchronous motor 1FK7-CT PN=4.3 kW; UDC=600V M0=27 Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=4) smooth shaft, tolerance N without holding brake, type of protection IP65",3367,"ΤΕΜ",1,"GMC",1,"1FK71012AC741SG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7101-2AF71-1QG1","SIMOTICS S synchronous motor 1FK7-CT PN=4.9kW; UDC=600V M0=27Nm (100K); NN=3000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 20-bit with Drive-CLiQ interface (encoder AS20DQI) Smooth shaft, tolerance N without holding brake, degree of protection IP65",3846,"ΤΕΜ",1,"GMC",1,"1FK71012AF711QG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7101-2AF74-1EH1","SIMOTICS S Synchronous motor 1FK7-CT PN=4.9kW; UDC=600V M0=27Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",5269,"ΤΕΜ",1,"GMC",1,"1FK71012AF741EH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7101-2AF74-1SH2","SIMOTICS S synchronous motor 1FK7-CT PN=4.9 kW; UDC=600V M0=27 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=4) smooth shaft, tolerance N with holding brake, degree of protection IP65 DE Flange IP67",3940,"ΤΕΜ",1,"GMC",1,"1FK71012AF741SH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7101-3BC74-1EA0","SIMOTICS S Synchronous motor 1FK7-HI PN=4.3kW; UDC=600V M0=27Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",4672,"ΤΕΜ",1,"GMC",1,"1FK71013BC741EA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7101-3BF71-1QG1","SIMOTICS S synchronous motor 1FK7-HI PN=4.9 kW; UDC=600V M0=27 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N without holding brake degree of protection IP65",3828,"ΤΕΜ",1,"GMC",1,"1FK71013BF711QG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7103-2AC71-1CH0","SIMOTICS S Synchronous motor 1FK7-CT PN=5.2kW; UDC=600V M0=36Nm (100K); NN=2000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 24-bit +12-bit multi-turn with Drive-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N with holding brake IP64 degree of protection",6062,"ΤΕΜ",1,"GMC",1,"1FK71032AC711CH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7103-2AC71-1QH0","SIMOTICS S Synchronous motor 1FK7-CT PN=5.2kW; UDC=600V M0=36Nm (100K); NN=2000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 20-bit with Drive-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N with holding brake IP64 degree of protection",4876,"ΤΕΜ",1,"GMC",1,"1FK71032AC711QH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7103-2AF71-1CH1","SIMOTICS S Synchronous motor 1FK7-CT PN=4.4kW; UDC=600V M0=36Nm (100K); NN=3000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 24-bit +12-bit multi-turn with Drive-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N with holding brake IP65 degree of protection",6192,"ΤΕΜ",1,"GMC",1,"1FK71032AF711CH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7103-2AF71-1RA0","SIMOTICS S Synchronous motor 1FK7-CT PN=4.4kW; UDC=600V M0=36Nm (100K); NN=3000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 20-bit +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N without holding brake IP64 degree of protection",4944,"ΤΕΜ",1,"GMC",1,"1FK71032AF711RA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7103-2AF74-1SG1","SIMOTICS S synchronous motor 1FK7-CT PN=4.4 kW; UDC=600V M0=36 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=4) smooth shaft, tolerance N without holding brake, type of protection IP65",3955,"ΤΕΜ",1,"GMC",1,"1FK71032AF741SG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7103-3BC71-1QA1","SIMOTICS S synchronous motor 1FK7-HI PN=5.2kW; UDC=600V M0=36Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 20-bit with Drive-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N without holding brake, degree of protection IP65",4530,"ΤΕΜ",1,"GMC",1,"1FK71033BC711QA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7103-3BF71-1QB1","SIMOTICS S synchronous motor 1FK7-HI PN=4.4 kW; UDC=600V M0=36 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65",5102,"ΤΕΜ",1,"GMC",1,"1FK71033BF711QB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7103-3BF74-1EH2","SIMOTICS S Synchronous motor 1FK7-HI PN=4.4kW; UDC=600V M0=36Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",5836,"ΤΕΜ",1,"GMC",1,"1FK71033BF741EH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7105-2AC71-1RG2","SIMOTICS S Synchronous motor 1FK7-CT PN=7.7kW; UDC=600V M0=48Nm (100K); NN=2000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 20-bit +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N without holding brake IP65 degree of protection DE flange IP67",6431,"ΤΕΜ",1,"GMC",1,"1FK71052AC711RG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7105-2AC74-1TB0","SIMOTICS S synchronous motor 1FK7-CT PN=7.7 kW; UDC=600V M0=48Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N with holding brake degree of protection IP64",5994,"ΤΕΜ",1,"GMC",1,"1FK71052AC741TB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7105-2AF71-1BA0","SIMOTICS S Synchronous motor 1FK7-CT PN=8.2kW; UDC=600V M0=48Nm (100K); NN=3000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 24-bit with Drive-CLiQ interface (encoder AS24DQI) shaft with feather key, tolerance N without holding brake IP64 degree of protection",6573,"ΤΕΜ",1,"GMC",1,"1FK71052AF711BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7105-2AF71-1RH1","SIMOTICS S Synchronous motor 1FK7-CT PN=8.2kW; UDC=600V M0=48Nm (100K); NN=3000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 20-bit +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N with holding brake IP65 degree of protection",7004,"ΤΕΜ",1,"GMC",1,"1FK71052AF711RH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7105-2AF74-1TH2","SIMOTICS S synchronous motor 1FK7-CT PN=8.2 kW; UDC=600V M0=48Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N with holding brake, degree of protection IP65 DE Flange IP67",6004,"ΤΕΜ",1,"GMC",1,"1FK71052AF741TH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FK7105-3BC74-1AG2","SIMOTICS S Synchronous motor 1FK7-HI PN=7.7kW; UDC=600V M0=48Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VP 2048 S/R WITH C- AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",6209,"ΤΕΜ",1,"GMC",1,"1FK71053BC741AG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FL2102-2AF00-1SC0","SIMOTICS S-1FL2 Supply voltage 400V 3AC Pn=50W;Nn=3000rpm M0=0.16Nm;Mn=0.16Nm Shaft height 20mm With hybrid connector AS21bit With shaft key, Tolerance N Without holding brake Protection class IP54 without oil seal Matching drive SINAMICS S200",800,"ΤΕΜ",1,"GMC",1,"1FL21022AF001SC0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FL2103-2AF00-1MC0","SIMOTICS S-1FL2 Supply voltage 400V 3AC Pn=0.2kW;Nn=3000rpm M0=0.64Nm;Mn=0.64Nm Shaft height 30mm With hybrid connector AM21bit With shaft key, Tolerance N Without holding brake Protection class IP54 without oil seal Matching drive SINAMICS S200",1133,"ΤΕΜ",1,"GMC",1,"1FL21032AF001MC0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FL2103-2AG00-1MC0","SIMOTICS S-1FL2 Supply voltage 200V 3AC Pn=0.2kW;Nn=3000rpm M0=0.64Nm;Mn=0.64Nm Shaft height 30mm With hybrid connector AM21bit With shaft key, Tolerance N Without holding brake Protection class IP54 without oil seal Matching drive SINAMICS S200",1133,"ΤΕΜ",1,"GMC",1,"1FL21032AG001MC0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FL2104-2AF01-0MC0","SIMOTICS S-1FL2 Supply voltage 400V 3AC Pn=0.75kW;Nn=3000rpm M0=2.4Nm;Mn=2.4Nm Shaft height 40mm With hybrid connector AM21bit Plain shaft, Tolerance N Without holding brake Protection class IP65 with oil seal Matching drive SINAMICS S200",1400,"ΤΕΜ",1,"GMC",1,"1FL21042AF010MC0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FL2104-2AG00-1HC0","SIMOTICS S-1FL2 Supply voltage 200V 3AC Pn=0.75kW;Nn=3000rpm M0=2.4Nm;Mn=2.4Nm Shaft height 40mm With hybrid connector AS17bit With shaft key, Tolerance N Without holding brake Protection class IP54 without oil seal Matching drive SINAMICS S200",769,"ΤΕΜ",1,"GMC",1,"1FL21042AG001HC0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FL2203-2AF01-0HC0","SIMOTICS S-1FL2 Supply voltage 400V 3AC Pn=0.2kW;Nn=3000rpm M0=0.64Nm;Mn=0.64Nm Shaft height 30mm With hybrid connector AS17bit Plain shaft, Tolerance N Without holding brake Protection class IP65 with oil seal Matching drive SINAMICS S200",628,"ΤΕΜ",1,"GMC",1,"1FL22032AF010HC0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FL2203-4AF00-0MC0","SIMOTICS S-1FL2 Supply voltage 400V 3AC Pn=0.4kW;Nn=3000rpm M0=1.27Nm;Mn=1.27Nm Shaft height 30mm With hybrid connector AM21bit Plain shaft, Tolerance N Without holding brake Protection class IP54 without oil seal Matching drive SINAMICS S200",1184,"ΤΕΜ",1,"GMC",1,"1FL22034AF000MC0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FL2203-4AF11-1MC0","SIMOTICS S-1FL2 Supply voltage 400V 3AC Pn=0.4kW;Nn=3000rpm M0=1.27Nm;Mn=1.27Nm Shaft height 30mm With hybrid connector AM21bit With shaft key, Tolerance N With holding brake Protection class IP65 with oil seal Matching drive SINAMICS S200",1518,"ΤΕΜ",1,"GMC",1,"1FL22034AF111MC0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FL2204-2AG01-1MC0","SIMOTICS S-1FL2 Supply voltage 200V 3AC Pn=0.75kW;Nn=3000rpm M0=2.4Nm;Mn=2.4Nm Shaft height 40mm With hybrid connector AM21bit With shaft key, Tolerance N Without holding brake Protection class IP65 with oil seal Matching drive SINAMICS S200",1400,"ΤΕΜ",1,"GMC",1,"1FL22042AG011MC0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FL2204-4AG11-1HC0","SIMOTICS S-1FL2 Supply voltage 200V 3AC Pn=1kW;Nn=3000rpm M0=3.2Nm;Mn=3.2Nm Shaft height 40mm With hybrid connector AS17bit With shaft key, Tolerance N With holding brake Protection class IP65 with oil seal Matching drive SINAMICS S200",1242,"ΤΕΜ",1,"GMC",1,"1FL22044AG111HC0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FL2306-4AC01-0HB0","SIMOTICS S-1FL2 Supply voltage 400V 3AC Pn=1.5kW;Nn=2000rpm M0=8Nm;Mn=7.16Nm Shaft height 65mm With angular connector AS17bit Plain shaft, Tolerance N Without holding brake Protection class IP65 with oil seal Matching drive SINAMICS S200",1108,"ΤΕΜ",1,"GMC",1,"1FL23064AC010HB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FL2310-4AC11-0HB0","SIMOTICS S-1FL2 Supply voltage 400V 3AC Pn=5kW;Nn=2000rpm M0=25.2Nm;Mn=23.9Nm Shaft height 90mm With angular connector AS17bit Plain shaft, Tolerance N With holding brake Protection class IP65 with oil seal Matching drive SINAMICS S200",3295,"ΤΕΜ",1,"GMC",1,"1FL23104AC110HB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FL6032-2AF21-1MH1","SIMOTICS S-1FL6 voltage supply 230 V 3AC Pn=0.2 kW; Nn=3000 rpm M0=0.64 Nm; MN=0.64 Nm. Shaft height 30 mm absolute encoder Single-turn 21-bit with smooth shaft Tolerance N with holding brake Degree of protection IP65 with fitting oil seal for drive V90",1091,"ΤΕΜ",1,"GMC",1,"1FL60322AF211MH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FL6042-2AF21-1AA1","SIMOTICS S-1FL6 Operating voltage 230 V 3AC Pn=0.75 kW; Nn=3000 rpm M0=2.39 Nm; MN=2.39 Nm Shaft height 40 mm Incremental encoder TTL 2500 incr./rev. with feather key Tolerance N without holding brake Degree of protection IP65 with sealing ring compatible with the converters SINAMICS V90",718,"ΤΕΜ",1,"GMC",1,"1FL60422AF211AA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FL6054-2AF21-2AB1","SIMOTICS S-1FL6 Operating voltage 230 V 3AC PN=2 kW; NN=3000 rpm M0=6.37 Nm; MN=6.37 Nm shaft he 50 mm with angle plug encoder incremental TTL 2500 incr./rev. with feather key Tolerance N wi holding brake, Degree of protec sealing ring compatible with th converters SINAMICS V90",1703,"ΤΕΜ",1,"GMC",1,"1FL60542AF212AB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FL6094-1AC61-2LH1","SIMOTICS S-1FL6-1FL6 Operating voltage 3AC 400 V Pn=5 kW; Nn=2000 rpm M0=30 Nm; MN=23.9 Nm Shaft height 90 mm, with angle plug; absolute encoder 20-bits (12-bit multi-turn) plain shaft, Tolerance N with holding brake Degree of protection IP65 with sealing ring compatible with the converters SINAMICS V70 & V90",3973,"ΤΕΜ",1,"GMC",1,"1FL60941AC612LH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FN3003-0TK02-1AD0","SIMOTICS L Cooling profile for secondary section Size 300 to 450 Hollow aluminum profile; per secondary section track 2 units required Length in number of secondary parts, cable grommet nipple Price per secondary section segment Number=0+3",103,"ΤΕΜ",1,"GMC",1,"1FN30030TK021AD0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FN3003-0TK04-1AG0","SIMOTICS L Secondary section cooling with plug-in coupling; Size 300 to 450; Hollow aluminum profile; per secondary section track 2 units required Length in number of secondary sections: 6",205,"ΤΕΜ",1,"GMC",1,"1FN30030TK041AG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FN3050-1ND00-0FA3","SIMOTICS L primary section; component 3-phase synchronous motor continuous load type FN=151 N; Fmax=255 N Vmax/FN= 429 m/min Vmax/Fmax= 236 m/min In=2.8 A; Imax=5.86 A with PTC120 and temperature sensor Pt1000 connection of power and signal separated with fixed-connected cables 0.5 m with plug size 1 and M17",2949,"ΤΕΜ",1,"GMC",1,"1FN30501ND000FA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FN3100-3PK10-0AA0","SIMOTICS L precision cooler for primary section 1FN3100-3N... Component 3-phase synchronous motor",637,"ΤΕΜ",1,"GMC",1,"1FN31003PK100AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FN3150-0TJ01-0AA0","SIMOTICS L Cooling profile connection for size 150; Component 3-phase synchronous motor; with plug-in coupling for water distribution and clamping of the Secondary section cover at each end of the secondary section track",443,"ΤΕΜ",1,"GMC",1,"1FN31500TJ010AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FN3300-1PK10-0AA0","SIMOTICS L precision cooler for primary section 1FN3300-1N... Component 3-phase synchronous motor",699,"ΤΕΜ",1,"GMC",1,"1FN33001PK100AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FN3450-0TB00-1AF0","SIMOTICS L Cover for 1 secondary section track, Size 450; cold-rolled sheet; Thickness 0.4 mm Price per secondary section segment; Length in number of secondary sections= 0 + 5",54.5,"ΤΕΜ",1,"GMC",1,"1FN34500TB001AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FN3450-4WB50-0BA3","SIMOTICS L primary section; component 3-phase synchronous motor peak load version FN=3860 N; Fmax=10300 N Vmax/FN= 236 m/min Vmax/Fmax= 102 m/min In=30.3 A; Imax=89.5 A with PTC120 and temperature sensor Pt1000 connection of power and signal separated connection via terminal box metric",5615,"ΤΕΜ",1,"GMC",1,"1FN34504WB500BA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FN3600-2WB00-0AA3","SIMOTICS L primary section; component 3-phase synchronous motor peak load version FN=2610 N; Fmax=6900 N Vmax/FN= 172 m/min Vmax/Fmax= 69.6 m/min In=16.8 A; Imax=45.8 A with PTC120 and temperature sensor Pt1000 connection of power and signal combined connection via terminal box PG",4454,"ΤΕΜ",1,"GMC",1,"1FN36002WB000AA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FN3900-4TP00-2BC0","SIMOTICS L Secondary section cover for size 900; component 3-phase synchronous motor; cover for 12 Secondary section segments",967,"ΤΕΜ",1,"GMC",1,"1FN39004TP002BC0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7034-1AK71-1BH1","SIMOTICS S Synchronous motor 1FT7, M0=2Nm (100K) NN=6000rpm, PN=0.88kW naturally cooled; Power connector rotatable; Vibration severity A Degree of protection IP65 Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N",4317,"ΤΕΜ",1,"GMC",1,"1FT70341AK711BH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7034-5AK70-1BB2","SIMOTICS S Synchronous motor 1FT7, M0=2Nm (100K) NN=6000rpm, PN=0.88kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",5436,"ΤΕΜ",1,"GMC",1,"1FT70345AK701BB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7034-5AK71-1CE1","SIMOTICS S Synchronous motor 1FT7, M0=2Nm (100K) NN=6000rpm, PN=0.88kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",6611,"ΤΕΜ",1,"GMC",1,"1FT70345AK711CE1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7034-5AK75-1NG1","SIMOTICS S Synchronous motor 1FT7, M0=2Nm (100K) NN=6000rpm, PN=0.88kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact), with Pt1000  temperature sensor POWER CONNECTOR ROTATABLE INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",3968,"ΤΕΜ",1,"GMC",1,"1FT70345AK751NG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7036-5AK70-1DA3","SIMOTICS S Synchronous motor 1FT7, M0=3Nm (100K) NN=6000rpm, PN=1.07kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",4829,"ΤΕΜ",1,"GMC",1,"1FT70365AK701DA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7036-5AK71-1CA1","SIMOTICS S Synchronous motor 1FT7, M0=3Nm (100K) NN=6000rpm, PN=1.07kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",5700,"ΤΕΜ",1,"GMC",1,"1FT70365AK711CA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7042-5AF70-1DH1","SIMOTICS S Synchronous motor 1FT7, M0=3Nm (100K) NN=3000rpm, PN=0.85kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",5759,"ΤΕΜ",1,"GMC",1,"1FT70425AF701DH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7042-5AF71-1BL2","SIMOTICS S Synchronous motor 1FT7, M0=3Nm (100K) NN=3000rpm, PN=0.85kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE R VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",5977,"ΤΕΜ",1,"GMC",1,"1FT70425AF711BL2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7042-5AF71-1FB5","SIMOTICS S Synchronous motor 1FT7, M0=3Nm (100K) NN=3000rpm, PN=0.85kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 67",7152,"ΤΕΜ",1,"GMC",1,"1FT70425AF711FB5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7042-5AK70-1CA2","SIMOTICS S Synchronous motor 1FT7, M0=3Nm (100K) NN=6000rpm, PN=1.26kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",5870,"ΤΕΜ",1,"GMC",1,"1FT70425AK701CA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7042-5AK71-1DG0","SIMOTICS S Synchronous motor 1FT7, M0=3Nm (100K) NN=6000rpm, PN=1.26kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",4672,"ΤΕΜ",1,"GMC",1,"1FT70425AK711DG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7042-5AK71-1FH0","SIMOTICS S Synchronous motor 1FT7, M0=3Nm (100K) NN=6000rpm, PN=1.26kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",6690,"ΤΕΜ",1,"GMC",1,"1FT70425AK711FH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7044-5AF70-1BG0","SIMOTICS S Synchronous motor 1FT7, M0=5Nm (100K) NN=3000rpm, PN=1.35kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",5065,"ΤΕΜ",1,"GMC",1,"1FT70445AF701BG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7044-5AF70-1FH2","SIMOTICS S Synchronous motor 1FT7, M0=5Nm (100K) NN=3000rpm, PN=1.35kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",7440,"ΤΕΜ",1,"GMC",1,"1FT70445AF701FH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7044-5AF71-1DH0","SIMOTICS S Synchronous motor 1FT7, M0=5Nm (100K) NN=3000rpm, PN=1.35kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",6130,"ΤΕΜ",1,"GMC",1,"1FT70445AF711DH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7044-5AK70-1DH0","SIMOTICS S Synchronous motor 1FT7, M0=5Nm (100K) NN=6000rpm, PN=1.41kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",6130,"ΤΕΜ",1,"GMC",1,"1FT70445AK701DH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7044-5AK71-1CG0","SIMOTICS S Synchronous motor 1FT7, M0=5Nm (100K) NN=6000rpm, PN=1.41kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",6130,"ΤΕΜ",1,"GMC",1,"1FT70445AK711CG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7046-5AF70-1CH3","SIMOTICS S Synchronous motor 1FT7, M0=7Nm (100K) NN=3000rpm, PN=1.76kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",7723,"ΤΕΜ",1,"GMC",1,"1FT70465AF701CH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7046-5AF70-1FA2","SIMOTICS S Synchronous motor 1FT7, M0=7Nm (100K) NN=3000rpm, PN=1.76kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",6910,"ΤΕΜ",1,"GMC",1,"1FT70465AF701FA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7046-5AF71-1FB0","SIMOTICS S Synchronous motor 1FT7, M0=7Nm (100K) NN=3000rpm, PN=1.76kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",7619,"ΤΕΜ",1,"GMC",1,"1FT70465AF711FB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7046-5AH70-1FG2","SIMOTICS S Synchronous motor 1FT7, M0=7Nm (100K) NN=4500rpm, PN=1.32kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",6910,"ΤΕΜ",1,"GMC",1,"1FT70465AH701FG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7062-1AK70-1DG1","SIMOTICS S Synchronous motor 1FT7, M0=6Nm (100K) NN=6000rpm, PN=2.13kW naturally cooled; Power connector rotatable; Vibration severity A Degree of protection IP65 Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACCURACY TOLERANCE N",4017,"ΤΕΜ",1,"GMC",1,"1FT70621AK701DG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7062-5AF70-1BH1","SIMOTICS S Synchronous motor 1FT7, M0=6Nm (100K) NN=3000rpm, PN=1.70kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",6230,"ΤΕΜ",1,"GMC",1,"1FT70625AF701BH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7062-5AF71-1FA0","SIMOTICS S Synchronous motor 1FT7, M0=6Nm (100K) NN=3000rpm, PN=1.70kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE Absolute encoder 22-bit Multiturn with DRIVE-CLiQ interface (encoder AM22DQ) Rotatable connector SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",6167,"ΤΕΜ",1,"GMC",1,"1FT70625AF711FA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7062-5AF71-1LA2","SIMOTICS S Synchronous motor 1FT7, M0=6Nm (100K) NN=3000rpm, PN=1.70kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) AND M17-CONNECTOR SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",6718,"ΤΕΜ",1,"GMC",1,"1FT70625AF711LA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7062-5AK71-1CK4","SIMOTICS S Synchronous motor 1FT7, M0=6Nm (100K) NN=6000rpm, PN=2.13kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",6628,"ΤΕΜ",1,"GMC",1,"1FT70625AK711CK4","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7062-5WK71-1BG0","SIMOTICS S Synchronous motor 1FT7, M0=10Nm (100K) NN=6000rpm, PN=5.80kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",5890,"ΤΕΜ",1,"GMC",1,"1FT70625WK711BG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7064-1AF71-1KG1","SIMOTICS S Synchronous motor 1FT7, M0=9Nm (100K) NN=3000rpm, PN=2.39kW naturally cooled; Power connector rotatable; Vibration severity A Degree of protection IP65 Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) AND M17 CONNECTOR PLAIN SHAFT, W/O HOLDING BRAKE; ACCURACY TOLERANCE N",4741,"ΤΕΜ",1,"GMC",1,"1FT70641AF711KG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7064-5AF70-1FA5","SIMOTICS S Synchronous motor 1FT7, M0=9Nm (100K) NN=3000rpm, PN=2.39kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE Absolute encoder 22-bit Multiturn with DRIVE-CLiQ interface (encoder AM22DQ) Rotatable connector SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 67",7220,"ΤΕΜ",1,"GMC",1,"1FT70645AF701FA5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7064-5AF71-1CA5","SIMOTICS S Synchronous motor 1FT7, M0=9Nm (100K) NN=3000rpm, PN=2.39kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 67",7108,"ΤΕΜ",1,"GMC",1,"1FT70645AF711CA5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7064-5AK70-1CB1","SIMOTICS S Synchronous motor 1FT7, M0=9Nm (100K) NN=6000rpm, PN=2.59kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",7885,"ΤΕΜ",1,"GMC",1,"1FT70645AK701CB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7064-5AK70-1FH4","SIMOTICS S Synchronous motor 1FT7, M0=9Nm (100K) NN=6000rpm, PN=2.59kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE Absolute encoder 22-bit Multiturn with DRIVE-CLiQ interface (encoder AM22DQ) Rotatable connector PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",8213,"ΤΕΜ",1,"GMC",1,"1FT70645AK701FH4","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7064-5WF71-1BG5","SIMOTICS S Synchronous motor 1FT7, M0=16Nm (100K) NN=3000rpm, PN=5.00kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 67",6936,"ΤΕΜ",1,"GMC",1,"1FT70645WF711BG5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7064-5WK71-1BK5","SIMOTICS S Synchronous motor 1FT7, M0=16Nm (100K) NN=6000rpm, PN=8.90kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 67",7158,"ΤΕΜ",1,"GMC",1,"1FT70645WK711BK5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7066-5AF70-1CB3","SIMOTICS S Synchronous motor 1FT7, M0=12Nm (100K) NN=3000rpm, PN=2.92kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",8397,"ΤΕΜ",1,"GMC",1,"1FT70665AF701CB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7066-5AF70-1DH2","SIMOTICS S Synchronous motor 1FT7, M0=12Nm (100K) NN=3000rpm, PN=2.92kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",7473,"ΤΕΜ",1,"GMC",1,"1FT70665AF701DH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7066-5AF71-1CA1","SIMOTICS S Synchronous motor 1FT7, M0=12Nm (100K) NN=3000rpm, PN=2.92kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",7211,"ΤΕΜ",1,"GMC",1,"1FT70665AF711CA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7066-5AH70-1CH4","SIMOTICS S Synchronous motor 1FT7, M0=12Nm (100K) NN=4500rpm, PN=2.55kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",8532,"ΤΕΜ",1,"GMC",1,"1FT70665AH701CH4","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7066-5AH71-1DD5","SIMOTICS S Synchronous motor 1FT7, M0=12Nm (100K) NN=4500rpm, PN=2.55kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 67",6808,"ΤΕΜ",1,"GMC",1,"1FT70665AH711DD5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7066-5WH74-1NH1","SIMOTICS S Synchronous motor 1FT7, M0=20Nm (100K) NN=4500rpm, PN=9.10kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible), with Pt1000 temperature sensor POWER CONNECTOR ROTATABLE INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",7669,"ΤΕΜ",1,"GMC",1,"1FT70665WH741NH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7067-7WF70-1BG0","SIMOTICS S Synchronous motor 1FT7, M0=25Nm (100K) NN=3000rpm, PN=7.40kW water-cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",7402,"ΤΕΜ",1,"GMC",1,"1FT70677WF701BG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7068-5AF70-1FA1","SIMOTICS S Synchronous motor 1FT7, M0=15Nm (100K) NN=3000rpm, PN=3.42kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE Absolute encoder 22-bit Multiturn with DRIVE-CLiQ interface (encoder AM22DQ) Rotatable connector SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",7753,"ΤΕΜ",1,"GMC",1,"1FT70685AF701FA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7068-5AF71-1CA1","SIMOTICS S Synchronous motor 1FT7, M0=15Nm (100K) NN=3000rpm, PN=3.42kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",7642,"ΤΕΜ",1,"GMC",1,"1FT70685AF711CA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7068-5WF75-1NH1","SIMOTICS S Synchronous motor 1FT7, M0=30Nm (100K) NN=3000rpm, PN=9.30kW water-cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact), with Pt1000  temperature sensor POWER CONNECTOR ROTATABLE INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",8100,"ΤΕΜ",1,"GMC",1,"1FT70685WF751NH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7082-5AC70-1DA1","SIMOTICS S Synchronous motor 1FT7, M0=13Nm (100K) NN=2000rpm, PN=2.39kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",5827,"ΤΕΜ",1,"GMC",1,"1FT70825AC701DA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7082-5AC71-1CA3","SIMOTICS S Synchronous motor 1FT7, M0=13Nm (100K) NN=2000rpm, PN=2.39kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",6862,"ΤΕΜ",1,"GMC",1,"1FT70825AC711CA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7082-5AC71-1FG1","SIMOTICS S Synchronous motor 1FT7, M0=13Nm (100K) NN=2000rpm, PN=2.39kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",6892,"ΤΕΜ",1,"GMC",1,"1FT70825AC711FG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7082-5AF70-1DA1","SIMOTICS S Synchronous motor 1FT7, M0=13Nm (100K) NN=3000rpm, PN=3.24kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",5827,"ΤΕΜ",1,"GMC",1,"1FT70825AF701DA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7082-5AF71-1FH5","SIMOTICS S Synchronous motor 1FT7, M0=13Nm (100K) NN=3000rpm, PN=3.24kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 67",8469,"ΤΕΜ",1,"GMC",1,"1FT70825AF711FH5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7082-5AH70-1BK4","SIMOTICS S Synchronous motor 1FT7, M0=13Nm (100K) NN=4500rpm, PN=3.77kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",6154,"ΤΕΜ",1,"GMC",1,"1FT70825AH701BK4","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7082-5AH71-1FA0","SIMOTICS S Synchronous motor 1FT7, M0=13Nm (100K) NN=4500rpm, PN=3.77kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",6758,"ΤΕΜ",1,"GMC",1,"1FT70825AH711FA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7084-1AH70-1BG1","SIMOTICS S Synchronous motor 1FT7, M0=20Nm (100K) NN=4500rpm, PN=4.82kW naturally cooled; Power connector rotatable; Vibration severity A Degree of protection IP65 Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACCURACY TOLERANCE N",5080,"ΤΕΜ",1,"GMC",1,"1FT70841AH701BG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7084-5AC70-1DK0","SIMOTICS S Synchronous motor 1FT7, M0=20Nm (100K) NN=2000rpm, PN=3.54kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",6961,"ΤΕΜ",1,"GMC",1,"1FT70845AC701DK0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7084-5AC71-1BA0","SIMOTICS S Synchronous motor 1FT7, M0=20Nm (100K) NN=2000rpm, PN=3.54kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",6628,"ΤΕΜ",1,"GMC",1,"1FT70845AC711BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7084-5AF70-1CA1","SIMOTICS S Synchronous motor 1FT7, M0=20Nm (100K) NN=3000rpm, PN=4.55kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",7826,"ΤΕΜ",1,"GMC",1,"1FT70845AF701CA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7084-5AF70-1DG0","SIMOTICS S Synchronous motor 1FT7, M0=20Nm (100K) NN=3000rpm, PN=4.55kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",6740,"ΤΕΜ",1,"GMC",1,"1FT70845AF701DG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7084-5AF71-1CD1","SIMOTICS S Synchronous motor 1FT7, M0=20Nm (100K) NN=3000rpm, PN=4.55kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",8048,"ΤΕΜ",1,"GMC",1,"1FT70845AF711CD1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7084-5AF71-1FH3","SIMOTICS S Synchronous motor 1FT7, M0=20Nm (100K) NN=3000rpm, PN=4.55kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",9269,"ΤΕΜ",1,"GMC",1,"1FT70845AF711FH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7084-5AH71-1DG3","SIMOTICS S Synchronous motor 1FT7, M0=20Nm (100K) NN=4500rpm, PN=4.82kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",6955,"ΤΕΜ",1,"GMC",1,"1FT70845AH711DG3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7084-5SF70-1BG1","SIMOTICS S Synchronous motor 1FT7, M0=27Nm (100K) NN=3000rpm, PN=7.20kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",7654,"ΤΕΜ",1,"GMC",1,"1FT70845SF701BG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7084-5SH70-1BG0","SIMOTICS S Synchronous motor 1FT7, M0=27Nm (100K) NN=4500rpm, PN=9.90kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",7520,"ΤΕΜ",1,"GMC",1,"1FT70845SH701BG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7084-5WF71-1FG1","SIMOTICS S Synchronous motor 1FT7, M0=35Nm (100K) NN=3000rpm, PN=11.00kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",8830,"ΤΕΜ",1,"GMC",1,"1FT70845WF711FG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7084-5WH70-1FH3","SIMOTICS S Synchronous motor 1FT7, M0=35Nm (100K) NN=4500rpm, PN=14.60kW water-cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",10161,"ΤΕΜ",1,"GMC",1,"1FT70845WH701FH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7085-7WF70-1DA4","SIMOTICS S Synchronous motor 1FT7, M0=43Nm (100K) NN=3000rpm, PN=11.90kW water-cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONTRAVERSE RIGHT INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",9332,"ΤΕΜ",1,"GMC",1,"1FT70857WF701DA4","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7086-1AH71-1DG1","SIMOTICS S Synchronous motor 1FT7, M0=28Nm (100K) NN=4500rpm, PN=4.71kW naturally cooled; Power connector rotatable; Vibration severity A Degree of protection IP65 Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACCURACY TOLERANCE N",6216,"ΤΕΜ",1,"GMC",1,"1FT70861AH711DG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7086-5AC71-1BB3","SIMOTICS S Synchronous motor 1FT7, M0=28Nm (100K) NN=2000rpm, PN=4.71kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",9446,"ΤΕΜ",1,"GMC",1,"1FT70865AC711BB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7086-5AC71-1DG1","SIMOTICS S Synchronous motor 1FT7, M0=28Nm (100K) NN=2000rpm, PN=4.71kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",8227,"ΤΕΜ",1,"GMC",1,"1FT70865AC711DG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7086-5AF70-1DA4","SIMOTICS S Synchronous motor 1FT7, M0=28Nm (100K) NN=3000rpm, PN=5.65kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",8444,"ΤΕΜ",1,"GMC",1,"1FT70865AF701DA4","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7086-5AF70-1FD2","SIMOTICS S Synchronous motor 1FT7, M0=28Nm (100K) NN=3000rpm, PN=5.65kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",9624,"ΤΕΜ",1,"GMC",1,"1FT70865AF701FD2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7086-5AF71-1CK5","SIMOTICS S Synchronous motor 1FT7, M0=28Nm (100K) NN=3000rpm, PN=5.65kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 67",9730,"ΤΕΜ",1,"GMC",1,"1FT70865AF711CK5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7086-5AH70-1BA0","SIMOTICS S Synchronous motor 1FT7, M0=28Nm (100K) NN=4500rpm, PN=4.71kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",7982,"ΤΕΜ",1,"GMC",1,"1FT70865AH701BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7086-5AH71-1DG2","SIMOTICS S Synchronous motor 1FT7, M0=28Nm (100K) NN=4500rpm, PN=4.71kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",8338,"ΤΕΜ",1,"GMC",1,"1FT70865AH711DG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7086-5SC71-1BG1","SIMOTICS S Synchronous motor 1FT7, M0=36Nm (100K) NN=2000rpm, PN=6.70kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",9008,"ΤΕΜ",1,"GMC",1,"1FT70865SC711BG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7086-5SF71-1BH0","SIMOTICS S Synchronous motor 1FT7, M0=36Nm (100K) NN=3000rpm, PN=9.10kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",10123,"ΤΕΜ",1,"GMC",1,"1FT70865SF711BH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7086-5WC71-1DG0","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=2000rpm, PN=10.50kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",8986,"ΤΕΜ",1,"GMC",1,"1FT70865WC711DG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7086-5WF71-1DG4","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=3000rpm, PN=15.40kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",9336,"ΤΕΜ",1,"GMC",1,"1FT70865WF711DG4","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7087-7SF70-3CA0","SIMOTICS S Synchronous motor 1FT7, M0=48Nm (100K) NN=3000rpm, PN=10.40kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONAXIAL NON-DRIVE END ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",11046,"ΤΕΜ",1,"GMC",1,"1FT70877SF703CA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7087-7SH71-3CH1","SIMOTICS S Synchronous motor 1FT7, M0=48Nm (100K) NN=4500rpm, PN=10.80kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONAXIAL NON-DRIVE END ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",12429,"ΤΕΜ",1,"GMC",1,"1FT70877SH713CH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7102-1AC74-1NG1","SIMOTICS S Synchronous motor 1FT7, M0=30Nm (100K) NN=2000rpm, PN=5.03kW naturally cooled; Power connector rotatable; Vibration severity A Degree of protection IP65 Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible), with Pt1000 temperature sensor INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACCURACY TOLERANCE N",5293,"ΤΕΜ",1,"GMC",1,"1FT71021AC741NG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7102-5AB70-1FG4","SIMOTICS S Synchronous motor 1FT7, M0=30Nm (100K) NN=1500rpm, PN=4.08kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",9078,"ΤΕΜ",1,"GMC",1,"1FT71025AB701FG4","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7102-5AB71-1BB0","SIMOTICS S Synchronous motor 1FT7, M0=30Nm (100K) NN=1500rpm, PN=4.08kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",8960,"ΤΕΜ",1,"GMC",1,"1FT71025AB711BB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7102-5AC70-1DB2","SIMOTICS S Synchronous motor 1FT7, M0=30Nm (100K) NN=2000rpm, PN=5.03kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",9316,"ΤΕΜ",1,"GMC",1,"1FT71025AC701DB2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7102-5AC71-1DH1","SIMOTICS S Synchronous motor 1FT7, M0=30Nm (100K) NN=2000rpm, PN=5.03kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",9206,"ΤΕΜ",1,"GMC",1,"1FT71025AC711DH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7102-5AF70-1DA3","SIMOTICS S Synchronous motor 1FT7, M0=30Nm (100K) NN=3000rpm, PN=6.28kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",7878,"ΤΕΜ",1,"GMC",1,"1FT71025AF701DA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7102-5AF70-1FH1","SIMOTICS S Synchronous motor 1FT7, M0=30Nm (100K) NN=3000rpm, PN=6.28kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",10270,"ΤΕΜ",1,"GMC",1,"1FT71025AF701FH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7102-5WC70-1CH0","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=2000rpm, PN=10.40kW water-cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",10917,"ΤΕΜ",1,"GMC",1,"1FT71025WC701CH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7102-5WF71-1CA1","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=3000rpm, PN=14.30kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",9642,"ΤΕΜ",1,"GMC",1,"1FT71025WF711CA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7105-5AB70-1DA5","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=1500rpm, PN=6.60kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 67",10247,"ΤΕΜ",1,"GMC",1,"1FT71055AB701DA5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7105-5AB71-1DA5","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=1500rpm, PN=6.60kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 67",10247,"ΤΕΜ",1,"GMC",1,"1FT71055AB711DA5","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7105-5AC70-1BG0","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=2000rpm, PN=7.96kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",9674,"ΤΕΜ",1,"GMC",1,"1FT71055AC701BG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7105-5AC70-1FA2","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=2000rpm, PN=7.96kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",11095,"ΤΕΜ",1,"GMC",1,"1FT71055AC701FA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7105-5AC71-1BH1","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=2000rpm, PN=7.96kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",11217,"ΤΕΜ",1,"GMC",1,"1FT71055AC711BH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7105-5AC71-1FH3","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=2000rpm, PN=7.96kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",12475,"ΤΕΜ",1,"GMC",1,"1FT71055AC711FH3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7105-5AF70-1DB3","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=3000rpm, PN=8.80kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",11410,"ΤΕΜ",1,"GMC",1,"1FT71055AF701DB3","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7105-5AF71-1CG1","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=3000rpm, PN=8.80kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",10872,"ΤΕΜ",1,"GMC",1,"1FT71055AF711CG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7105-5AF71-1FD2","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=3000rpm, PN=8.80kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",11317,"ΤΕΜ",1,"GMC",1,"1FT71055AF711FD2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7105-5SC71-1CG4","SIMOTICS S Synchronous motor 1FT7, M0=65Nm (100K) NN=2000rpm, PN=11.70kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",11982,"ΤΕΜ",1,"GMC",1,"1FT71055SC711CG4","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7105-5SF70-1CB0","SIMOTICS S Synchronous motor 1FT7, M0=65Nm (100K) NN=3000rpm, PN=15.10kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONTRAVERSE RIGHT ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",13040,"ΤΕΜ",1,"GMC",1,"1FT71055SF701CB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7105-5SF71-4CA1","SIMOTICS S Synchronous motor 1FT7, M0=65Nm (100K) NN=3000rpm, PN=15.10kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONAXIAL DRIVE END ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",11765,"ΤΕΜ",1,"GMC",1,"1FT71055SF714CA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7105-5SF71-8CB0","SIMOTICS S Synchronous motor 1FT7, M0=65Nm (100K) NN=3000rpm, PN=15.10kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) FOR CONNECT. OF TERMINAL BOXAND SIGNAL CONNECTOR, TERMINALBOX AXIAL DRIVE END ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",13040,"ΤΕΜ",1,"GMC",1,"1FT71055SF718CB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7105-5WC75-1NG1","SIMOTICS S Synchronous motor 1FT7, M0=90Nm (100K) NN=2000rpm, PN=18.80kW water-cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact), with Pt1000  temperature sensor POWER CONNECTOR ROTATABLE INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",10226,"ΤΕΜ",1,"GMC",1,"1FT71055WC751NG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7105-5WF71-1BG0","SIMOTICS S Synchronous motor 1FT7, M0=90Nm (100K) NN=3000rpm, PN=24.80kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONTRAVERSE RIGHT ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",10566,"ΤΕΜ",1,"GMC",1,"1FT71055WF711BG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7108-5AB70-1DA1","SIMOTICS S Synchronous motor 1FT7, M0=70Nm (100K) NN=1500rpm, PN=9.58kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",12719,"ΤΕΜ",1,"GMC",1,"1FT71085AB701DA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7108-5AB71-1BH1","SIMOTICS S Synchronous motor 1FT7, M0=70Nm (100K) NN=1500rpm, PN=9.58kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",14017,"ΤΕΜ",1,"GMC",1,"1FT71085AB711BH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7108-5AB71-1DE0","SIMOTICS S Synchronous motor 1FT7, M0=70Nm (100K) NN=1500rpm, PN=9.58kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",14216,"ΤΕΜ",1,"GMC",1,"1FT71085AB711DE0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7108-5AC70-1CB0","SIMOTICS S Synchronous motor 1FT7, M0=70Nm (100K) NN=2000rpm, PN=10.50kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",14948,"ΤΕΜ",1,"GMC",1,"1FT71085AC701CB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7108-5AC70-1FG2","SIMOTICS S Synchronous motor 1FT7, M0=70Nm (100K) NN=2000rpm, PN=10.50kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",13895,"ΤΕΜ",1,"GMC",1,"1FT71085AC701FG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7108-5AC71-1DK4","SIMOTICS S Synchronous motor 1FT7, M0=70Nm (100K) NN=2000rpm, PN=10.50kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",13158,"ΤΕΜ",1,"GMC",1,"1FT71085AC711DK4","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7108-5AC71-1FL1","SIMOTICS S Synchronous motor 1FT7, M0=70Nm (100K) NN=2000rpm, PN=10.50kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE R VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",15414,"ΤΕΜ",1,"GMC",1,"1FT71085AC711FL1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7108-5AF71-1CH4","SIMOTICS S Synchronous motor 1FT7, M0=70Nm (100K) NN=3000rpm, PN=6.28kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",15298,"ΤΕΜ",1,"GMC",1,"1FT71085AF711CH4","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7108-5SC70-1BB1","SIMOTICS S Synchronous motor 1FT7, M0=91Nm (100K) NN=2000rpm, PN=15.30kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONTRAVERSE RIGHT ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",14909,"ΤΕΜ",1,"GMC",1,"1FT71085SC701BB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7108-5SF70-1CA1","SIMOTICS S Synchronous motor 1FT7, M0=91Nm (100K) NN=3000rpm, PN=18.80kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONTRAVERSE RIGHT ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",14565,"ΤΕΜ",1,"GMC",1,"1FT71085SF701CA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7108-5SF70-3CH0","SIMOTICS S Synchronous motor 1FT7, M0=91Nm (100K) NN=3000rpm, PN=18.80kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONAXIAL NON-DRIVE END ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",15840,"ΤΕΜ",1,"GMC",1,"1FT71085SF703CH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7108-5SF71-8CA1","SIMOTICS S Synchronous motor 1FT7, M0=91Nm (100K) NN=3000rpm, PN=18.80kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) FOR CONNECT. OF TERMINAL BOXAND SIGNAL CONNECTOR, TERMINALBOX AXIAL DRIVE END ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",14565,"ΤΕΜ",1,"GMC",1,"1FT71085SF718CA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7108-5WB71-1DG0","SIMOTICS S Synchronous motor 1FT7, M0=125Nm (100K) NN=1500rpm, PN=19.60kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",13478,"ΤΕΜ",1,"GMC",1,"1FT71085WB711DG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7108-5WF70-3BA1","SIMOTICS S Synchronous motor 1FT7, M0=125Nm (100K) NN=3000rpm, PN=34.20kW water-cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONAXIAL NON-DRIVE END ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",13500,"ΤΕΜ",1,"GMC",1,"1FT71085WF703BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7108-5WF71-1DG0","SIMOTICS S Synchronous motor 1FT7, M0=125Nm (100K) NN=3000rpm, PN=34.20kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONTRAVERSE RIGHT INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",13478,"ΤΕΜ",1,"GMC",1,"1FT71085WF711DG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7108-5WF71-4DG4","SIMOTICS S Synchronous motor 1FT7, M0=125Nm (100K) NN=3000rpm, PN=34.20kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONAXIAL DRIVE END INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",13828,"ΤΕΜ",1,"GMC",1,"1FT71085WF714DG4","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7132-5AC74-1MG0","SIMOTICS S Synchronous motor 1FT7, M0=90Nm (100K) NN=2000rpm, PN=11.50kW naturally cooled; Power connector rotatable Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible), with Pt1000 temperature sensor ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER A-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",14487,"ΤΕΜ",1,"GMC",1,"1FT71325AC741MG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7132-5SC71-7BH1","SIMOTICS S Synchronous motor 1FT7, M0=140Nm (100K) NN=2000rpm, PN=26.5 kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) FOR CONNECT. OF TERMINAL BOXAND SIGNAL CONNECTOR, TERMINALBOX AXIAL NON-DRIVE END NOT IN COMBINATION WITH DEGREE OF PROTECTION IP67 ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",17489,"ΤΕΜ",1,"GMC",1,"1FT71325SC717BH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7134-5AB74-1NA0","SIMOTICS S Synchronous motor 1FT7, M0=118Nm (100K) NN=1500rpm, PN=12.9kW naturally cooled; Power connector rotatable Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible), with Pt1000 temperature sensor INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",15229,"ΤΕΜ",1,"GMC",1,"1FT71345AB741NA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7134-5AC71-1CE4","SIMOTICS S Synchronous motor 1FT7, M0=118Nm (100K) NN=2000rpm, PN=13.8kW naturally cooled; Power connector rotatable Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",19885,"ΤΕΜ",1,"GMC",1,"1FT71345AC711CE4","Ρυθμιστές στροφών και συστήματα Motion control"]
["1FT7136-5SC71-5BB0","SIMOTICS S Synchronous motor 1FT7, M0=235 Nm (100K) NN=2000rpm, PN=39.8 kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) For terminal box and signal Terminal box transverse right; Not in connection with degree of protection IP67 ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",20430,"ΤΕΜ",1,"GMC",1,"1FT71365SC715BB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8083-1DF00-0DA1","SIMOTICS M compact asynchronous motor 1500 rpm 2.8 kW 17.8 Nm 7.5 A 346 V 1750 rpm 3.3 kW 18 Nm 7.5 A 398 V 2000 rpm 3.7 kW 17.7 Nm 7.6 A 447 V 2200 rpm 4.1 kW 17.8 Nm 7.6 A 480 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE SR/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7242,"ΤΕΜ",1,"GMC",1,"1PH80831DF000DA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8083-1DF00-1CA1","SIMOTICS M compact asynchronous motor 1500 rpm 2.8 kW 17.8 Nm 7.5 A 346 V 1750 rpm 3.3 kW 18 Nm 7.5 A 398 V 2000 rpm 3.7 kW 17.7 Nm 7.6 A 447 V 2200 rpm 4.1 kW 17.8 Nm 7.6 A 480 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7136,"ΤΕΜ",1,"GMC",1,"1PH80831DF001CA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8083-1DG02-0BE1","SIMOTICS M compact asynchronous motor 2000 rpm 3.7 kW 17.7 Nm 11.6 A 293 V 2300 rpm 4.1 kW 17 Nm 11.3 A 332 V 2650 rpm 4.6 kW 16.6 Nm 11.2 A 376 V 2800 rpm 4.8 kW 16.4 Nm 11.3 A 400 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7071,"ΤΕΜ",1,"GMC",1,"1PH80831DG020BE1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8083-1DG12-2LF1","SIMOTICS M compact asynchronous motor 2000 rpm 3.7 kW 17.7 Nm 11.6 A 293 V 2300 rpm 4.1 kW 17 Nm 11.3 A 332 V 2650 rpm 4.6 kW 16.6 Nm 11.2 A 376 V 2800 rpm 4.8 kW 16.4 Nm 11.3 A 400 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",7894,"ΤΕΜ",1,"GMC",1,"1PH80831DG122LF1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8083-1FF12-0BA1","SIMOTICS M compact asynchronous motor 1500 rpm 2.8 kW 17.8 Nm 7.5 A 346 V 1750 rpm 3.3 kW 18 Nm 7.5 A 398 V 2000 rpm 3.7 kW 17.7 Nm 7.6 A 447 V 2200 rpm 4.1 kW 17.8 Nm 7.6 A 480 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8439,"ΤΕΜ",1,"GMC",1,"1PH80831FF120BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8083-1SF00-1LA1","SIMOTICS M compact asynchronous motor 1500 rpm 2.8 kW 17.8 Nm 7.5 A 346 V 1750 rpm 3.3 kW 18 Nm 7.5 A 398 V 2000 rpm 3.7 kW 17.7 Nm 7.6 A 447 V 2200 rpm 4.1 kW 17.8 Nm 7.6 A 480 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 19-bit Without commutation position (encoder IN19DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",9685,"ΤΕΜ",1,"GMC",1,"1PH80831SF001LA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8087-1DF00-2GB1","SIMOTICS M compact asynchronous motor 1500 rpm 3.7 kW 23.6 Nm 10 A 336 V 1750 rpm 4.3 kW 23.5 Nm 10 A 396 V 2000 rpm 4.9 kW 23.4 Nm 10 A 435 V 2200 rpm 5.3 kW 23 Nm 10 A 480 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",6666,"ΤΕΜ",1,"GMC",1,"1PH80871DF002GB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8087-1DF02-2GA1","SIMOTICS M compact asynchronous motor 1500 rpm 3.7 kW 23.6 Nm 10 A 336 V 1750 rpm 4.3 kW 23.5 Nm 10 A 396 V 2000 rpm 4.9 kW 23.4 Nm 10 A 435 V 2200 rpm 5.3 kW 23 Nm 10 A 480 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6894,"ΤΕΜ",1,"GMC",1,"1PH80871DF022GA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8087-1DM02-0BB1","SIMOTICS M compact asynchronous motor 3000 rpm 4.8 kW 15.3 Nm 17.3 A 284 V 3300 rpm 5.2 kW 15 Nm 17.1 A 303 V 3600 rpm 5.7 kW 15.1 Nm 17.1 A 329 V 3900 rpm 6 kW 14.7 Nm 17.1 A 357 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",7322,"ΤΕΜ",1,"GMC",1,"1PH80871DM020BB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8087-1HG10-1BA2","SIMOTICS M compact asynchronous motor 2000 rpm 4.9 kW 23.4 Nm 14.1 A 320 V 2300 rpm 5.4 kW 22.4 Nm 13.7 A 353 V 2650 rpm 6 kW 21.6 Nm 13.6 A 390 V 2800 rpm 6.3 kW 21.5 Nm 13.5 A 425 V forced ventilation; direction of air flow NDE --> DE; IP55 degree of protection Incremental encoder HTL 1024 S/R (encoder HTL1024S/R) With temperature sensor Pt1000 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5563,"ΤΕΜ",1,"GMC",1,"1PH80871HG101BA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8087-1UF02-1LA1","SIMOTICS M compact asynchronous motor 1500 rpm 3.7 kW 23.6 Nm 10 A 336 V 1750 rpm 4.3 kW 23.5 Nm 10 A 396 V 2000 rpm 4.9 kW 23.4 Nm 10 A 435 V 2200 rpm 5.3 kW 23 Nm 10 A 480 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 20-bit Without commutation position (encoder IN20DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8454,"ΤΕΜ",1,"GMC",1,"1PH80871UF021LA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8101-1AF02-2BD2","SIMOTICS M compact asynchronous motor 1500 rpm 3.7 kW 24 Nm 12.5 A 265 V 1750 rpm 4.3 kW 23 Nm 12.5 A 304 V 2000 rpm 4.7 kW 22 Nm 12.5 A 343 V 2200 rpm 5.1 kW 22 Nm 12.5 A 363 V forced ventilation; direction of air flow DE --> NDE; IP55 degree of protection Without encoder With temperature sensor Pt1000 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE D-END SIGNAL CONNECTION LEFT",5583,"ΤΕΜ",1,"GMC",1,"1PH81011AF022BD2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8101-1DF10-2BA1","SIMOTICS M compact asynchronous motor 1500 rpm 3.7 kW 24 Nm 12.5 A 265 V 1750 rpm 4.3 kW 23 Nm 12.5 A 304 V 2000 rpm 4.7 kW 22 Nm 12.5 A 343 V 2200 rpm 5.1 kW 22 Nm 12.5 A 363 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7201,"ΤΕΜ",1,"GMC",1,"1PH81011DF102BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8101-1UF02-0LA1","SIMOTICS M compact asynchronous motor 1500 rpm 3.7 kW 24 Nm 12.5 A 265 V 1750 rpm 4.3 kW 23 Nm 12.5 A 304 V 2000 rpm 4.7 kW 22 Nm 12.5 A 343 V 2200 rpm 5.1 kW 22 Nm 12.5 A 363 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 20-bit Without commutation position (encoder IN20DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8574,"ΤΕΜ",1,"GMC",1,"1PH81011UF020LA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8103-1DD10-1BA1","SIMOTICS M compact asynchronous motor 1000 rpm 3.7 kW 35 Nm 10 A 333 V 1150 rpm 4.3 kW 36 Nm 10 A 380 V 1350 rpm 4.7 kW 33 Nm 9.7 A 423 V 1500 rpm 5.2 kW 33 Nm 9.7 A 470 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7362,"ΤΕΜ",1,"GMC",1,"1PH81031DD101BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8103-1DF02-0GA1","SIMOTICS M compact asynchronous motor 1500 rpm 5.5 kW 35 Nm 13.5 A 368 V 1750 rpm 6.3 kW 34 Nm 13.1 A 412 V 2000 rpm 7 kW 33 Nm 12.7 A 460 V 2200 rpm 7.7 kW 33 Nm 12.7 A 480 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7227,"ΤΕΜ",1,"GMC",1,"1PH81031DF020GA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8103-1DF22-1BA1","SIMOTICS M compact asynchronous motor 1500 rpm 7.1 kW 45 Nm 19.7 A 317 V 1750 rpm 8.2 kW 45 Nm 19.7 A 364 V 2000 rpm 9.4 kW 45 Nm 19.7 A 411 V 2200 rpm 10.3 kW 45 Nm 19.7 A 430 V water cooling degree of protection IP65 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8277,"ΤΕΜ",1,"GMC",1,"1PH81031DF221BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8103-1DG02-1DA1","SIMOTICS M compact asynchronous motor 2000 rpm 7 kW 33 Nm 17.5 A 345 V 2300 rpm 7.5 kW 31 Nm 17 A 382 V 2650 rpm 8 kW 29 Nm 16 A 434 V 2800 rpm 8.5 kW 29 Nm 16 A 455 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: SR/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8053,"ΤΕΜ",1,"GMC",1,"1PH81031DG021DA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8103-1DG13-0BG1","SIMOTICS M compact asynchronous motor 2000 rpm 7 kW 33 Nm 17.5 A 345 V 2300 rpm 7.5 kW 31 Nm 17 A 382 V 2650 rpm 8 kW 29 Nm 16 A 434 V 2800 rpm 8.5 kW 29 Nm 16 A 455 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",8013,"ΤΕΜ",1,"GMC",1,"1PH81031DG130BG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8103-1DM10-1BH1","SIMOTICS M compact asynchronous motor 3000 rpm 8.4 kW 27 Nm 25.7 A 297 V 3300 rpm 9.3 kW 27 Nm 25.7 A 326 V 3600 rpm 10 kW 27 Nm 25.4 A 355 V 3900 rpm 10.8 kW 26 Nm 25 A 383 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",7362,"ΤΕΜ",1,"GMC",1,"1PH81031DM101BH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8103-1FF02-0CE1","SIMOTICS M compact asynchronous motor 1500 rpm 5.5 kW 35 Nm 13.5 A 368 V 1750 rpm 6.3 kW 34 Nm 13.1 A 412 V 2000 rpm 7 kW 33 Nm 12.7 A 460 V 2200 rpm 7.7 kW 33 Nm 12.7 A 480 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",9316,"ΤΕΜ",1,"GMC",1,"1PH81031FF020CE1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8103-1MF02-1GH2","SIMOTICS M compact asynchronous motor 1500 rpm 5.5 kW 35 Nm 13.5 A 368 V 1750 rpm 6.3 kW 34 Nm 13.1 A 412 V 2000 rpm 7 kW 33 Nm 12.7 A 460 V 2200 rpm 7.7 kW 33 Nm 12.7 A 480 V forced ventilation; direction of air flow DE --> NDE; IP55 degree of protection Incremental encoder sin/cos 1 Vpp 2048 S/R with C and D track (encoder IC2048S/R) With temperature sensor Pt1000 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",6185,"ΤΕΜ",1,"GMC",1,"1PH81031MF021GH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8103-1SG02-0LA1","SIMOTICS M compact asynchronous motor 2000 rpm 7 kW 33 Nm 17.5 A 345 V 2300 rpm 7.5 kW 31 Nm 17 A 382 V 2650 rpm 8 kW 29 Nm 16 A 434 V 2800 rpm 8.5 kW 29 Nm 16 A 455 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 19-bit Without commutation position (encoder IN19DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",10444,"ΤΕΜ",1,"GMC",1,"1PH81031SG020LA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8105-1DF02-0LA1","SIMOTICS M compact asynchronous motor 1500 rpm 7 kW 45 Nm 17.5 A 348 V 1750 rpm 8 kW 44 Nm 17.5 A 400 V 2000 rpm 9 kW 43 Nm 17 A 453 V 2200 rpm 9.9 kW 43 Nm 17 A 485 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8711,"ΤΕΜ",1,"GMC",1,"1PH81051DF020LA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8105-1DF02-2HA1","SIMOTICS M compact asynchronous motor 1500 rpm 7 kW 45 Nm 17.5 A 348 V 1750 rpm 8 kW 44 Nm 17.5 A 400 V 2000 rpm 9 kW 43 Nm 17 A 453 V 2200 rpm 9.9 kW 43 Nm 17 A 485 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7806,"ΤΕΜ",1,"GMC",1,"1PH81051DF022HA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8105-1DF20-1BA1","SIMOTICS M compact asynchronous motor 1500 rpm 11 kW 70 Nm 28.5 A 340 V 1750 rpm 12.5 kW 68 Nm 28.5 A 380 V 2000 rpm 14 kW 67 Nm 27.5 A 426 V 2200 rpm 15.4 kW 67 Nm 27.5 A 458 V water cooling degree of protection IP65 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8440,"ΤΕΜ",1,"GMC",1,"1PH81051DF201BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8105-1FF03-1BA1","SIMOTICS M compact asynchronous motor 1500 rpm 7 kW 45 Nm 17.5 A 348 V 1750 rpm 8 kW 44 Nm 17.5 A 400 V 2000 rpm 9 kW 43 Nm 17 A 453 V 2200 rpm 9.9 kW 43 Nm 17 A 485 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",9667,"ΤΕΜ",1,"GMC",1,"1PH81051FF031BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8105-1MF20-2GA2","SIMOTICS M compact asynchronous motor 1500 rpm 11 kW 70 Nm 28.5 A 340 V 1750 rpm 12.5 kW 68 Nm 28.5 A 380 V 2000 rpm 14 kW 67 Nm 27.5 A 426 V 2200 rpm 15.4 kW 67 Nm 27.5 A 458 V water cooling degree of protection IP65 Incremental encoder sin/cos 1 Vpp 2048 S/R with C and D track (encoder IC2048S/R) With temperature sensor Pt1000 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6970,"ΤΕΜ",1,"GMC",1,"1PH81051MF202GA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8107-1DD00-2BA1","SIMOTICS M compact asynchronous motor 1000 rpm 6.3 kW 60 Nm 17.5 A 307 V 1150 rpm 7.2 kW 60 Nm 17.5 A 348 V 1350 rpm 8 kW 57 Nm 17 A 400 V 1500 rpm 8.8 kW 56 Nm 17 A 440 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7861,"ΤΕΜ",1,"GMC",1,"1PH81071DD002BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8107-1DD02-1LB1","SIMOTICS M compact asynchronous motor 1000 rpm 6.3 kW 60 Nm 17.5 A 307 V 1150 rpm 7.2 kW 60 Nm 17.5 A 348 V 1350 rpm 8 kW 57 Nm 17 A 400 V 1500 rpm 8.8 kW 56 Nm 17 A 440 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",8924,"ΤΕΜ",1,"GMC",1,"1PH81071DD021LB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8107-1DF02-0CE1","SIMOTICS M compact asynchronous motor 1500 rpm 9 kW 57 Nm 23.5 A 330 V 1750 rpm 10 kW 55 Nm 22 A 380 V 2000 rpm 11 kW 53 Nm 21.5 A 428 V 2200 rpm 12.1 kW 53 Nm 21.5 A 470 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8447,"ΤΕΜ",1,"GMC",1,"1PH81071DF020CE1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8107-1DF03-2BC1","SIMOTICS M compact asynchronous motor 1500 rpm 9 kW 57 Nm 23.5 A 330 V 1750 rpm 10 kW 55 Nm 22 A 380 V 2000 rpm 11 kW 53 Nm 21.5 A 428 V 2200 rpm 12.1 kW 53 Nm 21.5 A 470 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",8512,"ΤΕΜ",1,"GMC",1,"1PH81071DF032BC1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8107-1DF13-1BC1","SIMOTICS M compact asynchronous motor 1500 rpm 9 kW 57 Nm 23.5 A 330 V 1750 rpm 10 kW 55 Nm 22 A 380 V 2000 rpm 11 kW 53 Nm 21.5 A 428 V 2200 rpm 12.1 kW 53 Nm 21.5 A 470 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",8512,"ΤΕΜ",1,"GMC",1,"1PH81071DF131BC1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8107-1DG00-0GA1","SIMOTICS M compact asynchronous motor 2000 rpm 10.5 kW 50 Nm 26 A 355 V 2300 rpm 12 kW 50 Nm 26 A 406 V 2650 rpm 13 kW 47 Nm 24 A 460 V 2800 rpm 13.7 kW 47 Nm 24 A 480 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7433,"ΤΕΜ",1,"GMC",1,"1PH81071DG000GA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8107-1DG12-2DA1","SIMOTICS M compact asynchronous motor 2000 rpm 10.5 kW 50 Nm 26 A 355 V 2300 rpm 12 kW 50 Nm 26 A 406 V 2650 rpm 13 kW 47 Nm 24 A 460 V 2800 rpm 13.7 kW 47 Nm 24 A 480 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: SR/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8552,"ΤΕΜ",1,"GMC",1,"1PH81071DG122DA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8107-1DM02-2BA1","SIMOTICS M compact asynchronous motor 3000 rpm 12 kW 38 Nm 38 A 294 V 3300 rpm 13 kW 38 Nm 38 A 314 V 3600 rpm 14 kW 37 Nm 37.5 A 350 V 3900 rpm 14 kW 34 Nm 35 A 380 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8154,"ΤΕΜ",1,"GMC",1,"1PH81071DM022BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8107-1FD12-1BB1","SIMOTICS M compact asynchronous motor 1000 rpm 6.3 kW 60 Nm 17.5 A 307 V 1150 rpm 7.2 kW 60 Nm 17.5 A 348 V 1350 rpm 8 kW 57 Nm 17 A 400 V 1500 rpm 8.8 kW 56 Nm 17 A 440 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",9522,"ΤΕΜ",1,"GMC",1,"1PH81071FD121BB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8107-1FF00-2BA1","SIMOTICS M compact asynchronous motor 1500 rpm 9 kW 57 Nm 23.5 A 330 V 1750 rpm 10 kW 55 Nm 22 A 380 V 2000 rpm 11 kW 53 Nm 21.5 A 428 V 2200 rpm 12.1 kW 53 Nm 21.5 A 470 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",9228,"ΤΕΜ",1,"GMC",1,"1PH81071FF002BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8107-1FG12-0BC1","SIMOTICS M compact asynchronous motor 2000 rpm 10.5 kW 50 Nm 26 A 355 V 2300 rpm 12 kW 50 Nm 26 A 406 V 2650 rpm 13 kW 47 Nm 24 A 460 V 2800 rpm 13.7 kW 47 Nm 24 A 480 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",9522,"ΤΕΜ",1,"GMC",1,"1PH81071FG120BC1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8107-1SF22-3MA1","SIMOTICS M compact asynchronous motor 1500 rpm 14 kW 89 Nm 43.7 A 277 V 1750 rpm 15.5 kW 85 Nm 42 A 314 V 2000 rpm 18 kW 86 Nm 42.6 A 363 V 2200 rpm 19.8 kW 86 Nm 42.6 A 381 V water cooling degree of protection IP65 Incremental encoder 19-bit Without commutation position (encoder IN19DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN HOLLOW-SHAFT BEARING: HIGH PERFORMANCE VIBRATION SEVERITY GRADE SPECIAL/B SHAFT AND FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",15125,"ΤΕΜ",1,"GMC",1,"1PH81071SF223MA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8107-1UD12-2LA1","SIMOTICS M compact asynchronous motor 1000 rpm 6.3 kW 60 Nm 17.5 A 307 V 1150 rpm 7.2 kW 60 Nm 17.5 A 348 V 1350 rpm 8 kW 57 Nm 17 A 400 V 1500 rpm 8.8 kW 56 Nm 17 A 440 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Incremental encoder 20-bit Without commutation position (encoder IN20DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",9234,"ΤΕΜ",1,"GMC",1,"1PH81071UD122LA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8131-1DF02-0DB1","SIMOTICS M compact asynchronous motor 1500 rpm 11 kW 70 Nm 24 A 360 V 1750 rpm 13 kW 71 Nm 24 A 416 V 2000 rpm 15 kW 72 Nm 24 A 460 V 2200 rpm 16.5 kW 72 Nm 24 A 500 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: SR/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",8856,"ΤΕΜ",1,"GMC",1,"1PH81311DF020DB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8131-1DF02-1LA1","SIMOTICS M compact asynchronous motor 1500 rpm 11 kW 70 Nm 24 A 360 V 1750 rpm 13 kW 71 Nm 24 A 416 V 2000 rpm 15 kW 72 Nm 24 A 460 V 2200 rpm 16.5 kW 72 Nm 24 A 500 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE: SPECIAL/B, SHAFT AND FLANGE ACCURACY: SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",9279,"ΤΕΜ",1,"GMC",1,"1PH81311DF021LA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8131-1DS03-2BC1","SIMOTICS M Compact induction motor 2000rpm, 14.6kW 70 Nm, 39A, 302V 5000rpm, 14.6kW 28Nm, 40A, 360V 1500rpm, 11 kW 70 Nm, 39A, 227V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",8914,"ΤΕΜ",1,"GMC",1,"1PH81311DS032BC1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8131-1SF00-2LA1","SIMOTICS M compact asynchronous motor 1500 rpm 11 kW 70 Nm 24 A 360 V 1750 rpm 13 kW 71 Nm 24 A 416 V 2000 rpm 15 kW 72 Nm 24 A 460 V 2200 rpm 16.5 kW 72 Nm 24 A 500 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 19-bit Without commutation position (encoder IN19DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE: SPECIAL/B, SHAFT AND FLANGE ACCURACY: SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",10940,"ΤΕΜ",1,"GMC",1,"1PH81311SF002LA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8131-2DF00-1BB1","SIMOTICS M Compact synchronous motor 1500rpm, 15.7kW 100 Nm, 29A, 388V 1750rpm, 18kW 98Nm, 29A, 415 V 2000rpm, 19.9kW 95Nm, 29A, 449V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",16128,"ΤΕΜ",1,"GMC",1,"1PH81312DF001BB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8131-2DL02-2BA1","SIMOTICS M Compact synchronous motor 2500rpm, 25kW 96Nm, 44A, 371V 2800rpm, 27.7kW 95Nm, 44A, 415 V 3000rpm, 29.5kW 94Nm, 43A, 449V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",16486,"ΤΕΜ",1,"GMC",1,"1PH81312DL022BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8131-2FF12-2BE1","SIMOTICS M Compact synchronous motor 1500rpm, 15.7kW 100 Nm, 29A, 388V 1750rpm, 18kW 98Nm, 29A, 415 V 2000rpm, 19.9kW 95Nm, 29A, 449V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",17854,"ΤΕΜ",1,"GMC",1,"1PH81312FF122BE1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8133-1DD02-0BC1","SIMOTICS M compact asynchronous motor 1000 rpm 12 kW 115 Nm 30 A 319 V 1150 rpm 13.5 kW 112 Nm 29 A 361 V 1350 rpm 15 kW 106 Nm 28 A 417 V 1500 rpm 16.6 kW 106 Nm 28 A 459 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",8645,"ΤΕΜ",1,"GMC",1,"1PH81331DD020BC1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8133-1DD02-2BA1","SIMOTICS M compact asynchronous motor 1000 rpm 12 kW 115 Nm 30 A 319 V 1150 rpm 13.5 kW 112 Nm 29 A 361 V 1350 rpm 15 kW 106 Nm 28 A 417 V 1500 rpm 16.6 kW 106 Nm 28 A 459 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8645,"ΤΕΜ",1,"GMC",1,"1PH81331DD022BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8133-1DD12-2GA1","SIMOTICS M compact asynchronous motor 1000 rpm 12 kW 115 Nm 30 A 319 V 1150 rpm 13.5 kW 112 Nm 29 A 361 V 1350 rpm 15 kW 106 Nm 28 A 417 V 1500 rpm 16.6 kW 106 Nm 28 A 459 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8217,"ΤΕΜ",1,"GMC",1,"1PH81331DD122GA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8133-1DF02-0DH1","SIMOTICS M compact asynchronous motor 1500 rpm 15 kW 96 Nm 34 A 342 V 1750 rpm 17.5 kW 96 Nm 34 A 392 V 2000 rpm 20 kW 96 Nm 34 A 445 V 2200 rpm 22 kW 96 Nm 34 A 480 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: SR/A, SHAFT AND FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE D-END SIGNAL CONNECTION LEFT",9044,"ΤΕΜ",1,"GMC",1,"1PH81331DF020DH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8133-1DF10-2GC1","SIMOTICS M compact asynchronous motor 1500 rpm 15 kW 96 Nm 34 A 342 V 1750 rpm 17.5 kW 96 Nm 34 A 392 V 2000 rpm 20 kW 96 Nm 34 A 445 V 2200 rpm 22 kW 96 Nm 34 A 480 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",7859,"ΤΕΜ",1,"GMC",1,"1PH81331DF102GC1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8133-1DF22-0FH1","SIMOTICS M compact asynchronous motor 1500 rpm 17 kW 108 Nm 38 A 345 V 1750 rpm 19.5 kW 106 Nm 38 A 403 V 2000 rpm 22.5 kW 107 Nm 38 A 452 V 2200 rpm 24 kW 104 Nm 37 A 495 V water cooling degree of protection IP65 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: INCREASED RADIAL FORCES, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE D-END SIGNAL CONNECTION LEFT",10054,"ΤΕΜ",1,"GMC",1,"1PH81331DF220FH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8133-1DG03-1BA1","SIMOTICS M compact asynchronous motor 2000 rpm 20 kW 96 Nm 45 A 350 V 2300 rpm 22.5 kW 93 Nm 44 A 400 V 2650 rpm 24 kW 86 Nm 41 A 456 V 2800 rpm 25 kW 85 Nm 41 A 480 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",9101,"ΤΕΜ",1,"GMC",1,"1PH81331DG031BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8133-1DG10-2BB1","SIMOTICS M compact asynchronous motor 2000 rpm 20 kW 96 Nm 45 A 350 V 2300 rpm 22.5 kW 93 Nm 44 A 400 V 2650 rpm 24 kW 86 Nm 41 A 456 V 2800 rpm 25 kW 85 Nm 41 A 480 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",8287,"ΤΕΜ",1,"GMC",1,"1PH81331DG102BB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8133-1FD02-0BE1","SIMOTICS M compact asynchronous motor 1000 rpm 12 kW 115 Nm 30 A 319 V 1150 rpm 13.5 kW 112 Nm 29 A 361 V 1350 rpm 15 kW 106 Nm 28 A 417 V 1500 rpm 16.6 kW 106 Nm 28 A 459 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",10013,"ΤΕΜ",1,"GMC",1,"1PH81331FD020BE1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8133-1FG00-1BA1","SIMOTICS M compact asynchronous motor 2000 rpm 20 kW 96 Nm 45 A 350 V 2300 rpm 22.5 kW 93 Nm 44 A 400 V 2650 rpm 24 kW 86 Nm 41 A 456 V 2800 rpm 25 kW 85 Nm 41 A 480 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",9655,"ΤΕΜ",1,"GMC",1,"1PH81331FG001BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8133-1SD02-3MA1","SIMOTICS M compact asynchronous motor 1000 rpm 12 kW 115 Nm 30 A 319 V 1150 rpm 13.5 kW 112 Nm 29 A 361 V 1350 rpm 15 kW 106 Nm 28 A 417 V 1500 rpm 16.6 kW 106 Nm 28 A 459 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 19-bit Without commutation position (encoder IN19DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN HOLLOW-SHAFT BEARING: HIGH PERFORMANCE VIBRATION SEVERITY GRADE SPECIAL/B SHAFT AND FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",14891,"ΤΕΜ",1,"GMC",1,"1PH81331SD023MA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8133-1SG02-0MC1","SIMOTICS M compact asynchronous motor 2000 rpm 20 kW 96 Nm 45 A 350 V 2300 rpm 22.5 kW 93 Nm 44 A 400 V 2650 rpm 24 kW 86 Nm 41 A 456 V 2800 rpm 25 kW 85 Nm 41 A 480 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 19-bit Without commutation position (encoder IN19DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: HIGH PERFORMANCE VIBRATION SEVERITY GRADE SPECIAL/B SHAFT AND FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",12497,"ΤΕΜ",1,"GMC",1,"1PH81331SG020MC1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8133-2DF13-1BB1","SIMOTICS M Compact synchronous motor 1500rpm, 19.9kW 127Nm, 44A, 316V 1750rpm, 23.1kW 126Nm, 43A, 366V 2000rpm, 26.2kW 125Nm, 43A, 415 V forced ventilation; direction of air flow NDE--> DE, Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",17674,"ΤΕΜ",1,"GMC",1,"1PH81332DF131BB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8133-2FF03-0CA1","SIMOTICS M Compact synchronous motor 1500rpm, 19.9kW 127Nm, 44A, 316V 1750rpm, 23.1kW 126Nm, 43A, 366V 2000rpm, 26.2kW 125Nm, 43A, 415 V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",19335,"ΤΕΜ",1,"GMC",1,"1PH81332FF030CA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8135-1DF00-0FA1","SIMOTICS M compact asynchronous motor 1500 rpm 18.5 kW 118 Nm 43 A 330 V 1750 rpm 21.5 kW 117 Nm 43 A 383 V 2000 rpm 24 kW 115 Nm 43 A 434 V 2200 rpm 26.4 kW 115 Nm 43 A 468 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: INCREASED RADIAL FORCES, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",9112,"ΤΕΜ",1,"GMC",1,"1PH81351DF000FA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8135-1DF02-1LA1","SIMOTICS M compact asynchronous motor 1500 rpm 18.5 kW 118 Nm 43 A 330 V 1750 rpm 21.5 kW 117 Nm 43 A 383 V 2000 rpm 24 kW 115 Nm 43 A 434 V 2200 rpm 26.4 kW 115 Nm 43 A 468 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE: SPECIAL/B, SHAFT AND FLANGE ACCURACY: SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",10094,"ΤΕΜ",1,"GMC",1,"1PH81351DF021LA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8135-1DF10-2BC1","SIMOTICS M compact asynchronous motor 1500 rpm 18.5 kW 118 Nm 43 A 330 V 1750 rpm 21.5 kW 117 Nm 43 A 383 V 2000 rpm 24 kW 115 Nm 43 A 434 V 2200 rpm 26.4 kW 115 Nm 43 A 468 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",8915,"ΤΕΜ",1,"GMC",1,"1PH81351DF102BC1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8135-1DS02-0DA1","SIMOTICS M Compact induction motor 2000rpm, 24.5kW, 117Nm, 51A, 372V; 5000rpm, 18.5kW, 47Nm, 52A, 425V; 1500rpm, 18.5kW, 118Nm, 51A, 283V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: SR/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",9672,"ΤΕΜ",1,"GMC",1,"1PH81351DS020DA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8135-1FF00-1BA1","SIMOTICS M compact asynchronous motor 1500 rpm 18.5 kW 118 Nm 43 A 330 V 1750 rpm 21.5 kW 117 Nm 43 A 383 V 2000 rpm 24 kW 115 Nm 43 A 434 V 2200 rpm 26.4 kW 115 Nm 43 A 468 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",10283,"ΤΕΜ",1,"GMC",1,"1PH81351FF001BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8135-2DF00-0BA1","SIMOTICS M Compact synchronous motor 1500rpm, 23.7kW 151Nm, 43A, 383V 1750rpm, 27.2kW 149Nm, 42A, 415 V 2000rpm, 30.2kW 144Nm, 42A, 449V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",17592,"ΤΕΜ",1,"GMC",1,"1PH81352DF000BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8135-2DF10-1GA1","SIMOTICS M Compact synchronous motor 1500rpm, 23.7kW 151Nm, 43A, 383V 1750rpm, 27.2kW 149Nm, 42A, 415 V 2000rpm, 30.2kW 144Nm, 42A, 449V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",17164,"ΤΕΜ",1,"GMC",1,"1PH81352DF101GA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8135-2FF02-0CH1","SIMOTICS M Compact synchronous motor 1500rpm, 23.7kW 151Nm, 43A, 383V 1750rpm, 27.2kW 149Nm, 42A, 415 V 2000rpm, 30.2kW 144Nm, 42A, 449V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE D-END SIGNAL CONNECTION LEFT",19611,"ΤΕΜ",1,"GMC",1,"1PH81352FF020CH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8137-1DB02-2GA1","SIMOTICS M compact asynchronous motor 400 rpm 6.9 kW 165 Nm 18 A 323 V 500 rpm 8.6 kW 164 Nm 18 A 391 V 600 rpm 10.3 kW 164 Nm 18 A 458 V 700 rpm 11.5 kW 157 Nm 17.5 A 500 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",9259,"ΤΕΜ",1,"GMC",1,"1PH81371DB022GA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8137-1DD02-2FA1","SIMOTICS M compact asynchronous motor 1000 rpm 17 kW 162 Nm 43 A 307 V 1150 rpm 19.5 kW 162 Nm 43 A 350 V 1350 rpm 22 kW 156 Nm 42 A 404 V 1500 rpm 24 kW 153 Nm 41 A 447 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: INCREASED RADIAL FORCES, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",9885,"ΤΕΜ",1,"GMC",1,"1PH81371DD022FA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8137-1DD10-0DH1","SIMOTICS M compact asynchronous motor 1000 rpm 17 kW 162 Nm 43 A 307 V 1150 rpm 19.5 kW 162 Nm 43 A 350 V 1350 rpm 22 kW 156 Nm 42 A 404 V 1500 rpm 24 kW 153 Nm 41 A 447 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: SR/A, SHAFT AND FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE D-END SIGNAL CONNECTION LEFT",9728,"ΤΕΜ",1,"GMC",1,"1PH81371DD100DH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8137-1DD12-2BA1","SIMOTICS M compact asynchronous motor 1000 rpm 17 kW 162 Nm 43 A 307 V 1150 rpm 19.5 kW 162 Nm 43 A 350 V 1350 rpm 22 kW 156 Nm 42 A 404 V 1500 rpm 24 kW 153 Nm 41 A 447 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",9687,"ΤΕΜ",1,"GMC",1,"1PH81371DD122BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8137-1DF02-2GA1","SIMOTICS M compact asynchronous motor 1500 rpm 22 kW 140 Nm 56 A 308 V 1750 rpm 25 kW 136 Nm 56 A 352 V 2000 rpm 28 kW 134 Nm 55 A 401 V 2200 rpm 30 kW 130 Nm 53 A 440 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",9259,"ΤΕΜ",1,"GMC",1,"1PH81371DF022GA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8137-1DF13-2BC1","SIMOTICS M compact asynchronous motor 1500 rpm 22 kW 140 Nm 56 A 308 V 1750 rpm 25 kW 136 Nm 56 A 352 V 2000 rpm 28 kW 134 Nm 55 A 401 V 2200 rpm 30 kW 130 Nm 53 A 440 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",10143,"ΤΕΜ",1,"GMC",1,"1PH81371DF132BC1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8137-1DG02-0BB1","SIMOTICS M compact asynchronous motor 2000 rpm 28 kW 134 Nm 60 A 350 V 2300 rpm 29 kW 120 Nm 56 A 398 V 2650 rpm 30 kW 108 Nm 52 A 460 V 2800 rpm 31 kW 106 Nm 52 A 494 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",9687,"ΤΕΜ",1,"GMC",1,"1PH81371DG020BB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8137-1DG03-1CB1","SIMOTICS M compact asynchronous motor 2000 rpm 28 kW 134 Nm 60 A 350 V 2300 rpm 29 kW 120 Nm 56 A 398 V 2650 rpm 30 kW 108 Nm 52 A 460 V 2800 rpm 31 kW 106 Nm 52 A 494 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",10436,"ΤΕΜ",1,"GMC",1,"1PH81371DG031CB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8137-1FD02-0BA1","SIMOTICS M compact asynchronous motor 1000 rpm 17 kW 162 Nm 43 A 307 V 1150 rpm 19.5 kW 162 Nm 43 A 350 V 1350 rpm 22 kW 156 Nm 42 A 404 V 1500 rpm 24 kW 153 Nm 41 A 447 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",11055,"ΤΕΜ",1,"GMC",1,"1PH81371FD020BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8137-1FD10-2CH1","SIMOTICS M compact asynchronous motor 1000 rpm 17 kW 162 Nm 43 A 307 V 1150 rpm 19.5 kW 162 Nm 43 A 350 V 1350 rpm 22 kW 156 Nm 42 A 404 V 1500 rpm 24 kW 153 Nm 41 A 447 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE D-END SIGNAL CONNECTION LEFT",10990,"ΤΕΜ",1,"GMC",1,"1PH81371FD102CH1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8137-1FG00-0LA1","SIMOTICS M compact asynchronous motor 2000 rpm 28 kW 134 Nm 60 A 350 V 2300 rpm 29 kW 120 Nm 56 A 398 V 2650 rpm 30 kW 108 Nm 52 A 460 V 2800 rpm 31 kW 106 Nm 52 A 494 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE: SPECIAL/B, SHAFT AND FLANGE ACCURACY: SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",11518,"ΤΕΜ",1,"GMC",1,"1PH81371FG000LA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8137-1MF00-2BG2","SIMOTICS M compact asynchronous motor 1500 rpm 22 kW 140 Nm 56 A 308 V 1750 rpm 25 kW 136 Nm 56 A 352 V 2000 rpm 28 kW 134 Nm 55 A 401 V 2200 rpm 30 kW 130 Nm 53 A 440 V forced ventilation; direction of air flow DE --> NDE; IP55 degree of protection Incremental encoder SIN/COS 1 VPP 2048 S/R with C and D track (encoder IC2048S/R) with temperature sensor Pt1000 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",8287,"ΤΕΜ",1,"GMC",1,"1PH81371MF002BG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8137-1UD00-2LA1","SIMOTICS M compact asynchronous motor 1000 rpm 17 kW 162 Nm 43 A 307 V 1150 rpm 19.5 kW 162 Nm 43 A 350 V 1350 rpm 22 kW 156 Nm 42 A 404 V 1500 rpm 24 kW 153 Nm 41 A 447 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 20-bit Without commutation position (encoder IN20DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE: SPECIAL/B, SHAFT AND FLANGE ACCURACY: SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",10461,"ΤΕΜ",1,"GMC",1,"1PH81371UD002LA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8137-2DF02-2FC1","SIMOTICS M Compact synchronous motor 1500rpm, 30.6kW 195Nm, 60A, 356V 1750rpm, 35.6kW 194Nm, 59A, 412V 2000rpm, 40 kW 191Nm, 59A, 449V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: INCREASED RADIAL FORCES, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",19710,"ΤΕΜ",1,"GMC",1,"1PH81372DF022FC1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8137-2DL02-0BA1","SIMOTICS M Compact synchronous motor 2500rpm, 48.4kW 185Nm, 83A, 371V 2800rpm, 53.4kW 182Nm, 82A, 415 V 3000rpm, 56.9kW 181Nm, 81A, 449V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",19512,"ΤΕΜ",1,"GMC",1,"1PH81372DL020BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8137-2FL02-0CA1","SIMOTICS M Compact synchronous motor 2500rpm, 48.4kW 185Nm, 83A, 371V 2800rpm, 53.4kW 182Nm, 82A, 415 V 3000rpm, 56.9kW 181Nm, 81A, 449V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",21173,"ΤΕΜ",1,"GMC",1,"1PH81372FL020CA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8138-1DF20-0BC1","SIMOTICS M compact asynchronous motor 1500 rpm 30 kW 191 Nm 80 A 289 V 1750 rpm 33 kW 180 Nm 77 A 332 V 2000 rpm 37 kW 177 Nm 76 A 380 V 2200 rpm 39 kW 169 Nm 72 A 410 V water cooling degree of protection IP65 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",11631,"ΤΕΜ",1,"GMC",1,"1PH81381DF200BC1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8138-2FF20-1BA1","SIMOTICS M Compact synchronous motor 1500rpm, 44.9kW 286Nm, 118A, 316V 1750rpm, 52.4kW 286Nm, 118A, 366V 2000rpm, 59.7kW 285Nm, 118A, 416V water cooling Degree of protection IP65 Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",21144,"ΤΕΜ",1,"GMC",1,"1PH81382FF201BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8163-1DB03-2BA1","SIMOTICS M compact asynchronous motor 400 rpm 9.5 kW 227 Nm 30 A 260 V 500 rpm 12 kW 229 Nm 30 A 325 V 600 rpm 14.5 kW 231 Nm 30 A 370 V 700 rpm 16.9 kW 231 Nm 30 A 427 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",12011,"ΤΕΜ",1,"GMC",1,"1PH81631DB032BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8163-1DD03-0FA1","SIMOTICS M compact asynchronous motor 1000 rpm 22 kW 210 Nm 55 A 300 V 1150 rpm 25 kW 208 Nm 55 A 343 V 1350 rpm 28 kW 198 Nm 52 A 400 V 1500 rpm 31 kW 197 Nm 52 A 442 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: INCREASED RADIAL FORCES, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",11988,"ΤΕΜ",1,"GMC",1,"1PH81631DD030FA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8163-1DD12-1BA1","SIMOTICS M compact asynchronous motor 1000 rpm 22 kW 210 Nm 55 A 300 V 1150 rpm 25 kW 208 Nm 55 A 343 V 1350 rpm 28 kW 198 Nm 52 A 400 V 1500 rpm 31 kW 197 Nm 52 A 442 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",12011,"ΤΕΜ",1,"GMC",1,"1PH81631DD121BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8163-1DF00-2BB1","SIMOTICS M compact asynchronous motor 1500 rpm 30 kW 191 Nm 71 A 319 V 1750 rpm 34 kW 186 Nm 70 A 366 V 2000 rpm 37 kW 177 Nm 68 A 416 V 2200 rpm 40.7 kW 177 Nm 68 A 456 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",11034,"ΤΕΜ",1,"GMC",1,"1PH81631DF002BB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8163-1DF10-1GB1","SIMOTICS M compact asynchronous motor 1500 rpm 30 kW 191 Nm 71 A 319 V 1750 rpm 34 kW 186 Nm 70 A 366 V 2000 rpm 37 kW 177 Nm 68 A 416 V 2200 rpm 40.7 kW 177 Nm 68 A 456 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",10606,"ΤΕΜ",1,"GMC",1,"1PH81631DF101GB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8163-1DF22-1CA1","SIMOTICS M compact asynchronous motor 1500 rpm 37 kW 236 Nm 84 A 328 V 1750 rpm 43 kW 235 Nm 84 A 380 V 2000 rpm 49 kW 234 Nm 84 A 430 V 2200 rpm 53 kW 230 Nm 83 A 460 V water cooling degree of protection IP65 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",14432,"ΤΕΜ",1,"GMC",1,"1PH81631DF221CA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8163-1DG20-0DA1","SIMOTICS M compact asynchronous motor 2000 rpm 42 kW 201 Nm 93 A 335 V 2300 rpm 48 kW 199 Nm 93 A 382 V 2650 rpm 55 kW 198 Nm 90 A 450 V 2800 rpm 56 kW 191 Nm 89 A 462 V water cooling degree of protection IP65 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE SR/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",13300,"ΤΕΜ",1,"GMC",1,"1PH81631DG200DA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8163-1FD13-2CA1","SIMOTICS M compact asynchronous motor 1000 rpm 22 kW 210 Nm 55 A 300 V 1150 rpm 25 kW 208 Nm 55 A 343 V 1350 rpm 28 kW 198 Nm 52 A 400 V 1500 rpm 31 kW 197 Nm 52 A 442 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",13672,"ΤΕΜ",1,"GMC",1,"1PH81631FD132CA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8163-1SD03-2LA1","SIMOTICS M compact asynchronous motor 1000 rpm 22 kW 210 Nm 55 A 300 V 1150 rpm 25 kW 208 Nm 55 A 343 V 1350 rpm 28 kW 198 Nm 52 A 400 V 1500 rpm 31 kW 197 Nm 52 A 442 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 19-bit (encoder IN19DQ) With DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",15019,"ΤΕΜ",1,"GMC",1,"1PH81631SD032LA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8165-1AF02-2BA2","SIMOTICS M compact asynchronous motor 1500 rpm 37 kW 236 Nm 78 A 350 V 1750 rpm 41 kW 224 Nm 76 A 400 V 2000 rpm 45 kW 215 Nm 75 A 440 V 2200 rpm 49.5 kW 215 Nm 75 A 493 V forced ventilation; direction of air flow DE --> NDE; IP55 degree of protection W/O ENCODER with TEMPERAT. SENSOR PT1000 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",10727,"ΤΕΜ",1,"GMC",1,"1PH81651AF022BA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8165-1DD00-1BB1","SIMOTICS M compact asynchronous motor 1000 rpm 28 kW 267 Nm 71 A 292 V 1150 rpm 31 kW 257 Nm 69 A 333 V 1350 rpm 34 kW 241 Nm 66 A 387 V 1500 rpm 37.7 kW 240 Nm 65 A 430 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",11864,"ΤΕΜ",1,"GMC",1,"1PH81651DD001BB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8165-1DD02-0BB1","SIMOTICS M compact asynchronous motor 1000 rpm 28 kW 267 Nm 71 A 292 V 1150 rpm 31 kW 257 Nm 69 A 333 V 1350 rpm 34 kW 241 Nm 66 A 387 V 1500 rpm 37.7 kW 240 Nm 65 A 430 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",12548,"ΤΕΜ",1,"GMC",1,"1PH81651DD020BB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8165-1DD13-1DA1","SIMOTICS M compact asynchronous motor 1000 rpm 28 kW 267 Nm 71 A 292 V 1150 rpm 31 kW 257 Nm 69 A 333 V 1350 rpm 34 kW 241 Nm 66 A 387 V 1500 rpm 37.7 kW 240 Nm 65 A 430 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE SR/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",13272,"ΤΕΜ",1,"GMC",1,"1PH81651DD131DA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8165-1DF00-2GA1","SIMOTICS M compact asynchronous motor 1500 rpm 37 kW 236 Nm 78 A 350 V 1750 rpm 41 kW 224 Nm 76 A 400 V 2000 rpm 45 kW 215 Nm 75 A 440 V 2200 rpm 49.5 kW 215 Nm 75 A 493 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",11436,"ΤΕΜ",1,"GMC",1,"1PH81651DF002GA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8165-1DF03-2QB1","SIMOTICS M compact asynchronous motor 1500 rpm 37 kW 236 Nm 78 A 350 V 1750 rpm 41 kW 224 Nm 76 A 400 V 2000 rpm 45 kW 215 Nm 75 A 440 V 2200 rpm 49.5 kW 215 Nm 75 A 493 V forced ventilation; direction of air flow DE--> NDE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: ADVANCED LIFETIME VIBRATION SEVERITY S/A SHAFT A. FLANGE ACCURACY GR. R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",13630,"ΤΕΜ",1,"GMC",1,"1PH81651DF032QB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8165-1DF13-0HA1","SIMOTICS M compact asynchronous motor 1500 rpm 37 kW 236 Nm 78 A 350 V 1750 rpm 41 kW 224 Nm 76 A 400 V 2000 rpm 45 kW 215 Nm 75 A 440 V 2200 rpm 49.5 kW 215 Nm 75 A 493 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",12413,"ΤΕΜ",1,"GMC",1,"1PH81651DF130HA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8165-1DF23-0DC1","SIMOTICS M compact asynchronous motor 1500 rpm 46 kW 293 Nm 104 A 330 V 1750 rpm 53 kW 289 Nm 104 A 374 V 2000 rpm 60 kW 287 Nm 103 A 426 V 2200 rpm 66 kW 287 Nm 103 A 457 V water cooling degree of protection IP65 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE SR/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",16556,"ΤΕΜ",1,"GMC",1,"1PH81651DF230DC1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8165-1DG10-1BB1","SIMOTICS M compact asynchronous motor 2000 rpm 41 kW 196 Nm 88 A 350 V 2300 rpm 44 kW 183 Nm 85 A 394 V 2650 rpm 50 kW 180 Nm 85 A 440 V 2800 rpm 50 kW 171 Nm 81 A 483 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",11864,"ΤΕΜ",1,"GMC",1,"1PH81651DG101BB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8165-1FD13-2BB1","SIMOTICS M compact asynchronous motor 1000 rpm 28 kW 267 Nm 71 A 292 V 1150 rpm 31 kW 257 Nm 69 A 333 V 1350 rpm 34 kW 241 Nm 66 A 387 V 1500 rpm 37.7 kW 240 Nm 65 A 430 V forced ventilation; direction of air flow NDE--> DE; IP55 degree of protection Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",14209,"ΤΕΜ",1,"GMC",1,"1PH81651FD132BB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8165-1FG23-0BA1","SIMOTICS M compact asynchronous motor 2000 rpm 53 kW 253 Nm 110 A 352 V 2300 rpm 60 kW 249 Nm 107 A 410 V 2650 rpm 65 kW 234 Nm 100 A 460 V 2800 rpm 68 kW 232 Nm 100 A 494 V water cooling degree of protection IP65 Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",17493,"ΤΕΜ",1,"GMC",1,"1PH81651FG230BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8165-2DF02-2BA1","SIMOTICS M Compact synchronous motor 1500rpm, 61kW 390Nm, 119A, 340V 1750rpm, 69kW 375Nm, 115A, 395V 2000rpm, 74kW 355Nm, 110 A, 445V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",23625,"ΤΕΜ",1,"GMC",1,"1PH81652DF022BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8165-2FF03-2QA1","SIMOTICS M Compact synchronous motor 1500rpm, 61kW 390Nm, 119A, 340V 1750rpm, 69kW 375Nm, 115A, 395V 2000rpm, 74kW 355Nm, 110 A, 445V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: ADVANCED LIFETIME VIBRATION SEVERITY S/A SHAFT A. FLANGE ACCURACY GR. R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",25782,"ΤΕΜ",1,"GMC",1,"1PH81652FF032QA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8166-1DF20-2BB1","SIMOTICS M compact asynchronous motor 1500 rpm 52 kW 331 Nm 116 A 332 V 1750 rpm 61 kW 333 Nm 116 A 381 V 2000 rpm 68 kW 325 Nm 116 A 426 V 2200 rpm 75 kW 326 Nm 116 A 470 V water cooling degree of protection IP65 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",16744,"ΤΕΜ",1,"GMC",1,"1PH81661DF202BB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8167-2DL13-2QA1","SIMOTICS M Compact synchronous motor 2500rpm, 95kW 360Nm, 177A, 350 V 2800rpm, 98kW 335Nm, 164A, 385 V 3000rpm, 99kW 315Nm, 155A, 410V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: ADVANCED LIFETIME VIBRATION SEVERITY S/A SHAFT A. FLANGE ACCURACY GR. R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",25988,"ΤΕΜ",1,"GMC",1,"1PH81672DL132QA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8167-2FF02-0BB1","SIMOTICS M Compact synchronous motor 1500rpm, 69kW 435Nm, 133A, 345V 1750rpm, 77kW 420Nm, 128A, 400 V 2000rpm, 82kW 395Nm, 123A, 450 V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",26274,"ΤΕΜ",1,"GMC",1,"1PH81672FF020BB1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8184-1DF03-2LC1","SIMOTICS M Compact induction motor 1500rpm, 51kW 325Nm, 116A, 335V 1750rpm, 60kW 327Nm, 120 A, 390V 2000rpm, 68kW 325Nm, 118A, 405V forced ventilation Direction of air flow DE-->NDE Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 with flange A450 (IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: PERFORMANCE VIBRATION SEVERITY GRADE SR/B SHAFT A. FLANGE ACCURACY GR. R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION RIGHT",26452,"ΤΕΜ",1,"GMC",1,"1PH81841DF032LC1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8184-1HF00-2EA2","SIMOTICS M Compact asynchronous motor 1500 rpm, 51 kW, 325 Nm, 116 A, 335 V 1750 rpm, 60 kW, 327 Nm, 120 A, 390 V 2000 rpm, 68 kW, 325 Nm, 118 A, 405 V Forced ventilation Direction of air flow DE-->NDE Degree of protection IP55 Incremental encoder HTL 1024 S/R (encoder HTL1024S/R) With temperature sensor Pt1000 DESIGN IM B3 (IMB6, IMB7, IMB8, IMV6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: GREATER CANTILEVER FORCES; VIBRATION SEVERITY GRADE A; SHAFT AND FLANGE ACCURACY GR. N TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",13949,"ΤΕΜ",1,"GMC",1,"1PH81841HF002EA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8186-1DD03-2BD1","SIMOTICS M Compact induction motor 1000rpm, 51kW 487Nm, 112A, 340V 1150rpm, 58kW 482Nm, 112A, 390V 1350rpm, 67kW 474Nm, 112A, 450 V forced ventilation Direction of air flow DE-->NDE Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 with flange A450 (IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD VIBRATION SEVERITY GRADE R/A; SHAFT A.FLANGE ACCURACY GR. R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE D-END SIGNAL CONNECTION RIGHT",22539,"ΤΕΜ",1,"GMC",1,"1PH81861DD032BD1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8186-1DF33-2BA1","SIMOTICS M Compact induction motor 1500rpm, 108kW 688Nm, 225 A, 330V 1750rpm, 125kW 682Nm, 225 A, 385 V 2000rpm, 135kW 645Nm, 210A, 445V Open-circuit ventilation Direction of air flow DE-->NDE Degree of protection IP23 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 with flange A450 (IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD VIBRATION SEVERITY GRADE R/A; SHAFT A.FLANGE ACCURACY GR. R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",26692,"ΤΕΜ",1,"GMC",1,"1PH81861DF332BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8186-2DF10-1BC1","SIMOTICS M Compact synchronous motor 1500rpm, 93kW, 592Nm, 215A, 282V 1750rpm, 109kW, 595Nm, 215A, 328V 2000rpm, 115kW, 549Nm, 200 A, 370V forced ventilation Direction of air flow NDE-->DE Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IMB6, IMB7, IMB8, IMV6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD VIBRATION SEVERITY GRADE R/A; SHAFT A.FLANGE ACCURACY GR. R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION RIGHT",30712,"ΤΕΜ",1,"GMC",1,"1PH81862DF101BC1","Ρυθμιστές στροφών και συστήματα Motion control"]
["1PH8224-3DL00-2AA1","SIMOTICS M Compact induction motor 2500rpm, 142kW, 542Nm, 295A, 340V 2900rpm, 149kW, 491Nm, 270A, 395V 3400rpm, 85kW, 239Nm, 168A, 460 V forced ventilation Direction of air flow DE-->NDE Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",25174,"ΤΕΜ",1,"GMC",1,"1PH82243DL002AA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["3KC0334-2NE00-0AA0","SENTRON, 3KC transfer switching equipment, manually operated, MTSE, size: 2, 3-pole, Iu: 160 A, Ue AC: 415 V, Ie at AC-33 B at 415 V: 160 A, Ie at AC-23 A at 690 V: 125 A, screw and standard mounting rail installation 35 mm, Front operating mechanism, centered, without handle, box terminal",426.11,"ΤΕΜ",1,"EP",1,"3KC03342NE000AA0","3KC Μεταγωγικοί διακόπτες"]
["3KC4450-0FA21-0AA3","SENTRON, transfer switching equipment 3KC, remotely operated, RTSE, 4-pole, Iu: 1000 A, Ue AC: 415 V, Ie at AC-33 B at 415 V: 1000 A, Ie at AC-23 A at 690 V: 630 A, screw mounting, motorized operating mechanism, at the right end, long handle, busbar connection",8132.49,"ΤΕΜ",1,"EP",1,"3KC44500FA210AA3","3KC Μεταγωγικοί διακόπτες"]
["3KC8360-0JA22-0GA3","SENTRON, ATE, transfer switching equipment 3KC, automatically, ATSE, 3- pole, Iu: 3200 A, Ue AC: 415 V, Ie at AC-33 B at 415 V: 1250 A, screw mounting, motorized operating mechanism, at the right end, long handle, busbar connection",24787.1,"ΤΕΜ",1,"EP",1,"3KC83600JA220GA3","3KC Μεταγωγικοί διακόπτες"]
["3KC9618-3","Accessory for 3KC3, 3KC6 Connecting jumper for load-side connection 4-pole for 160 A contains 1 unit",176.58,"ΤΕΜ",1,"EP",1,"3KC96183","3KC Μεταγωγικοί διακόπτες"]
["3KC9831-4","Accessory for 3KC8 Power supply cable for connection at the top 4-pole for 800-1000 A contains 1 unit",292.64,"ΤΕΜ",1,"EP",1,"3KC98314","3KC Μεταγωγικοί διακόπτες"]
["3KD0340-2LG20-3","Switch disconnector 63A, size 02, 4-pole Front operating mechanism center Basic unit without handle Box terminal",90.48,"ΤΕΜ",1,"EP",1,"3KD03402LG203","3KD  Διακόπτες φορτίου μεχρι 2000Α"]
["3KD2832-2NE10-0","Switch disconnector 80 A, Size 2, 3-pole Front operating mechanism left Complete unit with direct operating mechanism gray Box terminal",141.1,"ΤΕΜ",1,"EP",1,"3KD28322NE100","3KD  Διακόπτες φορτίου μεχρι 2000Α"]
["3KD3440-0NE20-0","Switch disconnector 160 A, Size 2, 4-pole Front operating mechanism center Basic unit without handle flat terminal incl. phase barriers",200.6,"ΤΕΜ",1,"EP",1,"3KD34400NE200","3KD  Διακόπτες φορτίου μεχρι 2000Α"]
["3KD3840-0NE20-0","SWITCH-DISCONNECTOR 250A, FRAME SIZE 2, 4-POLE FRONT OPERATING CENTER BASIC UNIT WITHOUT HANDLE FLAT TERMINAL INCL. PHASE BARRIERS",349.35,"ΤΕΜ",1,"EP",1,"3KD38400NE200","3KD  Διακόπτες φορτίου μεχρι 2000Α"]
["3KD4440-0PE10-0","SWITCH-DISCONNECTOR 500A, FRAME SIZE 3, 4-POLE FRONT OPERATING LEFT BASIC UNIT WITHOUT HANDLE FLAT TERMINAL",701.25,"ΤΕΜ",1,"EP",1,"3KD44400PE100","3KD  Διακόπτες φορτίου μεχρι 2000Α"]
["3KD5230-0RE20-0","Switch disconnector 1250 A, Size 5, 3-pole Front operating mechanism center Basic unit without handle flat terminal",2575.5,"ΤΕΜ",1,"EP",1,"3KD52300RE200","3KD  Διακόπτες φορτίου μεχρι 2000Α"]
["3KD9015-2","Accessory for 3KD0 size 01 Fourth pole, switchable Box terminal",22.15,"ΤΕΜ",1,"EP",1,"3KD90152","3KD  Διακόπτες φορτίου μεχρι 2000Α"]
["3KD9505-0","Accessory for 3KD size 5 Fourth pole, can be switched flat terminal",753.95,"ΤΕΜ",1,"EP",1,"3KD95050","3KD  Διακόπτες φορτίου μεχρι 2000Α"]
["3KF2312-0LF11","Switch disconnector with fuse 125 A, Size 2, 3-pole for LV HRC fuse Sz. 000 and 00 Front operating mechanism left Basic unit without handle flat terminal",254.7,"ΤΕΜ",1,"EP",1,"3KF23120LF11","3KF  Διακόπτες φορτίου με ασφάλειες"]
["3KF9105-1AA00","Accessory for 3KF size 1 Fourth pole, switchable for LV HRC fuse Sz. 000 flat terminal on the rear",62.27,"ΤΕΜ",1,"EP",1,"3KF91051AA00","3KF  Διακόπτες φορτίου με ασφάλειες"]
["3KF9412-0CA00","Replacement part for 3KF size 4 Fuse cover",22.66,"ΤΕΜ",1,"EP",1,"3KF94120CA00","3KF  Διακόπτες φορτίου με ασφάλειες"]
["3LD2064-1GP53","SENTRON, Switch disconnector 3LD, emergency switching-off switch, 3- pole, Iu: 16 A, operating power / at AC-23 A 400 V: 7.5 kW, Molded plastic encapsulation for metric cable gland, 1 NC, 1 NO, rotary operating mechanism, red/yellow",68,"ΤΕΜ",1,"EP",1,"3LD20641GP53","3LD Διακόπτες φορτίου μεχρι 250Α"]
["3LD2113-0TK53","SENTRON, Switch disconnector 3LD, emergency switching-off switch, 3- pole, Iu: 25 A, operating power / at AC-23 A 400 V: 9.5 kW, floor mounting with door coupling, rotary operating mechanism, Red / yellow, 4-hole mounting of the handle",64.61,"ΤΕΜ",1,"EP",1,"3LD21130TK53","3LD Διακόπτες φορτίου μεχρι 250Α"]
["3LD2164-0TB53-0US2","SENTRON, Switch disconnector 3LD, emergency switching-off switch, 3- pole, Iu: 25 A, operating power / at AC-23 A 400 V: 9.5 kW, Molded plastic encapsulation for inch cable gland, rotary operating mechanism, red/yellow",88.4,"ΤΕΜ",1,"EP",1,"3LD21640TB530US2","3LD Διακόπτες φορτίου μεχρι 250Α"]
["3LD2264-0TB51","SENTRON, Switch disconnector 3LD, main switch, 3-pole, Iu: 32 A, Operating power / at AC-23 A at 400 V: 11.5 kW, molded-plastic encapsulation for metric cable gland, rotary operating mechanism, black",66.31,"ΤΕΜ",1,"EP",1,"3LD22640TB51","3LD Διακόπτες φορτίου μεχρι 250Α"]
["3LD2515-0TK53","SENTRON, Switch disconnector 3LD, emergency switching-off switch, 3- pole, Iu: 63 A, operating power / at AC-23 A 400 V: 22 kW, floor mounting with door coupling, rotary operating mechanism, Red / yellow, 4-hole mounting of the handle, without tolerance compensation",91.8,"ΤΕΜ",1,"EP",1,"3LD25150TK53","3LD Διακόπτες φορτίου μεχρι 250Α"]
["3LD2704-1TP51","SENTRON, Switch disconnector 3LD, main switch, 3-pole, Iu: 100 A, Operating power / at AC-23 A at 400 V: 37 kW, front-mounted, 1 NC, 1 NO, rotary operating mechanism, black, 4-hole mounting of the handle",131.75,"ΤΕΜ",1,"EP",1,"3LD27041TP51","3LD Διακόπτες φορτίου μεχρι 250Α"]
["3LD3010-0TL05","Load disconnector 3LD3, Iu 16 A Main switch 3-pole + N Rated operating capacity at AC-23 A at 400V 7.5kW Installation in distribution boards, Basic switch without Knob-operated mechanism",32.42,"ΤΕΜ",1,"EP",1,"3LD30100TL05","3LD Διακόπτες φορτίου μεχρι 250Α"]
["3LD3130-0TL13","Load disconnector 3LD3, Iu 25 A Main switch 3-pole + N Rated operating capacity at AC-23 A at 400V 9.0kW Installation in distribution boards, Basic switch with selector knob red / yellow",38.17,"ΤΕΜ",1,"EP",1,"3LD31300TL13","3LD Διακόπτες φορτίου μεχρι 250Α"]
["3LD3230-0TL11","Load disconnector 3LD3, Iu 32 A Main switch 3-pole + N Rated operating capacity for AC-23 A at 400V 11.5kW Installation in distribution boards, Basic switch with selector knob black",42.85,"ΤΕΜ",1,"EP",1,"3LD32300TL11","3LD Διακόπτες φορτίου μεχρι 250Α"]
["3LD3354-1TL53","Load disconnector 3LD3, Iu 40 A Main switch 3-pole + N Rated operating capacity at AC-23 A at 400 V 18.5 kW Front plate mounting Basic switch with Central hole mounting 22.5mm Toggle drive red / yellow 66x66 mm with auxiliary switch 1OE + 1S",76.67,"ΤΕΜ",1,"EP",1,"3LD33541TL53","3LD Διακόπτες φορτίου μεχρι 250Α"]
["3LD3454-0TK53","Load disconnector 3LD3, Iu 63 A Main switch 3-pole Rated operating capacity at AC-23 A at 400V 22.0 kW Front plate mounting Basic switch with Central hole mounting 22.5mm Toggle drive red / yellow 66x66 mm",59.25,"ΤΕΜ",1,"EP",1,"3LD34540TK53","3LD Διακόπτες φορτίου μεχρι 250Α"]
["3LD9201-2A","Terminal cover, 1-pole, 16A, accessory for main and emergency switching-off switch 3LD2",106.25,"ΤΕΜ",100,"EP",4,"3LD92012A","3LD Διακόπτες φορτίου μεχρι 250Α"]
["3LD9340-2B","N-through terminal, Front installation, accessory for Load disconnector 3LD3",10.119999999999999,"ΤΕΜ",1,"EP",1,"3LD93402B","3LD Διακόπτες φορτίου μεχρι 250Α"]
["3LD9340-6B","Auxiliary switch, Front installation 1 OE + 1 S left and / or right mountable, accessory for Load disconnector 3LD3",13.52,"ΤΕΜ",1,"EP",1,"3LD93406B","3LD Διακόπτες φορτίου μεχρι 250Α"]
["3NA3236","LV HRC fuse element, NH2, In: 160 A, gG, Un AC: 500 V, Un DC: 440 V, Front indicator, live grip lugs",20.54,"ΤΕΜ",1,"EP",3,"3NA3236","3ΝΑ Μαχαιρωτές ασφάλειες"]
["3NA3807-6","LV HRC fuse element, NH000, In: 20 A, gG, Un AC: 690 V, Un DC: 250 V, Front indicator, live grip lugs",29.1,"ΤΕΜ",1,"EP",3,"3NA38076","3ΝΑ Μαχαιρωτές ασφάλειες"]
["3NA6140","LV HRC fuse element, NH1, In: 200 A, gG, Un AC: 500 V, Un DC: 440 V, Combined indicator, Insulated grip lugs",23.87,"ΤΕΜ",1,"EP",3,"3NA6140","3ΝΑ Μαχαιρωτές ασφάλειες"]
["3NA6236","LV HRC fuse element, NH2, In: 160 A, gG, Un AC: 500 V, Un DC: 440 V, Combined indicator, Insulated grip lugs",28.43,"ΤΕΜ",1,"EP",3,"3NA6236","3ΝΑ Μαχαιρωτές ασφάλειες"]
["3NA7232-6","LV HRC fuse element, NH2, In: 125 A, gG, Un AC: 690 V, Un DC: 440 V, Combined indicator, live grip lugs",73.319999999999993,"ΤΕΜ",1,"EP",3,"3NA72326","3ΝΑ Μαχαιρωτές ασφάλειες"]
["3NA7804","LV HRC fuse element, NH000, In: 4 A, gG, Un AC: 500 V, Un DC: 250 V, Combined indicator, live grip lugs",8.98,"ΤΕΜ",1,"EP",3,"3NA7804","3ΝΑ Μαχαιρωτές ασφάλειες"]
["3NC1401","SITOR cylindrical fuse link, 14x51 mm, 1 A, aR, Un AC: 660 V",11.97,"ΤΕΜ",1,"EP",10,"3NC1401","3NC Κυλινδρικές ασφάλειες"]
["3NC1440-0MK","SITOR cylindrical fuse link, 14x51 mm, 40 A, gR, Un AC: 690 V, Un DC: 440 V",15.21,"ΤΕΜ",1,"EP",10,"3NC14400MK","3NC Κυλινδρικές ασφάλειες"]
["3NC3243-6U","SITOR fuse link, with female thread on both sides, NH3, In: 1250 A, aR, Un AC: 690 V, Un DC: 440 V, front indicator",275.60000000000002,"ΤΕΜ",1,"EP",3,"3NC32436U","3NC Ασφάλειες υπερταχείας aR"]
["3NC8434-3C","SITOR fuse link, with slotted blade contacts, NH3, In: 500 A, gR, Un AC: 690 V, Un DC: 440 V, front indicator",252.2,"ΤΕΜ",1,"EP",3,"3NC84343C","3NC Ασφάλειες υπερταχείας gR"]
["3NE1332-4D","PV fuse link, with blade contacts, NH2L, In: 400 A, gPV, Un DC: 1000 V, front indicator",469.35,"ΤΕΜ",1,"EP",2,"3NE13324D","3NE Ασφάλειες PV"]
["3NE1435-3","SITOR fuse link, with slotted blade contacts, NH3, In: 560 A, gR, Un AC: 690 V, Un DC: 440 V, front indicator",265.2,"ΤΕΜ",1,"EP",3,"3NE14353","3NE Ασφάλειες υπερταχείας gS"]
["3NE3432-0C","SITOR fuse link, with slotted blade contacts, NH3, In: 400 A, aR, Un AC: 1000 V, Un DC: 440 V, front indicator",232.7,"ΤΕΜ",1,"EP",3,"3NE34320C","3NE Ασφάλειες υπερταχείας aR"]
["3NE8003-1","SITOR fuse link, with blade contacts, NH00, In: 35 A, gR, Un AC: 690 V, Un DC: 440 V, front indicator",53.04,"ΤΕΜ",1,"EP",3,"3NE80031","3NE Ασφάλειες υπερταχείας aR"]
["3NE8724-1","SITOR fuse link, with Bolt-on links, NH000, In: 160 A, aR, Un AC: 690 V, Un DC: 440 V, front indicator",82.16,"ΤΕΜ",1,"EP",10,"3NE87241","3NE Ασφάλειες υπερταχείας gR"]
["3NJ4133-3BJ01","In-line fuse switch disconnector 3-pole selectable, Sz. 2 I=400 A, U=690 V stud terminal M12, new design",645.53,"ΤΕΜ",1,"EP",1,"3NJ41333BJ01","3NJ Ασφαλειοαποζεύκτες"]
["3NJ4911-4AA00","accessory for In-line fuse switch disconnectors 3NJ4103 Kit saddle terminal CU 1.5 to 70 mm2 1 set = 3 units",5.1100000000000003,"ΤΕΜ",1,"EP",1,"3NJ49114AA00","3NJ Ασφαλειοαποζεύκτες"]
["3NJ4915-2GB11","Accessory for strips 3NJ41 In-line fuse switch disconnectors Sz. NH1-3 Current transformers can be integrated 250/5 A, Cl. 0.5 legal-for-trade calibrated",723.78,"ΤΕΜ",1,"EP",1,"3NJ49152GB11","3NJ Ασφαλειοαποζεύκτες"]
["3NJ6900-4HG11","accessory for Switch disconnector with fuses In-line design, pluggable Ammeter, Moving iron 250/1 A, Cl. 1, 0.6 VA 2-fold overload",123.06,"ΤΕΜ",1,"EP",1,"3NJ69004HG11","3NJ Ασφαλειοαποζεύκτες"]
["3NJ6930-3BF21","accessory for Switch disconnector with fuses In-line design, pluggable current transformer 200/5 A, Cl. 1, 2.5 VA",103.25,"ΤΕΜ",1,"EP",1,"3NJ69303BF21","3NJ Ασφαλειοαποζεύκτες"]
["3NJ6940-3BH21","accessory for Switch disconnector with fuses In-line design, pluggable current transformer 300/5 A, Cl. 1, 5 VA",110.82,"ΤΕΜ",1,"EP",1,"3NJ69403BH21","3NJ Ασφαλειοαποζεύκτες"]
["3NP1133-1CA21","SENTRON, Fuse switch disconnector 3NP1, 3-pole, NH00, 160 A, for assembly and installation on mounting plate, Box terminal, Fuse monitoring: electromechanical, Cover level 45 mm",389.16,"ΤΕΜ",1,"EP",1,"3NP11331CA21","3NP Ασφαλειοαποζεύκτες"]
["3NP1143-1DA20","SENTRON, Fuse switch disconnector 3NP1, 3-pole, NH1, 250 A, for assembly and installation on mounting plate, Box terminal, Cover level 70 mm",343.62,"ΤΕΜ",1,"EP",1,"3NP11431DA20","3NP Ασφαλειοαποζεύκτες"]
["3NP1153-1JC11","SENTRON, Fuse switch disconnector 3NP1, 3-pole, NH2, 400 A, for Rittal busbar system 60 mm, flat terminal, Fuse monitoring: electromechanical, Cover level 32/70 mm",902.52,"ΤΕΜ",1,"EP",1,"3NP11531JC11","3NP Ασφαλειοαποζεύκτες"]
["3NP1920-1FB00","Auxiliary switch, 1 changeover contact Solid-state compatible, for Size NH000, accessory for fuse switch disconnector 3NP1",29.39,"ΤΕΜ",1,"EP",1,"3NP19201FB00","3NP Ασφαλειοαποζεύκτες"]
["3NP1931-1EB00","Mounting kit, for conversion to installation on standard mounting rail, for Size NH00, 32 mm installation on standard mounting rail, for Size NH00 1-pole for fuse switch disconnector 3NP1",13.97,"ΤΕΜ",1,"EP",1,"3NP19311EB00","3NP Ασφαλειοαποζεύκτες"]
["3NP1953-1BA00","Saddle terminal 120 - 240 mm2, for size NH2 with screw terminal, accessory for fuse switch disconnector 3NP1 Contains 3 terminals",28.15,"ΤΕΜ",1,"EP",1,"3NP19531BA00","3NP Ασφαλειοαποζεύκτες"]
["3NP1961-1BB20","Prism terminal double 2x 150 - 185mm2, for size NH3 1-pole with flat terminal, accessory for fuse switch disconnector 3NP1 Contains 1 terminal",52.58,"ΤΕΜ",1,"EP",1,"3NP19611BB20","3NP Ασφαλειοαποζεύκτες"]
["3NW3300-0HG","SENTRON, cylindrical fuse link, Class CC, 30 A, time-lag, current-limiting, Un AC: 600 V, respect national installation rules! for protection of motor-circuits",45.18,"ΤΕΜ",1,"EP",10,"3NW33000HG","3NW Κυλινδρικές ασφάλειες UL"]
["3NW7014","SENTRON, cylindrical fuse holder, 10x38 mm, 1-pole, In: 32 A, Un AC: 690 V, LED signal detector",14.03,"ΤΕΜ",1,"EP",1,"3NW7014","3NW Κυλινδρικές ασφάλειες "]
["3NW7034-1","SENTRON, cylindrical fuse holder, 10x38 mm, 3-pole, In: 32 A, Un AC: 690 V, LED signal detector, compact version",107.9,"ΤΕΜ",1,"EP",1,"3NW70341","3NW Κυλινδρικές ασφάλειες "]
["3NW8105-1","SENTRON, cylindrical fuse link, 14x51 mm, 16 A, aM, Un AC: 690 V",6.64,"ΤΕΜ",1,"EP",10,"3NW81051","3NW Κυλινδρικές ασφάλειες "]
["3NX8201","Electronicmodule for Smart Fuse Sicherung BaugrΓ¶Γ\u009fe 2 mit Please consider Radio approval! List of countries: see Certificates",320.38,"ΤΕΜ",1,"EP",1,"3NX8201","3NX εξαρτήματα ασφαλειών"]
["3RA2110-0BH15-1AP0","Load feeder fuseless, Direct-on-line starting 400 V AC, Size S00 0.14...0.20 A 230 V AC Spring-type terminal for 60 mm busbar systems (also fulfills type of coordination 1) Type of coordination 2, Iq = 150 kA 1 NO (contactor)",204.51,"ΤΕΜ",1,"EP",1,"3RA21100BH151AP0","3RA Εκκινητές"]
["3RA2110-0JE15-1AP0","Load feeder fuseless, Direct-on-line starting 400 V AC, Size S00 0.70...1.00 A 230 V AC Spring-type terminal for installation on standard mounting rail (also fulfills type of coordination 1) Type of coordination 2, Iq = 150 kA 1 NO (contactor)",152.88,"ΤΕΜ",1,"EP",1,"3RA21100JE151AP0","3RA Εκκινητές"]
["3RA2110-1AD15-1FB4","Load feeder fuseless, Direct-on-line starting 400 V AC, Size S00 1.10...1.60 A 24 V DC screw terminal for 60 mm busbar systems (also fulfills type of coordination 1) Type of coordination 2, Iq = 150 kA 1 NO (contactor) with diode (integrated)",226.35,"ΤΕΜ",1,"EP",1,"3RA21101AD151FB4","3RA Εκκινητές"]
["3RA2110-1HA15-1BB4","Load feeder fuseless, Direct-on-line starting 400 V AC, Size S00 5.50...8.00 A 24 V DC screw terminal for installation on standard mounting rail Type of coordination 1, Iq = 150 kA 1 NO (contactor)",169.76,"ΤΕΜ",1,"EP",1,"3RA21101HA151BB4","3RA Εκκινητές"]
["3RA2115-0HE15-1FB4","Load feeder fuseless, Direct-on-line starting 400 V AC, Size S00 0.55...0.80 A 24 V DC Spring-type terminal for installation on standard mounting rail (also fulfills type of coordination 1) Type of coordination 2, Iq = 150 kA 1 NO (contactor) with diode (integrated)",191.6,"ΤΕΜ",1,"EP",1,"3RA21150HE151FB4","3RA Εκκινητές"]
["3RA2120-1GE24-0BB4","Load feeder fuseless, Direct-on-line starting 400 V AC, Size S0 4.50...6.30 A 24 V DC Spring-type terminal for installation on standard mounting rail (also fulfills type of coordination 1) Type of coordination 2, Iq = 150 kA 1 NO+1 NC (contactor)",243.22,"ΤΕΜ",1,"EP",1,"3RA21201GE240BB4","3RA Εκκινητές"]
["3RA2120-4DH27-0AP0","Load feeder fuseless, Direct-on-line starting 400 V AC, Size S0 18...25 A 230 V AC Spring-type terminal for 60 mm busbar systems (also fulfills type of coordination 1) Type of coordination 2, Iq = 150 kA 1 NO+1 NC (contactor)",391.14,"ΤΕΜ",1,"EP",1,"3RA21204DH270AP0","3RA Εκκινητές"]
["3RA2120-4ND27-0AP0","Load feeder fuseless, Direct-on-line starting 400 V AC, Size S0 23.0...28.0 A 230 V AC screw terminal for 60 mm busbar systems (also fulfills type of coordination 1) Type of coordination 2, Iq = 150 kA 1 NO+1 NC (contactor)",424.9,"ΤΕΜ",1,"EP",1,"3RA21204ND270AP0","3RA Εκκινητές"]
["3RA2210-0FA15-2AP0","Load feeder fuseless, Reversing duty 400 V AC, Size S00 0.35...0.50 A 230 V AC screw terminal for installation on standard mounting rail (also fulfills type of coordination 1) Type of coordination 2, Iq = 150 kA 1 NC (contactor)",218.41,"ΤΕΜ",1,"EP",1,"3RA22100FA152AP0","3RA Εκκινητές"]
["3RA2210-0FH15-2AP0","Load feeder fuseless, Reversing duty 400 V AC, Size S00 0.35...0.50 A 230 V AC Spring-type terminal for 60 mm busbar systems (also fulfills type of coordination 1) Type of coordination 2, Iq = 150 kA 1 NC (contactor)",300.8,"ΤΕΜ",1,"EP",1,"3RA22100FH152AP0","3RA Εκκινητές"]
["3RA2210-1BS15-2BB4","Load feeder fuseless, Reversing duty 400 V AC, Size S00 1.40...2.00 A 24 V DC Spring-type terminal for 60 mm busbar systems (also fulfills type of coordination 1) Type of coordination 2, Iq = 150 kA 1 NC (contactor) Adapter length 200 mm",334.56,"ΤΕΜ",1,"EP",1,"3RA22101BS152BB4","3RA Εκκινητές"]
["3RA2210-4AD18-2AP0","Load feeder fuseless, Reversing duty 400 V AC, Size S00 10.0...16.0 A 230 V AC screw terminal for 60 mm busbar systems Type of coordination 1, Iq = 150 kA 1 NC (contactor)",397.1,"ΤΕΜ",1,"EP",1,"3RA22104AD182AP0","3RA Εκκινητές"]
["3RA2220-1JF24-0BB4","Load feeder fuseless, Reversing duty 400 V AC, Size S0 7.00...10.0 A 24 V DC Spring-type terminal for installation on standard mounting rail with standard mounting rail adapter (also fulfills type of coordination 1) Type of coordination 2, Iq = 150 kA 1 NO+1 NC (contactor)",458.65,"ΤΕΜ",1,"EP",1,"3RA22201JF240BB4","3RA Εκκινητές"]
["3RA2315-8XB30-2AK6","Reversing contactor assembly AC-3, 3 kW/400 V 110 V AC 50 Hz/120 V 60 Hz, 3-pole Size S00, Spring-type terminal electrical and mechanical interlock",122.05,"ΤΕΜ",1,"EP",1,"3RA23158XB302AK6","3RA Εκκινητές"]
["3RA2316-8XB30-2AK6","Reversing contactor assembly AC-3, 4 kW/400 V 110 V AC 50 Hz/120 V 60 Hz, 3-pole Size S00, Spring-type terminal electrical and mechanical interlock",127.51,"ΤΕΜ",1,"EP",1,"3RA23168XB302AK6","3RA Εκκινητές"]
["3RA2318-8XE30-2BB4","Reversing contactor assembly for 3RA27 AC-3, 7.5 kW/400 V, 24 V DC 3-pole, Size S00 Spring-type terminal electrical and mechanical interlock with voltage tap",263.22000000000003,"ΤΕΜ",1,"EP",1,"3RA23188XE302BB4","3RA Εκκινητές"]
["3RA2326-8XB30-1BB4","Reversing contactor assembly AC-3, 11 kW/400 V, 24 V DC 3-pole, Size S0 screw terminal electrical and mechanical Interlock 2 NO integrated",366.14,"ΤΕΜ",1,"EP",1,"3RA23268XB301BB4","3RA Εκκινητές"]
["3RA2347-8XB30-1AG2","Reversing contactor assembly, AC-3, 55 kW 400 V, 110 V AC/50/60 Hz 3-pole, Size S3 screw terminal electrical and mechanical interlock 2 NO integrated",1120.28,"ΤΕΜ",1,"EP",1,"3RA23478XB301AG2","3RA Εκκινητές"]
["3RA2416-8XF31-2AF0","Contactor assembly for star-delta (wye-delta) start AC-3, 7.5 kW/400 V, 110 V AC 50 Hz / 120 V, 60Hz, 3-pole Size S00, Spring-type terminals electrical and mechanical interlock 3 NO integrated",409.86,"ΤΕΜ",1,"EP",1,"3RA24168XF312AF0","3RA Εκκινητές"]
["3RA2446-8XF32-1AC2","Contactor assembly for star-delta (wye-delta) start AC-3, 90 kW/400 V 24 V AC/50/60 Hz Size S3, screw terminal electrical and mechanical interlock 3 NO+3 NC",1639.44,"ΤΕΜ",1,"EP",1,"3RA24468XF321AC2","3RA Εκκινητές"]
["3RA2711-1BA00","Function module for IO-Link, Reversing start, screw terminal, Installation on contactors 3RT2 Communication-capable contactor required",145.94,"ΤΕΜ",1,"EP",1,"3RA27111BA00","3RA Εκκινητές"]
["3RA2913-2AA1","Wiring kit for screw terminal Electrical and mechanical Including mechanical interlocking for reversing starter Size S00",36.659999999999997,"ΤΕΜ",1,"EP",1,"3RA29132AA1","3RA Εκκινητές"]
["3RA2942-2G","Mechanical connectors for Contactor assemblies size S3 4-pole for reversing contactor clearance 10 mm comprising 2 mechanical Connectors for 1 combination",3.75,"ΤΕΜ",1,"EP",10,"3RA29422G","3RA Εκκινητές"]
["3RA6120-1EP33","SIRIUS Compact load feeder DOL starter 690 V 110...240 V AC/DC 50...60 Hz 8...32 A IP20 Connection main circuit: plug-in, without terminals Connection auxiliary circuit: screw terminal",1071.46,"ΤΕΜ",1,"EP",1,"3RA61201EP33","3RA6 Compact εκκινητές"]
["3RA6250-2CP33","SIRIUS Compact load feeder Reversing starter 690 V 110...240 V AC/DC 50...60 Hz 1...4 A IP20 Connection main circuit: plug-in, without terminals Connection control circuit: Spring-type terminal",1150.8900000000001,"ΤΕΜ",1,"EP",1,"3RA62502CP33","3RA6 Compact εκκινητές"]
["3RA6500-2CB42","SIRIUS Compact load feeder Reversing starter for IO-Link 690 V 24 V DC 1...4 A IP20 Connection main circuit: Spring-type terminal Connection control circuit: Spring-type terminal",1426.36,"ΤΕΜ",1,"EP",1,"3RA65002CB42","3RA6 Compact εκκινητές"]
["3RB2153-4FF2","Overload relay 50...200 A for motor protection Size S6, CLASS 5...30E Contactor mounting/stand-alone installation Main circuit: busbar connection Auxiliary circuit: Spring-type terminal Manual-Automatic-Reset Internal ground fault detection",421.99,"ΤΕΜ",1,"EP",1,"3RB21534FF2","3RB Ηλεκτρονικά θερμικά"]
["3RB2985-2AA1","Memory module analog Basic 1 GF for 3RB22/23 Size S00...S12",143.55000000000001,"ΤΕΜ",1,"EP",1,"3RB29852AA1","3RB Ηλεκτρονικά θερμικά"]
["3RB3046-2XD0","Overload relay 32...115 A Electronic For motor protection Size S3, Class 20E Contactor mounting Main circuit: Screw Auxiliary circuit: Spring-type terminal Manual-Automatic-Reset",294.98,"ΤΕΜ",1,"EP",1,"3RB30462XD0","3RB Ηλεκτρονικά θερμικά"]
["3RB3143-4XX1","Overload relay 32...115 A Electronic For motor protection Size S3, Class 5E...30E Stand-alone installation Main circuit: Straight-through transformer Auxiliary circuit: Spring-type terminal Manual-Automatic-Reset",327.58,"ΤΕΜ",1,"EP",1,"3RB31434XX1","3RB Ηλεκτρονικά θερμικά"]
["3RF2150-1AA04","Semiconductor relay, 1-phase 3RF2 Overall width 22.5 mm, 50 A 48-460 V / 24 V DC screw terminal",66.040000000000006,"ΤΕΜ",1,"EP",1,"3RF21501AA04","3RF Ρελέ ημιαγωγών"]
["3RF2170-1AA22","Semiconductor relay, 1-phase 3RF2 Overall width 22.5 mm, 70 A 24-230 V / 110-230 V AC screw terminal",75.540000000000006,"ΤΕΜ",1,"EP",1,"3RF21701AA22","3RF Ρελέ ημιαγωγών"]
["3RF2320-1BA24","Solid-state contactor 1-phase 3RF2 AC 15 / 12 A / 40 Β°C 48-460 V / 110-230 V AC Instantaneous switching",96.88,"ΤΕΜ",1,"EP",1,"3RF23201BA24","3RF Ρελέ ημιαγωγών"]
["3RF2320-2CA04","Solid-state contactor 1-phase 3RF2 AC 51 / 20 A / 40 Β°C 48-460 V / 24 V DC low noise",109.92,"ΤΕΜ",1,"EP",1,"3RF23202CA04","3RF Ρελέ ημιαγωγών"]
["3RF2340-3AA06","Solid-state contactor 1-phase 3RF2 AC 51 / 40 A / 40 Β°C 48-600 V / 24 V DC Ring cable connection",134.13999999999999,"ΤΕΜ",1,"EP",1,"3RF23403AA06","3RF Ρελέ ημιαγωγών"]
["3RF2410-2AC55","Solid-state contactor 3-phase 3RF2 AC 51 / 10 A / 40 Β°C 48-600 V / 230 V AC 3-phase controlled Spring-type terminal Blocking voltage 1200 V",248.71,"ΤΕΜ",1,"EP",1,"3RF24102AC55","3RF Ρελέ ημιαγωγών"]
["3RF3405-1BB04","Solid-state contactor 3-phase 3RF3 AC 53 / 5.2 A / 40 Β°C 48-480 V / 24 V DC 2-phase controlled Instantaneous switching screw terminal",188.16,"ΤΕΜ",1,"EP",1,"3RF34051BB04","3RF Ρελέ ημιαγωγών"]
["3RG9130-0AA03","AS-Interface coupling module FK-E coupling module 40-fold SKS",36.770000000000003,"ΤΕΜ",1,"EP",40,"3RG91300AA03","3RG AS-Interface module"]
["3RH1921-2EE02","first lateral auxiliary switch 2 NC contacts, encapsulated (solid-state compatible), spring-type terminal, for contactors 3RT1",52.48,"ΤΕΜ",1,"EP",1,"3RH19212EE02","3RH βοηθητικές επαφές για 3RT"]
["3RH2122-2HB40","Coupling contactor relay, 2 NO + 2 NC, 24 V DC, 0.7 ... 1.25* US, Size S00, Spring-type terminal suitable for PLC outputs",45.45,"ΤΕΜ",1,"EP",1,"3RH21222HB40","3RH21 βοηθητικά ρελέ"]
["3RH2131-1AN00","Contactor relay, 3 NO + 1 NC, 220 V AC, 50 Hz, Size S00, screw terminal",43.13,"ΤΕΜ",1,"EP",1,"3RH21311AN00","3RH21 βοηθητικά ρελέ"]
["3RH2131-2AK60","Contactor relay, 3 NO + 1 NC, 110 V AC, 50 Hz, 120 V, 60 Hz, Size S00, Spring-type terminal",39.26,"ΤΕΜ",1,"EP",1,"3RH21312AK60","3RH21 βοηθητικά ρελέ"]
["3RH2140-1AE00","Contactor relay, 4 NO, 60 V AC, 50 / 60 Hz, Size S00, screw terminal",43.13,"ΤΕΜ",1,"EP",1,"3RH21401AE00","3RH21 βοηθητικά ρελέ"]
["3RH2140-1KF40","Coupling contactor relay, 4 NO, 110 V DC, 0.7 ... 1.25* US, with integrated suppressor diode, Size S00, screw terminal suitable for PLC outputs",51.12,"ΤΕΜ",1,"EP",1,"3RH21401KF40","3RH21 βοηθητικά ρελέ"]
["3RH2262-4BG40","Contactor relay, 6 NO + 2 NC, 125 V DC, Size S00, Ring cable lug connection, Captive auxiliary switch,",74.650000000000006,"ΤΕΜ",1,"EP",1,"3RH22624BG40","3RH21 βοηθητικά ρελέ"]
["3RH2344-1CM20-0KA0","Contactor relay, 4 NO + 4 NC, 208 V AC, 50 / 60 Hz, Size S00, screw terminal, 2 NO + 2 NC basic unit / EN Varistor plugged on",79.81,"ΤΕΜ",1,"EP",1,"3RH23441CM200KA0","3RH21 βοηθητικά ρελέ"]
["3RH2431-1BB40","Contactor relay, latched, 3 NO + 1 NC, 24 V DC, Size S00, screw terminal",141.74,"ΤΕΜ",1,"EP",1,"3RH24311BB40","3RH21 βοηθητικά ρελέ"]
["3RH2911-1HA30","Auxiliary switch on the front, 3 NO Current path 1 NO, 1 NO, 1 NO for 3RH and 3RT screw terminal .3/.4, .3/.4, .3/.4",15.93,"ΤΕΜ",1,"EP",1,"3RH29111HA30","3RH βοηθητικές επαφές για 3RT"]
["3RH2911-4HA02","Auxiliary switch on the front, 2 NC Current path 1 NC, 1 NC for 3RH and 3RT Ring cable lug connection .1/.2, .1/.2",11.71,"ΤΕΜ",1,"EP",1,"3RH29114HA02","3RH βοηθητικές επαφές για 3RT"]
["3RK1207-3CE00-2AA2","AS-i SlimLine Compact module SC22.5, IP20, analog, 4AI-RTD Screw terminals 4 x analog input Thermal resistance/resistor Overall width 22.5 mm",508.6,"ΤΕΜ",1,"EP",1,"3RK12073CE002AA2","3RK AS-I module"]
["3RK1315-6KS41-0AA0","SIRIUS motor starter M200D AS-i Communication: AS-Interface DOL starter Basic Mechanical switching AC-3, 0.75KW / 400 V 0.15 A...2.00 A Electronic overload protection Thermistor: THERMOCLICK / PTC without brake contact 2DI AS-i + 2DI / 1DO on device Han Q4/2 - Han Q8/0",1012.6,"ΤΕΜ",1,"EP",1,"3RK13156KS410AA0","3RK ET200 εκκινητές"]
["3RK1315-6KS71-1AA0","SIRIUS motor starter M200D AS-i Communication: AS-Interface Reversing starter Basic Electronic switching AC-3, 0.75KW / 400 V 0.15 A...2.00 A Electronic overload protection Thermistor: THERMOCLICK / PTC without brake contact 2DI AS-i + 2DI / 1DO on device Han Q4/2 - Han Q8/0",1349.5,"ΤΕΜ",1,"EP",1,"3RK13156KS711AA0","3RK ET200 εκκινητές"]
["3RK1395-6KS71-1AD0","SIRIUS motor starter M200D Technology module Reversing starter Electronic switching AC-3, 0.75KW / 400 V 0.15 A...2.00 A Electronic overload protection Thermistor: THERMOCLICK / PTC without brake contact 4 DI / 2 DO Han Q4/2 - Han Q8/0 via communication module 3RK1305* can be used on PROFIBUS or PROFINET",1405.32,"ΤΕΜ",1,"EP",1,"3RK13956KS711AD0","3RK ET200 εκκινητές"]
["3RK1395-6KS71-3AD0","SIRIUS motor starter M200D Technology module Reversing starter Electronic switching AC-3, 0.75KW / 400 V 0.15 A...2.00 A Electronic overload protection Thermistor: THERMOCLICK / PTC without brake contact 4 DI / 2 DO Han Q4/2 - Han Q8/0 with manual on-site operation and key-operated switch via communication module 3RK1305* can be used on PROFIBUS or PROFINET",1505.43,"ΤΕΜ",1,"EP",1,"3RK13956KS713AD0","3RK ET200 εκκινητές"]
["3RK1901-3QA00","AS-Interface accessory Cable clip for cable adapter EC",267.58999999999997,"ΤΕΜ",100,"EP",10,"3RK19013QA00","3RK AS-I module"]
["3RK1902-3NC10","Power line 7/8\" for 24 V connected and unconnected assembled with 2 x 7/8\" angled on both ends 1.5 mm2 pin - socket 5-pole, Length 10 m Clamping range (cable diameter)",265.66000000000003,"ΤΕΜ",1,"EP",1,"3RK19023NC10","3RK AS-I module"]
["3RK1911-0EF31","Motor cable single-sided without brake with thermistor Han Q8 - open on one side angled 6 x 1.5 mm2 Length 5 m",160.16999999999999,"ΤΕΜ",1,"EP",1,"3RK19110EF31","3RK AS-I module"]
["3RK3122-2AC00","SIRIUS, Central unit 3RK3 ASIsafe Extended for modular Safety system 3RK3 2/4 F-DI, 4 DI, 1 F-RO, 1 F-DO,24 V DC Monitoring of ASI slaves Control of 10 safe outputs on AS-Interface bus parameterizable using software Safety ES 45 mm overall width Spring-type terminal Up to SIL3 (IEC 61508) Up to Performance Level E (ISO 13849-1) 2 extension modules connectable",1923.9,"ΤΕΜ",1,"EP",1,"3RK31222AC00","3RK AS-I module"]
["3RK4324-3AR51-0BC0","SIRIUS MCU motor starter Enclosure degree of protection IP54 plastic Communication AS-Interface electromechanically switching Short-circuit protection with circuit breaker DOL starter Brake without Performance class 0.63 A Motor circuit breaker with bi-metal thermal without manual operation Connection power M screw connection Special variant new design A/B slave AS-i SPEC V2.1 Sensor-actuator 1x AS-i 3xDI/DO Supply sensor U-AUX",1551.78,"ΤΕΜ",1,"EP",1,"3RK43243AR510BC0","3RK AS-I module"]
["3RK4340-3KR51-0BA0","SIRIUS MCU motor starter Enclosure degree of protection IP55 plastic Communication without electromechanically switching Short-circuit protection with circuit breaker DOL starter Brake without Performance class 5.00 A Motor circuit breaker with bi-metal thermal Manual operation without Connection power M screw connection Standard product",783.18,"ΤΕΜ",1,"EP",1,"3RK43403KR510BA0","3RK AS-I module"]
["3RM1002-3AA14","Direct starter, 3RM1, 500 V, 0.09 - 0.75 kW, 0.4 - 2 A, 110-230 V AC, screw/spring-type terminals",238.93,"ΤΕΜ",1,"EP",1,"3RM10023AA14","3RM Εκκινητές μέχρι 7Α"]
["3RN2010-1CW30","Thermistor motor protection relay Compact evaluation unit 17.5 mm enclosure Screw terminal 1 NO contact, 1 NC contact US = 24 V-240 V AC/DC Auto RESET suitable for bimetallic switch 2 LEDs (Ready/Tripped) galvanic isolation",92.74,"ΤΕΜ",1,"EP",1,"3RN20101CW30","3RN Ρελέ επιτήρησης θερμίστορ"]
["3RP2505-2RW30-0AX0","Timing relay, Multifunction with painted PCB 2 change-over contacts, 13 functions Positively driven Relay contacts 24...240 V AC/DC at 50/60 Hz AC 7 time ranges (0.05 s...100 h) with LED Spring-type terminal (push-in)",233.66,"ΤΕΜ",1,"EP",1,"3RP25052RW300AX0","3RP Χρονικά "]
["3RQ2000-2AW00","Coupling relay in industrial enclosure 1 changeover contact Wide voltage range 24 V to 240 V AC/DC Spring-type terminals",55.83,"ΤΕΜ",1,"EP",1,"3RQ20002AW00","3RQ Coupling ρελέ"]
["3RQ3038-1AF01","Input coupler Relay coupler, 1 change-over contact hard gold-plated contacts 230 V AC/DC screw terminal Overall width 6.2 mm Thermal current 6A",58.1,"ΤΕΜ",1,"EP",5,"3RQ30381AF01","3RQ Coupling ρελέ"]
["3RR2143-3AW30","Monitoring relay, can be mounted to Contactor 3RT2, Size S2 basic, analog adjustment Apparent current monitoring 8...80 A, 50...60 Hz, 2-phase Supply 24-240 V AC/DC 1 change-over contact Monitoring for Current overshoot and undershoot Phase failure, Cable break with or without fault buffer ON delay 0-60 s Noise pulse suppression 0-30 s Switching hysteresis 6% spring-type connection system",229.1,"ΤΕΜ",1,"EP",1,"3RR21433AW30","3RR Επιτηρητές εντασης"]
["3RS7005-2FE00","Separation amplifier 24 V AC/DC, 3-way separation input: 0-10 V, 0/4-20 mA; output: 0 - 10 V, 0/4 - 20mA Spring-type terminal (push-in)",256.63,"ΤΕΜ",1,"EP",1,"3RS70052FE00","3RS7 Ρελέ μετατροπής σημάτων"]
["3RT1054-6AB36","Power contactor, AC-3 115 A, 55 kW / 400 V AC (50-60 Hz) / DC operation 23-26 V UC Auxiliary contacts 2 NO + 2 NC 3-pole, Size S6 Busbar connections Drive: conventional screw terminal",470.3,"ΤΕΜ",1,"EP",1,"3RT10546AB36","3RT Ρελέ ισχύος"]
["3RT1055-2NF36","Power contactor, AC-3 150 A, 75 kW / 400 V AC (50-60 Hz) / DC operation 96-127 V UC Auxiliary contacts 2 NO + 2 NC 3-pole, Size S6 Busbar connections Drive: electronic with PLC interface 24 V DC Spring-type terminal",624.84,"ΤΕΜ",1,"EP",1,"3RT10552NF36","3RT Ρελέ ισχύος"]
["3RT1055-6SF36","Power contactor, AC-3 150 A, 75 kW / 400 V Coil AC 50/60 Hz and DC 96-127 V x (0.8-1.1) F-PLC input 24 V DC 3-pole size S6 Auxiliary contacts 2 NO + 2 NC Main circuit: Busbar Control and auxiliary circuit: screw terminal",652.17999999999995,"ΤΕΜ",1,"EP",1,"3RT10556SF36","3RT Ρελέ ισχύος"]
["3RT1064-2AV36","Power contactor, AC-3 225 A, 110 kW / 400 V AC (50-60 Hz) / DC operation 380-420 V UC Auxiliary contacts 2 NO + 2 NC 3-pole, Size S10 Busbar connections Drive: conventional Spring-type terminal",940.08,"ΤΕΜ",1,"EP",1,"3RT10642AV36","3RT Ρελέ ισχύος"]
["3RT1065-2NB36","Power contactor, AC-3 265 A, 132 kW / 400 V AC (50-60 Hz) / DC operation 21-27 UC, 3 V Auxiliary contacts 2 NO + 2 NC 3-pole, Size S10 Busbar connections Drive: electronic with PLC interface 24 V DC Spring-type terminal",1262.29,"ΤΕΜ",1,"EP",1,"3RT10652NB36","3RT Ρελέ ισχύος"]
["3RT1075-2AF36","Power contactor, AC-3 400 A, 200 kW / 400 V AC (50-60 Hz) / DC operation 110-127 V UC Auxiliary contacts 2 NO + 2 NC 3-pole, Size S12 Busbar connections Drive: conventional Spring-type terminal",1624.66,"ΤΕΜ",1,"EP",1,"3RT10752AF36","3RT Ρελέ ισχύος"]
["3RT1076-2AF36","Power contactor, AC-3 500 A, 250 kW / 400 V AC (50-60 Hz) / DC 110-127 V UC Auxiliary contacts 2 NO + 2 NC 3-pole, size S12 Busbar connections Operating mechanism: conventional Spring-type terminals",2047.88,"ΤΕΜ",1,"EP",1,"3RT10762AF36","3RT Ρελέ ισχύος"]
["3RT1266-6AT36","Vacuum contactor, AC-3 300 A, 160 kW / 400 V AC (50-60 Hz) / DC operation 575-600 V UC Auxiliary contacts 2 NO + 2 NC 3-pole, Size S10 Busbar connections Drive: conventional",2324.7800000000002,"ΤΕΜ",1,"EP",1,"3RT12666AT36","3RT Ρελέ ισχύος"]
["3RT1456-2AP36","Contactor, AC-1, 275 A/690 V/40 Β°C, S6, 3-pole, 220-240 V AC/DC, with varistor, 2 NO+2 NC, Connection rail/ Spring-type terminal",512.57000000000005,"ΤΕΜ",1,"EP",1,"3RT14562AP36","3RT Ρελέ ισχύος"]
["3RT1467-6AF36","Contactor, AC-1, 500 A/690 V/40 Β°C, S10, 3-pole, 110-127 V AC/DC, with varistor, 2 NO+2 NC, Connection rail/ screw terminal",1654.1,"ΤΕΜ",1,"EP",1,"3RT14676AF36","3RT Ρελέ ισχύος"]
["3RT1476-6AS36","Contactor, AC-1, 690 A/690 V/40 Β°C, S12, 3-pole, 500-550 V AC/DC, with varistor, 2 NO+2 NC, Connection rail/ screw terminal",2072.59,"ΤΕΜ",1,"EP",1,"3RT14766AS36","3RT Ρελέ ισχύος"]
["3RT1934-6A","Replacement contact pieces for contactor Size S2, 3-pole, AC-3, 15 kW, 3 NO, main contacts, Consists of 3 movable and 6 fixed contacts with mounting parts !!! Phased-out product !!! Successor is SIRIUS 3RT2",127.05,"ΤΕΜ",1,"EP",1,"3RT19346A","3RT Ρελέ ισχύος"]
["3RT1955-5XJ42","Changeover operating mechanism for 3RT105.-.X..-0LA2 or 3RT145.-.X..-0LA2 72 V DC x(0.7-1.25) Supply voltage PLC input 24...110 V DC Spring-type terminal",384.81,"ΤΕΜ",1,"EP",1,"3RT19555XJ42","3RT Ρελέ ισχύος"]
["3RT1966-5AB31","Changeover operating mechanism for vacuum contactor 3RT126 AC (50...60 Hz) / DC operation, 23 ... 26 V Operating mechanism: Standard,economy circuit Screw terminal",173.05,"ΤΕΜ",1,"EP",1,"3RT19665AB31","3RT Ρελέ ισχύος"]
["3RT1975-5NP32","Changeover operating mechanism for contactors 3RT107, 3RT127, 3RT147, AC (50...60 Hz) / DC operation, 200 ... 277 V Operating mechanism: electronic with PLC interface 24 V DC Spring-type terminal",658.05,"ΤΕΜ",1,"EP",1,"3RT19755NP32","3RT Ρελέ ισχύος"]
["3RT1983-4AA1","Phase barrier for 3RT1481, 3RT1482 and 3RT1483 (4 units)",15.73,"ΤΕΜ",1,"EP",1,"3RT19834AA1","3RT Ρελέ ισχύος"]
["3RT2015-1FB42-1AA0","Power contactor, AC-3 7 A, 3 kW / 400 V 1 NC, 24 V DC with diode integrated, 3-pole, Size S00, screw terminal Upright mounting position",51.09,"ΤΕΜ",1,"EP",1,"3RT20151FB421AA0","3RT Ρελέ ισχύος"]
["3RT2015-2MB41-0KT0","power contactor, AC-3 7 A, 3 kW / 400 V 1 NO, 24 V DC 0.85-1.85* US, 3-pole, size S00, spring-type terminal not expandable with auxiliary switch",40.99,"ΤΕΜ",1,"EP",1,"3RT20152MB410KT0","3RT Ρελέ ισχύος"]
["3RT2016-1AK61-1AA0","Power contactor, AC-3 9 A, 4 kW / 400 V 1 NO, 110 V AC/50 Hz 120 V/60 Hz 3-pole, Size S00 screw terminal upright mounting position",39.56,"ΤΕΜ",1,"EP",1,"3RT20161AK611AA0","3RT Ρελέ ισχύος"]
["3RT2016-1BE42","Power contactor, AC-3 9 A, 4 kW / 400 V 1 NC, 60 V DC, 3-pole, Size S00 screw terminal",47.71,"ΤΕΜ",1,"EP",1,"3RT20161BE42","3RT Ρελέ ισχύος"]
["3RT2016-1JB41","power contactor, AC-3 9 A, 4 kW / 400 V 1 NO, 24 V DC 0.7-1.25* US, with diode integrated, 3-pole, size S00, screw terminal suitable for PLC outputs not expandable with auxiliary switch",49.25,"ΤΕΜ",1,"EP",1,"3RT20161JB41","3RT Ρελέ ισχύος"]
["3RT2016-2BW41","Power contactor, AC-3 9 A, 4 kW / 400 V 1 NO, 48 V DC, 3-pole, Size S00 Spring-type terminal",42.15,"ΤΕΜ",1,"EP",1,"3RT20162BW41","3RT Ρελέ ισχύος"]
["3RT2016-4AN62","Power contactor, AC-3 9 A, 4 kW / 400 V 1 NC, 200 V AC, 50 Hz 200-220 V, 60 Hz, 3-pole, Size S00, ring cable lug connection",39.799999999999997,"ΤΕΜ",1,"EP",1,"3RT20164AN62","3RT Ρελέ ισχύος"]
["3RT2017-1BW41","power contactor, AC-3 12 A, 5.5 kW / 400 V 1 NO, 48 V DC 3-pole, Size S00 screw terminal",48.63,"ΤΕΜ",1,"EP",1,"3RT20171BW41","3RT Ρελέ ισχύος"]
["3RT2017-2HB41","power contactor, AC-3 12 A, 5.5 kW / 400 V 1 NO, 24 V DC 0.7-1.25*US 3-pole, size S00 spring-type terminal suitable for PLC outputs not expandable with auxiliary switch",48.63,"ΤΕΜ",1,"EP",1,"3RT20172HB41","3RT Ρελέ ισχύος"]
["3RT2017-2WB42","power contactor, AC-3 12 A, 5.5 kW / 400 V 1 NC, 24 V DC 0.85-1.85* US, with varistor plugged on, 3-pole size S00, spring-type terminal not expandable with auxiliary switch",54.69,"ΤΕΜ",1,"EP",1,"3RT20172WB42","3RT Ρελέ ισχύος"]
["3RT2018-1AP61-0UA0","Contactor, 5 HP, 460 / 575 V, 1 NO, 220 V AC, 50 Hz, 240 V, 60 Hz, 3-pole, Size S00 screw terminal NEMA VERSION",62.85,"ΤΕΜ",1,"EP",1,"3RT20181AP610UA0","3RT Ρελέ ισχύος"]
["3RT2018-2BB42","Power contactor, AC-3 16 A, 7.5 kW / 400 V 1 NC, 24 V DC 3-pole, Size S00 Spring-type terminals",87.52,"ΤΕΜ",1,"EP",1,"3RT20182BB42","3RT Ρελέ ισχύος"]
["3RT2018-2LB42-0LA0","Traction contactor, AC-3 16 A, 7.5 kW / 400 V 24 V DC, 0.7-1.25* Us with integrated varistor 3-pole, Size S00 Spring-type terminal",99.25,"ΤΕΜ",1,"EP",1,"3RT20182LB420LA0","3RT Ρελέ ισχύος"]
["3RT2023-1NB30","power contactor, AC-3 9 A, 4 kW / 400 V 1 NO + 1 NC, AC (50 / 60 Hz) DC operation 21-28 V AC/DC, 3-pole Size S0, screw terminal",101.56,"ΤΕΜ",1,"EP",1,"3RT20231NB30","3RT Ρελέ ισχύος"]
["3RT2023-2DB40","Power contactor, AC-3 9 A, 4 kW / 400 V 1 NO + 1 NC, 24 V DC with varistor 3-pole, Size S0, spring-type terminal",102.37,"ΤΕΜ",1,"EP",1,"3RT20232DB40","3RT Ρελέ ισχύος"]
["3RT2024-2AL20","power contactor, AC-3 12 A, 5.5 kW / 400 V 1 NO + 1 NC, 230 V AC 50 / 60 Hz, 3-pole Size S0, Spring-type terminal",45.48,"ΤΕΜ",1,"EP",1,"3RT20242AL20","3RT Ρελέ ισχύος"]
["3RT2025-1AB00","power contactor, AC-3 17 A, 7.5 kW / 400 V 1 NO + 1 NC, 24 V AC, 50 Hz, 3-pole, Size S0 screw terminal",61.13,"ΤΕΜ",1,"EP",1,"3RT20251AB00","3RT Ρελέ ισχύος"]
["3RT2025-1AV00","power contactor, AC-3 17 A, 7.5 kW / 400 V 1 NO + 1 NC, 400 V AC, 50 Hz 3-pole, Size S0 screw terminal",64.599999999999994,"ΤΕΜ",1,"EP",1,"3RT20251AV00","3RT Ρελέ ισχύος"]
["3RT2025-2BB44-3MA0","Power contactor, AC-3 17 A, 7.5 kW / 400 V 2 NO + 2 NC, 24 V DC, 3-pole, Size S0 Spring type terminal Captive auxiliary switch",126.68,"ΤΕΜ",1,"EP",1,"3RT20252BB443MA0","3RT Ρελέ ισχύος"]
["3RT2026-1AD20","Power contactor, AC-3 25 A, 11 kW / 400 V 42 V AC, 50/60 Hz 3-pole, Size S0 screw terminal",84.73,"ΤΕΜ",1,"EP",1,"3RT20261AD20","3RT Ρελέ ισχύος"]
["3RT2026-2AF04","power contactor, AC-3 25 A, 11 kW / 400 V 2 NO + 2 NC, 110 V AC, 50 Hz, 3-pole, Size S0 Spring-type terminal Removable auxiliary switch",97.39,"ΤΕΜ",1,"EP",1,"3RT20262AF04","3RT Ρελέ ισχύος"]
["3RT2027-1AH20","Power contactor, AC-3 32 A, 15 kW / 400 V 1 NO + 1 NC, 48 V AC 50/60 Hz, 3-pole size S0 screw terminals",120.35,"ΤΕΜ",1,"EP",1,"3RT20271AH20","3RT Ρελέ ισχύος"]
["3RT2027-1DB40","Contactor, AC-3, 15 kW / 400 V, 1 NO + 1 NC, 24 V DC, with varistor 3-pole, Size S0, screw terminal",195.08,"ΤΕΜ",1,"EP",1,"3RT20271DB40","3RT Ρελέ ισχύος"]
["3RT2027-2KB40","power contactor, AC-3 32 A, 15 kW / 400 V 1 NO + 1 NC, 24 V DC with integrated varistor 3-pole, size S0 spring-type terminal suitable for PLC outputs not expandable with auxiliary switch",182.49,"ΤΕΜ",1,"EP",1,"3RT20272KB40","3RT Ρελέ ισχύος"]
["3RT2028-1BF40","Power contactor, AC-3 38 A, 18.5 kW / 400 V 1 NO + 1 NC, 110 V DC 3-pole, size S0 screw terminals",186.88,"ΤΕΜ",1,"EP",1,"3RT20281BF40","3RT Ρελέ ισχύος"]
["3RT2028-2AC20-1AA0","Power contactor, AC-3 38 A, 18.5 kW / 400 V 1 NO + 1 NC, 24 V AC 50/60 Hz, 3-pole Size S0, Spring-type terminals Upright mounting position",137.86000000000001,"ΤΕΜ",1,"EP",1,"3RT20282AC201AA0","3RT Ρελέ ισχύος"]
["3RT2035-1AR60","power contactor, AC-3 40 A, 18.5 kW / 400 V 1 NO + 1 NC, 400 V AC AC (50-60 Hz) / DC operation 3-pole, Size S2, screw terminal",153.61000000000001,"ΤΕΜ",1,"EP",1,"3RT20351AR60","3RT Ρελέ ισχύος"]
["3RT2035-3AB00-1AA0","power contactor, AC-3 40 A, 18.5 kW / 400 V 1 NO + 1 NC, 24 V AC, 50 Hz 3-pole, Size S2 Spring-type terminal upright mounting position",171.44,"ΤΕΜ",1,"EP",1,"3RT20353AB001AA0","3RT Ρελέ ισχύος"]
["3RT2036-1AP60-0UA0","Contactor, 25 hp, 460 / 575 V 220 V AC, 50 Hz / 240 V, 60 Hz, 3-pole, Size S2 screw terminal NEMA size 2",184.06,"ΤΕΜ",1,"EP",1,"3RT20361AP600UA0","3RT Ρελέ ισχύος"]
["3RT2036-3AC20","power contactor, AC-3 50 A, 22 kW / 400 V 1 NO + 1 NC, 24 V AC, 50 / 60 Hz, 3-pole, Size S2, Spring-type terminal",179.22,"ΤΕΜ",1,"EP",1,"3RT20363AC20","3RT Ρελέ ισχύος"]
["3RT2036-3SB30","contactor, AC-3, 50 A/400 V/60 Β°C S2, 3-pole, 21-33 V AC/DC, F-PLC-IN, with varistor, 1 NC, spring-loaded terminal",341.09,"ΤΕΜ",1,"EP",1,"3RT20363SB30","3RT Ρελέ ισχύος"]
["3RT2037-3AC20","Power contactor, AC-3 65 A, 30 kW / 400 V 1 NO + 1 NC, 24 V AC, 50/60 Hz 3-pole, size S2 Spring-type terminals",249.45,"ΤΕΜ",1,"EP",1,"3RT20373AC20","3RT Ρελέ ισχύος"]
["3RT2038-1KB40","Power contactor, AC-3 80 A, 37 kW / 400 V 1 NO + 1 NC, 24 V DC with varistor 3-pole, Size S2 Screw terminal Suitable for 2 A PLC outputs",445.85,"ΤΕΜ",1,"EP",1,"3RT20381KB40","3RT Ρελέ ισχύος"]
["3RT2038-3XF40-0LA2","Traction contactor, AC-3 80 A, 37 kW / 400 V 1 NO + 1 NC 110 V DC, 0.7-1.25* Us with varistor 3-pole, size S2 Spring-type terminals",616.85,"ΤΕΜ",1,"EP",1,"3RT20383XF400LA2","3RT Ρελέ ισχύος"]
["3RT2045-1AH20","power contactor, AC-3 80 A, 37 kW / 400 V 1 NO + 1 NC, 48 V AC, 50/60 Hz 3-pole, 3 NO, Size S3 screw terminal",309.22000000000003,"ΤΕΜ",1,"EP",1,"3RT20451AH20","3RT Ρελέ ισχύος"]
["3RT2046-1AK64-3MA0","power contactor, AC-3 95 A, 45 kW / 400 V 2 NO + 2 NC, 110 V AC, 50 Hz Hz 120 V/60 Hz 3-pole, 3 NO, Size S3 screw terminal",397.68,"ΤΕΜ",1,"EP",1,"3RT20461AK643MA0","3RT Ρελέ ισχύος"]
["3RT2046-3AN20","power contactor, AC-3 95 A, 45 kW / 400 V 1 NO + 1 NC, 230 V AC, 50/60 Hz 3-pole, 3 NO, Size S3 Spring-type terminal",375.36,"ΤΕΜ",1,"EP",1,"3RT20463AN20","3RT Ρελέ ισχύος"]
["3RT2047-3CF04-3MA0","Contactor, AC-3, 55 kW/400 V 2 NO+2 NC, 110 V AC 50 Hz 3-pole, 3 NO, Size S3 Spring-type terminal Inserted varistor Captive auxiliary switch",467.81,"ΤΕΜ",1,"EP",1,"3RT20473CF043MA0","3RT Ρελέ ισχύος"]
["3RT2316-1BM40","Contactor, AC-1, 18 A/400 V/40 Β°C, S00, 4-pole, 220 V DC, screw terminal",47.34,"ΤΕΜ",1,"EP",1,"3RT23161BM40","3RT Ρελέ ισχύος"]
["3RT2317-2BM40","Contactor, AC-1, 22 A/400 V/40 Β°C, S00, 4-pole, 220 V DC, Spring-type terminal",52.16,"ΤΕΜ",1,"EP",1,"3RT23172BM40","3RT Ρελέ ισχύος"]
["3RT2327-1BA40","Contactor, AC-1, 50 A/400 V/40 Β°C, S0, 4-pole, 12 V DC, 1 NO+1 NC, screw terminal",211.14,"ΤΕΜ",1,"EP",1,"3RT23271BA40","3RT Ρελέ ισχύος"]
["3RT2346-1AP00","Contactor, AC-1, 140 A/400 V/40 Β°C, S3, 4-pole, 230 V AC/50 Hz, 1 NO+1 NC, screw terminal",447.12,"ΤΕΜ",1,"EP",1,"3RT23461AP00","3RT Ρελέ ισχύος"]
["3RT2348-1NP30","Contactor, AC-1, 160 A/400 V/40 Β°C, S3, 4-pole, 175-280 V AC/DC, 1 NO+1 NC, screw terminal",615.20000000000005,"ΤΕΜ",1,"EP",1,"3RT23481NP30","3RT Ρελέ ισχύος"]
["3RT2516-2AB00","Power contactor, AC-3 9 A, 4 kW / 400 V 2 NO + 2 NC 24 V AC, 50/60 Hz 4-pole Size S00 Spring-type terminal",39.58,"ΤΕΜ",1,"EP",1,"3RT25162AB00","3RT Ρελέ ισχύος"]
["3RT2526-1BJ80","Power contactor, AC-3 25 A, 11 kW / 400 V 2 NO + 2 NC 72 V DC 4-pole size S0 screw terminals 1 NO + 1 NC integrated",174.71,"ΤΕΜ",1,"EP",1,"3RT25261BJ80","3RT Ρελέ ισχύος"]
["3RT2625-1AP05","Capacitor contactor, AC-6b 16.7 kVAr, / 400 V 1 NO + 2 NC, 230 V AC, 50 Hz 3-pole, Size S0 screw terminal",119.23,"ΤΕΜ",1,"EP",1,"3RT26251AP05","3RT Ρελέ ισχύος"]
["3RT2628-1AP65","Capacitor contactor, AC-6b 33 kVAr, / 400 V 1 NO + 2 NC, 220 V AC, 50 Hz 240 V, 60 Hz 3-pole, Size S0 screw terminal",200.27,"ΤΕΜ",1,"EP",1,"3RT26281AP65","3RT Ρελέ ισχύος"]
["3RT2636-1NF35","Capacitor contactor, AC-6b 50 kVAr, / 400 V 2 NC, 50-60 Hz AC / 83-155 V DC 3-pole, Size S2 screw terminal",554.67999999999995,"ΤΕΜ",1,"EP",1,"3RT26361NF35","3RT Ρελέ ισχύος"]
["3RT2916-1JK00","Surge suppressor, Varistor with LED, 48 ... 127 V AC, 24 ... 70 V DC, for contactor relays and motor contactors Size S00",14.46,"ΤΕΜ",1,"EP",1,"3RT29161JK00","3RT Ρελέ ισχύος"]
["3RT2926-1ES00","Surge suppressor, diode combination, 30 ... 250 V DC, for motor contactors Size S0,",17.5,"ΤΕΜ",1,"EP",1,"3RT29261ES00","3RT Ρελέ ισχύος"]
["3RT2926-5AT61","Magnet coil for contactors 18.5 kW 600 V AC, 60Hz, for motor contactors, Size S0, Screw terminal",24.78,"ΤΕΜ",1,"EP",1,"3RT29265AT61","3RT Ρελέ ισχύος"]
["3RT2944-5AH21","Magnet coil for contactor S3, 48 V AC, 50 / 60 Hz,",45.04,"ΤΕΜ",1,"EP",1,"3RT29445AH21","3RT Ρελέ ισχύος"]
["3RU2116-0KB1","Overload relay 0.90...1.25 A Thermal For motor protection Size S00, Class 10 Stand-alone installation Main circuit: Screw Auxiliary circuit: Screw Manual-Automatic-Reset",75.31,"ΤΕΜ",1,"EP",1,"3RU21160KB1","3RU Θερμικό υπερφόρτωσης"]
["3RU2116-1HJ0","Overload relay 5.5...8.0 A Thermal For motor protection Size S00, Class 10 Contactor mounting Main circuit: Ring cable lug Auxiliary circuit: ring cable lug Manual-Automatic-Reset",59.04,"ΤΕΜ",1,"EP",1,"3RU21161HJ0","3RU Θερμικό υπερφόρτωσης"]
["3RU2126-4CB1","Overload relay 17...22 A Thermal For motor protection Size S0, Class 10 Stand-alone installation Main circuit: Screw Auxiliary circuit: Screw Manual-Automatic-Reset",73.47,"ΤΕΜ",1,"EP",1,"3RU21264CB1","3RU Θερμικό υπερφόρτωσης"]
["3RU2136-4FD1","Overload relay 28...40 A Thermal For motor protection Size S2, Class 10 Stand-alone installation Main circuit: Screw Auxiliary circuit: spring-type terminal Manual-Automatic-Reset",127.43,"ΤΕΜ",1,"EP",1,"3RU21364FD1","3RU Θερμικό υπερφόρτωσης"]
["3RU2146-4MD0","Overload relay 80...100 A Thermal For motor protection Size S3, Class 10 Contactor mounting Main circuit: Screw Auxiliary circuit: spring-type terminal Manual-Automatic-Reset",211.6,"ΤΕΜ",1,"EP",1,"3RU21464MD0","3RU Θερμικό υπερφόρτωσης"]
["3RV1903-5E","Indicator light with glow lamp 380...415 V AC/DC with colored lenses: red,green,clear for enclosure 3RV19 Size S00...S2",13.58,"ΤΕΜ",1,"EP",1,"3RV19035E","3RV Θερμομαγνητικοί διακόπτες ισχύος"]
["3RV1917-7B","Mounting rail 45 mm for mounting on 3-phase busbars 3RV2917-1/4",2.11,"ΤΕΜ",1,"EP",1,"3RV19177B","3RV Θερμομαγνητικοί διακόπτες ισχύος"]
["3RV2011-1BA40","Circuit breaker size S00 for motor protection, CLASS 10 A-release 1.4...2 A N-release 26 A ring cable lug connection Standard switching capacity",66.150000000000006,"ΤΕΜ",1,"EP",1,"3RV20111BA40","3RV Θερμομαγνητικοί διακόπτες ισχύος"]
["3RV2011-1EA40","Circuit breaker size S00 for motor protection, CLASS 10 A-release 2.8...4 A N release 52 A ring cable lug connection Standard switching capacity",66.150000000000006,"ΤΕΜ",1,"EP",1,"3RV20111EA40","3RV Θερμομαγνητικοί διακόπτες ισχύος"]
["3RV2021-0KA10","Circuit breaker size S0 for motor protection, CLASS 10 A-release 0.9...1.25 A N-release 16 A screw terminal Standard switching capacity",66.94,"ΤΕΜ",1,"EP",1,"3RV20210KA10","3RV Θερμομαγνητικοί διακόπτες ισχύος"]
["3RV2021-1KA25","Circuit breaker size S0 for motor protection, CLASS 10 A-release 9...12 A N-release 163 A Spring-type terminal Standard switching capacity with transverse auxiliary switches 1 NO+1 NC",91.41,"ΤΕΜ",1,"EP",1,"3RV20211KA25","3RV Θερμομαγνητικοί διακόπτες ισχύος"]
["3RV2031-4EB10-0BA0","Special type Circuit breaker size S2 for motor protection, Class 20 A-release 22...32 A N-release 416 A screw terminal Standard switching capacity Ambient temperature -50 Β°C 250 switching cycles",277.06,"ΤΕΜ",1,"EP",1,"3RV20314EB100BA0","3RV Θερμομαγνητικοί διακόπτες ισχύος"]
["3RV2031-4XB15","Circuit breaker size S2 for motor protection class 20 A-release 49...59 A N-release 845 A screw terminal Standard switching capacity with transverse auxiliary switch 1 NO+1 NC",320.12,"ΤΕΜ",1,"EP",1,"3RV20314XB15","3RV Θερμομαγνητικοί διακόπτες ισχύος"]
["3RV2111-1HA10","Circuit breaker size S00 for motor protection, CLASS 10 with overload relay function A-release 5.5...8 A N-release 104 A screw terminal Standard switching capacity",121.14,"ΤΕΜ",1,"EP",1,"3RV21111HA10","3RV Θερμομαγνητικοί διακόπτες ισχύος"]
["3RV2311-0GC20","Circuit breaker size S00 for starter combination Rated current 0.63 A N-release 8.2 A Spring-type terminal Standard switching capacity",57.53,"ΤΕΜ",1,"EP",1,"3RV23110GC20","3RV Θερμομαγνητικοί διακόπτες ισχύος"]
["3RV2321-4BC20","Circuit breaker size S0 for starter combination Rated current 20 A N-release 260 A Spring-type terminal Standard switching capacity",77.13,"ΤΕΜ",1,"EP",1,"3RV23214BC20","3RV Θερμομαγνητικοί διακόπτες ισχύος"]
["3RV2341-4RC10","Circuit breaker size S3 for starter combination Rated current 84 A N-release 1170 A screw terminal Standard switching capacity",297.3,"ΤΕΜ",1,"EP",1,"3RV23414RC10","3RV Θερμομαγνητικοί διακόπτες ισχύος"]
["3RV2411-1AA20-0DA0","circuit breaker size S00 for transformer protection without phase failure protection A-release 1.1...1.6 A short-circuit release 33 A spring-loaded terminal standard switching capacity",102.47,"ΤΕΜ",1,"EP",1,"3RV24111AA200DA0","3RV Θερμομαγνητικοί διακόπτες ισχύος"]
["3RV2431-4VA10","Circuit breaker size S2 for transformer protection A-release 35...45 A N-release 922 A screw terminal Standard switching capacity",252.28,"ΤΕΜ",1,"EP",1,"3RV24314VA10","3RV Θερμομαγνητικοί διακόπτες ισχύος"]
["3RV2742-5FD10","Circuit breaker size S3 for system protection with approval circuit breaker UL 489, CSA C22.2 No.5-02 A-release 35 A N-release 455 A screw terminal",370.27,"ΤΕΜ",1,"EP",1,"3RV27425FD10","3RV Θερμομαγνητικοί διακόπτες ισχύος"]
["3RV2917-4A","3-phase busbar including extension connector for 2 circuit breakers Size S00 and S0",15.08,"ΤΕΜ",1,"EP",1,"3RV29174A","3RV Θερμομαγνητικοί διακόπτες ισχύος"]
["3RV2921-2M","signaling switch for circuit breaker 3RV2 with spring-type terminal",22.41,"ΤΕΜ",1,"EP",1,"3RV29212M","3RV Θερμομαγνητικοί διακόπτες ισχύος"]
["3RW3017-1BB14","SIRIUS soft starter S00 12.5 A, 5.5 kW/400 V, 40 Β°C 200-480 V AC, 110-230 V AC/DC Screw terminals",298.86,"ΤΕΜ",1,"EP",1,"3RW30171BB14","3RW Ομαλοί εκκινητές"]
["3RW4028-1BB04","SIRIUS soft starter S0 38 A, 18.5 kW/400 V, 40 Β°C 200-480 V AC, 24 V AC/DC Screw terminals",898.9,"ΤΕΜ",1,"EP",1,"3RW40281BB04","3RW Ομαλοί εκκινητές"]
["3RW4038-2TB05","SIRIUS soft starter S2 72 A, 45 kW/500 V, 40 Β°C 400-600 V AC, 24 V AC/DC spring-type terminals Thermistor motor protection",1847.48,"ΤΕΜ",1,"EP",1,"3RW40382TB05","3RW Ομαλοί εκκινητές"]
["3RW4755-6SC44","Control unit 230 V for 3RW4455 with screw terminals",1379.84,"ΤΕΜ",1,"EP",1,"3RW47556SC44","3RW Ομαλοί εκκινητές"]
["3RW4766-0WC50","TSE PCB 690 V for 3RW44, Size 6 for 3RW4457, 3RW4458",515.28,"ΤΕΜ",1,"EP",1,"3RW47660WC50","3RW Ομαλοί εκκινητές"]
["3RW5055-6AB05","SIRIUS soft starter 200-600 V 143 A, 24 V AC/DC Screw terminals Analog output",2787.05,"ΤΕΜ",1,"EP",1,"3RW50556AB05","3RW Ομαλοί εκκινητές"]
["3RW5074-6TB04","SIRIUS soft starter 200-480 V 315 A, 24 V AC/DC Screw terminals Thermistor input",3786.44,"ΤΕΜ",1,"EP",1,"3RW50746TB04","3RW Ομαλοί εκκινητές"]
["3RW5214-1TC15","SIRIUS soft starter 200-600 V 18 A, 110-250 V AC Screw terminals Thermistor input",1238.69,"ΤΕΜ",1,"EP",1,"3RW52141TC15","3RW Ομαλοί εκκινητές"]
["3RW5217-1AC14","SIRIUS soft starter 200-480 V 38 A, 110-250 V AC Screw terminals Analog output",1534.28,"ΤΕΜ",1,"EP",1,"3RW52171AC14","3RW Ομαλοί εκκινητές"]
["3RW5225-3AC04","SIRIUS soft starter 200-480 V 63 A, 24 V AC/DC spring-type terminals Analog output",1942.49,"ΤΕΜ",1,"EP",1,"3RW52253AC04","3RW Ομαλοί εκκινητές"]
["3RW5236-6AC05","SIRIUS soft starter 200-600 V 171 A, 24 V AC/DC Screw terminals Analog output",4067.96,"ΤΕΜ",1,"EP",1,"3RW52366AC05","3RW Ομαλοί εκκινητές"]
["3RW5247-2TC04","SIRIUS soft starter 200-480 V 470 A, 24 V AC/DC spring-type terminals Thermistor input",8178.16,"ΤΕΜ",1,"EP",1,"3RW52472TC04","3RW Ομαλοί εκκινητές"]
["3RW5248-2TC14","SIRIUS soft starter 200-480 V 570 A, 110-250 V AC spring-type terminals Thermistor input",9177.5499999999993,"ΤΕΜ",1,"EP",1,"3RW52482TC14","3RW Ομαλοί εκκινητές"]
["3RW5516-1HA05","SIRIUS soft starter 200-600 V 32 A, 24 V AC/DC Screw terminals",2350.69,"ΤΕΜ",1,"EP",1,"3RW55161HA05","3RW Ομαλοί εκκινητές"]
["3RW5534-2HA04","SIRIUS soft starter 200-480 V 113 A, 24 V AC/DC spring-type terminals",4067.96,"ΤΕΜ",1,"EP",1,"3RW55342HA04","3RW Ομαλοί εκκινητές"]
["3RW5544-2HF04","SIRIUS soft starter 200-480 V 250 A, 24 V AC/DC spring-type terminals Fail-safe",8445.6,"ΤΕΜ",1,"EP",1,"3RW55442HF04","3RW Ομαλοί εκκινητές"]
["3RW5553-2HA16","SIRIUS soft starter 200-690 V 720 A, 110-250 V AC Spring-type terminals",19143.36,"ΤΕΜ",1,"EP",1,"3RW55532HA16","3RW Ομαλοί εκκινητές"]
["3RW5558-2HA04","SIRIUS soft starter 200-480 V 1280 A, 24 V AC/DC Spring-type terminals",25196.04,"ΤΕΜ",1,"EP",1,"3RW55582HA04","3RW Ομαλοί εκκινητές"]
["3RW5950-0GL30","Spring flap for 3RW55/52 with cutout for HMI module High-Feature",27.91,"ΤΕΜ",1,"EP",1,"3RW59500GL30","3RW Ομαλοί εκκινητές"]
["3RW5955-0SW04","Power semiconductor module 480 V, for 3RW55, 840 A",2866.43,"ΤΕΜ",1,"EP",1,"3RW59550SW04","3RW Ομαλοί εκκινητές"]
["3SB2000-2AG01","Selector switch, 16 mm, round, plastic, white, 2 switch positions O-I, latching, actuating angle 62 degree",19.55,"ΤΕΜ",1,"EP",1,"3SB20002AG01","3SB μπουτόν 16mm"]
["3SB2001-6BH06","Indicator light, 16 mm, round, plastic, clear, with concentric rings",6.14,"ΤΕΜ",1,"EP",1,"3SB20016BH06","3SB μπουτόν 16mm"]
["3SB2455-1J","Contact block and lampholder 1 NO, 1 NC, Wedge base W2 x 4.6 d, soldering pin connection",29.56,"ΤΕΜ",1,"EP",1,"3SB24551J","3SB μπουτόν 16mm"]
["3SB2901-2EW","Adhesive labeling plate, on label holder, Label size 9.5 x 18.5 mm, silver-colored, black font, with inscription: Fault",117.45,"ΤΕΜ",100,"EP",10,"3SB29012EW","3SB μπουτόν 16mm"]
["3SB2901-5QL","Insert cap for pushbutton and illuminated pushbutton raised, clear with black font, with graphic symbol: automatic sequence",150.02000000000001,"ΤΕΜ",100,"EP",10,"3SB29015QL","3SB μπουτόν 16mm"]
["3SB2910-0AH","pushbutton, clear, flat, for pushbutton and illuminated pushbutton",61.78,"ΤΕΜ",100,"EP",10,"3SB29100AH","3SB μπουτόν 16mm"]
["3SE2283-6GA53","Hinge switch Molded-plastic enclosure with aluminum hinge 3xNC, Slow-action contacts for 40 mm profiles Supplied with additional hinge and fixing material Cable entry 2 x M20 x 1.5 Actuating angle 8Β°",244.8,"ΤΕΜ",1,"EP",1,"3SE22836GA53","3SE Τερματικοί διακόπτες"]
["3SE5000-0AE04","Actuator head for position switch 3SE51 Roller lever Stainless steel lever and Stainless steel roller 22 mm",37.090000000000003,"ΤΕΜ",1,"EP",1,"3SE50000AE04","3SE Τερματικοί διακόπτες"]
["3SE5000-0AF03-1AJ0","Actuator head for position switch 3SE51 Angular roller lever,Stainless steel lever Stainless steel lever with plastic roller 22 mm functional at -40 Β°C",31.14,"ΤΕΜ",1,"EP",1,"3SE50000AF031AJ0","3SE Τερματικοί διακόπτες"]
["3SE5112-0CH62-1AJ0","Position switch Metal enclosure 40 mm according to EN 50041 Device connection 1x (M20 x 1.5) 1 NO/1 NC quick action contacts Rotary actuator right/left adjustable with adjustable-length stainless steel lever 100 mm long and with positive fit (grid hole) and plastic roller 19 mm functional at -40 Β°C Shock and vibration test according to EN 61373, Category 1B",92.93,"ΤΕΜ",1,"EP",1,"3SE51120CH621AJ0","3SE Τερματικοί διακόπτες"]
["3SE5112-0LE01","Position switch Metal enclosure 40 mm according to EN 50041 Device connection 1x (M20 x 1.5) 1 NO/2 NC quick action contacts Roller lever, Metal lever and plastic roller 22 mm",59.7,"ΤΕΜ",1,"EP",1,"3SE51120LE01","3SE Τερματικοί διακόπτες"]
["3SE5122-0BA00-1CA0","Basic switch with increased corrosion protection for position switch Metal enclosure 56 mm wide 1 NO/1 NC slow-action contacts without actuator head",42.28,"ΤΕΜ",1,"EP",1,"3SE51220BA001CA0","3SE Τερματικοί διακόπτες"]
["3SE5122-0QV10-1AA7","Safety position switch with separate actuator Metal enclosure, 56 mm Device connection 3x (M20x 1.5) Slow-action contacts 1 NO/2 NC 5 directions of approaches Pull-out force 30 N separate actuators actuator 3SE5000-0AV0. must ordered separately",98.79,"ΤΕΜ",1,"EP",1,"3SE51220QV101AA7","3SE Τερματικοί διακόπτες"]
["3SE5132-3QV20","Safety position switch with separate actuator Plastic enclosure 40 mm  1 x (M20 x 1.5) Slow-action contacts 1 NO+2 NC with 2 LEDs yellow/green 230 V AC 5 directions of approaches The matching separate actuator 3SE5000-0AV0. must be ordered separately",83.47,"ΤΕΜ",1,"EP",1,"3SE51323QV20","3SE Τερματικοί διακόπτες"]
["3SE5212-0BF10","Position switch Metal enclosure according to EN 50047, 31 mm Device connection 1 x (M20 x 1.5) 1 NO/1 NC slow-action contacts Angular roller plunger with plastic roller 13 mm",43.37,"ΤΕΜ",1,"EP",1,"3SE52120BF10","3SE Τερματικοί διακόπτες"]
["3SE5232-0CK62-1AJ0","Position switch Plastic 31 mm according to EN 50047 Increased corrosion protection Device connection 1 x (M20 x 1.5) 1 NO/1 NC quick action contacts Twist lever, adjustable length with grid hole on the right and/or left adjustable, with Stainless steel lever and plastic roller 19 mm functional at -40 Β°C Shock and vibration test according to EN 61373, Category 1B",70.33,"ΤΕΜ",1,"EP",1,"3SE52320CK621AJ0","3SE Τερματικοί διακόπτες"]
["3SE5232-0HK52-1AK3","Position switch Plastic enclosure according to EN 50047, 31 mm Device connection 1 x (M20 x 1.5) 1 NO/1 NC quick action contacts integrated (not replaceable) adjustable-length Twist lever made of stainless steel right/left adjustable with plastic roller 19 mm Mounted on cover at 30Β° angle Head rotated by 270Β° clockwise Actuating/restoring force 20 N customized",50.07,"ΤΕΜ",1,"EP",1,"3SE52320HK521AK3","3SE Τερματικοί διακόπτες"]
["3SE5240-1AA00","LED cover for position switch for plastic enclosure 50 mm LEDs, yellow/green, 24 V DC Color yellow",25.28,"ΤΕΜ",1,"EP",1,"3SE52401AA00","3SE Τερματικοί διακόπτες"]
["3SE5242-3QV40","Safety position switch with separate actuator Plastic enclosure, 50 mm Device connection 2x (M20x 1.5) Slow-action contacts 1 NO+2 NC with 2 LEDs yellow/green 115-230 V AC 5 directions of approaches The matching separate actuator 3SE5000-0AV0. must be ordered separately",83.72,"ΤΕΜ",1,"EP",1,"3SE52423QV40","3SE Τερματικοί διακόπτες"]
["3SE5312-2SF12","Safety position switch with tumbler Locking force 2600 N 5 directions of approaches Spring-locked Escape release from the front Magnet voltage 115 V AC Monitoring actuator 2 NC/1 NO Monitoring magnet 2 NC/1 NO LED display yellow/green Supplied without actuator. Actuator 3SE5000-0AV0. please order separately",428.66,"ΤΕΜ",1,"EP",1,"3SE53122SF12","3SE Τερματικοί διακόπτες"]
["3SE6310-1BC01","Actuator with magnet latching 18 N safety switches RFID Rectangular 91 mm x 25 mm with magnet latching",134.32,"ΤΕΜ",1,"EP",1,"3SE63101BC01","3SE Τερματικοί διακόπτες"]
["3SE6605-2BA10","magnetically-operated switch, contact block rectangular large 25 x 88 mm, contacts 1 NC+1 NO, with 10 m cable. required solenoid 3SE6704-2BA or with increased operating distance 8 mm 3SE6701-2BA.",113.16,"ΤΕΜ",1,"EP",1,"3SE66052BA10","3SE Τερματικοί διακόπτες"]
["3SF1314-1SE11-1BA1","Safety position switch with tumbler Locking force 2600 N 5 directions of approaches Metal enclosure, M12 connector ASIsafe integrated Channel 1=actuator 1 NC Channel 2=magnet 1 NC spring-locked Auxiliary release lock on front Magnet voltage 24 V DC/AC Monitoring actuator 2 NC/1 NO Monitoring magnet 2 NC/1 NO The matching separate Actuator 3SE5000-0AV0 must be ordered separately",1151.5899999999999,"ΤΕΜ",1,"EP",1,"3SF13141SE111BA1","3SF AS-I τερματικοί διακόπτες"]
["3SF1324-1SF21-1BA1","Safety position switch with tumbler Locking force 1300 N 5 directions of approaches Plastic enclosure, M12 connector ASIsafe integrated Channel 1=actuator 1 NC Channel 2=magnet 1 NC spring-locked Escape release on the front Magnet voltage 24 V DC/AC Monitoring actuator 2 NC/1 NO Monitoring magnet 2 NC/1 NO The matching separate Actuator 3SE5000-0AV0 must be ordered separately",1003.2,"ΤΕΜ",1,"EP",1,"3SF13241SF211BA1","3SF AS-I τερματικοί διακόπτες"]
["3SK2122-2AA10","SIRIUS safety relay Basic unit 3SK2 series 20 F-DI, 4 F-DQ, 2 DQ, 24 V DC Can be parameterized via SIRIUS Safety ES 45 mm overall width Spring-type terminal (push-in) up to SILCL 3 (DIN EN 62061) Up to Performance Level E (ISO 13849-1) Output expansions 3SK1 and fail-safe motor starters 3RM1 via device connector connectable",731.14,"ΤΕΜ",1,"EP",1,"3SK21222AA10","3SK Ρελέ ασφαλείας"]
["3SU1000-1HK20-0AA0","EMERGENCY STOP mushroom pushbutton, 22 mm, round, plastic, red, 40 mm, with lock BKS, lock number S1, positive latching, acc. to EN ISO 13850, key-operated release",121.22,"ΤΕΜ",1,"EP",1,"3SU10001HK200AA0","3SU Μπουτόν"]
["3SU1000-4CF11-0AA0","RONIS key-operated switch, 22 mm, round, plastic, lock number 455, with 2 keys, 2 switch positions O-I, latching, actuating angle 90Β°, 10:30h/13:30h, Key removal O+I",33.81,"ΤΕΜ",1,"EP",1,"3SU10004CF110AA0","3SU Μπουτόν"]
["3SU1000-5SF01-0AA0","Key-operated switch BKS, 22 mm, round, plastic, Lock No. E7 (VW), without key, 2 switch positions O-I, latching, actuating angle 90Β°, 10:30h/13:30h, Key removal O",124.06,"ΤΕΜ",1,"EP",1,"3SU10005SF010AA0","3SU Μπουτόν"]
["3SU1001-0AA60-0AA0","Illuminated pushbutton, 22 mm, round, plastic, white, pushbutton, flat, latching, Push-to-release mechanism",15.15,"ΤΕΜ",1,"EP",1,"3SU10010AA600AA0","3SU Μπουτόν"]
["3SU1002-2BF50-0AA0","Selector switch, illuminable, 22 mm, round, plastic, blue, selector switch, short, 2 switch positions O-I, latching, actuating angle 90Β°, 10:30h/13:30h",13.83,"ΤΕΜ",1,"EP",1,"3SU10022BF500AA0","3SU Μπουτόν"]
["3SU1050-0AB10-0AA0","Pushbutton, 22 mm, round, metal, shiny, black, pushbutton, flat momentary contact type",8.35,"ΤΕΜ",1,"EP",1,"3SU10500AB100AA0","3SU Μπουτόν"]
["3SU1050-3AB61-0AK0","Twin pushbutton, 22 mm, round, metal, shiny, white: I, Black: O, pushbuttons, flat",17.61,"ΤΕΜ",1,"EP",1,"3SU10503AB610AK0","3SU Μπουτόν"]
["3SU1050-4CM01-0AA0","RONIS key-operated switch, 22 mm, round, metal, shiny, lock number 455, with 2 keys, 3 switch positions I>O<II, momentary contact type, actuating angle 2x45Β°, 10:30h/12h/13:30h, Key removal O",37.119999999999997,"ΤΕΜ",1,"EP",1,"3SU10504CM010AA0","3SU Μπουτόν"]
["3SU1050-7BF88-0AA0","Coordinate switch, 22 mm, round, metal shiny, black, 4 switch positions, momentary contact type, with mechanical interlocking",99.44,"ΤΕΜ",1,"EP",1,"3SU10507BF880AA0","3SU Μπουτόν"]
["3SU1051-0BB70-0AA0","Illuminated pushbutton, 22 mm, round, metal, shiny, clear, pushbutton, raised, momentary contact type",10.99,"ΤΕΜ",1,"EP",1,"3SU10510BB700AA0","3SU Μπουτόν"]
["3SU1051-3AB61-0AK0","Illuminated twin pushbutton, 22 mm, round, metal, shiny, white: I, Black: O, pushbuttons, flat",21.31,"ΤΕΜ",1,"EP",1,"3SU10513AB610AK0","3SU Μπουτόν"]
["3SU1052-2CN20-0AA0","Selector switch, illuminable, 22 mm, round, metal, shiny, red, selector switch, long, 3 switch positions I-O<II, left latching, right momentary contact type, actuating angle 2x45Β°, 10:30h/12h/13:30h",21.4,"ΤΕΜ",1,"EP",1,"3SU10522CN200AA0","3SU Μπουτόν"]
["3SU1062-2EF40-0AA0","Selector switch, illuminable, 30 mm, round, metal, matte, green, selector switch, long, front ring for flush installation, 2 switch positions O-I, latching, actuating angle 90Β°, 10:30h/13:30h",46.31,"ΤΕΜ",1,"EP",1,"3SU10622EF400AA0","3SU Μπουτόν"]
["3SU1100-0BB10-1CA0","Pushbutton, 22 mm, round, plastic, black, pushbutton, raised, momentary contact type, with holder 1 NC, screw terminal",21.59,"ΤΕΜ",1,"EP",1,"3SU11000BB101CA0","3SU Μπουτόν"]
["3SU1100-7AF10-1QA0","Coordinate switch, 22 mm, round, plastic, black, 4 switch positions, momentary contact type, without mechanical interlocking in O position, with holder, 1 NO, 1 NO, 1 NO, 1 NO, screw terminal",105.12,"ΤΕΜ",1,"EP",1,"3SU11007AF101QA0","3SU Μπουτόν"]
["3SU1103-2BF64-1BA0","Selector switch, illuminable, 22 mm, round, plastic, white, knob, short, 2 switch positions O-I, latching, 10:30 / 13:30, with holder, with LED module, green, with integrated LED 110 V AC, 1 NO, screw terminal",46.88,"ΤΕΜ",1,"EP",1,"3SU11032BF641BA0","3SU Μπουτόν"]
["3SU1106-0AB40-1BA0","Illuminated pushbutton, 22 mm, round, plastic, green, pushbutton, flat, momentary contact type, with holder, 1 NO, LED module with integrated LED 230 V AC, screw terminal",38.450000000000003,"ΤΕΜ",1,"EP",1,"3SU11060AB401BA0","3SU Μπουτόν"]
["3SU1150-1HB20-1PA0","EMERGENCY STOP mushroom pushbutton, 22 mm, round, metal, shiny, red, 40 mm, positive latching, according to EN ISO 13850, rotate-to-unlatch, without yellow backing plate, with holder, 1 NC, 1 NC, screw terminal",59.66,"ΤΕΜ",1,"EP",1,"3SU11501HB201PA0","3SU Μπουτόν"]
["3SU1150-7AF88-1QA0","Coordinate switch, 22 mm, round, metal shiny, black, 4 switch positions, momentary contact type, without mechanical interlocking, in O position, with holder, 1 NO, 1 NO, 1 NO, 1 NO, screw terminal,",115.53,"ΤΕΜ",1,"EP",1,"3SU11507AF881QA0","3SU Μπουτόν"]
["3SU1153-0AB70-1FA0","Illuminated pushbutton, 22 mm, round, metal, shiny, clear, pushbutton, flat, momentary contact type, with holder, 1 NO+1 NC, LED module with integrated LED 110 V AC, screw terminal",45.17,"ΤΕΜ",1,"EP",1,"3SU11530AB701FA0","3SU Μπουτόν"]
["3SU1156-0AB60-3FA0","Illuminated pushbutton, 22 mm, round, metal, shiny, white, pushbutton, flat, momentary contact type, with holder, 1 NO+1 NC, LED module with integrated LED 230 V AC, Spring-type terminal",47.92,"ΤΕΜ",1,"EP",1,"3SU11560AB603FA0","3SU Μπουτόν"]
["3SU1400-1EA10-2AA0","AS-Interface module, 2 safe inputs, black, 4-pole connector with screw terminal and 4-pole connector with spring-type terminal, for front plate mounting",369.33,"ΤΕΜ",1,"EP",1,"3SU14001EA102AA0","3SU Μπουτόν"]
["3SU1400-2AA10-3BA0","Contact module with 1 contact element, 1 NO, spring-type terminal, for floor mounting, Minimum order quantity 5 or a multiple thereof",8.1300000000000008,"ΤΕΜ",1,"EP",5,"3SU14002AA103BA0","3SU Μπουτόν"]
["3SU1401-1BF50-1AA0","LED module with integrated LED 230 V AC, blue, screw terminal, for front plate mounting",17.8,"ΤΕΜ",1,"EP",1,"3SU14011BF501AA0","3SU Μπουτόν"]
["3SU1401-2BB00-3AA2","LED module with integrated LED 24 V AC/DC, amber, Spring-loaded terminal, for floor mounting, ATEX Zone 1-2: Intrinsic safety",30.49,"ΤΕΜ",1,"EP",1,"3SU14012BB003AA2","3SU Μπουτόν"]
["3SU1401-3BA50-5AA0","LED module with integrated LED, 5 V DC, blue, solder terminal, for use on printed circuit boards",25.1,"ΤΕΜ",1,"EP",1,"3SU14013BA505AA0","3SU Μπουτόν"]
["3SU1511-1AB20-3MA0","holder, 3-way, metal, 1 NO, 1 NC, LED module, red, 24 V AC/DC, spring-loaded terminal",35.32,"ΤΕΜ",1,"EP",1,"3SU15111AB203MA0","3SU Μπουτόν"]
["3SU1550-1AA10-1PA0","holder, universal, 3-way, plastic/metal, 1 NC, 1 NC,",17.8,"ΤΕΜ",1,"EP",1,"3SU15501AA101PA0","3SU Μπουτόν"]
["3SU1803-0AT00-2AB1","enclosure for command devices, 22 mm, round, enclosure material plastic, enclosure top part gray, 3 control points plastic, C=Pushbutton green, label: Forward, 1 NO, 1 NC, screw terminal, B=Pushbutton black, label: Reverse, 1 NO, 1 NC, screw terminal, A=Pushbutton red, label: Stop, 1 NO, 1 NC, screw terminal, floor mounting, 1xM20 each on top and bottom, Labels glued in",134.47,"ΤΕΜ",1,"EP",1,"3SU18030AT002AB1","3SU Μπουτόν"]
["3SU1804-0AB00-4SB1","Enclosure for command devices, 22 mm, round, enclosure material plastic, enclosure top part gray, 4 control points plastic, recess for labels, customer-specific equipment, spring-loaded terminal, floor mounting, M12 connector 8-pin wired, GΓ¶pfert no. 428652 on rating plate Labels glued in",224.44,"ΤΕΜ",1,"EP",1,"3SU18040AB004SB1","3SU Μπουτόν"]
["3SU1900-0AB71-0DU0","Inscription plate for illuminated pushbutton, round, milky with black font, with inscription: Reset",187.51,"ΤΕΜ",100,"EP",10,"3SU19000AB710DU0","3SU Μπουτόν"]
["3SU1900-0AC16-0AH0","Labeling plate for snapping on or gluing, on label holder, label size 12.5x27 mm, black label, white font, with inscription: Rechts",199.82,"ΤΕΜ",100,"EP",10,"3SU19000AC160AH0","3SU Μπουτόν"]
["3SU1900-0AC81-0DC0","Labeling plate for snapping on or adhering to label holder, label size 12.5x27 mm, silver label, black font, with inscription: Stop Start",187.51,"ΤΕΜ",100,"EP",10,"3SU19000AC810DC0","3SU Μπουτόν"]
["3SU1900-0AC81-0EE0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, silver label, black font, with inscription: Fast",187.51,"ΤΕΜ",100,"EP",10,"3SU19000AC810EE0","3SU Μπουτόν"]
["3SU1900-0AD16-0QB0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, black label, white font, with graphic symbol: I",199.82,"ΤΕΜ",100,"EP",10,"3SU19000AD160QB0","3SU Μπουτόν"]
["3SU1900-0AF16-0AF0","Labeling plate for gluing on enclosure, label size 22x22 mm, black label, white font, with inscription: Vor",4.62,"ΤΕΜ",1,"EP",10,"3SU19000AF160AF0","3SU Μπουτόν"]
["3SU1900-0AF81-0AP0","Labeling plate for gluing on enclosure, label size 22x22 mm, silver label, black font with inscription: Betrieb",4.38,"ΤΕΜ",1,"EP",10,"3SU19000AF810AP0","3SU Μπουτόν"]
["3SU1900-0BC31-0AT0","Backing plate round, for EMERGENCY STOP  mushroom pushbutton, yellow, self-adhesive, Outer diameter 75 mm, inside diameter 23 mm, with inscription: NOT-HALT",7.38,"ΤΕΜ",1,"EP",10,"3SU19000BC310AT0","3SU Μπουτόν"]
["3SU1900-0HG10-0AA0","metric screw connection M20 with hexagon nut for enclosure",14.77,"ΤΕΜ",1,"EP",1,"3SU19000HG100AA0","3SU Μπουτόν"]
["3SU1900-0HH10-0AA0","metric screw connection M25 with hexagon nut for enclosure",14.77,"ΤΕΜ",1,"EP",1,"3SU19000HH100AA0","3SU Μπουτόν"]
["3SU1950-0FD80-0AA0","Key for key-operated switch BKS, Lock No. S1",18.37,"ΤΕΜ",1,"EP",1,"3SU19500FD800AA0","3SU Μπουτόν"]
["3TC4417-0BK2","Contactor, Size 2, 2-pole, DC-3 and 5, 32 A Auxiliary contacts 22 (2 NO + 2 NC) 120 V AC 50/60 Hz AC operation",269.11,"ΤΕΜ",1,"EP",1,"3TC44170BK2","3TC 2πολκά ρελέ"]
["3TC4417-0BR2","Contactor, Size 2, 2-pole, DC-3 and 5, 32 A Auxiliary contacts 22 (2 NO + 2 NC) 440 V AC 50/60 Hz AC operation",279.08,"ΤΕΜ",1,"EP",1,"3TC44170BR2","3TC 2πολκά ρελέ"]
["3TC5217-0LB4","Contactor, Size 8, 2-pole, DC-3 and 5, 170 A at 750 V Auxiliary contacts 21 (2NO + 1NC) 24V DC DC operation with varistor and series resistor Operating range 0.7 to 1.25 x US DC operation",2436.39,"ΤΕΜ",1,"EP",1,"3TC52170LB4","3TC 2πολκά ρελέ"]
["3TF6833-1QG7","Contactor, Size 14, 3-pole, AC-3, 335kW, 400/380 V (690 V) Auxiliary switch 33 (3NO+3NC) Rectifier bridge built-in with reversing contactor 3TC44 AC operation 110 to 120 V AC 50/60 Hz",5533.52,"ΤΕΜ",1,"EP",1,"3TF68331QG7","3TF Ρελέ ισχύος "]
["3TG1001-0BB45","Power relay, AC-3, for LOGO 8.4 A, 4 kW / 400 V 3 NO+1 NC, 24 V DC (6ED1057-4CA00-0AA0)",38.43,"ΤΕΜ",1,"EP",10,"3TG10010BB45","3TG Ρελέ 4KW"]
["3TH4244-0LC8","Contactor relay 44 E EN 50011 for railway applications 4NO+4NC,screw terminal Operating range 0.7 to 1.25 x US connected to varistor 33 V DC",176.61,"ΤΕΜ",1,"EP",1,"3TH42440LC8","3TH βοηθητικά ρελέ"]
["3TH4262-0BD4","Contactor relay, 62E, DIN EN 50011, 6 NO + 2 NC, screw terminal DC operation 42 V DC",167.2,"ΤΕΜ",1,"EP",1,"3TH42620BD4","3TH βοηθητικά ρελέ"]
["3TH4346-0AP0","Contactor relay, 73E, EN 50011, 7 NO + 3 NC 1U screw terminal AC operation, 230 V AC 50 Hz, 277 V 60 Hz",158.84,"ΤΕΜ",1,"EP",1,"3TH43460AP0","3TH βοηθητικά ρελέ"]
["3TH4364-0BF4","Contactor relay, 64E, EN 50011, 6NO + 4NC, screw terminal, DC operation, 110 V DC",213.18,"ΤΕΜ",1,"EP",1,"3TH43640BF4","3TH βοηθητικά ρελέ"]
["3TK1955-0A","Arc chutes 1 arc chute, 4-pole, 3TK15",730.3,"ΤΕΜ",1,"EP",1,"3TK19550A","3TK 4πολκά ρελέ"]
["3TX7402-3U","Surge suppressor RC element with cable spacer 240-400 V AC for mounting to coil terminal for contactors size S0-S2",20.58,"ΤΕΜ",1,"EP",1,"3TX74023U","3TX εξαρτήματα για ρελέ"]
["3TY1304-1S","Series resistor 4.5 kohm",42.65,"ΤΕΜ",1,"EP",1,"3TY13041S","3TY εξαρτήματα για ρελέ"]
["3TY2522-0A","Arc chute for contactor, 3TC52, Size 8,",149.91,"ΤΕΜ",1,"EP",1,"3TY25220A","3TY εξαρτήματα για ρελέ"]
["3TY6443-0BM4","Magnet coil for contactor 3TB44, 3TC44, DC 220V",85.09,"ΤΕΜ",1,"EP",1,"3TY64430BM4","3TY εξαρτήματα για ρελέ"]
["3TY6563-0BF4","Magnet coil for 3TB56, 3TC56, DC 110V",657.7,"ΤΕΜ",1,"EP",1,"3TY65630BF4","3TY εξαρτήματα για ρελέ"]
["3TY7693-0CM7","Magnet coil for contactor 3TF6944-.C.., 200...240 V AC 50/60 Hz",1129.5999999999999,"ΤΕΜ",1,"EP",1,"3TY76930CM7","3TY εξαρτήματα για ρελέ"]
["3UF7111-1AA01-0","Current/voltage measuring module V2; Set current 3...40 A, Voltage measurement up to 690 V, Overall width 45 mm, Straight-through transformer, basic unit required pro V PB, pro V MR, pro V PN or pro V EIP",360.96,"ΤΕΜ",1,"EP",1,"3UF71111AA010","3UF SIMOCODE"]
["3UF7982-0AA10-0","PCS 7 block library, SIMOCODE pro V7.0, AS blocks and faceplates for integration of SIMOCODE pro in the process control system PCS 7 for the PCS 7 version V7.0, Engineering software for an engineering station (single license) including runtime software for execution of the AS block in an automation system, Single License German/English/French Type of delivery: CD",2245.9499999999998,"ΤΕΜ",1,"EP",1,"3UF79820AA100","3UF SIMOCODE"]
["3UG4621-1AA30","Digital monitoring relay Current monitoring, 22.5 mm from 2-500 mA AC/DC 0vershoot and undershoot Supply voltage: 24 V AC/DC 50 to 60 Hz DC and AC without galvanic isolation to measuring circuit ON delay and noise pulses delay 0.1 to 20 s Hysteresis 0.1 to 250 mA 1 change-over contact with or without fault buffer screw terminal Successor product for 3UG3521-1AC..",166.27,"ΤΕΜ",1,"EP",1,"3UG46211AA30","3UG Επιτηρητές ηλεκτρικών μεγεθών"]
["3UG5461-1AA41","DC load monitoring relay for PROFINET, max. 2x8 A / 1x16 A DC, max. 60 V Width: 22.5 mm Monitoring for violation of upper and lower limit of current, voltage and power; energy consumption counter, energy recovery counter, switching cycle counter, operating hours counter warning and alarm thresholds auto-reset or manual reset ON delay 0-999.0 sec, OFF delay 0-999.0 sec, automatic reclosing delay 0-999.0 sec Supply voltage: 24 VDC 1 change-over contact, screw terminal",719.36,"ΤΕΜ",1,"EP",1,"3UG54611AA41","3UG Επιτηρητές ηλεκτρικών μεγεθών"]
["3VA1010-2ED42-0BA0","Circuit breaker 3VA1 IEC Frame 100 Switching capacity class B Icu=16 kA @ 415 V 4-pole, system protection TM210, FTFM, In=100 A Overload protection Ir=100 A non-adjustable short-circuit protection Ii = 10 x In N-conductor unprotected Lug terminal Undervoltage release (UVR) 24V DC",343.71,"ΤΕΜ",1,"EP",1,"3VA10102ED420BA0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1010-3ED32-0DH0","Circuit breaker 3VA1 IEC Frame 100 Switching capacity class N Icu=25 kA @ 415 V 3-pole, system protection TM210, FTFM, In=100 A Overload protection Ir=100 A non-adjustable short-circuit protection Ii = 10 x In Lug terminal Undervoltage release (UVR) 208-230 V AC 50/60 Hz 2 auxiliary switches HQ 1 tripped signaling contact HQ",347.7,"ΤΕΜ",1,"EP",1,"3VA10103ED320DH0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1010-4ED32-0DH0","circuit breaker 3VA1 IEC frame 100 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM210, FTFM, In=100A overload protection Ir=100A fixed short-circuit protection Ii=10 x In nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",350.55,"ΤΕΜ",1,"EP",1,"3VA10104ED320DH0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1020-2ED32-0AF0","circuit breaker 3VA1 IEC frame 100 breaking capacity class B Icu=16kA @ 415V 3-pole, line protection TM210, FTFM, In=20A overload protection Ir=20A fixed short-circuit protection Ii=16 x In nut keeper kit 1 auxiliary switch HQ 1 trip alarm switch HQ",192.66,"ΤΕΜ",1,"EP",1,"3VA10202ED320AF0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1020-3ED32-0BA0","circuit breaker 3VA1 IEC frame 100 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM210, FTFM, In=20A overload protection Ir=20A fixed short-circuit protection Ii=16 x In nut keeper kit undervoltage release (UVR) 24V DC",247.38,"ΤΕΜ",1,"EP",1,"3VA10203ED320BA0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1020-3ED36-0AE0","circuit breaker 3VA1 IEC frame 100 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM210, FTFM, In=20A overload protection Ir=20A fixed short-circuit protection Ii=16 x In clamp connection 4 auxiliary switches HQ",253.08,"ΤΕΜ",1,"EP",1,"3VA10203ED360AE0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1020-4ED32-0JH0","circuit breaker 3VA1 IEC frame 100 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM210, FTFM, In=20A overload protection Ir=20A fixed short-circuit protection Ii=16 x In nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",287.85000000000002,"ΤΕΜ",1,"EP",1,"3VA10204ED320JH0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1025-3ED32-0HA0","circuit breaker 3VA1 IEC frame 100 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM210, FTFM, In=25A overload protection Ir=25A fixed short-circuit protection Ii=12.8 x In nut keeper kit shunt trip (STL) 12-30V DC, 24V AC 50/60Hz",226.86,"ΤΕΜ",1,"EP",1,"3VA10253ED320HA0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1032-2ED36-0CH0","circuit breaker 3VA1 IEC frame 100 breaking capacity class B Icu=16kA @ 415V 3-pole, line protection TM210, FTFM, In=32A overload protection Ir=32A fixed short-circuit protection Ii=10 x In clamp connection undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",319.77,"ΤΕΜ",1,"EP",1,"3VA10322ED360CH0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1032-3ED36-0DA0","circuit breaker 3VA1 IEC frame 100 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM210, FTFM, In=32A overload protection Ir=32A fixed short-circuit protection Ii=10 x In clamp connection undervoltage release (UVR) 208-230V AC 50/60Hz",264.48,"ΤΕΜ",1,"EP",1,"3VA10323ED360DA0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1032-4ED32-0AA0","circuit breaker 3VA1 IEC frame 100 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM210, FTFM, In=32A overload protection Ir=32A fixed short-circuit protection Ii=10 x In nut keeper kit",159.6,"ΤΕΜ",1,"EP",1,"3VA10324ED320AA0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1040-2ED36-0AA0","circuit breaker 3VA1 IEC frame 100 breaking capacity class B Icu=16kA @ 415V 3-pole, line protection TM210, FTFM, In=40A overload protection Ir=40A fixed short-circuit protection Ii=10 x In clamp connection",171.57,"ΤΕΜ",1,"EP",1,"3VA10402ED360AA0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1040-3ED36-0AD0","circuit breaker 3VA1 IEC frame 100 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM210, FTFM, In=40A overload protection Ir=40A fixed short-circuit protection Ii=10 x In clamp connection 3 auxiliary switches HQ",232.56,"ΤΕΜ",1,"EP",1,"3VA10403ED360AD0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1050-2ED36-0DA0","circuit breaker 3VA1 IEC frame 100 breaking capacity class B Icu=16kA @ 415V 3-pole, line protection TM210, FTFM, In=50A overload protection Ir=50A fixed short-circuit protection Ii=10 x In clamp connection undervoltage release (UVR) 208-230V AC 50/60Hz",261.06,"ΤΕΜ",1,"EP",1,"3VA10502ED360DA0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1050-3ED32-0BA0","circuit breaker 3VA1 IEC frame 100 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM210, FTFM, In=50A overload protection Ir=50A fixed short-circuit protection Ii=10 x In nut keeper kit undervoltage release (UVR) 24V DC",247.38,"ΤΕΜ",1,"EP",1,"3VA10503ED320BA0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1050-3ED42-0AA0","circuit breaker 3VA1 IEC frame 100 breaking capacity class N Icu=25kA @ 415V 4-pole, line protection TM210, FTFM, In=50A overload protection Ir=50A fixed short-circuit protection Ii=10 x In N conductor unprotected nut keeper kit",202.35,"ΤΕΜ",1,"EP",1,"3VA10503ED420AA0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1050-4ED36-0BA0","circuit breaker 3VA1 IEC frame 100 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM210, FTFM, In=50A overload protection Ir=50A fixed short-circuit protection Ii=10 x In clamp connection undervoltage release (UVR) 24V DC",267.89999999999998,"ΤΕΜ",1,"EP",1,"3VA10504ED360BA0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1063-2ED32-0AA0","circuit breaker 3VA1 IEC frame 100 breaking capacity class B Icu=16kA @ 415V 3-pole, line protection TM210, FTFM, In=63A overload protection Ir=63A fixed short-circuit protection Ii=10 x In nut keeper kit",152.76,"ΤΕΜ",1,"EP",1,"3VA10632ED320AA0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1063-3ED32-0AC0","circuit breaker 3VA1 IEC frame 100 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM210, FTFM, In=63A overload protection Ir=63A fixed short-circuit protection Ii=10 x In nut keeper kit 2 auxiliary switches HQ",194.94,"ΤΕΜ",1,"EP",1,"3VA10633ED320AC0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1063-3ED42-0AD0","circuit breaker 3VA1 IEC frame 100 breaking capacity class N Icu=25kA @ 415V 4-pole, line protection TM210, FTFM, In=63A overload protection Ir=63A fixed short-circuit protection Ii=10 x In N conductor unprotected nut keeper kit 3 auxiliary switches HQ",261.06,"ΤΕΜ",1,"EP",1,"3VA10633ED420AD0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1063-4ED36-0KC0","circuit breaker 3VA1 IEC frame 100 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM210, FTFM, In=63A overload protection Ir=63A fixed short-circuit protection Ii=10 x In clamp connection shunt trip (STL) 220-250V DC, 208-277V AC 2 auxiliary switches HQ",286.14,"ΤΕΜ",1,"EP",1,"3VA10634ED360KC0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1063-4ED42-0JC0","circuit breaker 3VA1 IEC frame 100 breaking capacity class S Icu=36kA @ 415V 4-pole, line protection TM210, FTFM, In=63A overload protection Ir=63A fixed short-circuit protection Ii=10 x In N conductor unprotected nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ",317.49,"ΤΕΜ",1,"EP",1,"3VA10634ED420JC0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1080-2ED42-0AC0","circuit breaker 3VA1 IEC frame 100 breaking capacity class B Icu=16kA @ 415V 4-pole, line protection TM210, FTFM, In=80A overload protection Ir=80A fixed short-circuit protection Ii=10 x In N conductor unprotected nut keeper kit 2 auxiliary switches HQ",257.64,"ΤΕΜ",1,"EP",1,"3VA10802ED420AC0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1080-3ED36-0HC0","circuit breaker 3VA1 IEC frame 100 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM210, FTFM, In=80A overload protection Ir=80A fixed short-circuit protection Ii=10 x In clamp connection shunt trip (STL) 12-30V DC, 24V AC 50/60Hz 2 auxiliary switches HQ",297.54000000000002,"ΤΕΜ",1,"EP",1,"3VA10803ED360HC0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1080-4ED36-0HH0","circuit breaker 3VA1 IEC frame 100 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM210, FTFM, In=80A overload protection Ir=80A fixed short-circuit protection Ii=10 x In clamp connection shunt trip (STL) 12-30V DC, 24V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",320.33999999999997,"ΤΕΜ",1,"EP",1,"3VA10804ED360HH0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1096-2ED32-0AD0","circuit breaker 3VA1 IEC frame 100 breaking capacity class B Icu=16kA @ 415V 3-pole, line protection TM210, FTFM, In=16A overload protection Ir=16A fixed short-circuit protection Ii=10 x In nut keeper kit 3 auxiliary switches HQ",212.04,"ΤΕΜ",1,"EP",1,"3VA10962ED320AD0","3VA10 Διακόπτες ισχύος κλειστού τύπου έως 100Α"]
["3VA1102-6MG36-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, starter protection TM110M, FM, In=2A without overload protection short-circuit protection Ii=15 x In clamp connection",279.93,"ΤΕΜ",1,"EP",1,"3VA11026MG360AA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1110-1AA36-0AM0","switch disconnector 3VA1 IEC frame 160 3-pole SD100, In=100A without overload protection w/o short-circuit protection clamp connection switch disconnector 3VA1 IEC frame 160 3-pole SD100, In=100A without overload protection w/o short-circuit protection clamp connection 2 AUXILIARY SWITCH CHANGEOVER H 1 short circuit alarm switch HQ",325.08,"ΤΕΜ",1,"EP",1,"3VA11101AA360AM0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1110-1AA46-0BF0","switch disconnector 3VA1 IEC frame 160 4-pole SD100, In=100A without overload protection w/o short-circuit protection clamp connection undervoltage release 24V DC 1 auxiliary switch 1 trip alarm switch",442.47,"ΤΕΜ",1,"EP",1,"3VA11101AA460BF0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1110-3EF36-0BC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM240, ATAM, In=100A overload protection Ir=70A...100A short-circuit protection Ii=5...10 x In clamp connection undervoltage release (UVR) 24V DC 2 auxiliary switches HQ",369.93,"ΤΕΜ",1,"EP",1,"3VA11103EF360BC0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1110-4ED46-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 4-pole, line protection TM210, FTFM, In=100A overload protection Ir=100A fixed short-circuit protection Ii=10 x In N conductor unprotected clamp connection",334.2,"ΤΕΜ",1,"EP",1,"3VA11104ED460AA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1110-5ED26-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 2-pole, line protection TM210, FTFM, In=100A overload protection Ir=100A fixed short-circuit protection Ii=10 x In clamp connection",256.68,"ΤΕΜ",1,"EP",1,"3VA11105ED260AA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1110-5EF32-0AM0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=100A overload protection Ir=70A...100A short-circuit protection Ii=5...10 x In nut keeper kit circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=100A overload protection Ir=70A...100A short-circuit protection Ii=5...10 x In nut 2 AUXILIARY SWITCH CHANGEOVER H 1 short circuit alarm switch HQ",383.16,"ΤΕΜ",1,"EP",1,"3VA11105EF320AM0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1110-5EF36-0JC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=100A overload protection Ir=70A...100A short-circuit protection Ii=5...10 x In clamp connection shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ",427.8,"ΤΕΜ",1,"EP",1,"3VA11105EF360JC0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1110-5MH36-0DC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, starter protection TM120M, AM, In=100A without overload protection short-circuit protection Ii=5...15 x In clamp connection undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ",450.74,"ΤΕΜ",1,"EP",1,"3VA11105MH360DC0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1110-6EF36-0BC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM240, ATAM, In=100A overload protection Ir=70A...100A short-circuit protection Ii=5...10 x In clamp connection undervoltage release (UVR) 24V DC 2 auxiliary switches HQ",475.54,"ΤΕΜ",1,"EP",1,"3VA11106EF360BC0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1110-6FE42-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 4-pole, line protection TM220, ATFM, In=100A overload protection Ir=70A...100A short-circuit protection Ii=10 x In N conductor protection 50% nut keeper kit",390.6,"ΤΕΜ",1,"EP",1,"3VA11106FE420AA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1110-6MH36-0AD0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, starter protection TM120M, AM, In=100A without overload protection short-circuit protection Ii=5...15 x In clamp connection 3 auxiliary switches HQ",399.28,"ΤΕΜ",1,"EP",1,"3VA11106MH360AD0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1112-1AA42-0AC0","switch disconnector 3VA1 IEC frame 160 4-pole SD100, In=125A without overload protection w/o short-circuit protection nut keeper kit 2 auxiliary switches HQ",373.86,"ΤΕΜ",1,"EP",1,"3VA11121AA420AC0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1112-3EF36-0BC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM240, ATAM, In=125A overload protection Ir=88A...125A short-circuit protection Ii=5...10 x In clamp connection undervoltage release (UVR) 24V DC 2 auxiliary switches HQ",488.4,"ΤΕΜ",1,"EP",1,"3VA11123EF360BC0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1112-3FD46-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 4-pole, line protection TM210, FTFM, In=125A overload protection Ir=125A fixed short-circuit protection Ii=10 x In N conductor protection 50% clamp connection",442.75,"ΤΕΜ",1,"EP",1,"3VA11123FD460AA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1112-4EF36-0JH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=125A overload protection Ir=88A...125A short-circuit protection Ii=5...10 x In clamp connection shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",518.1,"ΤΕΜ",1,"EP",1,"3VA11124EF360JH0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1112-5ED32-0JH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM210, FTFM, In=125A overload protection Ir=125A fixed short-circuit protection Ii=10 x In nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",548.11,"ΤΕΜ",1,"EP",1,"3VA11125ED320JH0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1112-5EF36-0AB0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=125A overload protection Ir=88A...125A short-circuit protection Ii=5...10 x In clamp connection 2 auxiliary switches HP",523.91999999999996,"ΤΕΜ",1,"EP",1,"3VA11125EF360AB0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1112-5MH36-0HC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, starter protection TM120M, AM, In=125A without overload protection short-circuit protection Ii=5...15 x In clamp connection shunt trip (STL) 12-30 V DC; 24 V AC 50/60 Hz 2 auxiliary switches HQ",575.25,"ΤΕΜ",1,"EP",1,"3VA11125MH360HC0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1112-6ED46-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 4-pole, line protection TM210, FTFM, In=125A overload protection Ir=125A fixed short-circuit protection Ii=10 x In N conductor unprotected clamp connection",644.79999999999995,"ΤΕΜ",1,"EP",1,"3VA11126ED460AA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1112-6MH32-0KC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, starter protection TM120M, AM, In=125A without overload protection short-circuit protection Ii=5...15 x In nut keeper kit shunt trip (STL) 220-250 V DC; 208-277 V AC 2 auxiliary switches HQ",626.20000000000005,"ΤΕΜ",1,"EP",1,"3VA11126MH320KC0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1112-6MH36-0BC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, starter protection TM120M, AM, In=125A without overload protection short-circuit protection Ii=5...15 x In clamp connection undervoltage release (UVR) 24V DC 2 auxiliary switches HQ",669.6,"ΤΕΜ",1,"EP",1,"3VA11126MH360BC0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1116-1AA36-0CA0","switch disconnector 3VA1 IEC frame 160 3-pole SD100, In=160A without overload protection w/o short-circuit protection clamp connection undervoltage release (UVR) 120-127V AC 50/60Hz",391.84,"ΤΕΜ",1,"EP",1,"3VA11161AA360CA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1116-3EF32-0CA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM240, ATAM, In=160A overload protection Ir=112A...160A short-circuit protection Ii=5...10 x In nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz",496.17,"ΤΕΜ",1,"EP",1,"3VA11163EF320CA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1116-3FD46-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 4-pole, line protection TM210, FTFM, In=160A overload protection Ir=160A fixed short-circuit protection Ii=10 x In N conductor protection 50% clamp connection",560.4,"ΤΕΜ",1,"EP",1,"3VA11163FD460AA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1116-4EF36-0JC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=160A overload protection Ir=112A...160A short-circuit protection Ii=5...10 x In clamp connection shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ",515.1,"ΤΕΜ",1,"EP",1,"3VA11164EF360JC0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1116-5EE32-0HA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM220, ATFM, In=160A overload protection Ir=112A...160A short-circuit protection Ii=10 x In nut keeper kit shunt trip (STL) 12-30V DC, 24V AC 50/60Hz",522.11,"ΤΕΜ",1,"EP",1,"3VA11165EE320HA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1116-5EF32-0BA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=160A overload protection Ir=112A...160A short-circuit protection Ii=5...10 x In nut keeper kit undervoltage release (UVR) 24V DC",566.79999999999995,"ΤΕΜ",1,"EP",1,"3VA11165EF320BA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1116-5EF36-0HA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=160A overload protection Ir=112A...160A short-circuit protection Ii=5...10 x In clamp connection shunt trip (STL) 12-30V DC, 24V AC 50/60Hz",561.35,"ΤΕΜ",1,"EP",1,"3VA11165EF360HA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1116-6EF32-0CA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM240, ATAM, In=160A overload protection Ir=112A...160A short-circuit protection Ii=5...10 x In nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz",705.6,"ΤΕΜ",1,"EP",1,"3VA11166EF320CA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1116-6EF36-0DC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM240, ATAM, In=160A overload protection Ir=112A...160A short-circuit protection Ii=5...10 x In clamp connection undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ",774.9,"ΤΕΜ",1,"EP",1,"3VA11166EF360DC0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1120-3EF36-0KA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM240, ATAM, In=20A overload protection Ir=14A...20A short-circuit protection Ii=8...16 x In clamp connection shunt trip (STL) 220-250V DC, 208-277V AC",292.74,"ΤΕΜ",1,"EP",1,"3VA11203EF360KA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1120-4EE36-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM220, ATFM, In=20A overload protection Ir=14A...20A short-circuit protection Ii=16 x In clamp connection",222.25,"ΤΕΜ",1,"EP",1,"3VA11204EE360AA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1120-5ED16-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 240V 1-pole, line protection TM210, FTFM, In=20A overload protection Ir=20A fixed short-circuit protection Ii=16 x In clamp connection",116.21,"ΤΕΜ",1,"EP",1,"3VA11205ED160AA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1120-5EF36-0HA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=20A overload protection Ir=14A...20A short-circuit protection Ii=8...16 x In clamp connection shunt trip (STL) 12-30V DC, 24V AC 50/60Hz",331.47,"ΤΕΜ",1,"EP",1,"3VA11205EF360HA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1120-6EF36-0JH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM240, ATAM, In=20A overload protection Ir=14A...20A short-circuit protection Ii=8...16 x In clamp connection shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",427.05,"ΤΕΜ",1,"EP",1,"3VA11206EF360JH0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1125-3EF32-0HA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM240, ATAM, In=25A overload protection Ir=18A...25A short-circuit protection Ii=6.4...12.8 x In nut keeper kit shunt trip (STL) 12-30V DC, 24V AC 50/60Hz",272.19,"ΤΕΜ",1,"EP",1,"3VA11253EF320HA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1125-5EE32-0BF0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM220,  ATFM, In=25A overload protection Ir=18A ...25A short-circuit protection Ii=12.8 x In nut keeper kit undervoltage release (UVR) 24V DC 1 auxiliary switch HQ 1 trip alarm switch HQ",366.51,"ΤΕΜ",1,"EP",1,"3VA11255EE320BF0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1125-5EF36-0BH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=25A overload protection Ir=18A...25A short-circuit protection Ii=6.4...12.8 x In clamp connection undervoltage release (UVR) 24V DC 2 auxiliary switches HQ 1 trip alarm switch HQ",417.78,"ΤΕΜ",1,"EP",1,"3VA11255EF360BH0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1125-5GE46-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection TM220, ATFM, In=25A overload protection Ir=18A...25A short-circuit protection Ii=12.8 x In N conductor protection 100% clamp connection",315.23,"ΤΕΜ",1,"EP",1,"3VA11255GE460AA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1132-3EF32-0KC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM240, ATAM, In=32A overload protection Ir=22A...32A short-circuit protection Ii=5...10 x In nut keeper kit shunt trip (STL) 220-250V DC, 208-277V AC 2 auxiliary switches HQ",315.87,"ΤΕΜ",1,"EP",1,"3VA11323EF320KC0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1132-3GF42-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 4-pole, line protection TM240, ATAM, In=32A overload protection Ir=22A...32A short-circuit protection Ii=5...10 x In N conductor protection 100% nut keeper kit",253.2,"ΤΕΜ",1,"EP",1,"3VA11323GF420AA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1132-5ED12-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 240V 1-pole, line protection TM210, FTFM, In=32A overload protection Ir=32A fixed short-circuit protection Ii=10 x In nut keeper kit",108.24,"ΤΕΜ",1,"EP",1,"3VA11325ED120AA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1132-5EF32-0HH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=32A overload protection Ir=22A...32A short-circuit protection Ii=5...10 x In nut keeper kit shunt trip (STL) 12-30V DC, 24V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",376.64,"ΤΕΜ",1,"EP",1,"3VA11325EF320HH0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1132-6EF36-0AE0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM240, ATAM, In=32A overload protection Ir=22A...32A short-circuit protection Ii=5...10 x In clamp connection 4 auxiliary switches HQ",369.2,"ΤΕΜ",1,"EP",1,"3VA11326EF360AE0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1132-6EF36-0KC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM240, ATAM, In=32A overload protection Ir=22A...32A short-circuit protection Ii=5...10 x In clamp connection shunt trip (STL) 220-250V DC, 208-277V AC 2 auxiliary switches HQ",405.6,"ΤΕΜ",1,"EP",1,"3VA11326EF360KC0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1140-3EF36-0HC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM240, ATAM, In=40A overload protection Ir=28A...40A short-circuit protection Ii=5...10 x In clamp connection shunt trip (STL) 12-30V DC, 24V AC 50/60Hz 2 auxiliary switches HQ",335.49,"ΤΕΜ",1,"EP",1,"3VA11403EF360HC0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1140-4EF32-0JC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=40A overload protection Ir=28A...40A short-circuit protection Ii=5...10 x In nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ",331.69,"ΤΕΜ",1,"EP",1,"3VA11404EF320JC0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1140-5EF32-0JA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=40A overload protection Ir=28A...40A short-circuit protection Ii=5...10 x In nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz",311.44,"ΤΕΜ",1,"EP",1,"3VA11405EF320JA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1140-6EE42-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 4-pole, line protection TM220, ATFM, In=40A overload protection Ir=28A...40A short-circuit protection Ii=10 x In N conductor unprotected nut keeper kit",323.7,"ΤΕΜ",1,"EP",1,"3VA11406EE420AA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1150-3ED36-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM210, FTFM, In=50A overload protection Ir=50A fixed short-circuit protection Ii=10 x In clamp connection",200.66,"ΤΕΜ",1,"EP",1,"3VA11503ED360AA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1150-3EF36-0BH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM240, ATAM, In=50A overload protection Ir=35A...50A short-circuit protection Ii=5...10 x In clamp connection undervoltage release (UVR) 24V DC 2 auxiliary switches HQ 1 trip alarm switch HQ",379.8,"ΤΕΜ",1,"EP",1,"3VA11503EF360BH0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1150-4EF32-0KH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=50A overload protection Ir=35A...50A short-circuit protection Ii=5...10 x In nut keeper kit shunt trip (STL) 220-250V DC, 208-277V AC 2 auxiliary switches HQ 1 trip alarm switch HQ",353.85,"ΤΕΜ",1,"EP",1,"3VA11504EF320KH0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1150-5ED16-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 240V 1-pole, line protection TM210, FTFM, In=50A overload protection Ir=50A fixed short-circuit protection Ii=10 x In clamp connection",115.84,"ΤΕΜ",1,"EP",1,"3VA11505ED160AA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1150-5EF36-0AE0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=50A overload protection Ir=35A...50A short-circuit protection Ii=5...10 x In clamp connection 4 auxiliary switches HQ",340.55,"ΤΕΜ",1,"EP",1,"3VA11505EF360AE0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1150-6EF32-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM240, ATAM, In=50A overload protection Ir=35A...50A short-circuit protection Ii=5...10 x In nut keeper kit",260.64999999999998,"ΤΕΜ",1,"EP",1,"3VA11506EF320AA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1163-1AA32-0DH0","switch disconnector 3VA1 IEC frame 160 3-pole SD100, In=63A without overload protection w/o short-circuit protection nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",332.8,"ΤΕΜ",1,"EP",1,"3VA11631AA320DH0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1163-3EE36-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM220, ATFM, In=63A overload protection Ir=44A...63A short-circuit protection Ii=10 x In clamp connection",185.41,"ΤΕΜ",1,"EP",1,"3VA11633EE360AA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1163-3EF32-0HA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM240, ATAM, In=63A overload protection Ir=44A...63A short-circuit protection Ii=5...10 x In nut keeper kit shunt trip (STL) 12-30V DC, 24V AC 50/60Hz",268.75,"ΤΕΜ",1,"EP",1,"3VA11633EF320HA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1163-4ED22-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 2-pole, line protection TM210, FTFM, In=63A overload protection Ir=63A fixed short-circuit protection Ii=10 x In nut keeper kit",175,"ΤΕΜ",1,"EP",1,"3VA11634ED220AA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1163-5ED22-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 2-pole, line protection TM210, FTFM, In=63A overload protection Ir=63A fixed short-circuit protection Ii=10 x In nut keeper kit",194.38,"ΤΕΜ",1,"EP",1,"3VA11635ED220AA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1163-5EF32-0CC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=63A overload protection Ir=44A...63A short-circuit protection Ii=5...10 x In nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ",372.5,"ΤΕΜ",1,"EP",1,"3VA11635EF320CC0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1163-5MH32-0AC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, starter protection TM120M, AM, In=63A without overload protection short-circuit protection Ii=5...15 x In nut keeper kit 2 auxiliary switches HQ",273.13,"ΤΕΜ",1,"EP",1,"3VA11635MH320AC0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1163-5MH32-0CH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, starter protection TM120M, AM, In=63A without overload protection short-circuit protection Ii=5...15 x In nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",393.75,"ΤΕΜ",1,"EP",1,"3VA11635MH320CH0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1163-6EF36-0KC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM240, ATAM, In=63A overload protection Ir=44A...63A short-circuit protection Ii=5...10 x In clamp connection shunt trip (STL) 220-250V DC, 208-277V AC 2 auxiliary switches HQ",405.6,"ΤΕΜ",1,"EP",1,"3VA11636EF360KC0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1163-6MH32-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, starter protection TM120M, AM, In=63A without overload protection short-circuit protection Ii=7...16 x In nut keeper kit",260.64999999999998,"ΤΕΜ",1,"EP",1,"3VA11636MH320AA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1180-3EF32-0DH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM240, ATAM, In=80A overload protection Ir=56A...80A short-circuit protection Ii=5...10 x In nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",379.17,"ΤΕΜ",1,"EP",1,"3VA11803EF320DH0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1180-3GF46-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 4-pole, line protection TM240, ATAM, In=80A overload protection Ir=56A...80A short-circuit protection Ii=5...10 x In N conductor protection 100% clamp connection",305.74,"ΤΕΜ",1,"EP",1,"3VA11803GF460AA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1180-4EF36-0AD0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=80A overload protection Ir=56A...80A short-circuit protection Ii=5...10 x In clamp connection 3 auxiliary switches HQ",317.13,"ΤΕΜ",1,"EP",1,"3VA11804EF360AD0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1180-5EF32-0AH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=80A overload protection Ir=56A...80A short-circuit protection Ii=5...10 x In nut keeper kit 2 auxiliary switches HQ 1 trip alarm switch HQ",320.93,"ΤΕΜ",1,"EP",1,"3VA11805EF320AH0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1180-5EF36-0KC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=80A overload protection Ir=56A...80A short-circuit protection Ii=5...10 x In clamp connection shunt trip (STL) 220-250V DC, 208-277V AC 2 auxiliary switches HQ",396.26,"ΤΕΜ",1,"EP",1,"3VA11805EF360KC0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1180-6GF46-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 4-pole, line protection TM240, ATAM, In=80A overload protection Ir=56A...80A short-circuit protection Ii=5...10 x In N conductor protection 100% clamp connection",399.75,"ΤΕΜ",1,"EP",1,"3VA11806GF460AA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1196-3EF32-0CA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM240, ATAM, In=16A overload protection Ir=11A...16A short-circuit protection Ii=10...20 x In nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz",294.35000000000002,"ΤΕΜ",1,"EP",1,"3VA11963EF320CA0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1196-4EF36-0CH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=16A overload protection Ir=11A...16A short-circuit protection Ii=10...20 x In clamp connection undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",398.16,"ΤΕΜ",1,"EP",1,"3VA11964EF360CH0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1196-5EF32-0KH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=16A overload protection Ir=11A...16A short-circuit protection Ii=10...20 x In nut keeper kit shunt trip (STL) 220-250V DC, 208-277V AC 2 auxiliary switches HQ 1 trip alarm switch HQ",376.64,"ΤΕΜ",1,"EP",1,"3VA11965EF320KH0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1196-6EF32-0DC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM240, ATAM, In=16A overload protection Ir=11A...16A short-circuit protection Ii=10...20 x In nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ",408.85,"ΤΕΜ",1,"EP",1,"3VA11966EF320DC0","3VA11 Διακόπτες ισχύος κλειστού τύπου έως 160Α"]
["3VA1216-4EF32-0AB0","circuit breaker 3VA1 IEC frame 250 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=160A overload protection Ir=112A...160A short-circuit protection Ii=5...10 x In nut keeper kit 2 auxiliary switches HP",683.64,"ΤΕΜ",1,"EP",1,"3VA12164EF320AB0","3VA12 Διακότπες ισχύος κλειστού τύπου έως 250Α"]
["3VA1216-5GF42-0KF0","circuit breaker 3VA1 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection TM240, ATAM, In=160A overload protection Ir=112A...160A short-circuit protection Ii=5...10 x In N conductor protection 100% nut keeper kit shunt trip (STL) 220-250V DC; 208-277V AC 1 auxiliary switch HQ 1 trip alarm switch HQ",1012.8,"ΤΕΜ",1,"EP",1,"3VA12165GF420KF0","3VA12 Διακότπες ισχύος κλειστού τύπου έως 250Α"]
["3VA1220-4EF32-0DA0","circuit breaker 3VA1 IEC frame 250 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=200A overload protection Ir=140A...200A short-circuit protection Ii=5...10 x In nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz",631.79999999999995,"ΤΕΜ",1,"EP",1,"3VA12204EF320DA0","3VA12 Διακότπες ισχύος κλειστού τύπου έως 250Α"]
["3VA1220-5EF32-0AF0","circuit breaker 3VA1 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=200A overload protection Ir=140A...200A short-circuit protection Ii=5...10 x In nut keeper kit 1 auxiliary switch HQ 1 trip alarm switch HQ",631.29999999999995,"ΤΕΜ",1,"EP",1,"3VA12205EF320AF0","3VA12 Διακότπες ισχύος κλειστού τύπου έως 250Α"]
["3VA1220-5EF42-0DF0","circuit breaker 3VA1 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection TM240, ATAM, In=200A overload protection Ir=140A...200A short-circuit protection Ii=5...10 x In N conductor unprotected nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 1 auxiliary switch HQ 1 trip alarm switch HQ",893.45,"ΤΕΜ",1,"EP",1,"3VA12205EF420DF0","3VA12 Διακότπες ισχύος κλειστού τύπου έως 250Α"]
["3VA1220-6EF32-0AG0","circuit breaker 3VA1 IEC frame 250 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM240, ATAM, In=200A overload protection Ir=140A...200A short-circuit protection Ii=5...10 x In nut keeper kit 1 auxiliary switch HP 1 trip alarm switch HP",666.4,"ΤΕΜ",1,"EP",1,"3VA12206EF320AG0","3VA12 Διακότπες ισχύος κλειστού τύπου έως 250Α"]
["3VA1220-6EF32-0KH0","circuit breaker 3VA1 IEC frame 250 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM240, ATAM, In=200A overload protection Ir=140A...200A short-circuit protection Ii=5...10 x In nut keeper kit shunt trip (STL) 220-250V DC, 208-277V AC 2 auxiliary switches HQ 1 trip alarm switch HQ",725.2,"ΤΕΜ",1,"EP",1,"3VA12206EF320KH0","3VA12 Διακότπες ισχύος κλειστού τύπου έως 250Α"]
["3VA1225-1AA32-0DA0","switch disconnector 3VA1 IEC frame 250 3-pole SD100, In=250A without overload protection w/o short-circuit protection nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz",579.15,"ΤΕΜ",1,"EP",1,"3VA12251AA320DA0","3VA12 Διακότπες ισχύος κλειστού τύπου έως 250Α"]
["3VA1225-1AA42-0JC0","switch disconnector 3VA1 IEC frame 250 4-pole SD100, In=250A without overload protection w/o short-circuit protection nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ",741,"ΤΕΜ",1,"EP",1,"3VA12251AA420JC0","3VA12 Διακότπες ισχύος κλειστού τύπου έως 250Α"]
["3VA1225-4EF42-0AE0","circuit breaker 3VA1 IEC frame 250 breaking capacity class S Icu=36kA @ 415V 4-pole, line protection TM240, ATAM, In=250A overload protection Ir=175A...250A short-circuit protection Ii=5...10 x In N conductor unprotected nut keeper kit 4 auxiliary switches HQ",810,"ΤΕΜ",1,"EP",1,"3VA12254EF420AE0","3VA12 Διακότπες ισχύος κλειστού τύπου έως 250Α"]
["3VA1225-5EF32-0HC0","circuit breaker 3VA1 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=250A overload protection Ir=175A...250A short-circuit protection Ii=5...10 x In nut keeper kit shunt trip (STL) 12-30V DC, 24V AC 50/60Hz 2 auxiliary switches HQ",886.6,"ΤΕΜ",1,"EP",1,"3VA12255EF320HC0","3VA12 Διακότπες ισχύος κλειστού τύπου έως 250Α"]
["3VA1225-5GF42-0AA0","circuit breaker 3VA1 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection TM240, ATAM, In=250A overload protection Ir=175A...250A short-circuit protection Ii=5...10 x In N conductor protection 100% nut keeper kit",1004.4,"ΤΕΜ",1,"EP",1,"3VA12255GF420AA0","3VA12 Διακότπες ισχύος κλειστού τύπου έως 250Α"]
["3VA1225-6EF32-0LA0","circuit breaker 3VA1 IEC frame 250 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM240, ATAM, In=250A overload protection Ir=175A...250A short-circuit protection Ii=5...10 x In nut keeper kit circuit breaker 3VA1 IEC frame 250 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM240, ATAM, In=250A overload protection Ir=175A...250A short-circuit protection Ii=5...10 x In nut UNIVERSAL RELEASE 24 V DC ACCESSORY FOR 3VA1 and 3VA20 up",1111.5,"ΤΕΜ",1,"EP",1,"3VA12256EF320LA0","3VA12 Διακότπες ισχύος κλειστού τύπου έως 250Α"]
["3VA1225-6EF42-0HH0","circuit breaker 3VA1 IEC frame 250 breaking capacity class H Icu=70kA @ 415V 4-pole, line protection TM240, ATAM, In=250A overload protection Ir=175A...250A short-circuit protection Ii=5...10 x In N conductor unprotected nut keeper kit shunt trip (STL) 12-30V DC; 24V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",1339,"ΤΕΜ",1,"EP",1,"3VA12256EF420HH0","3VA12 Διακότπες ισχύος κλειστού τύπου έως 250Α"]
["3VA1325-7MH32-0AH0","circuit breaker 3VA1 IEC frame 400 breaking capacity class C Icu=110kA @ 415 V 3-pole, starter protection TM120M,  AM, In=250A without overload protection short-circuit protection Ii=8...16 x In nut keeper kit circuit breaker 3VA1 IEC frame 400 breaking capacity class C Icu=110kA @ 415 V 3-pole, starter protection TM120M,  AM, In=250A without overload protection short-circuit protection Ii=8...16 x In nut 2 AUXILIARY SWITCH CHANGEOVER H 1 TRIP ALARM SWITCH CHANGEOVER",1748.5,"ΤΕΜ",1,"EP",1,"3VA13257MH320AH0","3VA13 Διακόπτες ισχύος κλειστού τύπου έως 400Α"]
["3VA1340-4EF42-0AH0","circuit breaker 3VA1 IEC frame 400 breaking capacity class S Icu=36kA @ 415V 4-pole, line protection TM240, ATAM, In=400A overload protection Ir=280A...400A short-circuit protection Ii=5...10 x In N conductor unprotected nut keeper kit circuit breaker 3VA1 IEC frame 400 breaking capacity class S Icu=36kA @ 415V 4-pole, line protection TM240, ATAM, In=400A overload protection Ir=280A...400A short-circuit 2 AUXILIARY SWITCH CHANGEOVER H 1 TRIP ALARM SWITCH CHANGEOVER",1314.4,"ΤΕΜ",1,"EP",1,"3VA13404EF420AH0","3VA13 Διακόπτες ισχύος κλειστού τύπου έως 400Α"]
["3VA1450-6EF32-0AC0","circuit breaker 3VA1 IEC frame 630 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM240, ATAM, In=500A overload protection Ir=350A...500A short-circuit protection Ii=5...10 x In nut keeper kit circuit breaker 3VA1 IEC frame 630 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM240, ATAM, In=500A overload protection Ir=350A...500A short-circuit protection Ii=5...10 x In nut 2 AUXILIARY SWITCH CHANGEOVER H",1630.6,"ΤΕΜ",1,"EP",1,"3VA14506EF320AC0","3VA14 Διακόπτες ισχύος κλειστού τύπου έως 630Α"]
["3VA1463-5EF32-0DH0","circuit breaker 3VA1 IEC frame 630 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=630A overload protection Ir=441A...630A short-circuit protection Ii=4...8 x In nut keeper kit circuit breaker 3VA1 IEC frame 630 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=630A overload protection Ir=441A...630A short-circuit protection Ii=4...8 x In nut UNDERVOLTAGE RELEASE 208-230 V AC 50/60 HZ ACCESSORY FOR 3VA1 2 AUXILIARY SWITCH CHANGEOVER H 1 TRIP ALARM SWITCH CHANGEOVER",1661.6,"ΤΕΜ",1,"EP",1,"3VA14635EF320DH0","3VA14 Διακόπτες ισχύος κλειστού τύπου έως 630Α"]
["3VA1463-6EF32-0AG0","circuit breaker 3VA1 IEC frame 630 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM240, ATAM, In=630A overload protection Ir=440A...630A short-circuit protection Ii=4...8 x In nut keeper kit circuit breaker 3VA1 IEC frame 630 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM240, ATAM, In=630A overload protection Ir=440A...630A short-circuit protection Ii=4...8 x In nut 1 AUXILIARY SWITCH CHANGEOVER H 1 TRIP ALARM SWITCH CHANGEOVER",1767,"ΤΕΜ",1,"EP",1,"3VA14636EF320AG0","3VA14 Διακόπτες ισχύος κλειστού τύπου έως 630Α"]
["3VA1563-5EF42-0AA0","circuit breaker 3VA1 IEC frame 1000 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection TM240, ATAM, In=630A overload protection Ir=440A...630A short-circuit protection Ii=5...10 x In N conductor unprotected nut keeper kit",2064.6,"ΤΕΜ",1,"EP",1,"3VA15635EF420AA0","3VA15 Διακόπτες ισχύος κλειστού τύπου έως 1000Α"]
["3VA2010-5HL32-0DH0","circuit breaker 3VA2 IEC frame 100 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU320, LI, In=100A overload protection Ir=40A...100A short-circuit protection Ii=1.5...12 x In nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",615.66,"ΤΕΜ",1,"EP",1,"3VA20105HL320DH0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2010-5HL36-0DL0","circuit breaker 3VA2 IEC frame 100 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU320, LI, In=100A overload protection Ir=40A...100A short-circuit protection Ii=1.5...12 x In clamp connection undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",669.6,"ΤΕΜ",1,"EP",1,"3VA20105HL360DL0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2010-5HN32-0DH0","circuit breaker 3VA2 IEC frame 100 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU350, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",669.6,"ΤΕΜ",1,"EP",1,"3VA20105HN320DH0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2010-5HN36-0HL0","circuit breaker 3VA2 IEC frame 100 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU350, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In clamp connection shunt trip (STL) 12-30V DC, 24V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",694.4,"ΤΕΜ",1,"EP",1,"3VA20105HN360HL0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2010-5KP32-0AD0","circuit breaker 3VA2 IEC frame 100 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU850, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer nut keeper kit 3 auxiliary switches HQ",1122.2,"ΤΕΜ",1,"EP",1,"3VA20105KP320AD0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2010-6HN32-0DA0","circuit breaker 3VA2 IEC frame 100 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU350, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz",657.2,"ΤΕΜ",1,"EP",1,"3VA20106HN320DA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2010-6HN36-0AE0","circuit breaker 3VA2 IEC frame 100 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU350, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In clamp connection 4 auxiliary switches HQ",663.4,"ΤΕΜ",1,"EP",1,"3VA20106HN360AE0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2010-7KP42-0AA0","circuit breaker 3VA2 IEC frame 100 breaking capacity class C Icu=110kA @ 415V 4-pole, line protection ETU850, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection adjustable (OFF, up to 100%) nut keeper kit",1302,"ΤΕΜ",1,"EP",1,"3VA20107KP420AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2025-5HM36-0AA0","circuit breaker 3VA2 IEC frame 100 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU330, LIG, In=25A overload protection Ir=10A...25A short-circuit protection Ii=1.5...12 x In ground-fault protection Ig=0.6... 1 x In, tg=0.1/0.3s clamp connection",663.4,"ΤΕΜ",1,"EP",1,"3VA20255HM360AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2025-7HL32-0AA0","circuit breaker 3VA2 IEC frame 100 breaking capacity class C Icu=110kA @ 415V 3-pole, line protection ETU320, LI, In=25A overload protection Ir=10A...25A short-circuit protection Ii=1.5...12 x In nut keeper kit",499.72,"ΤΕΜ",1,"EP",1,"3VA20257HL320AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2040-5HM42-0AA0","circuit breaker 3VA2 IEC frame 100 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection ETU330, LIG, In=40A overload protection Ir=16A...40A short-circuit protection Ii=1.5...12 x In N conductor protection adjustable (OFF, 100%) ground-fault protection Ig=0.4...1 x In= tg=0.1/0.3s nut keeper kit",762.6,"ΤΕΜ",1,"EP",1,"3VA20405HM420AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2040-5KP42-0AA0","circuit breaker 3VA2 IEC frame 100 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection ETU850, LSI, In=40A overload protection Ir=16A...40A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection adjustable (OFF, up to 160%) nut keeper kit",1140.8,"ΤΕΜ",1,"EP",1,"3VA20405KP420AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2040-8HN36-0AA0","circuit breaker 3VA2 IEC frame 100 breaking capacity class L Icu=150kA @ 415V 3-pole, line protection ETU350, LSI, In=40A overload protection Ir=16A...40A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In clamp connection",638.6,"ΤΕΜ",1,"EP",1,"3VA20408HN360AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2063-5HL32-0CC0","circuit breaker 3VA2 IEC frame 100 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU320, LI, In=63A overload protection Ir=25A...63A short-circuit protection Ii=1.5...12 x In nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ",560.48,"ΤΕΜ",1,"EP",1,"3VA20635HL320CC0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2063-5HN32-0HH0","circuit breaker 3VA2 IEC frame 100 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU350, LSI, In=63A overload protection Ir=25A...63A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In nut keeper kit shunt trip (STL) 12-30V DC, 24V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",613.79999999999995,"ΤΕΜ",1,"EP",1,"3VA20635HN320HH0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2063-5HN36-0KL0","circuit breaker 3VA2 IEC frame 100 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU350, LSI, In=63A overload protection Ir=25A...63A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In clamp connection shunt trip (STL) 220-250V DC, 208-277V AC 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",663.4,"ΤΕΜ",1,"EP",1,"3VA20635HN360KL0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2063-5KP32-0AB0","circuit breaker 3VA2 IEC frame 100 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU850, LSI, In=63A overload protection Ir=25A...63A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer nut keeper kit 2 auxiliary switches HP",1097.4000000000001,"ΤΕΜ",1,"EP",1,"3VA20635KP320AB0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2063-6HL32-0CA0","circuit breaker 3VA2 IEC frame 100 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU320, LI, In=63A overload protection Ir=25A...63A short-circuit protection Ii=1.5...12 x In nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz",566.05999999999995,"ΤΕΜ",1,"EP",1,"3VA20636HL320CA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2063-6HN32-0CL0","circuit breaker 3VA2 IEC frame 100 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU350, LSI, In=63A overload protection Ir=25A...63A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",706.8,"ΤΕΜ",1,"EP",1,"3VA20636HN320CL0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2063-8HN32-0AA0","circuit breaker 3VA2 IEC frame 100 breaking capacity class L Icu=150kA @ 415V 3-pole, line protection ETU350, LSI, In=63A overload protection Ir=25A...63A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In nut keeper kit",615.04,"ΤΕΜ",1,"EP",1,"3VA20638HN320AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2110-5HL32-0HC0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU320, LI, In=100A overload protection Ir=40A...100A short-circuit protection Ii=1.5...12 x In nut keeper kit shunt trip (STL) 12-30V DC, 24V AC 50/60Hz 2 auxiliary switches HQ",573.5,"ΤΕΜ",1,"EP",1,"3VA21105HL320HC0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2110-5HL36-0KL0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU320, LI, In=100A overload protection Ir=40A...100A short-circuit protection Ii=1.5...12 x In clamp connection shunt trip (STL) 220-250V DC, 208-277V AC 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",644.79999999999995,"ΤΕΜ",1,"EP",1,"3VA21105HL360KL0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2110-5HN36-0DC0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU350, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In clamp connection undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ",669.6,"ΤΕΜ",1,"EP",1,"3VA21105HN360DC0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2110-5JQ32-0AB0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU560, LSIG, In=100A overload protection Ir=40A...100A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer gr.-fault prot., can be sw. off Ig=0.2...1 x In, tg=0.05-0.8s nut keeper kit 2 auxiliary switches HP",1153.2,"ΤΕΜ",1,"EP",1,"3VA21105JQ320AB0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2110-5JQ32-0HC0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU560, LSIG, In=100A overload protection Ir=40A...100A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer gr.-fault prot., can be sw. off Ig=0.2...1 x In, tg=0.05-0.8s nut keeper kit shunt trip (STL) 12-30V DC; 24V AC 50/60Hz 2 auxiliary switches HQ",1196.5999999999999,"ΤΕΜ",1,"EP",1,"3VA21105JQ320HC0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2110-5MN36-0AG0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, motor protection ETU350M, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=3...15 x Ir, Ii=15 x In clamp connection 1 auxiliary switch HP 1 trip alarm switch HP",566.05999999999995,"ΤΕΜ",1,"EP",1,"3VA21105MN360AG0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2110-5MN36-0KC0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, motor protection ETU350M, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=3...15 x Ir, Ii=15 x In clamp connection shunt trip (STL) 220-250V DC, 208-277V AC 2 auxiliary switches HQ",620,"ΤΕΜ",1,"EP",1,"3VA21105MN360KC0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2110-6HN32-0DL0","circuit breaker 3VA2 IEC frame 160 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU350, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",762.6,"ΤΕΜ",1,"EP",1,"3VA21106HN320DL0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2110-6HN36-0AF0","circuit breaker 3VA2 IEC frame 160 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU350, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In clamp connection 1 auxiliary switch HQ 1 trip alarm switch HQ",620,"ΤΕΜ",1,"EP",1,"3VA21106HN360AF0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2110-7MN32-0HA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class C Icu=110kA @ 415V 3-pole, motor protection ETU350M, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=3...15 x Ir, Ii=15 x In nut keeper kit shunt trip (STL) 12-30V DC, 24V AC 50/60Hz",638.6,"ΤΕΜ",1,"EP",1,"3VA21107MN320HA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2110-7MN36-0BA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class C Icu=110kA @ 415V 3-pole, motor protection ETU350M, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=3...15 x Ir, Ii=15 x In clamp connection undervoltage release (UVR) 24V DC",682,"ΤΕΜ",1,"EP",1,"3VA21107MN360BA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2110-7MS36-0CH0","circuit breaker 3VA2 IEC frame 160 breaking capacity class C Icu=110kA @ 415V 3-pole, starter protection ETU310M, I, In=100A overload protection Ir=40A...100A short-circuit protection Ii=3...15 x In clamp connection undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",587.76,"ΤΕΜ",1,"EP",1,"3VA21107MS360CH0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2110-8JQ46-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class L Icu=150kA @ 415V 4-pole, line protection ETU560, LSIG, In=100A overload protection Ir=40A...100A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection adjustable (OFF, up to 160%) gr.-fault prot., can be sw. off Ig=0.2...1 x In= tg=0.05-0.8s clamp connection",1463.2,"ΤΕΜ",1,"EP",1,"3VA21108JQ460AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2116-5HL36-0AH0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU320, LI, In=160A overload protection Ir=63A...160A short-circuit protection Ii=1.5...10 x In clamp connection 2 auxiliary switches HQ 1 trip alarm switch HQ",775,"ΤΕΜ",1,"EP",1,"3VA21165HL360AH0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2116-5HN32-0AG0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU350, LSI, In=160A overload protection Ir=63A...160A short-circuit protection Isd=1.5...10 x Ir, Ii=10 x In nut keeper kit 1 auxiliary switch HP 1 trip alarm switch HP",799.8,"ΤΕΜ",1,"EP",1,"3VA21165HN320AG0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2116-5HN42-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection ETU350, LSI, In=160A overload protection Ir=63A...160A short-circuit protection Isd=1.5...10 x Ir, Ii=10 x In N conductor protection adjustable (OFF, 50%, 100%) nut keeper kit",942.4,"ΤΕΜ",1,"EP",1,"3VA21165HN420AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2116-5KP32-0AB0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU850, LSI, In=160A overload protection Ir=63A...160A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection optionally with external current transformer nut keeper kit 2 auxiliary switches HP",1351.6,"ΤΕΜ",1,"EP",1,"3VA21165KP320AB0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2116-5KP32-0HA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU850, LSI, In=160A overload protection Ir=63A...160A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection optionally with external current transformer nut keeper kit shunt trip (STL) 12-30V DC; 24V AC 50/60Hz",1357.8,"ΤΕΜ",1,"EP",1,"3VA21165KP320HA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2116-6HL32-0HL0","circuit breaker 3VA2 IEC frame 160 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU320, LI, In=160A overload protection Ir=63A...160A short-circuit protection Ii=1.5...10 x In nut keeper kit shunt trip (STL) 12-30V DC, 24V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",942.4,"ΤΕΜ",1,"EP",1,"3VA21166HL320HL0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2116-6KQ42-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class H Icu=85kA @ 415V 4-pole, line protection ETU860, LSIG, In=160A overload protection Ir=63A...160A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection adjustable (OFF, up to 100%) gr.-fault prot., can be sw. off Ig=0.2...1 x In= tg=0.05-0.8s nut keeper kit",1729.8,"ΤΕΜ",1,"EP",1,"3VA21166KQ420AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2125-0HN32-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class  E Icu=200 kA @ 415 V 3-pole, line protection ETU350,  LSI, In=25A overload protection Ir=10A ... 25A short circuit protection Isd=1,5...10xIr, Ii=12xIn busbar connection",682,"ΤΕΜ",1,"EP",1,"3VA21250HN320AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2125-5HL36-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU320, LI, In=25A overload protection Ir=10A...25A short-circuit protection Ii=1.5...12 x In clamp connection",442.68,"ΤΕΜ",1,"EP",1,"3VA21255HL360AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2125-6HL46-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class H Icu=85kA @ 415V 4-pole, line protection ETU320, LI, In=25A overload protection Ir=10A...25A short-circuit protection Ii=1.5...12 x In N conductor protection adjustable (OFF, 100%) clamp connection",626.20000000000005,"ΤΕΜ",1,"EP",1,"3VA21256HL460AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2125-8HL32-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class L Icu=150kA @ 415V 3-pole, line protection ETU320, LI, In=25A overload protection Ir=10A...25A short-circuit protection Ii=1.5...12 x In nut keeper kit",562.34,"ΤΕΜ",1,"EP",1,"3VA21258HL320AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2140-5KQ32-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU860, LSIG, In=40A overload protection Ir=16A...40A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% gr.-fault prot., can be sw. off Ig=0.4... 1 x In, tg=0.05-0.8s nut keeper kit",1153.2,"ΤΕΜ",1,"EP",1,"3VA21405KQ320AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2140-5MN32-0KL0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, motor protection ETU350M, LSI, In=40A overload protection Ir=16A...40A short-circuit protection Isd=3...15 x Ir, Ii=15 x In nut keeper kit shunt trip (STL) 220-250V DC, 208-277V AC 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",632.4,"ΤΕΜ",1,"EP",1,"3VA21405MN320KL0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2140-6HN42-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class H Icu=85kA @ 415V 4-pole, line protection ETU350, LSI, In=40A overload protection Ir=16A...40A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In N conductor protection adjustable (OFF, 100%) nut keeper kit",651,"ΤΕΜ",1,"EP",1,"3VA21406HN420AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2140-7MQ36-0AD0","circuit breaker 3VA2 IEC frame 160 breaking capacity class C Icu=110kA @ 415V 3-pole, motor protection ETU860M, LSIG, In=40A overload protection Ir=16A...40A short-circuit protection Isd=1.2..15x In, Ii=3..15x In gr.-fault prot., can be sw. off Ig=0.4... 1 x In, tg=0.05-0.8s clamp connection circuit breaker 3VA2 IEC frame 160 3 auxiliary switches HQ",1047.8,"ΤΕΜ",1,"EP",1,"3VA21407MQ360AD0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2163-0MN36-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class  E Icu=200 kA @ 415 V 3-pole motor protection ETU350M,  LSI, In=63A overload protection Ir=25A ... 63A short circuit protection Isd=3...15xIr, Ii=15xIn cable connection",611.32000000000005,"ΤΕΜ",1,"EP",1,"3VA21630MN360AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2163-5HN32-0CA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU350, LSI, In=63A overload protection Ir=25A...63A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz",573.5,"ΤΕΜ",1,"EP",1,"3VA21635HN320CA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2163-5HN36-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU350, LSI, In=63A overload protection Ir=25A...63A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In clamp connection",494.76,"ΤΕΜ",1,"EP",1,"3VA21635HN360AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2163-5JQ32-0AF0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU560, LSIG, In=63A overload protection Ir=25A...63A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer gr.-fault prot., can be sw. off Ig=0.25...1 x In, tg=0.05-0.8s nut keeper kit 1 auxiliary switch HQ 1 trip alarm switch HQ",1116,"ΤΕΜ",1,"EP",1,"3VA21635JQ320AF0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2163-5KP32-0BL0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU850, LSI, In=63A overload protection Ir=25A...63A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer nut keeper kit undervoltage release (UVR) 24V DC 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",1221.4000000000001,"ΤΕΜ",1,"EP",1,"3VA21635KP320BL0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2163-5MN32-0JC0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, motor protection ETU350M, LSI, In=63A overload protection Ir=25A...63A short-circuit protection Isd=3...15 x Ir, Ii=15 x In nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ",579.70000000000005,"ΤΕΜ",1,"EP",1,"3VA21635MN320JC0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2163-5MQ32-0AB0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, motor protection ETU860M, LSIG, In=63A overload protection Ir=25A...63A short-circuit protection Isd=1.2..15x In, Ii=3..15x In gr.-fault prot., can be sw. off Ig=0.25...1 x In, tg=0.05-0.8s 2 auxiliary switches HP",948.6,"ΤΕΜ",1,"EP",1,"3VA21635MQ320AB0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2163-6HL36-0AD0","circuit breaker 3VA2 IEC frame 160 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU320, LI, In=63A overload protection Ir=25A...63A short-circuit protection Ii=1.5...12 x In clamp connection 3 auxiliary switches HQ",552.41999999999996,"ΤΕΜ",1,"EP",1,"3VA21636HL360AD0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2163-6HN36-0DH0","circuit breaker 3VA2 IEC frame 160 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU350, LSI, In=63A overload protection Ir=25A...63A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In clamp connection undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",700.6,"ΤΕΜ",1,"EP",1,"3VA21636HN360DH0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2163-6KQ46-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class H Icu=85kA @ 415V 4-pole, line protection ETU860, LSIG, In=63A overload protection Ir=25A...63A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection adjustable (OFF, up to 160%) gr.-fault prot., can be sw. off Ig=0.25...1 x In= tg=0.05-0.8s clamp connection",1351.6,"ΤΕΜ",1,"EP",1,"3VA21636KQ460AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2163-7MN32-0BC0","circuit breaker 3VA2 IEC frame 160 breaking capacity class C Icu=110kA @ 415V 3-pole, motor protection ETU350M, LSI, In=63A overload protection Ir=25A...63A short-circuit protection Isd=3...15 x Ir, Ii=15 x In nut keeper kit undervoltage release (UVR) 24V DC",675.8,"ΤΕΜ",1,"EP",1,"3VA21637MN320BC0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2163-7MN32-0KH0","circuit breaker 3VA2 IEC frame 160 breaking capacity class C Icu=110kA @ 415V 3-pole, motor protection ETU350M, LSI, In=63A overload protection Ir=25A...63A short-circuit protection Isd=3...15 x Ir, Ii=15 x In nut keeper kit shunt trip (STL) 220-250V DC, 208-277V AC 2 auxiliary switches HQ 1 trip alarm switch HQ",675.8,"ΤΕΜ",1,"EP",1,"3VA21637MN320KH0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2163-7MS32-0JL0","circuit breaker 3VA2 IEC frame 160 breaking capacity class C Icu=110kA @ 415V 3-pole, starter protection ETU310M, I, In=63A overload protection Ir=25A...63A short-circuit protection Ii=3...15 x In nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",550.55999999999995,"ΤΕΜ",1,"EP",1,"3VA21637MS320JL0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2163-8HN42-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class L Icu=150kA @ 415V 4-pole, line protection ETU350, LSI, In=63A overload protection Ir=25A...63A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In N conductor protection adjustable (OFF, 100%) nut keeper kit",781.2,"ΤΕΜ",1,"EP",1,"3VA21638HN420AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2216-5MN32-0AC0","circuit breaker 3VA2 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 3-pole, motor protection ETU350M, LSI, In=160A overload protection Ir=63A...160A short-circuit protection Isd=3...15 x Ir, Ii=15 x In nut keeper kit 2 auxiliary switches HQ",837,"ΤΕΜ",1,"EP",1,"3VA22165MN320AC0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2216-6HN32-0AJ0","circuit breaker 3VA2 IEC frame 250 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU350, LSI, In=160A overload protection Ir=63A...160A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In nut keeper kit 2 auxiliary switches HP 1 trip alarm switch HP",1153.2,"ΤΕΜ",1,"EP",1,"3VA22166HN320AJ0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2216-7MQ32-0AA0","circuit breaker 3VA2 IEC frame 250 breaking capacity class C Icu=110kA @ 415V 3-pole, motor protection ETU860M, LSIG, In=160A overload protection Ir=63A...160A short-circuit protection Isd=1.2..15x In, Ii=3..15x In gr.-fault prot., can be sw. off Ig=0.2...1 x In, tg=0.05-0.8s nut keeper kit",1351.6,"ΤΕΜ",1,"EP",1,"3VA22167MQ320AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2220-5MN32-0DB0","circuit breaker 3VA2 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 3-pole, motor protection ETU350M, LSI, In=200A overload protection Ir=80A...200A short-circuit protection Isd=3...15 x Ir, Ii=15 x In nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HP",1085,"ΤΕΜ",1,"EP",1,"3VA22205MN320DB0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2220-7MP32-0DA0","CIRCUIT BREAKER 3VA2 IEC FRAME 250 BREAKING CAPACITY CLASS  C ICU=110KA @ 415 V 3-POLE, MOTOR PROTECTION ETU550M,  LSI, In=200A OVERLOAD PROTECTION IR=80A ...200A SHORT CIRCUIT PROTECTION ISD=1,2... 15X IN,II=3...15X IN BUSBAR CONNECTION CIRCUIT BREAKER 3VA2 IEC FRAME 250 BREAKING CAPACITY CLASS  C ICU=110KA @ 415 V 3-POLE, MOTOR PROTECTION ETU550M,  LSI, In=200A OVERLOAD PROTECTION IR=80A ...200A SHORT CIRCUIT UNDERVOLTAGE RELEASE 208-230 V AC 50/60 HZ ACCESSORY FOR 3VA1",2238.1999999999998,"ΤΕΜ",1,"EP",1,"3VA22207MP320DA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2220-7MS32-0KL0","circuit breaker 3VA2 IEC frame 250 breaking capacity class C Icu=110kA @ 415V 3-pole, starter protection ETU310M, I, In=200A overload protection Ir=80A...200A short-circuit protection Ii=3...15 x In nut keeper kit shunt trip (STL) 220-250V DC, 208-277V AC 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",1097.4000000000001,"ΤΕΜ",1,"EP",1,"3VA22207MS320KL0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2225-5HL32-0JH0","circuit breaker 3VA2 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU320, LI, In=250A overload protection Ir=100A...250A short-circuit protection Ii=1.5...10 x In nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",1029.2,"ΤΕΜ",1,"EP",1,"3VA22255HL320JH0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2225-5HN42-0BB0","circuit breaker 3VA2 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection ETU350, LSI, In=250A overload protection Ir=100A...250A short-circuit protection Isd=1.5...10 x Ir, Ii=10 x In N conductor protection adjustable (OFF, 50%, 100%) nut keeper kit circuit breaker 3VA2 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection ETU350, LSI, In=250A overload protection UNDERVOLTAGE RELEASE 24 V DC ACCESSORY FOR 3VA1 and 3VA20 up 2 AUXILIARY SWITCH CHANGEOVER H",1382.6,"ΤΕΜ",1,"EP",1,"3VA22255HN420BB0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2225-5JP32-0AB0","circuit breaker 3VA2 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU550, LSI, In=250A overload protection Ir=100A...250A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection optionally with external current transformer nut keeper kit 2 auxiliary switches HP",1376.4,"ΤΕΜ",1,"EP",1,"3VA22255JP320AB0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2225-5JQ42-0AA0","circuit breaker 3VA2 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection ETU560, LSIG, In=250A overload protection Ir=100A...250A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection adjustable (OFF, up to 100%) gr.-fault prot., can be sw. off Ig=0.2...1 x In= tg=0.05-0.8s nut keeper kit",1816.6,"ΤΕΜ",1,"EP",1,"3VA22255JQ420AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2225-5KP32-0BL0","circuit breaker 3VA2 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU850, LSI, In=250A overload protection Ir=100A...250A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection optionally with external current transformer nut keeper kit undervoltage release (UVR) 24V DC 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",1692.6,"ΤΕΜ",1,"EP",1,"3VA22255KP320BL0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2225-6HN32-0JA0","circuit breaker 3VA2 IEC frame 250 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU350, LSI, In=250A overload protection Ir=100A...250A short-circuit protection Isd=1.5...10 x Ir, Ii=10 x In nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz",1134.5999999999999,"ΤΕΜ",1,"EP",1,"3VA22256HN320JA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2225-6JP32-0BA0","circuit breaker 3VA2 IEC frame 250 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU550, LSI, In=250A overload protection Ir=100A...250A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection optionally with external current transformer nut keeper kit undervoltage release (UVR) 24V DC",1531.4,"ΤΕΜ",1,"EP",1,"3VA22256JP320BA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2225-6JQ32-0HC0","circuit breaker 3VA2 IEC frame 250 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU560, LSIG, In=250A overload protection Ir=100A...250A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection optionally with external current transformer gr.-fault prot., can be sw. off Ig=0.2...1 x In, tg=0.05-0.8s nut keeper kit shunt trip (STL) 12-30V DC; 24V AC 50/60Hz 2 auxiliary switches HQ",1767,"ΤΕΜ",1,"EP",1,"3VA22256JQ320HC0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2225-7HL32-0CH0","circuit breaker 3VA2 IEC frame 250 breaking capacity class C Icu=110kA @ 415V 3-pole, line protection ETU320, LI, In=250A overload protection Ir=100A...250A short-circuit protection Ii=1.5...10 x In nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",1252.4000000000001,"ΤΕΜ",1,"EP",1,"3VA22257HL320CH0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2225-7KP32-0AH0","circuit breaker 3VA2 IEC frame 250 breaking capacity class C Icu=110kA @ 415V 3-pole, line protection ETU850, LSI, In=250A overload protection Ir=100A...250A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection optionally with external current transformer nut keeper kit 2 auxiliary switches HQ 1 trip alarm switch HQ",1760.8,"ΤΕΜ",1,"EP",1,"3VA22257KP320AH0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2225-7KP32-0BC0","circuit breaker 3VA2 IEC frame 250 breaking capacity class C Icu=110kA @ 415V 3-pole, line protection ETU850, LSI, In=250A overload protection Ir=100A...250A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection optionally with external current transformer nut keeper kit undervoltage release (UVR) 24V DC 2 auxiliary switches HQ",1841.4,"ΤΕΜ",1,"EP",1,"3VA22257KP320BC0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2225-8HL42-0AA0","circuit breaker 3VA2 IEC frame 250 breaking capacity class L Icu=150kA @ 415V 4-pole, line protection ETU320, LI, In=250A overload protection Ir=100A...250A short-circuit protection Ii=1.5...10 x In N conductor protection adjustable (OFF, 50%, 100%) nut keeper kit",1649.2,"ΤΕΜ",1,"EP",1,"3VA22258HL420AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2325-5HN32-0AE0","circuit breaker 3VA2 IEC frame 400 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU350, LSI, In=250A overload protection Ir=100A...250A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In nut keeper kit 4 auxiliary switches HQ",1351.6,"ΤΕΜ",1,"EP",1,"3VA23255HN320AE0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2325-5MN32-0AC0","circuit breaker 3VA2 IEC frame 400 breaking capacity class M Icu=55kA @ 415V 3-pole, motor protection ETU350M, LSI, In=250A overload protection Ir=100A...250A short-circuit protection Isd=3...15 x Ir, Ii=15 x In nut keeper kit 2 auxiliary switches HQ",1351.6,"ΤΕΜ",1,"EP",1,"3VA23255MN320AC0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2325-5MQ32-0LD0","circuit breaker 3VA2 IEC frame 400 breaking capacity class M Icu=55kA @ 415V 3-pole, motor protection ETU860M, LSIG, In=250A overload protection Ir=100A...250A short-circuit protection Isd=1.2..15x In, Ii=3..15x In gr.-fault prot., can be sw. off Ig=0.2...1 x In, tg=0.05-0.8s nut keeper kit circuit breaker 3VA2 IEC frame 400 universal release 24V DC 3 auxiliary switches HQ",1965.4,"ΤΕΜ",1,"EP",1,"3VA23255MQ320LD0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2325-6HN32-0CH0","circuit breaker 3VA2 IEC frame 400 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU350, LSI, In=250A overload protection Ir=100A...250A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",1599.6,"ΤΕΜ",1,"EP",1,"3VA23256HN320CH0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2325-8HM42-0AA0","circuit breaker 3VA2 IEC frame 400 breaking capacity class L Icu=150kA @ 415V 4-pole, line protection ETU330, LIG, In=250A overload protection Ir=100A...250A short-circuit protection Ii=1.5...12 x In N conductor protection adjustable (OFF, 50%, 100%) ground-fault protection Ig=0.2...1 x In= tg=0.1/0.3s nut keeper kit",2405.6,"ΤΕΜ",1,"EP",1,"3VA23258HM420AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2340-5HL32-0AC0","circuit breaker 3VA2 IEC frame 400 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU320, LI, In=400A overload protection Ir=160A...400A short-circuit protection Ii=1.5...10 x In nut keeper kit 2 auxiliary switches HQ",1221.4000000000001,"ΤΕΜ",1,"EP",1,"3VA23405HL320AC0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2340-5HL42-0AD0","circuit breaker 3VA2 IEC frame 400 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection ETU320, LI, In=400A overload protection Ir=160A...400A short-circuit protection Ii=1.5...10 x In N conductor protection adjustable (OFF, 50%, 100%) nut keeper kit 3 auxiliary switches HQ",1618.2,"ΤΕΜ",1,"EP",1,"3VA23405HL420AD0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2340-5HN32-0KJ0","circuit breaker 3VA2 IEC frame 400 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU350, LSI, In=400A overload protection Ir=160A...400A short-circuit protection Isd=1.5...10 x Ir, Ii=10 x In nut keeper kit circuit breaker 3VA2 IEC frame 400 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU350, LSI, In=400A overload protection Ir=160A...400A short-circuit protection Isd=1.5...10 x Ir, SHUNT TRIP LEFT 208-277 V AC 50/60 HZ 220-250 V DC ACCESSORY 2 AUXILIARY SWITCH CHANGEOVER H 1 TRIP ALARM SWITCH CHANGEOVER",1432.2,"ΤΕΜ",1,"EP",1,"3VA23405HN320KJ0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2340-5JP32-0DC0","circuit breaker 3VA2 IEC frame 400 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU550, LSI, In=400A overload protection Ir=160A...400A short-circuit protection Isd=0.6...10 x In, Ii=1.5 x In N conductor protection optionally with external current transformer, up to 160% nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ",1779.4,"ΤΕΜ",1,"EP",1,"3VA23405JP320DC0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2340-5JQ42-0BH0","circuit breaker 3VA2 IEC frame 400 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection ETU560, LSIG, In=400A overload protection Ir=160A...400A short-circuit protection Isd=0.6...10 x In, Ii=1.5 x In N conductor protection adjustable (OFF, up to 100%) gr.-fault prot., can be sw. off Ig=0.2...1 x In= tg=0.05-0.8s nut keeper kit undervoltage release (UVR) 24V DC 2 auxiliary switches HQ 1 trip alarm switch HQ",2387,"ΤΕΜ",1,"EP",1,"3VA23405JQ420BH0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2340-5JQ42-0KL0","circuit breaker 3VA2 IEC frame 400 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection ETU560, LSIG, In=400A overload protection Ir=160A...400A short-circuit protection Isd=0.6...10 x In, Ii=1.5 x In N conductor protection adjustable (OFF, up to 100%) gr.-fault prot., can be sw. off Ig=0.2...1 x In= tg=0.05-0.8s nut keeper kit shunt trip (STL) 220-250V DC; 208-277V AC 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",2393.1999999999998,"ΤΕΜ",1,"EP",1,"3VA23405JQ420KL0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2340-6HL32-0DC0","circuit breaker 3VA2 IEC frame 400 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU320, LI, In=400A overload protection Ir=160A...400A short-circuit protection Ii=1.5...10 x In nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ",1481.8,"ΤΕΜ",1,"EP",1,"3VA23406HL320DC0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2340-6HN42-0KA0","circuit breaker 3VA2 IEC frame 400 breaking capacity class H Icu=85kA @ 415V 4-pole, line protection ETU350, LSI, In=400A overload protection Ir=160A...400A short-circuit protection Isd=1.5...10 x Ir, Ii=10 x In N conductor protection adjustable (OFF, 50%, 100%) nut keeper kit circuit breaker 3VA2 IEC frame 400 breaking capacity class H Icu=85kA @ 415V 4-pole, line protection ETU350, LSI, In=400A overload protection SHUNT TRIP LEFT 208-277 V AC 50/60 HZ 220-250 V DC ACCESSORY",1934.4,"ΤΕΜ",1,"EP",1,"3VA23406HN420KA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2340-6JQ42-0DJ0","circuit breaker 3VA2 IEC frame 400 breaking capacity class H Icu=85kA @ 415V 4-pole, line protection ETU560, LSIG, In=400A overload protection Ir=160A...400A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection adjustable (OFF, up to 100%) gr.-fault prot., can be sw. off Ig=0.2...1 x In= tg=0.05-0.8s nut keeper kit undervoltage release 208-230V AC 50/60Hz 2 auxiliary switches 1 trip alarm switch",2635,"ΤΕΜ",1,"EP",1,"3VA23406JQ420DJ0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2340-7HL32-0AD0","circuit breaker 3VA2 IEC frame 400 breaking capacity class C Icu=110kA @ 415V 3-pole, line protection ETU320, LI, In=400A overload protection Ir=160A...400A short-circuit protection Ii=1.5...10 x In nut keeper kit 3 auxiliary switches HQ",1506.6,"ΤΕΜ",1,"EP",1,"3VA23407HL320AD0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2340-7KQ32-0AA0","circuit breaker 3VA2 IEC frame 400 breaking capacity class C Icu=110kA @ 415V 3-pole, line protection ETU860, LSIG, In=400A overload protection Ir=160A...400A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection optionally with external current transformer, up to 160% gr.-fault prot., can be sw. off Ig=0.2...1 x In, tg=0.05-0.8s nut keeper kit",2194.8000000000002,"ΤΕΜ",1,"EP",1,"3VA23407KQ320AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2440-5HK42-0AA0","circuit breaker 3VA2 IEC frame 630 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection ETU340, ELISA LI, In=400A overload protection Ir=160A...400A short-circuit protection Ii=15 x In N conductor protection adjustable (OFF, 50%, 100%) nut keeper kit",2114.1999999999998,"ΤΕΜ",1,"EP",1,"3VA24405HK420AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2440-5JP42-0AA0","circuit breaker 3VA2 IEC frame 630 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection ETU550, LSI, In=400A overload protection Ir=160A...400A short-circuit protection Isd=0.6..10x In, Ii=1.5..15x In N conductor protection adjustable (OFF, up to 130%) nut keeper kit",2560.6,"ΤΕΜ",1,"EP",1,"3VA24405JP420AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2440-5MP32-0AF0","CIRCUIT BREAKER 3VA2 IEC FRAME 630 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3-POLE, MOTOR PROTECTION ETU550M,  LSI, In=400A OVERLOAD PROTECTION IR=160A ...400A SHORT CIRCUIT PROTECTION ISD=1,2... 15X IN,II=3...15X IN BUSBAR CONNECTION CIRCUIT BREAKER 3VA2 IEC FRAME 630 BREAKING CAPACITY CLASS  M ICU=55KA @ 415 V 3-POLE, MOTOR PROTECTION ETU550M,  LSI, In=400A OVERLOAD PROTECTION IR=160A ...400A SHORT CIRCUIT 1 AUXILIARY SWITCH CHANGEOVER H 1 TRIP ALARM SWITCH CHANGEOVER",1934.4,"ΤΕΜ",1,"EP",1,"3VA24405MP320AF0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2440-6HM32-0AA0","circuit breaker 3VA2 IEC frame 630 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU330, LIG, In=400A overload protection Ir=160A...400A short-circuit protection Ii=1.5...12 x In ground-fault protection Ig=0.2...1 x In, tg=0.1/0.3s nut keeper kit",2052.1999999999998,"ΤΕΜ",1,"EP",1,"3VA24406HM320AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2440-7JQ32-0AA0","circuit breaker 3VA2 IEC frame 630 breaking capacity class C Icu=110kA @ 415V 3-pole, line protection ETU560, LSIG, In=400A overload protection Ir=160A...400A short-circuit protection Isd=0.6..10x In, Ii=1.5..15x In N conductor protection optionally with external current transformer, up to 160% gr.-fault prot., can be sw. off Ig=0.2...1 x In, tg=0.05-0.8s nut keeper kit",2647.4,"ΤΕΜ",1,"EP",1,"3VA24407JQ320AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2450-5KP42-0AA0","circuit breaker 3VA2 IEC frame 630 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection ETU850, LSI, In=500A overload protection Ir=200A...500A short-circuit protection Isd=0.6..10x In, Ii=1.5..14x In N conductor protection adjustable (OFF, up to 100%) nut keeper kit",2752.8,"ΤΕΜ",1,"EP",1,"3VA24505KP420AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2450-5MQ32-0AA0","circuit breaker 3VA2 IEC frame 630 breaking capacity class M Icu=55kA @ 415V 3-pole, motor protection ETU860M, LSIG, In=500A overload protection Ir=200A...500A short-circuit protection Isd=1.2..15x In, Ii=3..15x In gr.-fault prot., can be sw. off Ig=0.2...1 x In, tg=0.05-0.8s nut keeper kit",2269.1999999999998,"ΤΕΜ",1,"EP",1,"3VA24505MQ320AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2450-8HK42-0AA0","circuit breaker 3VA2 IEC frame 630 breaking capacity class L Icu=150kA @ 415V 4-pole, line protection ETU340, ELISA LI, In=500A overload protection Ir=200A...500A short-circuit protection Ii=11 x In N conductor protection adjustable (OFF, 50%, 100%) nut keeper kit",3007,"ΤΕΜ",1,"EP",1,"3VA24508HK420AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2463-5HL32-0JL0","circuit breaker 3VA2 IEC frame 630 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU320, LI, In=630A overload protection Ir=250A...630A short-circuit protection Ii=1.5...9 x In nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",1767,"ΤΕΜ",1,"EP",1,"3VA24635HL320JL0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2463-5HN32-0AE0","circuit breaker 3VA2 IEC frame 630 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU350, LSI, In=630A overload protection Ir=250A...630A short-circuit protection Isd=1.5...9 x Ir, Ii=9 x In nut keeper kit 4 auxiliary switches HQ",1767,"ΤΕΜ",1,"EP",1,"3VA24635HN320AE0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2463-5JP32-0HL0","circuit breaker 3VA2 IEC frame 630 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU550, LSI, In=630A overload protection Ir=250A...630A short-circuit protection Isd=0.6..9 x In, Ii=1.5..9 x In N conductor protection optionally with external current transformer, up to 160% nut keeper kit shunt trip (STL) 12-30V DC; 24V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",2207.1999999999998,"ΤΕΜ",1,"EP",1,"3VA24635JP320HL0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2463-5JQ32-0JL0","circuit breaker 3VA2 IEC frame 630 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU560, LSIG, In=630A overload protection Ir=250A...630A short-circuit protection Isd=0.6..9 x In, Ii=1.5..9 x In N conductor protection, opt. w. ext. curr. transf., up to 160% gr.-fault prot., can be sw. off Ig=0.2...1 x In= tg=0.05-0.8s nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",2442.8000000000002,"ΤΕΜ",1,"EP",1,"3VA24635JQ320JL0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2463-6HL32-0HH0","circuit breaker 3VA2 IEC frame 630 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU320, LI, In=630A overload protection Ir=250A...630A short-circuit protection Ii=1.5...9 x In nut keeper kit shunt trip (STL) 12-30V DC, 24V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",1959.2,"ΤΕΜ",1,"EP",1,"3VA24636HL320HH0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2463-6HN32-0AF0","circuit breaker 3VA2 IEC frame 630 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU350, LSI, In=630A overload protection Ir=250A...630A short-circuit protection Isd=1.5...9 x Ir, Ii=9 x In nut keeper kit 1 auxiliary switch HQ 1 trip alarm switch HQ",1946.8,"ΤΕΜ",1,"EP",1,"3VA24636HN320AF0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2463-6JQ32-0BA0","circuit breaker 3VA2 IEC frame 630 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU560, LSIG, In=630A overload protection Ir=250A...630A short-circuit protection Isd=0.6..9 x In, Ii=1.5..9 x In N conductor protection optionally with external current transformer, up to 160% gr.-fault prot., can be sw. off Ig=0.2...1 x In, tg=0.05-0.8s nut keeper kit undervoltage release (UVR) 24V DC",2585.4,"ΤΕΜ",1,"EP",1,"3VA24636JQ320BA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2463-6KP32-0CA0","circuit breaker 3VA2 IEC frame 630 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU850, LSI, In=630A overload protection Ir=250A...630A short-circuit protection Isd=0.6..9 x In, Ii=1.5..9 x In N conductor protection optionally with external current transformer, up to 160% nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz",2548.1999999999998,"ΤΕΜ",1,"EP",1,"3VA24636KP320CA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2463-7HL32-0CC0","circuit breaker 3VA2 IEC frame 630 breaking capacity class C Icu=110kA @ 415V 3-pole, line protection ETU320, LI, In=630A overload protection Ir=250A...630A short-circuit protection Ii=1.5...9 x In nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ",2108,"ΤΕΜ",1,"EP",1,"3VA24637HL320CC0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2510-5HL32-0AC0","circuit breaker 3VA2 IEC frame 1000 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU320, LI, In=1000A overload protection Ir=400A...1000A short-circuit protection Ii=1.5...10 x In nut keeper kit 2 auxiliary switches HQ",3100,"ΤΕΜ",1,"EP",1,"3VA25105HL320AC0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2510-5HL32-0AG0","circuit breaker 3VA2 IEC frame 1000 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU320, LI, In=1000A overload protection Ir=400A...1000A short-circuit protection Ii=1.5...10 x In nut keeper kit 1 auxiliary switch HP 1 trip alarm switch HP",3112.4,"ΤΕΜ",1,"EP",1,"3VA25105HL320AG0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2510-5KQ32-0CC0","circuit breaker 3VA2 IEC frame 1000 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU860, LSIG, In=1000A overload protection Ir=400A...1000A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection optionally with external current transformer, up to 160% gr.-fault prot., can be sw. off Ig=0.2...1 x In, tg=0.05-0.8s nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ",4172.6000000000004,"ΤΕΜ",1,"EP",1,"3VA25105KQ320CC0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2510-5KQ32-0KL0","circuit breaker 3VA2 IEC frame 1000 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU860, LSIG, In=1000A overload protection Ir=400A...1000A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection, opt. w. ext. curr. transf., up to 160% gr.-fault prot., can be sw. off Ig=0.2...1 x In= tg=0.05-0.8s nut keeper kit shunt trip (STL) 220-250V DC; 208-277V AC 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",4197.3999999999996,"ΤΕΜ",1,"EP",1,"3VA25105KQ320KL0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2563-5HL32-0AA0","circuit breaker 3VA2 IEC frame 1000 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU320, LI, In=630A overload protection Ir=250A...630A short-circuit protection Ii=1.5...12 x In nut keeper kit",1705,"ΤΕΜ",1,"EP",1,"3VA25635HL320AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2563-5MN32-0KH0","circuit breaker 3VA2 IEC frame 1000 breaking capacity class M Icu=55kA @ 415V 3-pole, motor protection ETU350M, LSI, In=630A overload protection Ir=250A...630A short-circuit protection Isd=3...15 x Ir, Ii=15 x In nut keeper kit shunt trip (STL) 220-250V DC, 208-277V AC 2 auxiliary switches HQ 1 trip alarm switch HQ",2256.8000000000002,"ΤΕΜ",1,"EP",1,"3VA25635MN320KH0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2580-5HL32-0CA0","circuit breaker 3VA2 IEC frame 1000 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU320, LI, In=800A overload protection Ir=320A...800A short-circuit protection Ii=1.5...12 x In nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz",2337.4,"ΤΕΜ",1,"EP",1,"3VA25805HL320CA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2580-5HN42-0AA0","circuit breaker 3VA2 IEC frame 1000 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection ETU350, LSI, In=800A overload protection Ir=320A...800A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In N conductor protection adjustable (OFF, 50%, 100%) nut keeper kit",3056.6,"ΤΕΜ",1,"EP",1,"3VA25805HN420AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2580-5KQ32-0KE0","circuit breaker 3VA2 IEC frame 1000 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU860, LSIG, In=800A overload protection Ir=320A...800A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% gr.-fault prot., can be sw. off Ig=0.2...1 x In, tg=0.05-0.8s nut keeper kit circuit breaker 3VA2 IEC frame 1000 breaking capacity class M SHUNT TRIP LEFT 208-277 V AC 50/60 HZ 220-250 V DC ACCESSORY 4 AUXILIARY SWITCH CHANGEOVER H",3354.2,"ΤΕΜ",1,"EP",1,"3VA25805KQ320KE0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2580-6HN32-0BH0","circuit breaker 3VA2 IEC frame 1000 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU350, LSI, In=800A overload protection Ir=320A...800A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In nut keeper kit undervoltage release (UVR) 24V DC 2 auxiliary switches HQ 1 trip alarm switch HQ",2802.4,"ΤΕΜ",1,"EP",1,"3VA25806HN320BH0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA2580-7HL32-0AA0","circuit breaker 3VA2 IEC frame 1000 breaking capacity class C Icu=110kA @ 415V 3-pole, line protection ETU320, LI, In=800A overload protection Ir=320A...800A short-circuit protection Ii=1.5...12 x In nut keeper kit",2759,"ΤΕΜ",1,"EP",1,"3VA25807HL320AA0","3VA2 Διακόπτες ισχύος κλειστού τύπου με ηλεκτρονική μονάδα"]
["3VA4110-1BB24-3AA0","molded case switch 3VA4 UL frame 125 max short-circuit curr. rating 65kA @ 480 V 2-pole MCS110, In=100A without overload protection - self protection Ii=16 x In",323.10000000000002,"ΤΕΜ",1,"EP",18,"3VA41101BB243AA0","3VA4 Διακόπτες ισχύος κλειστού τύπου UL"]
["3VA4111-4ED24-1AA0","circuit breaker 3VA4 UL frame 125 breaking capacity class S 25kA @ 480 V 2-pole, line protection TM210,  FTFM, In=110A overload protection Ir=110A fixed short-circuit protection Ii=10 x In UL489 SB (naval), 50 deg. cel. clamp connection",468,"ΤΕΜ",1,"EP",1,"3VA41114ED241AA0","3VA4 Διακόπτες ισχύος κλειστού τύπου UL"]
["3VA4120-6ED34-0AA0","circuit breaker 3VA4 UL frame 125 breaking capacity class H 65kA @ 480 V 3-pole, line protection TM210,  FTFM, In=20A overload protection Ir=20A fixed short-circuit protection Ii=15 x In clamp connection",369,"ΤΕΜ",1,"EP",1,"3VA41206ED340AA0","3VA4 Διακόπτες ισχύος κλειστού τύπου UL"]
["3VA4125-5ED34-1AA0","circuit breaker 3VA4 UL frame 125 breaking capacity class M 35kA @ 480 V 3-pole, line protection TM210,  FTFM, In=25A overload protection Ir=25A fixed short-circuit protection Ii=12 x In UL489 SB (naval), 50 deg. cel. clamp connection",353.7,"ΤΕΜ",1,"EP",1,"3VA41255ED341AA0","3VA4 Διακόπτες ισχύος κλειστού τύπου UL"]
["3VA4140-6ED24-1AA0","circuit breaker 3VA4 UL frame 125 breaking capacity class H 65kA @ 480 V 2-pole, line protection TM210,  FTFM, In=40A overload protection Ir=40A fixed short-circuit protection Ii=10 x In UL489 SB (naval), 50 deg. cel. clamp connection",361.8,"ΤΕΜ",1,"EP",1,"3VA41406ED241AA0","3VA4 Διακόπτες ισχύος κλειστού τύπου UL"]
["3VA4145-5ED34-1AA0","circuit breaker 3VA4 UL frame 125 breaking capacity class M 35kA @ 480 V 3-pole, line protection TM210,  FTFM, In=45A overload protection Ir=45A fixed short-circuit protection Ii=10 x In UL489 SB (naval), 50 deg. cel. clamp connection",353.7,"ΤΕΜ",1,"EP",1,"3VA41455ED341AA0","3VA4 Διακόπτες ισχύος κλειστού τύπου UL"]
["3VA4170-4ED14-1AA0","circuit breaker 3VA4 UL frame 125 breaking capacity class S 25kA @ 277 V 1-pole, line protection TM210,  FTFM, In=70A overload protection Ir=70A fixed short-circuit protection Ii=10 x In UL489 SB (naval), 50 deg. cel. clamp connection",190.8,"ΤΕΜ",1,"EP",1,"3VA41704ED141AA0","3VA4 Διακόπτες ισχύος κλειστού τύπου UL"]
["3VA4180-5ED24-1AA0","circuit breaker 3VA4 UL frame 125 breaking capacity class M 35kA @ 480 V 2-pole, line protection TM210,  FTFM, In=80A overload protection Ir=80A fixed short-circuit protection Ii=10 x In UL489 SB (naval), 50 deg. cel. clamp connection",360.9,"ΤΕΜ",1,"EP",1,"3VA41805ED241AA0","3VA4 Διακόπτες ισχύος κλειστού τύπου UL"]
["3VA4195-5ED14-1AA0","circuit breaker 3VA4 UL frame 125 breaking capacity class M 35kA @ 277 V 1-pole, line protection TM210,  FTFM, In=15A overload protection Ir=15A fixed short-circuit protection Ii=20 x In UL489 SB (naval), 50 deg. cel. clamp connection",191.7,"ΤΕΜ",1,"EP",1,"3VA41955ED141AA0","3VA4 Διακόπτες ισχύος κλειστού τύπου UL"]
["3VA5110-5ED31-1AA0","circuit breaker 3VA5 UL frame 125 breaking capacity class M 35kA @ 480V 3-pole, line protection TM210, FTFM, In=100A overload protection Ir=100A fixed short-circuit protection Ii=10 x In UL 489 SB (naval), 50Β° C without connection",454.5,"ΤΕΜ",1,"EP",1,"3VA51105ED311AA0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5110-6GD41-0AA0","circuit breaker 3VA5 UL frame 125 breaking capacity class H 65kA @ 480V 4-pole, line protection TM210, FTFM, In=100A overload protection Ir=100A fixed short-circuit protection Ii=10 x In N conductor protection 100% without connection",620.1,"ΤΕΜ",1,"EP",1,"3VA51106GD410AA0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5120-4ED31-0AA0","circuit breaker 3VA5 UL frame 125 breaking capacity class S 25kA @ 480V 3-pole, line protection TM210, FTFM, In=20A overload protection Ir=20A fixed short-circuit protection Ii=15 x In without connection",302.39999999999998,"ΤΕΜ",1,"EP",1,"3VA51204ED310AA0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5120-6ED31-0AB0","circuit breaker 3VA5 UL frame 125 breaking capacity class H 65kA @ 480V 3-pole, line protection TM210, FTFM, In=20A overload protection Ir=20A fixed short-circuit protection Ii=15 x In without connection circuit breaker 3VA5 UL frame 125 breaking capacity class H 65kA @ 480V 3-pole, line protection TM210, FTFM, In=20A overload protection Ir=20A fixed short-circuit protection Ii=15 x In without connection",369,"ΤΕΜ",1,"EP",1,"3VA51206ED310AB0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5130-6ED31-1AA0","circuit breaker 3VA5 UL frame 125 breaking capacity class H 65kA @ 480V 3-pole, line protection TM210, FTFM, In=30A overload protection Ir=30A fixed short-circuit protection Ii=10 x In UL 489 SB (naval), 50Β° C without connection",387,"ΤΕΜ",1,"EP",1,"3VA51306ED311AA0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5140-4ED21-0AA0","circuit breaker 3VA5 UL frame 125 breaking capacity class S 25kA @ 480V 2-pole, line protection TM210, FTFM, In=40A overload protection Ir=40A fixed short-circuit protection Ii=10 x In without connection",281.7,"ΤΕΜ",1,"EP",1,"3VA51404ED210AA0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5150-4EF41-0AA0","circuit breaker 3VA5 UL frame 125 breaking capacity class S 25kA @ 480V 4-pole, line protection TM240, ATAM, In=50A overload protection Ir=40A...50A short-circuit protection Ii=5...10 x In N conductor unprotected without connection",423.9,"ΤΕΜ",1,"EP",1,"3VA51504EF410AA0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5150-6ED31-1AA0","circuit breaker 3VA5 UL frame 125 breaking capacity class H 65kA @ 480V 3-pole, line protection TM210, FTFM, In=50A overload protection Ir=50A fixed short-circuit protection Ii=10 x In UL 489 SB (naval), 50Β° C without connection",387,"ΤΕΜ",1,"EP",1,"3VA51506ED311AA0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5170-6ED11-0AA0","circuit breaker 3VA5 UL frame 125 breaking capacity class H 50kA @ 277V 1-pole, line protection TM210, FTFM, In=70A overload protection Ir=70A fixed short-circuit protection Ii=10 x In without connection",208.8,"ΤΕΜ",1,"EP",1,"3VA51706ED110AA0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5180-6ED31-0AA0","circuit breaker 3VA5 UL frame 125 breaking capacity class H 65kA @ 480V 3-pole, line protection TM210, FTFM, In=80A overload protection Ir=80A fixed short-circuit protection Ii=10 x In without connection",409.5,"ΤΕΜ",1,"EP",1,"3VA51806ED310AA0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5195-5EF41-0AA0","circuit breaker 3VA5 UL frame 125 breaking capacity class M 35kA @ 480 V 4-pole, line protection TM240, ATAM, In=15A overload protection Ir=12A...15A short-circuit protection Ii=10β€¦20 x In N conductor unprotected without connection",471.6,"ΤΕΜ",1,"EP",1,"3VA51955EF410AA0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5210-7GD41-0AA0","circuit breaker 3VA5 UL frame 250 breaking capacity class C 100kA @ 480V 4-pole, line protection TM210, FTFM, In=100A overload protection Ir=100A fixed short-circuit protection Ii=10 x In N conductor protection 100% without connection",1323,"ΤΕΜ",1,"EP",1,"3VA52107GD410AA0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5212-7ED31-0AA0","circuit breaker 3VA5 UL frame 250 breaking capacity class C 100kA @ 480V 3-pole, line protection TM210, FTFM, In=125A overload protection Ir=125A fixed short-circuit protection Ii=10 x In without connection",1152,"ΤΕΜ",1,"EP",1,"3VA52127ED310AA0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5215-6EF31-0HC0","circuit breaker 3VA5 UL frame 250 breaking capacity class H 65kA @ 480V 3-pole, line protection TM240, ATAM, In=150A overload protection Ir=120A...150A short-circuit protection Ii=5...10 x In without connection circuit breaker 3VA5 UL frame 250 breaking capacity class H 65kA @ 480V 3-pole, line protection TM240, ATAM, In=150A overload protection Ir=120A...150A short-circuit protection Ii=5...10 x In",1467,"ΤΕΜ",1,"EP",1,"3VA52156EF310HC0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5215-7EF31-0AA0","circuit breaker 3VA5 UL frame 250 breaking capacity class C 100kA @ 480V 3-pole, line protection TM240, ATAM, In=150A overload protection Ir=120A...150A short-circuit protection Ii=5...10 x In without connection",1413,"ΤΕΜ",1,"EP",1,"3VA52157EF310AA0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5220-7ED31-0AA0","circuit breaker 3VA5 UL frame 250 breaking capacity class C 100kA @ 480V 3-pole, line protection TM210, FTFM, In=200A overload protection Ir=200A fixed short-circuit protection Ii=10 x In without connection",1359,"ΤΕΜ",1,"EP",1,"3VA52207ED310AA0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5225-0BB41-0AA0","molded case switch 3VA5 UL frame 250 max short-circuit curr. rating 65kA @ 480 V 4-pole MCS110, In=250A without overload protection SELF PROTECTION Ii=10 x In w/o connection",1269,"ΤΕΜ",1,"EP",1,"3VA52250BB410AA0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5225-7EC61-0AA0","circuit breaker 3VA5 UL frame 250 breaking capacity class C 100kA @ 480V 2-pole, line protection TM230, FTAM, In=250A overload protection Ir=250A fixed short-circuit protection Ii=5...10 x In without connection",1404,"ΤΕΜ",1,"EP",1,"3VA52257EC610AA0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5260-6ED31-0AA0","Circuit breaker 3VA5 UL Frame 250 Breaking capacity class H 65kA @ 480 V 3-pole, line protection TM210, FTFM, In=60A Overload protection Ir=60A fixed Short-circuit protection Ii=10 x In Without connection",813.6,"ΤΕΜ",1,"EP",1,"3VA52606ED310AA0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5290-7GD41-0AA0","circuit breaker 3VA5 UL frame 250 breaking capacity class C 100kA @ 480V 4-pole, line protection TM210, FTFM, In=90A overload protection Ir=90A fixed short-circuit protection Ii=10 x In N conductor protection 100% without connection",1233,"ΤΕΜ",1,"EP",1,"3VA52907GD410AA0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5320-7EF31-0AA0","CIRCUIT BREAKER 3VA5 UL FRAME 400 BREAKING CAPACITY CLASS  C 100kA @ 480 V 3POLE, LINE PROTECTION TM240,  ATAM, In=200A OVERLOAD PROTECTION IR=140A ...200A SHORT CIRCUIT PROTECTION II=5...10 X IN W/O CONNECTION",1872,"ΤΕΜ",1,"EP",1,"3VA53207EF310AA0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5330-7EF41-0AA0","CIRCUIT BREAKER 3VA5 UL FRAME 400 BREAKING CAPACITY CLASS  C 100kA @ 480 V 4POLE, LINE PROTECTION TM240,  ATAM, In=300A OVERLOAD PROTECTION IR=210A ...300A SHORT CIRCUIT PROTECTION II=5...10 X IN NEUTRAL UNPROTECTED W/O CONNECTION",2835,"ΤΕΜ",1,"EP",1,"3VA53307EF410AA0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5340-5EC41-0BB0","CIRCUIT BREAKER 3VA5 UL Frame 400 BREAKING CAPACITY CLASS  M 35kA @ 480 V 4POLE, LINE PROTECTION TM230,  FTAM, In=400A WITHOUT OVERLOAD PROTECTION IR=400A FIXED SHORT CIRCUIT PROTECTION Ii=5...10 x In NEUTRAL UNPROTECTED W/O CONNECTION CIRCUIT BREAKER 3VA5 UL Frame 400 BREAKING CAPACITY CLASS  M 35kA @ 480 V 4POLE, LINE PROTECTION TM230,  FTAM, In=400A WITHOUT OVERLOAD PROTECTION IR=400A FIXED SHORT",2394,"ΤΕΜ",1,"EP",1,"3VA53405EC410BB0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5450-7EC61-0AA0","CIRCUIT BREAKER 3VA5 UL FRAME 600 BREAKING CAPACITY CLASS  C 100kA @ 480 V 2POLE, LINE PROTECTION TM230,  FTAM, In=500A OVERLOAD PROTECTION IR=500A FIXED SHORT CIRCUIT PROTECTION II=5...10 X IN W/O CONNECTION",2457,"ΤΕΜ",1,"EP",1,"3VA54507EC610AA0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5460-0BB61-0AA0","MOLDED CASE SWITCH 3VA5 UL FRAME 600 MAX SHORT CIRCUIT CURR. RATING 65kA @ 480 V 2POLE, LINE PROTECTION MCS110, In=600A WITHOUT OVERLOAD PROTECTION SELF PROTECTION Ii=10 x In W/O CONNECTION",1737,"ΤΕΜ",1,"EP",1,"3VA54600BB610AA0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA5560-7EC32-0AA0","circuit breaker 3VA5 UL frame 800 breaking capacity class  C 100kA @ 480 V 3-pole, line protection TM230,  FTAM, In=600A overload protection Ir=600A fixed short circuit protection Ii=5...10 x In",3150,"ΤΕΜ",1,"EP",1,"3VA55607EC320AA0","3VA5 Διακόπτες ισχύος κλειστού τύπου UL με θερμομαγνητική μονάδα"]
["3VA6110-5HM31-0AA0","circuit breaker 3VA6 UL frame 150 breaking capacity class M 35kA @ 480V 3-pole, line protection ETU330, LIG, In=100A overload protection Ir=40A...100A short-circuit protection Ii=1.5...12 x In ground-fault protection Ig=0.2...1 x In, tg=0.1/0.3s without connection",1152,"ΤΕΜ",1,"EP",1,"3VA61105HM310AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6110-5JT41-0AA0","circuit breaker 3VA6 UL frame 150 breaking capacity class M 35kA @ 480V 4-pole, line protection ETU556, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection adjustable (OFF, up to 150%) ground-fault alarm message via EFB300 or COM without connection",1683,"ΤΕΜ",1,"EP",1,"3VA61105JT410AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6110-7JP31-0AA0","circuit breaker 3VA6 UL frame 150 breaking capacity class C 100kA @ 480V 3-pole, line protection ETU550, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% without connection",1647,"ΤΕΜ",1,"EP",1,"3VA61107JP310AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6110-8HN41-2AA0","circuit breaker 3VA6 UL frame 150 breaking capacity class L 150kA @ 480V 4-pole, line protection ETU350, LSI, In=100A overload protection, 100% rated Ir=40A...100A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In N conductor protection adjustable (OFF, 50%, 100%) without connection",1557,"ΤΕΜ",1,"EP",1,"3VA61108HN412AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6115-5HN31-0AA0","circuit breaker 3VA6 UL frame 150 breaking capacity class M 35kA @ 480V 3-pole, line protection ETU350, LSI, In=150A overload protection Ir=60A...150A short-circuit protection Isd=1.5...10 x Ir, Ii=10 x In without connection",1242,"ΤΕΜ",1,"EP",1,"3VA61155HN310AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6115-6HN31-0AA0","circuit breaker 3VA6 UL frame 150 breaking capacity class H 65kA @ 480V 3-pole, line protection ETU350, LSI, In=150A overload protection Ir=60A...150A short-circuit protection Isd=1.5...10 x Ir, Ii=10 x In without connection",1404,"ΤΕΜ",1,"EP",1,"3VA61156HN310AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6115-7HM41-0AA0","circuit breaker 3VA6 UL frame 150 breaking capacity class C 100kA @ 480V 4-pole, line protection ETU330, LIG, In=150A overload protection Ir=60A...150A short-circuit protection Ii=1.5...10 x In N conductor protection adjustable (OFF, 100%) ground-fault protection Ig=0.2...1 x In= tg=0.1/0.3s without connection",2196,"ΤΕΜ",1,"EP",1,"3VA61157HM410AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6140-5HL31-2AA0","circuit breaker 3VA6 UL frame 150 breaking capacity class M 35kA @ 480V 3-pole, line protection ETU320, LI, In=40A overload protection, 100% rated Ir=16A...40A short-circuit protection Ii=1.5...12 x In without connection",769.5,"ΤΕΜ",1,"EP",1,"3VA61405HL312AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6140-5KP31-2AA0","circuit breaker 3VA6 UL frame 150 breaking capacity class M 35kA @ 480V 3-pole, line protection ETU850, LSI, In=40A overload protection, 100% rated Ir=16A...40A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% without connection",1926,"ΤΕΜ",1,"EP",1,"3VA61405KP312AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6140-7JT31-0AA0","circuit breaker 3VA6 UL frame 150 breaking capacity class C 100kA @ 480V 3-pole, line protection ETU556, LSI, In=40A overload protection Ir=16A...40A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% ground-fault alarm message via EFB300 or COM without connection",1575,"ΤΕΜ",1,"EP",1,"3VA61407JT310AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6140-8KT31-2AA0","circuit breaker 3VA6 UL frame 150 breaking capacity class L 150kA @ 480V 3-pole, line protection ETU856, LSI, In=40A overload protection, 100% rated Ir=16A...40A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% ground-fault alarm message via EFB300 or COM without connection",2430,"ΤΕΜ",1,"EP",1,"3VA61408KT312AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6210-5KP41-2AA0","circuit breaker 3VA6 UL frame 250 breaking capacity class M 35kA @ 480V 4-pole, line protection ETU850, LSI, In=100A overload protection, 100% rated Ir=40A...100A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection adjustable (OFF, up to 160%) without connection",3357,"ΤΕΜ",1,"EP",1,"3VA62105KP412AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6210-6HN41-2AA0","circuit breaker 3VA6 UL frame 250 breaking capacity class H 65kA @ 480V 4-pole, line protection ETU350, LSI, In=100A overload protection, 100% rated Ir=40A...100A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In N conductor protection adjustable (OFF, 50%, 100%) without connection",2583,"ΤΕΜ",1,"EP",1,"3VA62106HN412AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6210-7HN41-2AA0","circuit breaker 3VA6 UL frame 250 breaking capacity class C 100kA @ 480V 4-pole, line protection ETU350, LSI, In=100A overload protection, 100% rated Ir=40A...100A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In N conductor protection adjustable (OFF, 50%, 100%) without connection",2817,"ΤΕΜ",1,"EP",1,"3VA62107HN412AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6210-8KT31-2AA0","circuit breaker 3VA6 UL frame 250 breaking capacity class L 150kA @ 480V 3-pole, line protection ETU856, LSI, In=100A overload protection, 100% rated Ir=40A...100A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% ground-fault alarm message via EFB300 or COM without connection",3753,"ΤΕΜ",1,"EP",1,"3VA62108KT312AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6225-6HM31-2AA0","circuit breaker 3VA6 UL frame 250 breaking capacity class H 65kA @ 480V 3-pole, line protection ETU330, LIG, In=250A overload protection, 100% rated Ir=100A...250A short-circuit protection Ii=1.5...10 x In ground-fault protection Ig=0.2...1 x In, tg=0.1/0.3s without connection",2340,"ΤΕΜ",1,"EP",1,"3VA62256HM312AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6225-7HL31-0BA0","circuit breaker 3VA6 UL frame 250 breaking capacity class C 100kA @ 480V 3-pole, line protection ETU320, LI, In=250A overload protection Ir=100A...250A short-circuit protection Ii=1.5...10 x In without connection circuit breaker 3VA6 UL frame 250 breaking capacity class C 100kA @ 480V 3-pole, line protection ETU320, LI, In=250A overload protection Ir=100A...250A short-circuit protection Ii=1.5...10 x In",2007,"ΤΕΜ",1,"EP",1,"3VA62257HL310BA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6225-8HN41-2AA0","circuit breaker 3VA6 UL frame 250 breaking capacity class L 150kA @ 480V 4-pole, line protection ETU350, LSI, In=250A overload protection, 100% rated Ir=100A...250A short-circuit protection Isd=1.5...10 x Ir, Ii=10 x In N conductor protection adjustable (OFF, 50%, 100%) without connection",3186,"ΤΕΜ",1,"EP",1,"3VA62258HN412AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6325-0KQ31-0AA0","circuit breaker 3VA6 UL frame 400 breaking capacity class  E 200 kA @ 480 V 3-pole, line protection ETU860,  LSIG, In=250A overload protection Ir=100A ... 250A short circuit protection Isd=0,6..10x In, Ii=1,5..12x In neutral protection optional with ext. CT;up to160% ground fault protection Ig=0,2... 1 x In, tg=0,05-0,8s w/o connection",4320,"ΤΕΜ",1,"EP",1,"3VA63250KQ310AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6325-5KQ41-0AA0","circuit breaker 3VA6 UL frame 400 breaking capacity class M 35kA @ 480V 4-pole, line protection ETU860, LSIG, In=250A overload protection Ir=100A...250A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection adjustable (OFF, up to 160%) ground-fault protection Ig=0.2...1 x In= tg=0.05-0.8s without connection",3933,"ΤΕΜ",1,"EP",1,"3VA63255KQ410AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6325-7KT31-2AA0","circuit breaker 3VA6 UL frame 400 breaking capacity class C 100kA @ 480V 3-pole, line protection ETU856, LSI, In=250A overload protection, 100% rated Ir=100A...250A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% ground-fault alarm message via EFB300 or COM without connection",4122,"ΤΕΜ",1,"EP",1,"3VA63257KT312AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6325-8KL31-0AA0","circuit breaker 3VA6 UL frame 400 breaking capacity class L 150kA @ 480V 3-pole, line protection ETU820, LI, In=250A overload protection Ir=100A...250A short-circuit protection Ii=1.5...12 x In without connection",3753,"ΤΕΜ",1,"EP",1,"3VA63258KL310AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6340-6KP41-0AA0","circuit breaker 3VA6 UL frame 400 breaking capacity class H 65kA @ 480V 4-pole, line protection ETU850, LSI, In=400A overload protection Ir=160A...400A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection adjustable (OFF, up to 100%) without connection",4077,"ΤΕΜ",1,"EP",1,"3VA63406KP410AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6440-5JP31-0AA0","circuit breaker 3VA6 UL frame 600 breaking capacity class M 35kA @ 480V 3-pole, line protection ETU550, LSI, In=400A overload protection Ir=160A...400A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% without connection",3492,"ΤΕΜ",1,"EP",1,"3VA64405JP310AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6440-6JP41-2AA0","circuit breaker 3VA6 UL frame 600 breaking capacity class H 65kA @ 480V 4-pole, line protection ETU550, LSI, In=400A overload protection, 100% rated Ir=160A...400A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection adjustable (OFF, up to 150%) without connection",5373,"ΤΕΜ",1,"EP",1,"3VA64406JP412AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6440-6KQ31-0AA0","circuit breaker 3VA6 UL frame 600 breaking capacity class H 65kA @ 480V 3-pole, line protection ETU860, LSIG, In=400A overload protection Ir=160A...400A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% ground-fault protection Ig=0.2...1 x In, tg=0.05-0.8s without connection",4410,"ΤΕΜ",1,"EP",1,"3VA64406KQ310AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6440-7KT41-0AA0","circuit breaker 3VA6 UL frame 600 breaking capacity class C 100kA @ 480V 4-pole, line protection ETU856, LSI, In=400A overload protection Ir=160A...400A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection adjustable (OFF, up to 160%) ground-fault alarm message via EFB300 or COM without connection",5553,"ΤΕΜ",1,"EP",1,"3VA64407KT410AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6460-5JQ31-0AA0","circuit breaker 3VA6 UL frame 600 breaking capacity class M 35kA @ 480V 3-pole, line protection ETU560, LSIG, In=600A overload protection Ir=240A...600A short-circuit protection Isd=0.6..9x In, Ii=1.5..9x In N conductor protection optionally with external current transformer, up to 160% ground-fault protection Ig=0.2...1 x In, tg=0.05-0.8s without connection",3870,"ΤΕΜ",1,"EP",1,"3VA64605JQ310AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6460-8KL31-0AA0","circuit breaker 3VA6 UL frame 600 breaking capacity class L 150kA @ 480V 3-pole, line protection ETU820, LI, In=600A overload protection Ir=240A...600A short-circuit protection Ii=1.5...9 x In without connection",4833,"ΤΕΜ",1,"EP",1,"3VA64608KL310AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6560-5JT46-0AA0","circuit breaker 3VA6 UL frame 800 breaking capacity class  M 35kA @ 480 V 4-pole, line protection ETU556,  LSI, In=600A overload protection Ir=240A ...600A short circuit protection Isd=0,6..12x In, Ii=1,5..12x In",5976,"ΤΕΜ",1,"EP",1,"3VA65605JT460AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6560-5KL46-2AA0","circuit breaker 3VA6 UL frame 800 breaking capacity class  M 35kA @ 480 V 4-pole, line protection ETU820, LI, In=600A overload protection, 100% rated Ir=240A...600A short circuit protection Ii=1,5...10 x In",6273,"ΤΕΜ",1,"EP",1,"3VA65605KL462AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6560-6KQ36-0AA0","circuit breaker 3VA6 UL frame 800 breaking capacity class  H 65kA @ 480 V 3-pole, line protection ETU860,  LSIG, In=600A overload protection Ir=240A ...600A short circuit protection",5283,"ΤΕΜ",1,"EP",1,"3VA65606KQ360AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6560-7HN42-2AA0","circuit breaker 3VA6 UL frame 800 breaking capacity class  C 100kA @ 480 V 4-pole, line protection ETU350, LSI, In=600A overload protection, 100% rated Ir=240A...600A short circuit protection Isd=1,5... 12 x Ir, Ii=12 x In",5517,"ΤΕΜ",1,"EP",1,"3VA65607HN422AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6580-5JP46-2AA0","circuit breaker 3VA6 UL frame 800 breaking capacity class  M 35kA @ 480 V 4-pole, line protection ETU550, LSI, In=800A overload protection, 100% rated Ir=320A...800A short circuit protection Isd=0,6..10x In, Ii=1,5..10x In",7209,"ΤΕΜ",1,"EP",1,"3VA65805JP462AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6580-6HL36-0AA0","circuit breaker 3VA6 UL frame 800 breaking capacity class  H 65kA @ 480 V 3-pole, line protection ETU320,  LI, In=800A overload protection Ir=320A ...800A short circuit protection Ii=1,5...10 x In",4923,"ΤΕΜ",1,"EP",1,"3VA65806HL360AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6580-6KL32-2AA0","circuit breaker 3VA6 UL frame 800 breaking capacity class  H 65kA @ 480 V 3-pole, line protection ETU820, LI, In=800A overload protection, 100% rated Ir=320A...800A short circuit protection Ii=1,5...10 x In",6525,"ΤΕΜ",1,"EP",1,"3VA65806KL322AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6580-7JP36-2AA0","circuit breaker 3VA6 UL frame 800 breaking capacity class  C 100kA @ 480 V 3-pole, line protection ETU550, LSI, In=800A overload protection, 100% rated Ir=320A...800A short circuit protection",6651,"ΤΕΜ",1,"EP",1,"3VA65807JP362AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6610-6JP32-0CJ0","circuit breaker 3VA6 UL frame 1000 breaking capacity class  H 65kA @ 480 V 3-pole, line protection ETU550,  LSI, In=1000A overload protection Ir=400A ...1000A short circuit protection",6921,"ΤΕΜ",1,"EP",1,"3VA66106JP320CJ0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA6610-6KT32-0AA0","circuit breaker 3VA6 UL frame 1000 breaking capacity class  H 65kA @ 480 V 3-pole, line protection ETU856,  LSI, In=1000A overload protection Ir=400A ...1000A short circuit protection",7767,"ΤΕΜ",1,"EP",1,"3VA66106KT320AA0","3VA6 Διακόπτες ισχύος κλειστού τύπου UL με ηλεκτρονική μονάδα"]
["3VA9078-0VK10","REAR INTERLOCK MOUNTING BRACKET ACCESSORY FOR: 3VA5 125/250/400/600 3VA6 150/250/400/600",121.4,"ΤΕΜ",1,"EP",1,"3VA90780VK10","3VA9 εξαρτήματα για 3VA διακόπτες"]
["3VA9114-0KP00","plug-in unit complete kit accessory for: circuit breaker, 4-pole 3VA1 160",252.25,"ΤΕΜ",1,"EP",1,"3VA91140KP00","3VA9 εξαρτήματα για 3VA διακόπτες"]
["3VA9134-0JF60","distribution wire connector 6 cables 4 units accessory for: 3VA5 125",168.56,"ΤΕΜ",1,"EP",1,"3VA91340JF60","3VA9 εξαρτήματα για 3VA διακόπτες"]
["3VA9134-0QA00","nut keeper kit 4 units accessory for: 3VA51",32.630000000000003,"ΤΕΜ",1,"EP",1,"3VA91340QA00","3VA9 εξαρτήματα για 3VA διακόπτες"]
["3VA9143-0KD10","draw-out unit conversion kit for MCCB accessory for: circuit breaker 3-pole 3VA6 150/250",144.59,"ΤΕΜ",1,"EP",1,"3VA91430KD10","3VA9 εξαρτήματα για 3VA διακόπτες"]
["3VA9157-0PK53","side wall mounted rot. operator standard IEC IP65 with mounting bracket 24V DC lighting kit accessory for: 3VA1 100/160",186.67,"ΤΕΜ",1,"EP",1,"3VA91570PK53","3VA9 εξαρτήματα για 3VA διακόπτες"]
["3VA9201-0QE20","rear connection stud flat long 1 unit accessory for: 3VA2 100/160/250",21.01,"ΤΕΜ",1,"EP",1,"3VA92010QE20","3VA9 εξαρτήματα για 3VA διακόπτες"]
["3VA9231-0QE10","rear connection stud flat short 1 unit accessory for: 3VA5 250",21.96,"ΤΕΜ",1,"EP",1,"3VA92310QE10","3VA9 εξαρτήματα για 3VA διακόπτες"]
["3VA9233-0JJ22","wire connector 2 cables 3 units accessory for: 3VA5 250",98.97,"ΤΕΜ",1,"EP",1,"3VA92330JJ22","3VA9 εξαρτήματα για 3VA διακόπτες"]
["3VA9253-0JC13","wire connector large with control wire voltage tap-off 3 units accessory for: plug-in/draw-out unit 3VA1 250",70.92,"ΤΕΜ",1,"EP",1,"3VA92530JC13","3VA9 εξαρτήματα για 3VA διακόπτες"]
["3VA9257-0HA20","motor operator 110-230V AC/110-250V DC accessory for: 3VA1 250",524.14,"ΤΕΜ",1,"EP",1,"3VA92570HA20","3VA9 εξαρτήματα για 3VA διακόπτες"]
["3VA9267-0EK25","front mounted rotary operator emergency-off with door interlock IEC IP30/40 accessory for: 3VA2 100/160/250",96.35,"ΤΕΜ",1,"EP",1,"3VA92670EK25","3VA9 εξαρτήματα για 3VA διακόπτες"]
["3VA9278-0CC40","operating unit w. Bowden cable Max Flex operator Bowden cable single length 1.8 m (72'') accessory for: 3VA5/6 125/150/250",252.07,"ΤΕΜ",1,"EP",1,"3VA92780CC40","3VA9 εξαρτήματα για 3VA διακόπτες"]
["3VA9373-0JB13","WIRE CONNECTOR; 3 PCS. ACCESSORY FOR: 3VA5/6 400/600",119.84,"ΤΕΜ",1,"EP",1,"3VA93730JB13","3VA9 εξαρτήματα για 3VA διακόπτες"]
["3VA9403-0QA00","nut keeper kit 3 units accessory for: 3VA1 400/630 3VA2 400/630",41.42,"ΤΕΜ",1,"EP",1,"3VA94030QA00","3VA9 εξαρτήματα για 3VA διακόπτες"]
["3VA9467-0HA10","motor operator 24-60V DC accessory for: 3VA1 400/630 3VA2 400/630",654.9,"ΤΕΜ",1,"EP",1,"3VA94670HA10","3VA9 εξαρτήματα για 3VA διακόπτες"]
["3VA9474-0QE00","REAR CONNECTION STUDS FLAT 4 PCS. ACCESSORY FOR: 3VA5/6 400/600",168.56,"ΤΕΜ",1,"EP",1,"3VA94740QE00","3VA9 εξαρτήματα για 3VA διακόπτες"]
["3VA9481-0WD40","terminal cover 4-pole 1 unit accessory for: 3VA1 400/630 3VA2 400/630",32.03,"ΤΕΜ",1,"EP",1,"3VA94810WD40","3VA9 εξαρτήματα για 3VA διακόπτες"]
["3VA9578-0CC10","Operating Unit w/ Bowdencable Max-Flex Operator Bowdencable only length 36'' (0,9 m) accessory for: 3VA5 400, 3VA6 600 3VA6 400, 3VA5 600",190.96,"ΤΕΜ",1,"EP",1,"3VA95780CC10","3VA9 εξαρτήματα για 3VA διακόπτες"]
["3VA9673-0QA00","Busbar shield kit 3 pcs. imperial nutplate, bus shield, insulator accessory for: 3VA55/3VA65/3VA66",87.34,"ΤΕΜ",1,"EP",1,"3VA96730QA00","3VA9 εξαρτήματα για 3VA διακόπτες"]
["3VA9908-0BB25","UNDERVOLTAGE RELEASE 208-230 V AC 50/60 HZ ACCESSORY FOR 3VA1 and 3VA20 up to 3VA25",96.32,"ΤΕΜ",1,"EP",1,"3VA99080BB25","3VA9 εξαρτήματα για 3VA διακόπτες"]
["3VA9977-0UF10","Maintenance Mode Box MMB300 incl. connecting cable 1.5 m 3VA - MMB300 accessory for: 3VA6",369.6,"ΤΕΜ",1,"EP",1,"3VA99770UF10","3VA9 εξαρτήματα για 3VA διακόπτες"]
["3VA9988-0BA20","SHUNT TRIP FLEXIBLE 24 V AC 50/60 HZ ACCESSORY FOR 3VA10 up to 3VA14 and 3VA20 up to 3VA24",74.27,"ΤΕΜ",1,"EP",1,"3VA99880BA20","3VA9 εξαρτήματα για 3VA διακόπτες"]
["3VW8112-0AE01","guide frame for 3WL10 - 3p front-access. main circ. conn. equiv. to withdr. circ. breaker without frame accessory for circuit breaker 3WL10",1618.74,"ΤΕΜ",1,"EP",1,"3VW81120AE01","3VW εξαρτήματα για 3WL10/3VA27 διακόπτες"]
["3VW9011-0AE11","time-delay device (adjustable) for undervoltage release UVR 48V AC/DC standard rail mounting accessory for circuit breaker 3WL10 / 3VA27",467.15,"ΤΕΜ",1,"EP",1,"3VW90110AE11","3VW εξαρτήματα για 3WL10/3VA27 διακόπτες"]
["3VW9011-0BA80","locking device to prevent movement of withdrawable circ. br. on guide frame, Ronis accessory for circuit breaker 3WL10 / 3VA27",142.52000000000001,"ΤΕΜ",1,"EP",1,"3VW90110BA80","3VW εξαρτήματα για 3WL10/3VA27 διακόπτες"]
["3WA9111-0AA14","Accessory circuit breaker 3WA, Internal metering current sensor for the neutral pole, frame size 1",152.15,"ΤΕΜ",1,"EP",1,"3WA91110AA14","3WA9 εξαρτήματα για 3WA διακόπτες"]
["3WA9111-0AE06","Accessory 3WA/3WL instantaneous (0,08 s) and short-delay (0,2 s), 208-240 V AC / 220-250 V DC,",298.44,"ΤΕΜ",1,"EP",1,"3WA91110AE06","3WA9 εξαρτήματα για 3WA διακόπτες"]
["3WA9111-0AH03","Accessory Circuit breaker 3WA, 2nd Trip alarm switch 1 NO contact (S25)",93.63,"ΤΕΜ",1,"EP",1,"3WA91110AH03","3WA9 εξαρτήματα για 3WA διακόπτες"]
["3WA9111-0AS01","Accessory Circuit breaker 3WA, Arc chute, AC 690 V frame size 1",76.069999999999993,"ΤΕΜ",1,"EP",1,"3WA91110AS01","3WA9 εξαρτήματα για 3WA διακόπτες"]
["3WA9111-0AX23","Accessory Circuit breaker 3WA, Rear horizontal main- connection, top or bottom, frame size 2 - 3200 A not for breaking capacity C for withdrawable design, 1 piece",67.3,"ΤΕΜ",1,"EP",1,"3WA91110AX23","3WA9 εξαρτήματα για 3WA διακόπτες"]
["3WA9111-0BG11","Accessory Circuit breaker 3WA, Grounding connection between guide frame a. circuit breaker. Contacting module for circuit breaker, frame size  1 3 poles",87.04,"ΤΕΜ",1,"EP",1,"3WA91110BG11","3WA9 εξαρτήματα για 3WA διακόπτες"]
["3WA9111-0ES13","Accessory circuit breaker 3WA, Firmware module for ETU600 Enhanced Protective functions: Under voltage and Over voltage",138.97999999999999,"ΤΕΜ",1,"EP",1,"3WA91110ES13","3WA9 εξαρτήματα για 3WA διακόπτες"]
["3WL9111-0AJ05-0AA0","accessories circuit breaker 3WL electr. on-pushbut. In op.panel with ikon lock iNCl. connection cables",339.45,"ΤΕΜ",1,"EP",1,"3WL91110AJ050AA0","3WL9 εξαρτήματα για 3WL διακόπτες"]
["3WL9111-0AL61-0AA0","accessories circuit breaker 3WL maine conductor conn. 1 piece fixed-mounted circ.br. size II front conn. bottom dual hole front accessible up to2000A",101.47,"ΤΕΜ",1,"EP",1,"3WL91110AL610AA0","3WL9 εξαρτήματα για 3WL διακόπτες"]
["3WL9111-0AN33-0AA0","accessories circuit breaker 3WL maine conductor conn. 1 piece withdraw. circ. breaker sz i horizontal conn., up to 2000A",82.49,"ΤΕΜ",1,"EP",1,"3WL91110AN330AA0","3WL9 εξαρτήματα για 3WL διακόπτες"]
["3WL9111-0AT74-0AA0","access. f. 3WL air circ. br., size 1, conversion of the internal voltage tap from top to bottom requires 3 units for 3-pole ACB requires 4 units for 4-pole ACB",165.71,"ΤΕΜ",1,"EP",1,"3WL91110AT740AA0","3WL9 εξαρτήματα για 3WL διακόπτες"]
["3WL9111-0BA77-0AA0","accessories circuit breaker 3WL locking device against traversing of circ. breaker safety lock  at crank hole ronis lock",788.4,"ΤΕΜ",1,"EP",1,"3WL91110BA770AA0","3WL9 εξαρτήματα για 3WL διακόπτες"]
["3WL9111-1AT65-0AA0","3WL9-NAFTA-accessory WLCM15m COM15 profibus module",11038.83,"ΤΕΜ",1,"EP",1,"3WL91111AT650AA0","3WL9 εξαρτήματα για 3WL διακόπτες"]
["3WL9111-2AA77-0AA0","accessories circuit breaker 3WL rated current ref. module 3000A f. ETU25, 27, 45, 55, 75, 76 approved to UL 489",420.77,"ΤΕΜ",1,"EP",1,"3WL91112AA770AA0","3WL9 εξαρτήματα για 3WL διακόπτες"]
["3ZS1322-6CC00-0YL5","SIRIUS SIMOCODE ES (TIA Portal) software update service for 1 year with automatic extension, requires current software, engineering software, SW+docu on DVD online functions via system interface and PROFIBUS / PROFINET, int. graphic editor (CFC-based)",398.5,"ΤΕΜ",1,"EP",1,"3ZS13226CC000YL5","3ZS λογισμικα"]
["3ZS2718-2CC00-0YH0","power management software SENTRON powermanager option pack Distributed Systems (5) license on USB flash drive 2 languages (D/E)",4378.8,"ΤΕΜ",1,"EP",1,"3ZS27182CC000YH0","3ZS λογισμικα"]
["4AM3242-5AV00-0EA0","TRANSFORMER SITAS; PHASES:1; PN/PN(S6)(KVA):0,063 /0,19; UPRI(V):400+/-5%; USEC(V):42; ISEC(A):1,5; F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0 /0; TA/ISOKL:40 /B; IP00; TYPE OF TERMINALS:SCREW/TAB CONNECTION; INSTALLATION:SCREWS/MOUNTING RAILS; EN 61558-2-2, -2-6 >UL/CSA-RECOGNIZED< >CONTROL CIRCUIT TRANSFORMER< >SAFETY ISOLATING TRANSFORMER<",147.09,"ΤΕΜ",1,"EP",1,"4AM32425AV000EA0","4AM  Μετασχηματιστές τάσης 1φασικοί"]
["4AM3442-8JN00-0EA0","TRANSFORMER SITAS; PHASES:1; PN/PN(S6)(KVA):0,1 /0,31; UPRI(V):400-230+/-15; USEC(V):24; ISEC(A):4,17; F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0 /0; TA/ISOKL:40 /B; IP00; TYPE OF TERMINALS:SCREW/TAB CONNECTION; INSTALLATION:SCREWS/MOUNTING RAILS; EN 61558-2-2, -2-6 >UL/CSA-RECOGNIZED< >CONTROL CIRCUIT TRANSFORMER< >SAFETY ISOLATING TRANSFORMER<",170.15,"ΤΕΜ",1,"EP",1,"4AM34428JN000EA0","4AM  Μετασχηματιστές τάσης 1φασικοί"]
["4AM4342-4TN00-0EC0","TRANSFORMER SITAS; PHASES:1; PN/PN(S6)(KVA):0,268 /1,12; UPRI(V):230+/-5%; USEC(V):24; ISEC(A):11,3; F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0 /0; TA/ISOKL:40 /B; IP23; TYPE OF TERMINALS:SCREW/TAB CONNECTION; INSTALLATION:SCREW; EN 61558-2-2, -2-6 >UL/CSA-RECOGNIZED< >CONTROL CIRCUIT TRANSFORMER< >SAFETY ISOLATING TRANSFORMER<",591.61,"ΤΕΜ",1,"EP",1,"4AM43424TN000EC0","4AM  Μετασχηματιστές τάσης 1φασικοί"]
["4AM4642-8DN00-0EA0","TRANSFORMER SITAS; PHASES:1; PN/PN(S6)(KVA):0,4 /1,44; UPRI(V):550-525-500-480-460- 440-415-400-380-230-208; USEC(V):24; ISEC(A):16,7; F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0 /0; TA/ISOKL:40 /B; IP00; TYPE OF TERMINALS:SCREW/TAB CONNECTION; INSTALLATION:SCREW; EN 61558-2-2, -2-6 >UL/CSA-RECOGNIZED< >CONTROL CIRCUIT TRANSFORMER< >SAFETY ISOLATING TRANSFORMER<",455.77,"ΤΕΜ",1,"EP",1,"4AM46428DN000EA0","4AM  Μετασχηματιστές τάσης 1φασικοί"]
["4AM5542-5AN00-0EA0","TRANSFORMER SITAS; PHASES:1; PN/PN(S6)(KVA):0,8 /3,4; UPRI(V):400+/-5%; USEC(V):24; ISEC(A):33,3; F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0 /0; TA/ISOKL:40 /B; IP00; TYPE OF TERMINALS:SCREW/TAB CONNECTION; INSTALLATION:SCREW; EN 61558-2-2, -2-6 >UL/CSA-RECOGNIZED< >CONTROL CIRCUIT TRANSFORMER< >SAFETY ISOLATING TRANSFORMER<",596.98,"ΤΕΜ",1,"EP",1,"4AM55425AN000EA0","4AM  Μετασχηματιστές τάσης 1φασικοί"]
["4AM5742-5FT10-0FA0","TRANSFORMER SITAS; PHASES:1; PN/PN(S6)(KVA):1 /5; UPRI(V):500+/-5%; USEC(V):230; ISEC(A):4,35; F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0 /0; TA/ISOKL:40 /B; IP00; TYPE OF TERMINALS:SCREW/TAB CONNECTION; INSTALLATION:SCREW; EN 61558-2-1, -2-2, -2-4 >UL/CSA-RECOGNIZED< >CONTROL CIRCUIT TRANSFORMER< >ISOLATION TRANSFORMER<",731.03,"ΤΕΜ",1,"EP",1,"4AM57425FT100FA0","4AM  Μετασχηματιστές τάσης 1φασικοί"]
["4AM6142-5MT10-0FA0","TRANSFORMER SITAS; PHASES:1; PN/PN(S6)(KVA):1,6 /7,3; UPRI(V):690+/-5%; USEC(V):230; ISEC(A):6,96; F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0 /0; TA/ISOKL:40 /B; IP00; TYPE OF TERMINALS:SCREW/TAB CONNECTION; INSTALLATION:SCREW; EN 61558-2-1, -2-2, -2-4 >CONTROL CIRCUIT TRANSFORMER< >ISOLATION TRANSFORMER<",1097.44,"ΤΕΜ",1,"EP",1,"4AM61425MT100FA0","4AM  Μετασχηματιστές τάσης 1φασικοί"]
["4AT3032-5FJ10-0FA0","TRANSFORMER SITAS; PHASES:1; PN/PN(S6)(KVA):4 /16,1; UPRI(V):500+/-5%; USEC(V):110; ISEC(A):36,4; F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0 /0; TA/ISOKL:55 /H; IP00; TYPE OF TERMINALS:SCREW CONNECTION; INSTALLATION:SCREW; EN 61558-2-1, -2-2, -2-4 >UL/CSA-RECOGNIZED< >CONTROL CIRCUIT TRANSFORMER< >ISOLATION TRANSFORMER<",2377.19,"ΤΕΜ",1,"EP",1,"4AT30325FJ100FA0","4AT  Μετασχηματιστές τάσης 1φασικοί"]
["4AT3932-8ED40-0FA0","TRANSFORMER SITAS; PHASES:1; PN/PN(S6)(KVA):10 /36,4; UPRI(V):600-575-550-525-500- 480-460-440-415-400-240-230; USEC(V):2X115; ISEC(A):2X43,5; F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0 /0; TA/ISOKL:55 /H; IP00; TYPE OF TERMINALS:SCREW CONNECTION; INSTALLATION:SCREW; EN 61558-2-1, -2-2, -2-4 >UL/CSA-RECOGNIZED< >CONTROL CIRCUIT TRANSFORMER< >ISOLATION TRANSFORMER<",5219.09,"ΤΕΜ",1,"EP",1,"4AT39328ED400FA0","4AT  Μετασχηματιστές τάσης 1φασικοί"]
["4EM5100-2CB00","COMMUTATING CHOKE FOR CONVERTER; PHASES:1; UN1(V):400; ITHMAX 1(A) / F1(HZ):24 /50; I LN (A):21,6; UK(%):4; LN(MH):2,02; TA/ISOKL:40 /B; IP00; TYPE OF TERMINALS:SCREW CONNECTION; EN 61558-2-20 >CHOKE<",613.32000000000005,"ΤΕΜ",1,"EP",1,"4EM51002CB00","4EM CHOKE"]
["4EP3700-7US00","MAINS CHOKE F.FU; PHASES:3; UN1(V):480; ITHMAX 1(A) / F1(HZ):18 /60; I LN (A):16,2; UK(%):4; LN(MH):1,57; TA/ISOKL:40 /B; IP00; TYPE OF TERMINALS:SCREW CONNECTION; EN 61558-2-20 >UL/CSA-RECOGNIZED< >CHOKE<",1294.26,"ΤΕΜ",1,"EP",1,"4EP37007US00","4EP CHOKE"]
["4NC5124-2FE21","current transformer 300/5A 5VA CL 0.2s",72.760000000000005,"ΤΕΜ",1,"EP",1,"4NC51242FE21","4NC Μετασχηματιστές έντασης"]
["4NC5432-0DH21","current transformer 1000/1A 10 VA CL 0.5",137.61000000000001,"ΤΕΜ",1,"EP",1,"4NC54320DH21","4NC Μετασχηματιστές έντασης"]
["5SD7418-3","Plug-in part T1/T2, L-N, rated voltage UN 240 V AC UC 335 V A.C., IIMP 12.5 kA, only for 5SD7413-2 (3) and 5SD7414-2 (3)",134.76,"ΤΕΜ",1,"EP",1,"5SD74183","5SD7 Αντικεραυνικά"]
["5SE2300","NEOZED fuse-link, D03, 100 A, gG, Un AC: 400 V, Un DC: 250 V",6.89,"ΤΕΜ",1,"EP",10,"5SE2300","5SE Ασφάλειες NEOZED"]
["5SG7651-0KK16","MINIZED, fuse switch disconnector, D01, 2-pole, 1P+N, In: 16 A, Un AC: 230 V",29.77,"ΤΕΜ",1,"EP",6,"5SG76510KK16","5SG Ασφαλειοδιακόπτες MINIZED"]
["5SH5010","NEOZED adapter sleeve D01 10 A",0.63,"ΤΕΜ",1,"EP",50,"5SH5010","5SH εξαρτήματα ασφαλειών"]
["5SJ4108-7HG40","Miniature circuit breaker 240 V 14kA, 1-pole, C, 8A, D=70 mm according to UL 489, equal polarity",45.54,"ΤΕΜ",1,"EP",1,"5SJ41087HG40","5SJ Μικροαυτόματοι διακόπτες κατά UL489"]
["5SJ4114-8HG42","Circuit breaker 10kA, 1-pole, D, 0.3 A according to UL 489-277V",61.38,"ΤΕΜ",1,"EP",1,"5SJ41148HG42","5SJ Μικροαυτόματοι διακόπτες κατά UL489"]
["5SJ4132-7HG40","Miniature circuit breaker 240 V 14kA, 1-pole, C, 32 A, D=70 mm according to UL 489, equal polarity",45.54,"ΤΕΜ",1,"EP",1,"5SJ41327HG40","5SJ Μικροαυτόματοι διακόπτες κατά UL489"]
["5SJ4202-8HG42","Circuit breaker 10kA, 2-pole, D, 2A according to UL 489-480Y/277V",172.8,"ΤΕΜ",1,"EP",1,"5SJ42028HG42","5SJ Μικροαυτόματοι διακόπτες κατά UL489"]
["5SJ4220-8HG42","Circuit breaker 10kA, 2-pole, D, 20A according to UL 489-480Y/277V",142.19999999999999,"ΤΕΜ",1,"EP",1,"5SJ42208HG42","5SJ Μικροαυτόματοι διακόπτες κατά UL489"]
["5SJ4332-8HG41","Miniature circuit breaker 240 V 10kA, 3-pole, D, 32 A, D=70 mm according to UL 489",252,"ΤΕΜ",1,"EP",1,"5SJ43328HG41","5SJ Μικροαυτόματοι διακόπτες κατά UL489"]
["5SJ6210-7KS","Miniature circuit breaker 400 V 6kA, 2-pole, C, 10A, D=70 mm with screwless outgoing terminals",28.16,"ΤΕΜ",1,"EP",1,"5SJ62107KS","5SJ6 Μικροαυτόματοι διακόπτες με αυτόματους ακροδέκτες"]
["5SL3106-6","Miniature circuit breaker 230/400 V 4.5 kA, 1-pole, B, 6A",7.8,"ΤΕΜ",1,"EP",1,"5SL31066","5SL3 Μικροαυτόματοι διακόπτες 4,5kA"]
["5SL4115-8","Miniature circuit breaker 230/400 V 10kA, 1-pole, D, 1.6A",16,"ΤΕΜ",1,"EP",1,"5SL41158","5SL4 Μικροαυτόματοι διακόπτες 10kA"]
["5SL4225-7","Miniature circuit breaker 400 V 10kA, 2-pole, C, 25A",32,"ΤΕΜ",1,"EP",1,"5SL42257","5SL4 Μικροαυτόματοι διακόπτες 10kA"]
["5SL4350-7","Miniature circuit breaker 400 V 10kA, 3-pole, C, 50 A",81,"ΤΕΜ",1,"EP",1,"5SL43507","5SL4 Μικροαυτόματοι διακόπτες 10kA"]
["5SL4508-8","Miniature circuit breaker 230 V 10kA, 1+N-pole, D, 8A",29,"ΤΕΜ",1,"EP",1,"5SL45088","5SL4 Μικροαυτόματοι διακόπτες 10kA"]
["5SL4604-8","Miniature circuit breaker 400 V 10kA, 3+N-pole, D, 4A",68,"ΤΕΜ",1,"EP",1,"5SL46048","5SL4 Μικροαυτόματοι διακόπτες 10kA"]
["5SL4614-8","Miniature circuit breaker 400 V 10kA, 3+N-pole, D, 0.3A",90,"ΤΕΜ",1,"EP",1,"5SL46148","5SL4 Μικροαυτόματοι διακόπτες 10kA"]
["5SL6120-7","Miniature circuit breaker 230/400 V 6kA, 1-pole, C, 20 A",5,"ΤΕΜ",1,"EP",1,"5SL61207","5SL6 Μικροαυτόματοι διακόπτες 6kA"]
["5SL6305-7","Miniature circuit breaker 400 V 6kA, 3-pole, C, 0.5A",27,"ΤΕΜ",1,"EP",1,"5SL63057","5SL6 Μικροαυτόματοι διακόπτες 6kA"]
["5SL6463-6","Miniature circuit breaker 400 V 6kA, 4-pole, B, 63 A",92.3,"ΤΕΜ",1,"EP",1,"5SL64636","5SL6 Μικροαυτόματοι διακόπτες 6kA"]
["5SL6620-7","Miniature circuit breaker 400 V 6kA, 3+N-pole, C, 20 A",27.5,"ΤΕΜ",1,"EP",1,"5SL66207","5SL6 Μικροαυτόματοι διακόπτες 6kA"]
["5SM2647-8","RC unit for 5SP4, 4-pole, type A, selective, In: 100 A, 300 mA, Un AC: 400 V",320,"ΤΕΜ",1,"EP",1,"5SM26478","RC μονάδα διαρροής ρεύματος για 5SP4"]
["5SM6011-1XX02","Arc fault detection device block AFDD, 1-16 A 230 V 1 MW with miniature circuit breaker 1+N 6 kA, B 10 A 1 MW",467.82,"ΤΕΜ",1,"EP",1,"5SM60111XX02","5SM Στοιχεία AFDD"]
["5SP3740-2","Main miniature circuit breaker (SHU), 1-pole, E 40A, 230/400 V (block with L1, L2, L3)",382.14,"ΣΕΤ",1,"EP",1,"5SP37402","5SP3 Μικροαυτόματη ασφάλεια καμπύλης Ε - 25kA"]
["5ST2188","Fork-type busbar touch-safe, 3-phase 16 mm2, 12 MW",10.67,"ΤΕΜ",1,"EP",1,"5ST2188","Εξαρτήματα για υλικό ράγας"]
["5ST3022-2","Fault signal contact with test and acknowledgment key 2 NC for miniature circuit breaker 5SL, 5SY, 5SP RCBO 5SU1, FI 5SV (for 5SU1 handle coupler 5ST3805-1 is required)",29.57,"ΤΕΜ",1,"EP",1,"5ST30222","5ST3 βοηθητικές επαφές για υλικό ράγας"]
["5ST3632","Pin busbar, 16 mm2 connection: 12x 1-phase touch-safe",3.25,"ΤΕΜ",1,"EP",10,"5ST3632","5ST3 μπάρες για υλικό ράγας"]
["5ST3655","Touch protection for unassigned connections yellow",2.48,"ΤΕΜ",1,"EP",10,"5ST3655","5ST3 μπάρες για υλικό ράγας"]
["5ST3724","Pin busbar touch-safe, 16 mm2 2-phase, 393 mm long fully insulated for 6x (RC unit 5SM2+LS 5SY 2-pole)",10.33,"ΤΕΜ",1,"EP",1,"5ST3724","5ST3 μπάρες για υλικό ράγας"]
["5ST3764-1","Pin busbar 1PH 10 mm2, 54TE gray, Pin busbar, 1-phase straight, 10qmm, 54TE, Gray insulation, Can be cut for AFDDan be cut for AFDD 5SM6011-2, Pin spacing 2 MW",19.78,"ΤΕΜ",1,"EP",10,"5ST37641","5ST3 μπάρες για υλικό ράγας"]
["5ST3820-5","Adapter for RCBO 5SU1 up to 2 MW Accessory for remote operating mechanism",4.9000000000000004,"ΤΕΜ",1,"EP",1,"5ST38205","Εξαρτήματα για υλικό ράγας"]
["5SU1324-7FA40","RCBO, 10 kA, 2P, type A, 30 mA, C-Char, In: 40 A, Un AC: 230 V",170,"ΤΕΜ",1,"EP",1,"5SU13247FA40","5SU RCBO 10kA"]
["5SU1346-7FP32","RCBO, 6 kA, 4P Type A, 30 mA, C-Char, In: 32A Un: 400V",190,"ΤΕΜ",1,"EP",1,"5SU13467FP32","5SU RCBO 6kA"]
["5SU1353-7KK08","RCBO, 4.5 kA, 1P+N, type A, 30 mA, C-Char, In: 8 A, Un AC: 230 V",100,"ΤΕΜ",1,"EP",1,"5SU13537KK08","5SU RCBO 4,5kA"]
["5SU1354-7KK32","RCBO, 10 kA, 1P+N, type A, 30 mA, C-Char, In: 32 A, Un AC: 230 V",128,"ΤΕΜ",1,"EP",1,"5SU13547KK32","5SU RCBO 10kA"]
["5SU1356-6KK32","RCBO, 6 kA, 1P+N, type A, 30 mA, B char., In: 32 A, Un AC: 230 V",106.2,"ΤΕΜ",1,"EP",1,"5SU13566KK32","5SU RCBO 6kA"]
["5SU1636-7FP32","RCBO, 6 kA, 3P Type A, 300mA, C-Char, In: 32A Un: 400V Energy limiting class 1: check for normative use limitations",170,"ΤΕΜ",1,"EP",1,"5SU16367FP32","5SU RCBO 6kA"]
["5SU1656-0KK40","RCBO, 6 kA, 1P+N, Type AC, 300 mA, B char., In: 40 A, Un AC: 230 V",175.2,"ΤΕΜ",1,"EP",1,"5SU16560KK40","5SU RCBO 6kA"]
["5SU9354-8KK50","RCBO, 10 kA, 1P+N, type A, 30 mA, D char., In: 50 A, Un AC: 230 V",725.12,"ΤΕΜ",1,"EP",1,"5SU93548KK50","5SU RCBO 10kA Voltage Dependend - CY"]
["5SV1313-1GV10","5SV1 RCBO TypeAC 30mA C10 4.5kA 1+N 1MW, Big Pack 12 pcs",113,"ΤΕΜ",1,"EP",12,"5SV13131GV10","5SV RCBO 4,5kA"]
["5SV1316-0KK16","RCBO compact 1P+N 6 kA type AC 30 mA B16",205.2,"ΤΕΜ",1,"EP",1,"5SV13160KK16","5SV RCBO 6kA 1 στοιχείου"]
["5SV1613-1KK16","RCBO compact 1P+N 4.5 kA type AC 300 mA C16",110,"ΤΕΜ",1,"EP",1,"5SV16131KK16","5SV RCBO 4,5kA 1 στοιχείου"]
["5SV3324-4","Residual current operated circuit breaker, 2-pole, Type B, short-time delayed, In: 40 A, 30 mA, Un AC: 230 V",430,"ΤΕΜ",1,"EP",1,"5SV33244","5SV3 Ρελέ διαρροής τύπου A/F/B/B+"]
["5SV3444-8","Residual current operated circuit breaker, 4-pole, type A, selective, In: 40 A, 100 mA, Un AC: 400 V",160,"ΤΕΜ",1,"EP",1,"5SV34448","5SV3 Ρελέ διαρροής τύπου A/F/B/B+"]
["5SV3644-7","Residual current operated circuit breaker, 4-pole, type F, selective, In: 40 A, 300 mA, Un AC: 400 V",220,"ΤΕΜ",1,"EP",1,"5SV36447","5SV3 Ρελέ διαρροής τύπου A/F/B/B+"]
["5SV4314-0KK13","Residual current operated circuit breaker, 2-pole, Type AC, In: 40 A, 30 mA, Un AC: 24-125 V",85.49,"ΤΕΜ",1,"EP",1,"5SV43140KK13","5SV4 Ρελέ διαρροής τύπου AC"]
["5SV4346-0LA01","Residual current operated circuit breaker, 4-pole, Type AC, short-time delayed, In: 63 A, 30 mA, Un AC: 400 V, with thermal overload protection",250.92,"ΤΕΜ",1,"EP",1,"5SV43460LA01","5SV4 Ρελέ διαρροής τύπου AC"]
["5SV6016-6KP06","AFDD-MCB-combination 230V, 6kA, 1+N, B, 6A compact (1MW) pigtail",277.45,"ΤΕΜ",1,"EP",1,"5SV60166KP06","5SV6 AFDD / Μικροαυτόματος διακόπτης 1 στοιχείου"]
["5SV6016-7KP25","AFDD-MCB-combination 230V, 6kA, 1+N, C, 25A compact (1MW) pigtail",316.02,"ΤΕΜ",1,"EP",1,"5SV60167KP25","5SV6 AFDD / Μικροαυτόματος διακόπτης 1 στοιχείου"]
["5SV8701-2KP","Summation current transformer type B, 35 mm, 30 mA 1A, with metal shielding",1019.94,"ΤΕΜ",1,"EP",1,"5SV87012KP","5SV8 Επιτηρητες διαροής προς γη"]
["5SW3005","Terminal cover, gray IP40, for surface mounting for built-in devices 4, 5 MW max. wide",32.979999999999997,"ΤΕΜ",1,"EP",1,"5SW3005","5SW εξαρτήματα μικροαυτομάτων"]
["5SY4110-7","Miniature circuit breaker 230/400 V 10kA, 1-pole, C, 10A, D=70 mm",15,"ΤΕΜ",1,"EP",1,"5SY41107","5SY4 Μικροαυτόματοι διακόπτες 10kΑ - multistandard offer"]
["5SY4220-6","Miniature circuit breaker 400 V 10kA, 2-pole, B, 20 A, D=70 mm",59.79,"ΤΕΜ",1,"EP",1,"5SY42206","5SY4 Μικροαυτόματοι διακόπτες 10kΑ - multistandard offer"]
["5SY4250-8FA","Miniature circuit breaker 400 V 10kA, 2-pole, 50 A, D=70 mm as counter preliminary miniature circuit breaker",179.1,"ΤΕΜ",1,"EP",1,"5SY42508FA","5SY4 Μικροαυτόματοι διακόπτες 10kΑ - multistandard offer"]
["5SY4340-5","Miniature circuit breaker 400 V 10kA, 3-pole, A, 40A, D=70 mm",226.59,"ΤΕΜ",1,"EP",1,"5SY43405","5SY4 Μικροαυτόματοι διακόπτες 10kΑ - multistandard offer"]
["5SY4410-8","Miniature circuit breaker 400 V 10kA, 4-pole, D, 10A, D=70 mm",225.9,"ΤΕΜ",1,"EP",1,"5SY44108","5SY4 Μικροαυτόματοι διακόπτες 10kΑ - multistandard offer"]
["5SY4505-8","Miniature circuit breaker 230 V 10kA, 1+N-pole, D, 0.5 A, D=70 mm",84.66,"ΤΕΜ",1,"EP",1,"5SY45058","5SY4 Μικροαυτόματοι διακόπτες 10kΑ - multistandard offer"]
["5SY4604-5","Miniature circuit breaker 400 V 10kA, 3+N-pole, A, 4A, D=70 mm",226.59,"ΤΕΜ",1,"EP",1,"5SY46045","5SY4 Μικροαυτόματοι διακόπτες 10kΑ - multistandard offer"]
["5SY4614-8","Miniature circuit breaker 400 V 10kA, 3+N-pole, D, 0.3 A, D=70 mm",226.59,"ΤΕΜ",1,"EP",1,"5SY46148","5SY4 Μικροαυτόματοι διακόπτες 10kΑ - multistandard offer"]
["5SY5210-6","Circuit breaker Universal current 440 V DC 400 V AC 10kA, 2-pole, B, 10 A",108.77,"ΤΕΜ",1,"EP",1,"5SY52106","5SY5 Μικροαυτόματοι διακόπτες 10kA / 220-440 VDC - multistandard offer"]
["5SY5425-6","Circuit breaker Universal current 880 V DC 400 V AC 10kA, 4-pole, B, 25A max. 1000 V DC",214.62,"ΤΕΜ",1,"EP",1,"5SY54256","5SY5 Μικροαυτόματοι διακόπτες 10kA / 220-440 VDC - multistandard offer"]
["5SY6308-7","Miniature circuit breaker 400 V 6kA, 3-pole, C, 8A, D=70 mm",60.55,"ΤΕΜ",1,"EP",1,"5SY63087","5SY6 Μικροαυτόματοι διακόπτες 6kA - multistandard offer"]
["5SY6540-7","Miniature circuit breaker 230 V 6kA, 1+N-pole C, 40A, D=70 mm",36.049999999999997,"ΤΕΜ",1,"EP",1,"5SY65407","5SY6 Μικροαυτόματοι διακόπτες 6kA - multistandard offer"]
["5SY6615-7","Miniature circuit breaker 400 V 6kA, 3+N-pole C, 1.6 A, D=70 mm",76.3,"ΤΕΜ",1,"EP",1,"5SY66157","5SY6 Μικροαυτόματοι διακόπτες 6kA - multistandard offer"]
["5SY7125-7","Miniature circuit breaker 230/400 V 15kA, 1-pole, C, 25A, D=70 mm",23,"ΤΕΜ",1,"EP",1,"5SY71257","5SY7 Μικροαυτόματοι διακόπτες 15kA - multistandard offer"]
["5SY7340-6","Miniature circuit breaker 400 V 15kA, 3-pole, B, 40A, D=70 mm",116.82,"ΤΕΜ",1,"EP",1,"5SY73406","5SY7 Μικροαυτόματοι διακόπτες 15kA - multistandard offer"]
["5SY7414-7","Miniature circuit breaker 400 V 15kA, 4-pole, C, 0.3A, D=70 mm",160,"ΤΕΜ",1,"EP",1,"5SY74147","5SY7 Μικροαυτόματοι διακόπτες 15kA - multistandard offer"]
["5SY7550-8","Miniature circuit breaker 230 V 15kA, 1+N-pole, D, 50 A, D=70 mm",164.35,"ΤΕΜ",1,"EP",1,"5SY75508","5SY7 Μικροαυτόματοι διακόπτες 15kA - multistandard offer"]
["5SY7640-8","Miniature circuit breaker 400 V 15kA, 3+N-pole, D, 40A, D=70 mm",363.85,"ΤΕΜ",1,"EP",1,"5SY76408","5SY7 Μικροαυτόματοι διακόπτες 15kA - multistandard offer"]
["5SY8215-7","Miniature circuit breaker 400 V D=70 mm 25 kA according to EN 60947-2, 2P, C1.6",84,"ΤΕΜ",1,"EP",1,"5SY82157","5SY8 Μικροαυτόματοι διακόπτες 25kA - multistandard offer"]
["5SY8325-8","Miniature circuit breaker 400 V D=70 mm 25 kA according to EN 60947-2, 3P, D25",219.45,"ΤΕΜ",1,"EP",1,"5SY83258","5SY8 Μικροαυτόματοι διακόπτες 25kA - multistandard offer"]
["5SY8404-8","Miniature circuit breaker 400 V D=70 mm 25 kA according to EN 60947-2, 4P, D4",367.65,"ΤΕΜ",1,"EP",1,"5SY84048","5SY8 Μικροαυτόματοι διακόπτες 25kA - multistandard offer"]
["5SY8620-7","Miniature circuit breaker 400 V D=70 mm 25 kA according to EN 60947-2, 3P+N, C20",125,"ΤΕΜ",1,"EP",1,"5SY86207","5SY8 Μικροαυτόματοι διακόπτες 25kA - multistandard offer"]
["5TA2117","DELTA switch device insert FM, Intermediate switch 10 A 250 V",20.34,"ΤΕΜ",1,"EP",1,"5TA2117","Διακοπτικό Υλικό"]
["5TC8903","DELTA i-system carbon metallic Cover plate for dimmer with rotary knob 55x 55 mm",28.77,"ΤΕΜ",1,"EP",1,"5TC8903","Διακοπτικό Υλικό"]
["5TC9774-4CH00","DELTA style, Thermostat Chocolate",133.04,"ΤΕΜ",1,"EP",1,"5TC97744CH00","Διακοπτικό Υλικό"]
["5TE6801","SCHUKO socket outlet 16 A with cover according to DIN VDE 0620 for installation in distribution boards",12.26,"ΤΕΜ",1,"EP",1,"5TE6801","5TE Διακόπτες - μπουτόν - λυχνίες ράγας"]
["5TE8162","Two-way switch 20 A 2 CO",26.24,"ΤΕΜ",1,"EP",1,"5TE8162","5TE Διακόπτες - μπουτόν - λυχνίες ράγας"]
["5TG1203-2","DELTA miro glass Frame 3-fold Authentic material black glass 232x 90 mm",189.82,"ΤΕΜ",1,"EP",1,"5TG12032","Διακοπτικό Υλικό"]
["5TG1258","DELTA i-system aluminum-metallic Cover plate UAE connection socket suitable for Rutenbeck Cat. 3+5/ BTR Cat. 6, 55x 55 mm with labeling field",20.66,"ΤΕΜ",1,"EP",1,"5TG1258","Διακοπτικό Υλικό"]
["5TG1394","DELTA style, titanium white Cover plate UAE connection socket 68x 68 mm for Rutenbeck Cat. 3+5+6 BTR-DAT C6, E-DAT/UAE design TelegΓ¤rtner AMJ45, UMJ45",12.39,"ΤΕΜ",1,"EP",1,"5TG1394","Διακοπτικό Υλικό"]
["5TG2027-2","DELTA connection socket Universal connection unit 2x 8-pole RJ45 Cat. 6 A unshielded LSA-plus terminals Screw mounting",52.23,"ΤΕΜ",1,"EP",1,"5TG20272","Διακοπτικό Υλικό"]
["5TG2057","DELTA i-system electrical white Cover plate with shutter for support plates Modular jack connector",15.43,"ΤΕΜ",1,"EP",1,"5TG2057","Διακοπτικό Υλικό"]
["5TG2591","DELTA i-system electrical white antenna cover plate 55x 55 mm for broadband connection socket RF/TV",6.58,"ΤΕΜ",1,"EP",1,"5TG2591","Διακοπτικό Υλικό"]
["5TG4200","DELTA i-system Replacement window for light signal for switch and pushbutton Set 2x crystal clear, 2x red, 2x white",12.88,"ΣΕΤ",1,"EP",1,"5TG4200","Διακοπτικό Υλικό"]
["5TG6214","DELTA i-system titanium white Rocker switch with shutter symbols for shutter pushbutton, 55x 55 mm",11.3,"ΤΕΜ",1,"EP",1,"5TG6214","Διακοπτικό Υλικό"]
["5TG7141-0CH20","DELTA style, Chocolate Rocker switch with symbol Light for pushbutton, 68x 68 mm",15.21,"ΤΕΜ",1,"EP",1,"5TG71410CH20","Διακοπτικό Υλικό"]
["5TG7938","DELTA profil, silver Rocker switch with window for pushbutton 2-fold for pushbutton 2-fold Mid-position 65x 65 mm",39.89,"ΤΕΜ",1,"EP",1,"5TG7938","Διακοπτικό Υλικό"]
["5TG8066","Cap set for button 5TE48 and indicator light 5TE58 Set with 5x each white/transparent",11.89,"ΣΕΤ",1,"EP",1,"5TG8066","Διακοπτικό Υλικό"]
["5TT4101-2","Remote control switch with 1 NO contact, Contact for 230 V AC 16 A Control 24 V AC",30.57,"ΤΕΜ",1,"EP",1,"5TT41012","5TT Ρελέ ράγας"]
["5TT4112-2","Remote control switch with 2 NO contacts, Contact for 230 V AC, 400V 16A Control 24 V DC",34.17,"ΤΕΜ",1,"EP",1,"5TT41122","5TT Ρελέ ράγας"]
["5TT4455-5","Remote control switch Contact for 32 A Voltage 24 V DC 1 NO 1 NC",75.84,"ΤΕΜ",1,"EP",1,"5TT44555","5TT Ρελέ ράγας"]
["5TT4932","auxiliary current switch, group half module",30.26,"ΤΕΜ",1,"EP",1,"5TT4932","5TT Ρελέ ράγας"]
["5TT5843-0","INSTA contactor with 4 NC contacts Contact for 230 V AC, 400V 40A Control 230 V AC",125.88,"ΤΕΜ",1,"EP",1,"5TT58430","5TT Ρελέ ράγας"]
["5TT5910-1","Auxiliary current switch with 1 NO contact and 1 NC contact for 230 V/400 V AC for 5TT58 and 5TT50",29.83,"ΤΕΜ",1,"EP",1,"5TT59101","5TT Ρελέ ράγας"]
["5UB1520","DELTA i-system SCHUKO socket outlet with increased touch protection green, 55x 55 mm",28.41,"ΤΕΜ",1,"EP",1,"5UB1520","Διακοπτικό Υλικό"]
["5UB1858","DELTA style, titanium white SCHUKO socket outlet 10/16 A 250 V with overvoltage protection Labeling field, Function displays with increased touch protection cover plate 68 x 68 mm",208.66,"ΤΕΜ",1,"EP",1,"5UB1858","Διακοπτικό Υλικό"]
["5UB1970-0CM01","I-system,Schuko+ 2USB Chargers Carbon Metallic",129.32,"ΤΕΜ",1,"EP",1,"5UB19700CM01","Διακοπτικό Υλικό"]
["6AG1052-1FB08-7BA1","SIPLUS LOGO! 230RCE based on 6ED1052-1FB08-0BA1 with conformal coating, -25â€¦+60 Â°C, start up -20 Â°C, logic module, display power supply / I/O: 115V/230V/relay, 8 DI/4 DQ, memory 400 blocks, modularly expandable, Ethernet, integrated web server, data log, user-defined web pages, standard microSD card for LOGO! Soft Comfort V8.3 or higher older projects executable cloud connection in all LOGO! 8.3 basic units",476,"ΤΕΜ",1,"LOGO!",1,"6AG10521FB087BA1","LOGO!"]
["6AG1128-3KB06-4AX1","SIPLUS HMI MTP1000 Unified Comfort, with conformal coating based on 6AV2128-3KB06-0AX1",3472,"ΤΕΜ",1,"SIMATIC",1,"6AG11283KB064AX1","Βιομηχανικός αυτοματισμός SIMATIC"]
["6AG1155-6BA01-7CN0","SIPLUS ET 200SP IM155-6DP HF based on 6ES7155-6BA01-0CN0 with conformal coating, -40â€¦+70 Â°C, bundle PROFIBUS IM, max. 32 I/O modules and 16 ET 200AL modules, multi hot swap, bundle consists of: interface module (6AG1155-6BU01-7CN0), server module (6AG1193-6PA00-7AA0), PROFIBUS plug",734,"ΤΕΜ",1,"SIMATIC",1,"6AG11556BA017CN0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6AG1210-1PE28-2AL0","SIPLUS G120 PM240-2 IP20-FSE-A-400V 45 kW based on 6SL3210-1PE28-8AL0 with conformal coating, -20â€¦+50 Â°C, with integrated class A filter with integrated braking chopper 380-480 V 3 AC +10/-20% 47-63 Hz power high overload: 37 kW at 200% 3 s,150% 57 s,100% 240 s power low overload: 45 kW at 150% 3 s,110% 57 s,100% 240 s 551x 275x 237 (HxWxD), FSE design, degree of protection IP20 without CU and operating unit released as of CU FW version V4.7 HF8",10717,"ΤΕΜ",1,"SIMATIC",1,"6AG12101PE282AL0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6AG1222-1BF32-4XB0","SIPLUS S7-1200 SM 1222 8DQ based on 6ES7222-1BF32-0XB0 with conformal coating, -20â€¦+60 Â°C, digital output 8 DQ, 24 V DC, transistor 0.5 A",191,"ΤΕΜ",1,"S7-1200",1,"6AG12221BF324XB0","Βιομηχανικός αυτοματισμός SIMATIC S7-1200"]
["6AG1416-5HS06-7AB0","SIPLUS S7-400 CPU 416-5H based on 6ES7416-5HS06-0AB0 with conformal coating, -25â€¦+70 Â°C, central processing unit for S7-400H and S7-400F/FH, 5 interfaces: 1x MPI/DP, 1x DP, 1x PN and 2 for SYNC modules, 16 MB memory (512 KB data/512 KB program)",23311,"ΤΕΜ",1,"SIMATIC",1,"6AG14165HS067AB0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6AG1503-2CB00-2AA0","SIPLUS NET OLM/G11 V4.0 based on 6GK1503-2CB00 with conformal coating, -25â€¦+60 Â°C,",1283,"ΤΕΜ",1,"SIMATIC",1,"6AG15032CB002AA0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6AG1620-0AA00-7AA0","SIPLUS PN/CAN link based on 6BK1620-0AA00-0AA0 with conformal coating, -40â€¦+70 Â°C, from PROFINET to CAN/CANopen networks CAN 2.0 A/B CANopen manager to CiA301/302 CANopen slave to CiA301/302 IP20",1075,"ΤΕΜ",1,"SIMATIC",1,"6AG16200AA007AA0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6AG1952-1AL00-4AA0","SIPLUS S7-400 RAM card 2 MB based on 6ES7952-1AL00-0AA0 with conformal coating, 0â€¦+60 Â°C,",1735,"ΤΕΜ",1,"SIMATIC",1,"6AG19521AL004AA0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6AG2155-6AU01-1CN0","SIPLUS ET 200SP IM155-6PN HF T1 rail based on 6ES7155-6AU01-0CN0 with conformal coating, -25â€¦+60 Â°C, OT1 with ST1/2 (+70 Â°C fÃ¼r 10 minutes), 2-port interface module 1 slot for BusAdapter, max. 64 I/O modules, and 16 ET 200AL modules, S2 redundancy, multi hot swap, 0.25 ms, isochronous mode, optional PN strain relief, including server module (6AG1193-6PA00-7AA0)",727,"ΤΕΜ",1,"SIMATIC",1,"6AG21556AU011CN0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6AG2515-2RM00-4AB0","SIPLUS S7-1500 CPU 1515R-2 PN TX rail based on 6ES7515-2RM00-0AB0 with conformal coating, -40â€¦+70 Â°C, OT4 with ST1/2 (+85 Â°C for 10 minutes), heat sink, no PS usable, central processing unit without display with work memory 500 KB for program and 3 MB for data, 1st interface: PROFINET with 2-port switch, 2nd interface: PROFINET RT, SIMATIC Memory Card required",8152,"ΤΕΜ",1,"SIMATIC",1,"6AG25152RM004AB0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6AU1435-2AA00-0AA0","SIMOTION D435-2 DP",8606,"ΤΕΜ",1,"GMC",1,"6AU14352AA000AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6AU1820-1AA20-0AB0","Technology option Position",854,"ΤΕΜ",1,"GMC",1,"6AU18201AA200AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6AV2102-0AA08-0AA7","SIMATIC STEP 7 Basic/Professional V18, WinCC Basic/Comfort/Advanced, WinCC Unified Trial V18, engineering software in the TIA Portal; Trial License; software and documentation on DVD; class A; 9 languages: de,en,zh included, fr,es,it,ru,jp,ko as download; for configuration of SIMATIC Panels, SIMATIC S7-1200/1500, SIMATIC S7-300/400/WinAC, WinCC Runtime Advanced, WinCC Unified PC Runtime. please observe product release: support.industry.siemens.com entry ID: 109813587 ******************************* content: set (2x DVD)",32.1,"ΤΕΜ",1,"SIMATIC",1,"6AV21020AA080AA7","Βιομηχανικός αυτοματισμός SIMATIC"]
["6AV2103-0HA00-0UY0","SIMATIC WinCC Professional 4096 PowerTags, SUS (UCL download) Software Update Service, automatic follow-up deliveries of upgrades and service packs for one year with automatic extension; requires current software version; only valid in connection with Unlock Copy License agreement; minimum ordering quantity 20 units ******************************* Email address required for delivery",475,"ΤΕΜ",1,"SIMATIC",1,"6AV21030HA000UY0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6AV2104-0DA07-0AH0","SIMATIC WinCC Runtime Advanced 512 PowerTags V17, runtime software in TIA Portal; Single License; software, documentation and license key for download; class A; 6 languages: de,en,fr,es,it,zh; please observe product release: support.industry.siemens.com entry ID: 109795525 ******************************* Email address required for delivery",1575,"ΤΕΜ",1,"SIMATIC",1,"6AV21040DA070AH0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6AV2104-3DD07-0AE0","SIMATIC WinCC Runtime Advanced 512 PowerTags V17, upgrade V11..V16 -> V17; runtime software in TIA Portal; Single License; software and documentation on DVD; license key on USB flash drive; class A; 6 languages: de,en,fr,es,it,zh; please observe product release: support.industry.siemens.com entry ID: 109795525 ******************************* content: set (1x DVD + 1x USB)",708,"ΤΕΜ",1,"SIMATIC",1,"6AV21043DD070AE0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6AV2105-0HA08-0AH0","SIMATIC WinCC RT Professional, 4096 PowerTags V18, runtime software in TIA Portal, single license, software and documentation download, license key download, class A, 5 languages (de,en,fr,es,it), please observe product release: support.industry.siemens.com entry ID: 109813587 ******************************* Consignee e-mail address required for delivery",5723,"ΤΕΜ",1,"SIMATIC",1,"6AV21050HA080AH0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6AV2107-0GA00-0BB0","SIMATIC WinCC Logging for Runtime Advanced option for WinCC (TIA Portal) runtime software, single license without SW, without documentation license key on USB flash drive, Class A ******************************* Content: 1x USB",342,"ΤΕΜ",1,"SIMATIC",1,"6AV21070GA000BB0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6AV2107-3DB08-0AK0","SIMATIC WinCC RT Professional, client for V18 upgrade V16..V17 -> V18, runtime software in TIA Portal, single license, software and documentation download, license key download, class A, 5 languages (de,en,fr,es,it), please observe product release: support.industry.siemens.com entry ID: 109813587 ******************************* Consignee e-mail address required for delivery",1042,"ΤΕΜ",1,"SIMATIC",1,"6AV21073DB080AK0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6AV2114-2BA07-0AA0","SIMATIC WinCC Runtime Advanced SW package for SIMATIC IPC; 128 PowerTags; includes: WinCC Runtime Advanced 128 PowerTags V17, SIMATIC WinCC Recipes+Logging for Runtime Advanced; supplied only if the same number of SIMATIC IPCs is ordered simultaneously. ******************************* content: 6AV2104-0BA07-0AA0 and 6AV2107-0HA00-0BB0",436,"ΤΕΜ",1,"SIMATIC",1,"6AV21142BA070AA0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6AV2123-3MB32-0AW0","SIMATIC HMI MTP1200, Unified Basic Panel, touch operation, 12\" widescreen TFT display, 16 million colors, PROFINET interface, configurable as of WinCC Unified Basic V18 Update 3, contains open-source software, which is provided free of charge see enclosed Blu-ray",2061,"ΤΕΜ",1,"SIMATIC",1,"6AV21233MB320AW0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6AV2128-3XB06-0AX1","SIMATIC HMI MTP2200, Unified Comfort Panel, touch operation, 21.5\" widescreen TFT display, 16 million colors, PROFINET interface, configurable as of WinCC Unified Comfort V16, contains open-source software, which is provided free of charge see enclosed DVD",5587,"ΤΕΜ",1,"SIMATIC",1,"6AV21283XB060AX1","Βιομηχανικός αυτοματισμός SIMATIC"]
["6AV2145-6GB06-0AA0","SIMATIC HMI KTP700F Mobile Arctic, (extended operating temperature range), 7.0\" TFT display, 800x 480 pixel, 16m colors, key and touch operation, 8 function keys, 1x PROFINET/Industrial Ethernet interface, 1x multimedia card, 1x USB, 1x touch pen, keyswitch, acknowledgement button, emergency shutdown/stop button, configurable from WinCC Comfort V15 SP1",4785,"ΤΕΜ",1,"SIMATIC",1,"6AV21456GB060AA0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6AV2153-2FB00-0LY5","SIMATIC WinCC Unified PC ES 10k PowerTags, SUS (download) Software Update Service, automatic follow-up deliveries of upgrades and service packs for one year with automatic extension; requires current software version ******************************* Email address required for delivery",416,"ΤΕΜ",1,"SIMATIC",1,"6AV21532FB000LY5","Βιομηχανικός αυτοματισμός SIMATIC"]
["6AV2154-1EB31-8AB0","SIMATIC WinCC Unified V18 PC RT 500 upgrade V16..V17-> V18, including upgrade for Parameter Control, Report Execution, Collaboration, Audit Basis runtime software in the TIA Portal; single license; with software and documentation on DVD; license key on USB flash drive; class A; please observe product release: support.industry.siemens.com entry ID: 109807122 ******************************* content: set (1x DVD + 1x USB)",599,"ΤΕΜ",1,"SIMATIC",1,"6AV21541EB318AB0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6AV2154-3JW80-0LX0","WinCC Unified Runtime, Industrial Edge app, 3 client Operate, 12-month license ******************************* Consignee e-mail address required for delivery ******************************* requirement: Industrial Edge Access (6ES7823-0EE00-4AX0) ******************************* Only the specific terms under https://www.siemens.com/iest apply",342,"ΤΕΜ",1,"SIMATIC",1,"6AV21543JW800LX0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6AV2155-1EV01-8AA0","WinCC Unified Package for SIMATIC IPC; consists of: WinCC Unified V18 PC Runtime 500 PowerTags and and Parameter Ctrl. PC; WinCC Unified 200 LoggingTags; WinCC Unified 1 Operate Client; supplied only if the same number of SIMATIC IPCs is ordered simultaneously. Please observe product info: support.industry.siemens.com entry ID: 99860269 ******************************* content: 6AV2154-1EB01-8AA0; 6AV2154-0BP01-8AB0; 2x 6AV2157-2DA00-0AB0; 6AV2157-1JW00-0AB0;",3674,"ΤΕΜ",1,"SIMATIC",1,"6AV21551EV018AA0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6AV2157-0BL01-8AB0","SIMATIC WinCC Unified V18 Audit Basis; option for WinCC Unified, runtime software, single license without software and documentation; license key on USB flash drive; class A; ******************************* content: 1x USB",753,"ΤΕΜ",1,"SIMATIC",1,"6AV21570BL018AB0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6AV2170-2BA00-0AA0","EDGE Runtime for SIMATIC Unified Comfort, runtime software, Single License license key for download, without software and documentation class A, ************************* Email address required for delivery",238,"ΤΕΜ",1,"SIMATIC",1,"6AV21702BA000AA0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6AV2185-8AW50-0AA0","500 mm connecting cable for Advanced elements, only for Extension Unit Advanced (e.g.. RGB button, and others)",45.9,"ΤΕΜ",1,"SIMATIC",1,"6AV21858AW500AA0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6AV6362-2BF00-0BB0","SIMATIC WinCC/WebUX Operate, 10 client licenses (countable), Option f. WinCC V7.3 or higher and WinCC Prof. V14 or higher, runtime software, single license, license key on USB flash drive, Windows 64-bit on the server side required ******************************* Content: 1x USB",13617,"ΤΕΜ",1,"SIMATIC",1,"6AV63622BF000BB0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6AV6362-4AA08-0AK0","WinCC/IndustrialDataBridge V8.0, upgrade from V7.3/7.4 -> V8.0, option for WinCC V8.0 and WinCC Professional V15, Data exchange with databases and OPC servers, runtime/configuration software single license, software and license key download please observe product release: support.industry.siemens.com SIOS entry ID: 109816599 ******************************* Consignee e-mail address required for delivery",507,"ΤΕΜ",1,"SIMATIC",1,"6AV63624AA080AK0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6AV6371-1HV27-5AX0","WinCC/Change-Control V7.5 SP2 for configuration of the Audit Trail (English) with versioning, incl. RT license, option for WinCC V7.5 SP2, runtime/configuration software, single license, software and license key download ******************************* Email address required for delivery",5188,"ΤΕΜ",1,"SIMATIC",1,"6AV63711HV275AX0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6AV6371-2BG17-5AX0","WinCC Powerpack RC 512/2048 for WinCC V7.5 SP2, runtime/configuration license without version change from 512 to 2048 PowerTags, floating license license key on USB flash drive ******************************* Content: 1x USB",2262,"ΤΕΜ",1,"SIMATIC",1,"6AV63712BG175AX0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6AV6372-2DF07-0GH0","SIMATIC EnergyManager Basic/PRO Tag Package 1000; increases the number of tags by 1000 tags; engineering/runtime software; Single License; license key for download; without software and documentation ******************************* Email address required for delivery",29063,"ΤΕΜ",1,"SIMATIC",1,"6AV63722DF070GH0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6AV6372-2DF27-0AH0","SIMATIC EnergyManager Basic/PRO 3 web clients; runtime software; Single License; license key for download; without software and documentation ******************************* Email address required for delivery",2422,"ΤΕΜ",1,"SIMATIC",1,"6AV63722DF270AH0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6AV6377-1CF07-2AF3","FL migration package WinCC/Redundancy V8.0, option for SIMATIC WinCC V8.0, runtime software, single license. This is a special offer and is valid if you replace the previously used product FactoryLink with the product WinCC V8.0. By purchasing this product you obligate yourself to replace the previously used product FactoryLink (following a transitional period of 12 months after receiving this product) with WinCC V8.0 and to no longer use the FactoryLink license. for customer with SUS contract",2291,"ΤΕΜ",1,"SIMATIC",1,"6AV63771CF072AF3","Βιομηχανικός αυτοματισμός SIMATIC"]
["6AV6381-2BF07-5AX0","WinCC system software V7.5 SP2, RT 65536 (65536 PowerTags), runtime software, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Please observe product release: support.industry.siemens.com SIOS entry ID: 109783852 ******************************* Content: Set (3x DVD + 1x USB)",8605,"ΤΕΜ",1,"SIMATIC",1,"6AV63812BF075AX0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6AV6381-2BT07-5AV0","WinCC System SW V7.5 SP2 Asia, RC 102400 (102400 PowerTags), runtime/configuration software on DVD, Floating License, license key on USB flash drive, Class A, 9 languages (de, en,fr,es,it,zh-s,zh-t,kor,jpn); Please observe product release: support.industry.siemens.com SIOS entry ID: 109783852 ******************************* Content: Set (3x DVD + 1x USB)",15754,"ΤΕΜ",1,"SIMATIC",1,"6AV63812BT075AV0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6AV6381-2BV07-5AH0","WinCC system software V7.5 SP2, RC 262144 (262144 PowerTags), runtime/configuration software, Floating License, software including documentation and license key download, class A, 5 languages (de,en,fr,es,it), please observe product release: support.industry.siemens.com SIOS entry ID: 109783852 ******************************* Email address required for delivery",19714,"ΤΕΜ",1,"SIMATIC",1,"6AV63812BV075AH0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6AV6382-2EA08-0AV0","WinCC package for SIMATIC IPC, consists of: WinCC RT 2048, V8.0 Asia; supplied only if the same number of SIMATIC IPCs is ordered on the same order slip ******************************* content: 6AV6381-2BE08-0AV0",4376,"ΤΕΜ",1,"SIMATIC",1,"6AV63822EA080AV0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6AV6645-7AB15-0AS0","Protective film 10\" touch devices, type 10 Protective film 10\" touch devices, Mobile Panel 277 10\" Further information, Quantity and content: see technical data",317,"ΠΑΚ",1,"SIMATIC",1,"6AV66457AB150AS0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6AV6671-2DJ00-0AX0","Protective cover for OP 177B Quantity: see technical data",135,"ΤΕΜ",1,"SIMATIC",1,"6AV66712DJ000AX0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6AV6881-0AP40-0AA0","SIMATIC SD indoor card 32 GB, Secure Digital Card, Indoor use, can be used with TIA V16 or higher, Further information, Quantity and content: see technical data",195,"ΤΕΜ",1,"SIMATIC",1,"6AV68810AP400AA0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6AV6881-0GH21-2BA0","INOX frame 7\" type 1, set stainless steel, type 1 for Panel, Thin Client and IPC more information, quantity and content: see technical specifications",483,"ΤΕΜ",1,"SIMATIC",1,"6AV68810GH212BA0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6AV7672-1CE00-0AA0","protective film 19\" touch devices for Panel PC477, 577, 677, 877, MP 377, Flat Panel Quantity: see technical data",220,"ΠΑΚ",1,"SIMATIC",1,"6AV76721CE000AA0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6AV7674-1LA70-0AA0","Extension Unit box 24\" for mounting on all fully IP65-enclosed 16:9 HMI/IPC devices. Deep empty enclosure for the flexible installation of operator controls, (without pre-perforation)",636,"ΤΕΜ",1,"SIMATIC",1,"6AV76741LA700AA0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6AV7675-4GK50-0GC0","cable set for IFP2200 INOX PRO design (6AV7485-6AE00-0GC0) length: 5 m, consisting of: power cable, earthing connection, display port and USB cable; minimum order quantity 30 units",996,"ΤΕΜ",1,"SIMATIC",30,"6AV76754GK500GC0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6AV9681-1AA08-0AH0","WinCC/PMC-ChannelSuite V8.0 option for WinCC V8.0 runtime software, includes channels for: TDC PMC Industrial Ethernet TCP/IP ****************************** Consignee e-mail address required for delivery",4540,"ΤΕΜ",1,"SIMATIC",1,"6AV96811AA080AH0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6BK1602-8AA15-0AA0","Front flap neutral CPU 1215",40.800000000000004,"ΤΕΜ",1,"SIMATIC",1,"6BK16028AA150AA0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6DL5002-7AB57-0XH0",".",2590,"ΤΕΜ",1,"SIMATIC",1,"6DL50027AB570XH0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6DL5422-8XC15-0BA5","SIMATIC SIPAT, software Test Environment V5.1 SP2 floating license for 1 user R-SW, software on USB flash drive, license key on USB flash drive, Class A 1 language (en) executable in Windows 10 Version 21H2, Windows Server 2022, reference hardware: PC/PG for the license model see product information ********************* content: 3x USB",6800,"ΤΕΜ",1,"SIMATIC",1,"6DL54228XC150BA5","Βιομηχανικός αυτοματισμός SIMATIC"]
["6DL8913-0AL00-0AB5","SIMIT SP V11.0 ENGINEERING S",3414,"ΤΕΜ",1,"SIMATIC",1,"6DL89130AL000AB5","Βιομηχανικός αυτοματισμός SIMATIC"]
["6DL8913-0CK20-0AE5","SIMIT Simulation Platform V10.2 Software Upgrade Engineering L V10.1 -> V10.2 Floating License for 1 user Engineering software Without software, without docum., Class A, 2 languages (de, en), executable in Win 7 SP1, Win 10 LTSB 2015, Win 10 (1909), Win Server 2012 R2 / 2016; For further information see SIMIT V10.2 Readme; Reference HW: PG/PC Content: 1x certificate Order only poss. in connection with: 6DL8900-7XX00-0XB8-Z Y01 Y02",9240,"ΤΕΜ",1,"SIMATIC",1,"6DL89130CK200AE5","Βιομηχανικός αυτοματισμός SIMATIC"]
["6DL8913-0KL10-0AH5","SIMIT Virtual Controller V11.1 software 5 controllers (full) floating license for 1 user engineering software without software, without documentation, class A, 2 languages (de, en), executable in Windows 10 (21H2), Windows 10 LTSC 2019, Windows Server 2016 / 2019, for more information, see SIMIT V11.1 Readme, reference hardware: PC/PG ******_download_product_******* order only in connection with: 6DL8900-7XX00-0XH8-Z Y01 Y02",34104,"ΤΕΜ",1,"SIMATIC",1,"6DL89130KL100AH5","Βιομηχανικός αυτοματισμός SIMATIC"]
["6DL8913-0RX00-0AL8","SIMIT Virtual Controller ______ 5 controllers (Entry / SiS) ____ Software Update Service Within the framework of this contract, you will receive for one year all current software versions. The contract is extended automatically by 1 year if it is not canceled 3 months prior to expiration. Period of delivery and service: 1 year from date of invoice Requirement for conclusion: current version of the software. Content: 1x certificate",2043,"ΤΕΜ",1,"SIMATIC",1,"6DL89130RX000AL8","Βιομηχανικός αυτοματισμός SIMATIC"]
["6DR4004-1RN","Pneumatic terminal strips made of stainless steel 316. For replacement of the pneumatic terminal strip made of aluminum for the SIPART PS2 with Macrolon enclosure, single-action with 1/4-18 NPT",143,"ΤΕΜ",1,"PI5",1,"6DR40041RN","Όργανα Μέτρησης Πεδίου"]
["6DR4004-3ES","Position Transmitter in an aluminum enclosure with Non Contacting Sensor (NCS) and Inductive Limit Switches (ILS), without electronics, without pneumatic block, for separate mounting of position detection at the actuator. Review technical data for explosion protection (ATEX / IECEx / FM / CSA / not Ex d). SIPART PS2 externally mounted in protected area. Prerequisite: SIPART PS2 with integrated Analog Input Module (AIM) as order option or retrofit with 6DR4004-6F/-8F.",1105,"ΤΕΜ",1,"PI5",1,"6DR40043ES","Όργανα Μέτρησης Πεδίου"]
["6DR5110-0NN01-0AA0","SIPART PS2 smart electropneumatic positioner for pneumatic linear and part-turn actuators; 2-wire; 4...20mA with HART-interface; single action; polycarbonate enclosure Standard Without explosion protection. Connection thread el.: 1/2\" NPT / pneu.: 1/4\" NPT Without limit monitor. Analog Output Module (AOM), analog position feedback 4 ... 20 mA. Device plug M12 optionally orderable with -Z D53. Isolating power supply SITRANS I100 separately orderable (7NG4124-1AA00). . Brief instructions English / German / Chinese. Standard / Fail-Safe - Depressurizing the actuator in case of failure of electrical auxiliary power (single acting only). Without Manometer block / Booster.",1612,"ΤΕΜ",1,"PI5",1,"6DR51100NN010AA0","Όργανα Μέτρησης Πεδίου"]
["6DR5623-0FN00-0AA0","SIPART PS2 smart electropneumatic positioner for pneumatic linear and part-turn actuators; FOUNDATION fieldbus operation; double action; Enclosure Aluminium Standard Type of protection (Ex): Intrinsic safety (Ex i), Increased safety (Ex e). Output isolator SITRANS I200 separately orderable (7NG4131-1AA00). Connection thread el.: 1/2\" NPT / pneu.: 1/4\" NPT Without limit monitor. Without option module. . Brief instructions English / German / Chinese. Standard / Fail-Safe - Depressurizing the actuator in case of failure of electrical auxiliary power (single acting only). Without Manometer block / Venting gauge block / Booster.",1819,"ΤΕΜ",1,"PI5",1,"6DR56230FN000AA0","Όργανα Μέτρησης Πεδίου"]
["6ED1057-3BA01-0AA8","LOGO! starter kit 12/24RCE V8.3 with LOGO! 12/24RCE, LOGO! Soft Comfort, WinCC Basic, power supply, screwdriver, in Systainer",405,"ΤΕΜ",1,"LOGO!",1,"6ED10573BA010AA8","LOGO!"]
["6EP3322-6SB00-0AY0","LOGO!Power 12 V / 4.5 A stabilized power supply input: 100-240 V AC output: 12 V DC / 4.5 A *Ex approval no longer available*",123,"ΤΕΜ",1,"LOGO!",1,"6EP33226SB000AY0","τροφοδοτικά LOGO! Power"]
["6EP3437-8SB00-4AY0","SITOP PSU8400 3AC 40A IOL stabilized power supply input: 400-500 V 3 AC output: 24 V DC/40 A with IO-Link connection",538,"ΤΕΜ",1,"SIMATIC",1,"6EP34378SB004AY0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6EP4346-7RB00-0AX0","SITOP RED1200 redundancy module Input/output: 24/48 V DC/20 A Suitable for decoupling two SITOP power supplies with max. 10 A output current each",91.899999999999991,"ΤΕΜ",1,"SIMATIC",1,"6EP43467RB000AX0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6ES5710-8MA11","SIMATIC, Standard mounting rail 35mm, Length 483 mm for 19\" cabinet",34.300000000000004,"ΤΕΜ",1,"SIMATIC",1,"6ES57108MA11","Βιομηχανικός αυτοματισμός SIMATIC"]
["6ES7136-6PA00-0BC0","SIMATIC DP, POWER M. F-PM-E PPM PROFIsafe, for ET 200SP; 24 V DC safe shutdown of DQ and F-DQ up to PL D/SIL2 or PL E/SIL3 2 for safe dig. inputs 1 for safe dig. output PPM",328,"ΤΕΜ",1,"SIMATIC",1,"6ES71366PA000BC0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6ES7143-5AH00-0BA0","SIMATIC ET 200AL, DIQ 16x24 V DC/0.5 A, 8xM12, Degree of protection IP67",286,"ΤΕΜ",1,"SIMATIC",1,"6ES71435AH000BA0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6ES7155-6AU00-0DN0","SIMATIC ET 200SP, PROFINET interface module IM155-6PN High Speed max. 30 I/O modules, 0.125 ms isochronous mode Multi-hotswap, incl. server module",451,"ΤΕΜ",1,"SIMATIC",1,"6ES71556AU000DN0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6ES7193-6CP03-2MA0","SIMATIC ET 200SP, 10 color-coded labels Color code CC03, for I/O modules, module-specific, for 16 push-in terminals",13.4,"ΠΑΚ",1,"SIMATIC",1,"6ES71936CP032MA0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6ES7194-2LH50-0AA0","bus cable for ET connection M8, assembled on both ends with 2x M8 connectors, 4-pole, shielded Length 5.0m",49.9,"ΤΕΜ",1,"SIMATIC",1,"6ES71942LH500AA0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6ES7194-2MH50-0AC0","bus cable for ET connection M8, PUR cable Pre-assembled at one end with 1x M8 connector, 4-pole, shielded Length 5.0m",51.4,"ΤΕΜ",1,"SIMATIC",1,"6ES71942MH500AC0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6ES7194-4BA00-0AA0","SIMATIC DP, Connection module for Power module PM-E ET 200 PRO ECOFAST CU DP, 1x ECOFAST connection RS485",94.399999999999991,"ΤΕΜ",1,"SIMATIC",1,"6ES71944BA000AA0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6ES7212-0AB50-0AA0","EHB control system EMS650S with SIMATIC ET 200SP CPU 1512SP IRD400 Display, Basic cabinet",8464,"ΤΕΜ",1,"SIMATIC",20,"6ES72120AB500AA0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6ES7226-6RA32-0XB0","SIMATIC S7-1200, Relay output SM 1226, F-DQ 2x RLY 5A, PROFIsafe, 70 mm overall width, up to PL E (ISO 13849-1)/ SIL3 (IEC 61508)",312,"ΤΕΜ",1,"S7-1200",1,"6ES72266RA320XB0","Βιομηχανικός αυτοματισμός SIMATIC S7-1200"]
["6ES7292-2AG40-0XA2","SIMATIC S7-1200, spare part, I/O terminal block tin-coated, in push-in design, coded center, 7 pins for voltage terminal SM 1238 Energy Meter (4 units with 7 pins each)",30.6,"ΠΑΚ",1,"S7-1200",1,"6ES72922AG400XA2","Βιομηχανικός αυτοματισμός SIMATIC S7-1200"]
["6ES7307-1EA01-0AA0","SIMATIC S7-300 Regulated power supply PS307 input: 120/230 V AC, output: 24 V/5 A DC",255,"ΤΕΜ",1,"SIMATIC",1,"6ES73071EA010AA0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6ES7340-1AH02-0AE0","SIMATIC S7-300, CP 340 Communications processor with RS232C interface (RS-232-C) incl. configuration package on CD",858,"ΤΕΜ",1,"SIMATIC",1,"6ES73401AH020AE0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6ES7392-1BN00-0AA0","S7-300, Terminal block in spring-loaded connection system for 64-channel modules of the S7-300, 2 units per packing unit",254,"ΠΑΚ",1,"SIMATIC",1,"6ES73921BN000AA0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6ES7431-1KF20-0AB0","SIMATIC S7-400, analog input SM 431, isolated 8 AI, resolution 14 bit, U/IResistor 8 AI, cycle time 0.416 ms",2456,"ΤΕΜ",1,"SIMATIC",1,"6ES74311KF200AB0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6ES7492-2BX00-0AA0","SIMATIC S7-400, 10 labeling sheets A4, color: light-beige, 4 labeling strips/sheet, for signal modules, material: foil, pre-perforated, for printing with laser printer, 10 sheets per packing unit",86.3,"ΤΕΜ",1,"SIMATIC",1,"6ES74922BX000AA0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6ES7518-4FX00-1AB0","SIMATIC S7-1500F, CPU 1518F-4 PN/DP MFP, central processing unit with C/C++ Runtime pre-installed, 9 MB work memory for program and 60 MB for data, 1st interface: PROFINET IRT with 2-port switch, 2nd interface: PROFINET RT, 3rd interface: Ethernet, 4th interface: PROFIBUS, 1 ns bit performance, SIMATIC Memory Card required",9967,"ΤΕΜ",1,"SIMATIC",1,"6ES75184FX001AB0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6ES7547-1JF00-0AB0","S7-1500, CM 8xIO-Link, communication module IO-Link Master V1.1; Front connector (screw terminals or push-in) to be ordered separately",674,"ΤΕΜ",1,"SIMATIC",1,"6ES75471JF000AB0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6ES7648-2AK80-1PA0","SIMATIC IPC memory expansion memory module 16 GB (1x 16 GB), DDR4 2400 SD-RAM, SODIMM, ECC for SIMATIC Box IPC427E, SIMATIC Panel IPC477E, Field PG M5",1124,"ΤΕΜ",1,"SIMATIC",1,"6ES76482AK801PA0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6ES7651-5EX28-0YK5","SIMATIC PDM, software upgrade package from PDM V8.X to V8.2, floating license for 1 user, E-SW, without SW, without documentation, License key download, Class A, 6 languages (de, en, fr, it, sp, ch), executable in Windows 7 Ultimate/Server 2008 R2 Reference HW: PC/PG ******************************* E-mail address required for delivery",800,"ΤΕΜ",1,"SIMATIC",1,"6ES76515EX280YK5","Βιομηχανικός αυτοματισμός SIMATIC"]
["6ES7658-1ET18-0YH5","SIMATIC STEP 7 CFC V18.0, Advanced Engineering, software, floating license for 1 user, license key and software download, class A, 6 languages (de, en, fr, it, es, zh), executable in Windows 10 LTSC 2019, Windows Server 2019, reference HW: PC/PG ******************************* email address required for for delivery",1741,"ΤΕΜ",1,"SIMATIC",1,"6ES76581ET180YH5","Βιομηχανικός αυτοματισμός SIMATIC"]
["6ES7658-3XX01-7YV8","SIMATIC PDM ___________________ Software Update Service Basic Download, within the framework of this contract, you will receive for one year all up-to-date software versions. The contract is extended automatically by 1 year if it is not canceled 3 months prior to expiration. Period of delivery and service: 1 year from date of invoice Requirement for conclusion: current version of the software ******************************* E-mail address mandatory for delivery",198,"ΤΕΜ",1,"SIMATIC",1,"6ES76583XX017YV8","Βιομηχανικός αυτοματισμός SIMATIC"]
["6ES7810-4CC12-0KE5","SIMATIC S7 STEP7 V5.7 SP1 Chin. Upgrade, floating license for 1 user, engineering software, software and documentation on DVD, license key on USB flash drive, class A, 2 languages (en,zh), executable in Windows Server 2016/2019/2022, Windows 10/11 Professional, Windows 10/11 Enterprise reference hardware: S7-300/400, C7 ******************************* content: set (1x DVD + 1x USB)",728,"ΤΕΜ",1,"SIMATIC",1,"6ES78104CC120KE5","Βιομηχανικός αυτοματισμός SIMATIC"]
["6ES7813-0CC00-2YX1","SIMATIC, CFC EPL Royalty, Single license for 1 installation E-SW, without SW and without documentation, Class A, only valid in connection with enterprise license agreement, requires EPL Master",2634,"ΤΕΜ",1,"SIMATIC",1,"6ES78130CC002YX1","Βιομηχανικός αυτοματισμός SIMATIC"]
["6ES7822-1AA04-2XC6","SIMATIC STEP 7 Professional V18 powerpack & upgrade V5.X-> V18/2021 SR1 Combo UCL (2021 SR1 and TIA Portal) for one installation; engineering software; software and documentation on DVD; master license on USB flash drive; UCL agreement required ******************************* content: set (5x DVD + 1x USB)",1003,"ΤΕΜ",1,"SIMATIC",1,"6ES78221AA042XC6","Βιομηχανικός αυτοματισμός SIMATIC"]
["6ES7823-0ME00-1DA0","SIMATIC Modul Application Creator Adv.",858,"ΤΕΜ",1,"SIMATIC",1,"6ES78230ME001DA0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6ES7823-1EE23-0YE5","TIA Portal Teamcenter Gateway upgrade V14..V18->V19; download - floating license class A; compatibility exclusively between TIA Portal V19 and Teamcenter >V13/V14 ******************************* Consignee e-mail address required for delivery",484,"ΤΕΜ",1,"SIMATIC",1,"6ES78231EE230YE5","Βιομηχανικός αυτοματισμός SIMATIC"]
["6ES7833-1FA16-2YA0","SIMATIC S7, F-programming tool, STEP 7 Safety Advanced Combo; V16 Distributed Safety V5.4, Unlock Copy License (UCL); package for one installation; engineering software; software and documentation on DVD; master license key on CD-ROM; 2 languages (de, en), Class A; only valid in connection with UCL agreement ******************************* Content: set (3x DVD + 1x CD)",674,"ΤΕΜ",1,"SIMATIC",1,"6ES78331FA162YA0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6ES7840-0CE00-2YX2","SIMATIC S7, S7 PDIAG EPL Maintenance DL, price for maintenance of a royalty for 12 months, only valid in connection with enterprise license agreement; requires EPL master ******************************* consignee e-mail address required for delivery",387,"ΤΕΜ",1,"SIMATIC",1,"6ES78400CE002YX2","Βιομηχανικός αυτοματισμός SIMATIC"]
["6ES7900-5AA00-0XA0","SIMATIC PG, power supply cable 3 m For Field PG M6/M5/M4/M2 for Germany; France; Spain; The Netherlands; Belgium; Sweden; Austria; Finland",14.299999999999999,"ΤΕΜ",1,"SIMATIC",1,"6ES79005AA000XA0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6ES7922-3BC50-0AB0","Front connector for SIMATIC S7-300 20 pole (6ES7392-1AJ00-0AA0) with 20 single cores 0.5 mm2, Single cores H05V-K, Screw version VPE=1 unit L = 2.5 m",106,"ΤΕΜ",1,"SIMATIC",1,"6ES79223BC500AB0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6ES7922-3BD20-0UC0","Front connector for SIMATIC S7-300 40 pole (6ES7392-1AM00-0AA0) with 40 single cores AWG 20, Single cores UL / CSA AWM Style 1007/1569 FT2 TR64 Screw version VPE=1 unit L = 3.2 m",167,"ΤΕΜ",1,"SIMATIC",1,"6ES79223BD200UC0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6ES7923-0BG50-0CB0","Connecting cable unshielded for SIMATIC S7-300/1500 between front connector module and Connection module 16x0.14 mm2 with IDC connectors, Length = 6.5 m",42.800000000000004,"ΤΕΜ",1,"SIMATIC",1,"6ES79230BG500CB0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6ES7923-5CB00-0EB0","Connecting cable unshielded f. SIMATIC S7-300/1500 0.14 mm2 between front connector module 4 x 16 pole and connection module 1 x 50 pole with IDC connectors, L = 10.0 m",140,"ΤΕΜ",1,"SIMATIC",1,"6ES79235CB000EB0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6ES7928-5EA20-4AA0","Enclosure cover for Connection modules TPA 32-bit / TP3 Fuse / TPRI / TPOO 8-bit Packaging Unit = 4 PCs",27.3,"ΠΑΚ",1,"SIMATIC",1,"6ES79285EA204AA0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6ES7960-1BC00-5AA5","SIMATIC S7-1500H SYNC connecting cable fiber-optic cable 2 m",112,"ΤΕΜ",1,"SIMATIC",1,"6ES79601BC005AA5","Βιομηχανικός αυτοματισμός SIMATIC"]
["6FC5095-0AA10-0AP1","LOG BOOK A. LICENSE CERTIFICATE SINUMERIK/SIROTEC/SIMODRIVE EDITION 06.09 (replaces EDITION 11.02)",41.2,"ΤΕΜ",1,"GMC",1,"6FC50950AA100AP1","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FC5260-0AY00-0AG2","SINUMERIK 828D/840D SL 810D/840DI/840D CAD READER FOR PC SOFTWARE UPDATE SERVICE",1436,"ΤΕΜ",1,"GMC",1,"6FC52600AY000AG2","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FC5370-3AT03-0AA0","SINUMERIK 808D, Extended T PPU 151.3 horizontal with current software version English layout",4859,"ΤΕΜ",1,"GMC",1,"6FC53703AT030AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FC5397-0HP40-0BA1","SINUMERIK SINUMERIK 840D sl documentation PLC Function Manual edition 10/20, English",300,"ΤΕΜ",1,"GMC",1,"6FC53970HP400BA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FC5397-1GP40-0DA1","SINUMERIK Documentation SINUMERIK 840D sl Step 7 Toolbox V16 Getting Started Edition 12/19, French",68.5,"ΤΕΜ",1,"GMC",1,"6FC53971GP400DA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FC5397-2AP40-6CA1","SINUMERIK 840D SL DOCUMENTATION IBN CNC: NCK, PLC, DRIVE COMMISSIONING MANUAL EDITION 12/17, Italian",204,"ΤΕΜ",1,"GMC",1,"6FC53972AP406CA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FC5397-6BP40-6BA2","SINUMERIK 840D SL DOCUMENTATION TOOL MANAGEMENT FUNCTION MANUAL EDITION 08/18, English",315,"ΤΕΜ",1,"GMC",1,"6FC53976BP406BA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FC5397-7EP40-0BA4","SINUMERIK 808D, Extended Documentation Function Manual Edition 07/18 English,",60.800000000000004,"ΤΕΜ",1,"GMC",1,"6FC53977EP400BA4","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FC5397-8FP40-0RA1","SINUMERIK 840D sl Documentation SINUMERIK Integrate Create MyHMI/WinCC V15 (Update 1) Configuration Manual Edition 04/18, Chin. Simpl.",97.6,"ΤΕΜ",1,"GMC",1,"6FC53978FP400RA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FC5398-1BP40-6FA2","SINUMERIK 840D SL DOCUMENTATION FUNDAMENTALS PROGRAMMING MANUAL EDITION 08/18, Swedish",315,"ΤΕΜ",1,"GMC",1,"6FC53981BP406FA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FC5398-3DP10-0BA2","SINUMERIK 808D, Extended T Documentation MM+ Programming Manual Edition 08/15, English",62,"ΤΕΜ",1,"GMC",1,"6FC53983DP100BA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FC5398-4DP10-0BA6","SINUMERIK 808D, Extended Documentation Milling Programming Manual Edition 09/17, English",60.800000000000004,"ΤΕΜ",1,"GMC",1,"6FC53984DP100BA6","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FC5398-6AP40-6CA2","SINUMERIK 840D sl Documentation Operating Manual Universal Edition 12/19, Italian",226,"ΤΕΜ",1,"GMC",1,"6FC53986AP406CA2","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FC5398-6DP10-0BA5","SINUMERIK 808D, Extended Documentation Diagnostics Manual Edition 09/17, English",60.800000000000004,"ΤΕΜ",1,"GMC",1,"6FC53986DP100BA5","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FC5398-7CP41-0CA0","SINUMERIK 840D SL/828D DOCUMENTATION OPERATING MANUAL MILLING EDITION 08/18, Italian",315,"ΤΕΜ",1,"GMC",1,"6FC53987CP410CA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FC5398-8BP40-3RA1","SINUMERIK 828D, SINAMICS S120, ALARMS DOCUMENTATION DIAGNOSTICS MANUAL EDITION 03/13, Chin. Simpl.",256,"ΤΕΜ",1,"GMC",1,"6FC53988BP403RA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FC5398-8CP40-3CA1","SINUMERIK 840D SL/828D DOCUMENTATION OPERATING MANUAL TURNING EDITION 03/13, Italian",295,"ΤΕΜ",1,"GMC",1,"6FC53988CP403CA1","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FC5398-8CP40-5QA3","SINUMERIK 840D SL/828D DOCUMENTATION OPERATING MANUAL TURNING EDITION 10/15, Hungarian",337,"ΤΕΜ",1,"GMC",1,"6FC53988CP405QA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FC5398-8CP41-0XE0","SINUMERIK 840D sl/828D documentation Operating Manual Turning Edition 08/18, Thai",315,"ΤΕΜ",1,"GMC",1,"6FC53988CP410XE0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FC5548-0BA21-0AA0","SINAMICS V70 Bus terminal PPU-V70",39.1,"ΤΕΜ",1,"GMC",1,"6FC55480BA210AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FC5800-0AM77-0YH0","SINUMERIK 828D/840D sl determine the tool requirement software option delivery of an electronic license (PDF) ******************************* email address for delivery is absolutely essential",2055,"ΤΕΜ",1,"GMC",1,"6FC58000AM770YH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FC5800-0AS21-0YH0","SINUMERIK 840D sl nodding compensation advanced software option delivery of an electronic license (PDF) ******************************* email address for delivery is absolutely essential",4361,"ΤΕΜ",1,"GMC",1,"6FC58000AS210YH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FC5800-0BM65-0YB0","SINUMERIK ONE Run MyCC /CLCX Option for Free Direction software option. Delivery of an electronic license (PDF). Email address for delivery is essential.",2063,"ΤΕΜ",1,"GMC",1,"6FC58000BM650YB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FC5800-0BP57-0YB0","SINUMERIK ONE interpolation turning software option delivery of an electronic license (PDF) ******************************* email address for delivery is absolutely essential",3139,"ΤΕΜ",1,"GMC",1,"6FC58000BP570YB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FC5822-1XF00-0VB0","SINUMERIK MC CNC-SW 8-3 with ECO package delivery of an electronic license (PDF) ------------------------------- email address for delivery required",6780,"ΤΕΜ",1,"GMC",1,"6FC58221XF000VB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FC5860-0YC44-0YA8","SINUMERIK 828D/840D sl HMI language extensions 828D CNC-SW 4.95 SP1 840D SL CNC-SW 4.95 SP1 SINUMERIK Operate 4.95 SP1 DVD edition 08/22 without license",525,"ΤΕΜ",1,"GMC",1,"6FC58600YC440YA8","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FC6350-2GD00-0YA0","Optimize MyProgramming /NX CAM Editor Integrated CAM - CNC process Single license for connection of a machine Order via SISW Product ID MCS5170 In certain regions, this product is only sold via SISW/SW",4865,"ΤΕΜ",1,"GMC",1,"6FC63502GD000YA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX2001-2HC00","INCREM. ENCODER 6FX2001-2HC00 WITH RS 422 (TTL), 2000 P/R SYNCHRO-FLANGE SHAFT 6MM OPERATING VOLTAGE: 10-30 V AXIAL FLANGE CONNECTOR",504,"ΤΕΜ",1,"GMC",1,"6FX20012HC00","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX2001-2ND60","INCREM. ENCODER 6FX2001-2ND60 WITH RS 422 (TTL), 3600 P/R, CLAMP FLANGE SHAFT 10MM OPERATING VOLTAGE 10 - 30 V UNIVERSAL CABLE OUTGOING AXIAL / RADIAL CABLE 1M WITH CONNECTOR",504,"ΤΕΜ",1,"GMC",1,"6FX20012ND60","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX2001-5AD02","PRINTED CIRCUIT BOARD  SMI 20 6FX2001-5AD02 FOR DRIVE-CLIQ BUILT-ON ENCODER WITH SPRING PLUG CONNECTION QUANTITY 1",297,"ΤΕΜ",1,"GMC",1,"6FX20015AD02","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX2002-1DC00-1AE0","Signal cable pre-assembled type: 6FX2002-1DC00 (SINAMICS Drive CLiQ) Connector IP20/IP20, without 24 V Length (m)= 0 + 0 + 4 + 0",174,"ΤΕΜ",1,"GMC",1,"6FX20021DC001AE0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX2002-1DC00-1BA0","Signal cable pre-assembled type: 6FX2002-1DC00 (SINAMICS Drive CLiQ) Connector IP20/IP20, without 24 V Length (m)= 0 + 10 + 0 + 0",231,"ΤΕΜ",1,"GMC",1,"6FX20021DC001BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX2002-1DC00-1BD1","Signal cable pre-assembled type: 6FX2002-1DC00 (SINAMICS Drive CLiQ) Connector IP20/IP20, without 24 V Length (m)= 0 + 10 + 3 + 0,1",270,"ΤΕΜ",1,"GMC",1,"6FX20021DC001BD1","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX2002-1DC00-1CJ2","Signal cable pre-assembled type: 6FX2002-1DC00 (SINAMICS Drive CLiQ) Connector IP20/IP20, without 24 V Length (m)= 0 + 20 + 8 + 0,2",414,"ΤΕΜ",1,"GMC",1,"6FX20021DC001CJ2","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX2003-0AA50","Signal connector, D-sub type: 6FX2003-0AA50 50-pole socket Screw interlock Cable terminal 5.5-12 mm Pack=3 units",201,"ΠΑΚ",1,"GMC",1,"6FX20030AA50","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX2003-3HN00","Hybrid plug, NDE direction For S-1FL2 SH20/30/40",170,"ΤΕΜ",1,"GMC",1,"6FX20033HN00","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX2008-1DC00-1FA0","Signal cable sold by the meter type: 6FX2008-1DC00 (DRIVE-CLiQ) 2x2X0.22 C not trailable Type of delivery: Ring Dmax=7.0 mm, Length (m)=50",530,"ΤΕΜ",1,"GMC",1,"6FX20081DC001FA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX3002-5CL02-1AD0","Power cable pre-assembled 4x 1.5, for motor S-1FL6 HI 400 V with V70/V90 frame size AA and MOTION-CONNECT 300 No UL for connector on the motor side Dmax=8.1 mm Length (m)=3 m Version with straight connector Mot",139,"ΤΕΜ",1,"GMC",1,"6FX30025CL021AD0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX3502-2XB12-1AH0","Encoder cable, Preassembled 3x2x0.25 for motor S-1FL2 SH45/65/90 with S200, MOTION-CONNECT 350 Length(m)=7m Dmax encoder=7.0mm 1 million bending times",203,"ΤΕΜ",1,"GMC",1,"6FX35022XB121AH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX3502-5DK32-1AD0","Power cable, Preassembled 4x0.75 + 2x0.38 for motor S-1FL2 SH48/52 with S200, MOTION-CONNECT 350 Length(m)=3m Dmax power=7.5mm w. brake 1 million bending times",254,"ΤΕΜ",1,"GMC",1,"6FX35025DK321AD0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX3802-5CL12-1AH0","Power cable, Preassembled 4x2.5 for motor S-1FL2 SH45/65/90 with S200, MOTION-CONNECT 380 Length(m)=7m Dmax power=9mm w.o. brake 5 million bending times",281,"ΤΕΜ",1,"GMC",1,"6FX38025CL121AH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-2AH00-1CK0","Signal cable pre-assembled (HTL in motor 1-ph.) 4x 2x 0.34+4x 0.5 C UL/CSA, DESINA MOTION-CONNECT 500 Dmax=9.3 mm TYPE: 6FX5002-2AH00 LENGTH (M) = 0 + 20 + 9 + 0",332,"ΤΕΜ",1,"GMC",1,"6FX50022AH001CK0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-2AH00-1HG0","Signal cable pre-assembled (HTL in motor 1-ph.) 4x 2x 0.34+4x 0.5 C UL/CSA, DESINA MOTION-CONNECT 500 Dmax=9.3 mm TYPE: 6FX5002-2AH00 LENGTH (M) = 0 + 70 + 6 + 0",703,"ΤΕΜ",1,"GMC",1,"6FX50022AH001HG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-2CA12-1AC0","Signal cable pre-assembled type: 6FX5002-2CA12 (HTL and TTL encoder) 4x 2x 0.34+4x 0.5 C without sub-D connector UL/CSA, DESINA MOTION-CONNECT 500 Dmax=9.3 mm Length (m)= 0 + 0 + 2 + 0",123,"ΤΕΜ",1,"GMC",1,"6FX50022CA121AC0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-2CA31-2AA0","signal cable pre-assembled (encoder voltage signal) 3x 2x 0.14+4x 0.14+2x0.5+4x 0.23 C UL/CSA, DESINA MOTION-CONNECT 500 Dmax=9.9 mm TYPE: 6FX5002-2CA31 LENGTH (M) = 100 + 0 + 0 + 0",1170,"ΤΕΜ",1,"GMC",1,"6FX50022CA312AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-2CC11-1AG0","Signal cable pre-assembled (SSI absolute encoder SSI6FX2001-5) 4x 2x 0.34+4x 0.5 C UL/CSA, DESINA MOTION-CONNECT 500 Dmax=9.3 mm TYPE: 6FX5002-2CC11 LENGTH (M) = 0 + 0 + 6 + 0",192,"ΤΕΜ",1,"GMC",1,"6FX50022CC111AG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-2CF02-1BG0","Signal cable pre-assembled (resolver in motor) 3x 2x 0.14+4x 0.14+2x0.5 C UL/CSA, DESINA MOTION-CONNECT 500 Dmax=9.3 mm Length (m)= TYPE: 6FX5002-2CF02 LENGTH (M) = 0 + 10 + 6 + 0",298,"ΤΕΜ",1,"GMC",1,"6FX50022CF021BG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-2CF02-2AJ0","Signal cable pre-assembled (resolver in motor) 3x 2x 0.14+4x 0.14+2x0.5 C UL/CSA, DESINA MOTION-CONNECT 500 Dmax=9.3 mm Length (m)= TYPE: 6FX5002-2CF02 LENGTH (M) = 100 + 0 + 8 + 0",1080,"ΤΕΜ",1,"GMC",1,"6FX50022CF022AJ0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-2CH00-1GA0","Signal cable pre-assembled (810D/611D to encoder EnDat) 3x 2x 0.14+4x 0.14+2x0.5 C UL/CSA, DESINA MOTION-CONNECT 500 Dmax=9.3 mm TYPE: 6FX5002-2CH00 LENGTH (M) = 0 + 60 + 0 + 0",678,"ΤΕΜ",1,"GMC",1,"6FX50022CH001GA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-2CN20-1CA0","Signal cable pre-assembled Incr. encoder with C/D tracks in the motor, SPEED-CONNECT M17 3x 2x 0.14+4x 0.14+2x0.5+ 4x 0.22 C MOTION-CONNECT 500 UL/CSA, DESINA Dmax=9.8 mm TYPE: 6FX5002-2CN20 LENGTH (M) = 0 + 20 + 0 + 0",492,"ΤΕΜ",1,"GMC",1,"6FX50022CN201CA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-2DC00-1CA0","Signal cable pre-assembled type: 6FX5002-2DC00 (SINAMICS Drive CLiQ) connector IP20/IP20, with 24 V MOTION-CONNECT 500 Length (m)= 0 + 20 + 0 + 0",305,"ΤΕΜ",1,"GMC",1,"6FX50022DC001CA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-2DC10-1AH5","Signal cable pre-assembled type: 6FX5002-2DC10 (SINAMICS DRIVE-CLiQ) plug IP20/IP67, with 24 V MOTION-CONNECT 500 length (m)= 0 + 0 + 7 + 0,5",218,"ΤΕΜ",1,"GMC",1,"6FX50022DC101AH5","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-2DC10-1BG7","Signal cable pre-assembled type: 6FX5002-2DC10 (SINAMICS DRIVE-CLiQ) plug IP20/IP67, with 24 V MOTION-CONNECT 500 length (m)= 0 + 10 + 6 + 0,7",300,"ΤΕΜ",1,"GMC",1,"6FX50022DC101BG7","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-2DC10-1HB0","Signal cable pre-assembled type: 6FX5002-2DC10 (SINAMICS DRIVE-CLiQ) plug IP20/IP67, with 24 V MOTION-CONNECT 500 length (m)= 0 + 70 + 1 + 0",793,"ΤΕΜ",1,"GMC",1,"6FX50022DC101HB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-2DC20-1CB0","Signal cable pre-assembled type: 6FX5002-2DC20 (SINAMICS DRIVE-CLiQ) plug IP67/IP67, with 24 V MOTION-CONNECT 500 length (m)= 0 + 20 + 1 + 0",360,"ΤΕΜ",1,"GMC",1,"6FX50022DC201CB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-2DC30-1AD0","DRIVE-CLiQ cable type: 6FX5002-2DC30 Pre-assembled for direct measuring systems with 24 V Connector RJ45, IP20 and Mating connector M12, IP67 MOTION-CONNECT 500 UL/CSA, DESINA Dmax=7.1 mm Length (m)=3 + 0",181,"ΤΕΜ",1,"GMC",1,"6FX50022DC301AD0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-2DC34-1AG0","DRIVE-CLiQ extension type: 6FX5002-2DC34 for base 6FX8002-2DC30-.... with 24 V Connector and mating connector M12, IP67 MOTION-CONNECT 500 UL/CSA, DESINA Dmax=7.1 mm Length (m)=6 + 0",233,"ΤΕΜ",1,"GMC",1,"6FX50022DC341AG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-2DC46-1JA0","Signal cable pre-assembled Type: 6FX5002-2DC46 DRIVE-CLiQ with 24 V M12 female/ M17 male speed-connect-ready MOTION-CONNECT 500 Dmax=7.1 mm length (m)=80",1094,"ΤΕΜ",1,"GMC",1,"6FX50022DC461JA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-2EQ10-1AH0","signal cable pre-assembled (absolute encoder in motor) 3x 2x 0.14+4x 0.14+2x0.5+4x 0.23 C UL/CSA, DESINA MOTION-CONNECT 500 Dmax=9.9 mm TYPE: 6FX5002-2EQ10 LENGTH (M) = 0 + 0 + 7 + 0",219,"ΤΕΜ",1,"GMC",1,"6FX50022EQ101AH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-2EQ14-1AC0","signal cable, pre-assembled Extension (absolute encoder in motor) 3x 2x 0.14+4x 0.14+2x0.5+4x 0.22 C UL/CSA, DESINA MOTION-CONNECT 500 Dmax=9.9 mm TYPE: 6FX5002-2EQ14 LENGTH (M) = 0 + 0 + 2 + 0",218,"ΤΕΜ",1,"GMC",1,"6FX50022EQ141AC0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-2XQ10-1BA0","Signal cable pre-assembled type: 6FX5002-2xQ10 Basis 6FX5002-2EQ10 UL/CSA (EX motors) 100 Â°C DESINA MOTION-CONNECT 500 Dmax=9.9 mm, Length (m)= 0 + 10 + 0 + 0",274,"ΤΕΜ",1,"GMC",1,"6FX50022XQ101BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5CG01-1AB6","Power cable pre-assembled type: 6FX5002-5CG01 4x 1.5 C, Connector Sz. 1 (SINAMICS AC Drive) UL/CSA, DESINA MOTION-CONNECT 500 Dmax=8.4 mm 0 + 0 + 1 + 0,6",175,"ΤΕΜ",1,"GMC",1,"6FX50025CG011AB6","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5CG01-1CF0","Power cable pre-assembled type: 6FX5002-5CG01 4x 1.5 C, Connector Sz. 1 (SINAMICS AC Drive) UL/CSA, DESINA MOTION-CONNECT 500 Dmax=8.4 mm 0 + 20 + 5 + 0",311,"ΤΕΜ",1,"GMC",1,"6FX50025CG011CF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5CG01-1GF0","Power cable pre-assembled type: 6FX5002-5CG01 4x 1.5 C, Connector Sz. 1 (SINAMICS AC Drive) UL/CSA, DESINA MOTION-CONNECT 500 Dmax=8.4 mm 0 + 60 + 5 + 0",546,"ΤΕΜ",1,"GMC",1,"6FX50025CG011GF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5CG10-1EB0","Power cable pre-assembled 4x 1.5 C SPEED-CONNECT connector Sz. 1 (SINAMICS AC Drive) UL/CSA DESINA MOTION-CONNECT 500 Dmax=8.4 mm TYPE: 6FX5002-5CG10 LENGTH (M) = + 0 + 40 + 1 + 0",407,"ΤΕΜ",1,"GMC",1,"6FX50025CG101EB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5CG22-1CF0","Power cable pre-assembled 4x 1.5 C Speed connect connector Sz. 1.5 (SINAMICS AC Drive) UL/CSA DESINA MOTION-CONNECT 500 Dmax=8.4 mm TYPE: 6FX5002-5CG22 LENGTH (M) = + 0 + 20 + 5 + 0",503,"ΤΕΜ",1,"GMC",1,"6FX50025CG221CF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5CG42-1BA0","Power cable pre-assembled 4x 4 C Speed connect connector Sz. 1.5 (SINAMICS AC Drive) UL/CSA DESINA MOTION-CONNECT 500 Dmax=11.4 mm TYPE: 6FX5002-5CG42 LENGTH (M) = + 0 + 10 + 0 + 0",378,"ΤΕΜ",1,"GMC",1,"6FX50025CG421BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5CG61-1BA0","Power cable pre-assembled type: 6FX5002-5CG61 4x 10 C, Connector Sz. 1.5 (SINAMICS AC Drive) UL/CSA DESINA MOTION-CONNECT 500 Dmax=20.0 mm 0 + 10 + 0 + 0",500,"ΤΕΜ",1,"GMC",1,"6FX50025CG611BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5CN06-1DD5","Power cable pre-assembled TYPE 6FX5002-5CN06 4X1,5 C, SPEED-CONNECT SIZE 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 500 UL/CSA, DESINA DMAX=8.4 MM LENGTH (M) = + 0 + 30 + 3 + 0.5",430,"ΤΕΜ",1,"GMC",1,"6FX50025CN061DD5","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5CN16-1AJ0","Power cable pre-assembled TYPE 6FX5002-5CN16 4X2.5 C CONNECTOR SPEED-CONNECT SIZE 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 500 UL/CSA, DESINA DMAX=11 MM LENGTH (M) = + 0 + 0 + 8 + 0",312,"ΤΕΜ",1,"GMC",1,"6FX50025CN161AJ0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5CN27-1BH0","Power cable pre-assembled TYPE 6FX5002-5CN27 4X1,5C, SPEED-CONNECT SIZE 0.5 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 500 UL/CSA, DESINA DMAX=8.4 MM LENGTH (M) = + 0 + 10 + 7 + 0",347,"ΤΕΜ",1,"GMC",1,"6FX50025CN271BH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5CR73-1AK0","Power cable pre-assembled type: 6FX5002-5CR73 4x 35 C, M50 screw connection for SINAMICS S120 Power Module MOTION-CONNECT 500 UL/CSA, DESINA Dmax=31.5 mm, Length (m)= 0 0 + 9 + 0",1047,"ΤΕΜ",1,"GMC",1,"6FX50025CR731AK0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5CS06-1BA0","Power cable pre-assembled TYPE 6FX5002-5CS06 4X1,5 C, CONN. FULL THREAD S. 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 500 UL/CSA, DESINA DMAX=8.4 MM LENGTH (M) = + 0 + 10 + 0 + 0",307,"ΤΕΜ",1,"GMC",1,"6FX50025CS061BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5CS16-1BF0","Power cable pre-assembled TYPE 6FX5002-5CS16 4X2.5 C CONNECTOR FULL THREAD SIZE 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 500 UL/CSA, DESINA DMAX=11 MM LENGTH (M) = + 0 + 10 + 5 + 0",359,"ΤΕΜ",1,"GMC",1,"6FX50025CS161BF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5CS23-1DA0","Power cable pre-assembled type: 6FX5002-5CS23 (1FT/1FK for SINAMICS) 4x 16 C Connector Sz. 3/ring cable lug UL/CSA, DESINA MOTION-CONNECT 500 Dmax=24.2 mm; Length (m)= 0 + 30 + 0 + 0",1983,"ΤΕΜ",1,"GMC",1,"6FX50025CS231DA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5CS66-1HA0","Power cable pre-assembled Type 6FX5002-5CS66 4x 10 C Connector, full thread, Sz. 1.5 for SINAMICS S120 booksize Motor Module C/D types MOTION-CONNECT 500 UL/CSA, DESINA Dmax=20 mm Length (m)= + 0 + 70 + 0 + 0",1690,"ΤΕΜ",1,"GMC",1,"6FX50025CS661HA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5DA15-1BA0","power cable, pre-assembled, Extension 4x 2.5+(2x1.5) C, Connector Sz. 1 (1FT/1FK to 611/810D/SIMOVERT) UL/CSA, DESINA MOTION-CONNECT 500 Dmax=14.3 mm TYPE: 6FX5002-5DA15 LENGTH (M) = 0 + 10 + 0 + 0",459,"ΤΕΜ",1,"GMC",1,"6FX50025DA151BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5DG01-1AD7","Power cable pre-assembled type: 6FX5002-5DG01 4x 1.5+(2x1.5) C, Connector Sz. 1 (SINAMICS AC Drive) UL/CSA, DESINA MOTION-CONNECT 500 Dmax=10.8 mm 0 + 0 + 3 + 0,7",229,"ΤΕΜ",1,"GMC",1,"6FX50025DG011AD7","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5DG10-1CJ0","Power cable pre-assembled 4x 1.5+(2x1.5) C SPEED-CONNECT connector Sz. 1 (SINAMICS AC Drive) UL/CSA DESINA MOTION-CONNECT 500 Dmax=10.8 mm TYPE: 6FX5002-5DG10 LENGTH (M) = + 0 + 20 + 8 + 0",473,"ΤΕΜ",1,"GMC",1,"6FX50025DG101CJ0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5DG13-1BF0","Power cable pre-assembled type: 6FX5002-5DG13 4x 10+(2x1.5) C, Connector size 3 (1FT/1FK to 611/810D/SIMOVERT) UL/CSA DESINA MOTION-CONNECT 500 Dmax=20.8 mm 0 + 10 + 5 + 0",1388,"ΤΕΜ",1,"GMC",1,"6FX50025DG131BF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5DG32-1AC0","Power cable pre-assembled 4x 2.5+(2x1.5) C Speed connect connector Sz. 1.5 (SINAMICS AC Drive) UL/CSA DESINA MOTION-CONNECT 500 Dmax=12.4 mm TYPE: 6FX5002-5DG32 LENGTH (M) = + 0 + 0 + 2 + 0",310,"ΤΕΜ",1,"GMC",1,"6FX50025DG321AC0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5DG61-1AJ0","power cable, pre-assembled type: 6FX5002-5DG61 4x 10+(2x1.5) C, Connector Sz. 1.5 (SINAMICS AC Drive) UL/CSA, DESINA MOTION-CONNECT 500 Dmax=20.6 mm 0 + 0 + 8 + 0",622,"ΤΕΜ",1,"GMC",1,"6FX50025DG611AJ0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5DN05-1BF0","power cable, pre-assembled, Extension 4x 1.5+(2x1.5) C SPEED-CONNECT connector Sz. 1 (SIMODRIVE) UL/CSA DESINA MOTION-CONNECT 500 Dmax=13.1 mm TYPE: 6FX5002-5DN05 LENGTH (M) = + 0 + 10 + 5 + 0",468,"ΤΕΜ",1,"GMC",1,"6FX50025DN051BF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5DN06-1BG0","Power cable pre-assembled TYPE 6FX5002-5DN06 4X1.5, (2X1.5)C C CONNECTOR SPEED-CONNECT SIZE 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 500 UL/CSA, DESINA DMAX = 10.8 MM LENGTH (M) = + 0 + 10 + 6 + 0",408,"ΤΕΜ",1,"GMC",1,"6FX50025DN061BG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5DN30-1AJ0","Power cable pre-assembled 4x 1.5+(2x1.5) C C SPEED-CONNECT Sz. 0.5 for SINAMICS motor Module UL/CSA DESINA MOTION-CONNECT 500 Dmax=10.8 mm TYPE: 6FX5002-5DN30 LENGTH (M) = 0 + 0 + 8 + 0",285,"ΤΕΜ",1,"GMC",1,"6FX50025DN301AJ0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5DQ38-1BA0","power cable, pre-assembled, Extension 4x 2.5+(2x1.5) C Speed connect connector Sz. 1.5 (SIMODRIVE) UL/CSA DESINA MOTION-CONNECT 500 Dmax=14.3 mm TYPE: 6FX5002-5DQ38 LENGTH (M) = + 0 + 10 + 0 + 0",625,"ΤΕΜ",1,"GMC",1,"6FX50025DQ381BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5DS06-1BF0","Power cable pre-assembled TYPE 6FX5002-5DS06 4X1.5, (2X1.5)C C CONNECTOR FULL THREAD SIZE 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 500 UL/CSA, DESINA DMAX = 10.8 MM LENGTH (M) = + 0 + 10 + 5 + 0",400,"ΤΕΜ",1,"GMC",1,"6FX50025DS061BF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-5DS46-1AE0","Power cable pre-assembled TYPE 6FX5002-5DS46 4X4, (2X1.5)C C CONNECTOR FULL THREAD SIZE 1.5 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 500 UL/CSA, DESINA DMAX=14 MM LENGTH (M) = + 0 + 0 + 4 + 0",406,"ΤΕΜ",1,"GMC",1,"6FX50025DS461AE0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-8QE08-1BA0","Single cable extension 4G0.75+2x0.5+4x0.2 C Socket and plug Speed-Connect M17 female / M17 male UL/CSA DESINA MOTION-CONNECT 500 Dmax= 10.5 mm, length (m)= 0 + 10 + 0 + 0",473,"ΤΕΜ",1,"GMC",1,"6FX50028QE081BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-8QE21-1EJ0","Single cable extension 4G2.5+1Q0,2STC+1P1.5C-C SPEED-CONNECT M23 connector UL/CSA DESINA MOTION-CONNECT 500 Dmax.=13.3 mm Length (m)= 0 + 40 + 8 + 0",2189,"ΤΕΜ",1,"GMC",1,"6FX50028QE211EJ0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-8QN11-1FA0","Single cable connection pre-assembled 4G1,5+1Q0,2STC+1P1,5C-C SPEED-CONNECT connector M23 Cores with end sleeve Data cable with IX connector UL/CSA DESINA Motion-Connect 500 Dmax.=12.3 mm length (m)=50",1366,"ΤΕΜ",1,"GMC",1,"6FX50028QN111FA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5002-8QN21-1ED0","Single cable pre-assembled 4G2,5+1Q0,2STC+1P1,5C-C SPEED-CONNECT connector M23 Cores with end sleeve Data cable with IX connector UL/CSA DESINA Motion-Connect 500 Dmax.=13.3 mm length(M)= 0 + 40 + 3 + 0",1889,"ΤΕΜ",1,"GMC",1,"6FX50028QN211ED0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5008-1BA61-1AF0","Power cable sold by the meter type: 6FX5008-1BA61 4x 16+2x 1.5 C UL/CSA, DESINA MOTION-CONNECT 500 Type of delivery: up to 29 m ring from 30 m drum Dmax=25.0 mm, Length (m)= 0 + 0 + 5 + 0",253,"ΤΕΜ",1,"GMC",1,"6FX50081BA611AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5008-1BB05-1KK0","Power cable sold by the meter type: 6FX5008-1BB05 4x 95 C UL/CSA, DESINA MOTION-CONNECT 500 Dmax=51.7 mm, Length (m)= 0 + 90 + 9 + 0",21964,"ΤΕΜ",1,"GMC",1,"6FX50081BB051KK0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5008-1BB25-1CA0","Power cable sold by the meter type: 6FX5008-1BB25 4x 25 C UL/CSA, DESINA MOTION-CONNECT 500 Type of delivery: up to 19 m ring from 20 m drum Dmax=28.0 mm, Length (m)= 0 + 20 + 0 + 0",1077,"ΤΕΜ",1,"GMC",1,"6FX50081BB251CA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5008-1BB35-1FG0","Power cable sold by the meter type: 6FX5008-1BB35 4x 35 C UL/CSA, DESINA MOTION-CONNECT 500 Type of delivery: up to 14 m ring from 15 m drum Dmax=31.5 mm, Length (m)= 0 + 50 + 6 + 0",4252,"ΤΕΜ",1,"GMC",1,"6FX50081BB351FG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5008-1BB50-1FF0","Power cable sold by the meter type: 6FX5008-1BB50 4x 50 C UL/CSA, DESINA MOTION-CONNECT 500 Type of delivery: to 9 m ring from 10 m drum Dmax=38.0 mm, Length (m)= 0 + 50 + 5 + 0",5641,"ΤΕΜ",1,"GMC",1,"6FX50081BB501FF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5008-1BB61-1AH0","Power cable sold by the meter type: 6FX5008-1BB61 4x 16 C UL/CSA, DESINA MOTION-CONNECT 500 Type of delivery: up to 29 m ring from 30 m drum Dmax=24.2 mm, Length (m)= 0 + 0 + 7 + 0",285,"ΤΕΜ",1,"GMC",1,"6FX50081BB611AH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5008-1BB61-1FA0","Power cable sold by the meter type: 6FX5008-1BB61 4x 16 C UL/CSA, DESINA MOTION-CONNECT 500 Type of delivery: up to 29 m ring from 30 m drum Dmax=24.2 mm, Length (m)= 0 + 50 + 0 + 0",1932,"ΤΕΜ",1,"GMC",1,"6FX50081BB611FA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5012-2CF02-1DH0","Signal cable pre-assembled (resolver in motor) 3x 2x 0.14+4x 0.14+2x0.5 C UL/CSA, DESINA MOTION-CONNECT 500 Dmax=9.3 mm Length (m)= TYPE: 6FX5012-2CF02 MODULE SIDE: CRIMPED CONTACTS, CONNECTOR HOUSING INCLUDED LENGTH (M) = 0 + 30 + 7 + 0",477,"ΤΕΜ",1,"GMC",1,"6FX50122CF021DH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5012-2EQ10-1CF1","signal cable pre-assembled (absolute encoder in motor) 3x 2x 0.14+4x 0.14+2x0.5+4x 0.23 C UL/CSA, DESINA MOTION-CONNECT 500 Dmax=9.9 mm TYPE: 6FX5012-2EQ10 MODULE SIDE: CRIMPED CONTACTS, CONNECTOR HOUSING INCLUDED LENGTH (M) = 0 + 20 + 5 + 0,1",405,"ΤΕΜ",1,"GMC",1,"6FX50122EQ101CF1","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5022-5CN06-1CF0","Power cable pre-assembled TYPE 6FX5022-5CN06 4X1,5 C, SPEED-CONNECT SIZE 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES PREPARED CONDUCTORS W/O SINAMICS CONNECTOR MOTION-CONNECT 500 UL/CSA, DESINA DMAX=8.4 MM LENGTH (M) = + 0 + 20 + 5 + 0",344,"ΤΕΜ",1,"GMC",1,"6FX50225CN061CF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX5042-2CR00-1EF0","Signal cable pre-assembled for incr. encoder TTL 5 V DC 6FX2001-2, full thread M23 4x 2x 0.34+4x 0.5 C MOTION-CONNECT 500 UL/CSA DESINA Dmax=9.3 mm TYPE: 6FX5042-2CR00 MOTOR SIDE: CRIMPED CONTACTS, CONNECTOR HOUSING INCLUDED LENGTH (M) = 0 + 40 + 5 + 0",521,"ΤΕΜ",1,"GMC",1,"6FX50422CR001EF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX7002-5EA48-1AG0","power cable, pre-assembled Extension type: 6FX7002-5EA48 4x 4+(4x 0.5) C, Connector Sz. 1.5 (1FN to 611) trailable UL/CSA DESINA MOTION-CONNECT 700 Dmax=16.6 mm, Length (m)= 0 + 0 + 6 + 0",693,"ΤΕΜ",1,"GMC",1,"6FX70025EA481AG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX7002-5EB11-1AF0","power cable pre-assembled type: 6FX7002-5EB11 4x 2.5+(4x 0.5) C, Connector Sz. 1 (1FN to 611) trailable UL/CSA DESINA MOTION-CONNECT 700 Dmax=15.2 mm, Length (m)= 0 + 0 + 5 + 0",363,"ΤΕΜ",1,"GMC",1,"6FX70025EB111AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX7002-5LM80-1BE6","Power cable pre-assembled type: 6FX7002-5LM80 (1FN3) 4x 6+(4x 0.5) C Connector Sz. 1.5 and PG MOTION-CONNECT 700 Dmax=18.3 mm, Length (m)= 0 + 10 + 4 + 0,6",923,"ΤΕΜ",1,"GMC",1,"6FX70025LM801BE6","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX7008-1BC21-1FA0","Power cable sold by the meter type: 6FX7008-1BC21 4x 2.5+4x 0.5 C for linear motors trailable UL/CSA DESINA MOTION-CONNECT 700 Type of delivery: Ring Dmax=15.2 mm, Length (m)=50",1867,"ΤΕΜ",1,"GMC",1,"6FX70081BC211FA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-1AA01-1BA0","Signal cable pre-assembled for RS-232-C Interfaces 4x (2x0.18) C MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=6.7 mm Length (m)= TYPE: 6FX8002-1AA01 LENGTH (M) = + 0 + 10 + 0 + 0",282,"ΤΕΜ",1,"GMC",1,"6FX80021AA011BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2AD04-1CK0","Signal cable pre-assembled for absolute value encoder SSI and EnDat 5V DC, also extension for base 6FX8002-2AD00-XXXX 3x (2x0.14) C+4x 0.14+2x0.5 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.2 mm TYPE: 6FX8002-2AD04 LENGTH (M) = 0 + 20 + 9 + 0",629,"ΤΕΜ",1,"GMC",1,"6FX80022AD041CK0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2BB01-1AB0","Signal cable pre-assembled type: 6FX80.2-2BB01 for electr. handwheel for FM-NC 4x (2x0.18) C MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=6.7 mm Length (m)= LENGTH (M) = + 0 + 0 + 1 + 0",73.399999999999991,"ΤΕΜ",1,"GMC",1,"6FX80022BB011AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2CA11-1CG0","Signal cable pre-assembled for incremental encoder sin/cos 1 Vpp 6FX2001-3 4x (2x0.34)+4x 0.5 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=9.3 mm Length (m)= type: 6FX8002-2CA11 length (m)= + 0 + 20 + 6 + 0",415,"ΤΕΜ",1,"GMC",1,"6FX80022CA111CG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2CA12-1DA0","Signal cable pre-assembled type: 6FX8002-2CA12 for incremental encoder HTL 24 V, 6FX2001-4 4x (2x0.34)+4x 0.5 C Connector full thread M23 without sub-D connector MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=9.3 mm Length (m)= 0 + 30 + 0 + 0",401,"ΤΕΜ",1,"GMC",1,"6FX80022CA121DA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2CA31-1DA0","Signal cable pre-assembled for incr. encoder with C/D tracks integrated into the motor 3x (2x0.14) C+4x 0.14+2x0.5 +4x 0.22 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.8 mm Length (m)= TYPE: 6FX8002-2CA31 LENGTH (M) = + 0 + 30 + 0 + 0",615,"ΤΕΜ",1,"GMC",1,"6FX80022CA311DA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2CA31-1ED0","Signal cable pre-assembled for incr. encoder with C/D tracks integrated into the motor 3x (2x0.14) C+4x 0.14+2x0.5 +4x 0.22 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.8 mm Length (m)= TYPE: 6FX8002-2CA31 LENGTH (M) = + 0 + 40 + 3 + 0",800,"ΤΕΜ",1,"GMC",1,"6FX80022CA311ED0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2CA34-1CA0","Signal cable extension for base 2CA31-2CA80 or -2CA88 3x (2x0.14) C + 4x 0.14+2x0.5+4x 0.22 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.8 mm Length (m)= TYPE: 6FX8002-2CA34 LENGTH (M) = 0 + 20 + 0 + 0",504,"ΤΕΜ",1,"GMC",1,"6FX80022CA341CA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2CA80-2AA0","Signal cable pre-assembled type: 6FX8002-2CA80 for incremental encoder SIN/COS 1 VPP without C and D track 3x (2x0.14) C+4x 0.14+2x0.5 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=9.2 mm Length (m)= 100 + 0 + 0 + 0",1610,"ΤΕΜ",1,"GMC",1,"6FX80022CA802AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2CC11-1DA0","Signal cable pre-assembled for absolute encoder SSI 6FX2001-5 4x (2x0.34)+4x 0.5 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.3 mm Length (m)= TYPE: 6FX8002-2CC11 LENGTH (M) = 0 + 30 + 0 + 0",442,"ΤΕΜ",1,"GMC",1,"6FX80022CC111DA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2CF02-1AD0","Signal cable pre-assembled For resolvers 3x (2x0.14) C+4x 0.14+2x0.5 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=9.2 mm Length (m)= TYPE: 6FX8002-2CF02 LENGTH (M) = 0 + 0 + 3 + 0",229,"ΤΕΜ",1,"GMC",1,"6FX80022CF021AD0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2CF02-1BH0","Signal cable pre-assembled For resolvers 3x (2x0.14) C+4x 0.14+2x0.5 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=9.2 mm Length (m)= TYPE: 6FX8002-2CF02 LENGTH (M) = 0 + 10 + 7 + 0",427,"ΤΕΜ",1,"GMC",1,"6FX80022CF021BH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2CG00-1AD0","Signal cable pre-assembled for incremental encoder SIN/COS 1VPP, 6FX2001-3 4x (2x0.34)+4x 0.5 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.3 mm Length (m)= TYPE: 6FX8002-2CG00 LENGTH (M) = 0 + 0 + 3 + 0",174,"ΤΕΜ",1,"GMC",1,"6FX80022CG001AD0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2CH00-1AE0","Signal cable pre-assembled for absolute encoder EnDat 6FX2001-5 3x (2x0.14) C+4x 0.14+2x0.5 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.2 mm Length (m)= TYPE: 6FX8002-2CH00 LENGTH (M) = 0 + 0 + 4 + 0",249,"ΤΕΜ",1,"GMC",1,"6FX80022CH001AE0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2CH00-1HG0","Signal cable pre-assembled for absolute encoder EnDat 6FX2001-5 3x (2x0.14) C+4x 0.14+2x0.5 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.2 mm Length (m)= TYPE: 6FX8002-2CH00 LENGTH (M) = 0 + 70 + 6 + 0",1267,"ΤΕΜ",1,"GMC",1,"6FX80022CH001HG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2CQ31-1CF0","Signal cable pre-assembled for incr. encoder with C/D tracks integrated into the motor 3x (2x0.14) C+4x 0.14+2x0.5 +4x 0.22 C SPEED-CONNECT connector M23 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.8 mm Length (m)= TYPE: 6FX8002-2CQ31 LENGTH (M) = + 0 + 20 + 5 + 0",546,"ΤΕΜ",1,"GMC",1,"6FX80022CQ311CF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2DC10-1AA4","signal cable, pre-assembled type: 6FX8002-2DC10 DRIVE-CLiQ with 24 V plug RJ45 IP20 on module side and IP67 on motor side MOTION-CONNECT 800PLUS released only up to 75 m length Dmax=7.1 mm length (m)= 0 + 0 + 0 + 0,4",178,"ΤΕΜ",1,"GMC",1,"6FX80022DC101AA4","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2DC10-1AH5","signal cable, pre-assembled type: 6FX8002-2DC10 DRIVE-CLiQ with 24 V plug RJ45 IP20 on module side and IP67 on motor side MOTION-CONNECT 800PLUS released only up to 75 m length Dmax=7.1 mm length (m)= 0 + 0 + 7 + 0,5",255,"ΤΕΜ",1,"GMC",1,"6FX80022DC101AH5","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2DC10-1BD3","signal cable, pre-assembled type: 6FX8002-2DC10 DRIVE-CLiQ with 24 V plug RJ45 IP20 on module side and IP67 on motor side MOTION-CONNECT 800PLUS released only up to 75 m length Dmax=7.1 mm length (m)= 0 + 10 + 3 + 0,3",320,"ΤΕΜ",1,"GMC",1,"6FX80022DC101BD3","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2DC10-1EF0","signal cable, pre-assembled type: 6FX8002-2DC10 DRIVE-CLiQ with 24 V plug RJ45 IP20 on module side and IP67 on motor side MOTION-CONNECT 800PLUS released only up to 75 m length Dmax=7.1 mm length (m)= 0 + 40 + 5 + 0",659,"ΤΕΜ",1,"GMC",1,"6FX80022DC101EF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2DC20-1AG8","Signal cable pre-assembled type: 6FX8002-2DC20 DRIVE-CLiQ with 24 V plug RJ45 IP67 on both sides released only up to 75 m length Dmax=7.1 mm length (m)= 0 + 0 + 6 + 0,8",269,"ΤΕΜ",1,"GMC",1,"6FX80022DC201AG8","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2DC20-1DB0","Signal cable pre-assembled type: 6FX8002-2DC20 DRIVE-CLiQ with 24 V plug RJ45 IP67 on both sides released only up to 75 m length Dmax=7.1 mm length (m)= 0 + 30 + 1 + 0",531,"ΤΕΜ",1,"GMC",1,"6FX80022DC201DB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2DC34-1CF0","DRIVE-CLiQ extension for base Type: 6FX8002-2DC34 DRIVE-CLiQ with 24V M12 male/M12 female MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=7.1mm Length (m)=25",482,"ΤΕΜ",1,"GMC",1,"6FX80022DC341CF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2DC38-1BH0","DRIVE-CLiQ adapter cable pre-fabricated type: 6FX8002-2DC38 DRIVE-CLiQ with 24 V M12 male/ RJ45 IP67 MOTION-CONNECT 800PLUS MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=7.1 mm length (m)=17",397,"ΤΕΜ",1,"GMC",1,"6FX80022DC381BH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2DC40-1AK5","Signal cable pre-assembled type: 6FX8002-2DC40 DRIVE-CLiQ with 24 V M17 female SPEED-CONNECT/ RJ45 IP20 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=7.1 mm Length (m)= 0 + 0 + 9 + 0,5",313,"ΤΕΜ",1,"GMC",1,"6FX80022DC401AK5","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2DC46-1BE0","Signal cable pre-assembled type: 6FX8002-2DC46 DRIVE-CLiQ with 24 V M12 female/ M17 male speed-connect-ready MOTION-CONNECT 800PLUS UL/CSA, DESINA, Trailable Dmax=7.1 mm Length (m)=14",435,"ΤΕΜ",1,"GMC",1,"6FX80022DC461BE0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2EQ10-1AB0","Signal cable pre-assembled for absolute encoder EnDat integrated into the motor 3x (2x0.14) C+4x 0.14+2x0.5 +4x 0.22 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.8 mm Length (m)= TYPE: 6FX8002-2EQ10 LENGTH (M) = 0 + 0 + 1 + 0",207,"ΤΕΜ",1,"GMC",1,"6FX80022EQ101AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2EQ10-1DF0","Signal cable pre-assembled for absolute encoder EnDat integrated into the motor 3x (2x0.14) C+4x 0.14+2x0.5 +4x 0.22 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.8 mm Length (m)= TYPE: 6FX8002-2EQ10 LENGTH (M) = 0 + 30 + 5 + 0",685,"ΤΕΜ",1,"GMC",1,"6FX80022EQ101DF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2EQ10-1FE0","Signal cable pre-assembled for absolute encoder EnDat integrated into the motor 3x (2x0.14) C+4x 0.14+2x0.5 +4x 0.22 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.8 mm Length (m)= TYPE: 6FX8002-2EQ10 LENGTH (M) = 0 + 50 + 4 + 0",953,"ΤΕΜ",1,"GMC",1,"6FX80022EQ101FE0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2EQ20-1AK0","Signal cable pre-assembled type: 6FX8002-2EQ20 for absolute encoder EnDat in motor AH20 with connector full thread M17 (3x 2x 0.14) C+4x 0.14+2x 0.5+4x 0.22 C MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.8 mm Length (m)= 0 + 0 + 9 + 0",342,"ΤΕΜ",1,"GMC",1,"6FX80022EQ201AK0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2FN20-1AF0","Signal cable pre-assembled for resolver in motor AH20 3x (2x0.14) C+4x 0.14+2x0.5 C SPEED-CONNECT connector M17 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=9.2 mm Length (m)= TYPE: 6FX8002-2FN20 LENGTH (M) = 0 + 0 + 5 + 0",291,"ΤΕΜ",1,"GMC",1,"6FX80022FN201AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-2SL10-1AG0","Single line displacement Type: 6FX8002-2SL10 For temperature sensor 3x 2x 0.5+1x 1 C M17 male VG on M17 female VG MOTION-CONNECT 800PLUS UL/CSA, DESINA, trailable Dmax=11 mm Type of delivery: ring length (m)= 0 + 0 + 6 + 0",475,"ΤΕΜ",1,"GMC",1,"6FX80022SL101AG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-4AA41-1AF5","Signal cable pre-assembled I/O devices for 840D and 8 2x (2x0.18) C MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=5.3 mm Length (m)= TYPE: 6FX8002-4AA41 LENGTH (M) = +0 +0 +5 + 0,5",120,"ΤΕΜ",1,"GMC",1,"6FX80024AA411AF5","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5CA15-1BD0","power cable extension 4x 2.5 C MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=11 mm Length (m)= TYPE: 6FX8002-5CA15 LENGTH (M) = 0 + 10 + 3 + 0",591,"ΤΕΜ",1,"GMC",1,"6FX80025CA151BD0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5CA38-1CF0","power cable extension 4x 2.5 C Connector full thread Sz. 1.5 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=11 mm Length (m)= TYPE: 6FX8002-5CA38 LENGTH (M) = 0 + 20 + 5 + 0",993,"ΤΕΜ",1,"GMC",1,"6FX80025CA381CF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5CA58-1AB0","power cable extension 4x 6 C Connector full thread Sz. 1.5 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=14.9 mm Length (m)= TYPE: 6FX8002-5CA58 LENGTH (M) = 0 + 0 + 1 + 0",560,"ΤΕΜ",1,"GMC",1,"6FX80025CA581AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5CA68-1FA8","power cable extension 4x 10 C Connector full thread Sz. 1.5 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=18.2 mm Length (m)= TYPE: 6FX8002-5CA68 LENGTH (M) = 0 + 50 + 0 + 0,8",2784,"ΤΕΜ",1,"GMC",1,"6FX80025CA681FA8","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5CG01-1DA0","Power cable pre-assembled type: 6FX8002-5CG01 4x 1.5 C, connector Full-thread, size 1 for SINAMICS S120 Power Module MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.5 mm, Length (m)= 0 + 30 + 0 + 0",670,"ΤΕΜ",1,"GMC",1,"6FX80025CG011DA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5CG21-1BA0","Power cable pre-assembled type: 6FX8002-5CG21 4x 1.5 C, connector Full thread Sz. 1.5 for SINAMICS S120 Power Module MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.5 mm, Length (m)= + 0 + 10 + 0 + 0",440,"ΤΕΜ",1,"GMC",1,"6FX80025CG211BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5CG51-1BC0","Power cable pre-assembled type: 6FX8002-5CG51 4x 6 C Connector full thread Sz. 1.5 for SINAMICS S120 Power Module and Motor Module Booksize Compact MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=14.9 mm Length (m)= + 0 + 10 + 2 + 0",652,"ΤΕΜ",1,"GMC",1,"6FX80025CG511BC0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5CN05-1AK1","power cable extension 4x 1.5 C, SPEED-CONNECT Sz. 1 MOTION-CONNECT 800PLUS Trailable UL/CSA, DESINA Dmax=9.5 mm TYPE: 6FX8002-5CN05 LENGTH (M) = + 0 + 0 + 9 + 0,1",484,"ΤΕΜ",1,"GMC",1,"6FX80025CN051AK1","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5CN06-1AC5","Power cable pre-assembled TYPE 6FX8002-5CN06 4X1,5 C, SPEED-CONNECT SIZE 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=9.5 MM LENGTH (M) = + 0 + 0 + 2 + 0.5",313,"ΤΕΜ",1,"GMC",1,"6FX80025CN061AC5","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5CN26-1CF0","Power cable pre-assembled TYPE 6FX8002-5CN26 4X1,5C, SPEED-CONNECT SIZE 1.5 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=9.5 MM LENGTH (M) = + 0 + 20 + 5 + 0",688,"ΤΕΜ",1,"GMC",1,"6FX80025CN261CF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5CN36-1BA0","Power cable pre-assembled TYPE 6FX8002-5CN36 4X2.5 C CONNECTOR SPEED-CONNECT S. 1.5 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=11 MM LENGTH (M) = + 0 + 10 + 0 + 0",508,"ΤΕΜ",1,"GMC",1,"6FX80025CN361BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5CN54-1CG0","Power cable pre-assembled 4x 6 C SPEED-CONNECT connector Sz. 1.5 Ring cable lugs on module side for SINAMICS S120 Motor Module MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=14.9 mm Length (m)= TYPE: 6FX8002-5CN54 LENGTH (M) = + 0 + 20 + 6 + 0",1121,"ΤΕΜ",1,"GMC",1,"6FX80025CN541CG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5CN56-1BF0","Power cable pre-assembled TYPE 6FX8002-5CN56 4X6 C CONNECTOR SPEED-CONNECT S. 1.5 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=14.9 MM LENGTH (M) = + 0 + 10 + 5 + 0",732,"ΤΕΜ",1,"GMC",1,"6FX80025CN561BF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5CQ15-1BC0","power cable extension 4x 2.5 C SPEED-CONNECT connector Sz. 1 MOTION-CONNECT 800PLUS trailable; UL/CSA DESINA Dmax=11 mm Length (m)= TYPE: 6FX8002-5CQ15 LENGTH (M) = 0 + 10 + 2 + 0",572,"ΤΕΜ",1,"GMC",1,"6FX80025CQ151BC0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5CQ58-1AF5","power cable extension 4x 6 C SPEED-CONNECT connector Sz. 1.5 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=14.9 mm Length (m)= TYPE: 6FX8002-5CQ58 LENGTH (M) = 0 + 0 + 5 + 0,5",711,"ΤΕΜ",1,"GMC",1,"6FX80025CQ581AF5","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5CR11-1BA0","Power cable pre-assembled type: 6FX8002-5CR11 4x 2.5 C Screw connection M32/1PH810. for SINAMICS S120 Power Module and Motor Mod. Booksize Compact MOTION-CONNECT 800PLUS UL/CSA, DESINA Dmax=11 mm Length (m)= 0 + 10 + 0 + 0",515,"ΤΕΜ",1,"GMC",1,"6FX80025CR111BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5CR43-1BF0","Power cable pre-assembled type: 6FX8002-5CR43 4x 10 C, M50 screw connection SINAMICS S120 Power Module MOTION-CONNECT 800 trailable, UL/CSA, DESINA Dmax=19.4 mm, Length (m)= 0 + 10 + 5 + 0",1018,"ΤΕΜ",1,"GMC",1,"6FX80025CR431BF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5CS06-1AH0","Power cable pre-assembled TYPE 6FX8002-5CS06 4X1,5 C, FULL THREAD SIZE 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=9.5 MM LENGTH (M) = + 0 + 0 + 7 + 0",368,"ΤΕΜ",1,"GMC",1,"6FX80025CS061AH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5CS16-1BA5","Power cable pre-assembled TYPE 6FX8002-5CS16 4X2.5 C, CONN. FULL THREAD S. 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=11 MM LENGTH (M) = + 0 + 10 + 0 + 0.5",449,"ΤΕΜ",1,"GMC",1,"6FX80025CS161BA5","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5CS24-1AK0","Power cable pre-assembled type: 6FX8002-5CS24 4x 16 C Connector full thread Sz. 1.5 for SINAMICS S120 Motor Module Booksize MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=22.3 mm Length (m)= 0 + 0 + 9 + 0",709,"ΤΕΜ",1,"GMC",1,"6FX80025CS241AK0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5CS54-1BE0","Power cable pre-assembled type: 6FX8002-5CS54 4x 6 C Connector full thread Sz. 1.5 Ring cable lugs on module side for SINAMICS S120 Motor Module MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=14.9 mm Length (m)= 0 + 10 + 4 + 0",740,"ΤΕΜ",1,"GMC",1,"6FX80025CS541BE0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5CS64-1BG0","Power cable pre-assembled type: 6FX8002-5CS64 (1FT/1FK/1PH for SINAMICS) 4x 10 C, Connector Sz. 1.5/ Ring cable lug UL/CSA DESINA, Trailable MOTION-CONNECT 800 Dmax=18.4 mm, Length (m)= 0 + 10 + 6 + 0",1035,"ΤΕΜ",1,"GMC",1,"6FX80025CS641BG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5CS64-1EA0","Power cable pre-assembled type: 6FX8002-5CS64 (1FT/1FK/1PH for SINAMICS) 4x 10 C, Connector Sz. 1.5/ Ring cable lug UL/CSA DESINA, Trailable MOTION-CONNECT 800 Dmax=18.4 mm, Length (m)= 0 + 40 + 0 + 0",2128,"ΤΕΜ",1,"GMC",1,"6FX80025CS641EA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DA05-1CB0","power cable extension 4x 1.5+(2x1.5) C, connector Full-thread, size 1 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=12 mm, LONGUEUR (m)= TYPE: 6FX8002-5DA05 LENGTH (M) = 0 + 20 + 1 + 0",789,"ΤΕΜ",1,"GMC",1,"6FX80025DA051CB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DA28-1BD0","power cable extension 4x 1.5+(2x1.5) C, connector Full thread Sz. 1.5 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=12 mm, LONGUEUR (m)= TYPE: 6FX8002-5DA28 LENGTH (M) = 0 + 10 + 3 + 0",807,"ΤΕΜ",1,"GMC",1,"6FX80025DA281BD0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DA38-1AD5","power cable extension 4x 2.5+(2x1.5) C C Connector full thread Sz. 1.5 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=13.8 mm Length (m)= TYPE: 6FX8002-5DA38 LENGTH (M) = 0 + 0 + 3 + 0,5",632,"ΤΕΜ",1,"GMC",1,"6FX80025DA381AD5","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DA48-1AJ0","power cable extension 4x 4+(2x1.5) C, Connector Sz. 1.5 Connector full thread Sz. 1.5 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=15.2 mm LÃ¤nge (m)= TYPE: 6FX8002-5DA48 LENGTH (M) = 0 + 0 + 8 + 0",773,"ΤΕΜ",1,"GMC",1,"6FX80025DA481AJ0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DG01-1AJ0","Power cable pre-assembled type: 6FX8002-5DG01 4x 1.5+(2x1.5) C C, connector Connector full thread Sz. 1 for SINAMICS Power Module MOTION-CONNECT 800PLUS Dmax=12 mm, Length (m)= + 0 + 0 + 8 + 0",374,"ΤΕΜ",1,"GMC",1,"6FX80025DG011AJ0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DG10-1AD0","Power cable pre-assembled 4x 1.5+(2x1.5) C C, connector SPEED-CONNECT Sz. 1 for SINAMICS S120 Power Module MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=12 mm, Length (m)= TYPE: 6FX8002-5DG10 LENGTH (M) = + 0 + 0 + 3 + 0",266,"ΤΕΜ",1,"GMC",1,"6FX80025DG101AD0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DG13-1AF5","Power cable pre-assembled type: 6FX8002-5DG13 4x 10+(2x1.5) C C Connector full thread Sz. 3 for SINAMICS S120 Power Module and Motor Module Booksize compact; MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=20.1 mm LÃ¤nge (m)= 0 + 0 + 5 + 0,5",1270,"ΤΕΜ",1,"GMC",1,"6FX80025DG131AF5","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DG23-1DA0","Power cable pre-assembled type: 6FX8002-5DG23 4x 16+(2x1.5) C C Connector full thread Sz. 3 for SINAMICS S120 Power Module and Motor Mod. Booksize Compact MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=23.8 mm Length (m)= 0 + 30 + 0 + 0",3273,"ΤΕΜ",1,"GMC",1,"6FX80025DG231DA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DG41-1BH0","Power cable pre-assembled type: 6FX8002-5DG41 4x 4+(2x1.5) C C Connector full thread Sz. 1.5 for SINAMICS S120 Power Module and Motor Mod. Booksize Compact MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=15.2 mm LÃ¤nge (m)= 0 + 10 + 7 + 0",967,"ΤΕΜ",1,"GMC",1,"6FX80025DG411BH0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DG52-1BA0","Power cable pre-assembled 4x 6+(2x1.5) C C SPEED-CONNECT connector Sz. 1.5 for SINAMICS S120 Power Module and Motor Mod. Booksize Compact MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=17.3 mm LÃ¤nge (m)= TYPE: 6FX8002-5DG52 LENGTH (M) = + 0 + 10 + 0 + 0",702,"ΤΕΜ",1,"GMC",1,"6FX80025DG521BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DG62-1GA0","Power cable pre-assembled 4x 10+(2x1.5) C C SPEED-CONNECT connector Sz. 1.5 for SINAMICS S120 Power Module and Motor Mod. Booksize Compact MOTION-CONNECT 800PLUS Trailable UL/CSA, DESINA Dmax=20.1 mm LÃ¤nge (m)= TYPE: 6FX8002-5DG62 LENGTH (M) = + 0 + 60 + 0 + 0",4110,"ΤΕΜ",1,"GMC",1,"6FX80025DG621GA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DN06-1BC0","Power cable pre-assembled TYPE 6FX8002-5DN06 4X1,5 , (2X1.5)C C CONNECTOR SPEED-CONNECT SIZE 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=12 MM LENGTH (M) = + 0 + 10 + 2 + 0",504,"ΤΕΜ",1,"GMC",1,"6FX80025DN061BC0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DN06-1CB0","Power cable pre-assembled TYPE 6FX8002-5DN06 4X1,5 , (2X1.5)C C CONNECTOR SPEED-CONNECT SIZE 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=12 MM LENGTH (M) = + 0 + 20 + 1 + 0",663,"ΤΕΜ",1,"GMC",1,"6FX80025DN061CB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DN26-1CB0","Power cable pre-assembled TYPE 6FX8002-5DN26 4X1,5 , (2X1.5)C C CONNECTOR SPEED-CONNECT S. 1.5 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=12 MM LENGTH (M) = + 0 + 20 + 1 + 0",738,"ΤΕΜ",1,"GMC",1,"6FX80025DN261CB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DN30-1CA0","Power cable pre-assembled 4x 1.5+(2x1.5) C C, connector SPEED-CONNECT Sz. 0.5 for SINAMICS S120 Power Module and Motor Module Booksize Compact MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=12 mm, Length (m)= TYPE: 6FX8002-5DN30 LENGTH (M) = + 0 20 + 0 + 0",676,"ΤΕΜ",1,"GMC",1,"6FX80025DN301CA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DN54-1CD0","Power cable pre-assembled 4x 6+(2x1.5) C C SPEED-CONNECT connector Sz. 1.5 Ring cable lugs on module side for SINAMICS S120 Motor Module MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=17.3 mm LÃ¤nge (m)= TYPE: 6FX8002-5DN54 LENGTH (M) = + 0 + 20 + 3 + 0",1222,"ΤΕΜ",1,"GMC",1,"6FX80025DN541CD0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DN56-1CF0","Power cable pre-assembled TYPE 6FX8002-5DN56 4X6 , (2X1.5)C C CONNECTOR SPEED-CONNECT S. 1.5 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=17.3 MM LENGTH (M) = + 0 + 20 + 5 + 0",1156,"ΤΕΜ",1,"GMC",1,"6FX80025DN561CF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DQ38-1AJ0","power cable extension 4x 2.5+(2x1.5) C C SPEED-CONNECT connector Sz. 1.5 MOTION-CONNECT 800PLUS Trailable UL/CSA, DESINA Dmax=13.9 mm Length (m)= TYPE: 6FX8002-5DQ38 LENGTH (M) = + 0 + 0 + 8 + 0",731,"ΤΕΜ",1,"GMC",1,"6FX80025DQ381AJ0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DQ48-1BE5","power cable extension 4x 4+(2x1.5) C C SPEED-CONNECT connector Sz. 1.5 MOTION-CONNECT 800PLUS Trailable UL/CSA, DESINA Dmax=15.2 mm LÃ¤nge (m)= TYPE: 6FX8002-5DQ48 LENGTH (M) = + 0 + 10 + 4 + 0,5",983,"ΤΕΜ",1,"GMC",1,"6FX80025DQ481BE5","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DS06-1FA0","Power cable pre-assembled TYPE 6FX8002-5DS06 4X1,5 , (2X1.5)C C CONNECTOR FULL THREAD SIZE 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=12 MM LENGTH (M) = + 0 + 50 + 0 + 0",1177,"ΤΕΜ",1,"GMC",1,"6FX80025DS061FA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DS17-1CA0","Power cable pre-assembled TYPE 6FX8002-5DS17 4X10 , (2X1.5)C C CONNECTOR FULL THREAD SIZE 3 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=20.1 MM LENGTH (M) = + 0 + 20 + 0 + 0",1801,"ΤΕΜ",1,"GMC",1,"6FX80025DS171CA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DS36-1BC0","Power cable pre-assembled TYPE 6FX8002-5DS36 4X2.5 , (2X1.5)C C, CONNECTOR FULL THREAD SIZE 1.5 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=13.8 MM LENGTH (M) = + 0 + 10 + 2 + 0",617,"ΤΕΜ",1,"GMC",1,"6FX80025DS361BC0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DS46-1AK5","Power cable pre-assembled TYPE 6FX8002-5DS46 4X4, (2X1.5)C C CONNECTOR FULL THREAD SIZE 1.5 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=15.2 MM LENGTH (M) = + 0 + 0 + 9 + 0.5",619,"ΤΕΜ",1,"GMC",1,"6FX80025DS461AK5","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DS56-1BA0","Power cable pre-assembled TYPE 6FX8002-5DS56 4X6 , (2X1.5)C C CONNECTOR FULL THREAD SIZE 1.5 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=17.3 MM LENGTH (M) = + 0 + 10 + 0 + 0",689,"ΤΕΜ",1,"GMC",1,"6FX80025DS561BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DX18-1BE0","power cable extension 4x 10+(2x1.5) C C Connector full thread Sz. 3 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=20.1 mm LÃ¤nge (m)= TYPE: 6FX8002-5DX18 LENGTH (M) = 0 + 10 + 4 + 0",2983,"ΤΕΜ",1,"GMC",1,"6FX80025DX181BE0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-5DX48-1AF0","power cable, pre-assembled Extension 4x 35+(2x1.5) C, Connector size 3 (1FT/1FK to 611/810D/SIMOVERT) trailable UL/CSA DESINA MOTION-CONNECT 800 Dmax=32.0 mm TYPE: 6FX8002-5DX48 LENGTH (M) = 0 + 0 + 5 + 0",3650,"ΤΕΜ",1,"GMC",1,"6FX80025DX481AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-7HY00-1AC8","Pre-assembled hybrid cable type: 6FX8002-7HY00 Power and DRIVE-CLiQ Outlet direction NDE/NDE for SINAMICS S120M MOTION-CONNECT 800PLUS Trailing type, UL/CSA DESINA Dmax=15 mm, Length (m)= 0 + 0 + 2 + 0,8",594,"ΤΕΜ",1,"GMC",1,"6FX80027HY001AC8","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-7HY00-1DK0","Pre-assembled hybrid cable type: 6FX8002-7HY00 Power and DRIVE-CLiQ Outlet direction NDE/NDE for SINAMICS S120M MOTION-CONNECT 800PLUS Trailing type, UL/CSA DESINA Dmax=15 mm, Length (m)= 0 + 30 + 9 + 0",1713,"ΤΕΜ",1,"GMC",1,"6FX80027HY001DK0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-7HY22-1AB6","Pre-assembled hybrid cable type: 6FX8002-7HY22 Power and DRIVE-CLiQ Outlet direction DE/DE for SINAMICS S120M MOTION-CONNECT 800PLUS Trailing type, UL/CSA DESINA Dmax=15 mm, Length (m)= 0 + 0 + 1 + 0,6",563,"ΤΕΜ",1,"GMC",1,"6FX80027HY221AB6","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-7HY22-1AJ0","Pre-assembled hybrid cable type: 6FX8002-7HY22 Power and DRIVE-CLiQ Outlet direction DE/DE for SINAMICS S120M MOTION-CONNECT 800PLUS Trailing type, UL/CSA DESINA Dmax=15 mm, Length (m)= 0 + 0 + 8 + 0",749,"ΤΕΜ",1,"GMC",1,"6FX80027HY221AJ0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-8QE21-1CE0","Single cable extension 4G2.5+1Q0,2STC+1P1.5C-C SPEED-CONNECT M23 connector UL/CSA DESINA MOTION-CONNECT 800PLUS Dmax.=13.3 mm Length (m)= 0 + 20 + 4 + 0",1641,"ΤΕΜ",1,"GMC",1,"6FX80028QE211CE0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-8QE21-1FA0","single cable extension 4G2.5+1Q0,2STC+1P1.5C-C SPEED-CONNECT connector M23 UL/CSA DESINA MOTION-CONNECT 800PLUS Dmax.=13.3 mm length (m)= 50",2986,"ΤΕΜ",1,"GMC",1,"6FX80028QE211FA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-8QN21-1BG0","Single cable connection prefabricated 4G2.5+1Q0,2STC+1P1.5C-C SPEED-CONNECT connector M23 Cores with end sleeve Data cable with IX connector UL/CSA DESINA MOTION-CONNECT 800PLUS Dmax.=13.3 MM Length(M)= 0 + 10 + 6 + 0",1114,"ΤΕΜ",1,"GMC",1,"6FX80028QN211BG0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8002-8QN21-1DE0","Single cable connection prefabricated 4G2.5+1Q0,2STC+1P1.5C-C SPEED-CONNECT connector M23 Cores with end sleeve Data cable with IX connector UL/CSA DESINA MOTION-CONNECT 800PLUS Dmax.=13.3 MM Length(M)= 0 + 30 + 4 + 0",2046,"ΤΕΜ",1,"GMC",1,"6FX80028QN211DE0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8008-1BA25-1FA0","Power cable sold by the meter type: 6FX8008-1BA25 4x 25+(2x1.5) C C MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=27.6 mm Type of delivery: up to 19 m ring from 20 m drum Length (m)= 0 + 50 + 0 + 0",6922,"ΤΕΜ",1,"GMC",1,"6FX80081BA251FA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8008-1BA50-1AE0","Power cable sold by the meter type: 6FX8008-1BA50 4x 50+(2x1.5) C C MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=35 mm Type of delivery: to 9 m ring from 10 m drum Length (m)= 0 + 0 + 4 + 0",1024,"ΤΕΜ",1,"GMC",1,"6FX80081BA501AE0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8008-1BA51-1GB0","Power cable sold by the meter type: 6FX8008-1BA51 4x 10+(2x1.5) C C MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=20.1 mm Type of delivery: up to 39 m ring from 40 m drum Length (m)= 0 + 60 + 1 + 0",3525,"ΤΕΜ",1,"GMC",1,"6FX80081BA511GB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8008-1BB41-1BF0","Power cable sold by the meter type: 6FX8008-1BB41 4x 6.0 C trailable UL/CSA DESINA MOTION-CONNECT 800PLUS Type of delivery: to 69 m ring from 70 m drum Dmax=14.9 mm, Length (m)= 0 + 10 + 5 + 0",516,"ΤΕΜ",1,"GMC",1,"6FX80081BB411BF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8008-1BB51-1DA0","Power cable sold by the meter type: 6FX8008-1BB51 4x 10.0 C trailable UL/CSA DESINA MOTION-CONNECT 800PLUS Type of delivery: Disposable drum Dmax=18.2 mm, Length (m)= 0 + 30 + 0 + 0",1434,"ΤΕΜ",1,"GMC",1,"6FX80081BB511DA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8008-1BD21-2AA0","Signal cable sold by the meter type: 6FX8008-1BD21 4x (2x0.34)+4x 0.5 C MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Type of delivery: Ring Dmax=9.3 mm Length (m)=100",1162,"ΤΕΜ",1,"GMC",1,"6FX80081BD212AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8008-2DC00-2AA0","Signal cable sold by the meter type: 6FX8008-2DC00 (DRIVE-CLiQ) 2x2X0.2+2x 0.38 C trailable UL/CSA DESINA MOTION-CONNECT 800PLUS Type of delivery: Ring Dmax=7.0 mm, Length (m)=100 m",1367,"ΤΕΜ",1,"GMC",1,"6FX80082DC002AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8012-2EQ14-1AD0","Signal cable extension for base 6FX8002-2EQ10-.... 3x (2x0.14) C+4x 0.14+2x0.5 +4x 0.22 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.8 mm Length (m)= TYPE: 6FX8012-2EQ14 MODULE SIDE: CRIMPED CONTACTS, CONNECTOR HOUSING INCLUDED LENGTH (M) = 0 + 0 + 3 + 0",267,"ΤΕΜ",1,"GMC",1,"6FX80122EQ141AD0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8012-5CN06-1CF0","Power cable pre-assembled TYPE 6FX8012-5CN06 4X1,5 C, SPEED-CONNECT SIZE 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES PREPARED CONDUCTORS, SINAMICS CONNECTOR INCLUDED MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=9.5 MM LENGTH (M) = + 0 + 20 + 5 + 0",613,"ΤΕΜ",1,"GMC",1,"6FX80125CN061CF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8012-5CN46-1AE0","Power cable pre-assembled TYPE 6FX8012-5CN46 4X4 C CONNECTOR SPEED-CONNECT S 1.5 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES PREPARED CONDUCTORS, SINAMICS CONNECTOR INCLUDED MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=12,3 MM LENGTH (M) = + 0 + 0 + 4 + 0",433,"ΤΕΜ",1,"GMC",1,"6FX80125CN461AE0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8012-5DN06-1BB0","Power cable pre-assembled TYPE 6FX8012-5DN06 4X1,5 , (2X1.5)C C CONNECTOR SPEED-CONNECT SIZE 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES PREPARED CONDUCTORS, SINAMICS CONNECTOR INCLUDED MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=12 MM LENGTH (M) = + 0 + 10 + 1 + 0",486,"ΤΕΜ",1,"GMC",1,"6FX80125DN061BB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8012-5DS06-1CK0","Power cable pre-assembled TYPE 6FX8012-5DS06 4X1,5 , (2X1.5)C C CONNECTOR FULL THREAD SIZE 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES PREPARED CONDUCTORS, SINAMICS CONNECTOR INCLUDED MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=12 MM LENGTH (M) = + 0 + 20 + 9 + 0",805,"ΤΕΜ",1,"GMC",1,"6FX80125DS061CK0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8022-5CN36-1CF0","Power cable pre-assembled TYPE 6FX8022-5CN36 4X2.5 C CONNECTOR SPEED-CONNECT S 1.5 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES PREPARED CONDUCTORS, W/O SINAMICS CONNECTOR MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=11 MM LENGTH (M) = + 0 + 20 + 5 + 0",706,"ΤΕΜ",1,"GMC",1,"6FX80225CN361CF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6FX8022-5DN06-1AK0","Power cable pre-assembled TYPE 6FX8022-5DN06 4X1,5 , (2X1.5)C C CONNECTOR SPEED-CONNECT SIZE 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES PREPARED CONDUCTORS, W/O SINAMICS CONNECTOR MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=12 MM + 0 + 0 + 9 + 0",411,"ΤΕΜ",1,"GMC",1,"6FX80225DN061AK0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6GF3400-0LT01-7BA1","MV400 LED ring light IR clear Illuminant: LED 850 Nm; Lighting distance: 500 mm..3000 mm, for SIMATIC MV420 and MV440, suitable for lens protection enclosure: 6GF3440-8AC11-8AC12, -8AC13-8AC21; suitable for Lamp holder: 6GF3440-8CD01; 24 V power supply; Suitable for lamp cable: 6GF3440-8BC4, 6GF3440-8BD1; Dimensions: 142x 142x 43 mm (WxHxD), Degree of protection IP67;",1434,"ΤΕΜ",1,"SIMATIC",1,"6GF34000LT017BA1","Βιομηχανικός αυτοματισμός SIMATIC"]
["6GF9001-1AP02","CS-mount to C-mount Adapter ring 5 mm.",32.5,"ΤΕΜ",1,"SIMATIC",1,"6GF90011AP02","Βιομηχανικός αυτοματισμός SIMATIC"]
["6GK1704-0HB18-0AK0","SOFTNET-IE S7 REDCONNECT V18; incl. S7 OPC Server, SOFTNET-IE S7 V18 software for fail-safe S7 communication floating license R-SW, software + electronic manual; license key for download; class A; 3 languages (de, en, zh-CHS); for WindowsÂ® 10 Professional/Enterprise version 21H2, 22H2; WindowsÂ® 11 Professional/Enterprise version 21H2, 22H2; WindowsÂ® Server 2016, 2019, 2022 (Standard Edition, Datacenter); WindowsÂ® 10(IoT) Enterprise 2016 LTSB WindowsÂ® 10(IoT) Enterprise 2019 LTSC WindowsÂ® 10(IoT) Enterprise 2021 LTSC",5477,"ΤΕΜ",1,"SIMATIC",1,"6GK17040HB180AK0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6GK1704-5CW17-0AA0","SOFTNET-PB S7 V17 SP1 software for S7 communication incl. FDL with OPC Server and configuration software; floating license; runtime software, software and electr. manual on DVD, license key on USB flash drive; two languages (de, en); class A; for WindowsÂ® 10 Professional/Enterprise (64 bit) version 1909, 2004, 20H2; WindowsÂ® Server 2016 (Standard Edition, Datacenter); WindowsÂ® Server 2019 (Standard Edition, Enterprise) WindowsÂ® 10(IoT) Enterprise 2016 LTSB WindowsÂ® 10(IoT) Enterprise 2019 LTSC .",695,"ΤΕΜ",1,"SIMATIC",1,"6GK17045CW170AA0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6GK1716-0HB00-3AE0","HARDNET-IE S7 REDCONNECT upgrade from edition 2006; software for fail-safe S7 communication floating license; runtime software; software and electronic manual on DVD, license key on USB flash drive class A; 3 languages (de, en, zh-CHS); for 32/64-bit for maximum 4 CP 1613 A2, CP 1623.",790,"ΤΕΜ",1,"SIMATIC",1,"6GK17160HB003AE0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6GK1720-0AP02","Promotional package SINEMA RC LAN; SINEMA Remote Connect Virtual Appliance; KEY-PLUG SINEMA RC SCALANCE S615 LAN router can only be ordered once per customer. .",1062,"ΤΕΜ",1,"SIMATIC",1,"6GK17200AP02","Βιομηχανικός αυτοματισμός SIMATIC"]
["6GK1901-0BP10-6AA0","IE RJ45 coupler PRO; IP65; RJ45 push-pull coupler for on-site assembly with IE FC RJ45 plug PRO metal enclosure (packing unit 1 coupler) .",129,"ΤΕΜ",1,"SIMATIC",1,"6GK19010BP106AA0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6GK1951-0DC03","promo package - XB112 special promo package industrial strength networks switching SCALANCE hardware included: 50x SCALANCE XB112",18802,"ΤΕΜ",1,"SIMATIC",1,"6GK19510DC03","Βιομηχανικός αυτοματισμός SIMATIC"]
["6GK5204-0BA00-2KB2","SCALANCE X204RNA; redundant network access; 4x 100 Mbit/s RJ45 ports; LED diagnostics; error-signaling contact with set push-button; redundant power supply; network management; including electronic manual on CD-ROM, C-PLUG optional for PRP networks;",1115,"ΤΕΜ",1,"SIMATIC",1,"6GK52040BA002KB2","Βιομηχανικός αυτοματισμός SIMATIC"]
["6GK5208-0GA00-2TC2","SCALANCE XC208G (E/IP) manageable Layer 2 IE switch; IEC 62443-4-2 certified; 8x 10/100/1000 Mbps RJ45 ports; 1x console port; diagnostics LED; redundant power supply; temperature range -40 Â°C to +70 Â°C; assembly: DIN rail/S7 mounting rail/wall; redundancy functions; Office features (RSTP, VLAN,...); PROFINET IO device Ethernet/IP-compliant C-plug slot; Default EtherNet/IP. IEEE 1588v2 PTP",1171,"ΤΕΜ",1,"SIMATIC",1,"6GK52080GA002TC2","Βιομηχανικός αυτοματισμός SIMATIC"]
["6GK5224-0BA00-2AC2","SCALANCE XC224 manageable Layer 2 IE switch; IEC 62443-4-2 certified; 24x 10/100 Mbit/s RJ45 ports; 1x console port, diagnostics LED; redundant power supply; temperature range -40 Â°C to +70 Â°C; assembly: DIN rail/S7 mounting rail/wall Office redundancy functions features (RSTP, VLAN,...); PROFINET IO device Ethernet/IP-compliant, C-plug slot;",2173,"ΤΕΜ",1,"SIMATIC",1,"6GK52240BA002AC2","Βιομηχανικός αυτοματισμός SIMATIC"]
["6GK5722-1FC00-0AC0","IWLAN client, SCALANCE W722-1, RJ45, 1 radio, 1 R-SMA antenna port, iFeatures support IEEE 802.11a/b/g/h/n, 2.4/5GHz, gross data rate 150 Mbit/s, 1x RJ45 max. 100 Mbit/s, 24 V DC, joint block, IP20, 0... +55 Â°C, WPA2/802.11i/e, observe national approvals! CERT ID: ELN-W1-RJ-E1, scope of delivery: Manuals on CD-ROM, German/English, 1x joint block; only for operation in Israel.",801,"ΤΕΜ",1,"SIMATIC",1,"6GK57221FC000AC0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6GK5766-1GE00-3DB0","IWLAN client, SCALANCE WUM766-1 1 radio, 2.4/5 GHz, 2 N-Connect connections, iFeatures support via CLP, IEEE 802.11ax (Wi-Fi 6), 1201 Mbps (gross) per radio, 1x 10/100/1000 Mbps M12 socket, redundant 24 V DC, M12 L-coded PoE, IP65, -30...+60 Â°C, CLP slot, DI/DO, A-coded, observe national approvals! cert ID: MSAX65-W1-M12-E2, FCCID: LYHMSAX65V1, operation in the USA , scope of delivery: sealing caps for connections",1120,"ΤΕΜ",1,"SIMATIC",1,"6GK57661GE003DB0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6GK5798-8MG00-0AA0","mounting kit, can only be used in connection with SCALANCE W-786; scope of delivery: Adapter for wall mounting, Adapter for S7-300 busbar, Adapter for 35 mm DIN rail, clamps for mast mounting, operating instructions, German/English.",135,"ΤΕΜ",1,"SIMATIC",1,"6GK57988MG000AA0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6GK5980-5EB00-0AA5","5-pole terminal block for PROFIBUS OLM V4; 1 pack = 5 units; spare part.",50.1,"ΠΑΚ",1,"SIMATIC",1,"6GK59805EB000AA5","Βιομηχανικός αυτοματισμός SIMATIC"]
["6GK6000-8CL00-0AA0","RUGGEDCOM CONNECTOR FABMET M969 LC PLUG CONNECTOR MULTIMODE, RoHS",280,"ΤΕΜ",1,"SIMATIC",1,"6GK60008CL000AA0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6GK6000-8FE50-1AA0","RUGGEDCOM Accessory, SFP with active transceiver, 1 X 100MBIT/S, 100BASE-FX, LC-In terface, Optical: Multi Mode Fiber Optic up to max. 2km, 1310nm, -40...+85 Degrees Celcius.",275,"ΤΕΜ",1,"SIMATIC",1,"6GK60008FE501AA0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6GK6000-8FX01-4EA0","Media Module for RUGGEDCOM RSG2488, 4 x 100MBit/s ST-interface, Optical: 100BASE-FX, Multi Mode fiber optic up to 2 kilometer, 1300nm",947,"ΤΕΜ",1,"SIMATIC",1,"6GK60008FX014EA0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6GK6000-8FX06-2CA0","Media Module for RUGGEDCOM RSG2200, RSG2288, RSG2300, and RSG2300P, 2 x 100MBit/s LC-interface, Optical: 100BASE-FX, Single Mode fiber optic up to 20 kilometer, 1310nm (FXA06). Requires the in-field modification kit, 6GK6000-1BC50-0AA1.",958,"ΤΕΜ",1,"SIMATIC",1,"6GK60008FX062CA0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6GK6000-8HS02-0AA0","19\" rack form factor Power Supply with 120/264 VAC, or 150-250 VDC input and 54V/11.1 A output.  Designed for use in Power Over Ethernet (POE) systems, or any system that requires 54 VDC power.",2005,"ΤΕΜ",1,"SIMATIC",1,"6GK60008HS020AA0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6GK6001-0AC01-0FA0","RUGGEDCOM RMC is an industrially hardened fiber optical media converter specifically designed to operate in harsh environments such as those found in electric utility substations and factory floors. different Fiber optic types DIN rail mounting is standard 24 = 24 VDC (18-36 VDC) XX = No power supply 2 TXFXMMLC = MM 1300 nm, 2 km LC 1x 100TX to 1x 100FX XX = none XX = none Manufacturing modification",717,"ΤΕΜ",1,"SIMATIC",1,"6GK60010AC010FA0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6GK6015-0AL20-0BD1","RUGGEDCOM RX1500PN LM FL01 Line Module Tri-port 10FL/100SX - Multimode, 850nm, ST Conformal Coating",1120,"ΤΕΜ",1,"SIMATIC",1,"6GK60150AL200BD1","Βιομηχανικός αυτοματισμός SIMATIC"]
["6GK6015-0AL20-0PC0","RUGGEDCOM RX1500PN M12 4TX03 Line Module M12 Copper Ethernet Modules 4x 10/100TX 8-pin M12",600,"ΤΕΜ",1,"SIMATIC",1,"6GK60150AL200PC0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6GK6021-0MK00-0AA0","The RUGGEDCOM M2100 is a 19-Port MIL-STD hardened, fully managed, modular, Ethernet switch; 128-bit Encryption. 27290-514-1 M2100-B-DP-HI-HI-TX02-TX02- TX02-TX02-CG02-1CG02-TX02- TX02-FX01-FX01 94756ASSY464-0422-001",7784,"ΤΕΜ",1,"SIMATIC",1,"6GK60210MK000AA0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6GK6050-0AR00-8SM0","RUGGEDCOM REPN-8FSM1 8 x Single Mode Military Circular Fiber Connectors with LC connectors",11357,"ΤΕΜ",1,"SIMATIC",1,"6GK60500AR008SM0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6GK6050-0ML30-0CA1","CONTROL MODULE WITH LAYER 3 SECURITY EDITION LAYER-3-HARDWARE",3170,"ΤΕΜ",1,"SIMATIC",1,"6GK60500ML300CA1","Βιομηχανικός αυτοματισμός SIMATIC"]
["6GK6490-8CB00-3AN0","RUGGEDCOM RSG908C is an 8 port industrially hardened, fully managed Ethernet switch featuring integrated IEEE 1588 support for use in harsh industrial environments. The product has 4x 1Gbit/s SFP slots and 4x 100Mbit/s multimode LC ports (max 2km). -40Â°C to +85Â°C operating temperature (fanless). Reserved Reserved DIN Rail and Panel 10 - 60 VDC Reserved none",2428,"ΤΕΜ",1,"SIMATIC",1,"6GK64908CB003AN0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6GK8751-1JA01-0BK0","SINEC INS Basic 250 DL Type of delivery Download Services for management of industrial networks, RADIUS, syslog, NTP, DHCP, TFTP, SFTP, DNS Server license type single monitorable IP devices 250 Ubuntu Linux 20.4.4 LTS Ubuntu Linux Server 20.4.4 LTS Debian 9.6.0 SIMATIC OS 1.3.",1636,"ΤΕΜ",1,"SIMATIC",1,"6GK87511JA010BK0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6GK8821-1BG01-0BA0","SINEC Traffic Analyzer Industrial Edge app 12-month license, ****monitoring of PROFINET networks to reduce downtimes through efficient fault and cause identification****** billing MLFB, not visible in the Mall or dex store",699,"ΤΕΜ",1,"SIMATIC",1,"6GK88211BG010BA0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6GT2398-1CF10","SIMATIC RF200/RF300 antenna ANT 8 M8x 38 mm, IP67, -25 to +70 Â°C, with trailing antenna wire, both ends plug-in PUR, UL 758, Length 3 m Consisting of: 1x 6GT23981CF00 1x 6GT23910AH30.",413,"ΤΕΜ",1,"SIMATIC",1,"6GT23981CF10","Βιομηχανικός αυτοματισμός SIMATIC"]
["6GT2600-2BA00","transponder MDS D226S 30x3.2 mm (DxH) ISO 15693 13.56 MHz user memory 316 bytes/2528 bits; NXP SLI-X2 mounting screw M4 not printable -40 to +90 Â°C IP68/IPX9K range 280 mm MOQ 100",4.0999999999999996,"ΤΕΜ",1,"SIMATIC",100,"6GT26002BA00","Βιομηχανικός αυτοματισμός SIMATIC"]
["6GT2790-0CB00","SIMATIC RTLS accessory, IP65 protective sleeve for RJ45 plug on gateway, suitable for Ethernet cable: 6XV1870-3Qxxx minimum order quantity: 5 units.",19.100000000000001,"ΤΕΜ",1,"SIMATIC",5,"6GT27900CB00","Βιομηχανικός αυτοματισμός SIMATIC"]
["6GT2810-2AE82-1AX0","SIMATIC RF630L SmartLabel PET white, 80x26 mm ISO 18000-6C, EPC Class 1 Gen 2 frequency 860 to 960 MHz chip type NXP Ucode 8 128-bit (16 bytes) EPC memory no user memory strongly adhesive on plastic printable thermotransfer temperature from -25 Â°C to +160 Â°C roll 76.2 mm (3\") core diameter 3,500 units/role 2 rolls/carton 7000 units MOQ.",25,"ΤΕΜ",100,"SIMATIC",7000,"6GT28102AE821AX0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6GT2815-1BN10","SIMATIC RF600 connecting cable for antenna L10; damping 2 DB; pre-assembled; IP65; PE, CMR/MPR, length 10 m.",257,"ΤΕΜ",1,"SIMATIC",1,"6GT28151BN10","Βιομηχανικός αυτοματισμός SIMATIC"]
["6GT2881-1AA04-0AA0","SIMATIC IDENT CB 4 Gate RFID UHF system with four antennas for the detection of RFID labeled objects on a conveyor belt The system includes standard acquisition software and the necessary RFID and automation components including control cabinet and metal structure.",18174,"ΤΕΜ",1,"SIMATIC",1,"6GT28811AA040AA0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6NH7997-5DA10-0AA0","ST7 ScadaConnect basic license for connection of RTUs with SINAUT ST7 to HMI/SCADA applications via OPC UA, single license f. 1 installation engineering software, online software delivery (OSD).",672,"ΤΕΜ",1,"SIMATIC",1,"6NH79975DA100AA0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6RA8000-0MV62-0AA0","SINAMICS DCM control module without power unit incl. 40 A field device controllable field rectifier",11435,"ΤΕΜ",1,"GMC",1,"6RA80000MV620AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6RX1800-4DE04","Commutating reactor for converter; Phases: 1 F(Hz): 50/60; ILN=Ithmax(A): 25 UN(V): 400 (50Hz)/480 (60 Hz) UK (%): 4; Lrated (mH): 2.037 tA/insulating material class: 40Â°/B; IP00 connection: Terminal connection EN 61558-2-20",433,"ΤΕΜ",1,"GMC",1,"6RX18004DE04","Ρυθμιστές στροφών και συστήματα Motion control"]
["6RX1800-4GK07","Commutating reactor for converter; Phases: 3 F(Hz): 50/60; ILN=Ithmax(A): 664 UN(V): 575 (50Hz)/690 (60Hz) UK (%): 4; Lrated (mH): 0.064 tA/insulating material class: 40Â°/B; IP00 connection: Terminal connection EN 61558-2-20",9444,"ΤΕΜ",1,"GMC",1,"6RX18004GK07","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SE7028-0ES87-2DC0","SINAMICS/ SIMOVERT MASTERDRIVES BRAKING RESISTOR 510-620V DC, 50KW, 8 OHM",1789,"ΤΕΜ",1,"GMC",1,"6SE70280ES872DC0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3000-0CH31-6AA0","SINAMICS LINE FILTER INPUT: 3-PH. 660-690 V, 50/60 HZ, 155 A",1770,"ΤΕΜ",1,"GMC",1,"6SL30000CH316AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3000-2DE38-4BA0","SINAMICS Voltage Peak Limiter Spare part for Power Module/Motor Module 450kW, 380-480 V 3 AC",8669,"ΤΕΜ",1,"GMC",1,"6SL30002DE384BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3000-2DH31-5BA0","SINAMICS Voltage Peak Limiter Spare part for Power Module/Motor Module 132kW, 500-690V 3AC",3352,"ΤΕΜ",1,"GMC",1,"6SL30002DH315BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3054-0FC30-1BA0","SINAMICS S120 CompactFlash card without performance expansion incl. licensing (Certificate of License, stored on the card) V5.2 Service Pack 3",211,"ΤΕΜ",1,"GMC",1,"6SL30540FC301BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3060-4AK00-0AA0","SINAMICS DRIVE-CLIQ CABLE IP20/IP20 LENGTH: 0.31 M",49.7,"ΤΕΜ",1,"GMC",1,"6SL30604AK000AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3077-0AA00-2AB0","SINAMICS Technology Extension ADDFIL V1.x Additional current setpoint filter V1.x SOFTWARE OPTION FROM FIRMWARE V2.6 DELIVERY OF ONE LICENSE ON PAPER MACHINE-SPECIFIC DELIVERY RELEASE !",272,"ΤΕΜ",1,"GMC",1,"6SL30770AA002AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3126-1TE26-0AA3","SINAMICS S120 SINGLE MOTOR MODULE INPUT: DC 600V OUTPUT: 3AC 400V, 60A FRAME SIZE: BOOKSIZE COLD-PLATE COOLING OPTIMIZED PULSE SAMPLE AND SUPPORT OF THE EXTENDED SAFETY INTEGRATED FUNCTIONS INCL. DRIVE-CLIQ CABLE",9615,"ΤΕΜ",1,"GMC",1,"6SL31261TE260AA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3136-1TE24-0AA0","SINAMICS S120 BASIC LINE MODULE INPUT: 3PH 380-480V, 50/60HZ OUTPUT: DC 600V, 67 A, 40KW FRAME SIZE: BOOKSIZE COLD-PLATE-COOLING INCL. DRIVE-CLIQ CABLE",4127,"ΤΕΜ",1,"GMC",1,"6SL31361TE240AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3200-0UF01-0AA0","SINAMICS V20 Size A replacement fan Size: 40x40x11 (WxHxD)",17.700000000000003,"ΤΕΜ",1,"GMC",1,"6SL32000UF010AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3202-0AE21-8CA0","SINAMICS Output reactor FOR POWERMODULE FSB 3AC 380V-480V 18,5A",354,"ΤΕΜ",1,"GMC",1,"6SL32020AE218CA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3210-1KE12-3AF2","SINAMICS G120C RATED POWER 0,75KW WITH 150% OVERLOAD FOR 3 SEC 3AC380-480V +10/-20% 47-63HZ INTEGRATED FILTER CLASS A I/O-INTERFACE: 6DI, 2DO,1AI,1AO SAFE TORQUE OFF INTEGRATED FIELDBUS: PROFINET-PN PROTECTION: IP20/ UL OPEN TYPE SIZE: FSAA 173X73X178(HXWXD) EXTERNAL 24V",883,"ΤΕΜ",1,"GMC",1,"6SL32101KE123AF2","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3210-1NE21-8AG1","SINAMICS G120 Power Module PM230 with integrated Class A filter Degree of protection IP20 380-480 V 3 AC +10/-10% 47-63 Hz Power low overload: 7.5kW at 150% 3s, 110% 57s, 100% 240 s; Ambient temperature 0 to +40 Â°C (LO) 292x 100x 165 (HxWxD), FSB without Control Unit and operating unit released for CU240B/E-2 and CU230P-2 Firmware version V4.4 or higher",1619,"ΤΕΜ",1,"GMC",1,"6SL32101NE218AG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3210-1PE21-4AL0","SINAMICS POWER MODULE PM240-2 WITH BUILT IN CL. A FILTER WITH BUILT IN BRAKING CHOPPER 3AC380-480V +10/-10% 47-63HZ OUTPUT HIGH OVERLOAD: 4KW FOR 200% 3S,150% 57S,100% 240S AMBIENT TEMP -10 TO +50 DEG C OUTPUT LOW OVERLOAD: 5,5KW FOR 150% 3S,110% 57S,100% 240S AMBIENT TEMP -10 TO +40 DEG C 291 X 100 X 165 (HXWXD), FSB PROTECTION IP20 WITHOUT CONTROL UNIT AND PANEL APPROVED FOR CU FIRMWARE- VERSION V4.6",1459,"ΤΕΜ",1,"GMC",1,"6SL32101PE214AL0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3210-1PH23-5UL0","SINAMICS G120 POWER MODULE PM240-2 WITHOUT FILTER WITH BUILT IN BRAKING CHOPPER 3AC500-690V +10/-20% 47-63HZ OUTPUT HIGH OVERLOAD: 22KW FOR 200% 3S,150% 57S,100% 240S AMBIENT TEMP -20 TO +50 DEG C (HO) OUTPUT LOW OVERLOAD: 30kW FOR 150% 3S,110% 57S,100% 240S AMBIENT TEMP -20 TO +40 DEG C (LO) 472 X 200 X 237 (HXWXD), FSD PROTECTION IP20 WITHOUT CONTROL UNIT AND PANEL APPROVED FOR CU FIRMWARE- VERSION V4.7 HF8",5945,"ΤΕΜ",1,"GMC",1,"6SL32101PH235UL0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3210-1RE31-5AL0","SINAMICS G120 POWER MODULE PM240P-2 WITH BUILT IN CL. A FILTER 3AC380-480V +10/-20% 47-63HZ OUTPUT HIGH OVERLOAD: 55KW FOR 150% 60S, 100% 240S; AMBIENT TEMP -20 TO +50 DEG C (HO) OUTPUT LOW OVERLOAD: 75kW FOR 135% 3S,110% 57S,100% 240S AMBIENT TEMP -20 TO +40 DEG C (LO) 708x 305x 357 (HXWXD), FSF PROTECTION IP20 WITHOUT CONTROL UNIT AND PANEL APPROVED FOR CU FIRMWARE- VERSION V4.7 SP6 HF1",11381,"ΤΕΜ",1,"GMC",1,"6SL32101RE315AL0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3210-5BE27-5UV0","SINAMICS V20 380-480 V 3 AC -15/+10% 47-63Hz rated power 7.5 kW with 150% overload for 60 sec. unfiltered I/O: 4 DI, 2 DO,2 AI, 1 AQ fieldbus: USS/MODBUS RTU with built-in BOP protection: IP20/ UL open size: D 240x207x173 (WxHxD)",1286,"ΤΕΜ",1,"GMC",1,"6SL32105BE275UV0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3210-5FE12-0UA0","SINAMICS V90 Input voltage: 380-480 V 3 A -15%/+10% 9.8 A 45-66 Hz Output voltage: 0 â€“ Input 7.8 A 0-330 Hz Motor: 2.0/2.5 kW Degree of protection: IP20 Size B 100x180x220 (WxHxD)",1554,"ΤΕΜ",1,"GMC",1,"6SL32105FE120UA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-1YC22-1UP0","SINAMICS G120X Rated power: 5.5 kW At 110% 60s, 100% 240 s Unfiltered 200-240 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSC Degree of protection IP20 / UL open type painting 3C2 without operator panel with IO expansions Fieldbus integrated: PROFIBUS DP",1527,"ΤΕΜ",1,"GMC",1,"6SL32201YC221UP0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-1YE10-0AP0","SINAMICS G120X Rated power: 0.75 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSA Degree of protection IP20 / UL open type painting 3C2 without operator panel Without IO expansion Fieldbus integrated: PROFIBUS DP",932,"ΤΕΜ",1,"GMC",1,"6SL32201YE100AP0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-1YE22-0UP0","SINAMICS G120X Rated power: 5.5 kW At 110% 60s, 100% 240 s Unfiltered 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSB Degree of protection IP20 / UL open type painting 3C2 without operator panel Without IO expansion Fieldbus integrated: PROFIBUS DP",1324,"ΤΕΜ",1,"GMC",1,"6SL32201YE220UP0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-1YE28-1UP0","SINAMICS G120X Rated power: 15 kW At 110% 60s, 100% 240 s Unfiltered 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSC Degree of protection IP20 / UL open type painting 3C2 without operator panel with IO expansions Fieldbus integrated: PROFIBUS DP",2580,"ΤΕΜ",1,"GMC",1,"6SL32201YE281UP0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-1YE42-0UF0","SINAMICS G120X Rated power: 75 kW At 110% 60s, 100% 240 s Unfiltered 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSF Degree of protection IP20 / UL open type painting 3C2 without operator panel Without IO expansion Fieldbus integrated: PROFINET PN, Ethernet IP",8381,"ΤΕΜ",1,"GMC",1,"6SL32201YE420UF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-1YE46-0AF0","SINAMICS G120X Rated power: 110 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSF Degree of protection IP20 / UL open type painting 3C2 without operator panel Without IO expansion Fieldbus integrated: PROFINET PN, Ethernet IP",12309,"ΤΕΜ",1,"GMC",1,"6SL32201YE460AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-1YE60-1CP0","SINAMICS G120X Rated power: 400 kW at  135% 3 s or 110% 60 s, 100% 240 s; RFI suppression filter  For category C3 3AC380-480V+10/-20% 47-63Hz Ambient temperature 0 to +45 Â°C Size: FSH Degree of protection IP20 / UL open type Without operator panel With IO expansion Fieldbus integrated: PROFIBUS DP",35550,"ΤΕΜ",1,"GMC",1,"6SL32201YE601CP0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-1YH24-1AB0","SINAMICS G120X Rated power: 7.5 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSD Degree of protection IP20 / UL open type painting 3C2 without operator panel with IO expansions Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",2036,"ΤΕΜ",1,"GMC",1,"6SL32201YH241AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-1YH36-1UB0","SINAMICS G120X Rated power: 37 kW At 110% 60s, 100% 240 s Unfiltered 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSD Degree of protection IP20 / UL open type painting 3C2 without operator panel with IO expansions Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",5762,"ΤΕΜ",1,"GMC",1,"6SL32201YH361UB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-1YH42-0CB0","SINAMICS G120X Rated power: 75 kW At 110% 60s, 100% 240 s Radio interference suppression filter For category C3 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSF Degree of protection IP20 / UL open type painting 3C2 without operator panel Without IO expansion Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",9967,"ΤΕΜ",1,"GMC",1,"6SL32201YH420CB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-1YH48-0CP0","SINAMICS G120X Rated power: 132 kW At 110% 60s, 100% 240 s Radio interference suppression filter For category C3 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSF Degree of protection IP20 / UL open type painting 3C2 without operator panel Without IO expansion Fieldbus integrated: PROFIBUS DP",15266,"ΤΕΜ",1,"GMC",1,"6SL32201YH480CP0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-2YC18-1UP0","SINAMICS G120X Rated power: 3 kW At 110% 60s, 100% 240 s Unfiltered 200-240 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSB Degree of protection IP20 / UL open type painting 3C2 with Basic Operator Panel with IO expansions Fieldbus integrated: PROFIBUS DP",1136,"ΤΕΜ",1,"GMC",1,"6SL32202YC181UP0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-2YC34-0UB0","SINAMICS G120X Rated power: 30 kW At 110% 60s, 100% 240 s Unfiltered 200-240 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSE Degree of protection IP20 / UL open type painting 3C2 with Basic Operator Panel Without IO expansion Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",4445,"ΤΕΜ",1,"GMC",1,"6SL32202YC340UB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-2YE16-1AF0","SINAMICS G120X Rated power: 2.2 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSA Degree of protection IP20 / UL open type painting 3C2 with Basic Operator Panel with IO expansions Fieldbus integrated: PROFINET PN, Ethernet IP",1263,"ΤΕΜ",1,"GMC",1,"6SL32202YE161AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-2YE24-1UP0","SINAMICS G120X Rated power: 7.5 kW At 110% 60s, 100% 240 s Unfiltered 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSB Degree of protection IP20 / UL open type painting 3C2 with Basic Operator Panel with IO expansions Fieldbus integrated: PROFIBUS DP",1737,"ΤΕΜ",1,"GMC",1,"6SL32202YE241UP0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-2YE38-0AP0","SINAMICS G120X Rated power: 45 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSE Degree of protection IP20 / UL open type painting 3C2 with Basic Operator Panel Without IO expansion Fieldbus integrated: PROFIBUS DP",6459,"ΤΕΜ",1,"GMC",1,"6SL32202YE380AP0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-2YE46-0AF0","SINAMICS G120X Rated power: 110 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSF Degree of protection IP20 / UL open type painting 3C2 with Basic Operator Panel Without IO expansion Fieldbus integrated: PROFINET PN, Ethernet IP",12365,"ΤΕΜ",1,"GMC",1,"6SL32202YE460AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-2YE48-1AF0","SINAMICS G120X Rated power: 132 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSF Degree of protection IP20 / UL open type painting 3C2 with Basic Operator Panel with IO expansions Fieldbus integrated: PROFINET PN, Ethernet IP",13979,"ΤΕΜ",1,"GMC",1,"6SL32202YE481AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-2YH20-0UF0","SINAMICS G120X Rated power: 4 kW At 110% 60s, 100% 240 s Unfiltered 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSD Degree of protection IP20 / UL open type painting 3C2 with Basic Operator Panel Without IO expansion Fieldbus integrated: PROFINET PN, Ethernet IP",1589,"ΤΕΜ",1,"GMC",1,"6SL32202YH200UF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-2YH34-0AF0","SINAMICS G120X Rated power: 30 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSD Degree of protection IP20 / UL open type painting 3C2 with Basic Operator Panel Without IO expansion Fieldbus integrated: PROFINET PN, Ethernet IP",5303,"ΤΕΜ",1,"GMC",1,"6SL32202YH340AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-2YH40-0UB0","SINAMICS G120X Rated power: 55 kW At 110% 60s, 100% 240 s Unfiltered 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSE Degree of protection IP20 / UL open type painting 3C2 with Basic Operator Panel Without IO expansion Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",8031,"ΤΕΜ",1,"GMC",1,"6SL32202YH400UB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-2YH44-0CB0","SINAMICS G120X Rated power: 90 kW At 110% 60s, 100% 240 s Radio interference suppression filter For category C3 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSF Degree of protection IP20 / UL open type painting 3C2 with Basic Operator Panel Without IO expansion Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",11934,"ΤΕΜ",1,"GMC",1,"6SL32202YH440CB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-3YC14-0UP0","SINAMICS G120X Rated power: 1.5 kW At 110% 60s, 100% 240 s Unfiltered 200-240 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSA Degree of protection IP20 / UL open type painting 3C2 With Intelligent Operator Panel Without IO expansion Fieldbus integrated: PROFIBUS DP",978,"ΤΕΜ",1,"GMC",1,"6SL32203YC140UP0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-3YC24-1UP0","SINAMICS G120X Rated power: 7.5 kW At 110% 60s, 100% 240 s Unfiltered 200-240 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSC Degree of protection IP20 / UL open type painting 3C2 With Intelligent Operator Panel with IO expansions Fieldbus integrated: PROFIBUS DP",1949,"ΤΕΜ",1,"GMC",1,"6SL32203YC241UP0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-3YE14-0AP0","SINAMICS G120X Rated power: 1.5 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSA Degree of protection IP20 / UL open type painting 3C2 With Intelligent Operator Panel Without IO expansion Fieldbus integrated: PROFIBUS DP",1182,"ΤΕΜ",1,"GMC",1,"6SL32203YE140AP0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-3YE24-1AP0","SINAMICS G120X Rated power: 7.5 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSB Degree of protection IP20 / UL open type painting 3C2 With Intelligent Operator Panel with IO expansions Fieldbus integrated: PROFIBUS DP",2057,"ΤΕΜ",1,"GMC",1,"6SL32203YE241AP0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-3YE34-0AF0","SINAMICS G120X Rated power: 30 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSD Degree of protection IP20 / UL open type painting 3C2 With Intelligent Operator Panel Without IO expansion Fieldbus integrated: PROFINET PN, Ethernet IP",4798,"ΤΕΜ",1,"GMC",1,"6SL32203YE340AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-3YE36-1UF0","SINAMICS G120X Rated power: 37 kW At 110% 60s, 100% 240 s Unfiltered 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSD Degree of protection IP20 / UL open type painting 3C2 With Intelligent Operator Panel with IO expansions Fieldbus integrated: PROFINET PN, Ethernet IP",5337,"ΤΕΜ",1,"GMC",1,"6SL32203YE361UF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-3YE44-1AF0","SINAMICS G120X Rated power: 90 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSF Degree of protection IP20 / UL open type painting 3C2 With Intelligent Operator Panel with IO expansions Fieldbus integrated: PROFINET PN, Ethernet IP",11172,"ΤΕΜ",1,"GMC",1,"6SL32203YE441AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-3YE58-1CB0","SINAMICS G120X Rated power: 355 kW at  135% 3 s or 110% 60 s, 100% 240 s; RFI suppression filter  For category C3 3AC380-480V+10/-20% 47-63Hz Ambient temperature 0 to +45 Â°C Size: FSH Degree of protection IP20 / UL open type With Intelligent Operator Panel With IO expansion Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",30720,"ΤΕΜ",1,"GMC",1,"6SL32203YE581CB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-3YH22-1UF0","SINAMICS G120X Rated power: 5.5 kW At 110% 60s, 100% 240 s Unfiltered 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSD Degree of protection IP20 / UL open type painting 3C2 With Intelligent Operator Panel with IO expansions Fieldbus integrated: PROFINET PN, Ethernet IP",1915,"ΤΕΜ",1,"GMC",1,"6SL32203YH221UF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-3YH32-1AF0","SINAMICS G120X Rated power: 22 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSD Degree of protection IP20 / UL open type painting 3C2 With Intelligent Operator Panel with IO expansions Fieldbus integrated: PROFINET PN, Ethernet IP",4559,"ΤΕΜ",1,"GMC",1,"6SL32203YH321AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3220-3YH48-0UP0","SINAMICS G120X rated power: 132 kW at 110% 60s, 100% 240s unfiltered 500-690V3AC+10/-20% 47-63Hz ambient temperature -20 to +45 Â°C frame size: FSF degree of protection IP20 / UL open type painting 3C2 with Intelligent Operator Panel without IO expansion fieldbus integrated: PROFIBUS DP",14701,"ΤΕΜ",1,"GMC",1,"6SL32203YH480UP0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3223-0DE13-7AG1","SINAMICS G120P Power Module PM230 with integrated Class A filter Degree of protection IP55/UL Type 12 380-480 V 3 AC +10/-10% 47-63 Hz Power low overload: 0.37kW at 150% 3s, 110% 57s, 100% 240 s; Ambient temperature -10 to +40 Â°C (LO) 460x 154x 249 (HxWxD), FSA without Control Unit and operating unit released for CU230P-2 Firmware version V4.3.2 or higher",597,"ΤΕΜ",1,"GMC",1,"6SL32230DE137AG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3223-0DE31-1BG1","SINAMICS G120P Power Module PM230 with integrated Class B filter Degree of protection IP55/UL Type 12 380-480 V 3 AC +10/-10% 47-63 Hz Power low overload: 11kW at 150% 3s, 110% 57s, 100% 240 s; Ambient temperature -10 to +40 Â°C (LO) 620x 230x 249 (HxWxD), FSC without Control Unit and operating unit released for CU230P-2 Firmware version V4.3.2 or higher",2893,"ΤΕΜ",1,"GMC",1,"6SL32230DE311BG1","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-1YC26-1UP0","SINAMICS G120X Rated power: 11 kW At 110% 60s, 100% 240 s Unfiltered 200-240 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSD Degree of protection IP20 / UL open type Paint finish 3C3 without operator panel with IO expansions Fieldbus integrated: PROFIBUS DP",2512,"ΤΕΜ",1,"GMC",1,"6SL32301YC261UP0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-1YC36-1UB0","SINAMICS G120X Rated power: 37 kW At 110% 60s, 100% 240 s Unfiltered 200-240 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSF Degree of protection IP20 / UL open type Paint finish 3C3 without operator panel with IO expansions Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",5827,"ΤΕΜ",1,"GMC",1,"6SL32301YC361UB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-1YE20-0AB0","SINAMICS G120X Rated power: 4 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSB Degree of protection IP20 / UL open type Paint finish 3C3 without operator panel Without IO expansion Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",1455,"ΤΕΜ",1,"GMC",1,"6SL32301YE200AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-1YE22-0UF0","SINAMICS G120X Rated power: 5.5 kW At 110% 60s, 100% 240 s Unfiltered 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSB Degree of protection IP20 / UL open type Paint finish 3C3 without operator panel Without IO expansion Fieldbus integrated: PROFINET PN, Ethernet IP",1601,"ΤΕΜ",1,"GMC",1,"6SL32301YE220UF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-1YE38-1UP0","SINAMICS G120X Rated power: 45 kW At 110% 60s, 100% 240 s Unfiltered 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSE Degree of protection IP20 / UL open type Paint finish 3C3 without operator panel with IO expansions Fieldbus integrated: PROFIBUS DP",6469,"ΤΕΜ",1,"GMC",1,"6SL32301YE381UP0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-1YE42-1AP0","SINAMICS G120X Rated power: 75 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSF Degree of protection IP20 / UL open type Paint finish 3C3 without operator panel with IO expansions Fieldbus integrated: PROFIBUS DP",9802,"ΤΕΜ",1,"GMC",1,"6SL32301YE421AP0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-1YE50-1CF0","SINAMICS G120X Rated power: 160 kW At 110% 60s, 100% 240 s Radio interference suppression filter For category C3 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSG Degree of protection IP20 / UL open type Paint finish 3C3 without operator panel with IO expansions Fieldbus integrated: PROFINET PN, Ethernet IP",15678,"ΤΕΜ",1,"GMC",1,"6SL32301YE501CF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-1YH24-1AF0","SINAMICS G120X Rated power: 7.5 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSD Degree of protection IP20 / UL open type Paint finish 3C3 without operator panel with IO expansions Fieldbus integrated: PROFINET PN, Ethernet IP",2479,"ΤΕΜ",1,"GMC",1,"6SL32301YH241AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-1YH32-0AP0","SINAMICS G120X Rated power: 22 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSD Degree of protection IP20 / UL open type Paint finish 3C3 without operator panel Without IO expansion Fieldbus integrated: PROFIBUS DP",4672,"ΤΕΜ",1,"GMC",1,"6SL32301YH320AP0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-1YH42-0UF0","SINAMICS G120X Rated power: 75 kW At 110% 60s, 100% 240 s Unfiltered 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSF Degree of protection IP20 / UL open type Paint finish 3C3 without operator panel Without IO expansion Fieldbus integrated: PROFINET PN, Ethernet IP",10156,"ΤΕΜ",1,"GMC",1,"6SL32301YH420UF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-1YH48-0UB0","SINAMICS G120X Rated power: 132 kW At 110% 60s, 100% 240 s Unfiltered 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSF Degree of protection IP20 / UL open type Paint finish 3C3 without operator panel Without IO expansion Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",14994,"ΤΕΜ",1,"GMC",1,"6SL32301YH480UB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-2YC32-1UF0","SINAMICS G120X Rated power: 22 kW At 110% 60s, 100% 240 s Unfiltered 200-240 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSE Degree of protection IP20 / UL open type Paint finish 3C3 with Basic Operator Panel with IO expansions Fieldbus integrated: PROFINET PN, Ethernet IP",4254,"ΤΕΜ",1,"GMC",1,"6SL32302YC321UF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-2YE12-0UF0","SINAMICS G120X Rated power: 1.1 kW At 110% 60s, 100% 240 s Unfiltered 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSA Degree of protection IP20 / UL open type Paint finish 3C3 with Basic Operator Panel Without IO expansion Fieldbus integrated: PROFINET PN, Ethernet IP",1078,"ΤΕΜ",1,"GMC",1,"6SL32302YE120UF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-2YE16-0UB0","SINAMICS G120X Rated power: 2.2 kW At 110% 60s, 100% 240 s Unfiltered 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSA Degree of protection IP20 / UL open type Paint finish 3C3 with Basic Operator Panel Without IO expansion Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",1098,"ΤΕΜ",1,"GMC",1,"6SL32302YE160UB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-2YE28-1AB0","SINAMICS G120X Rated power: 15 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSC Degree of protection IP20 / UL open type Paint finish 3C3 with Basic Operator Panel with IO expansions Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",3136,"ΤΕΜ",1,"GMC",1,"6SL32302YE281AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-2YE40-1UF0","SINAMICS G120X Rated power: 55 kW At 110% 60s, 100% 240 s Unfiltered 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSE Degree of protection IP20 / UL open type Paint finish 3C3 with Basic Operator Panel with IO expansions Fieldbus integrated: PROFINET PN, Ethernet IP",7765,"ΤΕΜ",1,"GMC",1,"6SL32302YE401UF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-2YE48-0UP0","SINAMICS G120X Rated power: 132 kW At 110% 60s, 100% 240 s Unfiltered 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSF Degree of protection IP20 / UL open type Paint finish 3C3 with Basic Operator Panel Without IO expansion Fieldbus integrated: PROFIBUS DP",13314,"ΤΕΜ",1,"GMC",1,"6SL32302YE480UP0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-2YH22-1AP0","SINAMICS G120X Rated power: 5.5 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSD Degree of protection IP20 / UL open type Paint finish 3C3 with Basic Operator Panel with IO expansions Fieldbus integrated: PROFIBUS DP",2235,"ΤΕΜ",1,"GMC",1,"6SL32302YH221AP0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-2YH22-1UB0","SINAMICS G120X Rated power: 5.5 kW At 110% 60s, 100% 240 s Unfiltered 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSD Degree of protection IP20 / UL open type Paint finish 3C3 with Basic Operator Panel with IO expansions Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",1930,"ΤΕΜ",1,"GMC",1,"6SL32302YH221UB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-2YH34-0AF0","SINAMICS G120X Rated power: 30 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSD Degree of protection IP20 / UL open type Paint finish 3C3 with Basic Operator Panel Without IO expansion Fieldbus integrated: PROFINET PN, Ethernet IP",5735,"ΤΕΜ",1,"GMC",1,"6SL32302YH340AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-2YH46-0UF0","SINAMICS G120X Rated power: 110 kW At 110% 60s, 100% 240 s Unfiltered 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSF Degree of protection IP20 / UL open type Paint finish 3C3 with Basic Operator Panel Without IO expansion Fieldbus integrated: PROFINET PN, Ethernet IP",13632,"ΤΕΜ",1,"GMC",1,"6SL32302YH460UF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-3YC16-1UP0","SINAMICS G120X Rated power: 2.2 kW At 110% 60s, 100% 240 s Unfiltered 200-240 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSB Degree of protection IP20 / UL open type Paint finish 3C3 With Intelligent Operator Panel with IO expansions Fieldbus integrated: PROFIBUS DP",1339,"ΤΕΜ",1,"GMC",1,"6SL32303YC161UP0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-3YC36-1UB0","SINAMICS G120X Rated power: 37 kW At 110% 60s, 100% 240 s Unfiltered 200-240 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSF Degree of protection IP20 / UL open type Paint finish 3C3 With Intelligent Operator Panel with IO expansions Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",5995,"ΤΕΜ",1,"GMC",1,"6SL32303YC361UB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-3YE10-1AB0","SINAMICS G120X Rated power: 0.75 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSA Degree of protection IP20 / UL open type Paint finish 3C3 With Intelligent Operator Panel with IO expansions Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",1191,"ΤΕΜ",1,"GMC",1,"6SL32303YE101AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-3YE26-1AF0","SINAMICS G120X Rated power: 11 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSC Degree of protection IP20 / UL open type Paint finish 3C3 With Intelligent Operator Panel with IO expansions Fieldbus integrated: PROFINET PN, Ethernet IP",2834,"ΤΕΜ",1,"GMC",1,"6SL32303YE261AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-3YE34-1AB0","SINAMICS G120X Rated power: 30 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSD Degree of protection IP20 / UL open type Paint finish 3C3 With Intelligent Operator Panel with IO expansions Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",5203,"ΤΕΜ",1,"GMC",1,"6SL32303YE341AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-3YE42-1AP0","SINAMICS G120X Rated power: 75 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSF Degree of protection IP20 / UL open type Paint finish 3C3 With Intelligent Operator Panel with IO expansions Fieldbus integrated: PROFIBUS DP",9969,"ΤΕΜ",1,"GMC",1,"6SL32303YE421AP0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-3YE50-0CB0","SINAMICS G120X Rated power: 160 kW At 110% 60s, 100% 240 s Radio interference suppression filter For category C3 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSG Degree of protection IP20 / UL open type Paint finish 3C3 With Intelligent Operator Panel Without IO expansion Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",15582,"ΤΕΜ",1,"GMC",1,"6SL32303YE500CB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-3YH26-0AB0","SINAMICS G120X Rated power: 11 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSD Degree of protection IP20 / UL open type Paint finish 3C3 With Intelligent Operator Panel Without IO expansion Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",2879,"ΤΕΜ",1,"GMC",1,"6SL32303YH260AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-3YH32-0AP0","SINAMICS G120X Rated power: 22 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSD Degree of protection IP20 / UL open type Paint finish 3C3 With Intelligent Operator Panel Without IO expansion Fieldbus integrated: PROFIBUS DP",4840,"ΤΕΜ",1,"GMC",1,"6SL32303YH320AP0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-3YH34-1UP0","SINAMICS G120X Rated power: 30 kW At 110% 60s, 100% 240 s Unfiltered 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSD Degree of protection IP20 / UL open type Paint finish 3C3 With Intelligent Operator Panel with IO expansions Fieldbus integrated: PROFIBUS DP",5576,"ΤΕΜ",1,"GMC",1,"6SL32303YH341UP0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3230-3YH44-1UP0","SINAMICS G120X Rated power: 90 kW At 110% 60s, 100% 240 s Unfiltered 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Â°C Size: FSF Degree of protection IP20 / UL open type Paint finish 3C3 With Intelligent Operator Panel with IO expansions Fieldbus integrated: PROFIBUS DP",12279,"ΤΕΜ",1,"GMC",1,"6SL32303YH441UP0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3252-0BB01-0AA0","SINAMICS Safe brake relay for Power Module With SINAMICS S120 released as of V2.6!",181,"ΤΕΜ",1,"GMC",1,"6SL32520BB010AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3300-1AF32-5BA0","SINAMICS BRAKING MODULE INPUT: 860V DC OUTPUT: 250 KW/15S FOR CHASSIS UNITS H AND J",5416,"ΤΕΜ",1,"GMC",1,"6SL33001AF325BA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3330-6TE35-5AA3","SINAMICS S120 Smart Line Module 380-480V 3AC, 50/60 Hz Output: 510-650 V DC, 550 A Rated power: 250kW Built-in unit IP00 Internal air cooling incl. Drive-CLiQ cable",16861,"ΤΕΜ",1,"GMC",1,"6SL33306TE355AA3","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-0XA20-3AF0","SINAMICS G115D wall-mounted rated power: 0.37 kW for 3s 200%, 57s 150%, 240s 87%, RFI suppression filter for category C2 3AC380-480V+10/-10% 45-66Hz ambient temperature -30 to +40 Â°C frame size: FSA degree of protection IP65/66 / UL type 4X brake voltage 180 V DC without operation option with cable gland with communication Fieldbus integrated: PROFINET PN, Ethernet IP",1243,"ΤΕΜ",1,"GMC",1,"6SL35200XA203AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-0XA60-3AF0","SINAMICS G115D wall-mounted rated power: 0.37 kW for 3s 200%, 57s 150%, 240s 87%, RFI suppression filter for category C2 3AC380-480V+10/-10% 45-66Hz ambient temperature -30 to +40 Â°C frame size: FSA degree of protection IP65/66 / UL type 4X brake voltage 180 V DC without operation option with cable gland for 400 V AC and 24 V DC and M12 for I/O and communication Fieldbus integrated: PROFINET PN, Ethernet IP",1310,"ΤΕΜ",1,"GMC",1,"6SL35200XA603AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-0XB02-2AF0","SINAMICS G115D wall-mounted Rated power: 2.2 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSB Protection class IP65/66 / UL Type 4X brake voltage 180 V DC without operation option Q4/2 for 400 V AC and 7/8\" for 24 V DC and M12 for I/O and communication without looping through Q8/0 for motor connection Fieldbus integrated: PROFINET PN, Ethernet IP",1984,"ΤΕΜ",1,"GMC",1,"6SL35200XB022AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-0XD01-1AF0","SINAMICS G115D wall-mounted Rated power: 1.1 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 180 V DC without operation option with MQ(X)15 for 400 V AC and Power M12 for 24 V DC and M12 for I/O and communication without looping through Q8/0 for motor connection Fieldbus integrated: PROFINET PN, Ethernet IP",1644,"ΤΕΜ",1,"GMC",1,"6SL35200XD011AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-0XH03-0AB0","SINAMICS G115D wall-mounted Rated power: 3 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSB Protection class IP65/66 / UL Type 4X brake voltage 180 V DC without operation option with cable gland without communication with integrated 24 V DC PSU without fieldbus",1684,"ΤΕΜ",1,"GMC",1,"6SL35200XH030AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-0XH60-3AB0","SINAMICS G115D wall-mounted rated power: 0.37 kW for 3s 200%, 57s 150%, 240s 87%, RFI suppression filter for category C2 3AC380-480V+10/-10% 45-66Hz ambient temperature -30 to +40 Â°C frame size: FSA degree of protection IP65/66 / UL type 4X brake voltage 180 V DC without operation option with cable gland for 400 V AC and 24 V DC and M12 for I/O and communication with integrated 24 V DC PSU without fieldbus",1062,"ΤΕΜ",1,"GMC",1,"6SL35200XH603AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-0XM00-5AF0","SINAMICS G115D wall-mounted Rated power: 0.55 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 180 V DC without operation option MQ(X)15 for 400 V AC and M12 for I/O and communication with integrated 24 V DC PSU without looping through Fieldbus integrated: PROFINET PN, Ethernet IP",1710,"ΤΕΜ",1,"GMC",1,"6SL35200XM005AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-0XN03-0AA0","SINAMICS G115D wall-mounted Rated power: 3 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSB Protection class IP65/66 / UL Type 4X brake voltage 180 V DC without operation option Q4/2 for 400 V AC and M12 for I/O and communication with integrated 24 V DC PSU with looping through fieldbus integrated: AS-Interface",2202,"ΤΕΜ",1,"GMC",1,"6SL35200XN030AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-0XR10-7AF0","SINAMICS G115D wall-mounted Rated power: 0.75 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 180 V DC without operation option with cable gland for 400 V AC Power M12 for 24 V DC with looping through M12 for I/O and communication Fieldbus integrated: PROFINET PN, Ethernet IP",1416,"ΤΕΜ",1,"GMC",1,"6SL35200XR107AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-1XA62-2AA0","SINAMICS G115D wall-mounted Rated power: 2.2 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSB Protection class IP65/66 / UL Type 4X brake voltage 180 V DC repair switch with cable gland for 400 V AC and 24 V DC and M12 for I/O and communication fieldbus integrated: AS-Interface",1708,"ΤΕΜ",1,"GMC",1,"6SL35201XA622AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-1XB07-5AB0","SINAMICS G115D wall-mounted Rated power: 7.5 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSC Protection class IP65/66 / UL Type 4X brake voltage 180 V DC repair switch Q4/2 for 400 V AC and 7/8\" for 24 V DC and M12 for I/O and communication without looping through Q8/0 for motor connection without fieldbus",3212,"ΤΕΜ",1,"GMC",1,"6SL35201XB075AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-1XD04-0AF0","SINAMICS G115D wall-mounted Rated power: 4 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSB Protection class IP65/66 / UL Type 4X brake voltage 180 V DC repair switch with MQ(X)15 for 400 V AC and Power M12 for 24 V DC and M12 for I/O and communication without looping through Q8/0 for motor connection Fieldbus integrated: PROFINET PN, Ethernet IP",2598,"ΤΕΜ",1,"GMC",1,"6SL35201XD040AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-1XE01-1AA0","SINAMICS G115D wall-mounted Rated power: 1.1 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 180 V DC repair switch Q4/2 for 400 V AC and M12 for I/O and communication with looping through Q8/0 for motor connection fieldbus integrated: AS-Interface",1612,"ΤΕΜ",1,"GMC",1,"6SL35201XE011AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-1XK00-3AF0","SINAMICS G115D wall-mounted rated power: 0.37 kW for 3s 200%, 57s 150%, 240s 87%, RFI suppression filter for category C2 3AC380-480V+10/-10% 45-66Hz ambient temperature -30 to +40 Â°C frame size: FSA degree of protection IP65/66 / UL type 4X brake voltage 180 V DC repair switch Q4/2 for 400 V AC and M12 for I/O and communication with integrated 24 V DC PSU without looping through Fieldbus integrated: PROFINET PN, Ethernet IP",1809,"ΤΕΜ",1,"GMC",1,"6SL35201XK003AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-1XK04-0AF0","SINAMICS G115D wall-mounted Rated power: 4 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSB Protection class IP65/66 / UL Type 4X brake voltage 180 V DC repair switch Q4/2 for 400 V AC and M12 for I/O and communication with integrated 24 V DC PSU without looping through Fieldbus integrated: PROFINET PN, Ethernet IP",2805,"ΤΕΜ",1,"GMC",1,"6SL35201XK040AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-1XM01-5AB0","SINAMICS G115D wall-mounted Rated power: 1.5kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 180 V DC repair switch MQ(X)15 for 400 V AC and M12 for I/O and communication with integrated 24 V DC PSU without looping through without fieldbus",1594,"ΤΕΜ",1,"GMC",1,"6SL35201XM015AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-1XR10-5AB0","SINAMICS G115D wall-mounted Rated power: 0.55 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 180 V DC repair switch with cable gland for 400 V AC Power M12 for 24 V DC with looping through M12 for I/O and communication without fieldbus",1019,"ΤΕΜ",1,"GMC",1,"6SL35201XR105AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-2XA67-5AA0","SINAMICS G115D wall-mounted Rated power: 7.5 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSC Protection class IP65/66 / UL Type 4X brake voltage 180 V DC local remote control with cable gland for 400 V AC and 24 V DC and M12 for I/O and communication fieldbus integrated: AS-Interface",3375,"ΤΕΜ",1,"GMC",1,"6SL35202XA675AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-2XB07-5AA0","SINAMICS G115D wall-mounted Rated power: 7.5 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSC Protection class IP65/66 / UL Type 4X brake voltage 180 V DC local remote control Q4/2 for 400 V AC and M12 for I/O and communication without looping through Q8/0 for motor connection fieldbus integrated: AS-Interface",3551,"ΤΕΜ",1,"GMC",1,"6SL35202XB075AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-2XC01-5AA0","SINAMICS G115D wall-mounted Rated power: 1.5kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 180 V DC local remote control with Quickon for 400 V AC and M12 for I/O and communication without looping through Q8/0 for motor connection fieldbus integrated: AS-Interface",1726,"ΤΕΜ",1,"GMC",1,"6SL35202XC015AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-2XE47-5AF0","SINAMICS G115D wall-mounted Rated power: 7.5 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSC Protection class IP65/66 / UL Type 4X brake voltage 180 V DC local remote control Q4/2 for 400 V AC and Power M12 for 24 V DC and M12 for I/O and communication with looping through Q8/0 for motor connection Fieldbus integrated: PROFINET PN, Ethernet IP",3833,"ΤΕΜ",1,"GMC",1,"6SL35202XE475AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-2XH61-1AF0","SINAMICS G115D wall-mounted Rated power: 1.1 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 180 V DC local remote control with cable gland for 400 V AC and 24 V DC and M12 for I/O and communication with integrated 24 V DC PSU Fieldbus integrated: PROFINET PN, Ethernet IP",1889,"ΤΕΜ",1,"GMC",1,"6SL35202XH611AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-2XL00-7AA0","SINAMICS G115D wall-mounted Rated power: 0.75 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 180 V DC local remote control Quickon for 400 V AC and M12 for I/O and communication with integrated 24 V DC PSU without looping through fieldbus integrated: AS-Interface",1717,"ΤΕΜ",1,"GMC",1,"6SL35202XL007AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-2XM03-0AB0","SINAMICS G115D wall-mounted Rated power: 3 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSB Protection class IP65/66 / UL Type 4X brake voltage 180 V DC local remote control MQ(X)15 for 400 V AC and M12 for I/O and communication with integrated 24 V DC PSU without looping through without fieldbus",2090,"ΤΕΜ",1,"GMC",1,"6SL35202XM030AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-2XR14-0AF0","SINAMICS G115D wall-mounted Rated power: 4 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSB Protection class IP65/66 / UL Type 4X brake voltage 180 V DC local remote control with cable gland for 400 V AC Power M12 for 24 V DC with looping through M12 for I/O and communication Fieldbus integrated: PROFINET PN, Ethernet IP",2551,"ΤΕΜ",1,"GMC",1,"6SL35202XR140AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-3XA21-1AA0","SINAMICS G115D wall-mounted Rated power: 1.1 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 180 V DC repair switch local remote control with cable gland with communication fieldbus integrated: AS-Interface",1491,"ΤΕΜ",1,"GMC",1,"6SL35203XA211AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-3XA67-5AF0","SINAMICS G115D wall-mounted Rated power: 7.5 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSC Protection class IP65/66 / UL Type 4X brake voltage 180 V DC repair switch local remote control with cable gland for 400 V AC and 24 V DC and M12 for I/O and communication Fieldbus integrated: PROFINET PN, Ethernet IP",3706,"ΤΕΜ",1,"GMC",1,"6SL35203XA675AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-3XC00-5AB0","SINAMICS G115D wall-mounted Rated power: 0.55 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 180 V DC repair switch local remote control with Quickon for 400 V AC and Power M12 for 24 V DC and M12 for I/O and communication without looping through Q8/0 for motor connection without fieldbus",1327,"ΤΕΜ",1,"GMC",1,"6SL35203XC005AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-3XE00-7AF0","SINAMICS G115D wall-mounted Rated power: 0.75 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 180 V DC repair switch local remote control Q4/2 for 400 V AC and 7/8\" for 24 V DC and M12 for I/O and communication with looping through Q8/0 for motor connection Fieldbus integrated: PROFINET PN, Ethernet IP",1908,"ΤΕΜ",1,"GMC",1,"6SL35203XE007AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-3XH60-5AA0","SINAMICS G115D wall-mounted Rated power: 0.55 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 180 V DC repair switch local remote control with cable gland for 400 V AC and 24 V DC and M12 for I/O and communication with integrated 24 V DC PSU fieldbus integrated: AS-Interface",1649,"ΤΕΜ",1,"GMC",1,"6SL35203XH605AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-3XK00-7AF0","SINAMICS G115D wall-mounted Rated power: 0.75 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 180 V DC repair switch local remote control Q4/2 for 400 V AC and M12 for I/O and communication with integrated 24 V DC PSU without looping through Fieldbus integrated: PROFINET PN, Ethernet IP",2048,"ΤΕΜ",1,"GMC",1,"6SL35203XK007AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-3XN00-3AF0","SINAMICS G115D wall-mounted rated power: 0.37 kW for 3s 200%, 57s 150%, 240s 87%, RFI suppression filter for category C2 3AC380-480V+10/-10% 45-66Hz ambient temperature -30 to +40 Â°C frame size: FSA degree of protection IP65/66 / UL type 4X brake voltage 180 V DC repair switch local remote control Q4/2 for 400 V AC and M12 for I/O and communication with integrated 24 V DC PSU with looping through Fieldbus integrated: PROFINET PN, Ethernet IP",2034,"ΤΕΜ",1,"GMC",1,"6SL35203XN003AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3520-3XN04-0AF0","SINAMICS G115D wall-mounted Rated power: 4 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSB Protection class IP65/66 / UL Type 4X brake voltage 180 V DC repair switch local remote control Q4/2 for 400 V AC and M12 for I/O and communication with integrated 24 V DC PSU with looping through Fieldbus integrated: PROFINET PN, Ethernet IP",3030,"ΤΕΜ",1,"GMC",1,"6SL35203XN040AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-0XA63-0AA0","SINAMICS G115D wall-mounted Rated power: 3 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSB Protection class IP65/66 / UL Type 4X brake voltage 400 V AC without operation option with cable gland for 400 V AC and 24 V DC and M12 for I/O and communication fieldbus integrated: AS-Interface",2049,"ΤΕΜ",1,"GMC",1,"6SL35210XA630AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-0XB01-5AA0","SINAMICS G115D wall-mounted Rated power: 1.5kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 400 V AC without operation option Q4/2 for 400 V AC and M12 for I/O and communication without looping through Q8/0 for motor connection fieldbus integrated: AS-Interface",1802,"ΤΕΜ",1,"GMC",1,"6SL35210XB015AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-0XD00-7AB0","SINAMICS G115D wall-mounted Rated power: 0.75 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 400 V AC without operation option with MQ(X)15 for 400 V AC and Power M12 for 24 V DC and M12 for I/O and communication without looping through Q8/0 for motor connection without fieldbus",1320,"ΤΕΜ",1,"GMC",1,"6SL35210XD007AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-0XE03-0AF0","SINAMICS G115D wall-mounted Rated power: 3 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSB Protection class IP65/66 / UL Type 4X brake voltage 400 V AC without operation option Q4/2 for 400 V AC and 7/8\" for 24 V DC and M12 for I/O and communication with looping through Q8/0 for motor connection Fieldbus integrated: PROFINET PN, Ethernet IP",2507,"ΤΕΜ",1,"GMC",1,"6SL35210XE030AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-0XE45-5AB0","SINAMICS G115D wall-mounted Rated power: 5.5 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSC Protection class IP65/66 / UL Type 4X brake voltage 400 V AC without operation option Q4/2 for 400 V AC and Power M12 for 24 V DC and M12 for I/O and communication with looping through Q8/0 for motor connection without fieldbus",2815,"ΤΕΜ",1,"GMC",1,"6SL35210XE455AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-0XK00-7AB0","SINAMICS G115D wall-mounted Rated power: 0.75 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 400 V AC without operation option Q4/2 for 400 V AC and M12 for I/O and communication with integrated 24 V DC PSU without looping through without fieldbus",1528,"ΤΕΜ",1,"GMC",1,"6SL35210XK007AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-0XL03-0AF0","SINAMICS G115D wall-mounted Rated power: 3 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSB Protection class IP65/66 / UL Type 4X brake voltage 400 V AC without operation option Quickon for 400 V AC and M12 for I/O and communication with integrated 24 V DC PSU without looping through Fieldbus integrated: PROFINET PN, Ethernet IP",2647,"ΤΕΜ",1,"GMC",1,"6SL35210XL030AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-0XN03-0AF0","SINAMICS G115D wall-mounted Rated power: 3 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSB Protection class IP65/66 / UL Type 4X brake voltage 400 V AC without operation option Q4/2 for 400 V AC and M12 for I/O and communication with integrated 24 V DC PSU with looping through Fieldbus integrated: PROFINET PN, Ethernet IP",2683,"ΤΕΜ",1,"GMC",1,"6SL35210XN030AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-1XA07-5AB0","SINAMICS G115D wall-mounted Rated power: 7.5 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSC Protection class IP65/66 / UL Type 4X brake voltage 400 V AC repair switch with cable gland without communication without fieldbus",3235,"ΤΕΜ",1,"GMC",1,"6SL35211XA075AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-1XB05-5AA0","SINAMICS G115D wall-mounted Rated power: 5.5 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSC Protection class IP65/66 / UL Type 4X brake voltage 400 V AC repair switch Q4/2 for 400 V AC and M12 for I/O and communication without looping through Q8/0 for motor connection fieldbus integrated: AS-Interface",3129,"ΤΕΜ",1,"GMC",1,"6SL35211XB055AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-1XC01-5AF0","SINAMICS G115D wall-mounted Rated power: 1.5kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 400 V AC repair switch with Quickon for 400 V AC and Power M12 for 24 V DC and M12 for I/O and communication without looping through Q8/0 for motor connection Fieldbus integrated: PROFINET PN, Ethernet IP",2133,"ΤΕΜ",1,"GMC",1,"6SL35211XC015AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-1XE40-5AF0","SINAMICS G115D wall-mounted Rated power: 0.55 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 400 V AC repair switch Q4/2 for 400 V AC and Power M12 for 24 V DC and M12 for I/O and communication with looping through Q8/0 for motor connection Fieldbus integrated: PROFINET PN, Ethernet IP",1951,"ΤΕΜ",1,"GMC",1,"6SL35211XE405AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-1XH01-5AB0","SINAMICS G115D wall-mounted Rated power: 1.5kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 400 V AC repair switch with cable gland without communication with integrated 24 V DC PSU without fieldbus",1642,"ΤΕΜ",1,"GMC",1,"6SL35211XH015AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-1XK03-0AA0","SINAMICS G115D wall-mounted Rated power: 3 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSB Protection class IP65/66 / UL Type 4X brake voltage 400 V AC repair switch Q4/2 for 400 V AC and M12 for I/O and communication with integrated 24 V DC PSU without looping through fieldbus integrated: AS-Interface",2548,"ΤΕΜ",1,"GMC",1,"6SL35211XK030AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-1XM00-5AA0","SINAMICS G115D wall-mounted Rated power: 0.55 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 400 V AC repair switch MQ(X)15 for 400 V AC and M12 for I/O and communication with integrated 24 V DC PSU without looping through fieldbus integrated: AS-Interface",1876,"ΤΕΜ",1,"GMC",1,"6SL35211XM005AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-1XR07-5AB0","SINAMICS G115D wall-mounted Rated power: 7.5 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSC Protection class IP65/66 / UL Type 4X brake voltage 400 V AC repair switch with cable gland for 400 V AC and 24 V DC and M12 for I/O and communication Q8/0 for motor connection without fieldbus",3399,"ΤΕΜ",1,"GMC",1,"6SL35211XR075AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-2XA01-1AB0","SINAMICS G115D wall-mounted Rated power: 1.1 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 400 V AC local remote control with cable gland without communication without fieldbus",1375,"ΤΕΜ",1,"GMC",1,"6SL35212XA011AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-2XA61-5AB0","SINAMICS G115D wall-mounted Rated power: 1.5kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 400 V AC local remote control with cable gland for 400 V AC and 24 V DC and M12 for I/O and communication without fieldbus",1549,"ΤΕΜ",1,"GMC",1,"6SL35212XA615AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-2XC00-7AF0","SINAMICS G115D wall-mounted Rated power: 0.75 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 400 V AC local remote control with Quickon for 400 V AC and Power M12 for 24 V DC and M12 for I/O and communication without looping through Q8/0 for motor connection Fieldbus integrated: PROFINET PN, Ethernet IP",1990,"ΤΕΜ",1,"GMC",1,"6SL35212XC007AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-2XE00-7AB0","SINAMICS G115D wall-mounted Rated power: 0.75 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 400 V AC local remote control Q4/2 for 400 V AC and 7/8\" for 24 V DC and M12 for I/O and communication with looping through Q8/0 for motor connection without fieldbus",1577,"ΤΕΜ",1,"GMC",1,"6SL35212XE007AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-2XH21-1AF0","SINAMICS G115D wall-mounted Rated power: 1.1 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 400 V AC local remote control with cable gland with communication with integrated 24 V DC PSU Fieldbus integrated: PROFINET PN, Ethernet IP",2088,"ΤΕΜ",1,"GMC",1,"6SL35212XH211AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-2XK00-3AA0","SINAMICS G115D wall-mounted rated power: 0.37 kW for 3s 200%, 57s 150%, 240s 87%, RFI suppression filter for category C2 3AC380-480V+10/-10% 45-66Hz ambient temperature -30 to +40 Â°C frame size: FSA degree of protection IP65/66 / UL type 4X brake voltage 400 V AC local remote control Q4/2 for 400 V AC and M12 for I/O and communication with integrated 24 V DC PSU without looping through fieldbus integrated: AS-Interface",1933,"ΤΕΜ",1,"GMC",1,"6SL35212XK003AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-2XM01-1AF0","SINAMICS G115D wall-mounted Rated power: 1.1 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 400 V AC local remote control MQ(X)15 for 400 V AC and M12 for I/O and communication with integrated 24 V DC PSU without looping through Fieldbus integrated: PROFINET PN, Ethernet IP",2305,"ΤΕΜ",1,"GMC",1,"6SL35212XM011AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-2XN00-7AB0","SINAMICS G115D wall-mounted Rated power: 0.75 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 400 V AC local remote control Q4/2 for 400 V AC and M12 for I/O and communication with integrated 24 V DC PSU with looping through without fieldbus",1752,"ΤΕΜ",1,"GMC",1,"6SL35212XN007AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-3XA60-5AB0","SINAMICS G115D wall-mounted Rated power: 0.55 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 400 V AC repair switch local remote control with cable gland for 400 V AC and 24 V DC and M12 for I/O and communication without fieldbus",1416,"ΤΕΜ",1,"GMC",1,"6SL35213XA605AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-3XA65-5AB0","SINAMICS G115D wall-mounted Rated power: 5.5 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSC Protection class IP65/66 / UL Type 4X brake voltage 400 V AC repair switch local remote control with cable gland for 400 V AC and 24 V DC and M12 for I/O and communication without fieldbus",2876,"ΤΕΜ",1,"GMC",1,"6SL35213XA655AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-3XC05-5AA0","SINAMICS G115D wall-mounted Rated power: 5.5 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSC Protection class IP65/66 / UL Type 4X brake voltage 400 V AC repair switch local remote control with Quickon for 400 V AC and M12 for I/O and communication without looping through Q8/0 for motor connection fieldbus integrated: AS-Interface",3318,"ΤΕΜ",1,"GMC",1,"6SL35213XC055AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-3XE00-5AB0","SINAMICS G115D wall-mounted Rated power: 0.55 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 400 V AC repair switch local remote control Q4/2 for 400 V AC and 7/8\" for 24 V DC and M12 for I/O and communication with looping through Q8/0 for motor connection without fieldbus",1660,"ΤΕΜ",1,"GMC",1,"6SL35213XE005AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-3XH27-5AF0","SINAMICS G115D wall-mounted Rated power: 7.5 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSC Protection class IP65/66 / UL Type 4X brake voltage 400 V AC repair switch local remote control with cable gland with communication with integrated 24 V DC PSU Fieldbus integrated: PROFINET PN, Ethernet IP",4137,"ΤΕΜ",1,"GMC",1,"6SL35213XH275AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-3XH67-5AF0","SINAMICS G115D wall-mounted Rated power: 7.5 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSC Protection class IP65/66 / UL Type 4X brake voltage 400 V AC repair switch local remote control with cable gland for 400 V AC and 24 V DC and M12 for I/O and communication with integrated 24 V DC PSU Fieldbus integrated: PROFINET PN, Ethernet IP",4204,"ΤΕΜ",1,"GMC",1,"6SL35213XH675AF0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-3XL00-5AB0","SINAMICS G115D wall-mounted Rated power: 0.55 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 400 V AC repair switch local remote control Quickon for 400 V AC and M12 for I/O and communication with integrated 24 V DC PSU without looping through without fieldbus",1800,"ΤΕΜ",1,"GMC",1,"6SL35213XL005AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3521-3XN03-0AB0","SINAMICS G115D wall-mounted Rated power: 3 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Â°C size: FSB Protection class IP65/66 / UL Type 4X brake voltage 400 V AC repair switch local remote control Q4/2 for 400 V AC and M12 for I/O and communication with integrated 24 V DC PSU with looping through without fieldbus",2507,"ΤΕΜ",1,"GMC",1,"6SL35213XN030AB0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3540-6DF71-0RH2","DISTRIBUTED SERVO-DRIVE SINAMICS S120M AH48, M(0)=1,3Nm, N(N)=3000 RPM, INPUT: DC 600V ABSOLUTE ENCODER 20 BIT NATURAL AIR COOLING, IM B5, IM V1, IM V3 DEGREE OF PROTECTION: IP65 SHAFT END IP67 PLAIN SHAFT WITH HOLDING BRAKE",5403,"ΤΕΜ",1,"GMC",1,"6SL35406DF710RH2","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL3760-4AV22-0CA0","Rittal VX25 mechanical installation kit - Active Line Modules FS2/FS2+ 400mm",1614,"ΤΕΜ",1,"GMC",1,"6SL37604AV220CA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6SL5166-8AD03-0AA0","SINAMICS S220 terminal kit for Smart Line module 100 mm 16/24 kW design: booksize",148,"ΤΕΜ",1,"GMC",1,"6SL51668AD030AA0","Ρυθμιστές στροφών και συστήματα Motion control"]
["6XV1440-4AH50","Connecting cable for Mobile Panels (MPI/PROFIBUS), Length 5m",330,"ΤΕΜ",1,"SIMATIC",1,"6XV14404AH50","Βιομηχανικός αυτοματισμός SIMATIC"]
["6XV1801-2CH50","Control connecting cable M12-180/M12-180; 5-core; IO-Link port Class B; pre-assembled with M12 plug and M12 socket (A-coded); straight cable outlet; length 5.0 m.",51.300000000000004,"ΤΕΜ",1,"SIMATIC",1,"6XV18012CH50","Βιομηχανικός αυτοματισμός SIMATIC"]
["6XV1820-5AH10","fiber optic cable (62.5/125), standard cable splittable, without connector, sold by the meter, max. Length 2000 m minimum order quantity: 20 m.",5.0999999999999996,"M",1,"SIMATIC",20,"6XV18205AH10","Βιομηχανικός αυτοματισμός SIMATIC"]
["6XV1821-0BN15","PROFIBUS Plastic Fiber Optic, Standard cable with 4 BFOC connectors, length 15 m.",152,"ΤΕΜ",1,"SIMATIC",1,"6XV18210BN15","Βιομηχανικός αυτοματισμός SIMATIC"]
["6XV1843-5EH10-0CC0","MM FO Cord SC/SC; 50/125; pre-assembled with 2x SC duplex connectors; length 1.0 m.",71.699999999999989,"ΤΕΜ",1,"SIMATIC",1,"6XV18435EH100CC0","Βιομηχανικός αυτοματισμός SIMATIC"]
["6XV1860-3PN10","PROFIBUS ECOFAST Hybrid Cable GP, 2xCu 0.64 mm, 4x Cu 1.5 mm2, Cable pre-assembled with ECOFAST plug and socket, trailable, length 10 m.",157,"ΤΕΜ",1,"SIMATIC",1,"6XV18603PN10","Βιομηχανικός αυτοματισμός SIMATIC"]
["6XV1870-3QN50","Industrial Ethernet TP Cord RJ45/RJ45, CAT 6A, TP cable 4x2, pre-assembled with 2 RJ45 connectors, length 50 m.",157,"ΤΕΜ",1,"SIMATIC",1,"6XV18703QN50","Βιομηχανικός αυτοματισμός SIMATIC"]
["6XV1871-5BN12","IE connecting cable IE FC RJ45 Plug-180/IE FC RJ45 Plug-180; IE FC Trailing Cable GP Pre-assembled with 2x IE FC RJ45 plug 180; length 12.0 m.",98.3,"ΤΕΜ",1,"SIMATIC",1,"6XV18715BN12","Βιομηχανικός αυτοματισμός SIMATIC"]
["6XV1873-2D","FO Trailing Cable GP (50/125), UL approval, Trailing cable, splittable, without connector, Sold by the meter, max. length 1000 m Minimum order quantity: 20 m.",10.9,"M",1,"SIMATIC",20,"6XV18732D","Βιομηχανικός αυτοματισμός SIMATIC"]
["6XV1873-6AN20","FO Standard Cable GP (50/125), pre-assembled with 2x2 SC connectors, length 20 m.",168,"ΤΕΜ",1,"SIMATIC",1,"6XV18736AN20","Βιομηχανικός αυτοματισμός SIMATIC"]
["6XV1875-5UH10","N-Connect/ SMA male/male Flexible connection cable pre-assembled, for Suitable for railway applications; flexible connecting cable e.g. for SCALANCE M antenna length: 1 m.",57.2,"ΤΕΜ",1,"SIMATIC",1,"6XV18755UH10","Βιομηχανικός αυτοματισμός SIMATIC"]
["7KM2200-2EA30-1GA1","SENTRON, measuring device, 7KM PAC2200, LCD, L-L: 400 V, L-N: 230 V, 5 A, strd rail instr., 3-phase, M-Bus + MID, apparent /active/reactive energy, self-powered, screw terminals",423.73,"ΤΕΜ",1,"EP",1,"7KM22002EA301GA1","Sentron PAC μετρητές / αναλυτές ενέργειας"]
["7KM9200-0AB00-0AA0","expansion module 4DI / 2DQ, plug-in, for 7KM PAC3220/4200",271.56,"ΤΕΜ",1,"EP",1,"7KM92000AB000AA0","Sentron PAC μετρητές / αναλυτές ενέργειας"]
["7KT1280-5MA01","SEM3 Split Core CT 125:01 - 100 mA Secondary Output Current",200.8,"ΤΕΜ",1,"EP",1,"7KT12805MA01","Sentron PAC μετρητές / αναλυτές ενέργειας"]
["7LF4531-0","weekly time switch Astro digital 230 V 16A 1-channel 2MW",227.7,"ΤΕΜ",1,"EP",1,"7LF45310","Sentron Χρονικά - χρονοδιακόπτες"]
["7ME3411-2LC01-4ER2","SITRANS FUE380 Mains or battery-operated ultrasonic In-Line flowmeter, diameter DN 50 to DN 1200 (2\" to 48\"), custody transfer approved. Suitable for volume flow and thermal energy measurement of liquids, for use in custody transfer meteringÂ in district heating plants, local networks, boiler stations, chiller plants. DANFOSS \"DN250 (10\"\") Carbon Steel,\" EN 1434, qp=400m3/h, qs=1120m3/h, qi=8m3/h EN1092-1   PN16 Compact version, max. 120 Â°C (248 Â°F) Without EU type approval suitable for billing measurements outside Europe where national approvals exist Calibration according to selection pipe size / flow range Impulswert: 10 L/p (not suitable for FUE950 with nominal size 2K up to 3K) Power supply 115 - 230V AC, Backup: 3.6V DC Lithium battery, single pack is included Marking for Standard device with EU type examination certificate (MI004) Language on nameplate English Pulse width: 5 ms",5259,"ΤΕΜ",1,"PI1",1,"7ME34112LC014ER2","Όργανα Μέτρησης Πεδίου"]
["7ME3950-5GL20","Ultrasonic transit time Sensor Clamp-On, High Precision, Size B2H, paired, dedicated, Ex Zone 0,1,2, Class 1, Div 1,2, for steel pipe, Liquid/Gas, Pipe wall thickness from 3,0 - 4,1 mm (0.12 - 0.16 in), Best Temperature >80C (>176F) max. -40C - +121C/-40F - +250F Housing Polyetherimide/Alu non corrosion, incl. Couplant 7ME39600UC20 and sanding block for FST020, FST030 (FUS1010)",1982,"ΤΕΜ",1,"PI1",1,"7ME39505GL20","Όργανα Μέτρησης Πεδίου"]
["7ME3951-0LE20","Ultrasonic transit time Sensor Clamp-On, Universal Size D2, paired, Portabel-BNC any pipe materials, Liquid, Pipe Diameter range 152 - 610 mm (6 - 24 in), Temperature -40C - +121C (-40F - +250F) Housing Polyetherimide/StSt corrosion resistant, incl. Couplant 7ME39600UC20 and sanding block for FST020, FST030 (FUS1010)",1573,"ΤΕΜ",1,"PI1",1,"7ME39510LE20","Όργανα Μέτρησης Πεδίου"]
["7ME3960-0MD00","Mounting hardware for dedicated high precision transducer size C Legacy Part Number: 1012FNH-PC",642,"ΤΕΜ",1,"PI1",1,"7ME39600MD00","Όργανα Μέτρησης Πεδίου"]
["7ME3960-3CM10","Mounting chain for portable transducers: 4x 760mm lengths Legacy Part Number: 1012ML-1",360,"ΤΕΜ",1,"PI1",1,"7ME39603CM10","Όργανα Μέτρησης Πεδίου"]
["7ME6140-2DA10-1AA1","SITRANS FM MAG 1100 F Full-bore electromagnetic flow sensor, sanitary design, diameter DN 10 to DN 100 (3/8\" to 4\"). Suitable for volume flow measurement of liquids (conductive) , for applications in F&B, pharmaceutical industry. . DN25, 1 Inch None (not 3A approved) PFA (no ATEX) EPDM (FDA) Electrode material: Hastelloy C-276 Sensor for remote transmitter (order transmitter separately)- 3A approved No bus Communication Metric cable glands, Polyamid terminal box or MAG 6000i integral mount",1727,"ΤΕΜ",1,"PI4",1,"7ME61402DA101AA1","Όργανα Μέτρησης Πεδίου"]
["7ME6140-2YA20-2AA1","SITRANS FM MAG 1100 F Full-bore electromagnetic flow sensor, sanitary design, diameter DN 10 to DN 100 (3/8\" to 4\"). Suitable for volume flow measurement of liquids (conductive) , for applications in F&B, pharmaceutical industry. . DN50, 2 Inch None (not 3A approved) Ceramic EPDM (FDA) Electrode material: Platinum Sensor for remote transmitter (order transmitter separately)- 3A approved No bus Communication Metric cable glands, Polyamid terminal box or MAG 6000i integral mount",2153,"ΤΕΜ",1,"PI4",1,"7ME61402YA202AA1","Όργανα Μέτρησης Πεδίου"]
["7ME6310-4PE12-1AA1","SITRANS FM MAG 3100 Full-bore electromagnetic flow sensor, flanged, diameter DN 15 to DN 2000 (1/2\" to 78\"). Suitable for volume flow measurement of liquids (conductive), main applications in process industry, chemical industry, steel industry, mining, utility, power generation and distribution, O&G/HPI. . DN200, 8 Inch EN1092-1, PN25 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 EPDM Stainless steel AISI 316Ti / 1.4571 (not for PFA) Sensor for remote transmitter (Order transmitter separately) No bus communication Metric cable glands, Polyamid terminal box or MAG 6000i integral mount",3703,"ΤΕΜ",1,"PI4",1,"7ME63104PE121AA1","Όργανα Μέτρησης Πεδίου"]
["7ME6340-3TC17-6AA1","SITRANS FM MAG 3100 P Full-bore electromagnetic flow sensor, flanged, diameter DN 15 to DN 300 (1/2\" to 12\"). Suitable for volume flow measurement of liquids (conductive), main applications in chemical industry, process industry, pulp & paper, industrial wastewater. . DN100, 4 Inch EN 1092-1, PN 16 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 PFA max 150 deg.C Hastelloy C incl. grounding electrodes Sensor for remote transmitter (order transmitter separately) No bus communication Metric cable glands, Polyamid terminal box or MAG 6000i integral mount",2708,"ΤΕΜ",1,"PI4",1,"7ME63403TC176AA1","Όργανα Μέτρησης Πεδίου"]
["7ME6520-3MC13-2JA1","SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN80, 3 Inch EN 1092-1, PN 16 Carbon steel ASTM A 105, corrosion-resistant coating of category C4 Liner Material: Hard NBR Rubber Hastelloy C-276 incl. grounding electrodes MAG 6000, IP67 / NEMA 4X/6, Polyamid enclosure, With display, 115-230V AC 50/60 Hz No bus communication Metric cable glands, Polyamid terminal box or MAG 6000i integral mount",3137,"ΤΕΜ",1,"PI4",1,"7ME65203MC132JA1","Όργανα Μέτρησης Πεδίου"]
["7ME6520-4PC12-2KA1","SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN200, 8 Inch EN 1092-1, PN 16 Carbon steel ASTM A 105, corrosion-resistant coating of category C4 Liner Material: EPDM Hastelloy C-276 incl. grounding electrodes MAG 5000, IP67 / NEMA 4X/6, Polyamid enclosure, With display, 11-30V DC/11-24V AC 50/60 Hz No bus communication Metric cable glands, Polyamid terminal box or MAG 6000i integral mount",3878,"ΤΕΜ",1,"PI4",1,"7ME65204PC122KA1","Όργανα Μέτρησης Πεδίου"]
["7ME6520-4VB12-2KA1","SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN250, 10 Inch EN 1092-1, PN 10 Carbon steel ASTM A 105, corrosion-resistant coating of category C4 Liner Material: EPDM Hastelloy C-276 incl. grounding electrodes MAG 5000, IP67 / NEMA 4X/6, Polyamid enclosure, With display, 11-30V DC/11-24V AC 50/60 Hz No bus communication Metric cable glands, Polyamid terminal box or MAG 6000i integral mount",4331,"ΤΕΜ",1,"PI4",1,"7ME65204VB122KA1","Όργανα Μέτρησης Πεδίου"]
["7ME6520-5RC13-2JA1","SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN400, 16 Inch EN 1092-1, PN 16 Carbon steel ASTM A 105, corrosion-resistant coating of category C4 Liner Material: Hard NBR Rubber Hastelloy C-276 incl. grounding electrodes MAG 6000, IP67 / NEMA 4X/6, Polyamid enclosure, With display, 115-230V AC 50/60 Hz No bus communication Metric cable glands, Polyamid terminal box or MAG 6000i integral mount",8180,"ΤΕΜ",1,"PI4",1,"7ME65205RC132JA1","Όργανα Μέτρησης Πεδίου"]
["7ME6520-6PC13-2AA2","SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN600, 24 Inch EN 1092-1, PN 16 Carbon steel ASTM A 105, corrosion-resistant coating of category C4 Liner Material: Hard NBR Rubber Hastelloy C-276 incl. grounding electrodes Sensor for remote transmitter (order transmitter separately) No bus communication 1/2 inch NPT cable glands, Polyamid terminal box or MAG 6000i integral mount",9157,"ΤΕΜ",1,"PI4",1,"7ME65206PC132AA2","Όργανα Μέτρησης Πεδίου"]
["7ME6810-3FC31-1AB1","SITRANS FM MAG 8000 Battery-operated electromagnetic flowmeter, flanged, diameter DN 25 to DN 1200 (1\" to 48\"). Suitable for volume flow measurement of liquids (conductive) and water applications within abstraction, distribution network, revenue metering and irrigation. . DN65 / Qmx  100 m3/h(m3), 2 1/2 Inch / Qmx 440 GPM(G), DN65 / Qmx 2.4 Ml/d(Ml) EN 1092-1, PN 16, Conforms to PED EPDM liner and Hastelloy Electrodes, corrosion-resistant coating of category C4 Standard calibration w. max. 0,4% of rate +/- 2mm/s with certificate Region version: Europe Display: m3 based 50 Hz filter Basic version compact Transmitter on sensor Communication: Serial RS 485 interface module Modbus  RTU Internal 2 D-cell battery pack installed and disconnected inside meter",3824,"ΤΕΜ",1,"PI7",1,"7ME68103FC311AB1","Όργανα Μέτρησης Πεδίου"]
["7ME6810-3TC32-1KS1","SITRANS FM MAG 8000 Battery-operated electromagnetic flowmeter, flanged, diameter DN 25 to DN 1200 (1\" to 48\"). Suitable for volume flow measurement of liquids (conductive) and water applications within abstraction, distribution network, revenue metering and irrigation. . DN100  / Qmx  250 m3/h(m3), 4 Inch / Qmx 1100 GPM(Gx100) , DN100  / Qmx 6 Ml/d(Ml) EN 1092-1, PN 16, Conforms to PED EPDM liner and Hastelloy Electrodes, corrosion-resistant coating of category C4 Extended calibration 0,2% of rate +/- 2mm/s with certificate Region version: Europe Display: m3 based 50 Hz filter Advanced version compact Transmitter on sensor 3G/UMTS module for MAG8000 with remote antenna cable(5m) Internal 2 D-cell battery pack installed and disconnected inside meter",6192,"ΤΕΜ",1,"PI7",1,"7ME68103TC321KS1","Όργανα Μέτρησης Πεδίου"]
["7ME6810-6PB31-1AT1","SITRANS FM MAG 8000 Battery-operated electromagnetic flowmeter, flanged, diameter DN 25 to DN 1200 (1\" to 48\"). Suitable for volume flow measurement of liquids (conductive) and water applications within abstraction, distribution network, revenue metering and irrigation. . DN600 / Qmx  10178 m3/h(m3), 24 Inch / Qmx 44813 GPM(Gx100 0), 600 / Qmx 244.2 Ml/d(Ml) EN 1092-1, PN 10, Conforms to PED EPDM liner and Hastelloy Electrodes, corrosion-resistant coating of category C4 Standard calibration w. max. 0,4% of rate +/- 2mm/s with certificate Region version: Europe Display: m3 based 50 Hz filter Basic version compact Transmitter on sensor 3G/UMTS module for MAG8000 with remote antenna cable(5m)  and analog input cable(2.5m) Internal 2 D-cell battery pack installed and disconnected inside meter",17657,"ΤΕΜ",1,"PI7",1,"7ME68106PB311AT1","Όργανα Μέτρησης Πεδίου"]
["7ME6910-2CA30-1AA0","MAG 5000, 19 Inch Insert, IP20 / NEMA 2, Aluminium, 11-30V DC/11-24V AC 50/60 Hz",1775,"ΤΕΜ",1,"PI4",1,"7ME69102CA301AA0","Όργανα Μέτρησης Πεδίου"]
["7MF1565-3BD10-4CA1","SITRANS P200 Transmitters for pressure and absolute pressure for general applications Non-linearity: 0,25 percent (typically) wetted parts material:ceramics, stainless steel plus sealing material; non-wetted parts material: stainless steel Measuring range for gauge: 0 to 2,5 bar, Overload- pressure 6,25 bar Output signal: 0 to 10 V; three-wire connection, power supply DC 12 to 33 V without explosion protection Electrical connection: Cable quick connector PG9 (not with explosion protection) Process connection: G1/4\" male thread to  EN837-1 (1/4\"-BSP male) Sealing material between sensor and housing: Viton (FPM, Standard) Standard version",209,"ΤΕΜ",1,"PI2",1,"7MF15653BD104CA1","Όργανα Μέτρησης Πεδίου"]
["7MF1566-3AG00-1AA1","SITRANS P210 Transmitters for pressure and absolute pressure for low-pressure applications Non-linearity: 0,25 percent (typically) wetted parts material: stainless steel plus sealing material; non-wetted parts material: stainless steel Measuring range for gauge: 0 to 600 mbar, Overload- pressure 2000 mbar Output signal: 4 to 20 mA two-wire connection, power supply DC 7 to 33 V without explosion protection Electrical connection: plug to DIN EN 175301-803-A, threat for packed gland M16 (with connector) Process connection: G1/2\" male to EN 837-1 (1/2\" BSP male) (standard for metric pressure ranges mbar, bar) Sealing material between sensor and housing: Viton (FPM, Standard) Standard version",505,"ΤΕΜ",1,"PI2",1,"7MF15663AG001AA1","Όργανα Μέτρησης Πεδίου"]
["7MF1567-3CG01-1AA1","SITRANS P220 Transmitters for pressure and absolute pressure fully welded version for high-pressure and refrigerant applications Non-linearity: 0,25 Percent (typically) wetted parts material: stainless steel;  non-wetted parts material: stainless steel Measuring range for gauge: 0 to 60 bar, Overload- pressure 150 bar Output signal: 4 to 20 mA two-wire connection, power supply DC 7 to 33 V with Explosion protection: EEx ia Electrical connection: plug to DIN EN 175301-803-A, threat for packed gland M16 (with connector) Process connection: G1/2\" male to EN 837-1 (1/2\" BSP male) (standard for metric pressure ranges mbar, bar) Standard version Standard version",249,"ΤΕΜ",1,"PI2",1,"7MF15673CG011AA1","Όργανα Μέτρησης Πεδίου"]
["7MF1572-1FA21","Transmitters SITRANS LH100 for hydrostatic level measurement, submersible transmitter, two-wire connection, 4...20 mA housing material 316L (1.4404) measuring cell ceramics (96%) with fixed mounted LD-PE cable Measuring range: 0 - 6 mH2O Cable lenght: 10 m . . Sealing material between sensor and housing: EPDM (for drinking water) with ATEX II1 G Ex ia IIC T4 Ga and IECEx Ex ia IIC T4 Ga",707,"ΤΕΜ",1,"PI2",1,"7MF15721FA21","Όργανα Μέτρησης Πεδίου"]
["7MF5987-2EB","O-RING FOR SITRANS P500 FOR USE BETWEEN CELL AND HOUSING, MATERIAL: NBR, QUANTITY: 10",106,"ΤΕΜ",1,"PI1",1,"7MF59872EB","Όργανα Μέτρησης Πεδίου"]
["7MF7900-1AJ","Mounting bracket, stainless steel 1.4404/316L, incl. screw set and accessories M8",78,"ΤΕΜ",1,"PI2",1,"7MF79001AJ","Όργανα Μέτρησης Πεδίου"]
["7MF7906-2BQ","Cable socket Han 7D, metal, blue, straight",188,"ΤΕΜ",1,"PI1",1,"7MF79062BQ","Όργανα Μέτρησης Πεδίου"]
["7MF8997-1AA","Mounting bracket and mounting parts SITRANS P300 Made of stainless steel",72,"ΤΕΜ",1,"PI2",1,"7MF89971AA","Όργανα Μέτρησης Πεδίου"]
["7MF9011-8AB","MOUNTING SET TO SECURE THE VALVES 7MF9011-4DA AND -4EA 1 MOUNTING BRACKET; 2 HEX SCREWS M6X40;1 MOUNTING CLIP; 2 WASHERS 8,4 DIN 125 2 HEX NUTS M8 DIN EN 24032",52,"ΤΕΜ",1,"PI2",1,"7MF90118AB","Όργανα Μέτρησης Πεδίου"]
["7MF9412-6HA","4 SCREWS,7/16-20 UNF X 2 INCH, ANSI B 18.2.1, 2 FLAT-PROFILE GASKETS",19,"ΤΕΜ",1,"PI2",1,"7MF94126HA","Όργανα Μέτρησης Πεδίου"]
["7MH3115-2CA1","PRESSURE PLATE,TOP/BOTTOM FOR LOAD CELLS OF SERIES K (2 OFF REQUIRED) RATED LOAD 280 T",1676,"ΤΕΜ",1,"PI1",1,"7MH31152CA1","Όργανα Μέτρησης Πεδίου"]
["7MH5105-4PD00","Siwarex WL 250 Load Cell ST-S SA 5t C3 - Rated Load 5t - Accuracy class C3 - 6m Cable length, 4 Conductor - Material Stainless steel - Degree of protection IP67",630,"ΤΕΜ",1,"PI1",1,"7MH51054PD00","Όργανα Μέτρησης Πεδίου"]
["7MH5106-3PD01","Siwarex WL 230 Load cell BB-S SA 500kg C3 Ex - Rated Load 500kg - Accuracy class C3 - 3m Cable length, 4 Conductor - Material Stainless steel - Degree of protection IP68 - with explosion protection",536,"ΤΕΜ",1,"PI1",1,"7MH51063PD01","Όργανα Μέτρησης Πεδίου"]
["7MH5113-4LD01","SIWAREX WL280 Load Cell RN-S SA 3.5t C3 Ex - Rated Load 3.5t - Accuracy class C3 according to OIML R60, - 6 m Cable length, 4 Wires - Made of Stainless steel - protection class IP68 Explosion protection",1374,"ΤΕΜ",1,"PI1",1,"7MH51134LD01","Όργανα Μέτρησης Πεδίου"]
["7MH5114-5DL80","Siwarex WL270 Load Cell K-S CA SAFE HT 13 t - Rated Load 13 t - with double bridge - Accuracy 0,3 % - 15m Cable length, 4 Wires - Made of Steel, coated - protection class IP66 - extended Temperature range till 250 degrees cel.",4068,"ΤΕΜ",1,"PI1",1,"7MH51145DL80","Όργανα Μέτρησης Πεδίου"]
["7MH5121-4KD01","Siwarex WL230 load cell SB-S CA 3t C3 Ex, Rated load 3t, Accuracy class C3, 6m cable length, 4 conductor, Material steel, nickel plated Type of protection IP67, with explosion protection",407,"ΤΕΜ",1,"PI1",1,"7MH51214KD01","Όργανα Μέτρησης Πεδίου"]
["7MH5707-4GE00","Guide element for mounting unit SIWAREX WL230 SB-S SA 0,5â€¦2t Max. lateral force: 3 kN Adjusted to the mounting length one-sided or two-sided usable Material: stainless steel 1.4301",328,"ΤΕΜ",1,"PI1",1,"7MH57074GE00","Όργανα Μέτρησης Πεδίου"]
["7MH5713-5DE00","GUIDE ELEMENT FOR COMPACT MOUNTING UNIT SIWAREX WL280 RN-S SA 10 T ... 13 T MAX. LATERAL FORCE: 10 KN ADJUSTED TO THE MOUNTING LENGTH. ONE-SIDED OR ON BOTH SIDES USABLE. MATERIAL: STAINLESS STEEL",813,"ΤΕΜ",1,"PI1",1,"7MH57135DE00","Όργανα Μέτρησης Πεδίου"]
["7MH7560-1AA01","Sitrans AS100: acoustic sensor for flow detection. It can warn of changes to material flow to prevent costly damage or downtime. Sensor: Standard temperature range (-20 C to +80 C) Cable length: 4 meters (13.12 ft) Sensor mounting: none . Approvals: Ordinary Locations/General Purpose (Non-Ex), CE, UKCA, RCM, EAC, KC",1264,"ΤΕΜ",1,"PI1",1,"7MH75601AA01","Όργανα Μέτρησης Πεδίου"]
["7MH7723-1CJ","MD-256,enclosure cover,spare",91,"ΤΕΜ",1,"PI1",1,"7MH77231CJ","Όργανα Μέτρησης Πεδίου"]
["7MH7723-1GK","WS300 CIRCUIT CARD, WITH ENCODER, 32PPR, 2 INT",814,"ΤΕΜ",1,"PI1",1,"7MH77231GK","Όργανα Μέτρησης Πεδίου"]
["7MH7723-1KP","WF100 6\" (150mm) sensing plate 304 std",972,"ΤΕΜ",1,"PI1",1,"7MH77231KP","Όργανα Μέτρησης Πεδίου"]
["7MH7723-1SW","Screw type, telescoper module for adjustment for belt tracking and tensioning, with 150 mm (6\") travel, mild steel, set of 2",462,"ΤΕΜ",1,"PI1",1,"7MH77231SW","Όργανα Μέτρησης Πεδίου"]
["7MH7724-1BT","Weighfeeder calibration weight, 10,000g",359,"ΤΕΜ",1,"PI1",1,"7MH77241BT","Όργανα Μέτρησης Πεδίου"]
["7MH7725-1AP","LOADCELL,MSI,500LB,LOW PROFILE SS, with hardware",1951,"ΤΕΜ",1,"PI1",1,"7MH77251AP","Όργανα Μέτρησης Πεδίου"]
["7ML1100-0BA20","ST-H Ultrasonic level transducer: continuous, non-contact, 0.3 - 10m (1-33ft) range, for liquids. Process connection: ETFE, 2\" NPT ((Taper), ASME B1.20.1) Cable length: 10 m (32.81 ft) . Approvals: CE, UKCA, FM Class I, II, Div. 1, Groups C, D, E, F, G T4A .",953,"ΤΕΜ",1,"PI3",1,"7ML11000BA20","Όργανα Μέτρησης Πεδίου"]
["7ML1830-1BT","Universal Mounting Adapter, 2 inch NPT",178,"ΤΕΜ",1,"PI3",1,"7ML18301BT","Όργανα Μέτρησης Πεδίου"]
["7ML1830-1JA","CABLE GLAND, 1/2\" NPT, General Purpose DIP",32,"ΤΕΜ",1,"PI6",1,"7ML18301JA","Όργανα Μέτρησης Πεδίου"]
["7ML1930-1CV","Steel Enclosure for 2 RD Display",588,"ΤΕΜ",1,"PI1",1,"7ML19301CV","Όργανα Μέτρησης Πεδίου"]
["7ML1930-1GA","Sun shield kit, 304 stainless steel",390,"ΤΕΜ",1,"PI3",1,"7ML19301GA","Όργανα Μέτρησης Πεδίου"]
["7ML5050-0AC12-1DA0","SITRANS LUT400 Series Ultrasonic level controller: continuous, non-contact, 60 m (197 ft) range. Monitors level, volume, and volume flow in liquids, slurries, and solids. With high accuracy volume flow and built in data logging. - Model: SITRANS LUT420 - Level controller Enclosure Display Options: No display (blank lid provided) Input Voltage: 100 to 230 V AC +/- 15% Cable Inlet: 3 cable inlets, 3 M20 plastic cable glands supplied Number of measurement points: Single point system (includes one transducer input,one mA output and one external temperature sensor input) Communications & I/O: HART, 2 discrete inputs, 3 relays Approvals: Ordinary Locations/General Purpose (Non-Ex), CE, UKCA, FM, CCSAUS, UL, RCM, EAC, KC -",1352,"ΤΕΜ",1,"PI3",1,"7ML50500AC121DA0","Όργανα Μέτρησης Πεδίου"]
["7ML5310-1CA06-0AA0","SITRANS LR110 Radar level transmitter, continuous, non-contact, 15m (49.2ft) range, for liquids, slurries, or solids, integrated cable connection. Communications: HART (4 ... 20 mA) Bluetooth function: With Cable length: 30m Process connection: 1-1/2\" NPT [(Taper), ASME B1.20.1]/ electrical connection 1\" NPT . . . Type of protection: Non Ex (ordinary locations) cFMus, cCSAus,CE, RCM . .",1070,"ΤΕΜ",1,"PI1",1,"7ML53101CA060AA0","Όργανα Μέτρησης Πεδίου"]
["7ML5440-0AB00-0AC2","SITRANS LR560 Radar level transmitter with flush lens antenna: continuous, non-contact, 100 m (328 ft) range, for general solids applications. Measurement and process temperature range: 40m (131 ft) max range, -40 C degrees to +100 C degrees Process connection: Universal flat-faced flange fits ANSI/DIN/JIS flanges: 3\" / 80 mm, 304 stainless steel Enclosure (with cable inlet): Stainless Steel, 1 X M20 x 1.5 (plastic gland included) . Label: Sitrans LR560 Pressure Rating: 0.5 bar g (7.5 psi g) maximum Output/communication: 4 to 20 mA, HART Approvals: ATEX II 1 D 1/2 D 2 D Ex ta IIIC T139Â°C Da, ATEX II 3G Ex ic IIC T4 Gc, ATEX II 3G Ex ec IIC T4 Gc; UKEX II 1D 1/2D 2D Ex ta IIIC T139Â°C Da, UKEX II 3G Ex ic IIC T4 Gc, UKEX II 3G Ex ec IIC T4 Gc; INMETRO Ex nA IIC T4 Gc, INMETRO Ex ta IIIC T139Â°C Da, IP68; IECEx Ex ec IIC T4 Gc, IECEx Ex ic IIC T4 Gc, IECEx Ex ta IIIC T139Â°C Da, IP68; CE, UKCA, RED, RCM Local display interface: With LDI (local display interface)",3393,"ΤΕΜ",1,"PI1",1,"7ML54400AB000AC2","Όργανα Μέτρησης Πεδίου"]
["7ML5630-1DD00-0CA0","Pointek CLS200 RF Capacitance point level switch, rod design. Detects level and interface in liquids, solids, slurries, and foam. Adjustable, 5.5 m (18.04 ft), insertion, adaptable sensitivity, with the ability to tune out build-up on probe. Process Connection: Threaded, 316L (1.4404) stainless steel R 1 1/2\" ((BSPT), EN 10226/PT (JIS-T), JIS B 0203) Probe length: (length from flange face) (threaded lengths include process thread) Extended Rod, 500mm (19.69\") Thermal Isolator: Without thermal isolator Wetted Seals: FKM Probe Material: 316L Stainless Steel with PPS probe body Approvals: Dust Ignition Proof CE, RCM, ATEX II 1/2 D T100 Enclosure and Lid: Aluminum epoxy coated 2x 1/2\" NPT via adaptor- cable inlet,IP65 .",1306,"ΤΕΜ",1,"PI6",1,"7ML56301DD000CA0","Όργανα Μέτρησης Πεδίου"]
["7ML5725-1EE12-1AA0","SITRANS LPS200 Rotary paddle point level switch, compact design: level detection in solids. Compact, side or top mount with extension options to 300 mm (11.81 inch). Process temperature: Up to +80 C (+176 F) Power supply: 115 V AC, 1 rev/min. Process connection Threaded: 1-1/4\" NPT ((Taper), ANSI/ASME B1.20.1) Process pressure: Up to 0.5 bar (7.25 psi) Process connection material: Stainless steel 303 (1.4305) flanges 321 (1.4541), tri-clamp 304 (1.4301) Extension length: 100 mm (3.94 inch) Measuring vane: Boot shaped, 35 x 106 mm (1.38 x 4.17 inch) Approvals: CSA/FM Dust Ignition Proof, RCM .",768,"ΤΕΜ",1,"PI1",1,"7ML57251EE121AA0","Όργανα Μέτρησης Πεδίου"]
["7ML5745-1AA02-1CA0","SITRANS LVL100 Vibrating point level switch. Detects level and material in liquids and slurries. Compact, with 40 mm (1.6 inch) insertion. Approvals: ordinary location, CE Version/Process Temperature: Standard -40 to 100 C Process connection: Thread G 3/4\" A PN64 / 316L Electronics: Transistor output PNP 10...55 V DC Housing: 316L Electrical connection / Protection: Acc. to DIN43650 incl. plug with QuickOn connection / IP65 . .",343,"ΤΕΜ",1,"PI1",1,"7ML57451AA021CA0","Όργανα Μέτρησης Πεδίου"]
["7ND4800-8CC","SIREC DM firmware option: event markers (code nr.of recorder requested)",748,"ΤΕΜ",1,"PI1",1,"7ND48008CC","Όργανα Μέτρησης Πεδίου"]
["7ND4801-7AA","CPU SIREC D200 3 channels",2034,"ΤΕΜ",1,"PI1",1,"7ND48017AA","Όργανα Μέτρησης Πεδίου"]
["7NG0320-0HA10-0AA0","SITRANS TR320 Temperature transmitter for rail mounting, with one configurable input and a galvanically isolated 2-wire output. HART (4 â€¦ 20 mA) Input 1 TC Type J None Internal CJC Without enclosure (head mounted and rail mounted transmitter) - General purpose (CE, RCM, FM, KCC, EAC, CSA) None (head mounted and rail mounted transmitter) Without local operation",413,"ΤΕΜ",1,"PI1",1,"7NG03200HA100AA0","Όργανα Μέτρησης Πεδίου"]
["7NG3211-0BN00","Temperature transmitter SITRANS TH100 for PT100 for installation in connection head Type B (DIN 43729), two-wire system, 4...20 mA, programmable, without electrical isolation With explosion protection Intrinsic safety and for type of protection and zone 2, to FM (CFMUS) . .",141,"ΤΕΜ",1,"PI1",1,"7NG32110BN00","Όργανα Μέτρησης Πεδίου"]
["8GE3713-4","SIKUS, ALPHA 630 Mounting assembly for meter installation H=450 mm W=250 mm",356.45,"ΤΕΜ",1,"EP",1,"8GE37134","8GE εξαρτήματα πινάκων"]
["8GF5768","Busbar holder 4-pole ALPHA NF overall width 300 mm For busbar thickness 15x 5, 20x 5 30x 5 mm, for mounting on mounting stays for device installation sets",106.06,"ΤΕΜ",1,"EP",1,"8GF5768","8GF εξαρτήματα πινάκων"]
["8GK1032-1KK31","ALPHA 160, wall-mounted cabinet, IP44, Protection class 2, H: 500 mm, W: 800 mm, T: 140 mm, RAL 9016",601.6,"ΤΕΜ",1,"EP",1,"8GK10321KK31","Alpha πίνακες διανομής"]
["8GK1051-4KK10","ALPHA 160 DIN flush-mounted board with mounting kit for modular devices, RAL 9016, IP31 row distance 125mm with N/PE plug-in terminal SK2, h=950 w=300 d=120",742.4,"ΤΕΜ",1,"EP",1,"8GK10514KK10","Alpha πίνακες διανομής"]
["8GK1081-5KK20","ALPHA 160 DIN flush-mounted board with mounting kit for modular devices, and terminal blocks RAL 9016, IP31, row distance 150mm SK2, h=1100 w=550 d=120",1212.1600000000001,"ΤΕΜ",1,"EP",1,"8GK10815KK20","Alpha πίνακες διανομής"]
["8GK1121-4KK32","ALPHA 400, wall-mounted cabinet, Flush-mounting, IP31, type of protection 1, H: 950 mm, W: 800 mm, T: 210 mm, RAL 9016",658.05,"ΤΕΜ",1,"EP",1,"8GK11214KK32","Alpha πίνακες διανομής"]
["8GK1123-6KA22","ALPHA 400, wall-mounted cabinet, IP55, Protection class 1, H: 1250 mm, W: 550 mm, T: 210 mm, RAL 9016",871.88,"ΤΕΜ",1,"EP",1,"8GK11236KA22","Alpha πίνακες διανομής"]
["8GK1132-4KA52","ALPHA 400, wall-mounted cabinet, IP44, Protection class 2, H: 950 mm, W: 1300 mm, T: 210 mm, RAL 9016",1256.4100000000001,"ΤΕΜ",1,"EP",1,"8GK11324KA52","Alpha πίνακες διανομής"]
["8GK1323-8KN14","ALPHA 630, Floor-mounted cabinet, IP55, Protection class 1, H: 1950 mm, W: 300 mm, T: 320 mm, RAL 7035",1252.3499999999999,"ΤΕΜ",1,"EP",1,"8GK13238KN14","Alpha πίνακες διανομής"]
["8GK1383-2KK23","marshalling box safety class 1, IP55 h=650, w=550, d=250 screwed front plate without stays",758.24,"ΤΕΜ",1,"EP",1,"8GK13832KK23","Alpha πίνακες διανομής"]
["8GK2043-4KL21","ALPHA 125 UNIVERSAL, wall-mounted cabinet, Flush-mounting, with distribution board panel, IP31, Protection class 1, H: 1200 mm, W: 600 mm, T: 140 mm, RAL 7035, with door",1176.25,"ΤΕΜ",1,"EP",1,"8GK20434KL21","Alpha πίνακες διανομής"]
["8GK4101-8KK12","ALPHA 400 DIN, quick assembly Assembly kit for modular installation devices clearance between rows 150 mm with longitudinal stays, H=1200 W=250",248.19,"ΤΕΜ",1,"EP",1,"8GK41018KK12","Alpha πίνακες διανομής"]
["8GK4351-4KK32","ALPHA 400/630 DIN, Assembly kit for modular installation devices 150 mm clearance between rows, H=600 W=750",297.14999999999998,"ΤΕΜ",1,"EP",1,"8GK43514KK32","Alpha πίνακες διανομής"]
["8GK4551-2KK11","ALPHA 160 DIN, Mounting kit for Fuse switch disconnector NH000 and NH00 to 160 A DIN rail, 1x 3NP4010, H=300 W=250",85.84,"ΤΕΜ",1,"EP",1,"8GK45512KK11","Alpha πίνακες διανομής"]
["8GK4651-2KK12","ALPHA 400/630 DIN, Assembly kit for fuse switch disconnector 3NP4015/3NP4016, 1x NH00 for mounting on busbars 40/60 mm, H=300 W=250",89.83,"ΤΕΜ",1,"EP",1,"8GK46512KK12","Alpha πίνακες διανομής"]
["8GK4801-2KK33","ALPHA 400/630 DIN, Assembly kit for SR60 busbar N-system 60mm, 3-pole, H=300, W=750",144.11000000000001,"ΤΕΜ",1,"EP",1,"8GK48012KK33","Alpha πίνακες διανομής"]
["8GK4854-0KK50","Crossbeam for N/PE W=1250 mm for N and/or PE Busbar support",68.14,"ΤΕΜ",1,"EP",1,"8GK48540KK50","Alpha πίνακες διανομής"]
["8GK6714-2KK23","ALPHA 630 Universal, Circuit breaker kit 1x 3VL400, 3+4-pole H=200 mm W=600 mm, horizontal Installation",146.13,"ΤΕΜ",1,"EP",1,"8GK67142KK23","Alpha πίνακες διανομής"]
["8GK6723-2KK33","ALPHA 630 Universal Circuit breaker kit 1x 3VA20-22/100A/160A/250A 3+4-pole H=200 mm W=900 mm, horizontal Installation, for rotary operating mechanism",230.74,"ΤΕΜ",1,"EP",1,"8GK67232KK33","Alpha πίνακες διανομής"]
["8GK9100-0KK01","ALPHA 400/630 DIN, general distributor accessories, Two-component flange",21.52,"ΤΕΜ",1,"EP",1,"8GK91000KK01","Alpha πίνακες διανομής"]
["8GK9120-0KK10","ALPHA 630 Universal Flange plate floor-mounted distribution board IP43 W=300",18.75,"ΤΕΜ",1,"EP",1,"8GK91200KK10","Alpha πίνακες διανομής"]
["8GK9505-3KK20","ALPHA 125, 630 Universal, Door IP43, Transparent (simple version), RAL 7035, H=400, W=600",180.35,"ΤΕΜ",1,"EP",1,"8GK95053KK20","Alpha πίνακες διανομής"]
["8GK9510-8KK58","ALPHA, door half, on the right, IP55, H: 1400 mm, W: 525 mm, RAL 9016, type of protection 1 and 2",233.5,"ΤΕΜ",1,"EP",1,"8GK95108KK58","Alpha πίνακες διανομής"]
["8GK9515-7KK30","ALPHA 630 Universal, Door IP43, sheet, RAL 7035, H=1200, W=900",285.92,"ΤΕΜ",1,"EP",1,"8GK95157KK30","Alpha πίνακες διανομής"]
["8GK9535-8KK24","ALPHA 630 Universal, Cabinet-high mounting plate 2 mm thick for direct mounting in enclosure Height=1800 mm, Width=600 mm",231.7,"ΤΕΜ",1,"EP",1,"8GK95358KK24","Alpha πίνακες διανομής"]
["8GK9601-1KK20","ALPHA 630 DIN, cover Height=150 mm, Width=500 mm, Closed Minimum order quantity 10 units",33.69,"ΤΕΜ",1,"EP",10,"8GK96011KK20","Alpha πίνακες διανομής"]
["8GK9720-0KK01","ALPHA AS busbar holder Busbar clearance 100 mm or 185 mm incl. fixing screws for copper bars without retaining angle",104.58,"ΤΕΜ",1,"EP",1,"8GK97200KK01","Alpha πίνακες διανομής"]
["8GK9901-0KK22","ALPHA, Base, H: 100 mm, W: 550 mm, T: 210 mm, RAL 7035",190.44,"ΤΕΜ",1,"EP",1,"8GK99010KK22","Alpha πίνακες διανομής"]
["8GK9910-1KK24","Circuit diagram pocket depth 30 mm Pack of 25 units Plastic",20.62,"ΤΕΜ",1,"EP",25,"8GK99101KK24","Alpha πίνακες διανομής"]
["8GK9920-0KK13","ALPHA Universal, PE bar, W=900",85.17,"ΤΕΜ",1,"EP",1,"8GK99200KK13","Alpha πίνακες διανομής"]
["8MF1000-2HE","SIVACON, earthquake kit, for stabilisation of a swing frame",165.41,"ΤΕΜ",1,"EP",1,"8MF10002HE","Sivacon Πίνακες"]
["8MF1000-2UT14-4BA2","SIVACON, door, right, for the interior of the cabinet, H: 2000 mm, W: 1000 mm, RAL 7035, Protection class 1",545.9,"ΤΕΜ",1,"EP",1,"8MF10002UT144BA2","Sivacon Πίνακες"]
["8MF1000-2VS","SIVACON, Screw, M6x12",58.92,"ΤΕΜ",1,"EP",1,"8MF10002VS","Sivacon Πίνακες"]
["8MF1006-2GS30","SIVACON, Supporting structure, for standard Empty enclosure, H: 2000 mm, W: 1000 mm, T: 600 mm, zinc-plated",976.44,"ΤΕΜ",1,"EP",1,"8MF10062GS30","Sivacon Πίνακες"]
["8MF1008-3VR4","SIVACON, Control panel Empty enclosure, without side panels, according to IEC 62208, with Ventilation openings IP20, H: 2000 mm, W: 1000 mm, T: 800 mm",4284.8,"ΤΕΜ",1,"EP",1,"8MF10083VR4","Sivacon Πίνακες"]
["8MF1024-2UB52-0","SIVACON, base, with cutouts for flanges, IPXX, T: 400 mm, W: 1200 mm, zinc-plated",117.01,"ΤΕΜ",1,"EP",1,"8MF10242UB520","Sivacon Πίνακες"]
["8MF1026-2UD10-0A","SIVACON, Roof, Closed, IP40, W: 1200 mm, T: 600 mm, zinc-plated",153.47,"ΤΕΜ",1,"EP",1,"8MF10262UD100A","Sivacon Πίνακες"]
["8MF1040-2UT14-0BA2","SIVACON, door, right, IP55, H: 2000 mm, W: 400 mm, RAL 7035, Protection class 1",706.58,"ΤΕΜ",1,"EP",1,"8MF10402UT140BA2","Sivacon Πίνακες"]
["8MF1040-2VH","SIVACON, roof trough, for Increased degree of protection, IPX1, W: 400 mm, T: 1000 mm, RAL 7035",278.10000000000002,"ΤΕΜ",1,"EP",1,"8MF10402VH","Sivacon Πίνακες"]
["8MF1050-2UT14-3BA2","SIVACON, door, right, with cutout for filter fan, with ventilation openings H: 2000 mm, W: 500 mm, RAL 7035, Protection class 1",737.48,"ΤΕΜ",1,"EP",1,"8MF10502UT143BA2","Sivacon Πίνακες"]
["8MF1060-2UT14-0CA1","SIVACON, door, right, EMC, IP40, H: 2000 mm, W: 600 mm, RAL 7035, Protection class 1",1507.92,"ΤΕΜ",1,"EP",1,"8MF10602UT140CA1","Sivacon Πίνακες"]
["8MF1064-2UD12-0A","SIVACON, Roof, EMC, EMC, IP40, W: 600 mm, T: 400 mm, zinc-plated",284.27999999999997,"ΤΕΜ",1,"EP",1,"8MF10642UD120A","Sivacon Πίνακες"]
["8MF1066-2UD12-0A","SIVACON, Roof, EMC, EMC, IP40, W: 600 mm, T: 600 mm, zinc-plated",306.94,"ΤΕΜ",1,"EP",1,"8MF10662UD120A","Sivacon Πίνακες"]
["8MF1068-3VR4","SIVACON, Control panel Empty enclosure, without side panels, according to IEC 62208, with Ventilation openings IP20, H: 2000 mm, W: 600 mm, T: 800 mm",3110.6,"ΤΕΜ",1,"EP",1,"8MF10683VR4","Sivacon Πίνακες"]
["8MF1080-3BR4","SIVACON, Control panel Empty enclosure, without side panels, according to IEC 62208, IP40, H: 2000 mm, W: 800 mm, T: 1000 mm",3399,"ΤΕΜ",1,"EP",1,"8MF10803BR4","Sivacon Πίνακες"]
["8MF1084-2UD20-0A","SIVACON, Roof, with Ventilation openings with Ventilation openings IP20, W: 800 mm, T: 400 mm, zinc-plated",96,"ΤΕΜ",1,"EP",1,"8MF10842UD200A","Sivacon Πίνακες"]
["8MF1088-2UD20-0A","SIVACON, Roof, with Ventilation openings with Ventilation openings IP20, W: 800 mm, T: 800 mm, zinc-plated",188.49,"ΤΕΜ",1,"EP",1,"8MF10882UD200A","Sivacon Πίνακες"]
["8MF1090-2UT15-0CA1","SIVACON, door, left, EMC, IP40, H: 2000 mm, W: 900 mm, RAL 7035, Protection class 1",1631.52,"ΤΕΜ",1,"EP",1,"8MF10902UT150CA1","Sivacon Πίνακες"]
["8MF1096-2VH","SIVACON, roof trough, for Increased degree of protection, IPX1, W: 900 mm, T: 600 mm, RAL 7035",296.64,"ΤΕΜ",1,"EP",1,"8MF10962VH","Sivacon Πίνακες"]
["8MF1111-0AA00-0AB6","SIVACON 1800mm x 400mm x 400mm",1577.96,"ΤΕΜ",1,"EP",1,"8MF11110AA000AB6","Sivacon Πίνακες"]
["8MF1111-0AA00-0AK6","SIVACON 2000mm x 800mm x 400mm",3914,"ΤΕΜ",1,"EP",1,"8MF11110AA000AK6","Sivacon Πίνακες"]
["8MF1111-0AA00-0AN0","SIVACON 2000mm x 800mm x 600mm",3852.2,"ΤΕΜ",1,"EP",1,"8MF11110AA000AN0","Sivacon Πίνακες"]
["8MF1111-0AA00-0AT7","SIVACON 2000mm x 600mm x 500mm",3481.4,"ΤΕΜ",1,"EP",1,"8MF11110AA000AT7","Sivacon Πίνακες"]
["8MF1111-0AA00-0BC2","SIVACON 2200mm x 900mm x 600mm",9764.4,"ΤΕΜ",1,"EP",1,"8MF11110AA000BC2","Sivacon Πίνακες"]
["8MF1111-0AA00-0BL5","SIVACON 2000mm x 600mm x 600mm",3605,"ΤΕΜ",1,"EP",1,"8MF11110AA000BL5","Sivacon Πίνακες"]
["8MF1111-0AA00-0BR1","SIVACON 2000mm x 600mm x 400mm SIVACON 2000mm x 1000mm x 600mm",3914,"ΤΕΜ",1,"EP",1,"8MF11110AA000BR1","Sivacon Πίνακες"]
["8MF1111-0AA00-0BV6","SIVACON 2200mm x 900mm x 400mm",4326,"ΤΕΜ",1,"EP",1,"8MF11110AA000BV6","Sivacon Πίνακες"]
["8MF1111-0AA00-0CJ2","SIVACON 1800mm x 600mm x 400mm",3749.2,"ΤΕΜ",1,"EP",1,"8MF11110AA000CJ2","Sivacon Πίνακες"]
["8MF1111-0AA00-0CL5","SIVACON 2000mm x 800mm x 500mm",4058.2,"ΤΕΜ",1,"EP",1,"8MF11110AA000CL5","Sivacon Πίνακες"]
["8MF1111-0AA00-0CV0","SIVACON 2200mm x 800mm x 600mm",5932.8,"ΤΕΜ",1,"EP",1,"8MF11110AA000CV0","Sivacon Πίνακες"]
["8MF1111-0AA00-0DB4","SIVACON 2000mm x 600mm x 500mm",3605,"ΤΕΜ",1,"EP",1,"8MF11110AA000DB4","Sivacon Πίνακες"]
["8MF1111-0AA00-0DK7","SIVACON 2000mm x 800mm x 600mm",4655.6000000000004,"ΤΕΜ",1,"EP",1,"8MF11110AA000DK7","Sivacon Πίνακες"]
["8MF1111-0AA00-0DS8","SIVACON 2200mm x 600mm x 600mm",3831.6,"ΤΕΜ",1,"EP",1,"8MF11110AA000DS8","Sivacon Πίνακες"]
["8MF1111-0AA00-0EB6","SIVACON 2000mm x 600mm x 600mm",3625.6,"ΤΕΜ",1,"EP",1,"8MF11110AA000EB6","Sivacon Πίνακες"]
["8MF1111-0AA00-0EE0","SIVACON 2000mm x 800mm x 600mm",4717.3999999999996,"ΤΕΜ",1,"EP",1,"8MF11110AA000EE0","Sivacon Πίνακες"]
["8MF1111-0AA00-0EM2","SIVACON 2000mm x 1200mm x 500mm",5314.8,"ΤΕΜ",1,"EP",1,"8MF11110AA000EM2","Sivacon Πίνακες"]
["8MF1111-0AA00-0EU2","SIVACON 1800mm x 600mm x 500mm",3584.4,"ΤΕΜ",1,"EP",1,"8MF11110AA000EU2","Sivacon Πίνακες"]
["8MF1111-0AA00-0FD6","SIVACON 2000mm x 600mm x 400mm",3790.4,"ΤΕΜ",1,"EP",1,"8MF11110AA000FD6","Sivacon Πίνακες"]
["8MF1111-0AA00-0FH7","SIVACON 2200mm x 600mm x 400mm",4202.3999999999996,"ΤΕΜ",1,"EP",1,"8MF11110AA000FH7","Sivacon Πίνακες"]
["8MF1111-0AA00-0FM1","SIVACON 2000mm x 900mm x 600mm",5047,"ΤΕΜ",1,"EP",1,"8MF11110AA000FM1","Sivacon Πίνακες"]
["8MF1111-0AA00-0GB4","SIVACON 2200mm x 800mm x 800mm",5356,"ΤΕΜ",1,"EP",1,"8MF11110AA000GB4","Sivacon Πίνακες"]
["8MF1111-0AA00-0GG8","SIVACON 2000mm x 900mm x 800mm",4305.3999999999996,"ΤΕΜ",1,"EP",1,"8MF11110AA000GG8","Sivacon Πίνακες"]
["8MF1111-0AA00-0GP5","SIVACON 2000mm x 800mm x 800mm",4593.8,"ΤΕΜ",1,"EP",1,"8MF11110AA000GP5","Sivacon Πίνακες"]
["8MF1111-0AA00-0GV3","SIVACON 2000mm x 600mm x 500mm",3625.6,"ΤΕΜ",1,"EP",1,"8MF11110AA000GV3","Sivacon Πίνακες"]
["8MF1111-0AA00-0HF5","SIVACON 2000mm x 1200mm x 500mm",5417.8,"ΤΕΜ",1,"EP",1,"8MF11110AA000HF5","Sivacon Πίνακες"]
["8MF1111-0AA00-0HH1","SIVACON 2000mm x 800mm x 600mm",3996.4,"ΤΕΜ",1,"EP",1,"8MF11110AA000HH1","Sivacon Πίνακες"]
["8MF1111-0AA00-0HM8","SIVACON 2000mm x 400mm x 400mm",3419.6,"ΤΕΜ",1,"EP",1,"8MF11110AA000HM8","Sivacon Πίνακες"]
["8MF1200-2AN30","SIVACON, 19\" fixed mounting, for the installation of 19\" devices, H: 600 mm, zinc-plated",119.48,"ΤΕΜ",1,"EP",1,"8MF12002AN30","Sivacon Πίνακες"]
["8MF1206-3VR4","SIVACON, Control panel Empty enclosure, without side panels, according to IEC 62208, with Ventilation openings IP20, H: 2200 mm, W: 1000 mm, T: 600 mm",4367.2,"ΤΕΜ",1,"EP",1,"8MF12063VR4","Sivacon Πίνακες"]
["8MF1230-2UT15-2BA2","SIVACON, door, left, ventilated, IP40, H: 2200 mm, W: 300 mm, RAL 7035, Protection class 1",698.34,"ΤΕΜ",1,"EP",1,"8MF12302UT152BA2","Sivacon Πίνακες"]
["8MF1240-2UT15-1BA2","SIVACON, door, left, ventilated, IP20, H: 2200 mm, W: 400 mm, RAL 7035, Protection class 1",712.76,"ΤΕΜ",1,"EP",1,"8MF12402UT151BA2","Sivacon Πίνακες"]
["8MF1260-2UT15-2BA2","SIVACON, door, left, ventilated, IP40, H: 2200 mm, W: 600 mm, RAL 7035, Protection class 1",811.64,"ΤΕΜ",1,"EP",1,"8MF12602UT152BA2","Sivacon Πίνακες"]
["8MF1264-3BR5","SIVACON, Control panel Empty enclosure, without side panels, according to IEC 62208, IP55, H: 2200 mm, W: 600 mm, T: 400 mm",3172.4,"ΤΕΜ",1,"EP",1,"8MF12643BR5","Sivacon Πίνακες"]
["8MF1280-2UT25-3BA2","SIVACON, door half, left, with cutout for filter fan, with ventilation openings H: 2200 mm, W: 800 mm, RAL 7035, Protection class 1",733.36,"ΤΕΜ",1,"EP",1,"8MF12802UT253BA2","Sivacon Πίνακες"]
["8MF1290-3BR5","SIVACON, Control panel Empty enclosure, without side panels, according to IEC 62208, IP55, H: 2200 mm, W: 900 mm, T: 1000 mm",4490.8,"ΤΕΜ",1,"EP",1,"8MF12903BR5","Sivacon Πίνακες"]
["8MF1308-2HH","SIVACON, cable propping bar, D: 800 mm, H: 30 mm, zinc-plated",39.14,"ΤΕΜ",1,"EP",1,"8MF13082HH","Sivacon Πίνακες"]
["8MF1460-2HL7","SIVACON, cable channel, halogen-free, L: 2000 mm, H: 100 mm, W: 75 mm",226.6,"ΤΕΜ",1,"EP",1,"8MF14602HL7","Sivacon Πίνακες"]
["8MF1680-2AM12-0","SIVACON, mounting plate, mounting with bracket, perforated, H: 600 mm, W: 800 mm, zinc-plated",205.8,"ΤΕΜ",1,"EP",1,"8MF16802AM120","Sivacon Πίνακες"]
["8MF1806-3VS4","SIVACON, Control panel Empty enclosure, according to IEC 62208, with ventilation openings, IP20, H: 1800 mm, W: 1000 mm, T: 600 mm",4573.2,"ΤΕΜ",1,"EP",1,"8MF18063VS4","Sivacon Πίνακες"]
["8MF1825-3BS5","SIVACON, Control panel Empty enclosure, according to IEC 62208, IP55, H: 1800 mm, W: 1200 mm, T: 500 mm",4944,"ΤΕΜ",1,"EP",1,"8MF18253BS5","Sivacon Πίνακες"]
["8MF1844-3BR4","SIVACON, Control panel Empty enclosure, without side panels, according to IEC 62208, IP40, H: 1800 mm, W: 400 mm, T: 400 mm",2575,"ΤΕΜ",1,"EP",1,"8MF18443BR4","Sivacon Πίνακες"]
["8MF1860-2AA02-0","SIVACON, mounting plate, Quick assembly with screws, H: 800 mm, W: 600 mm, zinc-plated",171.6,"ΤΕΜ",1,"EP",1,"8MF18602AA020","Sivacon Πίνακες"]
["8MF1870-2UT14-2BA2","SIVACON, door, on the right, ventilated, IP40, H: 1800 mm, W: 450 mm, RAL 7035, Protection class 1",710.7,"ΤΕΜ",1,"EP",1,"8MF18702UT142BA2","Sivacon Πίνακες"]
["8MF1880-3BR4","SIVACON, Control panel Empty enclosure, without side panels, according to IEC 62208, IP40, H: 1800 mm, W: 800 mm, T: 1000 mm",3275.4,"ΤΕΜ",1,"EP",1,"8MF18803BR4","Sivacon Πίνακες"]
["8MF1890-3VS4","SIVACON, Control panel Empty enclosure, according to IEC 62208, with ventilation openings, IP20, H: 1800 mm, W: 900 mm, T: 1000 mm",4944,"ΤΕΜ",1,"EP",1,"8MF18903VS4","Sivacon Πίνακες"]
["8MF1896-3BS4","SIVACON, Control panel Empty enclosure, according to IEC 62208, IP40, H: 1800 mm, W: 900 mm, T: 600 mm",4305.3999999999996,"ΤΕΜ",1,"EP",1,"8MF18963BS4","Sivacon Πίνακες"]
["8MF2084-5E","standard cabinet 8MF2 HxWxD=2000x 800x 400 Installation: single non-ventilated, assembled, welded IP54,",5183.2,"ΤΕΜ",1,"EP",1,"8MF20845E","Sivacon Πίνακες"]
["8MF2098-4R","standard cabinet 8MF2 HxWxD=2000x 900x 800 Installation: Side-by-side non-ventilated, assembled, welded IP40",4340.93,"ΤΕΜ",1,"EP",1,"8MF20984R","Sivacon Πίνακες"]
["8MF2286-4E","standard cabinet 8MF2 HxWxD=2200x 800x 600 Installation: single non-ventilated, assembled, welded IP40",5053.62,"ΤΕΜ",1,"EP",1,"8MF22864E","Sivacon Πίνακες"]
["8MF2296-5R","standard cabinet 8MF2 HxWxD=2200x 900x 600 Installation: Side-by-side non-ventilated, assembled, welded IP54,",4924.04,"ΤΕΜ",1,"EP",1,"8MF22965R","Sivacon Πίνακες"]
["8MF2826-3RB","standard cabinet 8MF2 HxWxD=1800x 1200x 600 Installation: Side-by-side ventilated, mounted, welded IP30",5701.52,"ΤΕΜ",1,"EP",1,"8MF28263RB","Sivacon Πίνακες"]
["8MF2896-5R","standard cabinet 8MF2 HxWxD=1800x 900x 600 Installation: Side-by-side non-ventilated, assembled, welded IP54,",4567.7,"ΤΕΜ",1,"EP",1,"8MF28965R","Sivacon Πίνακες"]
["8MF3057","Double-wing door, asymmetrically separate, instead of single-wing door HxW=2000x 800 IP40 Price is an additional price for Standard version",783.96,"ΤΕΜ",1,"EP",1,"8MF3057","Sivacon Πίνακες"]
["8MF3203","standard door of standard rear panel HxW=1800x 1000 IP40 Price is an additional price for Standard version",910.3,"ΤΕΜ",1,"EP",1,"8MF3203","Sivacon Πίνακες"]
["8MF3302","lock insert for square key 8 mm pin instead of 3 mm pin Price is an additional price for Standard version",32.07,"ΤΕΜ",1,"EP",1,"8MF3302","Sivacon Πίνακες"]
["8MF3446","SIVACON, roof, with ventilation openings IP20, W: 800 mm, D: 600 mm, RAL 7032",440.57,"ΤΕΜ",1,"EP",1,"8MF3446","Sivacon Πίνακες"]
["8MF3527","Side cover panel for busbar top plate D=600 IP20 Price is an additional price for Standard version",70.62,"ΤΕΜ",1,"EP",1,"8MF3527","Sivacon Πίνακες"]
["8MF4048","Socket HxWxD=200x 1200x 800",978.33,"ΤΕΜ",1,"EP",1,"8MF4048","Sivacon Πίνακες"]
["8MF4085","Base plate subdivided once WxD=800x 400",524.79999999999995,"ΤΕΜ",1,"EP",1,"8MF4085","Sivacon Πίνακες"]
["8MF4304","Circuit diagram pocket made of sheet steel",217.37,"ΤΕΜ",1,"EP",1,"8MF4304","Sivacon Πίνακες"]
["8MF4427","C-section mounting rail Cable propping bar C50 D=800",174.29,"ΤΕΜ",1,"EP",1,"8MF4427","Sivacon Πίνακες"]
["8MF4711","Mounting kit for circuit breaker WxD=800x 600 2x supporting bars, 4x C50 profile, incl. Mounting material",975.09,"ΤΕΜ",1,"EP",1,"8MF4711","Sivacon Πίνακες"]
["8MF4838","19-inch frame for 7HU",333.67,"ΤΕΜ",1,"EP",1,"8MF4838","Sivacon Πίνακες"]
["8MF4888","19-inch swing frame 44 MW/43 MW H=2200",2429.63,"ΤΕΜ",1,"EP",1,"8MF4888","Sivacon Πίνακες"]
["8MF5088-5R","Standard cabinet 8MF5 HxWxD=2000x 800x 800 Installation: Side-by-side non-ventilated, not mounted, screwed IP54,",5247.99,"ΤΕΜ",1,"EP",1,"8MF50885R","Sivacon Πίνακες"]
["8MF5298-5E","Standard cabinet 8MF5 HxWxD=2200x 900x 800 Installation: single non-ventilated, not mounted, screwed IP54,",7029.72,"ΤΕΜ",1,"EP",1,"8MF52985E","Sivacon Πίνακες"]
["8MF5894-5R","Standard cabinet 8MF5 HxWxD=1800x 900x 400 Installation: Side-by-side non-ventilated, not mounted, screwed IP54,",5021.2299999999996,"ΤΕΜ",1,"EP",1,"8MF58945R","Sivacon Πίνακες"]
["8MF6024-5E","Standard cabinet 8MF6 HxWxD=2000x 1200x 400 Installation: single non-ventilated, assembled, welded IP54,",7515.64,"ΤΕΜ",1,"EP",1,"8MF60245E","Sivacon Πίνακες"]
["8MF6098-4E","Standard cabinet 8MF6 HxWxD=2000x 900x 800 Installation: single non-ventilated, assembled, welded IP40",6025.47,"ΤΕΜ",1,"EP",1,"8MF60984E","Sivacon Πίνακες"]
["8MF6824-5R","Standard cabinet 8MF6 HxWxD=1800x 1200x 400 Installation: Side-by-side non-ventilated, assembled, welded IP54,",6446.61,"ΤΕΜ",1,"EP",1,"8MF68245R","Sivacon Πίνακες"]
["8MF6894-5R","Standard cabinet 8MF6 HxWxD=1800x 900x 400 Installation: Side-by-side non-ventilated, assembled, welded IP54,",5021.2299999999996,"ΤΕΜ",1,"EP",1,"8MF68945R","Sivacon Πίνακες"]
["8MF9242","8MF system cabinets Mounting plate HxW=1200x 900M for 8MF system cabinet",592.83000000000004,"ΤΕΜ",1,"EP",1,"8MF9242","Sivacon Πίνακες"]
["8MR2151-3A","PTC w. thermostat Wall mounting fan heater CS130 120 V AC, 1200 W",751.75,"ΤΕΜ",1,"EP",1,"8MR21513A","8MR εξαρτήματα πινάκων"]
["8MR2210-2B","Accessory LED lamp 025 AC connecting cable 16AWG w. socket, UL",72.12,"ΤΕΜ",1,"EP",1,"8MR22102B","8MR εξαρτήματα πινάκων"]
["8MR6402-2LV41","Filter fan, Extract: W: 223 mm, H: 223 mm, RAL 7032, IP54, Airflow: 250 m3/h, Ue DC: 24 V",763.2,"ΤΕΜ",1,"EP",1,"8MR64022LV41","8MR εξαρτήματα πινάκων"]
["8MR6511-6LV41","Filter fan, Extract: W: 223 mm, H: 223 mm, RAL 7035, IP55, EMC, Airflow: 230 m3/h, Ue AC: 115 V",988.34,"ΤΕΜ",1,"EP",1,"8MR65116LV41","8MR εξαρτήματα πινάκων"]
["8PQ1010-8BA01","SIVACON S4 base cover lateral H: 100mm D: 800mm",81.31,"ΤΕΜ",1,"EP",1,"8PQ10108BA01","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ2000-8BA06","SIVACON S4 cover 3NJ4, H: 800mm W: 800mm",193.52,"ΤΕΜ",1,"EP",1,"8PQ20008BA06","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ2010-8BA01","SIVACON S4 cover, H: 100mm W: 800mm",67.849999999999994,"ΤΕΜ",1,"EP",1,"8PQ20108BA01","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ2025-4BA04","SIVACON S4 IP55 upgrade H: 250mm W: 400mm",104.2,"ΤΕΜ",1,"EP",1,"8PQ20254BA04","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ2025-8BA04","SIVACON S4, mod door, IP40, H: 250mm, W: 800mm",172.28,"ΤΕΜ",1,"EP",1,"8PQ20258BA04","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ2035-6BA26","SIVACON S4 cover 3VA10 (100A), 3-pole, fixed-mounted, plug-in tech, H: 350mm W: 600mm",110.22,"ΤΕΜ",1,"EP",1,"8PQ20356BA26","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ2045-8BA11","SIVACON S4 cover 3VA20 (100A), 3VA21 (160A), 3VA22 (250A), 3-pole, fixed-mounted, plug-in tech, 8US setup, H: 450mm W: 800mm",192.34,"ΤΕΜ",1,"EP",1,"8PQ20458BA11","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ2055-1BA06","SIVACON S4 protect. upgr. degr. IP55, H: 550mm W: 1000mm",100.89,"ΤΕΜ",1,"EP",1,"8PQ20551BA06","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ2067-1BA02","SIVACON S4 protect. upgr. degr. IP55, H: 675mm W: 1000mm",133.34,"ΤΕΜ",1,"EP",1,"8PQ20671BA02","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ2197-1BA20","SIVACON S4 Giugiaro glass door, IP55, H: 2000 mm, W: 1000 mm, double-bit key, right",1044.3,"ΤΕΜ",1,"EP",1,"8PQ21971BA20","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ2300-4BA04","SIVACON S4 top plate IP55, W: 350mm D: 400mm",59.82,"ΤΕΜ",1,"EP",1,"8PQ23004BA04","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ2301-4BA07","SIVACON S4 top plate MBB: rear IPX1 W: 1000mm D: 400mm",210.04,"ΤΕΜ",1,"EP",1,"8PQ23014BA07","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ2304-6BA01","SIVACON S4 top plate IP55, W: 400mm D: 600mm",80.83,"ΤΕΜ",1,"EP",1,"8PQ23046BA01","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ2306-8BA08","SIVACON S4 top plate for cable entrance IP40 W: 600mm D: 800mm",810.66,"ΤΕΜ",1,"EP",1,"8PQ23068BA08","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ3000-0BA68","SIVACON S4 MBB separation, mounting position: top,W: 600mm D: 400mm",106.67,"ΤΕΜ",1,"EP",1,"8PQ30000BA68","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ3000-1BA32","SIVACON S4 MBB section division top, H: 1600 mm, D: 600 mm",117.29,"ΤΕΜ",1,"EP",1,"8PQ30001BA32","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ3000-3BA11","SIVACON S4 side uprights int. MBB bottom, H: 1600mm D: 800mm",204.14,"ΤΕΜ",1,"EP",1,"8PQ30003BA11","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ3000-3BA18","SIVACON S4 MBB separation bottom, W: 1000 mm D: 400mm",212.4,"ΤΕΜ",1,"EP",1,"8PQ30003BA18","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ4000-0BA53","SIVACON S4 connecting lugs MBB 20 x 10 mm, 1 set =4 units",332.76,"ΤΕΜ",1,"EP",1,"8PQ40000BA53","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ5000-2BA51","SIVACON S4 separation, rear W: 600mm H: 50mm",26.74,"ΤΕΜ",1,"EP",1,"8PQ50002BA51","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ5000-4BA02","SIVACON S4 separation 3WL FS II cable connection, 3/4-pole, W: 800mm, modular door",224.2,"ΤΕΜ",1,"EP",1,"8PQ50004BA02","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ5000-4BA75","SIVACON S4 basic module separation, rear H:=250mm W:=600mm",73.400000000000006,"ΤΕΜ",1,"EP",1,"8PQ50004BA75","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ5000-5BA32","SIVACON S4 separation rear 2 x ACB MBB: double W: 400mm D: 1200mm",571.12,"ΤΕΜ",1,"EP",1,"8PQ50005BA32","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ6000-5BA33","SIVACON S4 3WA MBB connection FS III (4.000 A), fixed-mount, withdraw, 3/4-pole, W: 1000mm",801.22,"ΤΕΜ",1,"EP",1,"8PQ60005BA33","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ6000-6BA52","SIVACON S4 DIN rail for modular door, W: 600mm",35.159999999999997,"ΤΕΜ",1,"EP",1,"8PQ60006BA52","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ6000-8BA38","SIVACON S4 mounting panel 3VA20 (100A), 3-pole, plug-in socket, 8US setup, H: 400mm W: 600mm",142.78,"ΤΕΜ",1,"EP",1,"8PQ60008BA38","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ6001-0BA81","SIVACON S4 3WA cable connection size II 3/4-pole W: 800mm",427.16,"ΤΕΜ",1,"EP",1,"8PQ60010BA81","Sivacon S4 υλικά - εξαρτήματα"]
["8PQ9400-1BA40","SIVACON S4 Quick release cover 1 Pack=50 Pieces",108.44,"ΤΕΜ",1,"EP",1,"8PQ94001BA40","Sivacon S4 υλικά - εξαρτήματα"]
["8UC6024","Spare part for rotary operating mechanism 8UC6 adapter for shaft 12 mm x 12 mm",42.85,"ΤΕΜ",1,"EP",1,"8UC6024","8UC εξαρτήματα για χειριστήρια"]
["8UD1141-3AF21","Door coupling operating mechanism Standard with tolerance compensation Size 100 x 100, Shaft 10x 10, 300 mm, Test-0-1 Complete unit Handle size 100 mm Accessory for 3KF size 3",89.25,"ΤΕΜ",1,"EP",1,"8UD11413AF21","8UD χειριστήρια για 3KC/3KD/3KF"]
["8UD1171-2AD15","Door-coupling rotary operating mechanism Emergency switching-off without tolerance compensation Size 75x 75, Shaft 8x 8, 300 mm, 0-I, Complete unit Handle size 45 mm Accessory for 3KD size 1 and 2, 3KF size 1",46.58,"ΤΕΜ",1,"EP",1,"8UD11712AD15","8UD χειριστήρια για 3KC/3KD/3KF"]
["8UD1851-3AE05","handle with masking plate EMERGENCY-STOP size 100x 100, for shaft 10x 10, I-0-II, handle size 140mm accessory for 3KC0 size 4",93.5,"ΤΕΜ",1,"EP",1,"8UD18513AE05","8UD χειριστήρια για 3KC/3KD/3KF"]
["8US1213-4AU01","Device adapter MCCB, 3-pole, 160 A Busbar center-to-center spacing 60 mm for 3VA10/11, 200 x 77 mm Contacting to the adapter is included in supply",193.95,"ΤΕΜ",1,"EP",1,"8US12134AU01","8US Busbar system"]
["8US1922-1AC00","Busbar system, accessories Busbar center-to-center spacing 60 mm End cover for busbar holder for 8US1923-3AA01 3-pole or for 8US1923-2AA01 3-pole",7.84,"ΤΕΜ",1,"EP",10,"8US19221AC00","8US Busbar system"]
["8US1998-1DA54","Positioning piece 54 mm Lockable mounting rail",6.41,"ΤΕΜ",1,"EP",10,"8US19981DA54","8US Busbar system"]
["8WA1822-7AX02","cover, for Link rails, horizontal and vertical, Terminal width: 6.2 mm, L: 100 mm, transparent, 16 mm2, 35 mm2",2.1,"ΤΕΜ",1,"EP",10,"8WA18227AX02","8WA εξαρτήματα κλεμμών"]
["8WA8847-1AH","inscription label, front, with Y, horizontal, terminal width: 5 mm, H: 7 mm, white",8.44,"ΤΕΜ",100,"EP",100,"8WA88471AH","8WA εξαρτήματα κλεμμών"]
["8WD4250-5BC","Flashlight element, with integrated LED, green, 230 V AC, Diameter 50 mm",124.49,"ΤΕΜ",1,"EP",1,"8WD42505BC","8WD Βιομηχανικοί Φανοί"]
["8WD4440-5AB","Continuous light element, with integrated LED, red, 115 V AC, Diameter 70 mm",97.63,"ΤΕΜ",1,"EP",1,"8WD44405AB","8WD Βιομηχανικοί Φανοί"]
["8WD4450-5BE","Flashlight element, with integrated LED, clear, 230 V AC, Diameter 70 mm",135.41,"ΤΕΜ",1,"EP",1,"8WD44505BE","8WD Βιομηχανικοί Φανοί"]
["8WH1000-6AG00","Isolating terminal with screw terminal Terminal size 4.0 mm2 Terminal width 6.2 mm Color black",2.67,"ΤΕΜ",1,"EP",50,"8WH10006AG00","8WH Κλέμμες"]
["8WH2000-0AF02","Through-type terminals with spring-loaded connection, Cross-section: 2.5 mm2, Width: 5.2mm, Color: red",1.02,"ΤΕΜ",1,"EP",50,"8WH20000AF02","8WH Κλέμμες"]
["8WH2003-0AE00","Through-type terminals with spring-loaded connection, 3 connection points, Cross-section: 0.14-1.5 mm2, Width: 4.2mm, Color: gray",1.1100000000000001,"ΤΕΜ",1,"EP",50,"8WH20030AE00","8WH Κλέμμες"]
["8WH2035-0AF00","Three-tier terminal 2.5 mm2; with 1 potential for the 3L; gray; Width 5.2 mm",6.57,"ΤΕΜ",1,"EP",50,"8WH20350AF00","8WH Κλέμμες"]
["8WH6000-0AF01","IPO terminals, Through-type terminals 2.5 mm2",1.22,"ΤΕΜ",1,"EP",50,"8WH60000AF01","8WH Κλέμμες"]
["8WH6004-6AF00","IPO terminals, Instrument isolating terminal",5.04,"ΤΕΜ",1,"EP",50,"8WH60046AF00","8WH Κλέμμες"]
["8WH8111-4AA05","Labeling plate, flat, horizontal und vertical, Terminal width: 8.2 mm, H: 6.4 mm, white",6.18,"ΤΕΜ",100,"EP",100,"8WH81114AA05","8WH Κλέμμες"]
["8WH8121-3AB45","Labeling plate, flat, with 41-50 vertical, Terminal width: 6.2 mm, H: 6.4 mm, white",8.8000000000000007,"ΤΕΜ",100,"EP",100,"8WH81213AB45","8WH Κλέμμες"]
["8WH8140-2AB15","Labeling plate, front, with 11-20, horizontal, Terminal width: 5.2 mm, H: 6.4 mm, white",9.35,"ΤΕΜ",100,"EP",100,"8WH81402AB15","8WH Κλέμμες"]
["8WH8141-2XA05","Labeling plate, flat, only with order code -Z (Y01) ! Special inscription, horizontal, Terminal width: 5.2 mm, H: 6.4 mm, white",22.6,"ΤΕΜ",100,"EP",100,"8WH81412XA05","8WH Κλέμμες"]
["8WH9003-2HA00","cover for through-type terminal with screw/spring loaded connection 4 connection points, Cross-section: 4 mm2, Width: 2.2mm, Color: gray",65.760000000000005,"ΤΕΜ",100,"EP",50,"8WH90032HA00","8WH Κλέμμες"]
["8WH9020-6EC10","Jumper plug 10 divisions, for cross links in the center of the terminal, 2-pole, Color: Siemens color",1.46,"ΤΕΜ",1,"EP",10,"8WH90206EC10","8WH Κλέμμες"]
["8WH9040-1AB07","plug-in coupling left element can be assembled by the user, with spring-loaded connection Cross-section: 0.08-2.5 mm2, Width: 5.2mm, Color: green-yellow",1.45,"ΤΕΜ",1,"EP",50,"8WH90401AB07","8WH Κλέμμες"]
["9AE4160-4BA00","CMS X-TOOLS ANALYSE LIBRARY V05.00; FLOATING LICENSE; SOFT- WARE; DOCUMENTATION AND LICENSE AS DOWNLOAD; CLASS A; LIBRARY FOR SELECTIV AND AUTOMATIC FREQUENCY MONITORING; ALARM BANDS; REFERENCE CURVE MONITORING; NOTIFICATIONS; ************ E-MAIL ADDRESS REQUIRED FOR DELIVERY",8735,"ΤΕΜ",1,"GMC",1,"9AE41604BA00","Ρυθμιστές στροφών και συστήματα Motion control"]
["9AE7111-0SH11-0BA0","PM-QUALITY V11, software DVD, upgrade package for system package type S, for upgrading from Professional without Data Center to Professional with Data Center SW incl. config. system, Single License, return of the dongle from initial delivery required, software ID number and dongle serial number for order must be specified. Only for subsequent orders.",3393,"ΤΕΜ",1,"SIMATIC",1,"9AE71110SH110BA0","Βιομηχανικός αυτοματισμός SIMATIC"]
["9AE7130-1CS01-1AA0","PI-CONNECT OPC+ INTERFACE OPC DA/HDA interface license for connection of OPC servers to OSISoft PI. license per multiproject and interface computer basic license delivery by email.",10097,"ΤΕΜ",1,"SIMATIC",1,"9AE71301CS011AA0","Βιομηχανικός αυτοματισμός SIMATIC"]
["A5E00102018","Electronics, 2-, 3-, 4-Leiter, no HART, no Ex, for SIPART PS2: 6DR53..-0N*",701,"ΤΕΜ",1,"PI1",1,"A5E00102018","Όργανα Μέτρησης Πεδίου"]
["A5E00826932","LOADCELL,Weighfeeder, 10KG, nickle plated, mild steel, metric",405,"ΤΕΜ",1,"PI1",1,"A5E00826932","Όργανα Μέτρησης Πεδίου"]
["A5E01151553","Kit,100MM (4\") horn extension 1.5\" process connection, LR250",580,"ΤΕΜ",1,"PI1",1,"A5E01151553","Όργανα Μέτρησης Πεδίου"]
["A5E01153424","SITRANS F M Accessory MAG 3100 Grounding ring Type Flat ring, DN 80 (3\"), ANSI B16.5 Class 300, in alloy C-276 2.4819, for all liners (PTFE max. 130 Â°C (266 Â°F)), 1 pc.",733,"ΤΕΜ",1,"PI4",1,"A5E01153424","Όργανα Μέτρησης Πεδίου"]
["A5E01191966","SITRANS F M Accessory MAG 3100 Grounding ring Type Flat ring, DN 250 (10\"), ANSI B16.5 Class 150, in stainless steel AISI 316 14.436,00 for all liners (PTFE max. 130 Â°C (266 Â°F)), 1 pc.",366,"ΤΕΜ",1,"PI4",1,"A5E01191966","Όργανα Μέτρησης Πεδίου"]
["A5E01191974","SITRANS F M Accessory MAG 3100 Grounding ring Type Flat ring, DN 150 (6\"), EN 1092-1 PN 16, in alloy C-276 2.4819, for all liners (PTFE max. 130 Â°C (266 Â°F)), 1 pc.",818,"ΤΕΜ",1,"PI4",1,"A5E01191974","Όργανα Μέτρησης Πεδίου"]
["A5E02055287","SITRANS F M Accessory MAG 1100F P gasket, DN 15 (1/2\"), rubber: EPDM, for PFA-lined sensors, 2 pcs.",48,"ΤΕΜ",1,"PI4",1,"A5E02055287","Όργανα Μέτρησης Πεδίου"]
["A5E02218310","SITRANS F M Accessory MAG 1100F Threaded type connection fitting (P-gaskets for EHEDG), DN 25, for sensor DN 25, SMS 1145, in stainless steel AISI 316L 1.4404, for PFA liner, 2 pcs.",717,"ΤΕΜ",1,"PI4",1,"A5E02218310","Όργανα Μέτρησης Πεδίου"]
["A5E02344540","Short instructions (leporello) for SITRANS P,P500 series in Chinese and English",12,"ΤΕΜ",1,"PI1",1,"A5E02344540","Όργανα Μέτρησης Πεδίου"]
["A5E02734568","FUE080 sparepart transmitter for FUE380 systems with custody transfer approval (7ME341). Type SITRANS FUE080 IP67 Polyamide, Supply: 3.6V Battery. Note: A custody transfer verification is not possible. Mandatory requirements: Complete MLFB and serial number of original unit",2098,"ΤΕΜ",1,"PI1",1,"A5E02734568","Όργανα Μέτρησης Πεδίου"]
["A5E02956319","7ML5431XXX201XCX,HART SU<3.6mA,M20 LR250 enclosure with board stack for HORN Antenna versions, M20 cable inlet, approval option C, with HART (<3.6mA start up) communication, no process connection",2759,"ΤΕΜ",1,"PI1",1,"A5E02956319","Όργανα Μέτρησης Πεδίου"]
["A5E03588171","LR250 Threaded PVDF Antenna version enclosure with board stack,  M20 cable inlet, approval option A, with PROFIBUS PA communication, no process connection",2383,"ΤΕΜ",1,"PI1",1,"A5E03588171","Όργανα Μέτρησης Πεδίου"]
["A5E03736896","FC430 Compact Operating Instructions En-Et-Lv-Lt-Pl-Ro",54,"ΤΕΜ",1,"PI1",1,"A5E03736896","Όργανα Μέτρησης Πεδίου"]
["A5E32462827","Kit,LR250,Encap,DN80PN16 B1 RF,FEA,Lens",563,"ΤΕΜ",1,"PI1",1,"A5E32462827","Όργανα Μέτρησης Πεδίου"]
["A5E32868055","Short instructions (leporello) for SITRANS P, DS III series in German, English, French, Spanish, Italian, Portuguese",7,"ΤΕΜ",1,"PI2",1,"A5E32868055","Όργανα Μέτρησης Πεδίου"]
["A5E32910815","Kit DN100 DIN11864-3 Form A tank connection,Clamp,EPDM Seal Class II",292,"ΤΕΜ",1,"PI1",1,"A5E32910815","Όργανα Μέτρησης Πεδίου"]
["A5E35817107","LVL200, Namur Spare Part Module",573,"ΤΕΜ",1,"PI1",1,"A5E35817107","Όργανα Μέτρησης Πεδίου"]
["A5E37673439","WW100 CAL CHAIN,SS,3 ST, CUSTOM EYELET Further details can be found on the corresponding budgetary estimate previously provided by the PVC to the region.  Please take special consideration of the revision number.",1191,"ΤΕΜ",1,"PI1",1,"A5E37673439","Όργανα Μέτρησης Πεδίου"]
["A5E38846901","Spare Lid Assembly",317,"ΤΕΜ",1,"PI1",1,"A5E38846901","Όργανα Μέτρησης Πεδίου"]
["A5E39669934032","10m(32.8') Standard, Submersible Coax sensor cable pair with No Transmitter Glands",406,"ΤΕΜ",1,"PI1",1,"A5E39669934032","Όργανα Μέτρησης Πεδίου"]
["A5E43226455","MASS6000 19\"/IP20 Ex, 3 current ; 24V, Spare part PCB main",2829,"ΤΕΜ",1,"PI1",1,"A5E43226455","Όργανα Μέτρησης Πεδίου"]
["A5E45863473","Sound absorber plastic, 10 pieces for SIPART PS2/PS100",239,"ΤΕΜ",1,"PI5",1,"A5E45863473","Όργανα Μέτρησης Πεδίου"]
["A5E50507516","Bracket for mounting SITRANS LR1XX Radar Process Mount: 1.5\" Offset: 200 mm (7.87 inch) Material: 316L SS",133,"ΤΕΜ",1,"PI1",1,"A5E50507516","Όργανα Μέτρησης Πεδίου"]
["A5E50668340006","Tail pulley for Weighfeeder SITRANS WW200 for 42\"/1067mm belt width, 160mm diameter plus 6mm NBR lagging, 40mm shaft, stainless steel 304 (1.4301), crowned",4705,"ΤΕΜ",1,"PI1",1,"A5E50668340006","Όργανα Μέτρησης Πεδίου"]
["A5E51251920","Electronics, 2-wire, Ex, coated for SIPART PS2: 6DR50..-0{E,G,D,F,K}* -Z K50 / Y99",886,"ΤΕΜ",1,"PI1",1,"A5E51251920","Όργανα Μέτρησης Πεδίου"]
["A5E52756003","Electronics 4 ... 20 mA, Ex, coated for SIPART PS2 6DR50.{0,1,2,3}-0{E,D,G,F,K,}* 6DR50.{5,6}-0{F,G,K,P}*",878,"ΤΕΜ",1,"PI1",1,"A5E52756003","Όργανα Μέτρησης Πεδίου"]
["C73451-A3000-B20","clamping elements for SIPART DR19/20/21/22/24 (order 2 units)",9,"ΤΕΜ",1,"PI1",2,"C73451A3000B20","Όργανα Μέτρησης Πεδίου"]
["C73451-A430-D80","Pneumatic block, single-acting including seal and screws for SIPART PS2 6DR5.1*",405,"ΤΕΜ",1,"PI5",1,"C73451A430D80","Όργανα Μέτρησης Πεδίου"]
["FDK:083F5061","Verification tool for Siemens MID flow meters. The SITRANS F M Verificator verifies installed flow meters that they still work within their specifications. The SITRANS F M Verificator requires a mandatory recalibration withone year interval to maintain the accuracy. SERVICE NOTE: Please order re-calibrations of Sitrans FM Verificator with MLFB 9LA1110-8QT10-0BA0-Z Y99! Note the serial number of the Verificator in the purchase order at Y99.",21173,"ΤΕΜ",1,"PI4",1,"FDK:083F5061","Όργανα Μέτρησης Πεδίου"]
["FDK:083G0687","SITRANS F M Accessory MAG 1100 Grounding ring Type Flat ring, DN 15 (1/2\"), EN 1092-1 PN 40, ANSI B16.5 Class 300, in stainless steel AISI 316/1.4436, for all liners, 1 pc.",120,"ΤΕΜ",1,"PI4",1,"FDK:083G0687","Όργανα Μέτρησης Πεδίου"]
["FDK:083G2206","SITRANS F M Accessory MAG 1100F Flat Gasket, DN 10 (3/8\"), rubber: EPDM, for ceramic- & PFA-lined sensors, 2 pcs.",65,"ΤΕΜ",1,"PI4",1,"FDK:083G2206","Όργανα Μέτρησης Πεδίου"]
["FDK:083H3001","10m cable - 105 degrees",163,"ΤΕΜ",1,"PI1",1,"FDK:083H3001","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8083","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type C, DN 350 (14\"), EN 1092-1 PN 6, ANSI B16.5 JIS K10, in stainless steel AISI 304 14.301,00 for all liners except PTFE & PFA, 1 pc.",339,"ΤΕΜ",1,"PI4",1,"FDK:083N8083","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8178","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type E, DN 500 (20\"), EN 1092-1 PN 10, ANSI B16.5 JIS K10, in stainless steel AISI 316 14.436,00 for PTFE liners, 1 pc.",3545,"ΤΕΜ",1,"PI4",1,"FDK:083N8178","Όργανα Μέτρησης Πεδίου"]
["FDK:083N8282","SITRANS F M Accessory MAG 3100 Grounding & protection ring Type E, DN 50 (2\"), EN 1092-1 PN 40, ANSI B16.5 JIS K20, in stainless steel AISI 316 14.436,00 for PTFE liners, 1 pc.",480,"ΤΕΜ",1,"PI4",1,"FDK:083N8282","Όργανα Μέτρησης Πεδίου"]
["FDK:085B5330","SONOKIT Angle measurement tool",7955,"ΤΕΜ",1,"PI1",1,"FDK:085B5330","Όργανα Μέτρησης Πεδίου"]
["FDK:085U1029","Mating part for hygienic clamp DN25 ISO2852",246,"ΤΕΜ",1,"PI4",1,"FDK:085U1029","Όργανα Μέτρησης Πεδίου"]
["FDK:085U1052","Terminalbox with lid, Polyamid, 1/2 NPT cable glands",173,"ΤΕΜ",1,"PI1",1,"FDK:085U1052","Όργανα Μέτρησης Πεδίου"]
["FDK:085U1053","Wall mounting unit, 4x 1/2 NPT cable glands",268,"ΤΕΜ",1,"PI4",1,"FDK:085U1053","Όργανα Μέτρησης Πεδίου"]
["FDK:085U1514","FRAME FOR INDICATING DEVICE, IP67, MKIII AND IV",23,"ΤΕΜ",1,"PI1",1,"FDK:085U1514","Όργανα Μέτρησης Πεδίου"]
["FDK:085U2374","MASS 6000 screws & sealing, Ex piedestal",95,"ΤΕΜ",1,"PI1",1,"FDK:085U2374","Όργανα Μέτρησης Πεδίου"]
["FDK:085U3122","MAG INDUSTRY ACC. DISPLAY",177,"ΤΕΜ",1,"PI1",1,"FDK:085U3122","Όργανα Μέτρησης Πεδίου"]
["FDK:085U3123","MAG 6000 I standard (non-Ex) 18...30 VDC; 115...230/24 VAC Spare PCBA unit (not for use with Ex sensors)",1191,"ΤΕΜ",1,"PI1",1,"FDK:085U3123","Όργανα Μέτρησης Πεδίου"]
["FDK:085U3144","MAG 6000I Accessory bag",55,"ΤΕΜ",1,"PI1",1,"FDK:085U3144","Όργανα Μέτρησης Πεδίου"]
["FDK:085X6329","SITRANS F US QN-0020052912 Transmitter FST030 for use with inline flowmeters Alu wallmount, epoxy coated NEMA 4X, IP66/67 24-230 V DC/AC Graphical display Non-Ex Water applications only HART, 4-20mA active/passive Ch2: Current/Freq./Pulse Ch3: Relay Cable glands kit",4521,"ΤΕΜ",1,"PI1",1,"FDK:085X6329","Όργανα Μέτρησης Πεδίου"]
["FDK:085X6366","SITRANS F US QN-0020055358 Transmitter FST030 for use with inline flowmeters Alu wallmount, epoxy coated NEMA 4X, IP66/67 24-230 V DC/AC Graphical display Non-Ex Water applications only MODBUS RTU RS485 Ch2: Current/Freq./Pulse Ch3: Relay Cable glands kit",4823,"ΤΕΜ",1,"PI1",1,"FDK:085X6366","Όργανα Μέτρησης Πεδίου"]
["FDK:087H3007","Sparepart SITRANS F US: Transducer spare part set for SITRANS FUS880 retrofit system, with 2 pcs. transducer.",443,"ΤΕΜ",1,"PI1",1,"FDK:087H3007","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4080","MAG8000 Accessories Demo and training package",2447,"ΤΕΜ",1,"PI7",1,"FDK:087L4080","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4142","Alkaline battery for  MAG 8000 demo transmitter  (3 V 13 Ah) (No dangerous goods limitations)",34,"ΤΕΜ",1,"PI1",1,"FDK:087L4142","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4150","SITRANS F M Accessory MAG 8000 Internal Battery with connector, 2 D-cell (3.6 V, 34 Ah), incl. accessories for replacement and NBR O-ring.",268,"ΤΕΜ",1,"PI7",1,"FDK:087L4150","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4151","MAG8000 Accessories, External Battery pack IP68/NEMA 6P with connector, 4 D-Cell (3.6 V 68 Ah) Without power cable.",376,"ΤΕΜ",1,"PI7",1,"FDK:087L4151","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4152","MAG8000 Accessories, Power cable, 1,5 m (4.9 ft) with IP68/NEMA 6P plugs for external battery. PE jacket, ambient temperature - 20 Cel. ... +60 Cel. (-4 ... +140 F)",155,"ΤΕΜ",1,"PI7",1,"FDK:087L4152","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4154","MAG8000 Accessories Cable entry M20 brass, one entry 2-5mm,10pcs.",199,"ΤΕΜ",1,"PI7",1,"FDK:087L4154","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4155","MAG8000 Accessories Cable entry M20 brass, one 6-8mm, 10pcs.",157,"ΤΕΜ",1,"PI7",1,"FDK:087L4155","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4156","MAG8000 Accessories Cable entry M20 brass, one 8-11mm,10pcs.",157,"ΤΕΜ",1,"PI7",1,"FDK:087L4156","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4157","MAG8000 Accessories Cable entry M20 brass, one 11-15mm,10pcs.",172,"ΤΕΜ",1,"PI7",1,"FDK:087L4157","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4158","MAG8000  Accessories Cable entry M20 brass, two entries 3.5-5mm,10pcs",210,"ΤΕΜ",1,"PI7",1,"FDK:087L4158","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4159","MAG8000 Accessories Cable entry M20brass, two 5.5-7.5mm,10pcs.",215,"ΤΕΜ",1,"PI7",1,"FDK:087L4159","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4162","MAG8000 Servicetool Kit",393,"ΤΕΜ",1,"PI1",1,"FDK:087L4162","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4163","MAG8000 Accessories USB Irda adapter",251,"ΤΕΜ",1,"PI7",1,"FDK:087L4163","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4165","MAG8000 Hardware Key",65,"ΤΕΜ",1,"PI7",1,"FDK:087L4165","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4166","MAG8000 Transmitter Compact replacement kit. No battery included. Mandatory requirements: Complete MLFB and serial number of original unit and Not programmed version FDK-087L4203",1449,"ΤΕΜ",1,"PI1",1,"FDK:087L4166","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4167","MAG 8000 Accessories Enclosure top including plastic lid, screws and blank product label.",443,"ΤΕΜ",1,"PI7",1,"FDK:087L4167","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4168","MAG 8000 (Advanced version) transmitter PCB replacement kit. No system number required.",1432,"ΤΕΜ",1,"PI1",1,"FDK:087L4168","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4196","MAG8000 Accessories Cable entry M20 brass, one 6-8mm,1pcs",31,"ΤΕΜ",1,"PI7",1,"FDK:087L4196","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4202","MAG8000 Transmitter Remote replacement kit Mandatory requirements: Complete MLFB and serial number of original unit and Not programmed version FDK-087L4204",1803,"ΤΕΜ",1,"PI1",1,"FDK:087L4202","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4203","MAG8000 (Advanced Version) transmitter compact replacement kit. No battery included. No system number required.",1509,"ΤΕΜ",1,"PI1",1,"FDK:087L4203","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4204","MAG8000 (Advanced version) Transmitter remote replacement kit No battery included. No system number required.",1847,"ΤΕΜ",1,"PI1",1,"FDK:087L4204","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4210","SITRANS FM Accessory  MAG 8000 Mains power supply  12...24 V AC/DC with battery  backup and 3 m (9.8 ft)  power cable for external  connection (no battery  included)",624,"ΤΕΜ",1,"PI7",1,"FDK:087L4210","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4211","SITRANS FM Accessory  MAG 8000 Mains power supply  115 ... 230 VAC with battery  backup up and 3 m (9.8 ft)  power cable for external  connection (no battery  included)",619,"ΤΕΜ",1,"PI7",1,"FDK:087L4211","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4212","SITRANS FM Accessory  MAG 8000 RS 232 add-on module  point to point communication  interface with Modbus  RTU protocol",427,"ΤΕΜ",1,"PI7",1,"FDK:087L4212","Όργανα Μέτρησης Πεδίου"]
["FDK:087L4213","SITRANS FM Accessory  MAG 8000 RS485 add-on module  multidrop communication  interface with Modbus RTU  protocol",427,"ΤΕΜ",1,"PI7",1,"FDK:087L4213","Όργανα Μέτρησης Πεδίου"]
["FDK:087L6001","MAG8000 Accessories Flow Tool Configuration Software CD",259,"ΤΕΜ",1,"PI7",1,"FDK:087L6001","Όργανα Μέτρησης Πεδίου"]
["FDK:521H0552","LITERATURE - SFIDKPS029V201 ISSUER OF LITERATURE : SIEMENS FLOW INSTRUMENTS A/S DENMARK LITERATURE CATEGORY : PRINT/PAPER LITERATURE SUBCATEGORY : HANDBOOKS MAIN PRODUCT GROUP : SONO ISSUE : V VERSION : 2 LANGUAGE CODE : DANISH",13,"ΤΕΜ",1,"PI1",1,"FDK:521H0552","Όργανα Μέτρησης Πεδίου"]
["FDK:521H0553","LITERATURE - SFIDKPS029V202 ISSUER OF LITERATURE : SIEMENS FLOW INSTRUMENTS A/S DENMARK LITERATURE CATEGORY : PRINT/PAPER LITERATURE SUBCATEGORY : HANDBOOKS MAIN PRODUCT GROUP : SONO ISSUE : V VERSION : 2 LANGUAGE CODE : ENGLISH",13,"ΤΕΜ",1,"PI1",1,"FDK:521H0553","Όργανα Μέτρησης Πεδίου"]
["FDK:521H1189","Literature - SFIDKPS023C102 Issuer of literature : Siemens Flow Instruments A/S Denmark Literature category : Print/paper Literature subcategory : Handbooks Main product group : USM Issue : C Version : 1 Language code : English",7,"ΤΕΜ",1,"PI1",1,"FDK:521H1189","Όργανα Μέτρησης Πεδίου"]
["H62217-B2506-Z1","SREW FOR THE FIXING OF THE FRONTMODULE DR22/24 \"NEW\" (5 PIECES REQUESTED)",2,"ΤΕΜ",1,"PI1",10,"H62217B2506Z1","Όργανα Μέτρησης Πεδίου"]
["JJY:023146720008","Fa. Heine Breaking resistor FOR POWERMODULE FSA P_MAX=750W/12S/5% ED R=200 OHM P_DAUER=37,5W",120,"ΤΕΜ",1,"GMC",1,"JJY:023146720008","Ρυθμιστές στροφών και συστήματα Motion control"]
["JJY:023151720007","Fa. Heine Breaking resistor FOR POWERMODULE FSB P_MAX=2200W/12S/5% ED R=68 OHM P_DAUER=110W",166,"ΤΕΜ",1,"GMC",1,"JJY:023151720007","Ρυθμιστές στροφών και συστήματα Motion control"]
["JJY:023163720018","Fa. Heine Breaking resistor FOR POWERMODULE FSC1 P_MAX=4000W/12S/5% ED R=37 OHM P_DAUER=200W",231,"ΤΕΜ",1,"GMC",1,"JJY:023163720018","Ρυθμιστές στροφών και συστήματα Motion control"]
["JJY:023422620001","Fa. Heine Breaking resistor FOR POWERMODULE PM240-2 FSD P_MAX=22kW/12S/5% ED R=25 OHM P_DAUER=1100W",645,"ΤΕΜ",1,"GMC",1,"JJY:023422620001","Ρυθμιστές στροφών και συστήματα Motion control"]
["JJY:023422620002","Fa. Heine Breaking resistor FOR POWERMODULE PM240-2 FSD P_MAX=18,5kW/12S/5% ED R=7,5 OHM P_DAUER=930W",737,"ΤΕΜ",1,"GMC",1,"JJY:023422620002","Ρυθμιστές στροφών και συστήματα Motion control"]
["JJY:023423320001","Fa. Heine Breaking resistor FOR POWERMODULE PM240-2 FSE P_MAX=30kW/12S/5% ED R=4,5 OHM P_DAUER=1500W",1013,"ΤΕΜ",1,"GMC",1,"JJY:023423320001","Ρυθμιστές στροφών και συστήματα Motion control"]
["JJY:023424020001","Fa. Heine Breaking resistor FOR POWERMODULE PM240-2 FSD P_MAX=37kW/12S/5% ED R=15 OHM P_DAUER=1850W",921,"ΤΕΜ",1,"GMC",1,"JJY:023424020001","Ρυθμιστές στροφών και συστήματα Motion control"]
["JJY:023424020002","Fa. Heine Breaking resistor FOR POWERMODULE PM240-2 FSD P_MAX=37kW/12S/5% ED R=31 OHM P_DAUER=1850W",1059,"ΤΕΜ",1,"GMC",1,"JJY:023424020002","Ρυθμιστές στροφών και συστήματα Motion control"]
["JJY:023433720001","Heine company braking resistor for power module FSC2 P_max=7500 W/12 s/5% on-load factor R=20 Ohm P_duration=375 W",341,"ΤΕΜ",1,"GMC",1,"JJY:023433720001","Ρυθμιστές στροφών και συστήματα Motion control"]
["JJY:023434020001","Fa. Heine Breaking resistor FOR POWERMODULE PM240-2 FSE P_MAX=55kW/12S/5% ED R=10 OHM P_DAUER=2750W",1381,"ΤΕΜ",1,"GMC",1,"JJY:023434020001","Ρυθμιστές στροφών και συστήματα Motion control"]
["JJY:023434020002","Fa. Heine Breaking resistor FOR POWERMODULE PM240-2 FSE P_MAX=55kW/12S/5% ED R=21 OHM P_DAUER=2750W",1693,"ΤΕΜ",1,"GMC",1,"JJY:023434020002","Ρυθμιστές στροφών και συστήματα Motion control"]
["JJY:023434020003","Fa. Heine Breaking resistor FOR POWERMODULE PM240-2 FSF P_MAX=55kW/12S/5% ED R=2,5 OHM P_DAUER=2750W",1657,"ΤΕΜ",1,"GMC",1,"JJY:023434020003","Ρυθμιστές στροφών και συστήματα Motion control"]
["JJY:023454020001","Fa. Heine Breaking resistor FOR POWERMODULE PM240-2 FSF P_MAX=77kW/12S/5% ED R=7,1 OHM P_DAUER=3850W This braking resistor consists of the 2 braking resistors: JJY:023422620001 and JJY:023434020001, which must be connected in parallel on plant.",2097,"ΤΕΜ",1,"GMC",1,"JJY:023454020001","Ρυθμιστές στροφών και συστήματα Motion control"]
["JJY:023464020001","Fa. Heine Breaking resistor FOR POWERMODULE PM240-2 FSF P_MAX=110kW/12S/5% ED R=5 OHM P_DAUER=5500W This braking resistor consists of 2x JJY:023434020001 braking resistors, which must be connected in parallel on the plant",2833,"ΤΕΜ",1,"GMC",1,"JJY:023464020001","Ρυθμιστές στροφών και συστήματα Motion control"]
["JJY:023464020002","Fa. Heine Breaking resistor FOR POWERMODULE PM240-2 FSF P_MAX=110kW/12S/5% ED R=10,5 OHM P_DAUER=5500W This braking resistor consists of 2x JJY:023434020002 braking resistors, which must be connected in parallel on plant.",3459,"ΤΕΜ",1,"GMC",1,"JJY:023464020002","Ρυθμιστές στροφών και συστήματα Motion control"]
["KRH:16000100","Sparepart SITRANS FXT030 Electronic for SITRANS FX330 non-Ex/Ex-i in compact design with HART",3827,"ΤΕΜ",1,"PI1",1,"KRH:16000100","Όργανα Μέτρησης Πεδίου"]
["KRH:16000300","Cover gasket O-ring",56,"ΤΕΜ",1,"PI1",1,"KRH:16000300","Όργανα Μέτρησης Πεδίου"]
["KRH:16000400","Converter housing gasket 59,35,5-2-N",62,"ΤΕΜ",1,"PI1",1,"KRH:16000400","Όργανα Μέτρησης Πεδίου"]
["KRH:16000500","Cable feed through, 10 pole (non Ex)",461,"ΤΕΜ",1,"PI1",1,"KRH:16000500","Όργανα Μέτρησης Πεδίου"]
["KRH:16002000","Front Cover (non Ex)",312,"ΤΕΜ",1,"PI1",1,"KRH:16002000","Όργανα Μέτρησης Πεδίου"]
["KRH:16002500","Front Cover (Ex)",749,"ΤΕΜ",1,"PI1",1,"KRH:16002500","Όργανα Μέτρησης Πεδίου"]
["KRH:16003000","Back Cover",159,"ΤΕΜ",1,"PI1",1,"KRH:16003000","Όργανα Μέτρησης Πεδίου"]
["KRH:16111100","Sparepart SITRANS FXS300 Sensor replacement kit DN15 including seal disc, socket, pickup and O-rings (for pickup and pressure screw)",2121,"ΤΕΜ",1,"PI1",1,"KRH:16111100","Όργανα Μέτρησης Πεδίου"]
["KRH:16111110","Sparepart SITRANS FXS300 Sensor replacement kit DN15 Conical including seal disc, socket, pickup and O-rings (for pickup and pressure screw)",2121,"ΤΕΜ",1,"PI1",1,"KRH:16111110","Όργανα Μέτρησης Πεδίου"]
["KRH:16111150","Sparepart SITRANS FXS300 Sensor replacement kit DN25 including seal disc, socket, pickup and O-rings (for pickup and pressure screw)",2121,"ΤΕΜ",1,"PI1",1,"KRH:16111150","Όργανα Μέτρησης Πεδίου"]
["KRH:16111160","Sparepart SITRANS FXS300 Sensor replacement kit DN25 Conical including seal disc, socket, pickup and O-rings (for pickup and pressure screw)",2121,"ΤΕΜ",1,"PI1",1,"KRH:16111160","Όργανα Μέτρησης Πεδίου"]
["KRH:16111200","Sparepart SITRANS FXS300 Sensor replacement kit DN40 including seal disc, socket, pickup and O-rings (for pickup and pressure screw)",2121,"ΤΕΜ",1,"PI1",1,"KRH:16111200","Όργανα Μέτρησης Πεδίου"]
["KRH:16111210","Sparepart SITRANS FXS300 Sensor replacement kit DN50 including seal disc, socket, pickup and O-rings (for pickup and pressure screw)",2121,"ΤΕΜ",1,"PI1",1,"KRH:16111210","Όργανα Μέτρησης Πεδίου"]
["KRH:16111220","Sparepart SITRANS FXS300 Sensor replacement kit DN80 including seal disc, socket, pickup and O-rings (for pickup and pressure screw)",2121,"ΤΕΜ",1,"PI1",1,"KRH:16111220","Όργανα Μέτρησης Πεδίου"]
["KRH:16111230","Sparepart SITRANS FXS300 Sensor replacement kit DN100 including seal disc, socket, pickup and O-rings (for pickup and pressure screw)",2121,"ΤΕΜ",1,"PI1",1,"KRH:16111230","Όργανα Μέτρησης Πεδίου"]
["KRH:16111300","Sparepart SITRANS FXS300 Sensor replacement kit DN150-300 including seal disc, socket, pickup and O-rings (for pickup and pressure screw)",2121,"ΤΕΜ",1,"PI1",1,"KRH:16111300","Όργανα Μέτρησης Πεδίου"]
["KRH:16111350","Sparepart SITRANS FX330 Pressure sensor replacement kit 1 bar, including pressure sensor 1 bar with calibration certificate,DUBOX plug and 2x O-ring DIN 3771-20x1-FPM",2368,"ΤΕΜ",1,"PI1",1,"KRH:16111350","Όργανα Μέτρησης Πεδίου"]
["KRH:16111370","Sparepart SITRANS FX330 Pressure sensor replacement kit 2 bar, including pressure sensor 2 bar with calibration certificate,DUBOX plug and 2x O-ring DIN 3771-20x1-FPM",2368,"ΤΕΜ",1,"PI1",1,"KRH:16111370","Όργανα Μέτρησης Πεδίου"]
["KRH:16111400","Sparepart SITRANS FX330 Pressure sensor replacement kit 4 bar, including pressure sensor 4 bar with calibration certificate,DUBOX plug and 2x O-ring DIN 3771-20x1-FPM",2368,"ΤΕΜ",1,"PI1",1,"KRH:16111400","Όργανα Μέτρησης Πεδίου"]
["KRH:16111401","Sparepart SITRANS FX330 Pressure sensor replacement kit 6 bar, including pressure sensor 6 bar with calibration certificate,DUBOX plug and 2x O-ring DIN 3771-20x1-FPM",2368,"ΤΕΜ",1,"PI1",1,"KRH:16111401","Όργανα Μέτρησης Πεδίου"]
["KRH:16111402","Sparepart SITRANS FX330 Pressure sensor replacement kit 10 bar, including pressure sensor 10 bar with calibration certificate,DUBOX plug and 2x O-ring DIN 3771-20x1-FPM",2368,"ΤΕΜ",1,"PI1",1,"KRH:16111402","Όργανα Μέτρησης Πεδίου"]
["KRH:16111403","Sparepart SITRANS FX330 Pressure sensor replacement kit 16 bar, including pressure sensor 16 bar with calibration certificate,DUBOX plug and 2x O-ring DIN 3771-20x1-FPM",2368,"ΤΕΜ",1,"PI1",1,"KRH:16111403","Όργανα Μέτρησης Πεδίου"]
["KRH:16111404","Sparepart SITRANS FX330 Pressure sensor replacement kit 25 bar, including pressure sensor 25 bar with calibration certificate,DUBOX plug and 2x O-ring DIN 3771-20x1-FPM",2368,"ΤΕΜ",1,"PI1",1,"KRH:16111404","Όργανα Μέτρησης Πεδίου"]
["KRH:16111405","Sparepart SITRANS FX330 Pressure sensor replacement kit 40 bar, including pressure sensor 40 bar with calibration certificate,DUBOX plug and 2x O-ring DIN 3771-20x1-FPM",2368,"ΤΕΜ",1,"PI1",1,"KRH:16111405","Όργανα Μέτρησης Πεδίου"]
["KRH:16111406","Sparepart SITRANS FX330 Pressure sensor replacement kit 60 bar, including pressure sensor 60 bar with calibration certificate,DUBOX plug and 2x O-ring DIN 3771-20x1-FPM",2368,"ΤΕΜ",1,"PI1",1,"KRH:16111406","Όργανα Μέτρησης Πεδίου"]
["KRH:16111407","Sparepart SITRANS FX330 Pressure sensor replacement kit 100 bar, including pressure sensor 100 bar with calibration certificate,DUBOX plug and 2x O-ring DIN 3771-20x1-FPM",2368,"ΤΕΜ",1,"PI1",1,"KRH:16111407","Όργανα Μέτρησης Πεδίου"]
["KRH:16112000","Converter housing for compact or remote version with front and back cover Aluminium Type Plate attached to housing Non Ex/Ex-i Cable gland: 1pc. M20 x 1,5 (plastic-grey),2pc. Blind plug",1469,"ΤΕΜ",1,"PI1",1,"KRH:16112000","Όργανα Μέτρησης Πεδίου"]
["KRH:16112002","Wall housing incl. Neck (incl. Screws, Gaskets and cable glands)",1079,"ΤΕΜ",1,"PI1",1,"KRH:16112002","Όργανα Μέτρησης Πεδίου"]
["KRH:17000700","Seal disc 21,8-12-0,1",62,"ΤΕΜ",1,"PI1",1,"KRH:17000700","Όργανα Μέτρησης Πεδίου"]
["KRH:17000800","SITRANS FX300 DUBOX plug , 5-pole-ger-RM2",8,"ΤΕΜ",1,"PI1",1,"KRH:17000800","Όργανα Μέτρησης Πεδίου"]
["KRH:17001000","O-Ring 10x2-NBR",12,"ΤΕΜ",1,"PI1",1,"KRH:17001000","Όργανα Μέτρησης Πεδίου"]
["KRH:17001100","O-Ring DIN 3771-20x1-FPM",6,"ΤΕΜ",1,"PI1",1,"KRH:17001100","Όργανα Μέτρησης Πεδίου"]
["KRH:17001200","O-ring for pressure screw 17,13x2,62-FPM-70",8,"ΤΕΜ",1,"PI1",1,"KRH:17001200","Όργανα Μέτρησης Πεδίου"]
["KRH:17001400","O-ring pickup",6,"ΤΕΜ",1,"PI1",1,"KRH:17001400","Όργανα Μέτρησης Πεδίου"]
["KRH:17004000","Shut-off valve",2003,"ΤΕΜ",1,"PI1",1,"KRH:17004000","Όργανα Μέτρησης Πεδίου"]
["KRH:17006000","Centering rings for Sandwich-Version, DN15",68,"ΤΕΜ",1,"PI1",1,"KRH:17006000","Όργανα Μέτρησης Πεδίου"]
["KRH:17006001","Centering rings for Sandwich-Version, DN25",120,"ΤΕΜ",1,"PI1",1,"KRH:17006001","Όργανα Μέτρησης Πεδίου"]
["KRH:17006002","Centering rings for Sandwich-Version, DN40",139,"ΤΕΜ",1,"PI1",1,"KRH:17006002","Όργανα Μέτρησης Πεδίου"]
["KRH:17006003","Centering rings for Sandwich-Version, DN50",152,"ΤΕΜ",1,"PI1",1,"KRH:17006003","Όργανα Μέτρησης Πεδίου"]
["KRH:17006004","Centering rings for Sandwich-Version, DN50 (300lbs, 600lbs)",167,"ΤΕΜ",1,"PI1",1,"KRH:17006004","Όργανα Μέτρησης Πεδίου"]
["KRH:17006005","Centering rings forSandwich-Version, DN50 (JIS 10K, 16K, 20K)",240,"ΤΕΜ",1,"PI1",1,"KRH:17006005","Όργανα Μέτρησης Πεδίου"]
["KRH:17006006","Centering rings for Sandwich-Version, DN80",220,"ΤΕΜ",1,"PI1",1,"KRH:17006006","Όργανα Μέτρησης Πεδίου"]
["KRH:17006007","Centering rings for Sandwich-Version, DN100",431,"ΤΕΜ",1,"PI1",1,"KRH:17006007","Όργανα Μέτρησης Πεδίου"]
["KRH:TAGPLATE120X46","TAG name plate in stainless steel SITRANS FX330, 120 x 46 mm (Add plain text to order)",77,"ΤΕΜ",1,"PI1",1,"KRH:TAGPLATE120X46","Όργανα Μέτρησης Πεδίου"]
["KRH:TAGPLATE40X20","TAG name plate in stainless steel SITRANS FX330, 40 x 20 mm (Add plain text to order)",52,"ΤΕΜ",1,"PI1",1,"KRH:TAGPLATE40X20","Όργανα Μέτρησης Πεδίου"]
["LZS:PT17021","Fixing/reject bracket for plug-in relay RT series and PT screw terminals logical and PT spring-loaded terminal socket logical disconnection",41.3,"ΤΕΜ",100,"EP",10,"LZS:PT17021","LZS Μίνι Ρελέ"]
["LZS:PT17024","Fixing/reject bracket for plug-in relay RT series and PT screw terminal base not logical",41.84,"ΤΕΜ",100,"EP",10,"LZS:PT17024","LZS Μίνι Ρελέ"]
["LZS:PT17040","Labeling plate 26 mm for PT relay",29.67,"ΤΕΜ",100,"EP",10,"LZS:PT17040","LZS Μίνι Ρελέ"]
["LZS:PT170P1","fanning strip 2-pole for PT push-in terminal sockets",1.4,"ΤΕΜ",1,"EP",10,"LZS:PT170P1","LZS Μίνι Ρελέ"]
["LZS:PT170R6","Fanning strip 6-pole for PT screw-type terminal",8.06,"ΤΕΜ",1,"EP",10,"LZS:PT170R6","LZS Μίνι Ρελέ"]
["LZS:PT2D5L24","Plug-in relay complete unit 2 W, 24 V DC LED module red Socket with logic isolation Spring-type terminal (push-in)",24.56,"ΤΕΜ",1,"EP",5,"LZS:PT2D5L24","LZS Μίνι Ρελέ"]
["LZS:PT2D5T30","Plug-in relay complete unit 2 W, 230 V AC LED module red Socket with logic isolation Spring-type terminal (push-in)",28.26,"ΤΕΜ",1,"EP",5,"LZS:PT2D5T30","LZS Μίνι Ρελέ"]
["LZS:PT3A5L24","Plug-in relay complete unit 3 W, 24 V DC LED module red Standard plug-in socket screw terminal 3.5 mm pinning",20.54,"ΤΕΜ",1,"EP",5,"LZS:PT3A5L24","LZS Μίνι Ρελέ"]
["LZS:PT3A5R24","Plug-in relay complete unit 3 W, 24 V AC LED module red Standard plug-in socket screw terminal 3.5 mm pinning",20.54,"ΤΕΜ",1,"EP",5,"LZS:PT3A5R24","LZS Μίνι Ρελέ"]
["LZS:PT3A5S15","Plug-in relay complete unit 3 W, 115 V AC LED module red Standard plug-in socket screw terminal 3.5 mm pinning",21.84,"ΤΕΜ",1,"EP",5,"LZS:PT3A5S15","LZS Μίνι Ρελέ"]
["LZS:PT3A5T30","Plug-in relay complete unit 3 W, 230 V AC LED module red Standard plug-in socket screw terminal 3.5 mm pinning",21.84,"ΤΕΜ",1,"EP",5,"LZS:PT3A5T30","LZS Μίνι Ρελέ"]
["LZS:PT5A5L24","Plug-in relay complete unit 4 W, 24 V DC LED module red Standard plug-in socket screw terminal 3.5 mm pinning",20.54,"ΤΕΜ",1,"EP",5,"LZS:PT5A5L24","LZS Μίνι Ρελέ"]
["LZS:PT5A5R24","Plug-in relay complete unit 4 W, 24 V AC LED module red Standard plug-in socket screw terminal 3.5 mm pinning",20.54,"ΤΕΜ",1,"EP",5,"LZS:PT5A5R24","LZS Μίνι Ρελέ"]
["LZS:PT5A5S15","Plug-in relay complete unit 4 W, 115 V AC LED module red Standard plug-in socket screw terminal 3.5 mm pinning",21.84,"ΤΕΜ",1,"EP",5,"LZS:PT5A5S15","LZS Μίνι Ρελέ"]
["LZS:PT5A5T30","Plug-in relay complete unit 4 W, 230 V AC LED module red Standard plug-in socket screw terminal 3.5 mm pinning",21.84,"ΤΕΜ",1,"EP",5,"LZS:PT5A5T30","LZS Μίνι Ρελέ"]
["LZS:PT5B5L24","Plug-in relay complete unit 4 W, 24 V DC LED module red Socket with logic isolation screw terminal 3.5 mm pinning",20.54,"ΤΕΜ",1,"EP",5,"LZS:PT5B5L24","LZS Μίνι Ρελέ"]
["LZS:PT5B5R24","Plug-in relay complete unit 4 W, 24 V AC LED module red Socket with logic isolation screw terminal 3.5 mm pinning",20.54,"ΤΕΜ",1,"EP",5,"LZS:PT5B5R24","LZS Μίνι Ρελέ"]
["LZS:PT5B5S15","Plug-in relay complete unit 4 W, 115 V AC LED module red Socket with logic isolation screw terminal 3.5 mm pinning",21.84,"ΤΕΜ",1,"EP",5,"LZS:PT5B5S15","LZS Μίνι Ρελέ"]
["LZS:PT5B5T30","Plug-in relay complete unit 4 W, 230 V AC LED module red Socket with logic isolation screw terminal 3.5 mm pinning",21.84,"ΤΕΜ",1,"EP",5,"LZS:PT5B5T30","LZS Μίνι Ρελέ"]
["LZS:PT5B7L24-A","Plug-in relay complete unit 4 W, 24 V DC LED module green Socket with logic isolation screw terminal 3.5 mm pinning",19.12,"ΤΕΜ",1,"EP",1,"LZS:PT5B7L24A","LZS Μίνι Ρελέ"]
["LZS:PT5D5L24","Plug-in relay complete unit 4 W, 24 V DC LED module red Socket with logic isolation Spring-type terminal (push-in)",21.3,"ΤΕΜ",1,"EP",5,"LZS:PT5D5L24","LZS Μίνι Ρελέ"]
["LZS:PT5D5R24","Plug-in relay complete unit 4 W, 24 V AC LED module red Socket with logic isolation Spring-type terminal (push-in)",21.3,"ΤΕΜ",1,"EP",5,"LZS:PT5D5R24","LZS Μίνι Ρελέ"]
["LZS:PT5D5S15","Plug-in relay complete unit 4 W, 115 V AC LED module red Socket with logic isolation Spring-type terminal (push-in)",22.82,"ΤΕΜ",1,"EP",5,"LZS:PT5D5S15","LZS Μίνι Ρελέ"]
["LZS:PT5D5T30","Plug-in relay complete unit 4 W, 230 V AC LED module red Socket with logic isolation Spring-type terminal (push-in)",22.82,"ΤΕΜ",1,"EP",5,"LZS:PT5D5T30","LZS Μίνι Ρελέ"]
["LZS:PT78720","Plug-in socket for PT relay 2 change-over contacts screw terminal",5.76,"ΤΕΜ",1,"EP",1,"LZS:PT78720","LZS Μίνι Ρελέ"]
["LZS:PT78722","Plug-in socket for PT relay 2 change-over contacts with logic isolation screw terminal",5.76,"ΤΕΜ",1,"EP",1,"LZS:PT78722","LZS Μίνι Ρελέ"]
["LZS:PT7872P","Plug-in socket for PT relay 2 change-over contacts with logic isolation Spring-type terminal (push-in)",6.35,"ΤΕΜ",1,"EP",1,"LZS:PT7872P","LZS Μίνι Ρελέ"]
["LZS:PT78730","Plug-in socket for PT relay 3 changeover contacts screw terminal",5.76,"ΤΕΜ",1,"EP",1,"LZS:PT78730","LZS Μίνι Ρελέ"]
["LZS:PT78740","Plug-in socket for PT relay 4 changeover contacts screw terminal",5.76,"ΤΕΜ",1,"EP",1,"LZS:PT78740","LZS Μίνι Ρελέ"]
["LZS:PT78742","Plug-in socket for PT relay 4 changeover contacts with logic isolation screw terminal",5.76,"ΤΕΜ",1,"EP",1,"LZS:PT78742","LZS Μίνι Ρελέ"]
["LZS:PT7874P","Plug-in socket for PT relay 4 changeover contacts with logic isolation Spring-type terminal (push-in)",6.92,"ΤΕΜ",1,"EP",1,"LZS:PT7874P","LZS Μίνι Ρελέ"]
["LZS:PTMG0024","LED module, green, 24 V DC",4.03,"ΤΕΜ",1,"EP",1,"LZS:PTMG0024","LZS Μίνι Ρελέ"]
["LZS:PTMG0524","LED module green without freewheeling diode 24 V AC/DC",4.03,"ΤΕΜ",1,"EP",1,"LZS:PTMG0524","LZS Μίνι Ρελέ"]
["LZS:PTMG0730","LED module, green, 110-230 V AC",4.03,"ΤΕΜ",1,"EP",1,"LZS:PTMG0730","LZS Μίνι Ρελέ"]
["LZS:PTML0024","LED module, red for plug-in relay, PT and RT series, for DC 24 V with freewheeling diode",3.82,"ΤΕΜ",1,"EP",1,"LZS:PTML0024","LZS Μίνι Ρελέ"]
["LZS:PTML0524","LED module, red for plug-in relay, PT and RT series, for 24 V AC/DC without freewheeling diode",3.82,"ΤΕΜ",1,"EP",1,"LZS:PTML0524","LZS Μίνι Ρελέ"]
["LZS:PTML0730","LED module, red for plug-in relay, PT and RT series, 110-230 V AC without freewheeling diode",3.82,"ΤΕΜ",1,"EP",1,"LZS:PTML0730","LZS Μίνι Ρελέ"]
["LZS:PTMT00A0","Freewheeling diode with connection to A1 6-230 V DC",2.57,"ΤΕΜ",1,"EP",1,"LZS:PTMT00A0","LZS Μίνι Ρελέ"]
["LZS:PTMU0524","RC element, 24-48 V AC",6.07,"ΤΕΜ",1,"EP",1,"LZS:PTMU0524","LZS Μίνι Ρελέ"]
["LZS:PTMU0730","RC element, 110-230 V AC",6.07,"ΤΕΜ",1,"EP",1,"LZS:PTMU0730","LZS Μίνι Ρελέ"]
["LZS:RT17016","Fixing/reject bracket for plug-in relay RT series",68.91,"ΤΕΜ",100,"EP",10,"LZS:RT17016","LZS Μίνι Ρελέ"]
["LZS:RT17040","Label 15 mm for RT and RY relay",25,"ΤΕΜ",100,"EP",10,"LZS:RT17040","LZS Μίνι Ρελέ"]
["LZS:RT170P1","fanning strip 2-pole for RT push-in terminal sockets",104.98,"ΤΕΜ",100,"EP",10,"LZS:RT170P1","LZS Μίνι Ρελέ"]
["LZS:RT170R8","Fanning strip 8-pole for RT screw-type terminal",7.48,"ΤΕΜ",1,"EP",10,"LZS:RT170R8","LZS Μίνι Ρελέ"]
["LZS:RT3A4L24","Plug-in relay complete unit 1 W, 24 V DC LED module red Standard plug-in socket screw terminal",20.87,"ΤΕΜ",1,"EP",5,"LZS:RT3A4L24","LZS Μίνι Ρελέ"]
["LZS:RT3A4R24","Plug-in relay complete unit 1 W, 24 V AC LED module red Standard plug-in socket screw terminal",20.87,"ΤΕΜ",1,"EP",5,"LZS:RT3A4R24","LZS Μίνι Ρελέ"]
["LZS:RT3A4S15","Plug-in relay complete unit 1 W, 115 V AC LED module red Standard plug-in socket screw terminal",24.13,"ΤΕΜ",1,"EP",5,"LZS:RT3A4S15","LZS Μίνι Ρελέ"]
["LZS:RT3A4T30","Plug-in relay complete unit 1 W, 230 V AC LED module red Standard plug-in socket screw terminal",24.13,"ΤΕΜ",1,"EP",5,"LZS:RT3A4T30","LZS Μίνι Ρελέ"]
["LZS:RT3B4L24","Plug-in relay complete unit 1 W, 24 V DC LED module red Socket with logic isolation screw terminal",20.87,"ΤΕΜ",1,"EP",5,"LZS:RT3B4L24","LZS Μίνι Ρελέ"]
["LZS:RT3B4R24","Plug-in relay complete unit 1 W, 24 V AC LED module red Socket with logic isolation screw terminal",20.87,"ΤΕΜ",1,"EP",5,"LZS:RT3B4R24","LZS Μίνι Ρελέ"]
["LZS:RT3B4S15","Plug-in relay complete unit 1 W, 115 V AC LED module red Socket with logic isolation screw terminal",24.13,"ΤΕΜ",1,"EP",5,"LZS:RT3B4S15","LZS Μίνι Ρελέ"]
["LZS:RT3B4T30","Plug-in relay complete unit 1 W, 230 V AC LED module red Socket with logic isolation screw terminal",24.13,"ΤΕΜ",1,"EP",5,"LZS:RT3B4T30","LZS Μίνι Ρελέ"]
["LZS:RT3B6L24-A","Plug-in relay complete unit 1 W, 24 V DC LED module green Plug-in socket with safe isolation screw terminal",18.579999999999998,"ΤΕΜ",1,"EP",1,"LZS:RT3B6L24A","LZS Μίνι Ρελέ"]
["LZS:RT3D4L24","Plug-in relay complete unit 1 W, 24 V DC LED module red Socket with logic isolation Spring-type terminal (push-in)",21.96,"ΤΕΜ",1,"EP",5,"LZS:RT3D4L24","LZS Μίνι Ρελέ"]
["LZS:RT3D4R24","Plug-in relay complete unit 1 W, 24 V AC LED module red Socket with logic isolation Spring-type terminal (push-in)",21.96,"ΤΕΜ",1,"EP",5,"LZS:RT3D4R24","LZS Μίνι Ρελέ"]
["LZS:RT3D4S15","Plug-in relay complete unit 1 W, 115 V AC LED module red Socket with logic isolation Spring-type terminal (push-in)",25.22,"ΤΕΜ",1,"EP",5,"LZS:RT3D4S15","LZS Μίνι Ρελέ"]
["LZS:RT3D4T30","Plug-in relay complete unit 1 W, 230 V AC LED module red Socket with logic isolation Spring-type terminal (push-in)",25.22,"ΤΕΜ",1,"EP",5,"LZS:RT3D4T30","LZS Μίνι Ρελέ"]
["LZS:RT4A4L24","Plug-in relay complete unit 2 W, 24 V DC LED module red Standard plug-in socket screw terminal",21.96,"ΤΕΜ",1,"EP",5,"LZS:RT4A4L24","LZS Μίνι Ρελέ"]
["LZS:RT4A4R24","Plug-in relay complete unit 2 W, 24 V AC LED module red Standard plug-in socket screw terminal",21.96,"ΤΕΜ",1,"EP",5,"LZS:RT4A4R24","LZS Μίνι Ρελέ"]
["LZS:RT4A4S15","Plug-in relay complete unit 2 W, 115 V AC LED module red Standard plug-in socket screw terminal",25,"ΤΕΜ",1,"EP",5,"LZS:RT4A4S15","LZS Μίνι Ρελέ"]
["LZS:RT4A4T30","Plug-in relay complete unit 2 W, 230 V AC LED module red Standard plug-in socket screw terminal",25,"ΤΕΜ",1,"EP",5,"LZS:RT4A4T30","LZS Μίνι Ρελέ"]
["LZS:RT4B4L24","Plug-in relay complete unit 2 W, 24 V DC LED module red Socket with logic isolation screw terminal",21.96,"ΤΕΜ",1,"EP",5,"LZS:RT4B4L24","LZS Μίνι Ρελέ"]
["LZS:RT4B4R24","Plug-in relay complete unit 2 W, 24 V AC LED module red Socket with logic isolation screw terminal",21.96,"ΤΕΜ",1,"EP",5,"LZS:RT4B4R24","LZS Μίνι Ρελέ"]
["LZS:RT4B4S15","Plug-in relay complete unit 2 W, 115 V AC LED module red Socket with logic isolation screw terminal",25,"ΤΕΜ",1,"EP",5,"LZS:RT4B4S15","LZS Μίνι Ρελέ"]
["LZS:RT4B4T30","Plug-in relay complete unit 2 W, 230 V AC LED module red Socket with logic isolation screw terminal",25,"ΤΕΜ",1,"EP",5,"LZS:RT4B4T30","LZS Μίνι Ρελέ"]
["LZS:RT4B6L24-A","Plug-in relay complete unit 2 CO, 24 V DC LED module green Plug-in socket with logical separation, screw terminal",18.579999999999998,"ΤΕΜ",1,"EP",1,"LZS:RT4B6L24A","LZS Μίνι Ρελέ"]
["LZS:RT4D4L24","Plug-in relay complete unit 2 W, 24 V DC LED module red Socket with logic isolation Spring-type terminal (push-in)",22.93,"ΤΕΜ",1,"EP",5,"LZS:RT4D4L24","LZS Μίνι Ρελέ"]
["LZS:RT4D4R24","Plug-in relay complete unit 2 W, 24 V AC LED module red Socket with logic isolation Spring-type terminal (push-in)",22.93,"ΤΕΜ",1,"EP",5,"LZS:RT4D4R24","LZS Μίνι Ρελέ"]
["LZS:RT4D4S15","Plug-in relay complete unit 2 W, 115 V AC LED module red Socket with logic isolation Spring-type terminal (push-in)",26.19,"ΤΕΜ",1,"EP",5,"LZS:RT4D4S15","LZS Μίνι Ρελέ"]
["LZS:RT4D4T30","Plug-in relay complete unit 2 W, 230 V AC LED module red Socket with logic isolation Spring-type terminal (push-in)",26.19,"ΤΕΜ",1,"EP",5,"LZS:RT4D4T30","LZS Μίνι Ρελέ"]
["LZS:RT78725","Plug-in socket for RT relay Standard plug-in socket screw terminal",6.92,"ΤΕΜ",1,"EP",1,"LZS:RT78725","LZS Μίνι Ρελέ"]
["LZS:RT78726","Plug-in socket for RT relay Socket with logic isolation screw terminal",6.92,"ΤΕΜ",1,"EP",1,"LZS:RT78726","LZS Μίνι Ρελέ"]
["LZS:RT7872P","Plug-in socket for RT relay Socket with logic isolation Socket with logic isolation Spring-type terminal (push-in)",7.66,"ΤΕΜ",1,"EP",1,"LZS:RT7872P","LZS Μίνι Ρελέ"]
["LZX:MT321060","Plug-in relay, 3 changeover contacts Relay without LED 38 mm, 60 V DC",30.65,"ΤΕΜ",1,"EP",1,"LZX:MT321060","LZX Μίνι Ρελέ"]
["LZX:PT270024","Plug-in relay, 2 change-over contacts 24 V DC, also for LZS sockets",8.06,"ΤΕΜ",1,"EP",1,"LZX:PT270024","LZX Μίνι Ρελέ"]
["LZX:PT270524","Plug-in relay, 2 change-over contacts 24 V AC, also for LZS sockets",8.06,"ΤΕΜ",1,"EP",1,"LZX:PT270524","LZX Μίνι Ρελέ"]
["LZX:PT270615","Plug-in relay, 2 change-over contacts 115 V AC, also for LZS sockets",9.42,"ΤΕΜ",1,"EP",1,"LZX:PT270615","LZX Μίνι Ρελέ"]
["LZX:PT270730","Plug-in relay, 2 change-over contacts 230 V AC, also for LZS sockets",9.42,"ΤΕΜ",1,"EP",1,"LZX:PT270730","LZX Μίνι Ρελέ"]
["LZX:PT370024","Plug-in relay, 3 changeover contacts 24 V DC, 10 A, Width 22.5 mm for LZS sockets",8.06,"ΤΕΜ",1,"EP",1,"LZX:PT370024","LZX Μίνι Ρελέ"]
["LZX:PT370125","Plug-in relay, 3 changeover contacts 125 V DC, 10 A, Width 22.5 mm for LZS sockets",9.42,"ΤΕΜ",1,"EP",1,"LZX:PT370125","LZX Μίνι Ρελέ"]
["LZX:PT370524","Plug-in relay, 3 changeover contacts 24 V AC, 10 A, Width 22.5 mm  for LZS sockets",8.06,"ΤΕΜ",1,"EP",1,"LZX:PT370524","LZX Μίνι Ρελέ"]
["LZX:PT370615","Plug-in relay, 3 changeover contacts 115 V AC, 10 A, Width 22.5 mm  for LZS sockets",9.42,"ΤΕΜ",1,"EP",1,"LZX:PT370615","LZX Μίνι Ρελέ"]
["LZX:PT370730","Plug-in relay, 3 changeover contacts 230 V AC, 10 A, Width 22.5 mm  for LZS sockets",9.42,"ΤΕΜ",1,"EP",1,"LZX:PT370730","LZX Μίνι Ρελέ"]
["LZX:PT520024","Plug-in relay 4 changeover contacts, without test bracket 24 V DC,  for LZS sockets",8.06,"ΤΕΜ",1,"EP",1,"LZX:PT520024","LZX Μίνι Ρελέ"]
["LZX:PT520730","Plug-in relay 4 changeover contacts, without test bracket 230 V AC,  for LZS sockets",9.42,"ΤΕΜ",1,"EP",1,"LZX:PT520730","LZX Μίνι Ρελέ"]
["LZX:PT570024","Plug-in relay, 4 changeover contacts 24 V DC, 6 A, Width 22.5 mm  for LZS sockets",8.06,"ΤΕΜ",1,"EP",1,"LZX:PT570024","LZX Μίνι Ρελέ"]
["LZX:PT570125","Plug-in relay, 4 changeover contacts 125 V DC, 6 A, Width 22.5 mm  for LZS sockets",9.42,"ΤΕΜ",1,"EP",1,"LZX:PT570125","LZX Μίνι Ρελέ"]
["LZX:PT570524","Plug-in relay, 4 changeover contacts 24 V AC, 6 A, Width 22.5 mm  for LZS sockets",8.06,"ΤΕΜ",1,"EP",1,"LZX:PT570524","LZX Μίνι Ρελέ"]
["LZX:PT570615","Plug-in relay, 4 changeover contacts 115 V AC, 6 A, Width 22.5 mm  for LZS sockets",9.42,"ΤΕΜ",1,"EP",1,"LZX:PT570615","LZX Μίνι Ρελέ"]
["LZX:PT570730","Plug-in relay, 4 changeover contacts 230 V AC, 6 A, Width 22.5 mm  for LZS sockets",9.42,"ΤΕΜ",1,"EP",1,"LZX:PT570730","LZX Μίνι Ρελέ"]
["LZX:PT580024","Plug-in relay 4 changeover contacts, hard gold-plated 24 V DC,  for LZS sockets",10.41,"ΤΕΜ",1,"EP",1,"LZX:PT580024","LZX Μίνι Ρελέ"]
["LZX:PT580730","Plug-in relay 4 changeover contacts, hard gold-plated 230 V AC,  for LZS sockets",13.48,"ΤΕΜ",1,"EP",1,"LZX:PT580730","LZX Μίνι Ρελέ"]
["LZX:RT314024","Plug-in relay 1 W, Width 15 mm, 24 V DC  for LZS sockets",5.42,"ΤΕΜ",1,"EP",1,"LZX:RT314024","LZX Μίνι Ρελέ"]
["LZX:RT314524","Plug-in relay, 1 change-over contact 24 V AC, 16 A, Width 15.5 mm  for LZS sockets",5.42,"ΤΕΜ",1,"EP",1,"LZX:RT314524","LZX Μίνι Ρελέ"]
["LZX:RT314615","Plug-in relay, 1 change-over contact 115 V AC, 16 A, Width 15.5 mm  for LZS sockets",9.1300000000000008,"ΤΕΜ",1,"EP",1,"LZX:RT314615","LZX Μίνι Ρελέ"]
["LZX:RT314730","Plug-in relay 1 W, Width 15 mm, 230 V AC  for LZS sockets",9.1300000000000008,"ΤΕΜ",1,"EP",1,"LZX:RT314730","LZX Μίνι Ρελέ"]
["LZX:RT315024","Plug-in relay 1 change-over contact, hard gold-plated 24 V DC,  for LZS sockets",6.35,"ΤΕΜ",1,"EP",1,"LZX:RT315024","LZX Μίνι Ρελέ"]
["LZX:RT315730","Plug-in relay 1 change-over contact, hard gold-plated 230 V AC,  for LZS sockets",9.61,"ΤΕΜ",1,"EP",1,"LZX:RT315730","LZX Μίνι Ρελέ"]
["LZX:RT424012","Plug-in relay 2 W, Width 15 mm, 12 V DC  for LZS sockets",6.46,"ΤΕΜ",1,"EP",1,"LZX:RT424012","LZX Μίνι Ρελέ"]
["LZX:RT424024","Plug-in relay 2 W, Width 15 mm, 24 V DC  for LZS sockets",6.46,"ΤΕΜ",1,"EP",1,"LZX:RT424024","LZX Μίνι Ρελέ"]
["LZX:RT424110","Plug-in relay 2 W, Width 15 mm, 125 V DC  for LZS sockets",10.26,"ΤΕΜ",1,"EP",1,"LZX:RT424110","LZX Μίνι Ρελέ"]
["LZX:RT424524","Plug-in relay, 2 change-over contacts 24 V AC, 8 A, Width 15.5 mm  for LZS sockets",6.46,"ΤΕΜ",1,"EP",1,"LZX:RT424524","LZX Μίνι Ρελέ"]
["LZX:RT424615","Plug-in relay, 2 change-over contacts 115 V AC, 16 A, Width 15.5 mm  for LZS sockets",10.26,"ΤΕΜ",1,"EP",1,"LZX:RT424615","LZX Μίνι Ρελέ"]
["LZX:RT424730","Plug-in relay 2 W, Width 15 mm, 230 V AC  for LZS sockets",10.26,"ΤΕΜ",1,"EP",1,"LZX:RT424730","LZX Μίνι Ρελέ"]
["M56340-A0001","NIPPLE CONNECTION G 1/2 MAX. 400 BAR, MAT. NO.2.0401.26",4,"ΤΕΜ",1,"PI2",1,"M56340A0001","Όργανα Μέτρησης Πεδίου"]
["M56340-A0002","NIPPLE CONNECTION G 1/2 MAX. 400 BAR, MAT.NO. 1.0715/ 1.0037",5,"ΤΕΜ",1,"PI2",1,"M56340A0002","Όργανα Μέτρησης Πεδίου"]
["M56340-A0003","NIPPLE CONNECTION G 1/2 MAX. 400 BAR, MAT. NO. 1.43305/ 1.4571",19,"ΤΕΜ",1,"PI2",1,"M56340A0003","Όργανα Μέτρησης Πεδίου"]
["M56340-A0004","CLAMPING SLEEVE G 1/2 MAX. 400 BAR, MAT.NO. 2.0402.26",3,"ΤΕΜ",1,"PI2",1,"M56340A0004","Όργανα Μέτρησης Πεδίου"]
["M56340-A0005","CLAMPING SLEEVE G 1/2 MAX. 400 BAR, MAT.NO. 1.0715",2,"ΤΕΜ",1,"PI2",1,"M56340A0005","Όργανα Μέτρησης Πεδίου"]
["M56340-A0006","COLLAR CEONNECTION PIECE G 1/2 MAX. 400 BAR, MAT.NO. 2.0401.26",18,"ΤΕΜ",1,"PI2",1,"M56340A0006","Όργανα Μέτρησης Πεδίου"]
["M56340-A0007","COLLAR CONNECTION PIECE G 1/2 MAX. 400 BAR, MAT.NO. 1.0715",21,"ΤΕΜ",1,"PI2",1,"M56340A0007","Όργανα Μέτρησης Πεδίου"]
["M56340-A0008","NIPPLE CONNECTION M20 X 1,5, 14 MM, MAX. 400 BAR, MAT. NO. 1.43305/1.4571",19,"ΤΕΜ",1,"PI2",1,"M56340A0008","Όργανα Μέτρησης Πεδίου"]
["M56340-A0027","SINGLE SHUT-OFF VALVE TYPE A TO DIN 16270 MAX.OPERAT.PRESSURE 250BAR BRASS",19,"ΤΕΜ",1,"PI2",1,"M56340A0027","Όργανα Μέτρησης Πεδίου"]
["M56340-A0028","SINGLE SHUT-OFF VALVE TYPE A TO DIN 16270 MAX.OPERAT.PRESSURE 400BAR STEEL",21,"ΤΕΜ",1,"PI2",1,"M56340A0028","Όργανα Μέτρησης Πεδίου"]
["M56340-A0029","SINGLE SHUT-OFF VALVE TYPE A TO DIN 16270 MAX.OPERAT.PRESSURE 400BAR STAINL. STEEL",83,"ΤΕΜ",1,"PI2",1,"M56340A0029","Όργανα Μέτρησης Πεδίου"]
["M56340-A0030","SINGLE SHUT-OFF VALVE TYPE A TO DIN 16271 W/ TEST PEG MAX.OP.RESS.250BAR BRASS",26,"ΤΕΜ",1,"PI2",1,"M56340A0030","Όργανα Μέτρησης Πεδίου"]
["M56340-A0031","SINGLE SHUT-OFF VALVE TYPE A TO DIN 16271 W/ TEST PEG MAX.OP.RESS.400BAR STEEL",26,"ΤΕΜ",1,"PI2",1,"M56340A0031","Όργανα Μέτρησης Πεδίου"]
["M56340-A0032","SINGLE SHUT-OFF VALVE TYPE A TO DIN 16271 W/ TEST PEG MAX.OP.RESS.400BAR STAINL. STEEL",67,"ΤΕΜ",1,"PI2",1,"M56340A0032","Όργανα Μέτρησης Πεδίου"]
["M56340-A0033","DOUBLE SHUT-OFF VALVE TYPE A TEST CONNECT.SIMIL.TO DIN 16272 W/ NARROW TEST FLANGE MAX.OPER. PRESS. 250BAR BRASS",42,"ΤΕΜ",1,"PI2",1,"M56340A0033","Όργανα Μέτρησης Πεδίου"]
["M56340-A0034","DOUBLE SHUT-OFF VALVE TYPE A TEST CONNECT.SIMIL.TO DIN 16272 W/ NARROW TEST FLANGE MAX.OPER. PRESS. 400BAR STEEL",51,"ΤΕΜ",1,"PI2",1,"M56340A0034","Όργανα Μέτρησης Πεδίου"]
["M56340-A0035","DOUBLE SHUT-OFF VALVE TYPE A TEST CONNECT.SIMIL.TO DIN 16272 W/ NARROW TEST FLANGE MAX.OPER. PRESS. 400BAR STAINLESS STEEL",102,"ΤΕΜ",1,"PI2",1,"M56340A0035","Όργανα Μέτρησης Πεδίου"]
["M56340-A0036","DOUBLE SHUT-OFF VALVE TYPE A TEST CONNECT.SIMIL.TO DIN 16272 W/ TEST PEG MAX.OPER. PRESS. 250BAR BRASS",36,"ΤΕΜ",1,"PI2",1,"M56340A0036","Όργανα Μέτρησης Πεδίου"]
["M56340-A0037","DOUBLE SHUT-OFF VALVE TYPE A TEST CONNECT.SIMIL.TO DIN 16272 W/ TEST PEG MAX.OPER. PRESS. 400BAR STEEL",40,"ΤΕΜ",1,"PI2",1,"M56340A0037","Όργανα Μέτρησης Πεδίου"]
["M56340-A0038","DOUBLE SHUT-OFF VALVE TYPE A TEST CONNECT.SIMIL.TO DIN 16272 W/ TEST PEG MAX.OPER. PRESS. 400BAR STAINLESS STEEL",96,"ΤΕΜ",1,"PI2",1,"M56340A0038","Όργανα Μέτρησης Πεδίου"]
["M56340-A0043","WATER TRAP B TO DIN 16282 120 CEL/100 BAR, 400 CEL/63 BAR MAT. NO. 1.0305",18,"ΤΕΜ",1,"PI2",1,"M56340A0043","Όργανα Μέτρησης Πεδίου"]
["M56340-A0045","WATER TRAP D TO DIN 16282 120 CEL/100 BAR, 400 CEL/63 BAR MAT. NO. 1.0305",18,"ΤΕΜ",1,"PI2",1,"M56340A0045","Όργανα Μέτρησης Πεδίου"]
["M56340-A0046","INSTRUMENT BRACKET, DESIGN H TO DIN 16281, MADE OF ALUMINUM ALLOY, PROJECTION LENGTH 60 MM",11,"ΤΕΜ",1,"PI2",1,"M56340A0046","Όργανα Μέτρησης Πεδίου"]
["M56340-A0047","INSTRUMENT BRACKET, DESIGN H TO DIN 16281, MADE OF ALUMINUM ALLOY, PROJECTION LENGTH 100 MM",13,"ΤΕΜ",1,"PI2",1,"M56340A0047","Όργανα Μέτρησης Πεδίου"]
["M56340-A0048","INSTRUMENT BRACKET, DESIGN H TO DIN 16281, MADE OF ALUMINUM ALLOY, PROJECTION LENGTH 160 MM",18,"ΤΕΜ",1,"PI2",1,"M56340A0048","Όργανα Μέτρησης Πεδίου"]
["M56340-A0053","INSTRUMENT BRACKET, DESIGN A TO DIN 16281, MADE OF ANNEALED CAST IRON, PROJECTION LENGTH 100 MM",39,"ΤΕΜ",1,"PI2",1,"M56340A0053","Όργανα Μέτρησης Πεδίου"]
["M56340-A0054","PRESSURE IMPACT REDUCER BRASS",8,"ΤΕΜ",1,"PI2",1,"M56340A0054","Όργανα Μέτρησης Πεδίου"]
["M56340-A0059","PRESSURE IMPACT REDUCER STAINLESS STEEL",39,"ΤΕΜ",1,"PI2",1,"M56340A0059","Όργανα Μέτρησης Πεδίου"]
["M56340-A0061","WATER TRAP B TO DIN 16282 120 CEL/100 BAR, 400 CEL/63 BAR MAT. NO. 1.4571",42,"ΤΕΜ",1,"PI2",1,"M56340A0061","Όργανα Μέτρησης Πεδίου"]
["M56340-A0063","WATER TRAP D TO DIN 16282 120 CEL/100 BAR, 400 CEL/63 BAR MAT. NO. 1.4571",43,"ΤΕΜ",1,"PI2",1,"M56340A0063","Όργανα Μέτρησης Πεδίου"]
["M56340-A0079","INSTRUMENT BRACKET, DSIGN A TO DIN 16281, MADE OF ANNEALED CAST IRON, FOR MOUNTING ON A HORIZONTAL OR VERTICAL PIPE",55,"ΤΕΜ",1,"PI2",1,"M56340A0079","Όργανα Μέτρησης Πεδίου"]
["M56340-C1229","SINGLE SHUT-OFF VALVE TYPE A TO DIN 16270 MAX.OPERAT.PRESSURE 400BAR STAINL. STEEL WITH CERTIFICATE 3.1 ACCORDING EN 10204",140,"ΤΕΜ",1,"PI2",1,"M56340C1229","Όργανα Μέτρησης Πεδίου"]
["P73714-B1-A111","Firmware for SIPART DR22",48,"ΤΕΜ",1,"PI1",1,"P73714B1A111","Όργανα Μέτρησης Πεδίου"]
["P73715-B1-A111","Firmware for SIPART DR24 (old version)",48,"ΤΕΜ",1,"PI1",1,"P73715B1A111","Όργανα Μέτρησης Πεδίου"]
["P73720-B1-A111","Firmware for SIPART DR21",91,"ΤΕΜ",1,"PI1",1,"P73720B1A111","Όργανα Μέτρησης Πεδίου"]
["PBD:00000158","Siemens Canada - BID_McGinnis Cement Approval Drawing 1",697,"ΤΕΜ",1,"PI1",1,"PBD:00000158","Όργανα Μέτρησης Πεδίου"]
["PBD:00000159","Siemens Canada - BID_McGinnis Cement Approval Drawing 1",697,"ΤΕΜ",1,"PI1",1,"PBD:00000159","Όργανα Μέτρησης Πεδίου"]
["PBD:00000160","Siemens Canada - BID_McGinnis Cement Approval Drawing 1",697,"ΤΕΜ",1,"PI1",1,"PBD:00000160","Όργανα Μέτρησης Πεδίου"]
["PBD:20502087","MOUNTING PLATE 30 CM X 30 CM (12\" X 12\") FOR VS 100 VELOCITY SENOSR",107,"ΤΕΜ",1,"PI3",1,"PBD:20502087","Όργανα Μέτρησης Πεδίου"]
["PBD:22475K1A","KIT,horn antenna,short, SITRANS LR,SST",487,"ΤΕΜ",1,"PI1",1,"PBD:22475K1A","Όργανα Μέτρησης Πεδίου"]
["PBD:22475K2A","Kit,horn antenna, long, for SITRANS LR,stainless steel",428,"ΤΕΜ",1,"PI1",1,"PBD:22475K2A","Όργανα Μέτρησης Πεδίου"]
["PBD:22475K3A","Kit,horn antenna,short,LR400, PURG",502,"ΤΕΜ",1,"PI1",1,"PBD:22475K3A","Όργανα Μέτρησης Πεδίου"]
["PBD:22475K4A","KIT,horn ant,long,purge, GP approval only",536,"ΤΕΜ",1,"PI1",1,"PBD:22475K4A","Όργανα Μέτρησης Πεδίου"]
["PBD:23311020","WINDOW,DAMPER,E37,LUCITE",94,"ΤΕΜ",1,"PI1",1,"PBD:23311020","Όργανα Μέτρησης Πεδίου"]
["PBD:23900005","LOAD CELL, 50LB,COMP, 2mM/V,C462,CS",2182,"ΤΕΜ",1,"PI1",1,"PBD:23900005","Όργανα Μέτρησης Πεδίου"]
["PBD:23900010","LOAD CELL, 100LB,COMP, 2mM/V,C462,SS",1894,"ΤΕΜ",1,"PI1",1,"PBD:23900010","Όργανα Μέτρησης Πεδίου"]
["PBD:23900012","LOAD CELL, 250LB, COMP,2mM/V,C462,SS",1894,"ΤΕΜ",1,"PI1",1,"PBD:23900012","Όργανα Μέτρησης Πεδίου"]
["PBD:23900176","LOAD CELL,MLC/MILLFLO,2LB,SS,F LOAD CELL 2 LB FOR MILLFLO FLOWMETER",2354,"ΤΕΜ",1,"PI1",1,"PBD:23900176","Όργανα Μέτρησης Πεδίου"]
["PBD:23900177","LOAD CELL, 5 LB FOR MILLFLO FLOWMETER",2354,"ΤΕΜ",1,"PI1",1,"PBD:23900177","Όργανα Μέτρησης Πεδίου"]
["PBD:23900223","LOAD CELL 'Weighfeeder' 6KG, Stainless steel",1399,"ΤΕΜ",1,"PI1",1,"PBD:23900223","Όργανα Μέτρησης Πεδίου"]
["PBD:23900224","LOAD CELL 'Weighfeeder' 25LB, stainless steel",2216,"ΤΕΜ",1,"PI1",1,"PBD:23900224","Όργανα Μέτρησης Πεδίου"]
["PBD:23900225","LOAD CELL 'Weighfeeder' 50LB, stainless steel",1885,"ΤΕΜ",1,"PI1",1,"PBD:23900225","Όργανα Μέτρησης Πεδίου"]
["PBD:23900244","LOAD CELL 10 LB, FOR MLC BELT SCALE, MILLFLO FLOWMETER",2354,"ΤΕΜ",1,"PI1",1,"PBD:23900244","Όργανα Μέτρησης Πεδίου"]
["PBD:23900245","LOAD CELL 20 LB FOR MLC BELT SCALE",2354,"ΤΕΜ",1,"PI1",1,"PBD:23900245","Όργανα Μέτρησης Πεδίου"]
["PBD:23900246","LOAD CELL, 50 LB, STAINLESS STEEL, FOR MSI BELT SCALE, MILLFLO FLOWMETER",1857,"ΤΕΜ",1,"PI1",1,"PBD:23900246","Όργανα Μέτρησης Πεδίου"]
["PBD:23900247","LOAD CELL, 100 LB, STAINLESS STEEL, FOR MSI BELT SCALE, MILLFLO FLOWMETER",1857,"ΤΕΜ",1,"PI1",1,"PBD:23900247","Όργανα Μέτρησης Πεδίου"]
["PBD:23900248","LOAD CELL,MSI,250LB,SS,F",1857,"ΤΕΜ",1,"PI1",1,"PBD:23900248","Όργανα Μέτρησης Πεδίου"]
["PBD:23900249","LOAD CELL, 500 LB, STAINLESS STEEL, FOR MSI BELT SCALE",1857,"ΤΕΜ",1,"PI1",1,"PBD:23900249","Όργανα Μέτρησης Πεδίου"]
["PBD:23900250","LOAD CELL, 750 LB, STAINLESS STEEL, FOR MSI BELT SCALE",1857,"ΤΕΜ",1,"PI1",1,"PBD:23900250","Όργανα Μέτρησης Πεδίου"]
["PBD:23900251","LOAD CELL, 1000 LB, STAINLESS STEEL, FOR MSI BELT SCALE",1857,"ΤΕΜ",1,"PI1",1,"PBD:23900251","Όργανα Μέτρησης Πεδίου"]
["PBD:23900261","LOAD CELL,NTEP,OIML, 100LB,SS",3088,"ΤΕΜ",1,"PI1",1,"PBD:23900261","Όργανα Μέτρησης Πεδίου"]
["PBD:23900262","LOAD CELL,NTEP,OIML, 250LB,SS",3088,"ΤΕΜ",1,"PI1",1,"PBD:23900262","Όργανα Μέτρησης Πεδίου"]
["PBD:23900263","LOAD CELL,NTEP,OIML,  500LB,SS",3088,"ΤΕΜ",1,"PI1",1,"PBD:23900263","Όργανα Μέτρησης Πεδίου"]
["PBD:23900264","LOAD CELL,NTEP,OIML,  750LB,SS",3088,"ΤΕΜ",1,"PI1",1,"PBD:23900264","Όργανα Μέτρησης Πεδίου"]
["PBD:23900265","LOAD CELL,NTEP,OIML,1000LB,SS",2999,"ΤΕΜ",1,"PI1",1,"PBD:23900265","Όργανα Μέτρησης Πεδίου"]
["PBD:23900268","LOAD CELL, 500 LB,G4-CD500-S, HI-TEMP",2102,"ΤΕΜ",1,"PI1",1,"PBD:23900268","Όργανα Μέτρησης Πεδίου"]
["PBD:24250393","J-BOX CAUTION TAG,LOCKOUT",2,"ΤΕΜ",1,"PI1",1,"PBD:24250393","Όργανα Μέτρησης Πεδίου"]
["PBD:25500K02A","KIT,SPARE,RADAR,ANTENNA HORN, 80mm,316SS",670,"ΤΕΜ",1,"PI1",1,"PBD:25500K02A","Όργανα Μέτρησης Πεδίου"]
["PBD:25500K03A","KIT,SPARE,RADAR,ANTENNA HORN, 100mm,316SS",670,"ΤΕΜ",1,"PI1",1,"PBD:25500K03A","Όργανα Μέτρησης Πεδίου"]
["PBD:25500K05A","KIT,SPARE,RADAR,antenna horn, 150mm,316SS",670,"ΤΕΜ",1,"PI1",1,"PBD:25500K05A","Όργανα Μέτρησης Πεδίου"]
["PBD:25501K0100A","100MM (4\") horn antenna extension kit",486,"ΤΕΜ",1,"PI1",1,"PBD:25501K0100A","Όργανα Μέτρησης Πεδίου"]
["PBD:25501K0150A","150 mm (6\") horn antenna extension kit",499,"ΤΕΜ",1,"PI1",1,"PBD:25501K0150A","Όργανα Μέτρησης Πεδίου"]
["PBD:25501K0200A","200 mm (8\") horn antenna extension kit",513,"ΤΕΜ",1,"PI1",1,"PBD:25501K0200A","Όργανα Μέτρησης Πεδίου"]
["PBD:25501K0500A","7ML14100AA00-Z,Y01=0500MM",655,"ΤΕΜ",1,"PI1",1,"PBD:25501K0500A","Όργανα Μέτρησης Πεδίου"]
["PBD:25501K1000A","1000 mm (40\") horn antenna extension kit",857,"ΤΕΜ",1,"PI1",1,"PBD:25501K1000A","Όργανα Μέτρησης Πεδίου"]
["PBD:26950551","Spares - Weighfeeder BELT,CNVR,NITRILE,24X161, 135PIW,3PLY 3 Ply Poly 135 White Nit  161\" (13'5\") Long x 24in Wide Endless Hot bonded step splice, Standard angle White Nit,  B Section flange (2 ea.) Hot vulcanized each belt edge",3115,"ΤΕΜ",1,"PI1",1,"PBD:26950551","Όργανα Μέτρησης Πεδίου"]
["PBD:45000673","TAG, PAPER WITH HOLE, 100 X 50MM,MULTIPLE TEXT LINES",48,"ΤΕΜ",1,"PI3",1,"PBD:45000673","Όργανα Μέτρησης Πεδίου"]
["PBD:51002K0100AAA","KIT,IQ,ROD,SHLD,2\"NPT,100mm, 316,PTFE,FKM",1004,"ΤΕΜ",1,"PI1",1,"PBD:51002K0100AAA","Όργανα Μέτρησης Πεδίου"]
["PBD:51002K0100BAA","KIT,IQ,ROD,SHLD,2\"BSP,100mm, 316,PTFE,FKM",1004,"ΤΕΜ",1,"PI1",1,"PBD:51002K0100BAA","Όργανα Μέτρησης Πεδίου"]
["PBD:51002K0100CAA","KIT,IQ,ROD,SHLD,2\"G,100mm,316, PTFE,FKM",1144,"ΤΕΜ",1,"PI1",1,"PBD:51002K0100CAA","Όργανα Μέτρησης Πεδίου"]
["PBD:51002K0150CAA","KIT,LR,Rod,Shield,2G,150mm, 316,PTFE,VITON. PTFE rod antenna shielded kit, 2\"G 316 Stainless Steel Process Connection, FKM O-ring, 150 mm 316 Stainless Steel  shield",1078,"ΤΕΜ",1,"PI1",1,"PBD:51002K0150CAA","Όργανα Μέτρησης Πεδίου"]
["PBD:51002K0200CAA","KIT,LR,Rod,Shield,2G,200mm, 316,PTFE,VITON. PTFE rod antenna shielded kit, 2\"G 316 Stainless Steel Process Connection, FKM O-ring, 200 mm 316 Stainless Steel  shield",1509,"ΤΕΜ",1,"PI1",1,"PBD:51002K0200CAA","Όργανα Μέτρησης Πεδίου"]
["PBD:51002K0250CAA","KIT,LR,Rod,Shield,2G,250mm, 316,PTFE,VITON. PTFE rod antenna shielded kit, 2\"G 316 Stainless Steel Process Connection, FKM O-ring, 250 mm 316 Stainless Steel  shield",1804,"ΤΕΜ",1,"PI1",1,"PBD:51002K0250CAA","Όργανα Μέτρησης Πεδίου"]
["PBD:51002K0350CAA","KIT,LR,Rod,Shield,2G,350mm, 316,PTFE,VITON. PTFE rod antenna shielded kit, 2\"G 316 Stainless Steel Process Connection, FKM O-ring, 350 mm 316 Stainless Steel  shield",2242,"ΤΕΜ",1,"PI1",1,"PBD:51002K0350CAA","Όργανα Μέτρησης Πεδίου"]
["PBD:51003K020AAAA","KIT,IQ,ROD/GSKT,22452 2\"/150, 316,PTFE",859,"ΤΕΜ",1,"PI1",1,"PBD:51003K020AAAA","Όργανα Μέτρησης Πεδίου"]
["PBD:51003K050AJAA","KIT, Assembly flange PTFE rod with gasket,DIN50 PN16,316L",859,"ΤΕΜ",1,"PI1",1,"PBD:51003K050AJAA","Όργανα Μέτρησης Πεδίου"]
["PBD:51003K050AOAA","KIT,ROD/GSKT,22452 JIS10K50A, 316,PTFE",1144,"ΤΕΜ",1,"PI1",1,"PBD:51003K050AOAA","Όργανα Μέτρησης Πεδίου"]
["PBD:51004K2AAA","KIT,IQ,ROD,1.5\"NPT,PTFE,316, FKM",1238,"ΤΕΜ",1,"PI1",1,"PBD:51004K2AAA","Όργανα Μέτρησης Πεδίου"]
["PBD:51004K3AAA","KIT,RADAR ROD,2\"NPT,PTFE,316, FKM",1238,"ΤΕΜ",1,"PI1",1,"PBD:51004K3AAA","Όργανα Μέτρησης Πεδίου"]
["PBD:51005K1AAA","IQ,ROD, PROCESS CONNECTION THREAD SERIES: 2\"NPT, ANTENNA MATERIAL: PTFE, WETTED METALLIC MATERIAL: 316 STAINLESS STEEL, O-RING MATERIAL: FKM",956,"ΤΕΜ",1,"PI1",1,"PBD:51005K1AAA","Όργανα Μέτρησης Πεδίου"]
["PBD:51005K2AAA","IQ,ROD,PROCESS CONNECTION THREAD SERIES: 2\"BSP, ANTENNA MATERIAL: PTFE, WETTED METALLIC MATERIAL: 316 STAINLESS STEEL, O-RING MATERIAL: FKM",956,"ΤΕΜ",1,"PI1",1,"PBD:51005K2AAA","Όργανα Μέτρησης Πεδίου"]
["PBD:51005K3AAA","KIT,RADAR ROD,2\"G,PTFE,316, FKM",956,"ΤΕΜ",1,"PI1",1,"PBD:51005K3AAA","Όργανα Μέτρησης Πεδίου"]
["PBD:51006K020AAAA","KIT,IQ HN 3\",22452 2/150 316, PTFE,FKM,NP",1334,"ΤΕΜ",1,"PI1",1,"PBD:51006K020AAAA","Όργανα Μέτρησης Πεδίου"]
["PBD:51006K020AABA","KIT,IQ HN 4\",22452 2/150 316, PTFE,FKM,No,Pressure",1334,"ΤΕΜ",1,"PI1",1,"PBD:51006K020AABA","Όργανα Μέτρησης Πεδίου"]
["PBD:51006K020AACA","KIT,IQ HN 6\",22452 2/150 316, PTFE,FKM,No Pressure",1334,"ΤΕΜ",1,"PI1",1,"PBD:51006K020AACA","Όργανα Μέτρησης Πεδίου"]
["PBD:51006K020AADA","KIT,IQ HN 8\",22452 2/150 316, PTFE,FKM,No Pressure",1334,"ΤΕΜ",1,"PI1",1,"PBD:51006K020AADA","Όργανα Μέτρησης Πεδίου"]
["PBD:51006K050AJAA","Kit for IQ Radar with Horn 80MM,22452,50/16,316,PTFE,NP",1334,"ΤΕΜ",1,"PI1",1,"PBD:51006K050AJAA","Όργανα Μέτρησης Πεδίου"]
["PBD:51006K050AJBA","KIT,IQ HORN 4\",22452,50/16, 316,PTFE,FKM,NP",1334,"ΤΕΜ",1,"PI1",1,"PBD:51006K050AJBA","Όργανα Μέτρησης Πεδίου"]
["PBD:51006K050AJCA","KIT,IQ HORN 4\",22452,50/16, 316,PTFE,FKM,No Pressure",1334,"ΤΕΜ",1,"PI1",1,"PBD:51006K050AJCA","Όργανα Μέτρησης Πεδίου"]
["PBD:51006K050AJDA","KIT,IQ HORN 8\",22452, 50/16,316, PTFE,FKM,NP",1334,"ΤΕΜ",1,"PI1",1,"PBD:51006K050AJDA","Όργανα Μέτρησης Πεδίου"]
["PBD:51008K1000LCA","KIT,SLIDING WAVEGUIDE, DN100 PN16 flange with 150 mm HORN ANTENNA",2441,"ΤΕΜ",1,"PI1",1,"PBD:51008K1000LCA","Όργανα Μέτρησης Πεδίου"]
["PBD:51010K1AA","KIT,IQ Rod SAN 3A,2\",PTFE,PR",3144,"ΤΕΜ",1,"PI1",1,"PBD:51010K1AA","Όργανα Μέτρησης Πεδίου"]
["PBD:51010K1AB","KIT,IQ Rod SAN 3A 2\" SANITARY CLAMP UHMW-PE,PR",1850,"ΤΕΜ",1,"PI1",1,"PBD:51010K1AB","Όργανα Μέτρησης Πεδίου"]
["PBD:51010K3AA","KIT,IQ Rod SAN 3A 4\" SANITARY CLAMP PTFE,PR",3886,"ΤΕΜ",1,"PI1",1,"PBD:51010K3AA","Όργανα Μέτρησης Πεδίου"]
["PBD:51010K3AB","KIT,IQ Rod SAN 3A 4\"SANITARY CLAMP UHMW-PE,PR",2590,"ΤΕΜ",1,"PI1",1,"PBD:51010K3AB","Όργανα Μέτρησης Πεδίου"]
["PBD:51014K0100AAA","KIT,IQ,ROD,SHLD,3/150,100MM, 316,PTFE,FKM",1144,"ΤΕΜ",1,"PI1",1,"PBD:51014K0100AAA","Όργανα Μέτρησης Πεδίου"]
["PBD:51014K0100EJA","KIT,LR,FLNG SHLD ROD,80PN16, 100MM,SS,T,V",1194,"ΤΕΜ",1,"PI1",1,"PBD:51014K0100EJA","Όργανα Μέτρησης Πεδίου"]
["PBD:51014K0150AAA","KIT,LR,FLNG SHLD ROD,3/150, 150MM,SS,T,V",1383,"ΤΕΜ",1,"PI1",1,"PBD:51014K0150AAA","Όργανα Μέτρησης Πεδίου"]
["PBD:51014K0150EJA","KIT,LR,FLNG SHLD ROD,80PN16, 150MM,SS,T,V",1428,"ΤΕΜ",1,"PI1",1,"PBD:51014K0150EJA","Όργανα Μέτρησης Πεδίου"]
["PBD:51014K0200AAA","PTFE shielded rod antenna kit, flanged, 3\" ASME 150 lb 316L SS flange, 200 mm 316L SS shield.",1428,"ΤΕΜ",1,"PI1",1,"PBD:51014K0200AAA","Όργανα Μέτρησης Πεδίου"]
["PBD:51014K0200EJA","PTFE shielded rod antenna kit, flanged, DN 80 PN 16 316L SS flange, 200 mm 316L SS shield.",1480,"ΤΕΜ",1,"PI1",1,"PBD:51014K0200EJA","Όργανα Μέτρησης Πεδίου"]
["PBD:51014K0250AAA","KIT,LR,FLNG SHLD ROD,80PN16, 250MM,SS,T,V",1525,"ΤΕΜ",1,"PI1",1,"PBD:51014K0250AAA","Όργανα Μέτρησης Πεδίου"]
["PBD:51014K0250EJA","KIT,LR,FLNG SHLD ROD, DN80PN16, 250MM,SS,T,V",1576,"ΤΕΜ",1,"PI1",1,"PBD:51014K0250EJA","Όργανα Μέτρησης Πεδίου"]
["PBD:51014K0450EJA","Kit, Flanged shielded rod, DN80 PN16, 450 MM, PTFE",1598,"ΤΕΜ",1,"PI1",1,"PBD:51014K0450EJA","Όργανα Μέτρησης Πεδίου"]
["PBD:51035410","KIT,display,SITRANS LR 400, B&B",324,"ΤΕΜ",1,"PI1",1,"PBD:51035410","Όργανα Μέτρησης Πεδίου"]
["PBD:51035813","Kit,universal flange 3\"/80mm, no pressure",273,"ΤΕΜ",1,"PI1",1,"PBD:51035813","Όργανα Μέτρησης Πεδίου"]
["PBD:51035814","Kit,universal flange 4\"/100mm,no pressure",354,"ΤΕΜ",1,"PI1",1,"PBD:51035814","Όργανα Μέτρησης Πεδίου"]
["PBD:51035815","Kit,universal flange 6\"/150mm, no pressure",558,"ΤΕΜ",1,"PI1",1,"PBD:51035815","Όργανα Μέτρησης Πεδίου"]
["PBD:51035816","Kit,universal flange 8\"/200mm, no pressure",928,"ΤΕΜ",1,"PI1",1,"PBD:51035816","Όργανα Μέτρησης Πεδίου"]
["PBD:51036252","7ML56715GA001XA0, SOLAR 1064829-1, 508MM SITRANS LC 300, Stilling Well Version with Flanged Process Connection: An inverse frequency shift capacitance transmitter for continuous level measuring in liquids and solids applications.",2630,"ΤΕΜ",1,"PI6",1,"PBD:51036252","Όργανα Μέτρησης Πεδίου"]
["PBD:51036253","7ML56715GA001XA0, SOLAR 1064829-2, 578MM SITRANS LC 300, Stilling Well Version with Flanged Process Connection: An inverse frequency shift capacitance transmitter for continuous level measuring in liquids and solids applications.",2640,"ΤΕΜ",1,"PI6",1,"PBD:51036253","Όργανα Μέτρησης Πεδίου"]
["PBD:51036254","7ML56715GA001XA0, SOLAR 1064829-3, 482MM SITRANS LC 300, Stilling Well Version with Flanged Process Connection: An inverse frequency shift capacitance transmitter for continuous level measuring in liquids and solids applications.",2619,"ΤΕΜ",1,"PI6",1,"PBD:51036254","Όργανα Μέτρησης Πεδίου"]
["PBD:51036255","7ML56715KA001XA0, SOLAR 1064829-4, 482MM SITRANS LC 300, Stilling Well Version with Flanged Process Connection: An inverse frequency shift capacitance transmitter for continuous level measuring in liquids and solids applications.",2562,"ΤΕΜ",1,"PI6",1,"PBD:51036255","Όργανα Μέτρησης Πεδίου"]
["PBD:51040483","CERTIFICATE C11",318,"ΤΕΜ",1,"PI6",1,"PBD:51040483","Όργανα Μέτρησης Πεδίου"]
["PBD:51040484","CERTIFICATE TEST",234,"ΤΕΜ",1,"PI3",1,"PBD:51040484","Όργανα Μέτρησης Πεδίου"]
["PBD:51041448","Sitrans LG Mounting eye M12x20",60,"ΤΕΜ",1,"PI1",1,"PBD:51041448","Όργανα Μέτρησης Πεδίου"]
["PBD:51041449","Sitrans LG Mounting spring",93,"ΤΕΜ",1,"PI1",1,"PBD:51041449","Όργανα Μέτρησης Πεδίου"]
["PBD:51110KC2","KIT,horn antenna,2\"/50,solid",365,"ΤΕΜ",1,"PI1",1,"PBD:51110KC2","Όργανα Μέτρησης Πεδίου"]
["PBD:51110KC3","KIT,horn antenna,3\"/80,solid",411,"ΤΕΜ",1,"PI1",1,"PBD:51110KC3","Όργανα Μέτρησης Πεδίου"]
["PBD:51110KC4","KIT,horn antenna,4\"/100,solid",502,"ΤΕΜ",1,"PI1",1,"PBD:51110KC4","Όργανα Μέτρησης Πεδίου"]
["PBD:54000141","RING,MCH.ILE37CA DIAP 10C881-2A",80,"ΤΕΜ",1,"PI1",1,"PBD:54000141","Όργανα Μέτρησης Πεδίου"]
["PBD:61009731","Load cell asembly,tension, 100lb (45.4 kg)",2295,"ΤΕΜ",1,"PI1",1,"PBD:61009731","Όργανα Μέτρησης Πεδίου"]
["PBD:61009732","Load cell assembly, tension, 250 lb (113.4 kg)",2295,"ΤΕΜ",1,"PI1",1,"PBD:61009732","Όργανα Μέτρησης Πεδίου"]
["PBD:61009733","Load cell assembly, tension, 500 lb (226.8 kg)",2295,"ΤΕΜ",1,"PI1",1,"PBD:61009733","Όργανα Μέτρησης Πεδίου"]
["PBD:61009734","Load cell asembly, tension, 1000 lb (453.6 kg) ,GR1",2295,"ΤΕΜ",1,"PI1",1,"PBD:61009734","Όργανα Μέτρησης Πεδίου"]
["PBD:61009735","Load cell assembly, tension, 50lb (22.7 kg)",2295,"ΤΕΜ",1,"PI1",1,"PBD:61009735","Όργανα Μέτρησης Πεδίου"]
["PBD:61010081","Kit,2 IDLER CABLE SUSPENSION",224,"ΤΕΜ",1,"PI1",1,"PBD:61010081","Όργανα Μέτρησης Πεδίου"]
["PBD:61010082","KIT,2 IDLER CABLE SUSPN.HEAVY DUTY",285,"ΤΕΜ",1,"PI1",1,"PBD:61010082","Όργανα Μέτρησης Πεδίου"]
["PBD:61010741","Kit,4 idler cable suspension standard",565,"ΤΕΜ",1,"PI1",1,"PBD:61010741","Όργανα Μέτρησης Πεδίου"]
["PBD:61010742","Kit,4 Idler cable suspension heavy duty",641,"ΤΕΜ",1,"PI1",1,"PBD:61010742","Όργανα Μέτρησης Πεδίου"]
["PBD:61010743","Kit,4 idler cable suspension magnum",723,"ΤΕΜ",1,"PI1",1,"PBD:61010743","Όργανα Μέτρησης Πεδίου"]
["PMF:ZERTIFIKATE","Zertificate SITRANS P",95,"ΤΕΜ",1,"PI2",1,"PMF:ZERTIFIKATE","Όργανα Μέτρησης Πεδίου"]
["RUM:ANTN0018","RUGGEDCOM ANTN0018 ANT Omni 1350-1500MHz 5dBi 360 deg., N-Female",159,"ΤΕΜ",1,"SIMATIC",1,"RUM:ANTN0018","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:ANTN0023","RUGGEDCOM ANTN0023 GPS antenna for WiN7000 ANTN0023 ANT GPS Omni 1575.42MHz, +/- 1.023 30dB 360 degrees 3V TNC",296,"ΤΕΜ",1,"SIMATIC",1,"RUM:ANTN0023","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:ANTN0027","RUGGEDCOM ANTN0027 ANT Sector 3.3-3.8GHz 17dBi 65 deg. X-Pol",1299,"ΤΕΜ",1,"SIMATIC",1,"RUM:ANTN0027","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:ANTN0029","RUGGEDCOM ANTN0029 ANT Sector BST 3.3-3.8GHz 17dBi 90 deg. X-Pol",476,"ΤΕΜ",1,"SIMATIC",1,"RUM:ANTN0029","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:ANTN0040","RUGGEDCOM ANTN0040 ANT Omni 3.4-3.7GHz 8.5dBi 360 deg. N-Male",174,"ΤΕΜ",1,"SIMATIC",1,"RUM:ANTN0040","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:ANTN0043","RUGGEDCOM ANTN0043 Low gain Omni Antenna 3.4-3.6GHz 6dBi 360 deg.",188,"ΤΕΜ",1,"SIMATIC",1,"RUM:ANTN0043","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:ANTN0048","RUGGEDCOM ANTN0048 ANT Sector 2300-2700MHz 16dBi 90 Deg. X-Pol",808,"ΤΕΜ",1,"SIMATIC",1,"RUM:ANTN0048","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:ANTN0050","RUGGEDCOM ANTN0050 ANT Omni BST 2.3-2.7GHz 9dBi 360 deg. N-Female",520,"ΤΕΜ",1,"SIMATIC",1,"RUM:ANTN0050","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:ANTN0051","RUGGEDCOM ANTN0051 Low gain Omni Antenna 2.5-2.7GHz 5.5dBi 360 deg. N-male",188,"ΤΕΜ",1,"SIMATIC",1,"RUM:ANTN0051","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:ANTN0057","RUGGEDCOM ANTN0057 Low gain Omni Antenna 3.6-3.8GHz 6dBi 360 deg.",188,"ΤΕΜ",1,"SIMATIC",1,"RUM:ANTN0057","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:ANTN0061","RUGGEDCOM ANTN0061 High gain Omni Antenna 1.7-1.9 GHz - 10dBi N-female",916,"ΤΕΜ",1,"SIMATIC",1,"RUM:ANTN0061","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:ANTN0063","RUGGEDCOM ANTN0063 ANT Dual Slant Plate 2.3-2.7GHz 17dBi - KIT",549,"ΤΕΜ",1,"SIMATIC",1,"RUM:ANTN0063","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:ANTN0064","RUGGEDCOM ANTN0064 ANT Flat CPE 3.3-3.8GHz 18dBi 18 deg. N-Type",476,"ΤΕΜ",1,"SIMATIC",1,"RUM:ANTN0064","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:ANTN0065","RUGGEDCOM ANTN0065 Vehicular Antenna 0.68- 6.0 GHz, 6dBi",469,"ΤΕΜ",1,"SIMATIC",1,"RUM:ANTN0065","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:ANTN0066","RUGGEDCOM ANTN0066 ANT Dual Slant 1.78-1.85GHz 12DBI N-TYPE - KIT",476,"ΤΕΜ",1,"SIMATIC",1,"RUM:ANTN0066","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:ANTN0068","RUGGEDCOM ANTN0068 Sector Antenna 2.3-2.7 GHz, 16 dBi 65 Deg. X-Pol",1169,"ΤΕΜ",1,"SIMATIC",1,"RUM:ANTN0068","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:ANTN0070","RUGGEDCOM ANTN0070 Antenna Dual Slant sector 1.71-1.880 GHz 17 dBi 90 degree",1818,"ΤΕΜ",1,"SIMATIC",1,"RUM:ANTN0070","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:ANTN0071","RUGGEDCOM ANTN0071 ANT 1390-1525MHz Sector 16.0 dBi",1818,"ΤΕΜ",1,"SIMATIC",1,"RUM:ANTN0071","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:ANTN0073","RUGGEDCOM ANTN0073 ANT Dual Slant antenna 4.9-6.1GHz 22.5dBi NTYPE",476,"ΤΕΜ",1,"SIMATIC",1,"RUM:ANTN0073","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:ANTN0074","RUGGEDCOM ANTN0074 ANT Sector Dual Slant 4.9 - 5.95 GHz 16dBi 90",1068,"ΤΕΜ",1,"SIMATIC",1,"RUM:ANTN0074","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:ANTN0075","RUGGEDCOM ANTN0075 ANT Omni 806-5935MHz 9.5dBi N-Female",606,"ΤΕΜ",1,"SIMATIC",1,"RUM:ANTN0075","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:ANTN0076","RUGGEDCOM ANTN0076 ANT Omni 4.9-5.875GHz 9.5dBi N-Female",303,"ΤΕΜ",1,"SIMATIC",1,"RUM:ANTN0076","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:ANTN0077","RUGGEDCOM ANTN0077 Vehicular Antenna 2.3 - 6.1GHz 8dBi N-FemaleY",426,"ΤΕΜ",1,"SIMATIC",1,"RUM:ANTN0077","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:ANTN0078","RUGGEDCOM ANTN0078 Sector Antenna Dual Slant 5 - 5.95 GHz 16dBi 65Deg With mounting kit.",2784,"ΤΕΜ",1,"SIMATIC",1,"RUM:ANTN0078","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:ANTN0079","RUGGEDCOM ANTN0079 Antenna Dual Slant 1750-1850 MHz Dual Polarization, 17dBi",1320,"ΤΕΜ",1,"SIMATIC",1,"RUM:ANTN0079","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:ANTN0084","RUGGEDCOM ANTN0084 ANT Sector Dual Slant 4.9â€“5.95GHz 13.5dBi 120 KIT",2121,"ΤΕΜ",1,"SIMATIC",1,"RUM:ANTN0084","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBDC0017","RUGGEDCOM CBDC0017 BST serial Cable UART 3P to DB9F",54,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBDC0017","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBDC0034","Adapter Cable from WIN1210/WIN1212 to WINPS cables CBDC0041/53/54/60/64, L=350mm",231,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBDC0034","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBDC0037","RUGGEDCOM CBDC0037 Power supply cable 12VDC 5 meter; Used to connect to vehicular DC",61.6,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBDC0037","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBDC0041","Cable Combo PWR+Eth 30M WINPS - WiN7000 only. For WIN121X use CDBC0110",815,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBDC0041","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBDC0045","RUGGEDCOM CBDC0045 Power supply cable 12VDC 5 meter; Open End to connect to DC supply",61.6,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBDC0045","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBDC0048","Cable PWR 30M Open End - WiN7000. Requires external power supply.",606,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBDC0048","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBDC0051","Cable PWR 80M Open End - WiN7000. Requires external power supply.",1392,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBDC0051","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBDC0052","Cable PWR 80M for WINPS - Used with SFA option of WIN7000. Not suiatble for WIN1210/1212",1457,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBDC0052","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBDC0053","Cable Combo PWR+Eth 60M WINPS - WiN7000 only. For WIN121X use CDBC0111",1306,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBDC0053","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBDC0054","Cable Combo PWR+Eth 80M WINPS - WiN7000 only. For WIN121X use CDBC0112",1630,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBDC0054","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBDC0055","Cable PWR 60M Open End - WiN7000. Requires external power supply.",1097,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBDC0055","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBDC0056","Cable PWR 60M for WINPS - WiN7000 only. For WIN121X use CDBC0121",1154,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBDC0056","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBDC0058","Cable PWR 2M for WINPS - WiN7000 only. For WIN121X use CDBC0135",347,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBDC0058","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBDC0060","Cable Combo PWR+Eth 2M WINPS - WiN7000 only. For WIN121X use CDBC0131",347,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBDC0060","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBDC0061","RUGGEDCOM CBDC0061 Cable used to convert legacy Combo cable to new mechanicals of WIN7000",267,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBDC0061","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBDC0072","RUGGEDCOM CBDC0072 0.3M + 6M (CBDC0057-02 & CBDC0073) SOURIAU",621,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBDC0072","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBDC0110","Cable Combo PWR+Eth 30M WIN1210/WIN1212-WiN7000+48V",815,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBDC0110","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBDC0111","Cable Combo PWR+Eth 60M WIN1210/WIN1212-WiN7000+48V",1306,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBDC0111","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBDC0112","Cable Combo PWR+Eth 80M WIN1210/WIN1212-WiN7000+48V",1630,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBDC0112","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBDC0113","Cable Combo PWR+Eth 30M WIN1210/WIN1212-WiN7000-48V.",815,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBDC0113","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBDC0114","Cable Combo PWR+Eth 60M WIN1210/WIN1212-WiN7000-48V.",1306,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBDC0114","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBDC0115","Cable Combo PWR+Eth 80M WIN1210/WIN1212-WiN7000-48V.",1630,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBDC0115","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBDC0120","Cable PWR 30M WIN1210/WIN1212-WiN7000+48V.",606,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBDC0120","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBDC0121","Cable PWR 60M WIN1210/WIN1212-WiN7000+48V.",938,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBDC0121","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBDC0122","Cable PWR 80M WIN1210/WIN1212-WiN7000+48V.",1190,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBDC0122","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBDC0123","Cable PWR 30M WIN1210/WIN1212-WiN7000-48V.",606,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBDC0123","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBDC0124","Cable PWR 60M WIN1210/WIN1212-WiN7000-48V.",938,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBDC0124","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBDC0125","Cable PWR 80M WIN1210/WIN1212-WiN7000-48V.",1190,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBDC0125","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBDC0131","Cable Combo PWR+Eth 2M WIN1210/WIN1212-WiN7000+48V.",347,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBDC0131","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBDC0133","Cable Combo PWR+Eth 2M WIN1210/WIN1212-WiN7000-48V.",347,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBDC0133","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBDC0135","Cable PWR 2M WIN1210/WIN1212-WiN7000+48V.",354,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBDC0135","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBDC0136","Cable PWR 120M WIN1210/WIN1212-WiN7000+48V.",1775,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBDC0136","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBDC0137","Cable PWR 2M WIN1210/WIN1212-WiN7000-48V.",347,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBDC0137","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBDC0138","Cable PWR 120M WIN1210/WIN1212-WiN7000-48V.",1775,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBDC0138","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBDC0139","Cable DC open end, M12-4 female, 2m",94.199999999999989,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBDC0139","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBDC0140","Cable DC open end, M12-4 female, 5m",231,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBDC0140","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBDC0141","Cable DC open end, M12-4 female, 15m",347,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBDC0141","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBDC0160","Power cable 5m, 4 pin M12, PVC, left M12 male and 12 V cigarette lighter plug, -40 to 80 C operating and storage temperature rating",202,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBDC0160","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBET0151","Cable, M12-4 male, RJ45, 2m",73,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBET0151","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBET0152","Cable, M12-4 male, RJ45, 15m",210,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBET0152","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBET0153","Cable, M12-4 male, M12-4 male, 2m",82.8,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBET0153","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBET0154","Cable, M12-4 male, M12-4 male, 15m",231,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBET0154","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBET0160","Cable, M12-4 male, RJ45, 30m",296,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBET0160","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBET0161","Cable, M12-4 male, RJ45, 45m",469,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBET0161","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBET0162","Cable, M12-4 male, RJ45, 60m",599,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBET0162","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBET0163","Cable, M12-4 male, RJ45, 75m",707,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBET0163","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBET0164","Cable, M12-4 male, RJ45, 90m",873,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBET0164","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBET0165","Cable, M12-4 male, M12-4 male, 30m",383,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBET0165","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBET0166","Cable, M12-4 male, M12-4 male, 45m",491,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBET0166","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBET0167","Cable, M12-4 male, M12-4 male, 60m",621,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBET0167","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBET0168","Cable, M12-4 male, M12-4 male, 75m",729,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBET0168","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBET0169","Cable, M12-4 male, M12-4 male, 90m",895,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBET0169","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBRF0032","RUGGEDCOM CBRF0032 GPS cable for use with WiN7000 (LMR200) 900mm",100,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBRF0032","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBRF0037","Cable GPS RF RG58 Black 15m TNC male to TNC male",144,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBRF0037","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBRF0040","RUGGEDCOM CBRF0040 GPS cable for use with WiN7200 (LMR 200) 350 mm",100,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBRF0040","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBRF0055","RUGGEDCOM CBRF0055 Cable RF RG214/U 1.6m N-Type male to 7/16 male for 1.8 GHz band only",127,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBRF0055","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBRF0057","RUGGEDCOM CBRF0057 Cable RF 5m N-Type male to N-Type",127,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBRF0057","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBRF0061","RUGGEDCOM CBRF0061 Cable RF LMR400 1.6m N-Type male to N-Type male",127,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBRF0061","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBRF0064","RUGGEDCOM CBRF0064 Cable RF LMR400 3m N-Type male to N-Type male",127,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBRF0064","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBWR0009","RUGGEDCOM CBWR0009 Fiber Optic Ethernet 3m cable, SM, 1310 nm, Sealed LC Duplex connectors to LC Duplex",303,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBWR0009","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBWR0019","RUGGEDCOM CBWR0019 Fiber Optic Ethernet 30m cable, SM, 1310 nm, Sealed LC Duplex connectors To LC Duplex",476,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBWR0019","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBWR0020","RUGGEDCOM CBWR0020 Fiber Optic Ethernet 50m cable, SM, 1310 nm, Sealed LC Duplex connectors To LC Duplex",671,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBWR0020","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBWR0021","RUGGEDCOM CBWR0021 Fiber Optic Ethernet 100m cable, SM, 1310 nm, Sealed LC Duplex connectors To LC Duplex",1003,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBWR0021","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBWR0022","RUGGEDCOM CBWR0022 Fiber Optic Ethernet 150m cable, SM, 1310 nm, Sealed LC Duplex connectors To LC Duplex",1500,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBWR0022","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CBWR0023","RUGGEDCOM CBWR0023 Fiber Optic Ethernet 200m cable, SM, 1310 nm, Sealed LC Duplex connectors To LC Duplex",2005,"ΤΕΜ",1,"SIMATIC",1,"RUM:CBWR0023","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:CNAD0091","WIN7200 PoE cable Connector kit. RJ45 IP67 cable side shielded HARTING. Comes in the box with new WIN7200 base station.",159,"ΤΕΜ",1,"SIMATIC",1,"RUM:CNAD0091","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:DCPS0006","RUGGEDCOM DCPS0006 Indoor AC/DC Power Supply (PoE)",102,"ΤΕΜ",1,"SIMATIC",1,"RUM:DCPS0006","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:DCPS0008","RUGGEDCOM DCPS0008 DC-DC converter 130 VDC - 48 VDC for WIN7000 series",1500,"ΤΕΜ",1,"SIMATIC",1,"RUM:DCPS0008","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:DCPS0100","RUGGEDCOM DCPS0100 Power supply AC/DC 85-264V input , 48V output, 240W. TDK Lambda.",549,"ΤΕΜ",1,"SIMATIC",1,"RUM:DCPS0100","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:MKIT0028","RUGGEDCOM MKIT0028 CPE Wall and Tilt Mounting KIT",92.399999999999991,"ΤΕΜ",1,"SIMATIC",1,"RUM:MKIT0028","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:MKIT0060","RUGGEDCOM MKIT0060 19-In Rack Mount kit for WIN7000 base station, 1 for 2 BST",476,"ΤΕΜ",1,"SIMATIC",1,"RUM:MKIT0060","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:MKIT0066","RUGGEDCOM MKIT0066 Filters for WIN7023 Base station to meet FCC mask -- comes with mounting kit, 2 RF cables, 2 cavity filters (A/B band only)",1832,"ΤΕΜ",1,"SIMATIC",1,"RUM:MKIT0066","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:MKIT0073","RUGGEDCOM MKIT0073 Filters for WIN 7023 Base station to meet FCC mask ; comes with mounting kit, 2 RF cables, 2 cavity filters (C/D band only)",1659,"ΤΕΜ",1,"SIMATIC",1,"RUM:MKIT0073","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:MKIT0090","Required for Class1/Div2 in addtion with the standart package: WIN72XX,WIN52XX or WIN51XX-AC. Class1 Div2, includes Power supply AC/DC 85-264V input, 48V output, 50W, PoE and surge Protection, Power Cable 3 meter open End",397,"ΤΕΜ",1,"SIMATIC",1,"RUM:MKIT0090","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:MKIT0091","RUGGEDCOM MKIT0091 N-Male Omni antennas Mount kit , includes N-type adapter- one per antenna",86.5,"ΤΕΜ",1,"SIMATIC",1,"RUM:MKIT0091","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:MPHG0135","L-Shaped Mounting Bracket for GPS antenna",174,"ΤΕΜ",1,"SIMATIC",1,"RUM:MPHG0135","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:WIN1010","RUGGEDCOM WIN1010 Power Supply Indoor AC/DC PS 48V with PoE",92.399999999999991,"ΤΕΜ",1,"SIMATIC",1,"RUM:WIN1010","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:WIN1210","RUGGEDCOM WIN1210 with Power supply AC/DC 85-264V input, 48V output, 240W",1558,"ΤΕΜ",1,"SIMATIC",1,"RUM:WIN1210","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:WIN5251","High Gain Outdoor Subscriber unit, integrated directional dual slant antenna includes commercial grade power supply, 5000MHz to 5150MHz. This product is dedicated to AeroMACS.",2178,"ΤΕΜ",1,"SIMATIC",1,"RUM:WIN5251","Βιομηχανικός αυτοματισμός SIMATIC"]
["RUM:WIN7251","Small Form Factor Outdoor Base Station, includes power supply, 2x antenna cable 1.6 m, GPS receiver, GPS antenna and mounting kit; antenna and data cable ordered separately, 5000 MHz to 5150MHz. This product is dedicated to AeroMACS.",15577,"ΤΕΜ",1,"SIMATIC",1,"RUM:WIN7251","Βιομηχανικός αυτοματισμός SIMATIC"]
["S79220-B6273-F888","SIMATIC CFC, software for SPPA-T3000 AS-S7-CPU410H floating license for 1 user E-SW, without SW, without documentation License key on USB stick, Class A, 6 languages (de, en, fr, it, es, cn) executable under XPPROF SP3/ WINSRV2003R2 SP2/ WIN7 ULT SP1/WIN7 Prof SP1/ Server 2008 R2 SP1 Reference HW: PC/PG ******************************* Content: Set (1x DVD + 1x USB)",84,"ΤΕΜ",1,"SIMATIC",1,"S79220B6273F888","Βιομηχανικός αυτοματισμός SIMATIC"]
["S79220-B8655-P","SIMATIC WINCC V7.5 Data carrier without license, Use only in connection with valid license",32.700000000000003,"ΤΕΜ",1,"SIMATIC",1,"S79220B8655P","Βιομηχανικός αυτοματισμός SIMATIC"]
["S79220-B9194-P","SIMATIC WINCC V7.5 SP1 Data carrier without license, Use only in connection with valid license",32.700000000000003,"ΤΕΜ",1,"SIMATIC",1,"S79220B9194P","Βιομηχανικός αυτοματισμός SIMATIC"]
["S79220-C1106-F888","SIMIT Simulation Software Promoter ______________________ Software Update Service, within the framework of this contract, you will receive for one year all current software versions. The contract is extended automatically by 1 year if it is not canceled 3 months prior to expiration. Period of delivery and service: 1 year from date of invoice Requirement for conclusion: Current version of the software. Content: 1x certificate",127,"ΤΕΜ",1,"SIMATIC",1,"S79220C1106F888","Βιομηχανικός αυτοματισμός SIMATIC"]
["S79220-C1110-F888","SIMIT Simulation Platform software Engineering XS floating license for 1 user engineering software software and documentation on USB, class A, 2 languages (de, en), executable in Windows 7 SP1, Windows 10 LTSB 2015, Windows 10 (1909), Windows Server 2012 R2 / 2016, for more information, see SIMIT V10.2 Readme, reference hardware: PC/PG content: 2 x USB",560,"ΤΕΜ",1,"SIMATIC",1,"S79220C1110F888","Βιομηχανικός αυτοματισμός SIMATIC"]
["S79220-C1441-F888","SIMATIC STEP 7 Professional V17 engineering software,Trial365 license software and documentation on DVD class A license key on USB flash drive 9 languages: de,en,zh included, fr,sp,it,ru,jp,kr as download; executable in Windows 10, Windows Server 2016/2019; for configuration of SIMATIC S7-1200/1500 SIMATIC S7-300/400/WinAC SIMATIC Basic Panels ******************************* content: set (4x DVD + 1x USB)",2471,"ΤΕΜ",1,"SIMATIC",1,"S79220C1441F888","Βιομηχανικός αυτοματισμός SIMATIC"]
["S79220-C1553-F888","SIMIT Simulation V10.2 software Component creation Package Single Package Floating License for 1 user engineering software software and documentation on CD, class A, 2 languages (de, en), executable in Windows 7 SP1, Windows 10 LTSB 2015, Windows 10 (1909), Windows Server 2012 R2 / 2016, for more information see SIMIT V10.2 Readme, reference hardware: PC/PG content: 1x CD + 1x USB",4480,"ΤΕΜ",1,"SIMATIC",1,"S79220C1553F888","Βιομηχανικός αυτοματισμός SIMATIC"]
["S79220-C1634-F888","SIMIT Simulation Software Promoter ______________________ Software Update Service within the framework of this contract, you will receive for one year all up-to-date software versions. The contract is extended automatically by 1 year, if not canceled 3 months prior to expiration. period of delivery and service: 1 year from date of invoice requirement for conclusion: current version of the software. ******_download_product_******* e-mail address required for delivery",112,"ΤΕΜ",1,"SIMATIC",1,"S79220C1634F888","Βιομηχανικός αυτοματισμός SIMATIC"]
["S79220-C2163-F888","SIMATIC STEP 7 Professional V18 engineering software,Trial365 license software and documentation on DVD class A license key on USB flash drive 9 languages: de,en,zh included, fr,es,it,ru,ja,ko as download; executable on Windows 10; Windows 11; Windows Server 2016/2019/2022; for configuration of SIMATIC S7-1200/1500 SIMATIC S7-300/400/WinAC SIMATIC Basic Panels ******************************* content: set (4x DVD + 1x USB)",2471,"ΤΕΜ",1,"SIMATIC",1,"S79220C2163F888","Βιομηχανικός αυτοματισμός SIMATIC"]
["S79220-C2982-F888","SIMIT Simulation V11.1 software promoter package (for Siemens promoters only!) floating license for 1 user engineering software without software, without documentation, class A, 2 languages (de, en), executable in Windows 10 (21H2), Windows 10 LTSC 2019, Windows Server 2016 / 2019, for more information, see SIMIT V11.1 Readme, reference hardware: PC/PG content: 1x certificate order only in connection with: 6DL8900-7XX00-0XB8-Z Y01 Y02",270,"ΤΕΜ",1,"SIMATIC",1,"S79220C2982F888","Βιομηχανικός αυτοματισμός SIMATIC"]
["S79220-C2983-F888","SIMIT Simulation V11.1 software promoter package Single Package floating license for 1 user engineering software software and documentation on USB, class A, 2 languages (de, en), executable in Windows 10 (21H2), Windows 10 LTSC 2019, Windows Server 2016 / 2019, for more information, see SIMIT V11.1 Readme, reference hardware: PC/PG content: 2 x USB",324,"ΤΕΜ",1,"SIMATIC",1,"S79220C2983F888","Βιομηχανικός αυτοματισμός SIMATIC"]
["S79220-C2984-F888","SIMIT Simulation V11.1 software PoC Package (100 days) Single Package floating license for 1 user engineering software software and documentation on USB, class A, 2 languages (de, en), executable in Windows 10 (21H2), Windows 10 LTSC 2019, Windows Server 2016 / 2019, for more information, see SIMIT V11.1 Readme, reference hardware: PC/PG content: 2 x USB",336,"ΤΕΜ",1,"SIMATIC",1,"S79220C2984F888","Βιομηχανικός αυτοματισμός SIMATIC"]
["S79220-C2985-F888","SIMIT Simulation V11.1 software Component Creation Package Single Package floating license for 1 user engineering software software and documentation on USB, class A, 2 languages (de, en), executable in Windows 10 (21H2), Windows 10 LTSC 2019, Windows Server 2016 / 2019, for more information, see SIMIT V11.1 Readme, reference hardware: PC/PG content: 2 x USB",4704,"ΤΕΜ",1,"SIMATIC",1,"S79220C2985F888","Βιομηχανικός αυτοματισμός SIMATIC"]
["S79220-C2987-F888","SIMIT Simulation V11.1 software promoter package (for Siemens promoters only!) floating license for 1 user engineering software without software, without documentation, class A, 2 languages (de, en), executable in Windows 10 (21H2), Windows 10 LTSC 2019, Windows Server 2016 / 2019, for more information, see SIMIT V11.1 Readme, reference hardware: PC/PG ******_download_product_******* order only in connection with: 6DL8900-7XX00-0XH8-Z Y01 Y02",247,"ΤΕΜ",1,"SIMATIC",1,"S79220C2987F888","Βιομηχανικός αυτοματισμός SIMATIC"]
["S79630-G26-A900","Eeprom package",97,"ΤΕΜ",1,"PI1",1,"S79630G26A900","Όργανα Μέτρησης Πεδίου"]
["S79630-G27-A900","Read-only memory package",51,"ΤΕΜ",1,"PI1",1,"S79630G27A900","Όργανα Μέτρησης Πεδίου"]
["UAC:FN3440110118E2FAJRX","G120 LINE HARMONICS FILTER 400V 110 kW",10230,"ΤΕΜ",1,"GMC",1,"UAC:FN3440110118E2FAJRX","Ρυθμιστές στροφών και συστήματα Motion control"]
["UAC:FN344011113E2FAJRX","Schaffner Line harmonics filter 400V 11 kW",2753,"ΤΕΜ",1,"GMC",1,"UAC:FN344011113E2FAJRX","Ρυθμιστές στροφών και συστήματα Motion control"]
["UAC:FN3440132118E2FAJXX","G120 LINE HARMONICS FILTER 400V 132 kW",10962,"ΤΕΜ",1,"GMC",1,"UAC:FN3440132118E2FAJXX","Ρυθμιστές στροφών και συστήματα Motion control"]
["UAC:FN344015113E2FAJRX","G120 LINE HARMONICS FILTER 400V 15 kW",3295,"ΤΕΜ",1,"GMC",1,"UAC:FN344015113E2FAJRX","Ρυθμιστές στροφών και συστήματα Motion control"]
["UAC:FN3440160118E2FAJXX","G120 LINE HARMONICS FILTER 400V 160 kW",11997,"ΤΕΜ",1,"GMC",1,"UAC:FN3440160118E2FAJXX","Ρυθμιστές στροφών και συστήματα Motion control"]
["UAC:FN344019113E2FAJRX","G120 LINE HARMONICS FILTER 400V 18.5 kW",3295,"ΤΕΜ",1,"GMC",1,"UAC:FN344019113E2FAJRX","Ρυθμιστές στροφών και συστήματα Motion control"]
["UAC:FN3440200118E2FAJXX","G120 LINE HARMONICS FILTER 400V 200 kW",14298,"ΤΕΜ",1,"GMC",1,"UAC:FN3440200118E2FAJXX","Ρυθμιστές στροφών και συστήματα Motion control"]
["UAC:FN344022115E2FAJRX","G120 LINE HARMONICS FILTER 400V 22 kW",3805,"ΤΕΜ",1,"GMC",1,"UAC:FN344022115E2FAJRX","Ρυθμιστές στροφών και συστήματα Motion control"]
["UAC:FN344030115E2FAJRX","G120 LINE HARMONICS FILTER 400V 30 kW",4355,"ΤΕΜ",1,"GMC",1,"UAC:FN344030115E2FAJRX","Ρυθμιστές στροφών και συστήματα Motion control"]
["UAC:FN344037115E2FAJRX","G120 LINE HARMONICS FILTER 400V 37 kW",5103,"ΤΕΜ",1,"GMC",1,"UAC:FN344037115E2FAJRX","Ρυθμιστές στροφών και συστήματα Motion control"]
["UAC:FN344045115E2FAJRX","G120 LINE HARMONICS FILTER 400V 45 kW",5818,"ΤΕΜ",1,"GMC",1,"UAC:FN344045115E2FAJRX","Ρυθμιστές στροφών και συστήματα Motion control"]
["UAC:FN344055115E2FAJRX","G120 LINE HARMONICS FILTER 400V 55 kW",6738,"ΤΕΜ",1,"GMC",1,"UAC:FN344055115E2FAJRX","Ρυθμιστές στροφών και συστήματα Motion control"]
["UAC:FN34406112E2XXJRX","Schaffner Line harmonics filter 400V",2030,"ΤΕΜ",1,"GMC",1,"UAC:FN34406112E2XXJRX","Ρυθμιστές στροφών και συστήματα Motion control"]
["UAC:FN344075116E2FAJRX","G120 LINE HARMONICS FILTER 400V 75 kW",8308,"ΤΕΜ",1,"GMC",1,"UAC:FN344075116E2FAJRX","Ρυθμιστές στροφών και συστήματα Motion control"]
["UAC:FN34408112E2XXJRX","Schaffner Line harmonics filter 400V 7.5 Kw",2301,"ΤΕΜ",1,"GMC",1,"UAC:FN34408112E2XXJRX","Ρυθμιστές στροφών και συστήματα Motion control"]
["UAC:FN344090116E2FAJRX","G120 LINE HARMONICS FILTER 400V 90 kW",9351,"ΤΕΜ",1,"GMC",1,"UAC:FN344090116E2FAJRX","Ρυθμιστές στροφών και συστήματα Motion control"]
["W73078-B1001-A703","3-pin terminal for relay (6DR2804-8A/8B) MODULES",57,"ΤΕΜ",1,"PI1",2,"W73078B1001A703","Όργανα Μέτρησης Πεδίου"]
["W73078-B1001-A705","5-pin terminal for option modules 6DR2801-8A,B,C and 6DR2802-8A MODULES",59,"ΤΕΜ",1,"PI1",2,"W73078B1001A705","Όργανα Μέτρησης Πεδίου"]
["W73078-B1001-A706","6-pin terminal for option module 6DR2804-8A/8B MODULES",61,"ΤΕΜ",1,"PI1",2,"W73078B1001A706","Όργανα Μέτρησης Πεδίου"]
["W73078-B1001-A710","10-pin terminal (main board) for SIPART DR22/24",74,"ΤΕΜ",1,"PI1",1,"W73078B1001A710","Όργανα Μέτρησης Πεδίου"]
["W73078-B1001-A714","14-pin terminal (main board) for SIPART DR22/24",82,"ΤΕΜ",1,"PI1",2,"W73078B1001A714","Όργανα Μέτρησης Πεδίου"]
["W73078-B1001-A904","4-pin terminal for module I/U, R, P (6DR2800-8J / -8R / -8P) MODULES",62,"ΤΕΜ",1,"PI1",2,"W73078B1001A904","Όργανα Μέτρησης Πεδίου"]
["W73078-B1001-A906","6-pin terminal for option modules for 6DR2801-8D and 6DR2800-8A MODULES",61,"ΤΕΜ",1,"PI1",2,"W73078B1001A906","Όργανα Μέτρησης Πεδίου"]
["W73078-B1003-A904","4-pin terminal (6DR2800-8V) for SIPART DR19/21 and SITRANS T",9,"ΤΕΜ",1,"PI1",1,"W73078B1003A904","Όργανα Μέτρησης Πεδίου"]
["W73078-B1017-A908","8-pin terminal for SIPART DR19/21",16,"ΤΕΜ",1,"PI1",1,"W73078B1017A908","Όργανα Μέτρησης Πεδίου"]
["W73078-B1018-A903","3-pin terminal for SIPART DR19/21",5,"ΤΕΜ",1,"PI1",1,"W73078B1018A903","Όργανα Μέτρησης Πεδίου"]
["W73078-B3001-A705","5POL. TERMINAL FOR MODULE",14,"ΤΕΜ",1,"PI1",2,"W73078B3001A705","Όργανα Μέτρησης Πεδίου"]
["W73703-A1-A6","Screwed cable gland pg 13,5 fs",8,"ΤΕΜ",1,"PI2",5,"W73703A1A6","Όργανα Μέτρησης Πεδίου"]
["W79084-E1001-B2","Lithium battery SIMATIC HMI and C7 Further information, Quantity and content: see technical data",36.700000000000003,"ΤΕΜ",1,"SIMATIC",1,"W79084E1001B2","Βιομηχανικός αυτοματισμός SIMATIC"]
["ZNX:EIP200PRO","SIMATIC DP, Ethernet/IP head assembly for ET 200 PRO, max. 12 I/O modules incl. motor starter no F modules integrated 2-port switch incl. configuration tool (DVD)",548,"ΤΕΜ",1,"SIMATIC",1,"ZNX:EIP200PRO","Βιομηχανικός αυτοματισμός SIMATIC"]
["ZNX:EIP200PROCM1","SIMATIC DP, Connection module for Ethernet/IP head assembly ET 200 PRO; M12/7/8\", 2x M12 and 2x 7/8\"",94.399999999999991,"ΤΕΜ",1,"SIMATIC",1,"ZNX:EIP200PROCM1","Βιομηχανικός αυτοματισμός SIMATIC"]
["ZNX:SYSTA8","TANOS SYSTAINER II T-LOC anthracite RAL 7016",174,"ΤΕΜ",1,"SIMATIC",1,"ZNX:SYSTA8","Βιομηχανικός αυτοματισμός SIMATIC"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet1","index":2,"n_rows":13,"n_cols":2,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["PA","PMD Data available"]
[""]
["VF","Sales Release"]
[""]
["LF","Delivery Release"]
[""]
["AE","Phase Out Announce"]
[""]
["TS","Prod. Cancellation"]
[""]
["MH","Prod. Discont."]
[""]
["AK","End Prod.Lifecycl."]